#############################################################################################
## Configuration template for GXW42XX firmware version 1.0.11.3                           ##
#############################################################################################

################################################################################
#Maintenance-Network setting
################################################################################

#IP Address Mode. 0 - DHCP, 1 - Static IP, 2 - PPPoE
#Number: 0,1,2
#Mandatory 
#Reboot required 
P8=0

#Preferred DNS server
#Mandatory 
P92=0
P93=0
P94=0
P95=0

#Host name (Option 12). Max length allowed is 32 bytes.
#String: address 
P146=

#DHCP Domain
#String: address 
P147=

#Vendor Class ID (Option 60). Max length allowed is 32 bytes.
#String Max Length: 32 
P148=GXW4200

# Client Circuit ID (Option 82)
# String
P8560= 

# Remote Agent ID (Option 82)
# String
P8561= 

#PPPoE account ID
#P82=

#PPPoE password
#P83=

#PPPoE Service Name
#String Max Length: 64
#Reboot required 
P269=
	
#IP Address. Ignore if DHCP or PPPoE is used
#P9=192
#P10=168
#P11=0
#P12=160

#Subnet mask. Ignore if DHCP or PPPoE is used
#P13=255
#P14=255
#P15=0
#P16=0

#Gateway. Ignore if DHCP or PPPoE is used
#P17=0
#P18=0
#P19=0
#P20=0

#DNS server 1. Ignore if DHCP or PPPoE is used
#P21=0
#P22=0
#P23=0
#P24=0

#DNS server 2. Ignore if DHCP or PPPoE is used
#P25=0
#P26=0
#P27=0
#P28=

# Enable management interface. 0 - Disabled, 1 - Enabled
# Number: 0, 1
# Mandatory
P28161 = 0

# Management access. 0- Management interface only, 1 - Both on services and management interfaces
# Number： 0， 1
# Mandatory
P28162 = 0

# IP Address Mode for Management Interface. 0 - DHCP, 1 - Static IP
# Number: 0, 1
# Mandatory = 0
P22105 = 0

# Static IP Settings
# IP Address.
# ipaddress
P22106 = 192.168.100.100

# Subnet Mask. 
# ipaddress
P22107 = 255.255.255.0

# Gateway.
# ipaddress
P22108 = 192.168.100.1

# DNS Server 1
# ipaddress
P22109 = 0.0.0.0

# DNS Server 2
# ipaddress
P22110 = 0.0.0.0


#Enable LLDP. 0 - Disable, 1 - Enable
#Number: 0,1
#Mandatory                                      
P1684=1

#Layer 2 QoS 802.1Q/VLAN Tag for Service Interface
#Number
#Mandatory
P51=0

# Layer 2 QoS 802.1Q/VLAN Tag for Management Interface.
# Number
P22111 = 0

#Layer 2 QoS 802.1p Priority Value for SIP signaling
#Number: 0 to 7
#Mandatory
P5038=0

#Layer 2 QoS 802.1p Priority Value for RTP media
#Number: 0 to 7
#Mandatory
P5042=0

# Layer 2 QoS 802.1p Priority Value for Management Interface.
# Number
P22112 = 0

#Use STUN to detect network connectivity. 0 - No, 1 - Yes. 
#Number: 0,1
#Mandatory
P474=0

#STUN server
#String: serveraddress 
P76=

#Number of STUN Response Misses Allowed
#Number: 3 to 15
#Mandatory
P475=3

#Keep-alive interval (in seconds. default 20 seconds)
#Number: 10 to 160
#Mandatory
P84=20

#Black List for WAN Side Port.
P28115=

# Reply to ICMP. 0 -No, 1 -Yes
# Number: 0, 1
# Mandatory
P189 = 0

# Local DNS
# String
# Syntax: FQDN0/IP0; FQDN1/IP1; FQDN2/IP2; FQDN3/IP3
P8562= 

################################################################################
#Maintenance-Upgrade and Provisioning
################################################################################

#Lock keypad update.  0 - No, 1 - Yes.
#Number: 0,1
#Mandatory
P88=0

#Use firmware pre/postfix to determine if f/w is required
#0=Always Check for New Firmware 
#1=Check New Firmware only when F/W pre/suffix changes 
#2=Always Skip the Firmware Check
#For Firmware only.
#Number: 0,1,2
#Mandatory 
P238=0

#XML Config File Password
#String Max Length: 40
#Mandatory; between ascii values 33 and 126
P1359=

#HTTP/HTTPS User Name
#String Max Length: 40; between ascii values 33 and 126
P1360=

#HTTP/HTTPS Password
#String Max Length: 40; between ascii values 33 and 126
#Mandatory
P1361=

#Always send HTTP Basic Authentication Information. 0 - No, 1- Yes.
#Number: 0,1
#Mandatory
P20713=0

#Firmware Upgrade and Privisioning. 0 - TFTP Upgrade, 1 - HTTP Upgrade, 2 - HTTPS Upgrade.
#Number: 0 to 2
#Mandatory
P212=1

#Firmware Server Path
#String: serveraddress 
P192=fm.grandstream.com/gs

#Config Server Path
#String: serveraddress 
P237=fm.grandstream.com/gs

#Firmware File Prefix
#String Max Length: 32; between ascii values 33 and 126
P232=

#Firmware File Postfix
#String Max Length: 32; between ascii values 33 and 126
P233=

#Config File Prefix
#String Max Length: 32; between ascii values 33 and 126
P234=

#Config File Postfix
#String Max Length: 32; between ascii values 33 and 126
P235=

#Allow DHCP Option 66 to override server. 0 - No, 1 - Yes. Default is Yes.
#When set to Yes(1), it will override the configured provision path and method.
#Number: 0,1
#Mandatory
#Reboot required 
P145=1

#Automatic Upgrade. 0 - No, 1 - Check every () minutes, 2 - Check daily, 3 - Check weekly,. Default is No.
#Number: 0,1,2,3
#Mandatory
P22296=0

#Automatic Upgrade. Check for new firmware/config file every () minutes, unit is in minute, minimum 60 minutes, default is 7 days. P194=3
#Number: 60 to 5256000
#Mandatory 
P193=10080

# Randomized Automatic Upgrade. 0 - No, 1 - Yes
# Number: 0, 1
# Mandatory
P8458 = 0

# Hour of the Day - End(0 -23). 
# Minimum: 0
# Maximum: 23
# Mandatory
P8459 = 22

#Automatic Upgrade. Daily at hour(0-23). P194=1
#Number: 0 to 23
#Mandatory
P285=1

#Automatic Upgrade. Weekly on day (0-6). P194=2
#Number: 0 to 6
#Mandatory 
P286=1

#Authenticate Conf File
#Number: 0 No, 1 Yes  (cfg file would be authenticated before acceptance if set to Yes) 
#Mandatory
P240=0

#Firmware Key (AES 128, in Hexadecimal Representation)
#String Max Length: 32 0-9,A-Z,a-z
P242=

################################################################################
#Maintenance-Web/Telnet Access
################################################################################

#HTTP Web Port. Default HTTP is 80.
#Number: 1 to 65535
#Mandatory 
#Reboot required 
P901=80

# HTTPS Web Port. Default HTTPS Port is 443
# Number: 1 to 65535
# Mandatory
P27010=443

# Web Access Mode. 0 - HTTPS, 1 - HTTP
# Number: 0, 1
# Mandatory
P1650=1

#Disable SSH. 0 - No, 1 - Yes
#Number: 0,1
#Mandatory 
P276=0

# Lockout time interval. minimum - 1 minute, maximum - 15 minutes
# Mandatory
P1683=15

# Disable User Level Web Access. 0 - No, 1 - Yes
# Number: 0, 1
# Mandatory
P28158 = 0

# Disable Viewer Level Web Access. 0 - No, 1 - Yes
# Number: 0, 1
# Mandatory
P28159 = 0

#User Password
#P196=123

#Admin password
#String Max Length: 30; between ascii values 33 and 126
#Mandatory
#P2=admin

# White list for WAN side
# String: ip address
P20701=

# Black list for WAN side
# String: ip address
P20702=

################################################################################
#Maintenance-TR-069
################################################################################

#Enable TR-069. 0 - No, 1 - Yes. Default is 0.
#Number: 0, 1
#Mandatory -->
P1409=0

#ACS URL
#P4503=

#ACS Username
#String Max Length: 64
P4504=

#ACS Password
#String Max Length: 64
#Mandatory 
P4505=

#Periodic Inform Enable 0 - No, 1 - Yes (default is No)
#Number: 0,1
#Mandatory
P4506=  0

#Periodic Inform Interval (default is 300)
#String Max Length: 5 
P4507= 300

#Conncetion Request Username
#String Max Length: 64
P4511=

#Connection Request Password
#String Max Length: 64
#Mandatory 
P4512=

# Connection Request Port. Default is 7547
# Number: 0 - 65535
# Mandatory
P4518 = 7547

################################################################################
#Maintenance-SNMP
################################################################################

#SNMP enable/disable. 0 - No, 1 - Yes (default is No)
#Number: 0,1
#Mandatory
P21896= 0

#Trap Community
P21900=

#IP Address
#IP format
P21897=

#Port (default 162)
#Number: 1 to 65535
#Mandatory
P21898= 162

#Version. 1 - Version 1, 2 - Version 2c (default 2)
#Number: 1 or 2
#Mandatory
P21899= 2

#Trap interval (default 5)
#Mandatory
P21901= 5

################################################################################
#Maintenance-Security Settings
################################################################################

#SIP TLS Certificate
#String
#P280=

#SIP TLS Private Key
#String
#P279=

#SIP TLS Private Key Password
#String
#Max Length: 64 characters
P281= s1pphone

# Custom Certificate
# String
P8472 = 

# Validate Server Certificates. 0 - No, 1 - Yes
# Number: 0, 1
# Mandatory
P8463 = 0

# Disable Weak TLS Cipher Suites. 0 - Enable Weak TLS Ciphers Suites, 1 - Disable Symmetric Encryption RC4/DES/3DES, 2 - Disable Symmetric Encryption SEED, 3 - Disable All Of The Above Weak Symmetric Encryption, 4 - Disable Symmetric Authentication MD5, 5 - Disable All Of The Above Weak Symmetric Authentication, 6 - Disable Protocol Version SSLv2/SSLv3, 7 - Disable All Of The Above Weak Protocol Version, 8 - Disable All Of The Above Weak TLS Ciphers Suites
# Number: 0 - 8
# Mandatory
P8536 = 0

# Minumum TLS version. 99 - Unlimited, 10 - TLS 1.0, 11 - TLS 1.1, 12 - TLS 1.2
# Number: 99, 10, 11, 12
# Mandatory
P22293 = 99 

# Maximum TLS version. 99 - Unlimited, 10 - TLS 1.0, 11 - TLS 1.1, 12 - TLS 1.2
# Number: 99, 10, 11, 12
# Mandatory
P22294 = 99

# Trusted CA certificate A.
# String
P2386= 

# Trusted CA certificate B.
# String
P2486= 

# Trusted CA certificate C.
# String
P2586= 

# Trusted CA certificate D.
# String
P2686= 

# Load CA Certificates. 0 - Built-in trusted certificates, 1 - Custom trusted certificates, 2 - All trusted certificates
# Number: 0, 1 ,2
# Mandatory
P8502 = 0

#Primary RADIUS Server
#P4550=

#Primary RADIUS Auth Port (default 1812). 
#Number: 1 to 65535
#Mandatory
P4551=1812

#Primary RADIUS Acct Port (default 1813).
#Number: 1 to 65535
#Mandatory
P4552=1813

#Primary RADIUS Server Secret
#String Max Length: 32
#Mandatory 
P4553=

#Secondary RADIUS Server
#P4554=

#Secondary RADIUS Auth Port (default 1812).
#Number: 1 to 65535
#Mandatory 
P4555=1812

#Secondary RADIUS Acct Port (default 1813).
#Number: 1 to 65535 
#Mandatory
P4556=1813

#Secondary RADIUS Server Secret
#String Max Length: 32
#Mandatory 
P4557=

#RADIUS Timeout (default 2).
#Number: 1 to 65535
#Mandatory 
P4558=2

#RADIUS Retry (default 3).
#Number: 1 to 65535
#Mandatory
P4559=3

################################################################################
#Maintenance-Date and Time
################################################################################

#NTP Server
#String: serveraddress 
P30=us.pool.ntp.org

#NTP Update Interval in minutes(5-1440)(Default is set to 60 minutes)
#Number: 5 to 1440
#Mandatory 
P5005=60

#Allow DHCP Option 42 to NTP Server. (If DHCP Option 42 is enabled, the NTP server can be changed.)
#Number: 0, 1
#Mandatory
P144=1

#Time Zone. Offset in minutes to GMT
#<value="TZA+12"> GMT-12:00 </option>
#<value="TZB+11"> GMT-11:00 </option>
#<value="TZC+10"> GMT-10:00 </option>
#<value="TZD+9"> GMT-09:00 </option>
#<value="TZE+8"> GMT-08:00 </option>
#<value="TZF+7"> GMT-07:00 </option>
#<value="TZG+6"> GMT-06:00 </option>
#<value="TZH+5"> GMT-05:00 </option>
#<value="TZf+4:30"> GMT-04:30 </option>
#<value="TZI+4"> GMT-04:00 </option>
#<value="TZJ+3:30"> GMT-03:30 </option>
#<value="TZK+3"> GMT-03:00 </option>
#<value="TZL+2"> GMT-02:00 </option>
#<value="TZM+1"> GMT-01:00 </option>
#<value="TZN+0"> GMT </option>
#<value="TZO-1"> GMT+01:00 </option>
#<value="TZP-2"> GMT+02:00 </option>
#<value="TZQ-3"> GMT+03:00 </option>
#<value="TZR-4"> GMT+04:00 </option>
#<value="TZS-5"> GMT+05:00 </option>
#<value="TZT-5:30"> GMT+05:30 </option>
#<value="TZU-5:45"> GMT+05:45 </option>
#<value="TZV-6"> GMT+06:00 </option>
#<value="TZW-6:30"> GMT+06:30 </option>
#<value="TZX-7"> GMT+07:00 </option>
#<value="TZY-8"> GMT+08:00 </option>
#<value="TZZ-9"> GMT+09:00 </option>
#<value="TZa-9:30"> GMT+09:30 </option>
#<value="TZb-10"> GMT+10:00 </option>
#<value="TZc-11"> GMT+11:00 </option>
#<value="TZd-12"> GMT+12:00 </option>
#<value="TZe-13"> GMT+13:00 </option>
#<value="customize"> Self-Defined Time Zone </option>
#Mandatory Category: string Max Length: 9 Range0: Min=a Max=z Range1: Min=A Max=Z Range2: Min=+ Max=:
P64=customize

#Self-Defined Time Zone
#String Max Length: 32 a-z, A-Z, +,:
P246=MTZ+6MDT+5,M3.2.0,M11.1.0

#Allow DHCP Option 2 to override time zone (If DHCP Option 2 is enabled, the timezone can be offset.)
#Number: 0, 1
#Mandatory
P143=1

################################################################################
#Maintenance-Syslog
################################################################################

# Syslog Protocol. 0 - UDP, 1 - SSL/TLS
# Number: 0, 1
# Mandatory
P8402=0

#Syslog Server (name of the server, max length is 64 charactors)
#String: serveraddress 
P207=

#Syslog Level (Default setting is NONE)
#0 - NONE, 1 - DEBUG, 2 - INFO, 3 - WARNING, 4 - ERROR
#Number: 0,1,2,3,4
#Mandatory
P208=0

#Send SIP Log (0 - No, 1 - Yes, Default set to No)
#Number: 0,1 
P1387=0

# SIP Log Option. 0 - Keep, 1 - Override
# Number: 0, 1
# Mandatory 
P8535=0

# Save Syslog. 0 - No, 1 - Yes. Default is No
# Number: 0, 1
# Mandatory
P28100=0


################################################################################
#Call Record
################################################################################

# CDR record Option. 0 - Keep, 1 - Override
# Number: 0, 1
# Mandatory 
P8534=0

################################################################################
#Advanced Settings-Ring Tones
################################################################################

#System Ring Cadence 
#Syntax: c=on1/ off1[- on2/ off2[- on3/ off3]](Cadence on and off are in 10 ms units)
#String Max Length: 256
P4040=c=2000/4000;

#Call Progress Tones
#Syntax: f1=val, f2=val[, c=on1/ off1[- on2/ off2[- on3/ off3]]](Frequencies are in Hz and cadence on and off are in 10 ms units) 

#Dial Tone
#String Max Length: 256 
P4000=f1=350@-13,f2=440@-13,c=0/0;

#Ringback Tone
#String Max Length: 256 
P4001=f1=440@-19,f2=480@-19,c=2000/4000;

#Busy Tone
#String Max Length: 256 
P4002=f1=480@-24,f2=620@-24,c=500/500;

#Reorder Tone
#String Max Length: 256 
P4003=f1=480@-24,f2=620@-24,c=250/250;

#Confirmation Tone
#String Max Length: 256 
P4004=f1=350@-11,f2=440@-11,c=100/100-100/100-100/100;

#Call Waiting tone
#String Max Length: 256 
P4005=f1=440@-13,c=300/10000-300/10000-0/0;

#Prompt Tone
#String Max Length: 256 
P4041=f1=350@-13,f2=440@-13,c=0/0;

# Conference Party Hangup Tone. 
# String Max Length: 256
# Mandatory
P28133=f1=425@-15,c=600/600;

################################################################################
#Advanced Settings-FXO Failover
################################################################################

#Failover to FXO Gateway. 0 - Disable, 1 - Enable
#Number: 0,1
#Mandatory
P4205=0

#FXO Gateway. URI or IP address.
#String: serveraddress 
P4206=

################################################################################
#Advanced Settings-System Features
################################################################################

#Disable Direct IP Call. 0 - No, 1 - Yes.
#Number: 0,1
#Mandatory
P277=0

# Inter-port Calling. 0 - Disabled, 1 - Enabled
# Number: 0, 1
# Mandatory
P28146=0

#Disable SIP NOTIFY Authentication
#Number: 0 No, 1 Yes  (Device will not challenge NOTIFY with 401 when set to Yes) 
#Mandatory
#P4428=0

#Disable voice prompt. 0 - No, 1 - Yes.
#Number: 0,1
#Mandatory
P253=0

#IVR Language. en - English, zh - Chinese, es- Spanish
#text: en, zh, es
#Mandatory 
P342=en

#LCD Display Language. en - English, zh - Chinese, fr - French, es - Spanish
#String
#Mandatory 
P1362=en

#Prompt Dial Tone Code(Key pattern to get Prompt Tone. Maximum 20 digits. No default.)
#String Max Length: 20 
P4042=

#Country Specific Deployment. 0 - None(default), zh - China, zh1 - China ITSP, gm - Germany, us - USA
#String
#Mandatory
P4898=0

#Automatic Reboot. 0 - No, 1 - Yes, reboot every day, 2 - Yes, reboot every week
#Number: 0,1,2
#Mandatory
P21929=0

#Hour of the Day(0-23) Defines the hour of the day to reboot the gateway. Will valid after configured Automatic Reboot to yes.
#Number: 0-23
#Mandatory
P21930=1

#Day of the Week (0-6) Defines the day of the week to reboot the gateway.
#Number: 0-6
#Mandatory
P21931=1

# LED Pattern. 0 - Pattern A, 1 - Pattern B, 2 - Pattern C
# Number: 0, 1, 2
# Mandatory
P4049=0

################################################################################
#Profile 1-General Settings
################################################################################

#Profile Active.  0 - no, 1 - yes
#Number: 0,1
#Mandatory
P271=1

#Primary SIP Server
#String: serveraddress 
P47=

#Failover SIP Server
#String: serveraddress 
P967=

#Prefer Primary SIP Server. 0 - No, 1 - Yes.
#Number: 0,1
#Mandatory
P4567=0

#Primary Outbound Proxy
#String: serveraddress 
P48=

# Backup Outbound Proxy.
# String: serveraddress
P2333=


# Prefer Primary Outbound Proxy. 0 - No, 1 - Yes
# Number: 0, 1
# Mandatory
P28096=0

################################################################################
#Profile 1-Network Settings
################################################################################

#Layer 3 QoS SIP Diff-Serv (default 24)
#Number
#Mandatory
P5046=24

#Layer 3 QoS RTP Diff-Serv (default 46)
#Number
#Mandatory
P5050=46

#DNS Mode. 0 - A Record, 1 - SRV, 2 - NAPTR/SRV, 3 - Use Configured IP .
#Number: 0,1,2,3
#Mandatory 
P103=0

#Primary IP
#IP address
P2308=

#Backup IP1
#IP address
P2309=

#Backup IP2
#IP address
P2310=

#NAT Traversal (STUN). 0 - No, 2 - No but send keep-alive, 1 - Yes
#Number: 0,1,2
#Mandatory
P52=0

#Use NAT IP.  This will enable our SIP client to use this IP in the SIP message. Example 64.3.153.50.
#String: ipaddress 
P101=

#Proxy-Require (A SIP extension to enable firewall penetration)
#String: ipaddress 
P197=

################################################################################
#Profile 1-SIP Settings
################################################################################

#Basic Settings#################################################################

#SIP Transport. 0 - UDP, 1 - TCP, 2 - TLS
#Number: 0,1,2
#Mandatory
P130=0

#SIP Registration. 0 - no, 1 - yes
#Number: 0,1
#Mandatory 
P31=1

#Unregister On Reboot. 0 - no, 1 - yes
#Number: 0,1
#Mandatory 
P81=0

#Add Auth Header On Initial REGISTER
#Number: 0,1
#Mandatory 
P2359=0

#Outgoing call without Registration. 0 - no, 1 - yes
#Number: 0,1
#Mandatory 
P109=1

#Register Expiration (in minutes. default 1 hour, max 45 days)
#Number: 1 to 64800
#Mandatory 
P32=60

#SIP Registration Failure Retry Wait Time (in seconds. Between 1-3600, default is 30)
#Number: 1 to 3600
#Mandatory 
P138=30

# SIP Registration Failure Retry Wait Time upon 403 Forbidden. 0 second means stop retry registration. Default is 1200 sec.
# Number 0 to 3600
# Mandatory
P26002=1200

#Reregister before Expiration
#Number
#Mandatory
P2330=0

# Enable SIP OPTIONS/NOTIFY Keep Alive. 0 - No, 1 - OPTIONS, 2 - NOTIFY
# Number: 0, 1, 2
# Mandatory
P2397 = 0 

# Enable SIP OPTIONS/NOTIFY Keep Alive Interval. In seconds. The default value is 30 seconds.
# Number: 1 - 64800
# Mandatory
P2398 = 30

# SIP OPTIONS/NOTIFY Keep Alive Max Lost. In packages. The default value is 3 packages.
# Number: 3 - 10
# Mandatory
P2399 = 3

#Local SIP port (default 5060)
#Number: 1 to 65535
#Mandatory 
P40=5060

#Use Random SIP Port 0 - no, 1 - yes
#Number: 0,1
#Mandatory 
P78=0

#Local RTP port (1024-65535, default 50000)
#Number: 1024 to 65535
#Mandatory
P39 = 50000

#SIP T1 Timeout. RFC 3261 T1 value.
#50 - 0.5 sec, 100 - 1 sec, 200 - 2 sec, 400 - 4 sec, 800 - 8 sec. Default 100.
#Number: 50,100,200,400,800
#Mandatory
P209=50

#SIP T2 Timeout. RFC 3261 T2 value.
#200 - 2 sec, 400 - 4 sec, 800 - 8 sec, 1600 - 16 sec, 3200 - 32 sec. Default 400.
#Number: 1600,3200,200,400,800
#Mandatory 
P250=400

#Remove OBP from Route Header. 0 - no, 1 - yes
#NUmber: 0,1
#Mandatory
P4562=0

#Support SIP Instance ID. 0 - no, 1 - yes
#Number: 0,1
#Mandatory
P288=1

# Hold Target Before Refer 0 - No, 1 - Yes
# Number: 0, 1
# Mandatory
P26003=1

#Refer-To Use Target Contact. 0 - no, 1 - yes
#Number: 0,1
#Mandatory 
P135=

#SUBSCRIBE for MWI. 0 - No, 1 - Yes.
#Number: 0,1
#Mandatory
P99=0

#Enable 100rel. 0 - No, 1 - Yes
#Number: 0 to 1
#Mandatory 
P272=0

#Tel URI. 0 - Disabled, 1 - User=Phone, 2 - Enabled
#Number: 0,1,2
#Mandatory 
P63=0

#Use Request Routing ID in SIP Headers, 0 - No, 1 - Yes
#Number: 0,1
#Mandatory 
P4891=0

#Do Not Escape '#' as %23 in SIP URI. 0 - No, 1 - Yes
#Number: 0, 1
#Mandatory
P1406= 0

#Disable Multiple m Line in SDP. 0 - No, 1 - Yes
P137= 0

#Use Privacy Header. 0 - Default, 1 - No, 2 - Yes
#Number: 0, 1, 2
#Mandatory
P2338= 0

#Use P-Preferred-Identity Header. 0 - Default, 1 - No, 2 - Yes
#Number: 0, 1, 2
#Mandatory
P2339= 0

#SIP REGISTER Contact Header Uses. 0 - LAN Address, 1 - WAN Address
#Number: 0, 1
#Mandatory
#P4437=0

# Caller ID Display. 0 - Auto, 1 - Disable, 2 - From Header
# Number: 0, 1, 2
# Mandatory
P2324=0

# Use Actual Ephemeral Port in Contact with TCP/TLS. 0 - No, 1 - Yes
# Number: 0, 1
# Mandatory
P2331 = 0

# SIP User-Agent
# String
P29071 = 

# SIP User-Agent Postfix
# String
P4834 = 

#Session Timer################################################################################

#Session Expiration (in seconds. default 180 seconds. Allowed value: 90-65535)
#Number: 90 to 64800
#Mandatory 
P260=180

#Minimum SE (in seconds. default 90 seconds, must be lower than or equal to P260)
#Number 90 to 64800
#Mandatory 
P261=90

#Caller Request Timer (Request for timer when calling) 0 - no, 1 - yes
#Number: 0,1
#Mandatory 
P262=0

#Callee Request Timer (Request for timer when called. i.e. if remote party supports timer but did not request for one) 0 - no, 1 - yes
#Number: 0,1
#Mandatory 
P263=0

#Force Timer (Still use timer when remote party does not support timer) 0 - no, 1 - yes
#Number: 0,1
#Mandatory 
P264=0

#UAC Specify Refresher. 0 - omit, 1 - UAC, 2 - UAS
#Number: 0,1,2
#Mandatory 
P266=0

#UAS Specify Refresher. 1 - UAC, 2 - UAS
#Number: 1,2
#Mandatory 
P267=1

#Force INVITE (Always refresh with INVITE instead of UPDATE even when remote party supports UPDATE) 0 - no, 1 - yes
#Number: 0,1
#Mandatory 
P265=0

#Security Settings################################################################################

#Validate Incoming Messages. 0 - No, 1 - Yes
#Number: 0,1
#Mandatory 
P4340=0

#Check SIP User ID for Incoming INVITE. 0 - No, 1 - Yes (no direct IP calling if Yes)
#Number: 0,1
#Mandatory 
P258=0 

#Allow Incoming SIP Messages from SIP Proxy Only
#Number: 0,1
#Mandatory 
P243=0

#Authenticate incoming INVITE 
#Number: 0,1
P2346=0

# Authenticate server certificate domain. 0 - No, 1 - Yes, default is 0
# Number: 0, 1
# Mandatory
P2311=0

# Authenticate server certificate chain. 0 - No, 1 - Yes, default is 0
# Number: 0, 1
# Mandatory
P2367=0

################################################################################
#Profile 1-Fax Settings
################################################################################

#FAX Mode. 0 - T.38 (Auto Detect), 1 - Pass Through
#Number: 0,1
#Mandatory 
P228=0

#Fax Tone Detection Mode. 1 - Caller, 0 - Callee, 2 - Caller or Callee
#Number: 0,1,2
#Mandatory 
P894=0

#Send Re-INVITE After Fax. 0 - No, 1 - Yes
#Number: 0,1
#Mandatory 
P4367=0

#Send Re-INVITE After Fax Tone. 0 - No, 1 - Yes
#Number: 0,1
#Mandatory 
P4416=1

#Enable Silence Detection for Fax Disconnect. 0 - No, 1 - Yes
#Number: 0 to 1
#Mandatory 
P4406=1

################################################################################
#Profile 1-Audio Settings
################################################################################

#Preferred DTMF Method 1 
#100 - In-audio, 101 - RFC2833, 102 - SIP INFO
#Priority 1
#Number: 100 to 102
#Mandatory
P850=100

#Preferred DTMF Method 2
#Number: 100 to 102
#Mandatory 
P851=100

#Preferred DTMF Method 3
#Number: 100 to 102
#Mandatory 
P852=100

#DTMF-RELAY Tag Respect SIP INFO. 0 - No, 1 - Yes (If set to "NO", the dtmf-relay tag in Accept Header is always added in outbound INVITE. If set to "YES", it depends on if SIP INFO is chosen in Prefered DTMF Method.)
#Number: 0, 1
#Mandatory
P28088=0

#Disable DTMF Negotiation. 0 - no, 1 - yes 
#Number: 0,1
#Mandatory
P4825=0

#Enable Fast RFC2833. 0 - No, 1 - Yes
#Number: 0,1
#Mandatory
P21917=0

#DTMF Payload Type
#Number: 96 to 127
P79=101

#Preferred Vocoder
#0 - PCMU, 8 - PCMA, 4 - G.723, 18 - G.729, 2 - G.726-32, 100 - AAL2-G.726-16,
#102 - AAL2-G.726-24, 104 - AAL2-G726-32, 103 - AAL2-G.726-40, 98 - iLBC, 9 - G.722(wide band)
#Choice 1. 
#Mandatory
P57=0

#Choice 2. 
#Mandatory
P58=8

#Choice 3. 
#Mandatory
P59=4

#Choice 4. 
#Mandatory 
P60=18

#Choice 5. 
#Mandatory
P61=2

#Choice 6. 
#Mandatory 
P62=98

#Choice 7. 
#Mandatory
P46=104

#Choice 8. 
#Mandatory
P98=100

#Voice Frame per TX. (Default 2, from 1 to 4 for G711/G726/G729)
#Number: 1 to 4
P37=2

#G723 rate. 0 - 6.3kbps encoding rate, 1 - 5.3kbps encoding rate
#Number: 0,1
#Mandatory 
P49=0

#G726-32 Packing Mode. 0 - ITU, 1 - IETF
#Number: 0,1
#Mandatory 
P2323=0

#iLBC Frame Size. 0 - 20ms(default), 1 - 30ms.
#Number: 0,1
#Mandatory 
P97=0

#iLBC payload type. Between 96 and 127, default is 97.
#Number: 96 to 127
#Mandatory 
P96=97

#AAL2-G.726-16 Payload type. (between 96 and 127, default is 100)
#Number: 96 to 127
#Mandatory 
P125=100

#AAL2-G.726-24 Payload type. (between 96 and 127, default is 99)
#Number: 96 to 127
#Mandatory 
P126=99

#AAL2-G726-32 payload type. (between 96 and 127, default is 104)
#Number: 96 to 127
#Mandatory 
P127=104

#AAL2-G.726-40 Payload type. (between 96 and 127, default is 103)
#Number: 96 to 127
#Mandatory 
P128=103

#Use First Matching Vocoder in 200OK SDP. 0 - No, 1 - Yes
#Number: 0,1
#Mandatory 
P4363=0

#SRTP Mode
#0=Disabled
#1=Enabled but not forced
#2=Enabled and forced
#Number: 0,1,2
#Mandatory
P183=0

# Crypto Life Time
# 0 = Disabled
# 1 = Enabled
# Number: 0, 1
# Mandatory
P2363=1

#Silence Suppression (VAD). 0 - No, 1 - Yes
#Number: 0,1
#Mandatory 
P50=0

#Jitter Buffer Type. 0 - Fixed, 1 - Adaptive
#Number: 0,1
#Mandatory
P133= 1

#Jitter Buffer Length. 0 - Low, 1 - Medium, 2 - High
#Number: 0,1,2
#Mandatory
P132=1

# RTCP. 0 - Disable, 1 - Enable
# Number: 0, 1
# Mandatory
P2392=1

#SLIC Setting
#0 - USA, 1 - AUSTRIA, 2 - BELGIUM, 3 - FINELAND, 4 - FRANCE, 5 - GERMANY
#6 - GREECE, 7 -ITALY, 8 - JAPAN, 9 - NORWAY, 10 - SPAIN, 11 - SWEDEN,
#12 - UK, 13 - AUSTRALIA/NEW ZEALAND, 14 - CHINA
#Number: 0 to 14
#Mandatory 
P854=0

# Ringing Frequency. 0 - Default, 1 - 20Hz, 2 - 25Hz
# Number: 0, 1, 2
# Mandatory
P4429 = 0

#Caller ID Scheme
#0  - Bellcore/Telcordia
#1  - ETSI-FSK during ringing
#2  - ETSI-FSK prior to ringing with DTAS
#3  - ETSI-FSK prior to ringing with LR
#4  - ETSI-FSK prior to ringing with RP
#5  - ETSI-DTMF during ringing
#6  - ETSI-DTMF prior to ringing with DTAS
#7  - ETSI-DTMF prior to ringing with LR
#8  - ETSI-DTMF prior to ringing with RP
#9  - SIN 227 - BT
#10 - NTT Japan
#Number: 0 to 10
#Mandatory 
P853=0

#Polarity Reversal.  0 - No, 1 - Yes
#Number: 0,1
#Mandatory 
P205=0

#Loop Current Disconnect. 0 - No, 1 - Yes
#Number: 0,1
#Mandatory 
P892=0

# Play busy/reorder tone before Loop Current Disconnect
# 0 = Disabled
# 1 = Enabled
# Number: 0, 1
# Mandatory
P21925=0

#Loop Current Disconnect Duration. In 100 - 10000 milliseconds range, default is 200.
#Number: 100 to 10000
#Mandatory 
P856=200

#Enable Hook Flash
#Number: 0, 1
#Mandatory
P4424=1

#Hook Flash Timing. In 40-2000 milliseconds range
#minimum
#Number: 40 to 2000
#Mandatory
P251=300
#maximum
#Number: 40 to 2000
#Mandatory 
P252=1100

#On Hook Timing. (In 40-2000 milliseconds range, default is 400)
#Number: 40 to 2000
#Mandatory 
P833=400

#Gain:
#TX 
#<value=1> +6dB
#<value=2> +4dB
#<value=3> +2dB
#<value=0> 0dB
#<value=4> -2dB
#<value=5> -4dB
#<value=6> -6dB
#Number: 0 to 6
#Mandatory 
P247=0 

#RX 
#<value=1> +6dB
#<value=2> +4dB
#<value=3> +2dB
#<value=0> 0dB
#<value=4> -2dB
#<value=5> -4dB
#<value=6> -6dB
#Number: 0 to 6
#Mandatory 
P249=0

#Disable Line Echo Canceller (LEC).  0 - No, 1 - Yes
#Number: 0,1
#Mandatory
P824=0

################################################################################
#Profile 1-Call Settings
################################################################################

#Early Dial. 0 - No, 1 - Yes (use "Yes" only if proxy supports 484 response). 0 - no, 1 - yes
#Number: 0,1
#Mandatory 
P29=0

#Dial Plan Prefix.(this prefix string is added to each dialed number)
#String Max Length: 32
P66=

#Dial Plan 
#String Max Length: 1024
P4200={ x+ | *x+ }

#Use #as Dial Key (if set to Yes, "#" will function as the "(Re-)Dial" key). 0 - no, 1 - yes
#Number: 0,1
#Mandatory 
P72=1

# Disable # as Redial Key. 0 - No, 1 - Yes
# Number: 0, 1
# Mandatory
P28147 = 0

#No Key Entry Timeout. Default - 4 seconds.
#Number: 1 to 15
#Mandatory
P85=4

#Offhook Auto-Dial Delay (default is 0)
#String: 0 to 60
P4045=0

# Allow Auto-Dial Config Per Port. 0 - Disable, 1 - Enable
# Number: 0, 1
# Mandatory
P28129=0

#Disable Call Waiting. 0 - no, 1 - yes
#Number: 0,1
#Mandatory 
P91=0

# RFC2543 Hold. 0 - No, 1 - Yes
# Number: 0, 1
# Mandatory
P26062=1

#Disable Call Waiting Caller ID. 0 - no, 1 - yes
#Number: 0,1
#Mandatory 
P714=0

#Disable Call Waiting Tone. 0 - no, 1 - yes
#Number: 0,1
#Mandatory 
P186=0

#Disable Connected Line ID. 0 = Disabled, 1 = Enabled (If yes, Connected Line ID will not be displayed even received.)
#Number: 0, 1
#Mandatory
P20525=0

#Disable Receiver Offhook Tone. 0 - No, 1 - Yes.
#Number: 0,1
#Mandatory 
P4793=0

#Disable Reminder Ring for On-Hold Call:
#Number: 0,1
#Mandatory 
P4360=0

# Disable Reminder Ring for DND. 0 - No, 1 - Yes
# Number: 0, 1
# Mandatory
P29072 = 0

# Disable Voicemail Reminder Tone. 0 - No, 1 - Yes
# Number: 0, 1
# Mandatory
P28151 = 0

#Disable Visual MWI. 0 - No, 1 - Yes
#Number: 0,1
#Mandatory 
P855=0

#Visual MWI type: 1 - FSK, 2 - Neon
#Number: 1,2
#Mandatory
P4371=1

#Transfer on Conference Hangup. 0 - no, 1 - yes
#Number: 0,1
#Mandatory 
P4560=0

#Send Hook Flash Event. 0 - no, 1 - yes 
#Number: 0 to 1
#Mandatory 
P74=0

#Flash Digit Control. 0 - No, 1 - Yes(Set Yes will overrides the default settings for call control when both channels are in use.) 
#Number: 0, 1
#Mandatory
P28080=0

# Callee Flash to 3WC. 0 - No, 1 - Yes
# Number: 0, 1
# Mandatory
P28169 = 0

#Ring Timeout. (0, 10-300, default is 60 seconds. When set to 0, the Ring Timeout feature is disabled)
#Number: 10 to 300
#Mandatory 
P185=60

#Delayed Call Forward Wait Time. Allowed range 1-120, in seconds. Default 20 seconds.
#Number: 1 to 120
#Mandatory
P139=20

#Send Anonymous. 0 - no, 1 - yes (caller ID will be blocked if set to Yes).
#Number: 0 to 1
#Mandatory 
P65=0

#Anonymous Call Rejection. 0 - No, 1 - Yes.
#Number: 0 to 1
#Mandatory 
P129=0

# Replace Beginning '+' with 00 in Caller ID. 0 - No, 1 - Yes
# Number: 0, 1
# Mandatory
P29073=0


#Hunting Group Type. 0 - Circular, 1 - Linear
#Number: 0,1
#Mandatory
P4395=0

#Hunting Group Ring Timeout. (5-300, default is 20 seconds)
#Number: 5 to 300
#Mandatory 
P4330=20

#Special Feature
#100 - Standard, 102 - BroadSoft, 108 - CBCOM, 109 - RNK, 111 - Huawei, 114 - ZTE IMS, 119 - PhonePower, 120 - TELKOM SA.
#Number: 100, 102, 108, 109, 111, 114, 119, 120
#Mandatory 
P198=100

################################################################################
#Profile 1-Call Features Settings
################################################################################

#Enable Call Features. 0 - No, 1 - Yes, 2 - Enable All
P191=1

# Reset Call Features. 0 - No, 1 - Yes
# Number: 0, 1
# Mandatory
P24199=0

#SRTP Feature.
#First value - Enable/Disable feature, Mandatory 0 - No, 1 - Yes
#Second value - Enable feature code numbers
#Third value - Disable feature code numbers
P24060=1
P24001=16
P24002=17

#SRTP per call Feature.
#First value - Enable/Disable feature, Mandatory 0 - No, 1 - Yes
#Second value - Enable feature code numbers
#Third value - Disable feature code numbers
P24061=1
P24003=18
P24004=19

#CID Feature.
#First value - Enable/Disable feature, Mandatory 0 - No, 1 - Yes
#Second value - Enable feature code numbers
#Third value - Disable feature code numbers
P24062=1
P24005=31
P24006=30

#CID per call Feature.
#First value - Enable/Disable feature, Mandatory 0 - No, 1 - Yes
#Second value - Enable feature code numbers
#Third value - Disable feature code numbers
P24065=1
P24019=82
P24010=67

#Direct IP calling Feature.
#First value - Enable/Disable feature, Mandatory 0 - No, 1 - Yes
#Second value - Code numbers
P24063=1
P24007=47

#CW Feature. 
#First value - Enable/Disable feature, Mandatory 0 - No, 1 - Yes
#Second value - Enable feature code numbers
#Third value - Disable feature code numbers
P24064=1
P24009=51
P24008=50

#CW per call Feature. 
#First value - Enable/Disable feature, Mandatory 0 - No, 1 - Yes
#Second value - Enable feature code numbers
#Third value - Disable feature code numbers
P24067=1
P24013=71
P24012=70

#Call return Feature.
#First value - Enable/Disable feature, Mandatory 0 - No, 1 - Yes
#Second value - Code numbers
P24066=1
P24011=69

#Unconditional forward Feature.
#First value - Enable/Disable feature, Mandatory 0 - No, 1 - Yes
#Second value - Enable feature code numbers
#Third value - Disable feature code numbers
P24068=1
P24014=72
P24015=73

#Busy forward Feature.
#First value - Enable/Disable feature, Mandatory 0 - No, 1 - Yes
#Second value - Enable feature code numbers
#Third value - Disable feature code numbers
P24072=1
P24021=90
P24022=91

#Delayed forward Feature.
#First value - Enable/Disable feature, Mandatory 0 - No, 1 - Yes
#Second value - Enable feature code numbers
#Third value - Disable feature code numbers
P24073=1
P24023=92
P24024=93

#Paging Feature.
#First value - Enable/Disable feature, Mandatory 0 - No, 1 - Yes
#Second value - Code numbers
P24069=1
P24016=74

#DND Feature.
#First value - Enable/Disable feature, Mandatory 0 - No, 1 - Yes
#Second value - Enable feature code numbers
#Third value - Disable feature code numbers
P24070=1
P24017=78
P24018=79

#Blind Transfer Feature.
#First value - Enable/Disable feature, Mandatory 0 - No, 1 - Yes
#Second value - Code numbers
P24071=1
P24020=87

#Disable LEC per call Feature.
#First value - Enable/Disable feature, Mandatory 0 - No, 1 - Yes
#Second value - Code numbers
P24074=1
P24025=03

#Disable Bellcore-style 3-Way Conference. 0 - No, 1 - Yes
P4830=0
#Star Code 3WC Feature. 0 - No, 1 - Yes
P24075=1
#Star Code 3WC
P24026=23

#Provision start Feature.
#First value - Enable/Disable feature, Mandatory 0 - No, 1 - Yes
#Second value - Code numbers
P24086=1
P24037=99

#Play registration id Feature.
#First value - Enable/Disable feature, Mandatory 0 - No, 1 - Yes
#Second value - Code numbers
P24087=1
P24038=98

#Forced Codec Feature. 
#First value - Enable/Disable feature, Mandatory 0 - No, 1 - Yes
#Second value - Code numbers
P24059=1
P24000=02

#PCMU codec feature. 
#First value - Enable/Disable feature, Mandatory 0 - No, 1 - Yes
#Second value - Code numbers
P24076=1
P24027=7110

#PCMA codec feature
#First value - Enable/Disable feature, Mandatory 0 - No, 1 - Yes
#Second value - Code numbers
P24077=1
P24028=7111

#G723 codec feature
#First value - Enable/Disable feature, Mandatory 0 - No, 1 - Yes
#Second value - Code numbers
P24078=1
P24029=723

#G729 codec feature
#First value - Enable/Disable feature, Mandatory 0 - No, 1 - Yes
#Second value - Code numbers
P24079=1
P24030=729

#AAL2-G726-R16 codec 
#First value - Enable/Disable feature, Mandatory 0 - No, 1 - Yes
#Second value - Code numbers
P24080=1
P24031=72616

#AAL2-G726-R24 codec feature
#First value - Enable/Disable feature, Mandatory 0 - No, 1 - Yes
#Second value - Code numbers
P24081=1
P24032=72624

#AAL2-G726-R32 codec feature
#First value - Enable/Disable feature, Mandatory 0 - No, 1 - Yes
#Second value - Code numbers
P24082=1
P24033=72632

#AAL2-G726-R40 codec 
#First value - Enable/Disable feature, Mandatory 0 - No, 1 - Yes
#Second value - Code numbers
P24083=1
P24034=72640

#iLBC codec feature
#First value - Enable/Disable feature, Mandatory 0 - No, 1 - Yes
#Second value - Code numbers
P24084=1
P24035=7201

#G722 codec feature
#First value - Enable/Disable feature, Mandatory 0 - No, 1 - Yes
#Second value - Code numbers
P24085=1
P24036=722

################################################################################
#Profile 1-Ring Tones
################################################################################

#Distinctive Ring Tones#########################################################

#Distinctive Ring Tone 
#0 - Ring Tone 1, 1 - Ring Tone 2, 2 - Ring Tone 3, 3 - Ring Tone 4, 4 - Ring Tone 5, 
#5 - Ring Tone 6, 6 - Ring Tone 7, 7 - Ring Tone 8, 8 - Ring Tone 9, 9 - Ring Tone 10
#Distinctive Ring Tone 1
#Number: 0 to 9
#Mandatory
P870=0

#Choice 1 incoming caller ID
#String Max Length: 64
P871=

#Distinctive Ring Tone 2
#Number: 0 to 9
#Mandatory
P872=0

#Choice 2 incoming caller ID
#String Max Length: 64 
P873=

#Distinctive Ring Tone 3
#Number: 0 to 9
#Mandatory 
P874=0

#Choice 3 incoming caller ID
#String Max Length: 64
P875=

#Ring Tone Cadences################################################################################
#Syntax: c=on1/ off1[- on2/ off2[- on3/ off3]];(Cadence on and off are in 10 ms units)

#Ring Tone 1
#String Max Length: 256
P4010=c=2000/4000;

#Ring Tone 2
#String Max Length: 256 
P4011=c=2000/4000;

#Ring Tone 3
#String Max Length: 256 
P4012=c=2000/4000; 

#Ring Tone 4
#String Max Length: 256 
P4013=c=2000/4000;

#Ring Tone 5
#String Max Length: 256
P4014=c=2000/4000;

#Ring Tone 6
#String Max Length: 256 
P4015=c=2000/4000;

#Ring Tone 7
#String Max Length: 256
P4016=c=2000/4000;

#Ring Tone 8
#String Max Length: 256 
P4017=c=2000/4000;

#Ring Tone 9
#String Max Length: 256 
P4018=c=2000/4000; 

#Ring Tone 10
#String Max Length: 256 
P4019=c=2000/4000;


################################################################################
#Profile 1- Call Waiting Tones
################################################################################

# Distinctive Call Waiting Tones#########################################################

# Distinctive Call Waiting Tone 1
# Number: 0-9
# Mandatory
P29074=0 

# Distinctive Call Waiting Tone 2
# Number: 0-9
# Mandatory
P29075=0 

# Distinctive Call Waiting Tone 3
# Number: 0-9
# Mandatory
P29076=0

# Distinctive Call Waiting Tone CID matching plan for Tone 1
# Max Length: 64
P29077= 

# Distinctive Call Waiting Tone CID matching plan for Tone 2
# Max Length: 64
P29078= 

# Distinctive Call Waiting Tone CID matching plan for Tone 3
# Max Length: 64
P29079= 

# Call Waiting Tone Cadences#################################
# Syntax: f1=val, f2=val[, c=on1/ off1[- on2/ off2[- on3/ off3]]]; (Frequencies are in Hz and cadence on and off are in 1 ms units)
# Call Waiting Tone 1 - Call Waiting Tone 10
# Mandatory
P29080 = f1=440@-13,c=300/10000-300/10000-0/0;
P29081 = f1=440@-13,c=300/10000-300/10000-0/0;
P29082 = f1=440@-13,c=300/10000-300/10000-0/0;
P29083 = f1=440@-13,c=300/10000-300/10000-0/0;
P29084 = f1=440@-13,c=300/10000-300/10000-0/0;
P29085 = f1=440@-13,c=300/10000-300/10000-0/0;
P29086 = f1=440@-13,c=300/10000-300/10000-0/0;
P29087 = f1=440@-13,c=300/10000-300/10000-0/0;
P29088 = f1=440@-13,c=300/10000-300/10000-0/0;
P29089 = f1=440@-13,c=300/10000-300/10000-0/0;


################################################################################
#Profile 2-General Settings
################################################################################

#Profile Active.  0 - no, 1 - yes
#Number: 0,1
#Mandatory
P401=1

#Primary SIP Server
#String: serveraddress 
P747=sip.mycompany.com

#Failover SIP Server
#String: serveraddress 
P987=

#Prefer Primary SIP Server. 0 - No, 1 - Yes.
#Number: 0,1
#Mandatory
P4568=0

#Outbound Proxy
#String: serveraddress 
P748=proxy.mycompany.com

# Backup Outbound Proxy.
# String: serveraddress
P2433=

# Prefer Primary Outbound Proxy. 0 - No, 1 - Yes
# Number: 0, 1
# Mandatory
P28097=0

################################################################################
#Profile 2-Network Settings
################################################################################

#Layer 3 QoS SIP Diff-Serv (default 24)
#Number
#Mandatory
P5047=24

#Layer 3 QoS RTP Diff-Serv (default 46)
#Number
#Mandatory
P5051=46

#DNS Mode. 0 - A Record, 1 - SRV, 2 - NAPTR/SRV, 3 - Use Configured IP .
#Number: 0,1,2,3
#Mandatory 
P702=0

#Primary IP
#IP address
P2408=

#Backup IP1
#IP address
P2409=

#Backup IP2
#IP address
P2410=

#NAT Traversal (STUN). 0 - No, 2 - No but send keep-alive, 1 - Yes
#Number: 0,1,2
#Mandatory
P730=0

#Use NAT IP.  This will enable our SIP client to use this IP in the SIP message. Example 64.3.153.50.
#String: ipaddress 
P866=

#Proxy-Require (A SIP extension to enable firewall penetration)
#String: ipaddress 
P792=

################################################################################
#Profile 2-SIP Settings
################################################################################

#Basic Settings#################################################################

#SIP Transport. 0 - UDP, 1 - TCP, 2 - TLS
#Number: 0,1,2
#Mandatory
P830=0

#SIP Registration. 0 - no, 1 - yes
#Number: 0,1
#Mandatory 
P731=1

#Unregister On Reboot. 0 - no, 1 - yes
#Number: 0,1
#Mandatory 
P752=0

#Add Auth Header On Initial REGISTER
#Number: 0,1
#Mandatory 
P2459=0

#Outgoing call without Registration. 0 - no, 1 - yes
#Number: 0,1
#Mandatory 
P813=1

#Register Expiration (in minutes. default 1 hour, max 45 days)
#Number: 1 to 64800
#Mandatory 
P732=60

#SIP Registration Failure Retry Wait Time (in seconds. Between 1-3600, default is 30)
#Number: 1 to 3600
#Mandatory 
P471=30

# SIP Registration Failure Retry Wait Time upon 403 Forbidden. 0 second means stop retry registration. Default is 1200 sec.
# Number 0 to 3600
# Mandatory
P26102=1200

#Reregister before Expiration
#Number
#Mandatory
P2430=0

# Enable SIP OPTIONS/NOTIFY Keep Alive. 0 - No, 1 - OPTIONS, 2 - NOTIFY
# Number: 0, 1, 2
# Mandatory
P2497 = 0

# Enable SIP OPTIONS/NOTIFY Keep Alive Interval. In seconds. The default value is 30 seconds.
# Number: 1 - 64800
# Mandatory
P2498 = 30

# SIP OPTIONS/NOTIFY Keep Alive Max Lost. In packages. The default value is 3 packages.
# Number: 3 - 10
# Mandatory
P2499 = 3

#Local SIP port (default 6060)
#Number: 1 to 65535
#Mandatory 
P740=6060

#Use Random SIP Port 0 - no, 1 - yes
#Number: 0,1
#Mandatory 
P778=0

#Local RTP port (1024-65535, default 51000)
#Number: 1024 to 65535
#Mandatory
P739 = 51000

#SIP T1 Timeout. RFC 3261 T1 value.
#50 - 0.5 sec, 100 - 1 sec, 200 - 2 sec, 400 - 4 sec, 800 - 8 sec. Default 100.
#Number: 50,100,200,400,800
#Mandatory
P440=50

#SIP T2 Timeout. RFC 3261 T2 value.
#200 - 2 sec, 400 - 4 sec, 800 - 8 sec, 1600 - 16 sec, 3200 - 32 sec. Default 400.
#Number: 1600,3200,200,400,800
#Mandatory 
P441=400

#Remove OBP from Route Header. 0 - no, 1 - yes
#NUmber: 0,1
#Mandatory
P4563=0

#Support SIP Instance ID. 0 - no, 1 - yes
#Number: 0,1
#Mandatory
P489=1

# Hold Target Before Refer 0 - No, 1 - Yes
# Number: 0, 1
# Mandatory
P26103=1

#Refer-To Use Target Contact. 0 - no, 1 - yes
#Number: 0,1
#Mandatory 
P469=

#SUBSCRIBE for MWI. 0 - No, 1 - Yes.
#Number: 0,1
#Mandatory
P709=0

#Enable 100rel. 0 - No, 1 - Yes
#Number: 0 to 1
#Mandatory 
P435=0

#Tel URI. 0 - Disabled, 1 - User=Phone, 2 - Enabled
#Number: 0,1,2
#Mandatory 
P763=0

#Use Request Routing ID in SIP Headers, 0 - No, 1 - Yes
#Number: 0,1
#Mandatory 
P4892=0

#Do Not Escape '#' as %23 in SIP URI. 0 - No, 1 - Yes
#Number: 0, 1
#Mandatory
P4895= 0

#Disable Multiple m Line in SDP. 0 - No, 1 - Yes
P487= 0

#Use Privacy Header. 0 - Default, 1 - No, 2 - Yes
#Number: 0, 1, 2
#Mandatory
P2438= 0

#Use P-Preferred-Identity Header. 0 - Default, 1 - No, 2 - Yes
#Number: 0, 1, 2
#Mandatory
P2439= 0

#SIP REGISTER Contact Header Uses. 0 - LAN Address, 1 - WAN Address
#Number: 0, 1
#Mandatory
#P4438=0

# Caller ID Display. 0 - Auto, 1 - Disable, 2 - From Header
# Number: 0, 1, 2
# Mandatory
P2424=0

# Use Actual Ephemeral Port in Contact with TCP/TLS. 0 - No, 1 - Yes
# Number: 0, 1
# Mandatory
P2431 = 0

# SIP User-Agent
# String
P29171 = 

# SIP User-Agent Postfix
# String
P4835 = 

#Session Timer################################################################################

#Session Expiration (in seconds. default 180 seconds. Allowed value: 90-65535)
#Number: 90 to 64800
#Mandatory 
P434=180

#Minimum SE (in seconds. default 90 seconds, must be lower than or equal to P260)
#Number 90 to 64800
#Mandatory 
P427=90

#Caller Request Timer (Request for timer when calling) 0 - no, 1 - yes
#Number: 0,1
#Mandatory 
P428=0

#Callee Request Timer (Request for timer when called. i.e. if remote party supports timer but did not request for one) 0 - no, 1 - yes
#Number: 0,1
#Mandatory 
P429=0

#Force Timer (Still use timer when remote party does not support timer) 0 - no, 1 - yes
#Number: 0,1
#Mandatory 
P430=0

#UAC Specify Refresher. 0 - omit, 1 - UAC, 2 - UAS
#Number: 0,1,2
#Mandatory 
P432=0

#UAS Specify Refresher. 1 - UAC, 2 - UAS
#Number: 1,2
#Mandatory 
P433=1

#Force INVITE (Always refresh with INVITE instead of UPDATE even when remote party supports UPDATE) 0 - no, 1 - yes
#Number: 0,1
#Mandatory 
P431=0

#Security Settings################################################################################

#Validate Incoming Messages. 0 - No, 1 - Yes
#Number: 0,1
#Mandatory 
P4341=0

#Check SIP User ID for Incoming INVITE. 0 - No, 1 - Yes (no direct IP calling if Yes)
#Number: 0,1
#Mandatory 
P449=0 

#Allow Incoming SIP Messages from SIP Proxy Only
#Number: 0,1
#Mandatory 
P743=0

#Authenticate incoming INVITE 
#Number: 0,1
P2446=0

# Authenticate server certificate domain. 0 - No, 1 - Yes, default is 0
# Number: 0, 1
# Mandatory
P2411=0

# Authenticate server certificate chain. 0 - No, 1 - Yes, default is 0
# Number: 0, 1
# Mandatory
P2467=0

################################################################################
#Profile 2-Fax Settings
################################################################################

#FAX Mode. 0 - T.38 (Auto Detect), 1 - Pass Through
#Number: 0,1
#Mandatory 
P710=0

#Fax Tone Detection Mode. 1 - Caller, 0 - Callee, 2 - Caller or Callee
#Number: 0,1,2
#Mandatory 
P895=0

#Send Re-INVITE After Fax. 0 - No, 1 - Yes
#Number: 0,1
#Mandatory 
P4368=0

#Send Re-INVITE After Fax Tone. 0 - No, 1 - Yes
#Number: 0,1
#Mandatory 
P4417=1

#Enable Silence Detection for Fax Disconnect. 0 - No, 1 - Yes
#Number: 0 to 1
#Mandatory 
P4407=1

################################################################################
#Profile 2-Audio Settings
################################################################################

#Preferred DTMF Method 1 
#100 - In-audio, 101 - RFC2833, 102 - SIP INFO
#Priority 1
#Number: 100 to 102
#Mandatory
P860=100

#Preferred DTMF Method 2
#Number: 100 to 102
#Mandatory 
P861=100

#Preferred DTMF Method 3
#Number: 100 to 102
#Mandatory 
P862=100

#DTMF-RELAY Tag Respect SIP INFO. 0 - No, 1 - Yes (If set to "NO", the dtmf-relay tag in Accept Header is always added in outbound INVITE. If set to "YES", it depends on if SIP INFO is chosen in Prefered DTMF Method.)
#Number: 0, 1
#Mandatory
P28089=0

#Disable DTMF Negotiation. 0 - no, 1 - yes 
#Number: 0,1
#Mandatory
P4826=0

#Enable Fast RFC2833. 0 - No, 1 - Yes
#Number: 0,1
#Mandatory
P21918=0

#DTMF Payload Type
#Number: 96 to 127
P779=101

#Preferred Vocoder
#0 - PCMU, 8 - PCMA, 4 - G.723, 18 - G.729, 2 - G.726-32, 100 - AAL2-G.726-16,
#102 - AAL2-G.726-24, 104 - AAL2-G726-32, 103 - AAL2-G.726-40, 98 - iLBC, 9 - G.722(wide band)
#Choice 1. 
#Mandatory
P757=0

#Choice 2. 
#Mandatory
P758=8

#Choice 3. 
#Mandatory
P759=4

#Choice 4. 
#Mandatory 
P760=18

#Choice 5. 
#Mandatory
P761=2

#Choice 6. 
#Mandatory 
P762=98

#Choice 7. 
#Mandatory
P814=104

#Choice 8. 
#Mandatory
P815=100

#Voice Frame per TX. (Default 2, from 1 to 4 for G711/G726/G729)
#Number: 1 to 4
P737=2

#G723 rate. 0 - 6.3kbps encoding rate, 1 - 5.3kbps encoding rate
#Number: 0,1
#Mandatory 
P749=0

#G726-32 Packing Mode. 0 - ITU, 1 - IETF
#Number: 0,1
#Mandatory 
P2423=0

#iLBC Frame Size. 0 - 20ms(default), 1 - 30ms.
#Number: 0,1
#Mandatory 
P705=0

#iLBC payload type. Between 96 and 127, default is 97.
#Number: 96 to 127
#Mandatory 
P704=97

#AAL2-G.726-16 Payload type. (between 96 and 127, default is 100)
#Number: 96 to 127
#Mandatory 
P819=100

#AAL2-G.726-24 Payload type. (between 96 and 127, default is 99)
#Number: 96 to 127
#Mandatory 
P820=99

#AAL2-G726-32 payload type. (between 96 and 127, default is 104)
#Number: 96 to 127
#Mandatory 
P821=104

#AAL2-G.726-40 Payload type. (between 96 and 127, default is 103)
#Number: 96 to 127
#Mandatory 
P822=103

#Use First Matching Vocoder in 200OK SDP. 0 - No, 1 - Yes
#Number: 0,1
#Mandatory 
P4364=0

#SRTP Mode
#0=Disabled
#1=Enabled but not forced
#2=Enabled and forced
#Number: 0,1,2
#Mandatory
P443=0

# Crypto Life Time
# 0 = Disabled
# 1 = Enabled
# Number: 0, 1
# Mandatory
P2463=1

#Silence Suppression (VAD). 0 - No, 1 - Yes
#Number: 0,1
#Mandatory 
P750=0

#Jitter Buffer Type. 0 - Fixed, 1 - Adaptive
#Number: 0,1
#Mandatory
P831= 1

#Jitter Buffer Length. 0 - Low, 1 - Medium, 2 - High
#Number: 0,1,2
#Mandatory
P832=1

# RTCP. 0 - Disable, 1 - Enable
# Number: 0, 1
# Mandatory
P2492=1

#SLIC Setting
#0 - USA, 1 - AUSTRIA, 2 - BELGIUM, 3 - FINELAND, 4 - FRANCE, 5 - GERMANY
#6 - GREECE, 7 -ITALY, 8 - JAPAN, 9 - NORWAY, 10 - SPAIN, 11 - SWEDEN,
#12 - UK, 13 - AUSTRALIA/NEW ZEALAND, 14 - CHINA
#Number: 0 to 14
#Mandatory 
P864=0

# Ringing Frequency. 0 - Default, 1 - 20Hz, 2 - 25Hz
# Number: 0, 1, 2
# Mandatory
P4430 = 0

#Caller ID Scheme
#0  - Bellcore/Telcordia
#1  - ETSI-FSK during ringing
#2  - ETSI-FSK prior to ringing with DTAS
#3  - ETSI-FSK prior to ringing with LR
#4  - ETSI-FSK prior to ringing with RP
#5  - ETSI-DTMF during ringing
#6  - ETSI-DTMF prior to ringing with DTAS
#7  - ETSI-DTMF prior to ringing with LR
#8  - ETSI-DTMF prior to ringing with RP
#9  - SIN 227 - BT
#10 - NTT Japan
#Number: 0 to 10
#Mandatory 
P863=0

#Polarity Reversal.  0 - No, 1 - Yes
#Number: 0,1
#Mandatory 
P865=0

#Loop Current Disconnect. 0 - No, 1 - Yes
#Number: 0,1
#Mandatory 
P893=0

# Play busy/reorder tone before Loop Current Disconnect
# 0 = Disabled
# 1 = Enabled
# Number: 0, 1
# Mandatory
P21926=0

#Loop Current Disconnect Duration. In 100 - 10000 milliseconds range, default is 200.
#Number: 100 to 10000
#Mandatory 
P857=200

#Enable Hook Flash
#Number: 0, 1
#Mandatory
P4425=1

#Hook Flash Timing. In 40-2000 milliseconds range
#minimum
#Number: 40 to 2000
#Mandatory
P811=300
#maximum
#Number: 40 to 2000
#Mandatory 
P812=1100

#On Hook Timing. (In 40-2000 milliseconds range, default is 400)
#Number: 40 to 2000
#Mandatory 
P834=400

#Gain:
#TX 
#<value=1> +6dB
#<value=2> +4dB
#<value=3> +2dB
#<value=0> 0dB
#<value=4> -2dB
#<value=5> -4dB
#<value=6> -6dB
#Number: 0 to 6
#Mandatory 
P248=0 

#RX 
#<value=1> +6dB
#<value=2> +4dB
#<value=3> +2dB
#<value=0> 0dB
#<value=4> -2dB
#<value=5> -4dB
#<value=6> -6dB
#Number: 0 to 6
#Mandatory 
P283=0

#Disable Line Echo Canceller (LEC).  0 - No, 1 - Yes
#Number: 0,1
#Mandatory
P825=0

################################################################################
#Profile 2-Call Settings
################################################################################

#Early Dial. 0 - No, 1 - Yes (use "Yes" only if proxy supports 484 response). 0 - no, 1 - yes
#Number: 0,1
#Mandatory 
P729=0

#Dial Plan Prefix.(this prefix string is added to each dialed number)
#String Max Length: 32
P766=

#Dial Plan 
#String Max Length: 1024
P4201={ x+ | *x+ }

#Use #as Dial Key (if set to Yes, "#" will function as the "(Re-)Dial" key). 0 - no, 1 - yes
#Number: 0,1
#Mandatory 
P772=1

# Disable # as Redial Key. 0 - No, 1 - Yes
# Number: 0, 1
# Mandatory
P28148 = 0

#No Key Entry Timeout. Default - 4 seconds.
#Number: 1 to 15
#Mandatory
P292=4

#Offhook Auto-Dial Delay (default is 0)
#String: 0 to 60
P4046=0

# Allow Auto-Dial Config Per Port. 0 - Disable, 1 - Enable
# Number: 0, 1
# Mandatory
P28130=0

# RFC2543 Hold. 0 - No, 1 - Yes
# Number: 0, 1
# Mandatory
P26162=1 

#Disable Call Waiting. 0 - no, 1 - yes
#Number: 0,1
#Mandatory 
P791=0

#Disable Call Waiting Caller ID. 0 - no, 1 - yes
#Number: 0,1
#Mandatory 
P823=0

#Disable Call Waiting Tone. 0 - no, 1 - yes
#Number: 0,1
#Mandatory 
P817=0

#Disable Connected Line ID. 0 = Disabled, 1 = Enabled (If yes, Connected Line ID will not be displayed even received.)
#Number: 0, 1
#Mandatory
P20526=0

#Disable Receiver Offhook Tone. 0 - No, 1 - Yes.
#Number: 0,1
#Mandatory 
P4794=0

#Disable Reminder Ring for On-Hold Call:
#Number: 0,1
#Mandatory 
P4361=0

# Disable Reminder Ring for DND. 0 - No, 1 - Yes
# Number: 0, 1
# Mandatory
P29172 = 0

# Disable Voicemail Reminder Tone. 0 - No, 1 - Yes
# Number: 0, 1
# Mandatory
P28143 = 0

#Disable Visual MWI. 0 - No, 1 - Yes
#Number: 0,1
#Mandatory 
P869=0

#Visual MWI type: 1 - FSK, 2 - Neon
#Number: 1,2
#Mandatory
P4372=1

#Transfer on Conference Hangup. 0 - no, 1 - yes
#Number: 0,1
#Mandatory 
P4561=0

#Send Hook Flash Event. 0 - no, 1 - yes 
#Number: 0 to 1
#Mandatory 
P774=0

#Flash Digit Control. 0 - No, 1 - Yes(Set Yes will overrides the default settings for call control when both channels are in use.) 
#Number: 0, 1
#Mandatory
P28081=0

# Callee Flash to 3WC. 0 - No, 1 - Yes
# Number: 0, 1
# Mandatory
P28170 = 0 

#Ring Timeout. (0, 10-300, default is 60 seconds. When set to 0, the Ring Timeout feature is disabled)
#Number: 10 to 300
#Mandatory 
P816=60

#Delayed Call Forward Wait Time. Allowed range 1-120, in seconds. Default 20 seconds.
#Number: 1 to 120
#Mandatory
P470=20

#Send Anonymous. 0 - no, 1 - yes (caller ID will be blocked if set to Yes).
#Number: 0 to 1
#Mandatory 
P765=0

#Anonymous Call Rejection. 0 - No, 1 - Yes.
#Number: 0 to 1
#Mandatory 
P446=0

# Replace Beginning '+' with 00 in Caller ID. 0 - No, 1 - Yes
# Number: 0, 1
# Mandatory
P29173=0


#Hunting Group Type. 0 - Circular, 1 - Linear
#Number: 0,1
#Mandatory
P4396=0

#Hunting Group Ring Timeout. (5-300, default is 20 seconds)
#Number: 5 to 300
#Mandatory 
P4331=20

#Special Feature
#100 - Standard, 102 - BroadSoft, 108 - CBCOM, 109 - RNK, 111 - Huawei, 114 - ZTE IMS, 119 - PhonePower, 120 - TELKOM SA.
#Number: 100, 102, 108, 109, 111, 114, 119, 120
#Mandatory 
P767=100

################################################################################
#Profile 2-Call Features Settings
################################################################################

#Enable Call Features. 0 - No, 1 - Yes, 2 - Enable All
P751=1

# Reset Call Features. 0 - No, 1 - Yes
# Number: 0, 1
# Mandatory
P24399=0 

#SRTP Feature.
#First value - Enable/Disable feature, Mandatory 0 - No, 1 - Yes
#Second value - Enable feature code numbers
#Third value - Disable feature code numbers
P24260=1
P24201=16
P24202=17

#SRTP per call Feature.
#First value - Enable/Disable feature, Mandatory 0 - No, 1 - Yes
#Second value - Enable feature code numbers
#Third value - Disable feature code numbers
P24261=1
P24203=18
P24204=19

#CID Feature.
#First value - Enable/Disable feature, Mandatory 0 - No, 1 - Yes
#Second value - Enable feature code numbers
#Third value - Disable feature code numbers
P24262=1
P24205=31
P24206=30

#CID per call Feature.
#First value - Enable/Disable feature, Mandatory 0 - No, 1 - Yes
#Second value - Enable feature code numbers
#Third value - Disable feature code numbers
P24265=1
P24219=82
P24210=67

#Direct IP calling Feature.
#First value - Enable/Disable feature, Mandatory 0 - No, 1 - Yes
#Second value - Code numbers
P24263=1
P24207=47

#CW Feature. 
#First value - Enable/Disable feature, Mandatory 0 - No, 1 - Yes
#Second value - Enable feature code numbers
#Third value - Disable feature code numbers
P24264=1
P24209=51
P24208=50

#CW per call Feature. 
#First value - Enable/Disable feature, Mandatory 0 - No, 1 - Yes
#Second value - Enable feature code numbers
#Third value - Disable feature code numbers
P24267=1
P24213=71
P24212=70

#Call return Feature.
#First value - Enable/Disable feature, Mandatory 0 - No, 1 - Yes
#Second value - Code numbers
P24266=1
P24211=69

#Unconditional forward Feature.
#First value - Enable/Disable feature, Mandatory 0 - No, 1 - Yes
#Second value - Enable feature code numbers
#Third value - Disable feature code numbers
P24268=1
P24214=72
P24215=73

#Busy forward Feature.
#First value - Enable/Disable feature, Mandatory 0 - No, 1 - Yes
#Second value - Enable feature code numbers
#Third value - Disable feature code numbers
P24272=1
P24221=90
P24222=91

#Delayed forward Feature.
#First value - Enable/Disable feature, Mandatory 0 - No, 1 - Yes
#Second value - Enable feature code numbers
#Third value - Disable feature code numbers
P24273=1
P24223=92
P24224=93

#Paging Feature.
#First value - Enable/Disable feature, Mandatory 0 - No, 1 - Yes
#Second value - Code numbers
P24269=1
P24216=74

#DND Feature.
#First value - Enable/Disable feature, Mandatory 0 - No, 1 - Yes
#Second value - Enable feature code numbers
#Third value - Disable feature code numbers
P24270=1
P24217=78
P24218=79

#Blind Transfer Feature.
#First value - Enable/Disable feature, Mandatory 0 - No, 1 - Yes
#Second value - Code numbers
P24271=1
P24220=87

#Disable LEC per call Feature.
#First value - Enable/Disable feature, Mandatory 0 - No, 1 - Yes
#Second value - Code numbers
P24274=1
P24225=03

#Disable Bellcore-style 3-Way Conference. 0 - No, 1 - Yes
P4831=0
#Star Code 3WC Feature. 0 - No, 1 - Yes
P24275=1
#Star Code 3WC
P24226=23

#Provision start Feature.
#First value - Enable/Disable feature, Mandatory 0 - No, 1 - Yes
#Second value - Code numbers
P24286=1
P24237=99

#Play registration id Feature.
#First value - Enable/Disable feature, Mandatory 0 - No, 1 - Yes
#Second value - Code numbers
P24287=1
P24238=98

#Forced Codec Feature. 
#First value - Enable/Disable feature, Mandatory 0 - No, 1 - Yes
#Second value - Code numbers
P24259=1
P24200=02

#PCMU codec feature. 
#First value - Enable/Disable feature, Mandatory 0 - No, 1 - Yes
#Second value - Code numbers
P24276=1
P24227=7110

#PCMA codec feature
#First value - Enable/Disable feature, Mandatory 0 - No, 1 - Yes
#Second value - Code numbers
P24277=1
P24228=7111

#G723 codec feature
#First value - Enable/Disable feature, Mandatory 0 - No, 1 - Yes
#Second value - Code numbers
P24278=1
P24229=723

#G729 codec feature
#First value - Enable/Disable feature, Mandatory 0 - No, 1 - Yes
#Second value - Code numbers
P24279=1
P24230=729

#AAL2-G726-R16 codec 
#First value - Enable/Disable feature, Mandatory 0 - No, 1 - Yes
#Second value - Code numbers
P24280=1
P24231=72616

#AAL2-G726-R24 codec feature
#First value - Enable/Disable feature, Mandatory 0 - No, 1 - Yes
#Second value - Code numbers
P24281=1
P24232=72624

#AAL2-G726-R32 codec feature
#First value - Enable/Disable feature, Mandatory 0 - No, 1 - Yes
#Second value - Code numbers
P24282=1
P24233=72632

#AAL2-G726-R40 codec 
#First value - Enable/Disable feature, Mandatory 0 - No, 1 - Yes
#Second value - Code numbers
P24283=1
P24234=72640

#iLBC codec feature
#First value - Enable/Disable feature, Mandatory 0 - No, 1 - Yes
#Second value - Code numbers
P24284=1
P24235=7201

#G722 codec feature
#First value - Enable/Disable feature, Mandatory 0 - No, 1 - Yes
#Second value - Code numbers
P24285=1
P24236=722

################################################################################
#Profile 2-Ring Tones
################################################################################

#Distinctive Ring Tones#########################################################

#Distinctive Ring Tone 
#0 - Ring Tone 1, 1 - Ring Tone 2, 2 - Ring Tone 3, 3 - Ring Tone 4, 4 - Ring Tone 5, 
#5 - Ring Tone 6, 6 - Ring Tone 7, 7 - Ring Tone 8, 8 - Ring Tone 9, 9 - Ring Tone 10
#Distinctive Ring Tone 1
#Number: 0 to 9
#Mandatory
P880=0

#Choice 1 incoming caller ID
#String Max Length: 64
P881=

#Distinctive Ring Tone 2
#Number: 0 to 9
#Mandatory
P882=0

#Choice 2 incoming caller ID
#String Max Length: 64 
P883=

#Distinctive Ring Tone 3
#Number: 0 to 9
#Mandatory 
P884=0

#Choice 3 incoming caller ID
#String Max Length: 64
P885=

#Ring Tone Cadences################################################################################
#Syntax: c=on1/ off1[- on2/ off2[- on3/ off3]];(Cadence on and off are in 10 ms units)

#Ring Tone 1
#String Max Length: 256
P4030=c=2000/4000;

#Ring Tone 2
#String Max Length: 256 
P4031=c=2000/4000;

#Ring Tone 3
#String Max Length: 256 
P4032=c=2000/4000; 

#Ring Tone 4
#String Max Length: 256 
P4033=c=2000/4000;

#Ring Tone 5
#String Max Length: 256
P4034=c=2000/4000;

#Ring Tone 6
#String Max Length: 256 
P4035=c=2000/4000;

#Ring Tone 7
#String Max Length: 256
P4036=c=2000/4000;

#Ring Tone 8
#String Max Length: 256 
P4037=c=2000/4000;

#Ring Tone 9
#String Max Length: 256 
P4038=c=2000/4000; 

#Ring Tone 10
#String Max Length: 256 
P4039=c=2000/4000;

# Distinctive Call Waiting Tones##########################################################

# Distinctive Call Waiting Tone 1
# Number: 0-9
# Mandatory
P29174=0 

# Distinctive Call Waiting Tone 2
# Number: 0-9
# Mandatory
P29175=0

# Distinctive Call Waiting Tone 3
# Number: 0-9
# Mandatory
P29176=0

# Distinctive Call Waiting Tone CID matching plan for Tone 1
# Max Length: 64
P29177= 

# Distinctive Call Waiting Tone CID matching plan for Tone 2
# Max Length: 64
P29178= 

# Distinctive Call Waiting Tone CID matching plan for Tone 3
# Max Length: 64
P29179= 

# Call Waiting Tone Cadences ##############################################################
# Syntax: f1=val, f2=val[, c=on1/ off1[- on2/ off2[- on3/ off3]]];
# (Frequencies are in Hz and cadence on and off are in 1 ms units)
# Call Waiting Tone 1 - Call Waiting Tone 10
# Mandatory
P29180=f1=440@-13,c=300/10000-300/10000-0/0;
P29181=f1=440@-13,c=300/10000-300/10000-0/0;
P29182=f1=440@-13,c=300/10000-300/10000-0/0;
P29183=f1=440@-13,c=300/10000-300/10000-0/0;
P29184=f1=440@-13,c=300/10000-300/10000-0/0;
P29185=f1=440@-13,c=300/10000-300/10000-0/0;
P29186=f1=440@-13,c=300/10000-300/10000-0/0;
P29187=f1=440@-13,c=300/10000-300/10000-0/0;
P29188=f1=440@-13,c=300/10000-300/10000-0/0;
P29189=f1=440@-13,c=300/10000-300/10000-0/0;

################################################################################
#Profile 3-General Settings
################################################################################

#Profile Active.  0 - no, 1 - yes
#Number: 0,1
#Mandatory
P501=1

#Primary SIP Server
#String: serveraddress 
P547=sip.mycompany.com

#Failover SIP Server
#String: serveraddress 
P997=

#Prefer Primary SIP Server. 0 - No, 1 - Yes.
#Number: 0,1
#Mandatory
P4569=0

#Outbound Proxy
#String: serveraddress 
P548=proxy.mycompany.com

# Backup Outbound Proxy.
# String: serveraddress
P2533=

# Prefer Primary Outbound Proxy. 0 - No, 1 - Yes
# Number: 0, 1
# Mandatory
P28098=0


################################################################################
#Profile 3-Network Settings
################################################################################

#Layer 3 QoS SIP Diff-Serv (default 24)
#Number
#Mandatory
P5048=24

#Layer 3 QoS RTP Diff-Serv (default 46)
#Number
#Mandatory
P5052=46

#DNS Mode. 0 - A Record, 1 - SRV, 2 - NAPTR/SRV, 3 - Use Configured IP .
#Number: 0,1,2,3
#Mandatory 
P502=0

#Primary IP
#IP address
P2508=

#Backup IP1
#IP address
P2509=

#Backup IP2
#IP address
P2510=

#NAT Traversal (STUN). 0 - No, 2 - No but send keep-alive, 1 - Yes
#Number: 0,1,2
#Mandatory
P630=0

#Use NAT IP.  This will enable our SIP client to use this IP in the SIP message. Example 64.3.153.50.
#String: ipaddress 
P566=

#Proxy-Require (A SIP extension to enable firewall penetration)
#String: ipaddress 
P592=

################################################################################
#Profile 3-SIP Settings
################################################################################

#Basic Settings#################################################################

#SIP Transport. 0 - UDP, 1 - TCP, 2 - TLS
#Number: 0,1,2
#Mandatory
P530=0

#SIP Registration. 0 - no, 1 - yes
#Number: 0,1
#Mandatory 
P531=1

#Unregister On Reboot. 0 - no, 1 - yes
#Number: 0,1
#Mandatory 
P552=0

#Add Auth Header On Initial REGISTER
#Number: 0,1
#Mandatory 
P2559=0

#Outgoing call without Registration. 0 - no, 1 - yes
#Number: 0,1
#Mandatory 
P513=1

#Register Expiration (in minutes. default 1 hour, max 45 days)
#Number: 1 to 64800
#Mandatory 
P532=60

#SIP Registration Failure Retry Wait Time (in seconds. Between 1-3600, default is 30)
#Number: 1 to 3600
#Mandatory 
P571=30

# SIP Registration Failure Retry Wait Time upon 403 Forbidden. 0 second means stop retry registration. Default is 1200 sec.
# Number 0 to 3600
# Mandatory
P26202=1200

#Reregister before Expiration
#Number
#Mandatory
P2530=0

# Enable SIP OPTIONS/NOTIFY Keep Alive. 0 - No, 1 - OPTIONS, 2 - NOTIFY
# Number: 0, 1, 2
# Mandatory
P2597 = 0

# Enable SIP OPTIONS/NOTIFY Keep Alive Interval. In seconds. The default value is 30 seconds.
# Number: 1 - 64800
# Mandatory
P2598 = 30

# SIP OPTIONS/NOTIFY Keep Alive Max Lost. In packages. The default value is 3 packages.
# Number: 3 - 10
# Mandatory
P2599 = 3

#Local SIP port (default 7060)
#Number: 1 to 65535
#Mandatory 
P640=7060

#Use Random SIP Port 0 - no, 1 - yes
#Number: 0,1
#Mandatory 
P578=0

#Local RTP port (1024-65535, default 52000)
#Number: 1024 to 65535
#Mandatory
P539 = 52000

#SIP T1 Timeout. RFC 3261 T1 value.
#50 - 0.5 sec, 100 - 1 sec, 200 - 2 sec, 400 - 4 sec, 800 - 8 sec. Default 100.
#Number: 50,100,200,400,800
#Mandatory
P540=50

#SIP T2 Timeout. RFC 3261 T2 value.
#200 - 2 sec, 400 - 4 sec, 800 - 8 sec, 1600 - 16 sec, 3200 - 32 sec. Default 400.
#Number: 1600,3200,200,400,800
#Mandatory 
P541=400

#Remove OBP from Route Header. 0 - no, 1 - yes
#NUmber: 0,1
#Mandatory
P4564=0

#Support SIP Instance ID. 0 - no, 1 - yes
#Number: 0,1
#Mandatory
P589=1

# Hold Target Before Refer 0 - No, 1 - Yes
# Number: 0, 1
# Mandatory
P26203=1

#Refer-To Use Target Contact. 0 - no, 1 - yes
#Number: 0,1
#Mandatory 
P569=

#SUBSCRIBE for MWI. 0 - No, 1 - Yes.
#Number: 0,1
#Mandatory
P509=0

#Enable 100rel. 0 - No, 1 - Yes
#Number: 0 to 1
#Mandatory 
P535=0

#Tel URI. 0 - Disabled, 1 - User=Phone, 2 - Enabled
#Number: 0,1,2
#Mandatory 
P563=0

#Use Request Routing ID in SIP Headers, 0 - No, 1 - Yes
#Number: 0,1
#Mandatory 
P4893=0

#Do Not Escape '#' as %23 in SIP URI. 0 - No, 1 - Yes
#Number: 0, 1
#Mandatory
P4896= 0

#Disable Multiple m Line in SDP. 0 - No, 1 - Yes
P587= 0

#Use Privacy Header. 0 - Default, 1 - No, 2 - Yes
#Number: 0, 1, 2
#Mandatory
P2538= 0

#Use P-Preferred-Identity Header. 0 - Default, 1 - No, 2 - Yes
#Number: 0, 1, 2
#Mandatory
P2539= 0

#SIP REGISTER Contact Header Uses. 0 - LAN Address, 1 - WAN Address
#Number: 0, 1
#Mandatory
#P4439=0

# Caller ID Display. 0 - Auto, 1 - Disable, 2 - From Header
# Number: 0, 1, 2
# Mandatory
P2524=0

# Use Actual Ephemeral Port in Contact with TCP/TLS. 0 - No, 1 - Yes
# Number: 0, 1
# Mandatory
P2531 = 0

# SIP User-Agent
# String
P29271 = 

# SIP User-Agent Postfix
# String
P4836 = 

#Session Timer################################################################################

#Session Expiration (in seconds. default 180 seconds. Allowed value: 90-65535)
#Number: 90 to 64800
#Mandatory 
P534=180

#Minimum SE (in seconds. default 90 seconds, must be lower than or equal to P260)
#Number 90 to 64800
#Mandatory 
P527=90

#Caller Request Timer (Request for timer when calling) 0 - no, 1 - yes
#Number: 0,1
#Mandatory 
P528=0

#Callee Request Timer (Request for timer when called. i.e. if remote party supports timer but did not request for one) 0 - no, 1 - yes
#Number: 0,1
#Mandatory 
P629=0

#Force Timer (Still use timer when remote party does not support timer) 0 - no, 1 - yes
#Number: 0,1
#Mandatory 
P664=0

#UAC Specify Refresher. 0 - omit, 1 - UAC, 2 - UAS
#Number: 0,1,2
#Mandatory 
P632=0

#UAS Specify Refresher. 1 - UAC, 2 - UAS
#Number: 1,2
#Mandatory 
P533=1

#Force INVITE (Always refresh with INVITE instead of UPDATE even when remote party supports UPDATE) 0 - no, 1 - yes
#Number: 0,1
#Mandatory 
P365=0

#Security Settings################################################################################

#Validate Incoming Messages. 0 - No, 1 - Yes
#Number: 0,1
#Mandatory 
P4342=0

#Check SIP User ID for Incoming INVITE. 0 - No, 1 - Yes (no direct IP calling if Yes)
#Number: 0,1
#Mandatory 
P549=0 

#Allow Incoming SIP Messages from SIP Proxy Only
#Number: 0,1
#Mandatory 
P4043=0

#Authenticate incoming INVITE 
#Number: 0,1
P2546=0

# Authenticate server certificate domain. 0 - No, 1 - Yes, default is 0
# Number: 0, 1
# Mandatory
P2511=0

# Authenticate server certificate chain. 0 - No, 1 - Yes, default is 0
# Number: 0, 1
# Mandatory
P2567=0


################################################################################
#Profile 3-Fax Settings
################################################################################

#FAX Mode. 0 - T.38 (Auto Detect), 1 - Pass Through
#Number: 0,1
#Mandatory 
P510=0

#Fax Tone Detection Mode. 1 - Caller, 0 - Callee, 2 - Caller or Callee
#Number: 0,1,2
#Mandatory 
P595=0

#Send Re-INVITE After Fax. 0 - No, 1 - Yes
#Number: 0,1
#Mandatory 
P4369=0

#Send Re-INVITE After Fax Tone. 0 - No, 1 - Yes
#Number: 0,1
#Mandatory 
P4418=1

#Enable Silence Detection for Fax Disconnect. 0 - No, 1 - Yes
#Number: 0 to 1
#Mandatory 
P4408=1

################################################################################
#Profile 3-Audio Settings
################################################################################

#Preferred DTMF Method 1 
#100 - In-audio, 101 - RFC2833, 102 - SIP INFO
#Priority 1
#Number: 100 to 102
#Mandatory
P560=100

#Preferred DTMF Method 2
#Number: 100 to 102
#Mandatory 
P561=100

#Preferred DTMF Method 3
#Number: 100 to 102
#Mandatory 
P562=100

#DTMF-RELAY Tag Respect SIP INFO. 0 - No, 1 - Yes (If set to "NO", the dtmf-relay tag in Accept Header is always added in outbound INVITE. If set to "YES", it depends on if SIP INFO is chosen in Prefered DTMF Method.)
#Number: 0, 1
#Mandatory
P28090=0

#Disable DTMF Negotiation. 0 - no, 1 - yes 
#Number: 0,1
#Mandatory
P4827=0

#Enable Fast RFC2833. 0 - No, 1 - Yes
#Number: 0,1
#Mandatory
P21919=0

#DTMF Payload Type
#Number: 96 to 127
P579=101

#Preferred Vocoder
#0 - PCMU, 8 - PCMA, 4 - G.723, 18 - G.729, 2 - G.726-32, 100 - AAL2-G.726-16,
#102 - AAL2-G.726-24, 104 - AAL2-G726-32, 103 - AAL2-G.726-40, 98 - iLBC, 9 - G.722(wide band)
#Choice 1. 
#Mandatory
P557=0

#Choice 2. 
#Mandatory
P558=8

#Choice 3. 
#Mandatory
P559=4

#Choice 4. 
#Mandatory 
P660=18

#Choice 5. 
#Mandatory
P661=2

#Choice 6. 
#Mandatory 
P662=98

#Choice 7. 
#Mandatory
P514=104

#Choice 8. 
#Mandatory
P515=100

#Voice Frame per TX. (Default 2, from 1 to 4 for G711/G726/G729)
#Number: 1 to 4
P4593=2

#G723 rate. 0 - 6.3kbps encoding rate, 1 - 5.3kbps encoding rate
#Number: 0,1
#Mandatory 
P4350=0

#G726-32 Packing Mode. 0 - ITU, 1 - IETF
#Number: 0,1
#Mandatory 
P2523=0

#iLBC Frame Size. 0 - 20ms(default), 1 - 30ms.
#Number: 0,1
#Mandatory 
P505=0

#iLBC payload type. Between 96 and 127, default is 97.
#Number: 96 to 127
#Mandatory 
P504=97

#AAL2-G.726-16 Payload type. (between 96 and 127, default is 100)
#Number: 96 to 127
#Mandatory 
P519=100

#AAL2-G.726-24 Payload type. (between 96 and 127, default is 99)
#Number: 96 to 127
#Mandatory 
P520=99

#AAL2-G726-32 payload type. (between 96 and 127, default is 104)
#Number: 96 to 127
#Mandatory 
P521=104

#AAL2-G.726-40 Payload type. (between 96 and 127, default is 103)
#Number: 96 to 127
#Mandatory 
P522=103

#Use First Matching Vocoder in 200OK SDP. 0 - No, 1 - Yes
#Number: 0,1
#Mandatory 
P4365=0

#SRTP Mode
#0=Disabled
#1=Enabled but not forced
#2=Enabled and forced
#Number: 0,1,2
#Mandatory
P543=0

# Crypto Life Time
# 0 = Disabled
# 1 = Enabled
# Number: 0, 1
# Mandatory
P2563=1

#Silence Suppression (VAD). 0 - No, 1 - Yes
#Number: 0,1
#Mandatory 
P550=0

#Jitter Buffer Type. 0 - Fixed, 1 - Adaptive
#Number: 0,1
#Mandatory
P631= 1

#Jitter Buffer Length. 0 - Low, 1 - Medium, 2 - High
#Number: 0,1,2
#Mandatory
P835=1

# RTCP. 0 - Disable, 1 - Enable
# Number: 0, 1
# Mandatory
P2592=1

#SLIC Setting
#0 - USA, 1 - AUSTRIA, 2 - BELGIUM, 3 - FINELAND, 4 - FRANCE, 5 - GERMANY
#6 - GREECE, 7 -ITALY, 8 - JAPAN, 9 - NORWAY, 10 - SPAIN, 11 - SWEDEN,
#12 - UK, 13 - AUSTRALIA/NEW ZEALAND, 14 - CHINA
#Number: 0 to 14
#Mandatory 
P564=0

# Ringing Frequency. 0 - Default, 1 - 20Hz, 2 - 25Hz
# Number: 0, 1, 2
# Mandatory
P4431 = 0

#Caller ID Scheme
#0  - Bellcore/Telcordia
#1  - ETSI-FSK during ringing
#2  - ETSI-FSK prior to ringing with DTAS
#3  - ETSI-FSK prior to ringing with LR
#4  - ETSI-FSK prior to ringing with RP
#5  - ETSI-DTMF during ringing
#6  - ETSI-DTMF prior to ringing with DTAS
#7  - ETSI-DTMF prior to ringing with LR
#8  - ETSI-DTMF prior to ringing with RP
#9  - SIN 227 - BT
#10 - NTT Japan
#Number: 0 to 10
#Mandatory 
P663=0

#Polarity Reversal.  0 - No, 1 - Yes
#Number: 0,1
#Mandatory 
P665=0

#Loop Current Disconnect. 0 - No, 1 - Yes
#Number: 0,1
#Mandatory 
P593=0

# Play busy/reorder tone before Loop Current Disconnect
# 0 = Disabled
# 1 = Enabled
# Number: 0, 1
# Mandatory
P21927=0

#Loop Current Disconnect Duration. In 100 - 10000 milliseconds range, default is 200.
#Number: 100 to 10000
#Mandatory 
P657=200

#Enable Hook Flash
#Number: 0, 1
#Mandatory
P4426=1

#Hook Flash Timing. In 40-2000 milliseconds range
#minimum
#Number: 40 to 2000
#Mandatory
P511=300
#maximum
#Number: 40 to 2000
#Mandatory 
P512=1100

#On Hook Timing. (In 40-2000 milliseconds range, default is 400)
#Number: 40 to 2000
#Mandatory 
P634=400

#Gain:
#TX 
#<value=1> +6dB
#<value=2> +4dB
#<value=3> +2dB
#<value=0> 0dB
#<value=4> -2dB
#<value=5> -4dB
#<value=6> -6dB
#Number: 0 to 6
#Mandatory 
P648=0 

#RX 
#<value=1> +6dB
#<value=2> +4dB
#<value=3> +2dB
#<value=0> 0dB
#<value=4> -2dB
#<value=5> -4dB
#<value=6> -6dB
#Number: 0 to 6
#Mandatory 
P683=0

#Disable Line Echo Canceller (LEC).  0 - No, 1 - Yes
#Number: 0,1
#Mandatory
P4366=0

################################################################################
#Profile 3-Call Settings
################################################################################

#Early Dial. 0 - No, 1 - Yes (use "Yes" only if proxy supports 484 response). 0 - no, 1 - yes
#Number: 0,1
#Mandatory 
P529=0

#Dial Plan Prefix.(this prefix string is added to each dialed number)
#String Max Length: 32
P666=

#Dial Plan 
#String Max Length: 1024
P4202={ x+ | *x+ }

#Use #as Dial Key (if set to Yes, "#" will function as the "(Re-)Dial" key). 0 - no, 1 - yes
#Number: 0,1
#Mandatory 
P572=1

# Disable # as Redial Key. 0 - No, 1 - Yes
# Number: 0, 1
# Mandatory
P28149 = 0

#No Key Entry Timeout. Default - 4 seconds.
#Number: 1 to 15
#Mandatory
P492=4

#Offhook Auto-Dial Delay (default is 0)
#String: 0 to 60
P4047=0

# Allow Auto-Dial Config Per Port. 0 - Disable, 1 - Enable
# Number: 0, 1
# Mandatory
P28131=0

# RFC2543 Hold. 0 - No, 1 - Yes
# Number: 0, 1
# Mandatory
P26262=1

#Disable Call Waiting. 0 - no, 1 - yes
#Number: 0,1
#Mandatory 
P591=0

#Disable Call Waiting Caller ID. 0 - no, 1 - yes
#Number: 0,1
#Mandatory 
P523=0

#Disable Call Waiting Tone. 0 - no, 1 - yes
#Number: 0,1
#Mandatory 
P517=0

#Disable Connected Line ID. 0 = Disabled, 1 = Enabled (If yes, Connected Line ID will not be displayed even received.)
#Number: 0, 1
#Mandatory
P20527=0

#Disable Receiver Offhook Tone. 0 - No, 1 - Yes.
#Number: 0,1
#Mandatory 
P4795=0

#Disable Reminder Ring for On-Hold Call:
#Number: 0,1
#Mandatory 
P4362=0

# Disable Reminder Ring for DND. 0 - No, 1 - Yes
# Number: 0, 1
# Mandatory
P29272 = 0

# Disable Voicemail Reminder Tone. 0 - No, 1 - Yes
# Number: 0, 1
# Mandatory
P28144 = 0

#Disable Visual MWI. 0 - No, 1 - Yes
#Number: 0,1
#Mandatory 
P669=0

#Visual MWI type: 1 - FSK, 2 - Neon
#Number: 1,2
#Mandatory
P4373=1

#Transfer on Conference Hangup. 0 - no, 1 - yes
#Number: 0,1
#Mandatory 
P4565=0

#Send Hook Flash Event. 0 - no, 1 - yes 
#Number: 0 to 1
#Mandatory 
P574=0

#Flash Digit Control. 0 - No, 1 - Yes(Set Yes will overrides the default settings for call control when both channels are in use.) 
#Number: 0, 1
#Mandatory
P28082=0

# Callee Flash to 3WC. 0 - No, 1 - Yes
# Number: 0, 1
# Mandatory
P28171 = 0

#Ring Timeout. (0, 10-300, default is 60 seconds. When set to 0, the Ring Timeout feature is disabled)
#Number: 10 to 300
#Mandatory 
P516=60

#Delayed Call Forward Wait Time. Allowed range 1-120, in seconds. Default 20 seconds.
#Number: 1 to 120
#Mandatory
P570=20

#Send Anonymous. 0 - no, 1 - yes (caller ID will be blocked if set to Yes).
#Number: 0 to 1
#Mandatory 
P565=0

#Anonymous Call Rejection. 0 - No, 1 - Yes.
#Number: 0 to 1
#Mandatory 
P546=0

# Replace Beginning '+' with 00 in Caller ID. 0 - No, 1 - Yes
# Number: 0, 1
# Mandatory
P29273=0


#Hunting Group Type. 0 - Circular, 1 - Linear
#Number: 0,1
#Mandatory
P4397=0

#Hunting Group Ring Timeout. (5-300, default is 20 seconds)
#Number: 5 to 300
#Mandatory 
P4332=20

#Special Feature
#100 - Standard, 102 - BroadSoft, 108 - CBCOM, 109 - RNK, 111 - Huawei, 114 - ZTE IMS, 119 - PhonePower, 120 - TELKOM SA.
#Number: 100, 102, 108, 109, 111, 114, 119, 120
#Mandatory 
P567=100

################################################################################
#Profile 3-Call Features Settings
################################################################################

#Enable Call Features. 0 - No, 1 - Yes, 2 - Enable All
P551=1

# Reset Call Features. 0 - No, 1 - Yes
# Number: 0, 1
# Mandatory
P24599=0

#SRTP Feature.
#First value - Enable/Disable feature, Mandatory 0 - No, 1 - Yes
#Second value - Enable feature code numbers
#Third value - Disable feature code numbers
P24460=1
P24401=16
P24402=17

#SRTP per call Feature.
#First value - Enable/Disable feature, Mandatory 0 - No, 1 - Yes
#Second value - Enable feature code numbers
#Third value - Disable feature code numbers
P24461=1
P24403=18
P24404=19

#CID Feature.
#First value - Enable/Disable feature, Mandatory 0 - No, 1 - Yes
#Second value - Enable feature code numbers
#Third value - Disable feature code numbers
P24462=1
P24405=31
P24406=30

#CID per call Feature.
#First value - Enable/Disable feature, Mandatory 0 - No, 1 - Yes
#Second value - Enable feature code numbers
#Third value - Disable feature code numbers
P24465=1
P24419=82
P24410=67

#Direct IP calling Feature.
#First value - Enable/Disable feature, Mandatory 0 - No, 1 - Yes
#Second value - Code numbers
P24463=1
P24407=47

#CW Feature. 
#First value - Enable/Disable feature, Mandatory 0 - No, 1 - Yes
#Second value - Enable feature code numbers
#Third value - Disable feature code numbers
P24464=1
P24409=51
P24408=50

#CW per call Feature. 
#First value - Enable/Disable feature, Mandatory 0 - No, 1 - Yes
#Second value - Enable feature code numbers
#Third value - Disable feature code numbers
P24467=1
P24413=71
P24412=70

#Call return Feature.
#First value - Enable/Disable feature, Mandatory 0 - No, 1 - Yes
#Second value - Code numbers
P24466=1
P24411=69

#Unconditional forward Feature.
#First value - Enable/Disable feature, Mandatory 0 - No, 1 - Yes
#Second value - Enable feature code numbers
#Third value - Disable feature code numbers
P24468=1
P24414=72
P24415=73

#Busy forward Feature.
#First value - Enable/Disable feature, Mandatory 0 - No, 1 - Yes
#Second value - Enable feature code numbers
#Third value - Disable feature code numbers
P24472=1
P24421=90
P24422=91

#Delayed forward Feature.
#First value - Enable/Disable feature, Mandatory 0 - No, 1 - Yes
#Second value - Enable feature code numbers
#Third value - Disable feature code numbers
P24473=1
P24423=92
P24424=93

#Paging Feature.
#First value - Enable/Disable feature, Mandatory 0 - No, 1 - Yes
#Second value - Code numbers
P24469=1
P24416=74

#DND Feature.
#First value - Enable/Disable feature, Mandatory 0 - No, 1 - Yes
#Second value - Enable feature code numbers
#Third value - Disable feature code numbers
P24470=1
P24417=78
P24418=79

#Blind Transfer Feature.
#First value - Enable/Disable feature, Mandatory 0 - No, 1 - Yes
#Second value - Code numbers
P24471=1
P24420=87

#Disable LEC per call Feature.
#First value - Enable/Disable feature, Mandatory 0 - No, 1 - Yes
#Second value - Code numbers
P24474=1
P24425=03

#Disable Bellcore-style 3-Way Conference. 0 - No, 1 - Yes
P4832=0
#Star Code 3WC Feature. 0 - No, 1 - Yes
P24475=1
#Star Code 3WC
P24426=23

#Provision start Feature.
#First value - Enable/Disable feature, Mandatory 0 - No, 1 - Yes
#Second value - Code numbers
P24486=1
P24437=99

#Play registration id Feature.
#First value - Enable/Disable feature, Mandatory 0 - No, 1 - Yes
#Second value - Code numbers
P24487=1
P24438=98

#Forced Codec Feature. 
#First value - Enable/Disable feature, Mandatory 0 - No, 1 - Yes
#Second value - Code numbers
P24459=1
P24400=02

#PCMU codec feature. 
#First value - Enable/Disable feature, Mandatory 0 - No, 1 - Yes
#Second value - Code numbers
P24476=1
P24427=7110

#PCMA codec feature
#First value - Enable/Disable feature, Mandatory 0 - No, 1 - Yes
#Second value - Code numbers
P24477=1
P24428=7111

#G723 codec feature
#First value - Enable/Disable feature, Mandatory 0 - No, 1 - Yes
#Second value - Code numbers
P24478=1
P24429=723

#G729 codec feature
#First value - Enable/Disable feature, Mandatory 0 - No, 1 - Yes
#Second value - Code numbers
P24479=1
P24430=729

#AAL2-G726-R16 codec 
#First value - Enable/Disable feature, Mandatory 0 - No, 1 - Yes
#Second value - Code numbers
P24480=1
P24431=72616

#AAL2-G726-R24 codec feature
#First value - Enable/Disable feature, Mandatory 0 - No, 1 - Yes
#Second value - Code numbers
P24481=1
P24432=72624

#AAL2-G726-R32 codec feature
#First value - Enable/Disable feature, Mandatory 0 - No, 1 - Yes
#Second value - Code numbers
P24482=1
P24433=72632

#AAL2-G726-R40 codec 
#First value - Enable/Disable feature, Mandatory 0 - No, 1 - Yes
#Second value - Code numbers
P24483=1
P24434=72640

#iLBC codec feature
#First value - Enable/Disable feature, Mandatory 0 - No, 1 - Yes
#Second value - Code numbers
P24484=1
P24435=7201

#G722 codec feature
#First value - Enable/Disable feature, Mandatory 0 - No, 1 - Yes
#Second value - Code numbers
P24485=1
P24436=722

################################################################################
#Profile 3-Ring Tones
################################################################################

#Distinctive Ring Tones#########################################################

#Distinctive Ring Tone 
#0 - Ring Tone 1, 1 - Ring Tone 2, 2 - Ring Tone 3, 3 - Ring Tone 4, 4 - Ring Tone 5, 
#5 - Ring Tone 6, 6 - Ring Tone 7, 7 - Ring Tone 8, 8 - Ring Tone 9, 9 - Ring Tone 10
#Distinctive Ring Tone 1
#Number: 0 to 9
#Mandatory
P580=0

#Choice 1 incoming caller ID
#String Max Length: 64
P581=

#Distinctive Ring Tone 2
#Number: 0 to 9
#Mandatory
P582=0

#Choice 2 incoming caller ID
#String Max Length: 64 
P583=

#Distinctive Ring Tone 3
#Number: 0 to 9
#Mandatory 
P584=0

#Choice 3 incoming caller ID
#String Max Length: 64
P585=

#Ring Tone Cadences################################################################################
#Syntax: c=on1/ off1[- on2/ off2[- on3/ off3]];(Cadence on and off are in 10 ms units)

#Ring Tone 1
#String Max Length: 256
P4020=c=2000/4000;

#Ring Tone 2
#String Max Length: 256 
P4021=c=2000/4000;

#Ring Tone 3
#String Max Length: 256 
P4022=c=2000/4000; 

#Ring Tone 4
#String Max Length: 256 
P4023=c=2000/4000;

#Ring Tone 5
#String Max Length: 256
P4024=c=2000/4000;

#Ring Tone 6
#String Max Length: 256 
P4025=c=2000/4000;

#Ring Tone 7
#String Max Length: 256
P4026=c=2000/4000;

#Ring Tone 8
#String Max Length: 256 
P4027=c=2000/4000;

#Ring Tone 9
#String Max Length: 256 
P4028=c=2000/4000; 

#Ring Tone 10
#String Max Length: 256 
P4029=c=2000/4000;

#######################################
# Call Waiting Tones for Profile 3 ####
#######################################
# Distinctive Call Waiting Tones#########################################################

# Distinctive Call Waiting Tone 1
# Number: 0-9
# Mandatory
P29274=0

# Distinctive Call Waiting Tone 2
# Number: 0-9
# Mandatory
P29275=0

# Distinctive Call Waiting Tone 3
# Number: 0-9
# Mandatory
P29276=0

# Distinctive Call Waiting Tone CID matching plan for Tone 1
# Max Length: 64
P29277= 

# Distinctive Call Waiting Tone CID matching plan for Tone 2
# Max Length: 64
P29278= 

# Distinctive Call Waiting Tone CID matching plan for Tone 3
# Max Length: 64
P29279= 

# Call Waiting Tone Cadences##############################################################
# Syntax: f1=val, f2=val[, c=on1/ off1[- on2/ off2[- on3/ off3]]]; (Frequencies are in Hz and cadence on and off are in 1 ms units)
# Call Waiting Tone 1 - Call Waiting Tone 10
# Mandatory
P29280=f1=440@-13,c=300/10000-300/10000-0/0;
P29281=f1=440@-13,c=300/10000-300/10000-0/0;
P29282=f1=440@-13,c=300/10000-300/10000-0/0;
P29283=f1=440@-13,c=300/10000-300/10000-0/0;
P29284=f1=440@-13,c=300/10000-300/10000-0/0;
P29285=f1=440@-13,c=300/10000-300/10000-0/0;
P29286=f1=440@-13,c=300/10000-300/10000-0/0;
P29287=f1=440@-13,c=300/10000-300/10000-0/0;
P29288=f1=440@-13,c=300/10000-300/10000-0/0;
P29289=f1=440@-13,c=300/10000-300/10000-0/0;

################################################################################
#Profile 4-General Settings
################################################################################

#Profile Active.  0 - no, 1 - yes
#Number: 0,1
#Mandatory
P601=1

#Primary SIP Server
#String: serveraddress 
P602=sip.mycompany.com

#Failover SIP Server
#String: serveraddress 
P998=

#Prefer Primary SIP Server. 0 - No, 1 - Yes.
#Number: 0,1
#Mandatory
P4570=0

#Outbound Proxy
#String: serveraddress 
P603=proxy.mycompany.com

# Backup Outbound Proxy.
# String: serveraddress
P2633=

# Prefer Primary Outbound Proxy. 0 - No, 1 - Yes
# Number: 0, 1
# Mandatory
P28099=0

################################################################################
#Profile 4-Network Settings
################################################################################

#Layer 3 QoS SIP Diff-Serv (default 24)
#Number
#Mandatory
P5049=24

#Layer 3 QoS RTP Diff-Serv (default 46)
#Number
#Mandatory
P5053=46

#DNS Mode. 0 - A Record, 1 - SRV, 2 - NAPTR/SRV, 3 - Use Configured IP .
#Number: 0,1,2,3
#Mandatory 
P608=0

#Primary IP
#IP address
P2608=

#Backup IP1
#IP address
P2609=

#Backup IP2
#IP address
P2610=

#NAT Traversal (STUN). 0 - No, 2 - No but send keep-alive, 1 - Yes
#Number: 0,1,2
#Mandatory
P614=0

#Use NAT IP.  This will enable our SIP client to use this IP in the SIP message. Example 64.3.153.50.
#String: ipaddress 
P4576=

#Proxy-Require (A SIP extension to enable firewall penetration)
#String: ipaddress 
P618=

################################################################################
#Profile 4-SIP Settings
################################################################################

#Basic Settings#################################################################

#SIP Transport. 0 - UDP, 1 - TCP, 2 - TLS
#Number: 0,1,2
#Mandatory
P4648=0

#SIP Registration. 0 - no, 1 - yes
#Number: 0,1
#Mandatory 
P610=1

#Unregister On Reboot. 0 - no, 1 - yes
#Number: 0,1
#Mandatory 
P611=0

#Add Auth Header On Initial REGISTER
#Number: 0,1
#Mandatory 
P2659=0

#Outgoing call without Registration. 0 - no, 1 - yes
#Number: 0,1
#Mandatory 
P4378=1

#Register Expiration (in minutes. default 1 hour, max 45 days)
#Number: 1 to 64800
#Mandatory 
P612=60

#SIP Registration Failure Retry Wait Time (in seconds. Between 1-3600, default is 30)
#Number: 1 to 3600
#Mandatory 
P671=30

# SIP Registration Failure Retry Wait Time upon 403 Forbidden. 0 second means stop retry registration. Default is 1200 sec.
# Number 0 to 3600
# Mandatory
P26302=1200

#Reregister before Expiration
#Number
#Mandatory
P2630=0

# Enable SIP OPTIONS/NOTIFY Keep Alive. 0 - No, 1 - OPTIONS, 2 - NOTIFY
# Number: 0, 1, 2
# Mandatory
P2697 = 0

# Enable SIP OPTIONS/NOTIFY Keep Alive Interval. In seconds. The default value is 30 seconds.
# Number: 1 - 64800
# Mandatory
P2698 = 30

# SIP OPTIONS/NOTIFY Keep Alive Max Lost. In packages. The default value is 3 packages.
# Number: 3 - 10
# Mandatory
P2699 = 3

#Local SIP port (default 8060)
#Number: 1 to 65535
#Mandatory 
P613=8060

#Use Random SIP Port 0 - no, 1 - yes
#Number: 0,1
#Mandatory 
P4792=0

#Local RTP port (1024-65535, default 53000)
#Number: 1024 to 65535
#Mandatory
P4573 = 53000

#SIP T1 Timeout. RFC 3261 T1 value.
#50 - 0.5 sec, 100 - 1 sec, 200 - 2 sec, 400 - 4 sec, 800 - 8 sec. Default 100.
#Number: 50,100,200,400,800
#Mandatory
P4640=50

#SIP T2 Timeout. RFC 3261 T2 value.
#200 - 2 sec, 400 - 4 sec, 800 - 8 sec, 1600 - 16 sec, 3200 - 32 sec. Default 400.
#Number: 1600,3200,200,400,800
#Mandatory 
P641=400

#Remove OBP from Route Header. 0 - no, 1 - yes
#NUmber: 0,1
#Mandatory
P4790=0

#Support SIP Instance ID. 0 - no, 1 - yes
#Number: 0,1
#Mandatory
P689=1

# Hold Target Before Refer 0 - No, 1 - Yes
# Number: 0, 1
# Mandatory
P26303=1

#Refer-To Use Target Contact. 0 - no, 1 - yes
#Number: 0,1
#Mandatory 
P4649=

#SUBSCRIBE for MWI. 0 - No, 1 - Yes.
#Number: 0,1
#Mandatory
P615=0

#Enable 100rel. 0 - No, 1 - Yes
#Number: 0 to 1
#Mandatory 
P635=0

#Tel URI. 0 - Disabled, 1 - User=Phone, 2 - Enabled
#Number: 0,1,2
#Mandatory 
P609=0

#Use Request Routing ID in SIP Headers, 0 - No, 1 - Yes
#Number: 0,1
#Mandatory 
P4894=0

#Do Not Escape '#' as %23 in SIP URI. 0 - No, 1 - Yes
#Number: 0, 1
#Mandatory
P4897= 0

#Disable Multiple m Line in SDP. 0 - No, 1 - Yes
P687= 0

#Use Privacy Header. 0 - Default, 1 - No, 2 - Yes
#Number: 0, 1, 2
#Mandatory
P2638= 0

#Use P-Preferred-Identity Header. 0 - Default, 1 - No, 2 - Yes
#Number: 0, 1, 2
#Mandatory
P2639= 0

#SIP REGISTER Contact Header Uses. 0 - LAN Address, 1 - WAN Address
#Number: 0, 1
#Mandatory
#P4440=0

# Caller ID Display. 0 - Auto, 1 - Disable, 2 - From Header
# Number: 0, 1, 2
# Mandatory
P2624=0

# Use Actual Ephemeral Port in Contact with TCP/TLS. 0 - No, 1 - Yes
# Number: 0, 1
# Mandatory
P2631 = 0

# SIP User-Agent
# String
P29371 = 

# SIP User-Agent Postfix
# String
P4837 = 

#Session Timer################################################################################

#Session Expiration (in seconds. default 180 seconds. Allowed value: 90-65535)
#Number: 90 to 64800
#Mandatory 
P4634=180

#Minimum SE (in seconds. default 90 seconds, must be lower than or equal to P260)
#Number 90 to 64800
#Mandatory 
P627=90

#Caller Request Timer (Request for timer when calling) 0 - no, 1 - yes
#Number: 0,1
#Mandatory 
P628=0

#Callee Request Timer (Request for timer when called. i.e. if remote party supports timer but did not request for one) 0 - no, 1 - yes
#Number: 0,1
#Mandatory 
P4629=0

#Force Timer (Still use timer when remote party does not support timer) 0 - no, 1 - yes
#Number: 0,1
#Mandatory 
P4630=0

#UAC Specify Refresher. 0 - omit, 1 - UAC, 2 - UAS
#Number: 0,1,2
#Mandatory 
P4632=0

#UAS Specify Refresher. 1 - UAC, 2 - UAS
#Number: 1,2
#Mandatory 
P633=1

#Force INVITE (Always refresh with INVITE instead of UPDATE even when remote party supports UPDATE) 0 - no, 1 - yes
#Number: 0,1
#Mandatory 
P4631=0

#Security Settings################################################################################

#Validate Incoming Messages. 0 - No, 1 - Yes
#Number: 0,1
#Mandatory 
P4343=0

#Check SIP User ID for Incoming INVITE. 0 - No, 1 - Yes (no direct IP calling if Yes)
#Number: 0,1
#Mandatory 
P649=0 

#Allow Incoming SIP Messages from SIP Proxy Only
#Number: 0,1
#Mandatory 
P4044=0

#Authenticate incoming INVITE 
#Number: 0,1
P2646=0

# Authenticate server certificate domain. 0 - No, 1 - Yes, default is 0
# Number: 0, 1
# Mandatory
P2611=0

# Authenticate server certificate chain. 0 - No, 1 - Yes, default is 0
# Number: 0, 1
# Mandatory
P2667=0

################################################################################
#Profile 4-Fax Settings
################################################################################

#FAX Mode. 0 - T.38 (Auto Detect), 1 - Pass Through
#Number: 0,1
#Mandatory 
P4384=0

#Fax Tone Detection Mode. 1 - Caller, 0 - Callee, 2 - Caller or Callee
#Number: 0,1,2
#Mandatory 
P4382=0

#Send Re-INVITE After Fax. 0 - No, 1 - Yes
#Number: 0,1
#Mandatory 
P4370=0

#Send Re-INVITE After Fax Tone. 0 - No, 1 - Yes
#Number: 0,1
#Mandatory 
P4419=1

#Enable Silence Detection for Fax Disconnect. 0 - No, 1 - Yes
#Number: 0 to 1
#Mandatory 
P4409=1

################################################################################
#Profile 4-Audio Settings
################################################################################

#Preferred DTMF Method 1 
#100 - In-audio, 101 - RFC2833, 102 - SIP INFO
#Priority 1
#Number: 100 to 102
#Mandatory
P4583=100

#Preferred DTMF Method 2
#Number: 100 to 102
#Mandatory 
P4584=100

#Preferred DTMF Method 3
#Number: 100 to 102
#Mandatory 
P4585=100

#DTMF-RELAY Tag Respect SIP INFO. 0 - No, 1 - Yes (If set to "NO", the dtmf-relay tag in Accept Header is always added in outbound INVITE. If set to "YES", it depends on if SIP INFO is chosen in Prefered DTMF Method.)
#Number: 0, 1
#Mandatory
P28091=0

#Disable DTMF Negotiation. 0 - no, 1 - yes 
#Number: 0,1
#Mandatory
P4828=0

#Enable Fast RFC2833. 0 - No, 1 - Yes
#Number: 0,1
#Mandatory
P21920=0

#DTMF Payload Type
#Number: 96 to 127
P4574=101

#Preferred Vocoder
#0 - PCMU, 8 - PCMA, 4 - G.723, 18 - G.729, 2 - G.726-32, 100 - AAL2-G.726-16,
#102 - AAL2-G.726-24, 104 - AAL2-G726-32, 103 - AAL2-G.726-40, 98 - iLBC, 9 - G.722(wide band)
#Choice 1. 
#Mandatory
P651=0

#Choice 2. 
#Mandatory
P652=8

#Choice 3. 
#Mandatory
P653=4

#Choice 4. 
#Mandatory 
P654=18

#Choice 5. 
#Mandatory
P655=2

#Choice 6. 
#Mandatory 
P656=98

#Choice 7. 
#Mandatory
P4657=104

#Choice 8. 
#Mandatory
P658=100

#Voice Frame per TX. (Default 2, from 1 to 4 for G711/G726/G729)
#Number: 1 to 4
P4594=2

#G723 rate. 0 - 6.3kbps encoding rate, 1 - 5.3kbps encoding rate
#Number: 0,1
#Mandatory 
P4349=0

#G726-32 Packing Mode. 0 - ITU, 1 - IETF
#Number: 0,1
#Mandatory 
P2623=0

#iLBC Frame Size. 0 - 20ms(default), 1 - 30ms.
#Number: 0,1
#Mandatory 
P695=0

#iLBC payload type. Between 96 and 127, default is 97.
#Number: 96 to 127
#Mandatory 
P694=97

#AAL2-G.726-16 Payload type. (between 96 and 127, default is 100)
#Number: 96 to 127
#Mandatory 
P4411=100

#AAL2-G.726-24 Payload type. (between 96 and 127, default is 99)
#Number: 96 to 127
#Mandatory 
P4412=99

#AAL2-G726-32 payload type. (between 96 and 127, default is 104)
#Number: 96 to 127
#Mandatory 
P4413=104

#AAL2-G.726-40 Payload type. (between 96 and 127, default is 103)
#Number: 96 to 127
#Mandatory 
P4414=103

#Use First Matching Vocoder in 200OK SDP. 0 - No, 1 - Yes
#Number: 0,1
#Mandatory 
P4791=0

#SRTP Mode
#0=Disabled
#1=Enabled but not forced
#2=Enabled and forced
#Number: 0,1,2
#Mandatory
P643=0

# Crypto Life Time
# 0 = Disabled
# 1 = Enabled
# Number: 0, 1
# Mandatory
P2663=1

#Silence Suppression (VAD). 0 - No, 1 - Yes
#Number: 0,1
#Mandatory 
P685=0

#Jitter Buffer Type. 0 - Fixed, 1 - Adaptive
#Number: 0,1
#Mandatory
P698= 1

#Jitter Buffer Length. 0 - Low, 1 - Medium, 2 - High
#Number: 0,1,2
#Mandatory
P697=1

# RTCP. 0 - Disable, 1 - Enable
# Number: 0, 1
# Mandatory
P2692=1

#SLIC Setting
#0 - USA, 1 - AUSTRIA, 2 - BELGIUM, 3 - FINELAND, 4 - FRANCE, 5 - GERMANY
#6 - GREECE, 7 -ITALY, 8 - JAPAN, 9 - NORWAY, 10 - SPAIN, 11 - SWEDEN,
#12 - UK, 13 - AUSTRALIA/NEW ZEALAND, 14 - CHINA
#Number: 0 to 14
#Mandatory 
P4335=0

# Ringing Frequency. 0 - Default, 1 - 20Hz, 2 - 25Hz
# Number: 0, 1, 2
# Mandatory
P4432 = 0

#Caller ID Scheme
#0  - Bellcore/Telcordia
#1  - ETSI-FSK during ringing
#2  - ETSI-FSK prior to ringing with DTAS
#3  - ETSI-FSK prior to ringing with LR
#4  - ETSI-FSK prior to ringing with RP
#5  - ETSI-DTMF during ringing
#6  - ETSI-DTMF prior to ringing with DTAS
#7  - ETSI-DTMF prior to ringing with LR
#8  - ETSI-DTMF prior to ringing with RP
#9  - SIN 227 - BT
#10 - NTT Japan
#Number: 0 to 10
#Mandatory 
P4337=0

#Polarity Reversal.  0 - No, 1 - Yes
#Number: 0,1
#Mandatory 
P4339=0

#Loop Current Disconnect. 0 - No, 1 - Yes
#Number: 0,1
#Mandatory 
P4346=0

# Play busy/reorder tone before Loop Current Disconnect
# 0 = Disabled
# 1 = Enabled
# Number: 0, 1
# Mandatory
P21928=0 Profile4

#Loop Current Disconnect Duration. In 100 - 10000 milliseconds range, default is 200.
#Number: 100 to 10000
#Mandatory 
P4347=200

#Enable Hook Flash
#Number: 0, 1
#Mandatory
P4427=1

#Hook Flash Timing. In 40-2000 milliseconds range
#minimum
#Number: 40 to 2000
#Mandatory
P4387=300
#maximum
#Number: 40 to 2000
#Mandatory 
P4388=1100

#On Hook Timing. (In 40-2000 milliseconds range, default is 400)
#Number: 40 to 2000
#Mandatory 
P4390=400

#Gain:
#TX 
#<value=1> +6dB
#<value=2> +4dB
#<value=3> +2dB
#<value=0> 0dB
#<value=4> -2dB
#<value=5> -4dB
#<value=6> -6dB
#Number: 0 to 6
#Mandatory 
P4393=0 

#RX 
#<value=1> +6dB
#<value=2> +4dB
#<value=3> +2dB
#<value=0> 0dB
#<value=4> -2dB
#<value=5> -4dB
#<value=6> -6dB
#Number: 0 to 6
#Mandatory 
P4394=0

#Disable Line Echo Canceller (LEC).  0 - No, 1 - Yes
#Number: 0,1
#Mandatory
P4355=0

################################################################################
#Profile 4-Call Settings
################################################################################

#Early Dial. 0 - No, 1 - Yes (use "Yes" only if proxy supports 484 response). 0 - no, 1 - yes
#Number: 0,1
#Mandatory 
P622=0

#Dial Plan Prefix.(this prefix string is added to each dialed number)
#String Max Length: 32
P619=

#Dial Plan 
#String Max Length: 1024
P4203={ x+ | *x+ }

#Use #as Dial Key (if set to Yes, "#" will function as the "(Re-)Dial" key). 0 - no, 1 - yes
#Number: 0,1
#Mandatory 
P692=1

# Disable # as Redial Key. 0 - No, 1 - Yes
# Number: 0, 1
# Mandatory
P28150 = 0

#No Key Entry Timeout. Default - 4 seconds.
#Number: 1 to 15
#Mandatory
P4588=4

#Offhook Auto-Dial Delay (default is 0)
#String: 0 to 60
P4048=0

# Allow Auto-Dial Config Per Port. 0 - Disable, 1 - Enable
# Number: 0, 1
# Mandatory
P28132=0

# RFC2543 Hold. 0 - No, 1 - Yes
# Number: 0, 1
# Mandatory
P26362=1

#Disable Call Waiting. 0 - no, 1 - yes
#Number: 0,1
#Mandatory 
P4577=0

#Disable Call Waiting Caller ID. 0 - no, 1 - yes
#Number: 0,1
#Mandatory 
P4578=0

#Disable Call Waiting Tone. 0 - no, 1 - yes
#Number: 0,1
#Mandatory 
P4579=0

#Disable Connected Line ID. 0 = Disabled, 1 = Enabled (If yes, Connected Line ID will not be displayed even received.)
#Number: 0, 1
#Mandatory
P20528=0

#Disable Receiver Offhook Tone. 0 - No, 1 - Yes.
#Number: 0,1
#Mandatory 
P4796=0

#Disable Reminder Ring for On-Hold Call:
#Number: 0,1
#Mandatory 
P4359=0

# Disable Reminder Ring for DND. 0 - No, 1 - Yes
# Number: 0, 1
# Mandatory
P29372 = 0

# Disable Voicemail Reminder Tone. 0 - No, 1 - Yes
# Number: 0, 1
# Mandatory
P28145 = 0

#Disable Visual MWI. 0 - No, 1 - Yes
#Number: 0,1
#Mandatory 
P4375=0

#Visual MWI type: 1 - FSK, 2 - Neon
#Number: 1,2
#Mandatory
P4374=1

#Transfer on Conference Hangup. 0 - no, 1 - yes
#Number: 0,1
#Mandatory 
P4566=0

#Send Hook Flash Event. 0 - no, 1 - yes 
#Number: 0 to 1
#Mandatory 
P4575=0

#Flash Digit Control. 0 - No, 1 - Yes(Set Yes will overrides the default settings for call control when both channels are in use.) 
#Number: 0, 1
#Mandatory
P28083=0

# Callee Flash to 3WC. 0 - No, 1 - Yes
# Number: 0, 1
# Mandatory
P28172 = 0 

#Ring Timeout. (0, 10-300, default is 60 seconds. When set to 0, the Ring Timeout feature is disabled)
#Number: 10 to 300
#Mandatory 
P676=60

#Delayed Call Forward Wait Time. Allowed range 1-120, in seconds. Default 20 seconds.
#Number: 1 to 120
#Mandatory
P670=20

#Send Anonymous. 0 - no, 1 - yes (caller ID will be blocked if set to Yes).
#Number: 0 to 1
#Mandatory 
P621=0

#Anonymous Call Rejection. 0 - No, 1 - Yes.
#Number: 0 to 1
#Mandatory 
P646=0

# Replace Beginning '+' with 00 in Caller ID. 0 - No, 1 - Yes
# Number: 0, 1
# Mandatory
P29373=0


#Hunting Group Type. 0 - Circular, 1 - Linear
#Number: 0,1
#Mandatory
P4398=0

#Hunting Group Ring Timeout. (5-300, default is 20 seconds)
#Number: 5 to 300
#Mandatory 
P4333=20

#Special Feature
#100 - Standard, 102 - BroadSoft, 108 - CBCOM, 109 - RNK, 111 - Huawei, 114 - ZTE IMS, 119 - PhonePower, 120 - TELKOM SA.
#Number: 100, 102, 108, 109, 111, 114, 119, 120
#Mandatory 
P624=100

################################################################################
#Profile 4-Call Features Settings
################################################################################

#Enable Call Features. 0 - No, 1 - Yes, 2 - Enable All
P620=1

# Reset Call Features. 0 - No, 1 - Yes
# Number: 0, 1
# Mandatory
P24799 = 0

#SRTP Feature.
#First value - Enable/Disable feature, Mandatory 0 - No, 1 - Yes
#Second value - Enable feature code numbers
#Third value - Disable feature code numbers
P24660=1
P24601=16
P24602=17

#SRTP per call Feature.
#First value - Enable/Disable feature, Mandatory 0 - No, 1 - Yes
#Second value - Enable feature code numbers
#Third value - Disable feature code numbers
P24661=1
P24603=18
P24604=19

#CID Feature.
#First value - Enable/Disable feature, Mandatory 0 - No, 1 - Yes
#Second value - Enable feature code numbers
#Third value - Disable feature code numbers
P24662=1
P24605=31
P24606=30

#CID per call Feature.
#First value - Enable/Disable feature, Mandatory 0 - No, 1 - Yes
#Second value - Enable feature code numbers
#Third value - Disable feature code numbers
P24665=1
P24619=82
P24610=67

#Direct IP calling Feature.
#First value - Enable/Disable feature, Mandatory 0 - No, 1 - Yes
#Second value - Code numbers
P24663=1
P24607=47

#CW Feature. 
#First value - Enable/Disable feature, Mandatory 0 - No, 1 - Yes
#Second value - Enable feature code numbers
#Third value - Disable feature code numbers
P24664=1
P24609=51
P24608=50

#CW per call Feature. 
#First value - Enable/Disable feature, Mandatory 0 - No, 1 - Yes
#Second value - Enable feature code numbers
#Third value - Disable feature code numbers
P24667=1
P24613=71
P24612=70

#Call return Feature.
#First value - Enable/Disable feature, Mandatory 0 - No, 1 - Yes
#Second value - Code numbers
P24666=1
P24611=69

#Unconditional forward Feature.
#First value - Enable/Disable feature, Mandatory 0 - No, 1 - Yes
#Second value - Enable feature code numbers
#Third value - Disable feature code numbers
P24668=1
P24614=72
P24615=73

#Busy forward Feature.
#First value - Enable/Disable feature, Mandatory 0 - No, 1 - Yes
#Second value - Enable feature code numbers
#Third value - Disable feature code numbers
P24672=1
P24621=90
P24622=91

#Delayed forward Feature.
#First value - Enable/Disable feature, Mandatory 0 - No, 1 - Yes
#Second value - Enable feature code numbers
#Third value - Disable feature code numbers
P24673=1
P24623=92
P24624=93

#Paging Feature.
#First value - Enable/Disable feature, Mandatory 0 - No, 1 - Yes
#Second value - Code numbers
P24669=1
P24616=74

#DND Feature.
#First value - Enable/Disable feature, Mandatory 0 - No, 1 - Yes
#Second value - Enable feature code numbers
#Third value - Disable feature code numbers
P24670=1
P24617=78
P24618=79

#Blind Transfer Feature.
#First value - Enable/Disable feature, Mandatory 0 - No, 1 - Yes
#Second value - Code numbers
P24671=1
P24620=87

#Disable LEC per call Feature.
#First value - Enable/Disable feature, Mandatory 0 - No, 1 - Yes
#Second value - Code numbers
P24674=1
P24625=03

#Disable Bellcore-style 3-Way Conference. 0 - No, 1 - Yes
P4833=0
#Star Code 3WC Feature. 0 - No, 1 - Yes
P24675=1
#Star Code 3WC
P24626=23

#Provision start Feature.
#First value - Enable/Disable feature, Mandatory 0 - No, 1 - Yes
#Second value - Code numbers
P24686=1
P24637=99

#Play registration id Feature.
#First value - Enable/Disable feature, Mandatory 0 - No, 1 - Yes
#Second value - Code numbers
P24687=1
P24638=98

#Forced Codec Feature. 
#First value - Enable/Disable feature, Mandatory 0 - No, 1 - Yes
#Second value - Code numbers
P24659=1
P24600=02

#PCMU codec feature. 
#First value - Enable/Disable feature, Mandatory 0 - No, 1 - Yes
#Second value - Code numbers
P24676=1
P24627=7110

#PCMA codec feature
#First value - Enable/Disable feature, Mandatory 0 - No, 1 - Yes
#Second value - Code numbers
P24677=1
P24628=7111

#G723 codec feature
#First value - Enable/Disable feature, Mandatory 0 - No, 1 - Yes
#Second value - Code numbers
P24678=1
P24629=723

#G729 codec feature
#First value - Enable/Disable feature, Mandatory 0 - No, 1 - Yes
#Second value - Code numbers
P24679=1
P24630=729

#AAL2-G726-R16 codec 
#First value - Enable/Disable feature, Mandatory 0 - No, 1 - Yes
#Second value - Code numbers
P24680=1
P24631=72616

#AAL2-G726-R24 codec feature
#First value - Enable/Disable feature, Mandatory 0 - No, 1 - Yes
#Second value - Code numbers
P24681=1
P24632=72624

#AAL2-G726-R32 codec feature
#First value - Enable/Disable feature, Mandatory 0 - No, 1 - Yes
#Second value - Code numbers
P24682=1
P24633=72632

#AAL2-G726-R40 codec 
#First value - Enable/Disable feature, Mandatory 0 - No, 1 - Yes
#Second value - Code numbers
P24683=1
P24634=72640

#iLBC codec feature
#First value - Enable/Disable feature, Mandatory 0 - No, 1 - Yes
#Second value - Code numbers
P24684=1
P24635=7201

#G722 codec feature
#First value - Enable/Disable feature, Mandatory 0 - No, 1 - Yes
#Second value - Code numbers
P24685=1
P24636=722

################################################################################
#Profile 4-Ring Tones
################################################################################

#Distinctive Ring Tones#########################################################

#Distinctive Ring Tone 
#0 - Ring Tone 1, 1 - Ring Tone 2, 2 - Ring Tone 3, 3 - Ring Tone 4, 4 - Ring Tone 5, 
#5 - Ring Tone 6, 6 - Ring Tone 7, 7 - Ring Tone 8, 8 - Ring Tone 9, 9 - Ring Tone 10
#Distinctive Ring Tone 1
#Number: 0 to 9
#Mandatory
P4400=0

#Choice 1 incoming caller ID
#String Max Length: 64
P4401=

#Distinctive Ring Tone 2
#Number: 0 to 9
#Mandatory
P4402=0

#Choice 2 incoming caller ID
#String Max Length: 64 
P4403=

#Distinctive Ring Tone 3
#Number: 0 to 9
#Mandatory 
P4404=0

#Choice 3 incoming caller ID
#String Max Length: 64
P4405=

#Ring Tone Cadences################################################################################
#Syntax: c=on1/ off1[- on2/ off2[- on3/ off3]];(Cadence on and off are in 10 ms units)

#Ring Tone 1
#String Max Length: 256
P4050=c=2000/4000;

#Ring Tone 2
#String Max Length: 256 
P4051=c=2000/4000;

#Ring Tone 3
#String Max Length: 256 
P4052=c=2000/4000; 

#Ring Tone 4
#String Max Length: 256 
P4053=c=2000/4000;

#Ring Tone 5
#String Max Length: 256
P4054=c=2000/4000;

#Ring Tone 6
#String Max Length: 256 
P4055=c=2000/4000;

#Ring Tone 7
#String Max Length: 256
P4056=c=2000/4000;

#Ring Tone 8
#String Max Length: 256 
P4057=c=2000/4000;

#Ring Tone 9
#String Max Length: 256 
P4058=c=2000/4000; 

#Ring Tone 10
#String Max Length: 256 
P4059=c=2000/4000;

#######################################
# Call Waiting Tones for Profile 4 ####
#######################################

# Distinctive Call Waiting Tones#########################################################

# Distinctive Call Waiting Tone 1
# Number: 0-9
# Mandatory
P29374=0

# Distinctive Call Waiting Tone 2
# Number: 0-9
# Mandatory
P29375=0

# Distinctive Call Waiting Tone 3
# Number: 0-9
# Mandatory
P29376=0

# Distinctive Call Waiting Tone CID matching plan for Tone 1
# Max Length: 64
P29377= 

# Distinctive Call Waiting Tone CID matching plan for Tone 2
# Max Length: 64
P29378= 

# Distinctive Call Waiting Tone CID matching plan for Tone 3
# Max Length: 64
P29379= 

# Call Waiting Tone Cadences#####################################################
# Call Waiting Tone 1 - Call Waiting Tone 10
# Mandatory
P29380=f1=440@-13,c=300/10000-300/10000-0/0;
P29381=f1=440@-13,c=300/10000-300/10000-0/0;
P29382=f1=440@-13,c=300/10000-300/10000-0/0;
P29383=f1=440@-13,c=300/10000-300/10000-0/0;
P29384=f1=440@-13,c=300/10000-300/10000-0/0;
P29385=f1=440@-13,c=300/10000-300/10000-0/0;
P29386=f1=440@-13,c=300/10000-300/10000-0/0;
P29387=f1=440@-13,c=300/10000-300/10000-0/0;
P29388=f1=440@-13,c=300/10000-300/10000-0/0;
P29389=f1=440@-13,c=300/10000-300/10000-0/0;

################################################################################
#FXS Ports
################################################################################

#FXS Port
#SIP USER ID; String Max Length: 64
#Authenticate ID; String Max Length: 64
#Password; String Max Length: 64
#Name; String Max Length: 64
#Profile ID (0 - Profile 1, 1 - Profile 2, 2 - Profile 3, 3 - Profile 4);
#Enable FXS (TR-069) (0 - No, 1 - Yes, default is Yes)

#Offhook Auto-dial; String Max Length: 64 0 to 9,#,*
#Hunting Group (0 - None, 1 - Active, 2~32 - hunting group number 2~32)
#Request URI Routing ID

#Map to FXO Port 
#Map to FXO Gateway IP
#Map to FXO Gateway Port

#FXS 1################################################################################
P4060=
P4090=
P4120=
P4180=
P4150=0
P4595=1

P4210=
P4300=0
P4669=

P4521=1
P4264=
P4858=5060

#FXS 2################################################################################
P4061=
P4091=
P4121=
P4181=
P4151=0
P4596=1

P4211=
P4301=0
P4670=

P4522=1
P4265=
P4859=5060

#FXS 3################################################################################
P4062=
P4092=
P4122=
P4182=
P4152=0
P4597=1

P4212=
P4302=0
P4671=

P4523=1
P4266=
P4860=5060

#FXS 4################################################################################
P4063=
P4093=
P4123=
P4183=
P4153=0
P4598=1

P4213=
P4303=0
P4672=

P4524=1
P4267=
P4861=5060

#FXS 5################################################################################
P4064=
P4094=
P4124=
P4184=
P4154=0
P4599=1

P4214=
P4304=0
P4673=

P4525=1
P4268=
P4862=5060

#FXS 6################################################################################
P4065=
P4095=
P4125=
P4185=
P4155=0
P4600=1

P4215=
P4305=0
P4674=

P4526=1
P4269=
P4863=5060

#FXS 7################################################################################
P4066=
P4096=
P4126=
P4186=
P4156=0
P4601=1

P4216=
P4306=0
P4675=

P4527=1
P4270=
P4864=5060

#FXS 8################################################################################
P4067=
P4097=
P4127=
P4187=
P4157=0
P4602=1

P4217=
P4307=0
P4676=

P4528=1
P4271=
P4865=5060

#FXS 9################################################################################
P4068=
P4098=
P4128=
P4188=
P4158=0
P4603=1

P4218=
P4308=0
P4677=

P4529=1
P4272=
P4866=5060

#FXS 10################################################################################
P4069=
P4099=
P4129=
P4189=
P4159=0
P4604=1

P4219=
P4309=0
P4678=

P4530=1
P4273=
P4867=5060

#FXS 11################################################################################
P4070=
P4100=
P4130=
P4190=
P4160=0
P4605=1

P4220=
P4310=0
P4679=

P4531=1
P4274=
P4868=5060

#FXS 12################################################################################
P4071=
P4101=
P4131=
P4191=
P4161=0
P4606=1

P4221=
P4311=0
P4680=

P4532=1
P4275=
P4869=5060

#FXS 13################################################################################
P4072=
P4102=
P4132=
P4192=
P4162=0
P4607=1

P4222=
P4312=0
P4681=

P4533=1
P4276=
P4870=5060

#FXS 14################################################################################
P4073=
P4103=
P4133=
P4193=
P4163=0
P4608=1

P4223=
P4313=0
P4682=

P4534=1
P4277=
P4871=5060

#FXS 15################################################################################
P4074=
P4104=
P4134=
P4194=
P4164=0
P4609=1

P4224=
P4314=0
P4683=

P4535=1
P4278=
P4872=5060

#FXS 16################################################################################
P4075=
P4105=
P4135=
P4195=
P4165=0
P4610=1

P4225=
P4315=0
P4684=

P4536=1
P4279=
P4873=5060

#FXS 17################################################################################
P4076=
P4106=
P4136=
P4196=
P4166=0
P4611=1

P4226=
P4316=0
P4685=

P4537=1
P4280=
P4874=5060

#FXS 18################################################################################
P4077=
P4107=
P4137=
P4197=
P4167=0
P4612=1

P4227=
P4317=0
P4686=

P4538=1
P4281=
P4875=5060

#FXS 19################################################################################
P4078=
P4108=
P4138=
P4198=
P4168=0
P4613=1

P4228=
P4318=0
P4687=

P4539=1
P4282=
P4876=5060

#FXS 20################################################################################
P4079=
P4109=
P4139=
P4199=
P4169=0
P4614=1

P4229=
P4319=0
P4688=

P4540=1
P4283=
P4877=5060

#FXS 21################################################################################
P4080=
P4110=
P4140=
P4252=
P4170=0
P4615=1

P4230=
P4320=0
P4689=

P4541=1
P4284=
P4878=5060

#FXS 22################################################################################
P4081=
P4111=
P4141=
P4253=
P4171=0
P4616=1

P4231=
P4321=0
P4690=

P4542=1
P4285=
P4879=5060

#FXS 23################################################################################
P4082=
P4112=
P4142=
P4254=
P4172=0
P4617=1

P4232=
P4322=0
P4691=

P4543=1
P4286=
P4880=5060

#FXS 24################################################################################
P4083=
P4113=
P4143=
P4255=
P4173=0
P4618=1

P4233=
P4323=0
P4692=

P4544=1
P4287=
P4881=5060

#FXS 25################################################################################
P4084=
P4114=
P4144=
P4256=
P4174=0
P4619=1

P4800=
P4324=0
P4693=

P4545=1
P4288=
P4882=5060


#FXS 26################################################################################
P4085=
P4115=
P4145=
P4257=
P4175=0
P4620=1

P4801=
P4325=0
P4694=

P4546=1
P4289=
P4883=5060

#FXS 27################################################################################
P4086=
P4116=
P4146=
P4258=
P4176=0
P4621=1

P4802=
P4326=0
P4695=

P4547=1
P4290=
P4884=5060

#FXS 28################################################################################
P4087=
P4117=
P4147=
P4259=
P4177=0
P4622=1

P4803=
P4327=0
P4696=

P4548=1
P4291=
P4885=5060

#FXS 29################################################################################
P4088=
P4118=
P4148=
P4260=
P4178=0
P4623=1

P4804=
P4328=0
P4697=

P4549=1
P4292=
P4886=5060

#FXS 30################################################################################
P4089=
P4119=
P4149=
P4261=
P4179=0
P4624=1

P4805=
P4329=0
P4698=

P4808=1
P4293=
P4887=5060

#FXS 31################################################################################
P4240=
P4242=
P4244=
P4262=
P4246=0
P4625=1

P4806=
P4250=0
P4699=

P4809=1
P4294=
P4888=5060

#FXS 32################################################################################
P4241=
P4243=
P4245=
P4263=
P4247=0
P4626=1

P4807=
P4251=0
P4700=

P4810=1
P4295=
P4889=5060

#FXS 33################################################################################
P21000=
P21064=
P21128=
P21192=
P21256=0
P21384=1

P21448=
P21320=0
P21704=

P21512=1
P21576=
P21640=5060

#FXS 34################################################################################
P21001=
P21065=
P21129=
P21193=
P21257=0
P21385=1

P21449=
P21321=0
P21705=

P21513=1
P21577=
P21641=5060

#FXS 35################################################################################
P21002=
P21066=
P21130=
P21194=
P21258=0
P21386=1

P21450=
P21322=0
P21706=

P21514=1
P21578=
P21642=5060

#FXS 36################################################################################
P21003=
P21067=
P21131=
P21195=
P21259=0
P21387=1

P21451=
P21323=0
P21707=

P21515=1
P21579=
P21643=5060

#FXS 37################################################################################
P21004=
P21068=
P21132=
P21196=
P21260=0
P21388=1

P21452=
P21324=0
P21708=

P21516=1
P21580=
P21644=5060

#FXS 38################################################################################
P21005=
P21069=
P21133=
P21197=
P21261=0
P21389=1

P21453=
P21325=0
P21709=

P21517=1
P21581=
P21645=5060

#FXS 39################################################################################
P21006=
P21070=
P21134=
P21198=
P21262=0
P21390=1

P21454=
P21326=0
P21710=

P21518=1
P21582=
P21646=5060

#FXS 40################################################################################
P21007=
P21071=
P21135=
P21199=
P21263=0
P21391=1

P21455=
P21327=0
P21711=

P21519=1
P21583=
P21647=5060

#FXS 41################################################################################
P21008=
P21072=
P21136=
P21200=
P21264=0
P21392=1

P21456=
P21328=0
P21712=

P21520=1
P21584=
P21648=5060

#FXS 42################################################################################
P21009=
P21073=
P21137=
P21201=
P21265=0
P21393=1

P21457=
P21329=0
P21713=

P21521=1
P21585=
P21649=5060

#FXS 43################################################################################
P21010=
P21074=
P21138=
P21202=
P21266=0
P21394=1

P21458=
P21330=0
P21714=

P21522=1
P21586=
P21650=5060

#FXS 44################################################################################
P21011=
P21075=
P21139=
P21203=
P21267=0
P21395=1

P21459=
P21331=0
P21715=

P21523=1
P21587=
P21651=5060

#FXS 45################################################################################
P21012=
P21076=
P21140=
P21204=
P21268=0
P21396=1

P21460=
P21332=0
P21716=

P21524=1
P21588=
P21652=5060

#FXS 46################################################################################
P21013=
P21077=
P21141=
P21205=
P21269=0
P21397=1

P21461=
P21333=0
P21717=

P21525=1
P21589=
P21653=5060

#FXS 47################################################################################
P21014=
P21078=
P21142=
P21206=
P21270=0
P21398=1

P21462=
P21334=0
P21718=

P21526=1
P21590=
P21654=5060

#FXS 48################################################################################
P21015=
P21079=
P21143=
P21207=
P21271=0
P21399=1

P21463=
P21335=0
P21719=

P21527=1
P21591=
P21655=5060

##############################################################################
## Telnet P values                                                          ##
##############################################################################
#Ping/traceroute tool destination IP/URL
#IP address or URL
#P22005=

##############################################################################
## P values not on WEB                                                      ##
##############################################################################
#TTL values for keep alive messages
#Number: 1 to 255
#P20517=64(FXS1)
#P20518=64(FXS2)
