################################################################################################
##                General Configuration Template for GDS3705 Door System         			  ##
##                        (Firmware Version:   1.0.1.11)                                      ##
################################################################################################

################################################################################################
##                              Door System Settings                                          ##
################################################################################################
	##### Door Relay Options #####
	## P15440
	## value: 0/1 (0:Loacl Relay  1: WebRelay)
	
	##### Webrelay IP Adress #####
	## P15441
	## value: string, MAX length is 255
	
	##### Webrelay Username #####
	## P15442
	## value: string, MAX length is 128
	
	##### Webrelay Password #####
	## P15443
	## value: string, MAX length is 128
	
	##### ALMOUT1 Feature #####
	## P15450
	## value: 0/1 (0:Alarm Output  1: Open Door)
	
	##### ALMOUT1 Status #####
	## P15470
	## value: 0/1 (0:Normal Close  1: Normal Open (Default))
	
	##### Control Options #####
	## P15467
	## value: 0/1/2/3 (0: Door1  1:Door2  2:Door1 & Door2  3:None)
	
	##### Wiegand Control Options #####
	## P15468
	## value: 0/1/2/3 (0: Door1  1:Door2  2:Door1 & Door2  3:None)
	
	##### Delay before Unlock Action(s) #####
	## P14100
	## value: 0 - 20 (Integer)
	
	##### Door 2 Delay before Unlock(s) #####
	## P15465
	## value: 0 - 20 (Integer)
	
	##### Unlock Action Holding Time(s) #####
	## P14101
	## value: 0 - 1800 (Integer)
	
	##### Door 2 Unlock Action Holding Time(s) #####
	## P15466
	## value: 0 - 1800 (Integer)
	
	##### Min. Interval of Swiping Card(ms) #####
	## P14829
	## value: 0 - 2000 (Integer)
	
	##### No Key Input Timeout(s) #####
	## P15436
	## value: 1 - 15 (Integer)
	
	##### Call Mode #####
	## P14856
	## value: 0/1 (0:Virtual Number 1:SIP Number)
	
	##### Doorbell Mode #####
	## P14827
	## value: 0/1/2 (0:Call Doorbell Number 1:Control Doorbell Output 2:Both of the above)
	
	##### Doorbell Call Out Account #####
	## P10470
	## value: 0/1/2/3/4 (0:auto N>0: account N)
	
	##### Door Bell Call Mode #####
	## P15434
	## value: 0/1/2  (0:Serial Hunting 1:Parallel Hunting)
	
	##### Number Called When Door Bell Pressed #####
	## P10462
	## value: A pure digital string. Example: 6688
	
	##### Press Doorbell Schedule #####
	## P15418
	## value: 0 - 10 (Integer)
	
	##### Maximum Number of Dialed Digits #####
	## P15419
	## value: 0 - 20 (Integer)
	
	##### Remote PIN to Open the Door1 #####
	## P10457
	## value: A pure digital string, MAX length is 8. Example: 6688
	
	##### Remote PIN to Open the Door2 #####
	## P15460
	## value: A pure digital string, MAX length is 8. Example: 6688
	
	##### Local PIN to Open Door Schedule #####
	## P15498
	## value: 0 - 10 (Integer)
	
	##### Remote PIN to Open the Door2 #####
	## P10460
	## value: A pure digital string, MAX length is 8. Example: 6688
	
	##### Local PIN Type #####
	## P10464
	## value: 0/1/2 (0:Private Card PIN  1:Unified PIN  2:Card + Private PIN)
	
	##### Unified PIN Open Door Option #####
	## 15461
	## value: 0/1/2/3 (0: Door1  1: Door2  2: Door1 & Door2 3:None)
	
	##### Guest PIN Open Door Option #####
	## 15462
	## value: 0/1/2/3 (0: Door1  1: Door2  2: Door1 & Door2 3:None)
	
	##### Local PIN to Open the Door #####
	## P10463
	## value: A pure digital string, MAX length is 8. Example: 6688
	
	##### Enable Guest PIN #####
	## P14850
	## value: 0/1 (0:Disable  1:Enable)

	##### Guest PIN #####
	## P14851
	## value: A pure digital string, MAX length is 8. Example: 6688
	
	##### Guest PIN Duration Start Time #####
	## P14852
	## value: A pure digital string, Example: 2017/02/28 02:31:56 value:20170228023156
	
	##### Guest PIN Duration End Time #####
	## P14853
	## value: A pure digital string, Example: 2017/02/28 02:31:56 value:20170228023156
	
	##### Disable Auto Answer #####
	## P14580
	## value: 0/1 	(0:Disable  1:Enable)
	
	##### Enable Doorbell Button to Hang Up Call #####
	## P14582
	## value: 0/1 	(0:Disable  1:Enable)
	
	##### Disable Keypad (except Doorbell Button) #####
	## P15421
	## value: 0/1 	(0:Disable  1:Enable)
	
	##### Enable On Hook After Remote Unlock #####
	## P15422
	## value: 0/1 	(0:Disable  1:Enable)
	
	##### Enable DTMF Open Door #####
	## P14858
	## value: 0/1 	(0:Disable  1:Enable)
	
	##### Card Issuing State Expire Time(m) #####
	## P15423
	## value: 1 - 1440
	
	##### Enable Key Blue Light #####
	## P14800
	## value: 0/1 	(0:Disable  1:Enable)
	
	##### Enable Blue Doorbell Light #####
	## P14562
	## value: 0/1	(0:Disable  1:Enable)
	
	##### Blue Doorbell Light Lighting Start Time #####
	## P14560
	## value: A pure digital string, MAX length is 6. Example: 125900 -> 12:59:00
	
	##### Blue Doorbell Light Lighting End Time #####
	## P14561
	## value: A pure digital string, MAX length is 6. Example: 125900 -> 12:59:00
	
	##### Central Mode #####
	## P15301
	## value: 0/1	(0:Disable  1:Enable)
	
	##### Key Tone Type #####
	## P14340
	## value: 0/1/2	(0:Default 1:DTMF 2:Mute)

	##### Wiegand Input Enable #####
	## P14120
	## value: 0/1	(0:Disable  1:Enable)
	
	##### Wiegand Output #####
	## P14121
	## value: 0/1/2	(0:Disabled  1:Relay and  Local Authentication  2:Relay and Bypass Local)
	
	##### Enable HTTP API Remote Open Door #####
	## P15424
	## value: 0/1	(0:Disabled  1:Enable)
	
	##### Disable Keypad SIP Number Dialing #####
	## P15433
	## value: 0/1	(0:Disabled  1:Enable)
	
	######################################  Group Settings   ######################################
	##### Group string #####
	## P15300
	## value: Format:index@scheduleX@name. Example:1@1@info,2@1@test,
	
	
	######################################  Schedule Settings   ######################################
	##### Schedule string 0 #####
	## P15200
	## value: Format: name@holiday_mode,weekday@start_time@end_time,weekday@start_time@end_time,
	## Example: rest@0,0@1200@1300,
	
	##### Schedule string 1 #####
	## P15201
	## value: Format: name@holiday_mode,weekday@start_time@end_time,weekday@start_time@end_time,
	## Example: rest@0,0@1200@1300,
	
	##### Schedule string 2 #####
	## P15202
	## value: Format: name@holiday_mode,weekday@start_time@end_time,weekday@start_time@end_time,
	## Example: rest@0,0@1200@1300,
	
	##### Schedule string 3 #####
	## P15203
	## value: Format: name@holiday_mode,weekday@start_time@end_time,weekday@start_time@end_time,
	## Example: rest@0,0@1200@1300,
	
	##### Schedule string 4 #####
	## P15204
	## value: Format: name@holiday_mode,weekday@start_time@end_time,weekday@start_time@end_time,
	## Example: rest@0,0@1200@1300,
	
	##### Schedule string 5 #####
	## P15205
	## value: Format: name@holiday_mode,weekday@start_time@end_time,weekday@start_time@end_time,
	## Example: rest@0,0@1200@1300,
	
	##### Schedule string 6 #####
	## P15206
	## value: Format: name@holiday_mode,weekday@start_time@end_time,weekday@start_time@end_time,
	## Example: rest@0,0@1200@1300,
	
	##### Schedule string 7 #####
	## P15207
	## value: Format: name@holiday_mode,weekday@start_time@end_time,weekday@start_time@end_time,
	## Example: rest@0,0@1200@1300,
	
	##### Schedule string 8 #####
	## P15208
	## value: Format: name@holiday_mode,weekday@start_time@end_time,weekday@start_time@end_time,
	## Example: rest@0,0@1200@1300,
	
	##### Schedule string 9 #####
	## P15209
	## value: Format: name@holiday_mode,weekday@start_time@end_time,weekday@start_time@end_time,
	## Example: rest@0,0@1200@1300,
	
	
	######################################  Holiday Settings   ######################################
	##### Holiday string 1 #####
	## P15250
	## value: Format: name,start_date@end_date, Example: hahaha,20170708@20170910,
	
	##### Holiday string 2 #####
	## P15251
	## value: Format: name,start_date@end_date, Example: hahaha,20170708@20170910,
	
	##### Holiday string 3 #####
	## P15252
	## value: Format: name,start_date@end_date, Example: hahaha,20170708@20170910,
	
	##### Holiday string 4 #####
	## P15253
	## value: Format: name,start_date@end_date, Example: hahaha,20170708@20170910,
	
	##### Holiday string 5 #####
	## P15254
	## value: Format: name,start_date@end_date, Example: hahaha,20170708@20170910,
	
	##### Holiday string 6 #####
	## P15255
	## value: Format: name,start_date@end_date, Example: hahaha,20170708@20170910,
	
	##### Holiday string 7 #####
	## P15256
	## value: Format: name,start_date@end_date, Example: hahaha,20170708@20170910,
	
	##### Holiday string 8 #####
	## P15257
	## value: Format: name,start_date@end_date, Example: hahaha,20170708@20170910,
	
	##### Holiday string 9 #####
	## P15258
	## value: Format: name,start_date@end_date, Example: hahaha,20170708@20170910,
	
	##### Holiday string 10 #####
	## P15259
	## value: Format: name,start_date@end_date, Example: hahaha,20170708@20170910,
	
################################################################################################
##                              System Settings                                               ##
################################################################################################	

######			    			  Date & Time 											  ######	

# TimeZone
# 1  --GMT-12 		(Eniwetok, Kwajalein)
# 2  --GMT-11 		(Midway Isl., Samoa)
# 3  --GMT-10 		(Hawaii, Aleutian Isl.)
# 4  --GMT-09  		(Alaska)
# 5  --GMT-08  		(Las Vegas, San Francisco, Vancouver)
# 6  --GMT-07  		(Calgary, Denver, Salt Lake City)
# 7  --GMT-06  		(Chicago, Dallas, Mexico City)
# 8  --GMT-05  		(Cuba)
# 9  --GMT-05  		(New York, Toronto, Washington DC)
# 10 --GMT-04  		(Paraguay)
# 11 --GMT-04  		(Chile)
# 12 --GMT-04  		(Charlottetown, Manaus)
# 55 --GMT-04  		(Charlottetown, Manaus)
# 13 --GMT-03  		(Brazilia, Sao Paulo)
# 14 --GMT-02  		(Noronha, Mid-Atlantic)
# 15 --GMT-01  		(Azores, Cap Verde Isl.)
# 16 --GMT-00  		(Dublin, Lisbon, London, Reykjavik)
# 17 --GMT+01  		(Amsterdam, Berlin, Rome, Stockholm)
# 18 --GMT+02  		(Athens, Helsinki, Istanbul, Riga)
# 19 --GMT+02  		(Egypt)
# 20 --GMT+02  		(Israel)
# 21 --GMT+02  		(Lebanon)
# 22 --GMT+02  		(Syria)
# 23 --GMT+03  		(Moscow, Riyadh)
# 24 --GMT+03  		(Iraq)
# 25 --GMT+03:30  	(Iran)
# 26 --GMT+04  		(Abu Dubai, Baku)
# 27 --GMT+04:30  	(Kabul)
# 28 --GMT+05  		(Islamabad, Karachi, Tashkent)
# 29 --GMT+05:30  	(Bombay, Calcutta, New Delhi)
# 30 --GMT+06  		(Novosibirsk, Omsk)
# 31 --GMT+07  		(Bangkok, Hanoi, Jakarta)
# 32 --GMT+08  		(Beijing, Hong Kong, Shanghai, Taipei, Taiwan)
# 33 --GMT+09  		(Osaka, Sapporo, Tokyo)
# 34 --GMT+09:30  	(Adelaide, Darwin)
# 35 --GMT+10 		(Hobart)
# 36 --GMT+10 		(Canberra, Melbourne, Sydney)
# 37 --GMT+11 		(Solomon Isl.)
# 38 --GMT+12 		(Auckland, Wellington)
# 56 --GMT+13 		(Auckland, Wellington)

	##### Time Zone #####
	## P64
	## value: TimeZone option	(Integer)
	
	##### Allow DHCP Option 42 to override NTP server #####
	## P144
	## value: 0/1 (0:Disable  1:Enable)
	
	
	##### Enable Daylight Saving Time #####
	## P10004
	## value: 0/1	(0:Disable  1:Enable)
	
	##### Enable NTP #####
	## P5006
	## value: 0/1	(0:Disable  1:Enable)
	
	##### NTP Server #####
	## P30
	## value: String and MAX length is 255 .
	
	##### DST #####
	## P10005
	## value: DST string.
	
	##### Update Interval(m) #####
	## P10006
	## value: 60 - 1440 (Integer)

######			    			  Network Settings 									  ######	

	##### IP Address Mode #####
	## P8
	## value: 0/1 (0:DHCP  1:Static IP)
	
	##### IP Address segment1 #####
	## P9
	## value: 0 - 255 (Integer)
	
	##### IP Address segment2 #####
	## P10
	## value: 0 - 255 (Integer)
	
	##### IP Address segment3 #####
	## P11
	## value: 0 - 255 (Integer)
	
	##### IP Address segment4 #####
	## P12
	## value: 0 - 255 (Integer)
	
	##### Subnet Mask segment1 #####
	## P13
	## value: 0 - 255 (Integer)
	
	##### Subnet Mask segment2 #####
	## P14
	## value: 0 - 255 (Integer)
	
	##### Subnet Mask segment3 #####
	## P15
	## value: 0 - 255 (Integer)
	
	##### Subnet Mask segment4 #####
	## P16
	## value: 0 - 255 (Integer)

	##### Gateway segment1 #####
	## P17
	## value: 0 - 255 (Integer)
	
	##### Gateway segment2 #####
	## P18
	## value: 0 - 255 (Integer)
	
	##### Gateway segment3 #####
	## P19
	## value: 0 - 255 (Integer)
	
	##### Gateway segment4 #####
	## P20
	## value: 0 - 255 (Integer)

	##### DNS Address Type #####
	## P10107
	## value: 0/1	(0:Dynamic  1:Static DNS)

	##### DNS Server 1 segment1 #####
	## P21
	## value: 0 - 255 (Integer)
	
	##### DNS Server 1 segment2 #####
	## P22
	## value: 0 - 255 (Integer)
	
	##### DNS Server 1 segment3 #####
	## P23
	## value: 0 - 255 (Integer)
	
	##### DNS Server 1 segment4 #####
	## P24
	## value: 0 - 255 (Integer)
	
	##### DNS Server 2 segment1 #####
	## P25
	## value: 0 - 255 (Integer)
	
	##### DNS Server 2 segment2 #####
	## P26
	## value: 0 - 255 (Integer)
	
	##### DNS Server 2 segment3 #####
	## P27
	## value: 0 - 255 (Integer)
	
	##### DNS Server 2 segment4 #####
	## P28
	## value: 0 - 255 (Integer)
	
	##### LLDP Enable #####
	## P1684
	## value: 0/1	(0:Disable  1:Enable)
	
	##### Enable VLAN #####
	## P27004
	## value: 0/1	(0:Disable  1:Enable)
	
	##### Layer 2 QoS 802.1Q/VLAN Tag #####
	## P51
	## value: 0 - 4094 (Integer)
	
	##### Layer 2 QoS 802.1p Priority Value #####
	## P87
	## value: 0 - 7 (Integer)
	
	##### Layer 2 QoS 802.1p Priority Value for SIP signaling #####
	## P5038
	## value: 0 - 7 (Integer)
	
	##### Layer 2 QoS 802.1p Priority Value for RTP media #####
	## P5042
	## value: 0 - 7 (Integer)
	
######			 			Access Settings 					######

	##### Web Connection Mode #####
	## P12054
	## value: 0/1	(0:HTTP  1:HTTPS)
	
	##### Web Access Port #####
	## P901
	## value: 80 - 65535	(Integer)
	
	##### User Login Timeout(min) #####
	## P12056
	## value: 3 - 60 (Integer)
	
	##### Max Times Consecutively Login Error #####
	## P14832
	## value: 3 - 10 (Integer)
	
	##### Login Error Lock Time (min) #####
	## P14834
	## value: 3 - 10 (Integer)
	
	##### Disable Web Access #####
	## P15473
	## value: 0/1	(0:No  1:Yes)

	##### Enable UPnP Discovery #####
	## P12053
	## value: 0/1	(0:Disable  1:Enable)
	
	##### Enable SSH  #####
	## P276 
	## value: 0/1	(0:Disable  1:Enable)
	
	##### SSH Port   #####
	## P27006
	## value: 22 or 444-65535, default 22
	
######			 			User Management 					######
	##### admin PW  #####
	## P2
	## value: String (Rule: [^!#%(-*,.0-9=@-Z_-z|~&*]) Max.length=32
	
################################################################################################
##                                 SIP Settings                                               ##
################################################################################################	

	#Account 1 Settings
	
	##### Account Active #####
	## P271
	## value: 0/1	(0:No  1:Yes)
	
	##### Account Name #####
	## P3
	## value: String & MAX length is 64
	
	##### SIP Server #####
	## P47
	## value: String & MAX length is 64
	
	##### Secondary SIP Server #####
	## P2312
	## value: String & MAX length is 255
	
	##### Outbound Proxy #####
	## P48
	## value: String & MAX length is 255
	
	##### Backup Outbound Proxy #####
	## P2333
	## value: String & MAX length is 255
	
	##### DNS Mode #####
	## P103
	## value: 0/1/2£¨0:A Record  1:SRV  2:NAPTR/SRV£©
	
	##### SIP User ID #####
	## P35
	## value: String & MAX length is 255
	
	##### Authenticate ID #####
	## P36
	## value: String & MAX length is 255
	
	##### SIP Authenticate Password  #####
	## P34
	## value: String & MAX length is 255
	
	##### TEL URI #####
	## P63
	## value: 0/1/2 (0:Disabled 1:User=phone 2:Enabled)
	
	##### Register Expiration(m)  #####
	## P32
	## value: 60~64800 (default:3600)
	
	##### Re-register before Expiration(s)  #####
	## P2330
	## value: 60~64800 (default:0)
	
	
	##### Local SIP Port  #####
	## P40
	## value:1~65535 && != 6789 && no conflict others
	
	##### SIP Transport  #####
	## P130
	## value: 0/1/2 (0:UDP  1:TCP  2:TLS/TCP)
	
	##### RFC2833  #####
	## P2302
	## value: 0/1  (0:Disable  1:Enable)
	
	##### SIP INFO #####
	## P2303 
	## value: 0/1   (0:Disable  1:Enable)
	
	##### DTMF Payload Type   #####
	## P79
	## value: 96-127 (default:101)
	
	##### Enable Keep Alive  #####
	## P490
	## value: 0/1  (0:Disable  1:Enable)
	
	##### Unregister On Reboot  #####
	## P81
	## value: 0/1  (0:Disable  1:Enable)
	
	##### NAT Traversal  #####
	## P52
	## value: 0/1/2/3/4/5   (0:no  1:STUN  2:Keep Alive  3:UPnP  4:Auto  5:VPN)
	
	##### Enable SRTP  #####
	## P183 
	## value: 0/1  (0:Disable  1:Enable)
	
	##### Special Feature  #####
	## P198
	## value: 100/102   (100:Standard  102:Broadsoft 129:Telefonica Spain)
	
	##### Outbound Proxy Mode  #####
	## P2305
	## value: 0/1/2   (0:in route  1:not in route  2:always send to)
	
	##### Validate Incoming Messages  #####
	## P2306
	## value: 0/1   (0:No  1:Yes)
	
	##### Enable RTCP  #####
	## P2392
	## value: 0/1   (0:No  1:Yes)
	
	##### Preferred Vocoder 1  #####
	## P57
	## value: 0/8/9/18   (0:PCMU  8:PCMA  9:G.722  18:G.729A/B)
	
	##### Preferred Vocoder 1  #####
	## P58
	## value: 0/8/9/18   (0:PCMU  8:PCMA  9:G.722  18:G.729A/B)
	
	##### Preferred Vocoder 1  #####
	## P59
	## value: 0/8/9/18   (0:PCMU  8:PCMA  9:G.722  18:G.729A/B)
	
	##### Preferred Vocoder 1  #####
	## P60
	## value: 0/8/9/18   (0:PCMU  8:PCMA  9:G.722  18:G.729A/B)
	
	
	##### Voice Frames Per TX   #####
	## P37
	## value: 1~64
	
	
	#Account 2 Settings
	##### Account Active #####
	## P401
	## value: 0/1	(0:No  1:Yes)
	
	##### Account Name #####
	## P407
	## value: String & MAX length is 64
	
	##### SIP Server #####
	## P402
	## value: String & MAX length is 64
	
	##### Secondary SIP Server #####
	## P2412
	## value: String & MAX length is 255
	
	##### Outbound Proxy #####
	## P403
	## value: String & MAX length is 255
	
	##### Backup Outbound Proxy #####
	## P2433
	## value: String & MAX length is 255
	
	##### DNS Mode #####
	## P408
	## value: 0/1/2£¨0:A Record  1:SRV  2:NAPTR/SRV£©
	
	##### SIP User ID #####
	## P404
	## value: String & MAX length is 255
	
	##### Authenticate ID #####
	## P405
	## value: String & MAX length is 255
	
	##### SIP Authenticate Password  #####
	## P406
	## value: String & MAX length is 255
	
	##### TEL URI #####
	## P409
	## value: 0/1/2 (0:Disabled 1:User=phone 2:Enabled)
	
	##### Register Expiration(m)  #####
	## P412
	## value: 60~64800 (default:3600)
	
	##### Re-register before Expiration(s)  #####
	## P2430
	## value: 60~64800 (default:0)
	
	##### Local SIP Port  #####
	## P413
	## value:1~65535 && != 6789 && no conflict others
	
	##### SIP Transport  #####
	## P448
	## value: 0/1/2 (0:UDP  1:TCP  2:TLS/TCP)
	
	##### RFC2833  #####
	## P2402
	## value: 0/1  (0:Disable  1:Enable)
	
	##### SIP INFO #####
	## P2403 
	## value: 0/1   (0:Disable  1:Enable)

  ##### DTMF Payload Type   #####
	## P496
	## value: 96-127 (default:101)
	
	##### Enable Keep Alive  #####
	## P1309
	## value: 0/1  (0:Disable  1:Enable)
	
	##### Unregister On Reboot  #####
	## P411
	## value: 0/1  (0:Disable  1:Enable)
	
	##### NAT Traversal  #####
	## P414
	## value: 0/1/2/3/4/5   (0:no  1:STUN  2:Keep Alive  3:UPnP  4:Auto  5:VPN)
	
	##### Enable SRTP  #####
	## P443 
	## value: 0/1  (0:Disable  1:Enable)
	
	##### Special Feature  #####
	## P424
	## value: 100/102   (100:Standard  102:Broadsoft 129:Telefonica Spain)
	
	##### Outbound Proxy Mode  #####
	## P2405
	## value: 0/1/2   (0:in route  1:not in route  2:always send to)
	
	##### Validate Incoming Messages  #####
	## P2406
	## value: 0/1   (0:No  1:Yes)
	
	##### Enable RTCP  #####
	## P2492
	## value: 0/1   (0:No  1:Yes)
	
	##### Preferred Vocoder 1  #####
	## P451
	## value: 0/8/9/18   (0:PCMU  8:PCMA  9:G.722  18:G.729A/B)
	
	##### Preferred Vocoder 1  #####
	## P452
	## value: 0/8/9/18   (0:PCMU  8:PCMA  9:G.722  18:G.729A/B)
	
	##### Preferred Vocoder 1  #####
	## P453
	## value: 0/8/9/18   (0:PCMU  8:PCMA  9:G.722  18:G.729A/B)
	
	##### Preferred Vocoder 1  #####
	## P454
	## value: 0/8/9/18   (0:PCMU  8:PCMA  9:G.722  18:G.729A/B)
	
	##### Voice Frames Per TX   #####
	## P486
	## value: 1~64
	
		
	#Account 3 Settings
	
	##### Account Active #####
	## P501
	## value: 0/1	(0:No  1:Yes)
	
	##### Account Name #####
	## P507
	## value: String & MAX length is 64
	
	##### SIP Server #####
	## P502
	## value: String & MAX length is 64
	
	##### Secondary SIP Server #####
	## P2512
	## value: String & MAX length is 255
	
	##### Outbound Proxy #####
	## P503
	## value: String & MAX length is 255
	
	##### Backup Outbound Proxy #####
	## P2533
	## value: String & MAX length is 255
	
	##### DNS Mode #####
	## P508
	## value: 0/1/2£¨0:A Record  1:SRV  2:NAPTR/SRV£©
	
	##### SIP User ID #####
	## P504
	## value: String & MAX length is 255
	
	##### Authenticate ID #####
	## P505
	## value: String & MAX length is 255
	
	##### SIP Authenticate Password  #####
	## P506
	## value: String & MAX length is 255
	
	##### TEL URI #####
	## P509
	## value: 0/1/2 (0:Disabled 1:User=phone 2:Enabled)
	
	##### Register Expiration(m)  #####
	## P512
	## value: 60~64800 (default:3600)
	
	##### Re-register before Expiration(s)  #####
	## P2530
	## value: 60~64800 (default:0)
	
	##### Local SIP Port  #####
	## P513
	## value:1~65535 && != 6789 && no conflict others
	
	##### SIP Transport  #####
	## P548
	## value: 0/1/2 (0:UDP  1:TCP  2:TLS/TCP)
	
	##### RFC2833  #####
	## P2502
	## value: 0/1  (0:Disable  1:Enable)
	
	##### SIP INFO #####
	## P2503 
	## value: 0/1   (0:Disable  1:Enable)
	
	##### DTMF Payload Type   #####
	## P596
	## value: 96-127 (default:101)
	
	##### Enable Keep Alive  #####
	## P590
	## value: 0/1  (0:Disable  1:Enable)
	
	##### Unregister On Reboot  #####
	## P511
	## value: 0/1  (0:Disable  1:Enable)
	
	##### NAT Traversal  #####
	## P514
	## value: 0/1/2/3/4/5   (0:no  1:STUN  2:Keep Alive  3:UPnP  4:Auto  5:VPN)
	
	##### Enable SRTP  #####
	## P543 
	## value: 0/1  (0:Disable  1:Enable)
	
	##### Special Feature  #####
	## P524
	## value: 100/102   (100:Standard  102:Broadsoft 129:Telefonica Spain)
	
	##### Outbound Proxy Mode  #####
	## P2505
	## value: 0/1/2   (0:in route  1:not in route  2:always send to)
	
	##### Validate Incoming Messages  #####
	## P2506
	## value: 0/1   (0:No  1:Yes)
	
	##### Enable RTCP  #####
	## P2592
	## value: 0/1   (0:No  1:Yes)
	
	##### Preferred Vocoder 1  #####
	## P551
	## value: 0/8/9/18   (0:PCMU  8:PCMA  9:G.722  18:G.729A/B)
	
	##### Preferred Vocoder 1  #####
	## P552
	## value: 0/8/9/18   (0:PCMU  8:PCMA  9:G.722  18:G.729A/B)
	
	##### Preferred Vocoder 1  #####
	## P553
	## value: 0/8/9/18   (0:PCMU  8:PCMA  9:G.722  18:G.729A/B)
	
	##### Preferred Vocoder 1  #####
	## P554
	## value: 0/8/9/18   (0:PCMU  8:PCMA  9:G.722  18:G.729A/B)
	
	##### Voice Frames Per TX   #####
	## P586
	## value: 1~64
		
	#Account 4 Settings
	
	##### Account Active #####
	## P601
	## value: 0/1	(0:No  1:Yes)
	
	##### Account Name #####
	## P607
	## value: String & MAX length is 64
	
	##### SIP Server #####
	## P602
	## value: String & MAX length is 64
	
	##### Secondary SIP Server #####
	## P2612
	## value: String & MAX length is 255
	
	##### Outbound Proxy #####
	## P603
	## value: String & MAX length is 255
	
	##### Backup Outbound Proxy #####
	## P2633
	## value: String & MAX length is 255
	
	##### DNS Mode #####
	## P608
	## value: 0/1/2£¨0:A Record  1:SRV  2:NAPTR/SRV£©
	
	##### SIP User ID #####
	## P604
	## value: String & MAX length is 255
	
	##### Authenticate ID #####
	## P605
	## value: String & MAX length is 255
	
	##### SIP Authenticate Password  #####
	## P606
	## value: String & MAX length is 255
	
	##### TEL URI #####
	## P609
	## value: 0/1/2 (0:Disabled 1:User=phone 2:Enabled)
	
	##### Register Expiration(m)  #####
	## P612
	## value: 60~64800 (default:3600)
	
	##### Re-register before Expiration(s)  #####
	## P2630
	## value: 60~64800 (default:0)
	
	##### Local SIP Port  #####
	## P613
	## value:1~65535 && != 6789 && no conflict others
	
	##### SIP Transport  #####
	## P648
	## value: 0/1/2 (0:UDP  1:TCP  2:TLS/TCP)
	
	##### RFC2833  #####
	## P2602
	## value: 0/1  (0:Disable  1:Enable)
	
	##### SIP INFO #####
	## P2603 
	## value: 0/1   (0:Disable  1:Enable)
	
	##### DTMF Payload Type   #####
	## P696
	## value: 96-127 (default:101)
	
	##### Enable Keep Alive  #####
	## P690
	## value: 0/1  (0:Disable  1:Enable)
	
	##### Unregister On Reboot  #####
	## P611
	## value: 0/1  (0:Disable  1:Enable)
	
	##### NAT Traversal  #####
	## P614
	## value: 0/1/2/3/4/5   (0:no  1:STUN  2:Keep Alive  3:UPnP  4:Auto  5:VPN)
	
	##### Enable SRTP  #####
	## P643 
	## value: 0/1  (0:Disable  1:Enable)
	
	##### Voice Frames Per TX   #####
	## P686
	## value: 1~64
	
	##### Special Feature  #####
	## P624
	## value: 100/102   (100:Standard  102:Broadsoft 129:Telefonica Spain)
	
	
	##### Outbound Proxy Mode  #####
	## P2605
	## value: 0/1/2   (0:in route  1:not in route  2:always send to)
	
	##### Validate Incoming Messages  #####
	## P2606
	## value: 0/1   (0:No  1:Yes)
	
	##### Enable RTCP  #####
	## P2692
	## value: 0/1   (0:No  1:Yes)
	
	##### Preferred Vocoder 1  #####
	## P651
	## value: 0/8/9/18   (0:PCMU  8:PCMA  9:G.722  18:G.729A/B)
	
	##### Preferred Vocoder 1  #####
	## P652
	## value: 0/8/9/18   (0:PCMU  8:PCMA  9:G.722  18:G.729A/B)
	
	##### Preferred Vocoder 1  #####
	## P653
	## value: 0/8/9/18   (0:PCMU  8:PCMA  9:G.722  18:G.729A/B)
	
	##### Preferred Vocoder 1  #####
	## P654
	## value: 0/8/9/18   (0:PCMU  8:PCMA  9:G.722  18:G.729A/B)
		
	#Phone Settings
	
	##### STUN Server  #####
	## P76
	## value: String & MAX length is 255
	
	##### Local RTP Port  #####
	## P39
	## value:1024~65400 && != 6789 && no conflict others
	
	##### Local RTP Port Range  #####
	## P29610
	## value: 48~10000
	
	##### Use Random Port  #####
	## P78
	## value: 0/1 (0:Disable  1:Enable)
	
	##### Auto On-Hook Timer(s)  #####
	## P10451
	## value: 0~65535
	
	##### Ring Timeout(s)  #####
	## P14847
	## value: 0~90
	
	##### DNS Cache Expiration Time(m)  #####
	## P4208
	## value: 1 - 1440
	
	##### DNS Cache Duration(m)  #####
	## P28160
	## value: 1 - 1440
	
	##### SIP TLS Certificate  #####
	## P280
	## value: String & MAX length is 4096
	
	##### SIP TLS Private Key  #####
	## P279
	## value: String & MAX length is 4096
	
	##### SIP TLS Private Key Password  #####
	## P281
	## value: String & MAX length is 4096
	
	##### Enable Direct IP Call  #####
	## P10453
	## value: 0/1  (0:Disable  1:Enable)
	
	##### Enable two-way SIP Calling  #####
	## P8001
	## value: 0/1  (0:Disable  1:Enable)
	
	##### SIP Proxy Compatibility Mode  #####
	## P8003
	## value: 0/1  (0:Disable  1:Enable)
	
	##### Allow Reset Via SIP NOTIFY  #####
	## P15476
	## value: 0/1  (0:No  1:Yes)
	
	<!-- Account 1 White List -->	
	##### Enable White Number List  #####
	## P10410
	## value: 0/1  (0:Disable  1:Enable)
	
	##### sip white phone number list  #####
	## P10411
	## value: String. (Format:123,4567,)
	
	<!-- Account 2 White List -->
	##### Enable White Number List  #####
	## P10454
	## value: 0/1  (0:Disable  1:Enable)
	
	##### sip white phone number list  #####
	## P10460
	## value: String. (Format:123,4567,)
		
	<!-- Account 3 White List -->	
	##### Enable White Number List  #####
	## P10420
	## value: 0/1  (0:Disable  1:Enable)
	
	##### sip white phone number list  #####
	## P10421
	## value: String. (Format:123,4567,)
	
	<!-- Account 4 White List -->
	##### Enable White Number List  #####
	## P10430
	## value: 0/1  (0:Disable  1:Enable)
	
	##### sip white phone number list  #####
	## P10431
	## value: String. (Format:123,4567,) 


################################################################################################
##                            Audio Settings                                          ##
################################################################################################

######			 				  Audio Settings	        						 ######

	##### Preferred Audio Codec #####
	## P14000
	## value: 1/2/4	(1:PCMU 2:PCMA 4:G722)
	
	##### System Volume #####
	## P14003
	## value:  1/2/3/4/5/6/7
	
	##### Doorbell Volume #####
	## P14835
	## value:  0/1/2/3/4/5/6/7
	
	##### Enable Custom Doorbell Ringtone #####
	## P15499
	## value:  0/1 (0:Disable  1:Enable)

###   P VALUE MISSING HERE, PLEASE ADD THEM !!!

################################################################################################
##                            Alarm Config                                                    ##
################################################################################################

######			 			  Alarm Events Config     		       						  ######

	##### Digital Input 1 #####
	## P14320
	## value: 0/1/2		(0:Disable 1:Alarm Input 2:Open Door)
	
	##### Digital Input 1 State#####
	## P15431
	## value: 0/1		(:Normal Open 1:Normal Close)
	
	##### Digit Input 1 Open Door Option #####
	## P15451
	## value: 0/1/2/3		(0: Door1  1: Door2  2: Door1 & Door2 3:None)

	##### Digital Input 1 -> Select Alarm Schedule 1 #####
	## P14321
	## value: 0 - 10	(Integer)
	
	##### Digital Input 1 -> Select Alarm Action Profile 1 #####
	## P14322
	## value: 1 - 10	(Integer)
	
	##### Digital Input 2 #####
	## P14325
	## value: 0/1/2		(0:Disable 1:Alarm Input 2:Open Door)
	
	##### Digital Input 2 State#####
	## P15432
	## value: 0/1		(:Normal Open 1:Normal Close)
	
	##### Digit Input 2 Open Door Option #####
	## P15452
	## value: 0/1/2/3		(0: Door1  1: Door2  2: Door1 & Door2 3:None)

	##### Digital Input 2 -> Select Alarm Schedule 2 #####
	## P14326
	## value: 0 - 10	(Integer)
	
	##### Digital Input 2 -> Select Alarm Action Profile 2 #####
	## P14327
	## value: 1 - 10	(Integer)
	
	##### Alarm Output Duration(s) #####
	## P14341
	## value: 5/15/30/60/180/300	(Integer)
	
	##### Enable Silently Alarm Mode #####
	## P14568
	## Format:enable@DI@MD@Tamper@Passwd_Err   Exmaple: 0@1@1@0@1)
	
	##### Enable Hostage Code #####
	## P10467
	## value: 0/1	(0:Disable  1:Enable)

	##### Hostage Code #####
	## P10466
	## value: A pure digital string, MAX length is 8. Example: 6688
	
	##### Hostage Code Alarm Action Profile #####
	## P10468
	## value: 1 - 10	(Integer)
	
	##### Enable Tamper Alarm #####
	## P14350
	## value: 0/1	(0:Disable  1:Enable)
	
	##### Tamper Alarm Action Profile #####
	## P14355
	## value: 1 - 10	(Integer)
	
	##### Enable Keypad Input Error Alarm #####
	## P14825
	## value: 0/1	(0:Disable  1:Enable  Define:1)
	
	##### Keypad Input Error Alarm profile #####
	## P14826
	## value: 1 - 10
	
	##### Enable Non-scheduled Access Alarm #####
	## P15407
	## value: 0/1	(0:Disable  1:Enable)
	
	##### Non-scheduled Access Alarm profile #####
	## P15408
	## value: 1 - 10

######			 				  Alarm Schedule	 		       						  ######

	##### schedule 1 #####
	## P14200
	## value: String  (Format:name,Date@start_time@end_time. example:schedule1,0@0000@1011,0@1100@2300)
	
	##### schedule 2 #####
	## P14201
	## value: String  (Format:name,Date@start_time@end_time. example:schedule1,0@0000@1011,0@1100@2300)
	
	##### schedule 3 #####
	## P14202
	## value: String  (Format:name,Date@start_time@end_time. example:schedule1,0@0000@1011,0@1100@2300)
	
	##### schedule 4 #####
	## P14203
	## value: String  (Format:name,Date@start_time@end_time. example:schedule1,0@0000@1011,0@1100@2300)
	
	##### schedule 5 #####
	## P14204
	## value: String  (Format:name,Date@start_time@end_time. example:schedule1,0@0000@1011,0@1100@2300)
	
	##### schedule 6 #####
	## P14205
	## value: String  (Format:name,Date@start_time@end_time. example:schedule1,0@0000@1011,0@1100@2300)
	
	##### schedule 7 #####
	## P14206
	## value: String  (Format:name,Date@start_time@end_time. example:schedule1,0@0000@1011,0@1100@2300)
	
	##### schedule 8 #####
	## P14207
	## value: String  (Format:name,Date@start_time@end_time. example:schedule1,0@0000@1011,0@1100@2300)
	
	##### schedule 9 #####
	## P14208
	## value: String  (Format:name,Date@start_time@end_time. example:schedule1,0@0000@1011,0@1100@2300)
	
	##### schedule 10 #####
	## P14209
	## value: String  (Format:name,Date@start_time@end_time. example:schedule1,0@0000@1011,0@1100@2300)
	
######			 				  Alarm Action	 		       						   ######

	##### Alarm Action Profile 1 #####
	## P14300
	## value: String  (Format:profileName@Alarm-Center,Sound,Sip,Output,Email,JPEG, example:night@1,1,1,0,1,0,)
	
	##### Alarm Action Profile 2 #####
	## P14301
	## value: String  (Format:profileName@Alarm-Center,Sound,Sip,Output,Email,JPEG, example:night@1,1,1,0,1,0,)
	
	##### Alarm Action Profile 3 #####
	## P14302
	## value: String  (Format:profileName@Alarm-Center,Sound,Sip,Output,Email,JPEG, example:night@1,1,1,0,1,0,)
	
	##### Alarm Action Profile 4 #####
	## P14303
	## value: String  (Format:profileName@Alarm-Center,Sound,Sip,Output,Email,JPEG, example:night@1,1,1,0,1,0,)
	
	##### Alarm Action Profile 5 #####
	## P14304
	## value: String  (Format:profileName@Alarm-Center,Sound,Sip,Output,Email,JPEG, example:night@1,1,1,0,1,0,)
	
	##### Alarm Action Profile 6 #####
	## P14305
	## value: String  (Format:profileName@Alarm-Center,Sound,Sip,Output,Email,JPEG, example:night@1,1,1,0,1,0,)
	
	##### Alarm Action Profile 7 #####
	## P14306
	## value: String  (Format:profileName@Alarm-Center,Sound,Sip,Output,Email,JPEG, example:night@1,1,1,0,1,0,)
	
	##### Alarm Action Profile 8 #####
	## P14307
	## value: String  (Format:profileName@Alarm-Center,Sound,Sip,Output,Email,JPEG, example:night@1,1,1,0,1,0,)
	
	##### Alarm Action Profile 9 #####
	## P14308
	## value: String  (Format:profileName@Alarm-Center,Sound,Sip,Output,Email,JPEG, example:night@1,1,1,0,1,0,)
	
	##### Alarm Action Profile 10 #####
	## P14309
	## value: String  (Format:profileName@Alarm-Center,Sound,Sip,Output,Email,JPEG, example:night@1,1,1,0,1,0,)
	
######			 				  Alarm Phone List 	 		       						  ######
	
	##### Alarm Call Out Account #####
	## P10471
	## value: 0/1/2/3/4 (0:auto N>0: account N)
	
	##### Alarm Phone List #####
	## P10459
	## value: String  (Example:1122,3344,5566, Don't forget the last ',')
	
################################################################################################
##                           Email Settings                                             ##
################################################################################################
	
######			 			 Email Settings     	 		       						  ######
	
	############### Email Settings ###############
	##### SMTP Server #####
	## P10121
	## value: String  (Example: smtp.google.com)
	
	##### SMTP Server Port #####
	## P10122
	## value: 0 - 65535  (Integer)
	
	##### From E-Mail Address #####
	## P10123
	## value: A valid email address (String)
	
	##### Sender User Name #####
	## P10127
	## value: String. Max length 63.
	
	##### Sender Password #####
	## P10128
	## value: String. Max length 63.
	
	##### Password Recovery Email #####
	## P10124
	## value: A valid email address (String)
	
	##### Alarm Receive Email 1 #####
	## P14348
	## value: A valid email address (String)
	
	##### Alarm Receive Email 2 #####
	## P14349
	## value: A valid email address (String)
	
	##### SSL #####
	## P10129
	## value: 0/1	(0:Disable  1:Enable)

################################################################################################
##                           Maintenance                                                      ##
################################################################################################

######			 		     Upgrade      	       						                  ######

	##### Firmware Upgrade Via #####
	## P6767
	## value: 0/1/2		(0:TFTP  1:HTTP  2:HTTPS)
	
	##### Firmware Server Path #####
	## P192
	## value: (String)
	
	##### Firmware HTTP/HTTS User Name #####
	## P6768
	## value: (String)
	
	##### Firmware HTTP/HTTS Password #####
	## P6769
	## value: (String)
	
	##### Firmware Upgrade File Prefix #####
	## P232
	## value: (String)
	
	##### Firmware Upgrade File Postfix #####
	## P233
	## value: (String)
	
	##### Automatic Upgrade Interval(minutes) #####
	## P193
	## value: 60 - 525600	(Integer)
	
	##### Randomized Automatic Upgrade #####
	## P8458
	## value: 0/1 (0: Disable  1: Enable)
	
	##### Hour of the Day Start Time #####
	## P285
	## value:  0 - 23	(Integer)
	
	##### Hour of the Day End Time #####
	## P8459
	## value: 0 - 23		(Integer)
	
	##### Day of the Week #####
	## P286
	## value: 0 - 6	(Integer)
	
	##### Disable SIP NOTIFY Authentication #####
	## P4428
	## value: 0/1 (0: Disable  1: Enable)
	
	##### Config Upgrade Via #####
	## P212
	## value: 0/1/2		(0:TFTP  1:HTTP  2:HTTPS)
	
	##### Config Server Path #####
	## P237
	## value: (String)
	
	##### Config HTTP/HTTS User Name #####
	## P1360
	## value: (String)
	
	##### Config HTTP/HTTS Password #####
	## P1361
	## value: (String)
	
	##### Config Upgrade File Prefix #####
	## P234
	## value: (String)
	
	##### Config Upgrade File Postfix #####
	## P235
	## value: (String)
	
	##### XML Config File Password #####
	## P1359
	## value: String.
	
	
	##### DHCP Option 66 Override Server #####
	## P145
	## value: 0/1	(0:Disable  1:Enable)
	
	##### Zero Config #####
	## P1414
	## value: 0/1	(0:Disable  1:Enable)
	
	##### Automatic Upgrade #####
	## P194
	## value: 0/1/2/3	((0:Disable  1:check for xxx minute  2:check for every day  3: check for every week))
	
	##### Validate Server Certificates #####
	## P8463
	## value: 0/1	(0:Disable  1:Enable)
	
######			 		   Debug Log   	       						                  ######

	##### Debug Log Server #####
	## P207
	## value: A valid server path	(String)
	
	##### Debug Log Level #####
	## P208
	## value: 0/1/2/3/4	(0:None 1:Debug 2:Info 3:Warning 4:Error)
	
	######			 		  Event Notification  	       						       ######
	
	##### Enable Event Notification #####
	## P15410
	## value: 0: Disable  1: Enable
	
	##### Event Notification Type #####
	## P15417
	## value: 1:HTTP 2:HTTPS
	
	##### HTTP Server URL #####
	## P15413
	## value: string Max.length=256. 
	
	##### HTTP Server Username #####
	## P15414
	## value: string Max.length=128 . 
	
	##### HTTP Server Password #####
	## P15415
	## value: string Max.length=128 . 
	
	##### URL Template #####
	## P15416
	## value: string Max.length=1024 . Example:{"mac":"${MAC}","content":"${WARNING_MSG}"}
	
	######			 		  Keep Open Door  	       						       ######
	
	##### Door 1  Forced Opening #####
	## P15429
	## value: 0/1/2 (0: Disable  1: Forced Opening  2: Scheduled Door Opening)
	
	#####  Door 1 Forced Opening Time #####
	## P15430
	## value: 5-480
	
	##### Door 1  Schedule Valid Start Time #####
	## P15211
	## value: string (Example: 20180322110506 -> Year:2018 Month:03 Date:22 Hour:11 Min:05 Second:06)
	
	##### Door 1  Schedule Valid End Time #####
	## P15212
	## value: string (Example: 20180322110506 -> Year:2018 Month:03 Date:22 Hour:11 Min:05 Second:06)
	
	##### Door 1  Schedule #####
	## P15213
	## value: string (Example: door_sch,0@0000@1259  The first '0' is 'Sun', '0000' start and '2359' end)
	
##### Emergency PIN to Disable Keep Door 1 Open #####
	## P15435
	## value: A pure digital string (Max.Length=8)
	
	##### Door 2  Forced Opening #####
	## P15455
	## value: 0/1/2 (0: Disable  1: Forced Opening  2: Scheduled Door Opening)
	
	#####  Door 2 Forced Opening Time #####
	## P15456
	## value: 5-480
	
	##### Door 2  Schedule Valid Start Time #####
	## P15457
	## value: string (Example: 20180322110506 -> Year:2018 Month:03 Date:22 Hour:11 Min:05 Second:06)
	
	##### Door 2  Schedule Valid End Time #####
	## P15458
	## value: string (Example: 20180322110506 -> Year:2018 Month:03 Date:22 Hour:11 Min:05 Second:06)
	
	##### Door 2  Schedule #####
	## P15459
	## value: string (Example: door_sch,0@0000@1259  The first '0' is 'Sun', '0000' start and '2359' end)
	
##### Emergency PIN to Disable Keep Door 2 Open #####
	## P15472
	## value: A pure digital string (Max.Length=8)
	
	##### Enable System Health Alert #####
	## P15490
	## value: 0/1 (0: Disable  1: Enable)
	
	##### Delivery Method #####
	## P15491
	## value: 0/1  0:Real-time 1:Periodic)
	
	##### Alert Interval(m) #####
	## P15492
	## value: digital 1-9999
	
	##### SIP Registration Status #####
	## P15493
	## value: 0/1  0:No 1:Yes)
	
	##### System Running Status #####
	## P15494
	## value: 0/1  0:No 1:Yes)
	
	##### System Temperature #####
	## P15495
	## value: 0/1  (0:No 1:Yes)
	
	##### Email Title #####
	## P15496
	## value: string (Max.Length=128)
	
	##### Openvpn Enable #####
	## P7050
	## value: 0/1  (0:Disable 1:Enable)
	
	##### Openvpn Server Address #####
	## P7051
	## value: string (Max.Length=256)
	
	##### Openvpn Port #####
	## P7052
	## value: 0~65535
	
	##### Openvpn Transport #####
	## P2912
	## value: 0/1 (0 UDP 1:TCP)
	
	##### Trusted CA #####
	## P9902
	## value: string (Max.Length=8192)
	
	##### Trusted Client Certificate #####
	## P9903
	## value: string (Max.Length=8192)
	
	##### Trusted Client Key #####
	## P9904
	## value: string (Max.Length=8192)
	
	##### Openvpn Cipher Method #####
	## P8396
	## value: 0/1/2/3 (0:Blowfish 1:AES-128  2:AES-256  3:Triple-DES)
	
	##### Openvpn Username #####
	## P8394
	## value: string (Max.Length=256)
	
	##### Openvpn Password #####
	## P8395
	## value: string (Max.Length=256)
	
	##### Openvpn Additional Options #####
	## P8460
	## value: string (Max.Length=1024)


################################################################################################
##                End of the Configuration Template for GDS3705 Door System        			  ##
##                           (Firmware Version:   1.0.1.11)                                   ##
################################################################################################
