###############################################################################################
####         Configuration Template for GVC3200/GVC3202 Firmware Version 1.0.3.69          ####
###############################################################################################
#######################################################################
##  Contacts - Contacts                                              ##
#######################################################################
# Clear The Old List. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P1435 = 0

# Replace Duplicate Entries. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P1436 = 0

# Download Mode. 0 - OFF, 1 - TFTP, 2 - HTTP, 3 - HTTPS. Default value is 0
# Number: 0, 1, 2, 3
P330 = 2

# File Encoding. GBK - GBK, UTF-8 - UTF-8, UTF-16 - UTF-16, UTF-32 - UTF-32, Big5 - Big5, Big5-HKSCS - Big5-HKSCS, Shift-JIS - Shift-JIS
# ISO8859-1 - ISO8859-1, ISO8859-15 - ISO8859-15, Windows-1251 - Windows-1251, EUC-KR - EUC-KR
# Default Value is UTF-8
# String: GBK, UTF-8, UTF-16, UTF-32, Big5, Big5-HKSCS, Shift-JIS, ISO8859-1, ISO8859-15, Windows-1251, EUC-KR 
P1681 = UTF-8

# Download Interval. 0 - None, 120 - 2 Hours, 240 - 4 Hours, 360 - 6 Hours, 480 - 8 Hours, 720 - 12 Hours. Default is 0 for disabled.
# Number: 0, 120, 240, 360, 480, 720
P332 = 0

# Download Server. It MUST be in the host/path format
# For example: directory.grandstream.com/engineering
# String
P331 = 

# HTTP/HTTPS Username for phonebook downloading
# String
P6713 =

# HTTP/HTTPS Password for phonebook downloading
# String
P6714 =

#######################################################################
##  Contacts - LDAP                                                  ##
#######################################################################

# Connection Mode. 0 - LDAP, 1 - LDAPS. Default Value is 0
# Number : 0, 1
P8037 =0

# Server Address
# LDAP Server Address, up to 256 characters can be used. It can be IP address or Domain name
# String
P8020 =

# Port
# Number: 1 - 65535. Default value is 389
P8021 = 389

# Base DN. The LDAP search base refers to the location in the directory where the search is requested to begin
# Example 1: dc=grandstream,dc=com
# Example 2: ou=Boston, dc=grandstream,dc=com
# String
P8022 =

# User Name. The bind "Username" for querying LDAP servers. Some LDAP servers allow anonymous binds in which case the setting can be left blank
# String
P8023 =

# Password. The bind "Password" for querying LDAP servers. And the field can be left blank if the LDAP server allows anonymous binds
# String
P8024 =

# LDAP Name Attributes. This setting specifies the "name" attributes of each record which are returned in the LDAP search result
# The setting allows the users to configure multiple space separated name attributes
# String
P8028 =

# LDAP Number Attributes. This setting specifies the "number" attributes of each record which are returned in the LDAP search result
# The setting allows the users to configure multiple space separated number attributes
# String
P8029 =

# LDAP Mail Attributes. This setting specifies the "mail" attributes of each record which are returned in the LDAP search result
# The setting allows the users to configure multiple space separated mail attributes
# String
P8038 =

# LDAP Name Filter
# LDAP name filter is the filter used for name look ups. Please refer to usermanual for examples
# String
P8026 =

# LDAP Number Filter
# LDAP name filter is the filter used for number look ups. Please refer to usermanual for examples
# String
P8025 =

# LDAP Mail Filter
# LDAP mail filter is the filter used for mail look ups. Please refer to usermanual for examples
# String
P8039 =

# LDAP Displaying Name Attributes. The entry information to be shown on phone LCD. Grandstream phones will display up to 3 fields
# String
P8030 =

# Max Hits. The setting specifies the maximum number of results to be returned by the LDAP server
# If the value is set to 0, server will return all search results. Default is 50
# Number: 0 - 32000
P8031 = 50

# Search Timeout (ms). Default is 4000
# The setting specifies how long the server should process the request and client waits for server to return
# Number: 0 - 10000
P8032 = 4000

# LDAP Lookup When Dialing. 0 - No, 1 - Yes. Default is 0
P8034 = 0

# Search LDAP for Incoming Calls. 0 - No, 1 - Yes. Default is 0
P8035 = 0

#######################################################################
##  Device Control - Audio Control                                   ##
#######################################################################

# Audio Device. 0 - Auto, 1 - Bluetooth, 2 - USB, 3 - HDMI. Default value is 0
# Number: 0, 1, 2, 3
P22050 = 0

# USB External Sound Card TX gain(db). -6, 0, +6, +12, +18, +24. Default value is 0
# Number: -6, 0, +6, +12, +18, +24
P25107 = 0

# USB External Sound Card RX gain(db). -6, 0, +6. Default value is 0
# Number: -6, 0, +6
P25108 = 0

# Ring Back Tone
P4001 = f1=440@-19,f2=480@-19,c=2000/4000;

# Busy Tone
P4002 = f1=480@-24,f2=620@-24,c=500/500;

# Reorder Tone
P4003 = f1=480@-24,f2=620@-24,c=250/250;

# Confirmation Tone
P4004 = f1=350@-11,f2=440@-11,c=100/100-100/100-100/100;

# Call-Waiting Tone
P4005 = f1=440@-13,c=300/2000-300/2000-0/0;

# Call-Waiting Tone Gain. 0 - Low, 1 - Medium, 2 - High. Default value is 0
# Number: 0, 1, 2
P1555 = 0

# Ring Cadence
P4040 = c=2000/4000;

#######################################################################
##  Settings - SIP - General                                         ##
#######################################################################

# Account Active. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P271 = 1

# Account Name
P270 =

# SIP Server
P47 =

# Secondary SIP Server
P602 =

# Tertiary SIP Server
P1702 =

# SIP User ID
P35 =

# SIP Authenticate ID
P36 =

# SIP Authentication Password
P34 =

# Voice Mail Access Number
P33 =

# Display Name (Display Name, e.g., John Doe)
P3 =

# Tel URI. 0 - Disable, 1 - User=Phone, 2 - Enabled. Default value is 0
# Number: 0, 1, 2
P63 = 0

#######################################################################
##  Settings - SIP - Network                                         ##
#######################################################################

# Outbound Proxy
P48 =

# Secondary Outbound Proxy
P2333 =

# DNS Mode. 0 - A Record, 1 - SRV, 2 - NAPTR/SRV. Default value is 0
# Number: 0, 1, 2
P103 = 0

# NAT Traversal. 0 - NAT No, 1 - STUN, 2 - Keep-alive, 3 - UPnP, 4 - Auto, 5 - VPN, 6 - TURN. Default value is 2
# Number: 0, 1, 2, 3, 4, 5, 6
P52 = 2

# Proxy-Require
P197 =

#######################################################################
##  Settings - SIP - SIP                                             ##
#######################################################################

# SIP Registration. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P31 = 1

# Unregister Before New Registration. 0 - No, 1 - All, 2 -  Instance . Default value is 2
# Number: 0, 1, 2
P81 = 2

# Register Expiration (m). In minutes. Default value is 60
# Number: 0 - 64800
P32 = 60

# Wait Time Retry Registration(s). In seconds. Default value is 20
# Number: 1 - 3600
P138 = 20

# Local SIP Port. Default value is 5060
# Number: 5 - 65535
P40 = 5060

# SUBSCRIBE For MWI. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P99 = 0

# Enable Session Timer/ Session Expiration(s).  In seconds. Default value is 180 seconds.
# By default,  Session Timer is Enabled.  Session Timer is disabled if the value is 0.
# Number: 0 or 90 - 64800
P260 = 180

# Min-SE (s). Default value is 90 seconds
# Number: 90 - 64800
P261 = 90

# UAC Specify Refresher. 0 - Omit, 1 - UAC, 2 - UAS. Default value is 0
# Number: 0, 1, 2
P266 = 0

# UAS Specify Refresher. 1 - UAC, 2 - UAS. Default value is 1
# Number: 1, 2
P267 = 1

# Force INVITE. Always refresh with INVITE instead of UPDATE even when remote party supports UPDATE
# 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P265 = 0

# Caller Request Timer. Request for timer when calling
# 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P262 = 0

# Callee Request Timer
# Request for timer when being called (i.e., if remote party supports timer but did not request for one)
# 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P263 = 0

# Force Timer. Still use timer when remote party does not support timer.
# 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P264 = 0

# Enable 100rel. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P272 = 0

# Caller ID Display. 0 - Auto, 1 - Disabled, 2 - From Header. Default value is 0
# Number: 0, 1, 2
P2324 = 0

# Use Privacy Header
# 0 - Default, 1 - No, 2 - Yes. Default is 0
# Number: 0, 1, 2
P2338 = 0

# Use P-Preferred-Identity Header
# 0 - Default, 1 - No, 2 - Yes. Default is 0
# Number: 0, 1, 2
P2339 = 0

# SIP Transport
# 0 - UDP , 1 - TCP, 2 - TLS. Default value is 0
# Number: 0, 1, 2
P130 = 0

# SIP URI Scheme When Using TLS
# 0 -sip, 1 - sips. Default value is 0.
# Number: 0, 1
P2329 = 0

# Use Actual Ephemeral Port in Contact with TCP/TLS
# 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P2331 = 0

# Symmetric RTP. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P291 = 0

# RTP IP Filter. 0 - Disable, 1 - IP Only, 2- IP and Port. Default value is 0
# Number: 0, 1, 2
P26026 = 0

# Support SIP Instance ID
# 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P288 = 1

# Validate Incoming SIP Messages
# 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P2306 = 0

# Check SIP User ID for Incoming INVITE
# 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P258 = 0

# Authenticate Incoming INVITE
# 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P2346 = 0

# SIP Realm Used for Challenge INVITE & NOTIFY
# String
P26021 =

# Only Accept SIP Requests from Known Servers
# 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P2347 = 0

# SIP T1 Timeout. RFC 3261 T1 value (RTT estimate)
# 50 - 0.5 sec, 100 - 1 sec, 200 - 2 sec. Default value is 50
# Number: 50, 100, 200
P209 = 50

# SIP T2 Interval. RFC 3261 T2 value
# The maximum retransmit interval for non-INVITE requests and INVITE responses
# 200 - 2 sec, 400 - 4 sec, 800 - 8 sec. Default value is 400
# Number: 200, 400, 800.
P250 = 400

# Remove OBP from route
# 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P2305 = 0

# Check Domain Certificates
# 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P2311 = 0

# Validate certification chain
# 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P2367 = 0

#######################################################################
##  Settings - SIP - Codec                                           ##
#######################################################################

# DTMF: in audio. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P2301 = 0

# DTMF: via RFC2833. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P2302 = 1

# DTMF: via SIP INFO. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P2303 = 0

# DTMF Payload Type. Default value is 101
# Number: 96 - 127
P79 = 101

# Preferred Vocoder
# First codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 103 - G722.1C, 104 - G.722.1, 123 - Opus. Default value is 0
# Number: 0, 8, 9, 103, 104, 123
P57 = 0

# Second codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 103 - G722.1C, 104 - G.722.1, 123 - Opus. Default value is 8
# Number: 0, 8, 9, 103, 104, 123
P58 = 8

# Third codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 103 - G722.1C, 104 - G.722.1, 123 - Opus. Default value is 9
# Number: 0, 8, 9, 103, 104, 123
P59 = 9

# Forth codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 103 - G722.1C, 104 - G.722.1, 123 - Opus. Default value is 104
# Number: 0, 8, 9, 103, 104, 123
P60 = 104

# Fifth codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 103 - G722.1C, 104 - G.722.1, 123 - Opus. Default value is 104
# Number: 0, 8, 9, 103, 104, 123
P61 = 104

# Sixth codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 103 - G722.1C, 104 - G.722.1, 123 - Opus. Default value is 104
# Number: 0, 8, 9, 103, 104, 123
P62 = 104

# Codec Negotiation Priority.
# 0 - Caller, 1 - Callee. Default value is 1
P29061 = 1

# Silence Suppression. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P50 = 0

# Voice Frames Per TX. Default value is 2
# Number: 1 - 64.
P37 = 2

# G.722.1 Rate. 0 - 24kbps encoding rate, 1 - 32kbps encoding rate. Default value is 0
# Number: 0, 1
P2373 = 0

# G.722.1 Payload Type. Default value is 104
# Number: 96 - 126
P2374 = 104

# G722.1C Rate. 0 - 24kbps encoding rate, 1 - 32kbps encoding rate, 2 - 48Kbps encoding rate. Default value is 0
# Number: 0, 1, 2
P26417 = 0

# G.722.1C Payload Type. Default value is 103
# Number: 96 - 126
P26016 = 103

# Opus Payload Type. Defaualt value is 123
# Number: 96 - 126
P2385 = 123

# Use First Matching Vocoder in 200OK SDP
# 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P2348 = 0

# Enable RFC5168 support. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P1331 = 1

# Enable Video FEC. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P2393 = 1

# Video FEC Mode. Default is 0
# Number: 0, 1
P26022 = 0

# FEC Payload Type. Default value is 120
# Number: 96 - 127
P2394 = 120

# Enable FECC. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P26004 = 1

# FECC H.224 Payload Type. Default value is 125
# Number: 96 - 127
P26008 = 125

# H.264 Payload Type. Default value is 99
# Number: 96 - 127
P293 = 99

# Packetization-mode. 0 - 0, 1 - 1, 2 - Auto. Default is 1
# Number: 0, 1, 2
P26005 = 1

# H.264 Image Size. 10 - 1080P, 9 - 720P, 4 - 4CIF, 7 - 4SIF, 1 - VGA. Default value is 10
# Number: 10, 9, 4, 7, 1
P2307 = 10

# H.264 Profile Type. 0 - Baseline Profile, 1 - Main Profile, 2 - High Profile, 3 - BP&MP&HP
# Number: 0, 1, 2, 3. Default value is 3
P2377 = 3

# Video Bit Rate.
# 384 - 384 kbps, 400 - 400 kbps, 416 - 416 kbps, 448 - 448 kbps, 512 - 512 kbps, 640 - 640 kbps,
# 768 - 768 kbps, 896 - 896 kbps, 1024 - 1024 kbps, 1280 - 1280 kbps, 1536 - 1536 kbps, 1792 - 1792 kbps,
# 2048 - 2048 kbps, 2560 - 2560 kbps, 3072 - 3072 kbps, 3584 - 3584 kbps, 4096 - 4096 kbps.
# Default value and the available selections vary, depending on H.264 image size.
# If H.264 Image Size is 1080P, Video Bit Rate default value is 2048;
# If H.264 Image Size is 720P, Video Bit Rate default value is 2048;
# If H.264 Image Size is 4CIF/4SIF/VGA, Video Bit Rate default value is 512.
# Number: 384, 400, 416, 448, 512, 640, 768, 896, 1024, 1280, 1536, 1792, 2048, 2560, 3072, 3584, 4096
P2315 = 2048

# SDP Bandwidth Attribute. 0 - Standard, 1 - Media Level, 3 - None. Default value is Media Level
# Number: 0, 1, 3
P2360 = 1

# Video Frame Rate. 5 - 5 fps, 15 - 15 fps, 25 - 25 fps, 30 - 30 fps, 29 - VFR. Default value is 30
# Number: 5, 15, 25, 30, 29
P25004 = 30

# Video Jitter Buffer Maximum (ms). Default value is 50
# Number: 0 - 1000
P2381 = 50

# Disable Presentation. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P26001 = 0

# Presentation H.264 Image Size. 10 - 1080P, 9 - 720P. Default is 10
# Number: 10, 9
P2376 = 10

# Presentation H.264 Profile Type. 0 - Baseline Profile, 1 - Main Profile, 2 - High Profile, 3 - BP&MP&HP
# Number: 0, 1, 2, 3. Default value is 3
P2377 = 3

# Presentation Video Bit Rate.
# 512 - 512 kbps, 640 - 640 kbps, 768 - 768 kbps, 896 - 896 kbps,
# 1024 - 1024 kbps, 1280 - 1280 kbps, 1536 - 1536 kbps, 1792 - 1792 kbps, 2048 - 2048 kbps.
# Default value is 1024 kbps.
# Number: 512, 640, 768, 896, 1024, 1280, 1536, 1792, 2048
P2378 = 1024

# Presentation Video Frame Rate. Default value is 15.
# 5 - 5 fps, 10 - 10 fps, 15 = 15 fps
P26042 = 15

# BFCP Transport Protocol. Default value is 1.
# 0 - Audo, 1 - UDP, 2 - TCP
P26041 = 1

# SRTP Mode. Default value is 0. 0 - Disable, 1 - Enable but not forced, 2 - Enable and forced.
# Number: 0, 1, 2
P183 = 0

# SRTP Key Length. Default value is 0. 0 - AES 128&256 bit, 1 - AES 128 bit, 2 - AES 256 bit.
# Number: 0, 1, 2
P2383 = 0

#######################################################################
##  Settings - SIP - Call                                            ##
#######################################################################

# Remote Video Request. 0 - Prompt, 1 - Accept, 2 - Deny. Default value is 0
# Number: 0, 1, 2
P2326 = 0

# Dial Plan Prefix
# String
P66 = 

# Dial Plan. Default value is { x+ | \+x+ | *x+ | *xx*x+ | x+*x+*x+*x+[#x]+ }
P290 = { x+ | \+x+ | *x+ | *xx*x+ | x+*x+*x+*x+[#x]+ }

# Refer-To Use Target Contact. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P135 = 0

# Auto Answer. 0 - No, 1 - Yes, 2 - Enable Intercom/Paging. Default value is 0
# Number: 0, 1, 2
#tried 1, 2
P90 = 0

# Send Anonymous. 0 - No, 1 - Yes (caller ID will be blocked if set to Yes). Default value is 0
# Number: 0, 1
P65 = 0

# Reject Anonymous Call. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P129 = 0

# Call Log
# 0 - Log All, 1 - Log Incoming/Outgoing only (Missed Calls Not Recorded), 2 - Disable Call log. Default value is 0
# Number: 0, 1, 2
P182 = 0

# Special Feature. Default value is 100
# 100 - Standard, 102 - Broadsoft, 108 - CBCOM, 109 - RNK, 113 - China Mobile
# 114 - ZTE IMS, 115 - Mobotix, 116 - ZTE NGN, 117 - Huawei IMS
# Number: 100, 102, 108, 109, 113, 114, 115, 116, 117
P198 = 100

# Feature Key Synchronization. 0 - Disable,  1 - Broadsoft. Default value is 0
# Number: 0, 1
P2325 = 0

# Enable Call Features. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P191 = 0

# Ring Timeout(s). Default value is 60
# Number: 10 - 300
P1328 = 60

# Transfer on 3 way conference Hangup. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P2304 = 0

# Use # as Dial Key. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P72 = 1

# Conference-URI
# String
P2318 =

# Enable Local MOH. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P2357 = 0

# Account Ring Tone
# String
P104 = content://settings/system/ringtone

# Call Forwarding - Others
# No Answer Timeout(sec). Default value is 20
# Number: 1 - 120
P139 = 20

# Matching Incoming Caller ID. Matching Rule 1
# String
P1488 =

# Matching Rule 1 Distinctive Ringtone. See ring tone options and value in the Ring Tone Value Table below
# String
P1489 = content://settings/system/ringtone

# Matching Incoming Caller ID. Matching Rule 2
# String
P1490 =

# Matching Rule 2 Distinctive Ringtone. See ring tone options and value in the Ring Tone Value Table below
# String
P1491 = content://settings/system/ringtone

# Matching Incoming Caller ID. Matching Rule 3
# String
P1492 =

# Matching Rule 3 Distinctive Ringtone. See ring tone options and value in the Ring Tone Value Table below
# String
P1493 = content://settings/system/ringtone

############            Ring Tone Value Table            ###############
# Web GUI Option                            Value
# Use System Ring tone                      content://settings/system/ringtone 
# Silent                                    ringtone_silence
# Andromeda									/system/media/audio/ringtones/Andromeda.ogg
# Aquila									/system/media/audio/ringtones/Aquila.ogg
# ArgoNavis									/system/media/audio/ringtones/ArgoNavis.ogg
# Atria										/system/media/audio/ringtones/Atria.ogg
# Backroad									/system/media/audio/ringtones/Backroad.ogg
# BeatPlucker								/system/media/audio/ringtones/BeatPlucker.ogg
# BentleyDubs								/system/media/audio/ringtones/BentleyDubs.ogg
# Big_Easy                                  /system/media/audio/ringtones/Big_Easy.ogg
# BirdLoop                                  /system/media/audio/ringtones/BirdLoop.ogg
# Bollywood                                 /system/media/audio/ringtones/Bollywood.ogg
# BussaMove                                 /system/media/audio/ringtones/BussaMove.ogg
# CASSIOPEIA								/system/media/audio/ringtones/CASSIOPEIA.ogg
# Cairo                                     /system/media/audio/ringtones/Cairo.ogg
# Calypso_Steel                             /system/media/audio/ringtones/Calypso_Steel.ogg
# CanisMajor								/system/media/audio/ringtones/CanisMajor.ogg
# CaribbeanIce								/system/media/audio/ringtones/CaribbeanIce.ogg
# Carina									/system/media/audio/ringtones/Carina.ogg
# Centaurus									/system/media/audio/ringtones/Centaurus.ogg
# Champagne_Edition							/system/media/audio/ringtones/Champagne_Edition.ogg
# Club_Cubano                               /system/media/audio/ringtones/Club_Cubano.ogg
# CrayonRock                                /system/media/audio/ringtones/CrayonRock.ogg
# CrazyDream								/system/media/audio/ringtones/CrazyDream.ogg
# CurveBall                                 /system/media/audio/ringtones/CurveBall.ogg
# Cygnus									/system/media/audio/ringtones/Cygnus.ogg
# DancinFool                                /system/media/audio/ringtones/DancinFool.ogg
# Ding 										/system/media/audio/ringtones/Ding.ogg
# DonMessWivlt                              /system/media/audio/ringtones/DonMessWivIt.ogg
# Draco										/system/media/audio/ringtones/Draco.ogg
# DreamTheme								/system/media/audio/ringtones/DreamTheme.ogg
# Eastern_Sky                               /system/media/audio/ringtones/Eastern_Sky.ogg
# Enter_the_Nexus                           /system/media/audio/ringtones/Enter_the_Nexus.ogg
# Eridani									/system/media/audio/ringtones/Eridani.ogg
# EtherShake								/system/media/audio/ringtones/EtherShake.ogg
# FreeFlight								/system/media/audio/ringtones/FreeFlight.ogg
# FriendlyGhost								/system/media/audio/ringtones/FriendlyGhost.ogg
# Funk_Yall                                 /system/media/audio/ringtones/Funk_Yall.ogg
# GameOverGuitar							/system/media/audio/ringtones/GameOverGuitar.ogg
# Gimme_Mo_Town                             /system/media/audio/ringtones/Gimme_Mo_Town.ogg
# Girtab									/system/media/audio/ringtones/Girtab.ogg
# Glacial_Groove                      		/system/media/audio/ringtones/Glacial_Groove.ogg
# Growl                                     /system/media/audio/ringtones/Growl.ogg
# HalfwayHome								/system/media/audio/ringtones/HalfwayHome.ogg
# InsertCoin								/system/media/audio/ringtones/InsertCoin.ogg
# Kuma										/system/media/audio/ringtones/Kuma.ogg
# LoopyLounge                               /system/media/audio/ringtones/LoopyLounge.ogg
# LoveFlute                                 /system/media/audio/ringtones/LoveFlute.ogg
# Lyra										/system/media/audio/ringtones/Lyra.ogg
# Machina									/system/media/audio/ringtones/Machina.ogg
# MidEvilJaunt                        		/system/media/audio/ringtones/MidEvilJaunt.ogg
# MildlyAlarming							/system/media/audio/ringtones/MildlyAlarming.ogg
# Nairobi                             		/system/media/audio/ringtones/Nairobi.ogg
# Nassau                             		/system/media/audio/ringtones/Nassau.ogg
# NewPlayer									/system/media/audio/ringtones/NewPlayer.ogg
# No_Limits                                 /system/media/audio/ringtones/No_Limits.ogg
# Noises1									/system/media/audio/ringtones/Noises1.ogg
# Noises2									/system/media/audio/ringtones/Noises2.ogg
# Noises3									/system/media/audio/ringtones/Noises3.ogg
# OrganDub                            		/system/media/audio/ringtones/OrganDub.ogg
# Orion										/system/media/audio/ringtones/Orion.ogg
# Paradise_Island                     		/system/media/audio/ringtones/Paradise_Island.ogg
# Pegasus									/system/media/audio/ringtones/Pegasus.ogg
# Perseus									/system/media/audio/ringtones/Perseus.ogg
# Playa                                     /system/media/audio/ringtones/Playa.ogg
# Pyxis										/system/media/audio/ringtones/Pyxis.ogg
# Rasalas									/system/media/audio/ringtones/Rasalas.ogg
# Revelation								/system/media/audio/ringtones/Revelation.ogg
# Rigel										/system/media/audio/ringtones/Rigel.ogg
# Ring_Classic_02                           /system/media/audio/ringtones/Ring_Classic_02.ogg
# Ring_Digital_02                           /system/media/audio/ringtones/Ring_Digital_02.ogg
# Ring_Synth_02                             /system/media/audio/ringtones/Ring_Synth_02.ogg
# Ring_Synth_04                             /system/media/audio/ringtones/Ring_Synth_04.ogg
# Road_Trip                                 /system/media/audio/ringtones/Road_Trip.ogg
# RomancingTheTone							/system/media/audio/ringtones/RomancingTheTone.ogg
# Safari                                    /system/media/audio/ringtones/Safari.ogg
# Savannah									/system/media/audio/ringtones/Savannah.ogg
# Scarabaeus								/system/media/audio/ringtones/Scarabaeus.ogg
# Sceptrum									/system/media/audio/ringtones/Sceptrum.ogg
# Seville                                   /system/media/audio/ringtones/Seville.ogg
# Shes_All_That                             /system/media/audio/ringtones/Shes_All_That.ogg
# SilkyWay                                  /system/media/audio/ringtones/SilkyWay.ogg
# SitarVsSitar								/system/media/audio/ringtones/SitarVsSitar.ogg
# Solarium									/system/media/audio/ringtones/Solarium.ogg
# SpringyJalopy								/system/media/audio/ringtones/SpringyJalopy.ogg
# Steppin_Out                               /system/media/audio/ringtones/Steppin_Out.ogg
# Terminated                                /system/media/audio/ringtones/Terminated.ogg
# Testudo									/system/media/audio/ringtones/Testudo.ogg"
# Themos									/system/media/audio/ringtones/Themos.ogg
# Third_Eye                                 /system/media/audio/ringtones/Third_Eye.ogg
# Thunderfoot								/system/media/audio/ringtones/Thunderfoot.ogg
# TwirlAway                                 /system/media/audio/ringtones/TwirlAway.ogg
# UrsaMinor									/system/media/audio/ringtones/UrsaMinor.ogg
# VeryAlarmed								/system/media/audio/ringtones/VeryAlarmed.ogg
# Vespa										/system/media/audio/ringtones/Vespa.ogg
# World                                     /system/media/audio/ringtones/World.ogg
# Zeta										/system/media/audio/ringtones/Zeta.ogg
# bellcore-dr1                              /system/media/audio/ringtones/bellcore-dr1.ogg
# bellcore-dr2                              /system/media/audio/ringtones/bellcore-dr2.ogg
# bellcore-dr3                              /system/media/audio/ringtones/bellcore-dr3.ogg
# bellcore-dr4                              /system/media/audio/ringtones/bellcore-dr4.ogg
# bellcore-dr5                              /system/media/audio/ringtones/bellcore-dr5.ogg
# hydra										/system/media/audio/ringtones/hydra.ogg
# speaker									/system/media/audio/ringtones/speaker.wav

##############################################################################
##  Settings - IPVideoTalk - General                                        ##
##############################################################################

# Account active. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P7059 = 1

# Display Name
# String
P407 =

# SIP Transport. 1 - TCP, 2 - TLS. Default is 2
# Number: 1, 2
P448 = 2


##############################################################################
##  Settings - IPVideoTalk - Call                                           ##
##############################################################################

# Auto Answer When Idle. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P425 = 0


##############################################################################
##  Settings - BlueJeans - General                                          ##
##############################################################################

# Account Active. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P501 = 1

# Display Name. Default value is BlueJeans
# String
P507 = BlueJeans

##############################################################################
##  Settings - BlueJeans - Codec                                            ##
##############################################################################

# DTMF: in audio. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P2501 = 0

# DTMF: via RFC2833. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P2502 = 1

# DTMF: via SIP INFO. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P2503 = 0

# DTMF Payload Type. Default value is 101
# Number: 96 - 127
P596 = 101

# Preferred Vocoder
# First codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 104 - G.722.1. Default value is 0
# Number: 0, 8, 9, 2, 104
P551 = 0

# Second codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 104 - G.722.1. Default value is 8
# Number: 0, 8, 9, 104
P552 = 8

# Third codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 104 - G.722.1. Default value is 9
# Number: 0, 8, 9, 104
P553 = 9

# Forth codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 104 - G.722.1. Default value is 104
# Number: 0, 8, 9, 104
P554 = 104

# Codec Negotiation Priority.
# 0 - Caller, 1 - Callee. Default value is 1
P29261 = 1

# Silence Suppression. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P585 = 0

# Voice Frames Per TX. Default value is 2
# Number: 1 - 64.
P586 = 2

# G.722.1 Rate. 0 - 24kbps encoding rate, 1 - 32kbps encoding rate. Default value is 0
# Number: 0, 1
P2573 = 0

# G.722.1 Payload Type. Default value is 104
# Number: 96 - 126
P2574 = 104

# Use First Matching Vocoder in 200OK SDP
# 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P2548 = 0

# Enable RFC5168 support. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P578 = 1

# Enable Video FEC. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P2593 = 0

# FEC Payload Type. Default value is 120
# Number: 96 - 127
P2594 = 120

# H.264 Payload Type. Default value is 99
# Number: 96 - 127
P562 = 99

# Packetization-mode. 0 - 0, 1 - 1, 2 - Auto. Default is 1
# Number: 0, 1, 2
P26205 = 1

# H.264 Image Size. 10 - 1080P, 9 - 720P, 4 - 4CIF, 7 - 4SIF, 1 - VGA. Default value is 10
# Number: 10, 9, 4, 7, 1
P2507 = 10

# H.264 Profile Type. 0 - Baseline Profile, 1 - Main Profile, 2 - High Profile, 3 - BP&MP&HP
# Number: 0, 1, 2, 3. Default value is 3
P2562 = 3

# Video Bit Rate.
# 384 - 384 kbps, 400 - 400 kbps, 416 - 416 kbps, 448 - 448 kbps, 512 - 512 kbps, 640 - 640 kbps,
# 768 - 768 kbps, 896 - 896 kbps, 1024 - 1024 kbps, 1280 - 1280 kbps, 1536 - 1536 kbps, 1792 - 1792 kbps,
# 2048 - 2048 kbps, 2560 - 2560 kbps, 3072 - 3072 kbps, 3584 - 3584 kbps, 4096 - 4096 kbps.
# Default value and the available selections vary, depending on H.264 image size.
# If H.264 Image Size is 1080P, Video Bit Rate default value is 2048;
# If H.264 Image Size is 720P, Video Bit Rate default value is 2048;
# If H.264 Image Size is 4CIF/4SIF/VGA, Video Bit Rate default value is 512.
# Number: 384, 400, 416, 448, 512, 640, 768, 896, 1024, 1280, 1536, 1792, 2048, 2560, 3072, 3584, 4096
P2515 = 2048

# SDP Bandwidth Attribute. 0 - Standard, 1 - Media Level, 3 - None. Default value is Media Level
# Number: 0, 1, 3
P2560 = 1

# Video Frame Rate. 5 - 5 fps, 15 - 15 fps, 25 - 25 fps, 30 - 30 fps, 29 - VFR. Default value is 30
# Number: 5, 15, 25, 30, 29
P25006 = 30

# Video Jitter Buffer Maximum (ms). Default value is 50
# Number: 0 - 1000
P2581 = 50

# Disable Presentation. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P26201 = 0

# Presentation H.264 Image Size. 10 - 1080P, 9 - 720P. Default is 10
# Number: 10, 9
P2576 = 10

# Presentation H.264 Profile Type. 0 - Baseline Profile, 1 - Main Profile, 2 - High Profile, 3 - BP&MP&HP
# Number: 0, 1, 2, 3. Default value is 3
P2577 = 3

# Presentation Video Bit Rate.
# 512 - 512 kbps, 640 - 640 kbps, 768 - 768 kbps, 896 - 896 kbps,
# 1024 - 1024 kbps, 1280 - 1280 kbps, 1536 - 1536 kbps, 1792 - 1792 kbps, 2048 - 2048 kbps.
# Default value is 1024 kbps.
# Number: 512, 640, 768, 896, 1024, 1280, 1536, 1792, 2048
P2578 = 1024

# Presentation Video Frame Rate. Default value is 15.
# 5 - 5 fps, 10 - 10 fps, 15 = 15 fps
P26242 = 15

##############################################################################
##  Settings - BlueJeans - Call                                             ##
##############################################################################

# Call Log
# 0 - Log All, 2 - Disable call log. Default value is 0
# Number: 0, 2
P542 = 0

# Use # as Dial Key. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P592 = 1

# Enable Local MOH. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P2557 = 0


##############################################################################
##  Settings - H.323 - General                                              ##
##############################################################################

# Account Active
# 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P25059 = 0

# Enable GK. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P25032 = 0

# Enable H.460. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P25066 = 0

# GK Discover Mode. 0 - Audo, 1 - Manual. Default value is 0
# Number: 0, 1
P25051 = 0

# GK Address
# String
P25033 =

# Site Number
# String
P25034 =

# GK Authentication Username
# String
P25035 =

# GK Authentication Password
# String
P25036 =

# Register Expiration. In Minutes. Default value is 60
# Number: 1 - 1440
P25054 = 60

# H.323 Local Port. Default value is 1720
# TCP (local H.323 signal port): port 1720, UDP (H.225-RAS): port 4000 - 4100
# TCP (H.225-CS H.245): port 4200 - 4300, UDP (RTP/RTCP): port 6004 - 6080
# Number: 1720, 4000 - 4100, 4200 - 4300, 6004 - 6080
P25068 = 1720

# Symmetric RTP. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P25067 = 0

##############################################################################
##  Settings - H.323 - Codec                                                ##
##############################################################################
# DTMF: 0 - In audio. 1 - RFC2833, 2 - H245 signal. Default value is 0
# Number: 0, 1, 2
P25049 = 0

# Preferred Vocoder
# First codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 104 - G.722.1. Default value is 0
# Number: 0, 8, 9, 104
P25037 = 0

# Second codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 104 - G.722.1. Default value is 0
# Number: 0, 8, 9, 104
P25038 = 0

# Third codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 104 - G.722.1. Default value is 0
# Number: 0, 8, 9, 104
P25039 = 0

# Fourth codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 104 - G.722.1. Default value is 0
# Number: 0, 8, 9, 104
P25040 = 0

# H.264 payload type. Default value is 99
P25064 = 99

# H.264 image size. 10 - 1080P, 9 - 720P, 4 - 4CIF, 7 - 4SIF, 1 - VGA. Default value is 10
# Number: 10, 9, 4, 7, 1
P25061 = 10

# Video Bit Rate.
# 384 - 384 kbps, 400 - 400 kbps, 416 - 416 kbps, 448 - 448 kbps, 512 - 512 kbps, 640 - 640 kbps,
# 768 - 768 kbps, 896 - 896 kbps, 1024 - 1024 kbps, 1280 - 1280 kbps, 1536 - 1536 kbps, 1792 - 1792 kbps,
# 2048 - 2048 kbps, 2560 - 2560 kbps, 3072 - 3072 kbps, 3584 - 3584 kbps, 4096 - 4096 kbps.
# Default value and the available selections vary, depending on H.264 image size.
# If H.264 Image Size is 1080P, Video Bit Rate default value is 2048;
# If H.264 Image Size is 720P, Video Bit Rate default value is 2048;
# If H.264 Image Size is 4CIF/4SIF/VGA, Video Bit Rate default value is 512.
# Number: 384, 400, 416, 448, 512, 640, 768, 896, 1024, 1280, 1536, 1792, 2048, 2560, 3072, 3584, 4096
P25063 = 2048

# Video frame rate. 5 - 5 fps, 15 - 15 fps, 25 - 25 fps, 30 - 30 fps, 29 - VFR
# Default value is 30
# Number: 5, 15, 25, 30, 29
P25062 = 30

# Presentation H.264 Image Size. 10 - 1080P, 9 - 720P. Default value is 10.
# Number: 9, 10
P25071 = 10

# Presentation Video Bit Rate.
# 512 - 512 kbps, 640 - 640 kbps, 768 - 768 kbps, 896 - 896 kbps,
# 1024 - 1024 kbps, 1280 - 1280 kbps, 1536 - 1536 kbps, 1792 - 1792 kbps, 2048 - 2048 kbps.
# Default value is 1024 kbps.
# Number: 512, 640, 768, 896, 1024, 1280, 1536, 1792, 2048
P25070 = 1024

# Presentation Video Frame Rate. Default value is 15.
# 5 - 5 fps, 10 - 10 fps, 15 = 15 fps
P25069 = 15

##############################################################################
##  Settings - H.323 - Call                                                 ##
##############################################################################
# Auto Answer. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P25048 = 0

# Enable H255 Keep-alive. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P25058 = 0

# Enable H245 Keep-alive. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P25057 = 0

# Enable RTDR. 0 - 1, 1 - Yes. Default value is 0
# Number: 0, 1
P25060 = 0


##############################################################################
##  Settings - Network Settings                                             ##
##############################################################################
# Internet Protocol. 0 - Prefer IPv4, 1 - Prefer IPv6. Default is 0
# Number: 0, 1
# Mandatory
P1415 = 0

# Address Type. 0 - DHCP, 1 - Static, 2 - PPPoE. Default value is 0
# Number: 0, 1, 2
P8 = 0

# DHCP VLAN override. 0 - Disable, 1 - DHCP Option 132 and DHCP Option 133, 2 - Encapsulated in DHCP Option 43
# Number: 0, 1, 2. Default is 2
# Mandatory
P8300 = 2

# Host name (DHCP option 12)
P146 = 

# Vendor Class ID (DHCP option 60). 
# The default value for GVC3200 is Grandstream GVC3200
# The default value for GVC3202 is Grandstream GVC3202
# P148 = Grandstream GVC3200

# DHCP Option 120 Override SIP Server. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P1411 = 1

# Static IP. IP address
#P9 = 192
#P10 = 168
#P11 = 0
#P12 = 160

# Static IP. Subnet Mask
#P13 = 255
#P14 = 255
#P15 = 0
#P16 = 0

# Static IP. Default Gateway
#P17 = 0
#P18 = 0
#P19 = 0
#P20 = 0

# Static IP. DNS Server 1. Ignore if DHCP or PPPoE is used
#P21 = 0
#P22 = 0
#P23 = 0
#P24 = 0

# Static IP. DNS Server 2. Ignore if DHCP or PPPoE is used
P25 = 0
P26 = 0
P27 = 0
P28 = 0

# PPPoE Account ID
#P82 = 

# PPPoE Password
#P83 = 

# 802.1x Mode. 0 - Close, 1 - EAP-MD5, 2 - EAP-TLS, 3-EAP-PEAP. Default is 0
# Number: 0, 1, 2, 3
P7901 = 0

# 802.1x Identity
#P7902 =

# 802.1 Secret
#P7903 =

# Enable LLDP. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P1684 = 1

# Layer 3 QoS for SIP. Default value is 48
P1558 = 26

# Layer 3 QoS for Audio. Default value is 48
P1559 = 46

# Layer 3 QoS for Video. Default is 48
P1560 = 34

# Layer 2 QoS 802.1Q/VLAN Tag. Default value is 0
# Number: 0 - 4095
P51 = 0

# Layer 2 QoS 802.1p Priority. Default value is 0
# Number: 0 - 7
P87 = 0

# Bypass Proxy For
# String
P22011 =

# Alternate DNS Server
#P92 = 0
#P93 = 0
#P94 = 0
#P95 = 0

# Second Alternate DNS Server
#P5026 =
#P5027 =
#P5028 =
#P5029 =

# User-Agent
P1541 =

# SIP User-Agent
# For GVC3200, the value is Grandstream GVC3200 $version
# For GVC3202, the value is Grandstream GVC3202 $version
# P26027 =

# IPv6 Address type. 0 - Auto Configured, 1 - Statically Configured. Default is 0.
# Number: 0, 1
# Mandatory
P1419 = 0

# Full Static: Static IPv6 Address
# P1420 =

# Full Static: IPv6 Prefix Length
# P1421 =

# DNS Server 1 for IPv6 Address
# String: a-z, A-Z, 0-9, ".", ":", "[", "]"
# P1424 =

# DNS Server 2 for IPv6 Address
# String: a-z, A-Z, 0-9, ".", ":", "[", "]"
# P1425 =

# Preferred DNS Server for IPv6 Address
# String: a-z, A-Z, 0-9, ".", ":", "[", "]"
# P1423 =

##############################################################################
##  Settings - Peripheral                                                   ##
##############################################################################

# HDMI 2 out resolution. 10 – 1080P 60HZ, 9 – 1080P 50HZ, 6 – 720P 60HZ, 5 – 720P 50HZ. Default value is 10.
# Number: 10, 9, 6, 5
P25105 = 10

# Enable Presentation Automatically When HDMI/VGA Plugged. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
P25109 = 0

# Move Speed. The move speed range is from 1 to 16.
# Number: 1-16. Default value is 5
P25029 = 5

# Initial Position. 0 - System default positon, 100 - Position when power off, 1 - Preset 1, 2 - Preset 2, 3 - Preset 3,
# 4 - Preset 4, 5 - Preset 5, 6 - - Preset 6, 7 - Preset 7, 8 - Preset 8, 9 - Preset 9, 10 - Preset 10,
# 11 - Preset 11, 12 - Preset 12, 13 - Preset 13, 14 - Preset 14, 15 - Preset 15, 16 - Preset 16, 17 - Preset 17,
# 18 - Preset 18, 19 - Preset 19, 20 - Preset 20, 21 - Preset 21, 22 - Preset 22, 23 - Preset 23, 24 - Preset 24
# Default value is 0
# Number: 0, 100, 1, 2, 3, 4, 5, 6, 7, 8, 9, 10, 11, 12, 13, 14, 15, 16, 17, 18, 19, 20, 21, 22, 23, 24
P25030 = 0

# Disable Missed Call OLED Indicator. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
P1691 = 0

# Disable MWI OLED Indicator. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
P1692 = 0

# Disable New Message OLED Indicator. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
P1693 = 0

# Disable Contact Full OLED Indicator. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
P1694 = 0

#######################################################################
##  Settings - Call Features                                         ##
#######################################################################

# Start Video Automatically. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P25023 = 1

# Always Ring Internal Speaker. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P1439 = 0

# Disable DialPlan. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P1687 = 0

# Filter Characters. Default is [()-]
P22012 = [()-]

# Disable Call-Waiting. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P91 = 0

# Disable Call-Waiting Tone. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P186 = 0

# Disable DND Reminder Ring. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P1486 = 0

# Disable Direct IP Call. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P277 = 0

# Use Quick IP-Call Mode. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P184 = 0

# Enable frame skipping in video decoder. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P22008 = 0

# Escape '#' as %23 in SIP URI. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P1406 = 0

# Auto mute on entry. 0 - Disable, 1 - Auto mute on incoming call, 2 - Auto mute on outgoing call, 3 - Auto mute on incoming and outgoing call
# Number： 0, 1, 2, 3. Default is 0
# Mandatory
P29607 = 0

#######################################################################
##  Settings -> General Settings                                     ##
#######################################################################

# Fan Speed. 0 - Normal, 1 - Full Speed. Default is 0
# Number: 0, 1
P22049 = 0

# Local RTP Port. Default value is 5004
# Number: 1024 - 65535
P39 = 5004

# Use Random Port. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P78 = 0

# Disable in-call DTMF display.  0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P338 = 0

# Enable Enterprise Contacts Backend Matching. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P22128 = 0

# Disable Remote Control App Connect. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P25022 = 0

# Remote Control Touchpad Sensitivity. 2 - Normal, 3 - Faster, 1 - Slower. Default is 2
# Number: 1, 2, 3
P25031 = 2

# Keep-alive Interval (s). Default value is 20 seconds
# Number: 10 - 160
P84 = 20

# STUN/TURN Server
P76 = stun.ipvideotalk.com

# TURN Server Username
# String
P22042 = 

# TURN Server Password
# String
P22043 = 

# Use NAT IP. This will enable our SIP client to use this IP in the SIP message.
# Example 64.3.153.50
P101 = 

#######################################################################
##  Settings -> Security Settings                                    ##
#######################################################################
# Admin password for web interface
P2 = admin

# End User Password
P196 = user

# Disable SSH. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P276 = 0

# Access Method. 0 - HTTP, 1 - HTTPS. Default value is 0
# Number: 0, 1
P900 = 0

# Port. HTTP default is 80, HTTPS default is 443
# Number: 0 - 65535
P901 = 80

# SIP TLS Certificate
# P280 =

# SIP TLS Private Key
# P279 = 

# SIP TLS Private Key Password
P281 = s1pphone

# Minimum TLS Version. 10 - TLS1.0,  11 - TLS1.1,  12 - TLS1.2. Default value is 11.
# Number: 10, 11, 12
P22293 = 11

# Maximum TLS Version. 10 - TLS1.0,  11 - TLS1.1,  12 - TLS1.2, 99 - No limit. Default value is 99.
# Number: 10, 11, 12, 99
P22294 = 99
#######################################################################
##  Maintenance - Upgrade                                            ##
#######################################################################

# Firmware Upgrade Mode.0 - TFTP, 1 - HTTP, 2 - HTTPS. Default value is 2
# Number: 0, 1, 2
P6767 = 2

# Firmware HTTP/HTTPS Username
P6768 =

# Firmware HTTP/HTTPS Password
P6769 =

# Firmware Server Path
P192 = fm.grandstream.com/gs

# Firmware File Prefix
P232 =

# Firmware File Postfix
P233 =

# Config Upgrade Mode. 0 - TFTP, 1 - HTTP, 2 - HTTPS. Default value is 2
# Number: 0, 1, 2
P212 = 2

# Config HTTP/HTTPS User Name
P1360 =

# Config HTTP/HTTPS Password
P1361 =

# Config Server Path
P237 = fm.grandstream.com/gs

# Config File Prefix
P234 =

# Config File Postfix
P235 = 

# XML Config File Password
P1359 = 

# Authenticate Conf File. 0 - No, 1 - Yes. Default is 0.
# Number: 0, 1
P240 = 0

# Always send HTTP Basic Authentication Information. 0 - No, 1 - Yes.
# Number: 0, 1
P20713 = 0

# CUST File
# GUI Customization File URL.
# String
P6774 = fm.grandstream.com/gs

# CUST File
# GUI Customization File Download Mode. 0 - TFTP, 1 - HTTP, 2 - HTTPS. Default value is 1.
# Number: 0, 1, 2
P6775 = 1

# CUST File
# GUI Customization File HTTP/HTTPS Username.
P6776 =

# CUST File
# GUI Customization File HTTP/HTTPS Password.
P6777 =

# CUST File
# Use Configurations of Config File Server. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1
P6778 = 0

# Automatic Upgrade. 0 - No, 1 - Check Every Day, 2 - Check Every Week, 3 - Check at a Period Time. Default value is 1
# Number: 0, 1, 2, 3
P194 = 1

# Automatic Upgrade Check Interval (m). Minimum 60 minutes. Default value is 10080 (7 days)
# Number: 60 - 5256000
P193 = 10080

# Hour of the day (0-23)
# Number: 0 - 23
P285 = 1

# Day of the week (0-6)
# Number: 0 - 6
P286 = 1

# Firmware Upgrade and configuration File Detection. Default value is 0
# 0 - Always Check When Bootup
# 1 - When F/W pre/suffix changes
# 2 - Skip the Firmware Check
# Number: 0, 1, 2
P238 = 0

# Auto Reboot to Upgrade Without Prompt. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P1549 = 1

# Validate Server Certificate. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P22030 = 0

# mDNS Override Server. 0 - Disable, 1 - Use Type A, 2 - Use Type SRV. Default value is 1
# Number: 0, 1
P1407 = 1

# Allow DHCP Option 43 and option 66 Override server. 0 - No, 1 - Yes. Default value is 1
# When set to Yes(1), it will override the configured provision path and method
# Number: 0, 1
P145 = 1

# 3CX Auto Provision. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P1414 = 1

# Disable SIP NOTIFY Authentication. 0 - No, 1 - Yes. Default Value is 0
# Number : 0, 1
P4428 = 0

#######################################################################
##  Maintenance - TR-069                                             ##
#######################################################################

# Enable TR-069. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1
P1409 = 0

# ACS URL.
# String
P4503 = 

# ACS Username.
# String
P4504 = 

# ACS Password.
# String
P4505 = 

# Enable Periodic Inform. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1
P4506 = 0

# Periodic Inform Interval (s). Default value is 86400.
P4507 = 86400

# Connection Request Username.
# String
P4511 = 

# Connection Request Password.
# String
P4512 = 

# Connection Request Port.
# String
P4518 = 

# CPE Cert File.
# String
P8220 = 

# CPE Cert Key.
# String
P8221 = 

#######################################################################
##  Maintenance - Time & Language                                    ##
#######################################################################

# Assign NTP Server Address 1
P30 = us.pool.ntp.org

# Assign NTP Server Address 2
P8333 =

# Time Zone
# Web GUI Option         			   							P Value
# GMT-11:00(Midway Island)             							TZB+11
# GMT-10:00(Hawaii)                    							HAW10
# GMT-8:00(Alaska)                     							AKST9AKDT
# GMT-7:00(Pacific Time)               							PST8PDT
# GMT-7:00(Tijuana)                    							PST8PDT,M4.1.0,M10.5.0
# GMT-7:00(Arizona)												MST7
# GMT-6:00(Chihuahua)                  							MST7MDT,M4.1.0,M10.5.0
# GMT-6:00(Mountain Time)										MST7MDT
# GMT-6:00(Central America)            							CST+6
# GMT-5:00(Central Time)               							CST6CDT     
# GMT-5:00(Mexico City)                							CST6CDT,M4.1.0,M10.5.0
# *GMT-6:00(Saskatchewan)
# GMT-5:00(Bogota)												COT5
# *GMT-5:00(Estern Time without daylight saving)                
# GMT-4:00(Estern Time)                                         EST5EDT
# GMT-4:30(Venezuela)											TZf+4:30
# GMT-4:00(Atlantic Time(Barbados))   						    AST4ADT
# GMT-4:00(Atlantic Time(Canada)) 								AST4ADT
# GMT-4:00(Manaus)												AMT4
# GMT-3:30(Newfoundland)                            			NST+3:30NDT+2:30,M3.2.0/00:01:00,M11.1.0/00:01:00
# *GMT-3:00(Santiago)
# *GMT-3:00(Recife)
# GMT-3:00(Buenos Aires)										UTC+3
# GMT-3:00(Greenland)                               			TZK+3
# GMT-2:00(Brasilia) 											BRST+3BRDT+2,M10.3.0,M2.3.0
# GMT-2:00(Montevideo)											UYT3UYST,M10.1.0,M3.2.0
# GMT-2:00(Mid-Atlantic)                            			TZL+2
# GMT-1:00(Azores)                                  			TZM+1
# GMT-1:00(Cape Verde Islands)									CVT1
# GMT+0:00(GMT)													GMT+0BST-1,M3.5.0/01:00:00,M10.5.0/02:00:00
# GMT+0:00(Casablanca)                              			TZN+0
# GMT+0:00(London)                                  			GMT+0BST-1,M3.5.0/01:00:00,M10.5.0/02:00:00
# *GMT+1:00(Amsterdam,Berlin)
# GMT+1:00(Belgrade)											CET-1CEST,M3.5.0,M10.5.0/3
# GMT+1:00(Brussels)											TZO-1
# GMT+1:00(Madrid)			                                    CET-1CEST-2,M3.5.0/02:00:00,M10.5.0/03:00:00
# GMT+1:00(Sarajevo)											CET-1CEST,M3.5.0,M10.5.0/3
# *GMT+1:00(W. Africa Time)
# GMT+2:00(Windhoek)											WAT-1WAST,M9.1.0,M4.1.0
# *GMT+2:00(Amman, Jordan)
# GMT+2:00(Athens, Istanbul)									TZP-2
# GMT+2:00(Istanbul)									        
# GMT+2:00(Beirut, Lebanon)										EET-2EEST,M3.5.0/0,M10.5.0/0
# GMT+2:00(Cairo)												TZP-2
# GMT+2:00(Helsinki)	                                        EET-2EEST-3,M3.5.0/03:00:00,M10.5.0/04:00:00
# GMT+2:00(Jerusalem)											TZP-2
# GMT+2:00(Harare)												CAT-2
# GMT+3:00(Minsk)												EET-2EEST,M3.5.0,M10.5.0/3
# GMT+3:00(Baghdad)												AST-3
# GMT+3:00(Moscow)												MST-3MDT,M3.5.0/2,M10.5.0/3
# GMT+3:00(Kuwait)												TZQ-3
# GMT+3:00(Nairobi)												TZQ-3
# GMT+3:30(Tehran)												TZQ-3
# GMT+4:00(Baku)												TZR-4
# GMT+4:00(Tbilisi)												GET-4
# GMT+4:00(Yerevan)												AMT-4AMST,M3.5.0,M10.5.0/3
# GMT+4:00(Dubai)												GST-4
# GMT+4:30(Kabul)												AFT-4:30
# GMT+5:00(Islamabad, Karachi)									TZS-5
# *GMT+5:00(Ural'sk)
# GMT+5:00(Yekaterinburg)										YEKT-5YEKST,M3.5.0,M10.5.0/3
# *GMT+5:30(Kolkata)
# *GMT+5:30(Sri Lanka)										
# GMT+5:45(Kathmandu)											TZU-5:45
# GMT+6:00(Astana)												TZV-6
# GMT+6:30(Yangon)												TZW-6:30
# GMT+7:00(Krasnoyarsk)											TZX-7 
# GMT+7:00(Bangkok)												TZX-7
# GMT+7:00(Jakarta)												TZX-7
# GMT+8:00(Beijing)												TZY-8
# GMT+8:00(Hong Kong)											TZY-8
# GMT+8:00(Irkutsk)												TZY-8
# GMT+8:00(Kuala Lumpur)										TZY-8
# GMT+8:00(Perth)												WST-8
# GMT+8:00(Taipei)                                				TZY-8
# GMT+9:00(Seoul)												TZZ-9
# GMT+9:00(Tokyo, Osaka)										TZZ-9
# GMT+9:00(Yakutsk)											    YAKT-9YAKST,M3.5.0,M10.5.0/3
# GMT+9:30(Darwin)												CST-9:30
# GMT+10:00(Brisbane)											EST-10
# GMT+10:00(Vladivostok)										VLAT-10VLAST,M3.5.0,M10.5.0/3
# GMT+10:00(Guam)												TZb-10
# GMT+10:30(Adelaide)											CST-9:30CDT-10:30,M10.5.0/02:00:00,M3.5.0
# GMT+11:00(Hobart)												EST-10EDT-11,M10.1.0/02:00:00,M3.5.0/03:00:00
# GMT+11:00(Sydney, Canberra)									EST-10EDT-11,M10.5.0/02:00:00,M3.5.0/03:00:00
# *GMT+11:00(Noumea, New Caledonia)
# *GMT+12:00(Magadan)											MAGT-11MAGST,M3.5.0,M10.5.0/3			
# *GMT+12:00(Marshall Islands)                                   
# GMT+13:00(Auckland)											NZST-12NZDT-13,M10.1.0/02:00:00,M3.3.0/03:00:00
# GMT+13:00(Fiji)												FJT-12
# GMT+13:00(Tonga)                                              TZe-13
P64 = EST5EDT

# Use 24-hour Format. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P122 = 1

# DHCP Option 42 override NTP server. 0 - No, 1 - Yes. Default value is 1
# When set to Yes (1), it will override the configured NTP server
# Number: 0, 1
P144 = 1

# DHCP Option 2 to Override Time Zone setting. 0 - No, 1 - Yes. Default value is 1
# When set to Yes (1), it will override the configured Time Zone setting if available
# Number: 0, 1
P143 = 1

# Date Display Format. Default value is 1
# 0: YYYY-MM-DD
# 1: MM-DD-YYYY
# 2: DD-MM-YYYY
# 3: Normal (M-D-YYYY)
# Number: 0, 1, 2, 3
P102 = 1

# Language. Configure the language to be displayed on LCD
# Note: for some languages that have 2 codes avaiable, both are working
# ja_JP - 日本語
# zh_TW - 中文 (繁體), or zh-tw - 中文 (繁體)
# zh_CN - 中文 (简体), or zh - 中文 (简体)
# zh_HK - 中文 (香港), or zh - 中文 (香港)
# in_ID - Indonesian
# ms_MY - Bahasa Melayu
# af_ZA - Afrikaans
# ca_ES - Català
# cs_CZ - Ceština
# da_DK - Dansk
# de_DE - Deutsch
# de_LI - Deutsch (Liechtenstein)
# de_AT - Deutsch (Österreich)
# de_CH - Deutsch (Schweiz)
# en_AU - English (Australia)
# en_CA - English (Canada)
# en_NZ - English (New Zealand)
# en_SG - English (Singapore)
# en_GB - English (United Kingdom)
# en_US - English (United States), en - English (United States)
# es_ES - Español (España)
# es_US - Español (Estados Unidos)
# tl_PH - Filipino
# fr_BE - Français (Belgique)
# fr_CA - Français (Canada)
# fr_FR - Français, fr - Français
# fr_CH - Français (Suisse)
# hr_HR - Hrvatski
# zu_ZA - IsiZulu
# it_IT - Italiano, or it - Italiano
# it_CH - Italiano (Svizzera)
# sw_TZ - Kiswahili
# lv_LV - Latviešu
# lt_LT - Lietuvių
# hu_HU - Magyar, or hu - Magyar
# nl_BE - Nederlands (België)
# nl_NL - Nederlands, or nld - Nederlands
# nb_NO - Norsk bokmål
# pl_PL - Polski, or pl - Polski
# pt_BR - Português (Brasil)
# pt_PT - Português (Portugal)
# ro_RO - Româna
# rm_CH - Romansh
# sk_SK - Slovencina
# sl_SI - Slovenšcina
# fi_FI - Suomi, or fi
# sv_SE - Svenska, or sv - Svenska
# vi_VN - Tiếng Việt
# tr_TR - Türkçe, or tr - Türkçe
# el_GR - Greek
# bg_BG - Bulgarian
# ru_RU - Russian, or ru - Russian
# sr_RS - Serbian
# uk_UA - Ukrainian
# iw_IL - Hebrew
# ar_EG - العربية
# fa_IR - فارسی
# am_ET - አማርኛ
# hi_IN - हिन्दी
# th_TH - ไทย
# ko_KR - Korean
# Customized - Custom Language
P1362 = en_US

#######################################################################
##  Maintenance - Troubleshooting - Debug                           ##
#######################################################################

# Enable Core Dump Generation. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P29611 = 0

#######################################################################
##  Maintenance - Troubleshooting - Syslog                           ##
#######################################################################

# Syslog Protocol. 0 - UDP, 1 - SSL/TLS. Default value is 0.
# Number: 0, 1
P8402 = 0

# Syslog Server Address. Name of the server
# String
P207 = log.ipvideotalk.com

# Syslog Level
# 0 - NONE, 1 - DEBUG, 2 - INFO, 3 - WARNING, 4 - ERROR. Default value is 0
# Number: 0, 1, 2, 3, 4
P208 = 0

# Send SIP Log
# 0 - No, 1- Yes. Default value is 0
# Number: 0, 1
P1387 = 0

# Syslog Keyword Filter.
# String
P22129 = 

# H.323 Syslog Level. Default value is 0
# 0 - Off, 1 - 1, 2 - 2, 3 - 3, 4 - 4, 5 - 5, 6 - 6, 7 - 7, 8 - 8, 9 - 9, 10 - 10 
P25055 = 0

#######################################################################
##  Others                                                           ##
#######################################################################

# Lock SD card function. 0 - SD card function is locked, 1 - SD card function can be used. Default value is 1.
# When set to No(0), SD card will not be detected when it’s plugged in.
# Number: 0, 1
P22035 = 1

# Lock USB function. 0 - USB function is locked, 1 - USB function can be used. Default value is 1.
# When set to No(0), USB device will not be detected when it’s plugged in.
# Number: 0, 1
P22036 = 1

# Lock WiFi function. 0 - WiFi function is locked, 1 - WiFi function can be used. Default value is 1.
# When set to No(0), WiFi icon will not display on the screen top status bar and WiFi will not work.
# Number: 0, 1
P22038 = 1