################################################################################################
## Configuration template for firmware version 1.1.0.45 (HT486 REV.2, HT286 REV.3)
################################################################################################
 
###########################################################################
# Advanced Settings. You must change this section for the device.
########################################################################### 

# Admin password for web interface
P2 = admin

# SIP Server
P47 = sip.mycompany.com

# Outbound Proxy
P48 = proxy.mycompany.com

# SIP User ID
P35 = 8000

# Authentication ID
P36 = 8000

# Authentication password
P34 = 0000

# NAT Traversal. 0 - Yes, 1 - No.
P52 = 0

# STUN server
P76 = stun.mycompany.com

################################################################################
# Firmware Upgrade
################################################################################

# Firmware Upgrade. 0 - TFTP Upgrade,  1 - HTTP Upgrade.
P212 = 0

# Firmware Server Path
P192 =

# Config Server Path
P237 =

# Firmware File Prefix
P232 =

# Firmware File Postfix
P233 =

# Config File Prefix
P234 =

# Config File Postfix
P235 =

# Automatic Upgrade. 0 - No, 1 - Yes (checking every defined days). Default is No.
# For both Firmware and Configuration update.
P194 = 0

# Check for new firmware every () minutes, unit is in minute, default is 7 days.
P193 = 10080

# Use firmware pre/postfix to determine if f/w is required
# 0 = Always Check for New Firmware 
# 1 = Check New Firmware only when F/W pre/suffix changes 
# 2 = Always Skip the Firmware Check
# For Firmware only.
P238 = 0

################################################################################
# Network Settings
################################################################################

# Allow incoming SIP messages from SIP proxy only. 0 - No, 1 - Yes.
P243 = 0

# Use DNS SRV. 0 - No, 1 - Yes.
P103 = 

# Use NAT IP.  This will enable our SIP client to use this IP in the SIP message. 
# Example 64.3.153.50.
P101 =

# Use STUN keep-alive to detect networks connectivity. 0 - No, 1 - Yes.
P474 = 0

# Total number of STUN response misses before DHCP restart.
P475 =

# Proxy-Require (A SIP extension to enable firewall penetration)
P197 =

# Use Random Port. 0 - No, 1 - Yes.
P78 = 0

# Local SIP port (default 5060)
P40 = 5060

# Local RTP port (1024-65535, default 5004)
P39 = 5004 

# Preferred Vocoder
# 0 - PCMU, 2 - G.726-32, 4 - G.723.1, 8 - PCMA, 18 - G.729A/B, 98 - iLBC, 9 - G.722

# First codec. 
P57 = 0

# Second codec. 
P58 = 8

# Third codec. 
P59 = 4

# Forth codec. 
P60 = 18

# Fifth codec. 
P61 = 2

# Sixth codec. 
P62 = 0

# Seventh codec. 
P46 = 98

# BudgeTone Specific
# Eighth codec. 
P98 = 9

# G723 rate. 0 - 6.3kbps encoding rate, 1 - 5.3kbps encoding rate
P49 = 0

# iLBC payload type. Between 96 and 127, default is 97.
P96 = 97

# iLBC Frame Size. 0 - 20ms(default), 1 - 30ms.
P97 = 0

# Silence Suppression. 0 - No, 1 - Yes.
P50 = 0

# Voice Frames per TX (up to 10/20/32/64 frames for G711/G726/G723/other codecs respectively)
P37 = 2

# Layer 3 QoS (IP Diff-Serv or Precedence value for RTP)
P38 = 48

# VoIP Layer 2 QoS. 802.1Q/VLAN Tag (VLAN classification for RTP)
P51 = 0

# VoIP Layer 2 QoS. 802.1p priority value (0 - 7)
P87 = 0

# PC Layer 2 QoS. 802.1Q/VLAN Tag (VLAN classification for RTP)
# HT486 Rev.2 only
P229 = 0

# PC Layer 2 QoS. 802.1p priority value (0 - 7)
# HT486 Rev.2 only
P230 = 0

################################################################################
# Registration settings
################################################################################

# SIP Registration. 0 - No, 1 - Yes.
P31 = 1

# Register Expiration (in seconds. default 1 hour, max 45 days) 
P239 = 3600

# Unregister On Reboot. 0 - No, 1 - Yes.
P81 = 0

# SIP Registration Failure Retry Wait Time. (in seconds. Between 1-3600, default is 20)
P138 = 20

# Keep-alive interval (in seconds. default 20 seconds)
P84 = 20

################################################################################
# DTMF settings
################################################################################

# Send DTMF. 8 - in audio, 1 - via RTP, 2 - via SIP INFO, 11 - In Audio & RTP & SIP INFO
# 9 - In Audio & RTP, 10 - IN Audio & SIP INFO, 3 - RTP & SIP INFO
P73 = 8

# DTMF Payload Type
P79 = 101

# Send Flash Event (Flash will be sent as a DTMF event if set to Yes). 0 - No, 1 - Yes.
P74 = 0

################################################################################
# Time settings
################################################################################

# NTP Server
P30 = time.nist.gov

################################################################################
# Misc settings
################################################################################

# User Caller Name (John Doe)
P3 = 

# Home NPA (For AOL dial plan translation)
# HT486 Rev.2, HT286 Rev.3 only
P259 =

# SIP User ID is phone number. 0 - No, 1 - Yes.
P63 = 0

# Early Dial (use "Yes" only if proxy supports 484 response). 0 - No, 1 - Yes.
P29 = 0

# Allow outgoing call without Registration. 0 - No, 1 - Yes.
P109 = 0

# Dial Plan Prefix (dial plan prefix string).
P66 =

# No Key Entry Timeout. Default - 4 seconds.
P85 = 4

# Use # as Dial Key (if set to Yes, "#" will function as the Dial key).
# 0 - No, 1 - Yes.
P72 = 1

# Voice Mail UserID (User ID/extension for 3rd party voice mail system)
# BT100 only
P33 =

# SUBSCRIBE for MWI. Whether or not send SUBSCRIBE for Message Waiting Indication.
# 0 - No, 1 - Yes.
P99 =

# Offhook Auto-Dial (User ID/extension to dial automatically when offhook)
P71 =

# Enable Call Features.  0 - No, 1 - Yes.
P191 = 1

# Use Bell-style 3-way Conference. 0 - No, 1 - Yes.
# For HT286/HT486 only
P108 = 0

# Disable Call-Waiting. 0 - No, 1 - Yes.
P91 = 0

# Disable Call-Waiting Caller-ID. 0 - No, 1 - Yes.
P714 = 0

# Onhook Threshold. Default 800ms.
# <value=0>Hookflash OFF
# <value=2>200 ms
# <value=4>400 ms
# <value=6>600 ms
# <value=8>800 ms
# <value=10>1000 ms
# <value=12>1200 ms
P245 = 8

# Send Anonymous (caller ID will be blocked if set to Yes). 0 - No, 1 - Yes.
P65 = 0

# Anonymous Method. 0 -Use From Header, 1 - Use Privacy Header.
P268 = 0

# Time to ring. The length of ringing if it does not answer a call. Default 60 seconds.
# Valid values 30/60/90/120 in seconds.
P185 = 60

# Special Feature.    100 - Standard, 101 - Nortel MCS, 102 - BroadSoft, 104 - Sonus ASX
# 106 - MediaRing, 107 - Level3, 108 - CBCOM, 109 - RNK
# BT100 Supports 100, 102, 106, 108, 109 only.
P198 = 

# Syslog Server (name of the server, max length is 64 charactors)
P207 = 

# Syslog Level (Default setting is NONE)
# 0 - NONE, 1 - DEBUG, 2 - INFO, 3 - WARNING, 4 - ERROR
P208 = 0

# Firmwae Key (AES 128, in Hexadecimal Representation) 
P242 =

# Lock Keypad Update. (configuration update via keypad is disabled if set to Yes)
# 0 - No, 1 - Yes.
P88 = 0

# Allow conf SIP Account in Basic Settings. 0 - No, 1 - Yes.
P241 = 0

# Override MTU Size.
P244 = 0

################################################################################
# BudgeTone Specific Settings
################################################################################

# Auto Answer. 0 - No, 1 - Yes.
P90 = 0

# Default Ring Tone. 0 - system ring tone, 1 - custom ring tone 1, 2 - custom ring tone 2
# 3 - custom ring tone 3.
P104 = 0

# Use custom ring tone 1 if incoming caller ID is the following:
P105 =

# Use custom ring tone 2 if incoming caller ID is the following:
P106 =

# Use custom ring tone 3 if incoming caller ID is the following:
P107 =

################################################################################
# HandyTone Specific Settings
################################################################################

# FXS Impedence
#
# <value="0" > Default setting is "600 Ohm (North America)"
# <value=0>600 Ohm (North America)
# <value=1>900 Ohm
# <value=2>600 Ohm + 2.16uF
# <value=3>900 Ohm + 2.16uF
# <value=4>CTR21 (270 Ohm + 750 Ohm||150nF)
# <value=5>Australia/New Zealand #1 (220 Ohm + 820 Ohm||120nF)
# <value=6>Slovakia/Slovenia/South Africa (220 Ohm + 820 Ohm||115nF)
# <value=7>New Zealand #2 (370 Ohm + 620 Ohm||310nF)
P86 = 0

# Caller ID Scheme
#
# <value="0">current setting is "Bellcore"
# <value=0>Bellcore (North America)
# <value=1>ETSI-FSK (France, Germany, Norway, Taiwan, UK-CCA)
# <value=2>ETSI-DTMF (Finland, Sweden)
# <value=3>DTMF-Denmark
# <value=4>CID-Canada
# <value=5>DTMF-Sweden
# <value=6>DTMF-Brazil
P200 = 0

# Onhook Voltage
#
# <value="2">current setting is "36V (High Power)"
# <value=1>18V (High Power)
# <value=5>24V (High Power)
# <value=2>36V (High Power)
# <value=3>48V (High Power)
# <value=4>51V (High Power)
# <value=6>18V (Low Power)
# <value=10>24V(Low Power)
# <value=7>36V (Low Power)
# <value=8>48V (Low Power)
# <value=9>51V (Low Power)
P206 = 2

# Polarity Reversal. 0 - No, 1 - Yes.
P205 = 0

# FAX Mode. 0 - T.38 (Auto Detect), 1 - Pass Through.
P228 = 0

# Default Session Expires (in seconds. default 180 seconds. Allowed value: 90-65535)
P260 = 180

# Minimum SE (in seconds. default 90 seconds, must be lower than or equal to P260)
P261 = 90

# Caller Request Timer (Request for timer when calling) 0 - no, 1 - yes
P262 = 0

# Callee Request Timer (Request for timer when called. i.e. if remote party supports timer but did not request for one) 0 - no, 1 - yes
P263 = 0

# Force Timer (Still use timer when remote party does not support timer) 0 - no, 1 - yes
P264 = 0

# UAC Specify Refresher. 0 - omit, 1 - UAC, 2 - UAS
P266 = 0

# UAS Specify Refresher. 1 - UAC, 2 - UAS
P267 = 1

# Force INVITE (Always refresh with INVITE instead of UPDATE even when remote party supports UPDATE) 0 - no, 1 - yes
P265 = 0

# Volume Amplification
# TX 
# <value=1> +6dB
# <value=2> +4dB
# <value=3> +2dB
# <value=0> 0dB
# <value=4> -2dB
# <value=5> -4dB
# <value=6> -6dB
P247 = 0 

# RX 
# <value=1> +6dB
# <value=2> +4dB
# <value=3> +2dB
# <value=0> 0dB
# <value=4> -2dB
# <value=5> -4dB
# <value=6> -6dB
P249 = 0

# Powerline Ring Tone
# Frequency (Hz). Allowed: 15-100. Default 20Hz
P1810 = 20
# ON (x10ms). Allowed: 5-800. Default 200.
P1811 = 200
# OFF (x10ms). Allowed: 5-800. Default 400.
P1812 = 400

##### Call Progress Tones #####
#
### Dial Tone ###
# Frequency 1 (Hz)
P1820 = 350
# Frequency 2 (Hz)
P1840 = 440
# ON (x 10ms)
P1860 = 0
# OFF (x 10ms)
P1880 = 0

### Recall Dial Tone ###
# Frequency 1 (Hz)
P1821 = 350
# Frequency 2 (Hz)
P1841 = 440
# ON (x 10ms)
P1861 = 10
# OFF (x 10ms)
P1881 = 10

### Message Waiting Tone ###
# Frequency 1 (Hz)
P1822 = 350
# Frequency 2 (Hz)
P1842 = 440
# ON (x 10ms)
P1862 = 10
# OFF (x 10ms)
P1882 = 10

### Confirmation Tone ###
# Frequency 1 (Hz)
P1823 = 350
# Frequency 2 (Hz)
P1843 = 440
# ON (x 10ms)
P1863 = 10
# OFF (x 10ms)
P1883 = 10

### Audiable Ringing ###
# Frequency 1 (Hz)
P1824 = 440
# Frequency 2 (Hz)
P1844 = 480
# ON (x 10ms)
P1864 = 200
# OFF (x 10ms)
P1884 = 400

### Busy Tone ###
# Frequency 1 (Hz)
P1825 = 480
# Frequency 2 (Hz)
P1845 = 620
# ON (x 10ms)
P1865 = 50
# OFF (x 10ms)
P1885 = 50

### Reorder Tone ###
# Frequency 1 (Hz)
P1826 = 480
# Frequency 2 (Hz)
P1846 = 620
# ON (x 10ms)
P1866 = 25
# OFF (x 10ms)
P1886 = 25

### Receiver offhook ###
# Frequency 1 (Hz)
P1827 = 1400
# Frequency 2 (Hz)
P1847 = 2600
# ON (x 10ms)
P1867 = 10
# OFF (x 10ms)
P1887 = 10

# Disable Line Echo Canceller (LEC). 0 - No, 1 - Yes.
P824 = 0

# Disable Voice Prompt. 0 - No, 1 - Yes.
P253 = 0

# Enable Toll Application. 0 - No, 1 - Yes. 
# Default No, set to Yes if connecting to toll pay device or phone
P257 = 0

###############################################################################
# End User Settings. Please do not edit this section.
###############################################################################

# End User Password
#P196 = 123

# Web Port. Device internal HTTP server port number. Default is 80.
# HT486 Rev.2, HT286 Rev.3 only
P901 = 80

# The following 4 fields will show in Basic Settings if
# "Allow conf SIP Account in Basic Settings" is set to "Yes". (P241 = 1)
# SIP User ID
#P35 = 

# Authentication ID
#P36 =

# Authentication password
#P34 = 0000

# User Caller Name (John Doe)
#P3 = 

# DHCP support. 0 - Yes, 1 - No.
#P8 = 0

# Host name, DHCP option 12. Max length allowed is 32 bytes.
P146 =

# Domain name, DHCP option 15. Max length allowed is 32 bytes.
P147 =

# Vendor Class ID, DHCP option 60. Max length allowed is 32 bytes.
P148 = 

# PPPoE support. PPPoE user ID
#P82 =

# PPPoE password
#P83 =

# PPPoE Service Name
#P269 =

# IP Address. Ignore if DHCP or PPPoE is used
#P9 = 
#P10 = 
#P11 = 
#P12 = 

# Subnet mask. Ignore if DHCP or PPPoE is used
#P13 = 255
#P14 = 255
#P15 = 255
#P16 = 0

# Router. Ignore if DHCP or PPPoE is used
#P17 = 
#P18 = 
#P19 = 
#P20 = 

# Use this DNS server.  (if specified).
#P92 = 
#P93 = 
#P94 = 
#P95 = 

# DNS 1. Ignore if DHCP or PPPoE is used
#P21 = 
#P22 = 
#P23 = 
#P24 = 

# DNS 2. Ignore if DHCP or PPPoE is used
#P25 = 0
#P26 = 0
#P27 = 0
#P28 = 0

# Time Zone. Offset in minutes to GMT
#P64 = 420

# Daylight Savings Time. 0 - No, 1 - Yes.
#P75 = 0

# Optional Rule. Daylight Saving rule.
# HT486 Rev.2, HT286 Rev.3 only
P246 = 4,1,7,2,0;10,-1,7,2,0;60

# Date Display Format. 0 - Year-Month-Day, 1 - Month-Day-Year, 2 - Day-Month-Year
# BT100 only
P102 = 0

########################################################################
# HandyTone 486 Specific End User NAT Settings. Please do not edit.
########################################################################

# PSTN Access Code.   Default = *00
P195 =

# Device Mode. 0 - NAT Router, 1 - Bridge. Default is 0.
P231 = 0

# WAN side http access.  0 - Disable(default), 1 - Yes.
P190 = 0 

# Reply to ICMP on WAN port (Unit will not respond to PING from WAN side if set to No)
# 0 - No, 1 - Yes.
P189 = 0

#Cloned WAN MAC Address.
P115 =
P116 =
P117 =
P118 =
P119 =
P120 =

#LAN Subnet Mask.  Default is 255.255.255.0.
P110 = 

#LAN Base/Gateway/Router IP for the LAN port, default is 192.168.2.1.
P111 = 

#DHCP IP Lease Time, in units of hours, default is 120 hours or 5 days.
P112 = 

#DMZ IP.
P113 =

################################################################################
# Port Forwarding.
################################################################################

#############  Choice 1 ####################################
# WAN Port
P150 =
# LAN IP
P158 =
# LAN Port
P166 =
# Protocol.  0 - UDP Only, 1 - TCP Only, 2 - TCP and UDP.
P174 =
#############  Choice 2 ####################################
# WAN Port
P151 =
# LAN IP
P159 =
# LAN Port
P167 =
# Protocol.  0 - UDP Only, 1 - TCP Only, 2 - TCP and UDP.
P175 =
#############  Choice 3 ####################################
# WAN Port
P152 =
# LAN IP
P160 =
# LAN Port
P168 =
# Protocol.  0 - UDP Only, 1 - TCP Only, 2 - TCP and UDP.
P176 =
#############  Choice 4 ####################################
# WAN Port
P153 =
# LAN IP
P161 =
# LAN Port
P169 =
# Protocol.  0 - UDP Only, 1 - TCP Only, 2 - TCP and UDP.
P177 =
#############  Choice 5 ####################################
# WAN Port
P154 =
# LAN IP
P162 =
# LAN Port
P170 =
# Protocol.  0 - UDP Only, 1 - TCP Only, 2 - TCP and UDP.
P178 =
#############  Choice 6 ####################################
# WAN Port
P155 =
# LAN IP
P163 =
# LAN Port
P171 =
# Protocol.  0 - UDP Only, 1 - TCP Only, 2 - TCP and UDP.
P179 =
#############  Choice 7 ####################################
# WAN Port
P156 =
# LAN IP
P164 =
# LAN Port
P172 =
# Protocol.  0 - UDP Only, 1 - TCP Only, 2 - TCP and UDP.
P180 =
#############  Choice 8 ####################################
# WAN Port
P157 = 
# LAN IP
P165 = 
# LAN Port
P173 = 
# Protocol.  0 - UDP Only, 1 - TCP Only, 2 - TCP and UDP.
P181 = 

