###############################################################################################
####         Configuration Template for GVC3212 Firmware Version 1.0.1.6                   ####
###############################################################################################

##############################################################################
##		Network Settings - Ethernet Settings                       			##
##############################################################################
# IP Mode. 0 - Both, prefer IPv4, 1 - Both, prefer IPv6, 2 - IPv4 Only, 3 - IPv6 Only. Default is 0
# Number: 0, 1
# Mandatory
P1415=0

# IPv4 Address Type. 0 - DHCP, 1 - Static, 2 - PPPoE. Default value is 0
# Number: 0, 1. 2
P8=0

# DHCP VLAN override. 0 - Disable, 1 - DHCP Option 132 and DHCP Option 133, 2 - Encapsulated in DHCP Option 43
# Number: 0, 1, 2. Default is 2
# Mandatory
P8300=2

# Host name (DHCP option 12)
P146=

# Vendor Class ID (DHCP option 60). 
P148=Grandstream GVC3212

# Static IP. IP address
# P9=192
# P10=168
# P11=0
# P12=160

# Static IP. Subnet Mask
# P13=255
# P14=255
# P15=255
# P16=0

# Static IP. Default Gateway
# P17=192
# P18=168
# P19=0
# P20=1

# Static IP. DNS Server 1. Ignore if DHCP or PPPoE is used
# P21=0
# P22=0
# P23=0
# P24=0

# Static IP. DNS Server 2. Ignore if DHCP or PPPoE is used
# P25=0
# P26=0
# P27=0
# P28=0

# PPPoE Account ID
# P82=

# PPPoE Password
# P83=

# Layer 2 QoS 802.1Q/VLAN Tag(Ethernet). Default value is 0
# Number: 0 - 4095
P51=0

# Layer 2 QoS 802.1p Priority(Ethernet). Default value is 0
# Number: 0 - 7
P87=0

# IPv6 Address type. 0 - Auto Configured, 1 - Statically Configured. Default is 0.
# Number: 0, 1
# Mandatory
P1419=0

# Statically Configured: Static IPv6 Address
# P1420=

# Statically Configured: IPv6 Prefix Length
# P1421=

# Statically Configured: DNS Server 1 for IPv6 Address
# String: a-z, A-Z, 0-9, ".", ":", "[", "]"
# P1424=

# Statically Configured: DNS Server 2 for IPv6 Address
# String: a-z, A-Z, 0-9, ".", ":", "[", "]"
# P1425=

# Preferred DNS Server for IPv6 Address
# String: a-z, A-Z, 0-9, ".", ":", "[", "]"
# P1423=

# 802.1x Mode. 0 - Close, 1 - EAP-MD5, 2 - EAP-TLS, 3-EAP-PEAP. Default is 0
# Number: 0, 1, 2, 3
P7901=0

# 802.1x Identity
#P7902=

# 802.1 Secret
#P7903=

##############################################################################
##				Network Settings - Wi-Fi Settings                           ##
##############################################################################
# Wi-Fi Function. 0 - off, 1 - on. 
P7800=0

# Add Network
# ESSID 
P7812=

# Security Mode for Hidden SSID. 0 - None, 1 - WEP, 2 - WPA WPA2 PSK. Default value is 0.
# Number: 0, 1, 2
P7814=0

# Password
P7830=

# Advanced Settings
# Layer 2 QoS 802.1p Priority Value (Wi-Fi)
P22048=

# Country Code. Default is US.
# String
P7831=US



 
##############################################################################
##     			 Network Settings - Advanced Network Settings       	    ##
##############################################################################

# Preferred DNS 1
#P92=0
#P93=0
#P94=0
#P95=0

# Preferred DNS 2
#P5026=
#P5027=
#P5028=
#P5029=

# Enable LLDP. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P1684=1

# LLDP TX Interval (s)
P22122=30

# Enable CDP. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P22119=1


# HTTP/HTTPS User-Agent
P1541=

# HTTP/HTTPS Proxy Hostname and Port.
# The default format is "hostname:port number". If the host name is "Grandstream", the port number is "123", the value should be "Grandstream:123".
P1553=

# Bypass Proxy For
# String
P22011=
##################################################################
##     	       System Settings - Power Manager				    ##
##################################################################
# Auto Sleep Timeout 

##################################################################
##     	       System Settings - Time and Language			    ##
##################################################################
# NTP Server
P30=us.pool.ntp.org

# Allow DHCP Option 42 override NTP server. 0 - No, 1 - Yes. Default value is 1
# When set to Yes (1), it will override the configured NTP server
# Number: 0, 1
P144=1

# Allow DHCP Option 2 to Override Time Zone setting. 0 - No, 1 - Yes. Default value is 1
# When set to Yes (1), it will override the configured Time Zone setting if available
# Number: 0, 1
P143=1

# Time Zone
# Web GUI Option         			   							P Value
# GMT-11:00(Midway Island)             							TZB+11
# GMT-10:00(Hawaii)                    							HAW10
# GMT-8:00(Alaska)                     							AKST9AKDT
# GMT-7:00(Pacific Time)               							PST8PDT
# GMT-7:00(Tijuana)                    							PST8PDT,M4.1.0,M10.5.0
# GMT-7:00(Arizona)												MST7
# GMT-6:00(Chihuahua)                  							MST7MDT,M4.1.0,M10.5.0
# GMT-6:00(Mountain Time)										MST7MDT
# GMT-6:00(Central America)            							CST+6
# GMT-5:00(Central Time)               							CST6CDT     
# GMT-5:00(Mexico City)                							CST6CDT,M4.1.0,M10.5.0
# *GMT-6:00(Saskatchewan)
# GMT-5:00(Bogota)												COT5
# *GMT-5:00(Estern Time without daylight saving)                
# GMT-4:00(Estern Time)                                         EST5EDT
# GMT-4:30(Venezuela)											TZf+4:30
# GMT-4:00(Atlantic Time(Barbados))   						    AST4ADT
# GMT-4:00(Atlantic Time(Canada)) 								AST4ADT
# GMT-4:00(Manaus)												AMT4
# GMT-3:30(Newfoundland)                            			NST+3:30NDT+2:30,M3.2.0/00:01:00,M11.1.0/00:01:00
# *GMT-3:00(Santiago)
# *GMT-3:00(Recife)
# GMT-3:00(Buenos Aires)										UTC+3
# GMT-3:00(Greenland)                               			TZK+3
# GMT-2:00(Brasilia) 											BRST+3BRDT+2,M10.3.0,M2.3.0
# GMT-2:00(Montevideo)											UYT3UYST,M10.1.0,M3.2.0
# GMT-2:00(Mid-Atlantic)                            			TZL+2
# GMT-1:00(Azores)                                  			TZM+1
# GMT-1:00(Cape Verde Islands)									CVT1
# GMT+0:00(GMT)													GMT+0BST-1,M3.5.0/01:00:00,M10.5.0/02:00:00
# GMT+0:00(Casablanca)                              			TZN+0
# GMT+0:00(London)                                  			GMT+0BST-1,M3.5.0/01:00:00,M10.5.0/02:00:00
# *GMT+1:00(Amsterdam,Berlin)
# GMT+1:00(Belgrade)											CET-1CEST,M3.5.0,M10.5.0/3
# GMT+1:00(Brussels)											TZO-1
# GMT+1:00(Madrid)			                                    CET-1CEST-2,M3.5.0/02:00:00,M10.5.0/03:00:00
# GMT+1:00(Sarajevo)											CET-1CEST,M3.5.0,M10.5.0/3
# *GMT+1:00(W. Africa Time)
# GMT+2:00(Windhoek)											WAT-1WAST,M9.1.0,M4.1.0
# *GMT+2:00(Amman, Jordan)
# GMT+2:00(Athens, Istanbul)									TZP-2
# GMT+2:00(Istanbul)									        
# GMT+2:00(Beirut, Lebanon)										EET-2EEST,M3.5.0/0,M10.5.0/0
# GMT+2:00(Cairo)												TZP-2
# GMT+2:00(Helsinki)	                                        EET-2EEST-3,M3.5.0/03:00:00,M10.5.0/04:00:00
# GMT+2:00(Jerusalem)											TZP-2
# GMT+2:00(Harare)												CAT-2
# GMT+3:00(Minsk)												EET-2EEST,M3.5.0,M10.5.0/3
# GMT+3:00(Baghdad)												AST-3
# GMT+3:00(Moscow)												MST-3MDT,M3.5.0/2,M10.5.0/3
# GMT+3:00(Kuwait)												TZQ-3
# GMT+3:00(Nairobi)												TZQ-3
# GMT+3:30(Tehran)												TZQ-3
# GMT+4:00(Baku)												TZR-4
# GMT+4:00(Tbilisi)												GET-4
# GMT+4:00(Yerevan)												AMT-4AMST,M3.5.0,M10.5.0/3
# GMT+4:00(Dubai)												GST-4
# GMT+4:30(Kabul)												AFT-4:30
# GMT+5:00(Islamabad, Karachi)									TZS-5
# *GMT+5:00(Ural'sk)
# GMT+5:00(Yekaterinburg)										YEKT-5YEKST,M3.5.0,M10.5.0/3
# *GMT+5:30(Kolkata)
# *GMT+5:30(Sri Lanka)										
# GMT+5:45(Kathmandu)											TZU-5:45
# GMT+6:00(Astana)												TZV-6
# GMT+6:30(Yangon)												TZW-6:30
# GMT+7:00(Krasnoyarsk)											TZX-7 
# GMT+7:00(Bangkok)												TZX-7
# GMT+7:00(Jakarta)												TZX-7
# GMT+8:00(Beijing)												TZY-8
# GMT+8:00(Hong Kong)											TZY-8
# GMT+8:00(Irkutsk)												TZY-8
# GMT+8:00(Kuala Lumpur)										TZY-8
# GMT+8:00(Perth)												WST-8
# GMT+8:00(Taipei)                                				TZY-8
# GMT+9:00(Seoul)												TZZ-9
# GMT+9:00(Tokyo, Osaka)										TZZ-9
# GMT+9:00(Yakutsk)											    YAKT-9YAKST,M3.5.0,M10.5.0/3
# GMT+9:30(Darwin)												CST-9:30
# GMT+10:00(Brisbane)											EST-10
# GMT+10:00(Vladivostok)										VLAT-10VLAST,M3.5.0,M10.5.0/3
# GMT+10:00(Guam)												TZb-10
# GMT+10:30(Adelaide)											CST-9:30CDT-10:30,M10.5.0/02:00:00,M3.5.0
# GMT+11:00(Hobart)												EST-10EDT-11,M10.1.0/02:00:00,M3.5.0/03:00:00
# GMT+11:00(Sydney, Canberra)									EST-10EDT-11,M10.5.0/02:00:00,M3.5.0/03:00:00
# *GMT+11:00(Noumea, New Caledonia)
# *GMT+12:00(Magadan)											MAGT-11MAGST,M3.5.0,M10.5.0/3			
# *GMT+12:00(Marshall Islands)                                   
# GMT+13:00(Auckland)											NZST-12NZDT-13,M10.1.0/02:00:00,M3.3.0/03:00:00
# GMT+13:00(Fiji)												FJT-12
# GMT+13:00(Tonga)                                              TZe-13
P64=PST8PDT

# Use 24-hour Format. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P122=1


# Date Display Format. Default value is 3
# 0: YYYY-MM-DD
# 1: MM-DD-YYYY
# 2: DD-MM-YYYY
# 3: Normal (YYYY-M-D)
# Number: 0, 1, 2, 3
P102=3

# Language. Configure the language to be displayed on LCD
# Note: for some languages that have 2 codes avaiable, both are working
# ja_JP - 日本語
# zh_TW - 中文 (繁體), or zh-tw - 中文 (繁體)
# zh_CN - 中文 (简体), or zh - 中文 (简体)
# zh_HK - 中文 (香港), or zh - 中文 (香港)
# in_ID - Indonesian
# ms_MY - Bahasa Melayu
# af_ZA - Afrikaans
# ca_ES - Català
# cs_CZ - Ceština
# da_DK - Dansk
# de_DE - Deutsch
# de_LI - Deutsch (Liechtenstein)
# de_AT - Deutsch (Österreich)
# de_CH - Deutsch (Schweiz)
# en_AU - English (Australia)
# en_CA - English (Canada)
# en_NZ - English (New Zealand)
# en_SG - English (Singapore)
# en_GB - English (United Kingdom)
# en_US - English (United States), en - English (United States)
# es_ES - Español (España)
# es_US - Español (Estados Unidos)
# tl_PH - Filipino
# fr_BE - Français (Belgique)
# fr_CA - Français (Canada)
# fr_FR - Français, fr - Français
# fr_CH - Français (Suisse)
# hr_HR - Hrvatski
# zu_ZA - IsiZulu
# it_IT - Italiano, or it - Italiano
# it_CH - Italiano (Svizzera)
# sw_TZ - Kiswahili
# lv_LV - Latviešu
# lt_LT - Lietuvių
# hu_HU - Magyar, or hu - Magyar
# nl_BE - Nederlands (België)
# nl_NL - Nederlands, or nld - Nederlands
# nb_NO - Norsk bokmål
# pl_PL - Polski, or pl - Polski
# pt_BR - Português (Brasil)
# pt_PT - Português (Portugal)
# ro_RO - Româna
# rm_CH - Romansh
# sk_SK - Slovencina
# sl_SI - Slovenšcina
# fi_FI - Suomi, or fi
# sv_SE - Svenska, or sv - Svenska
# vi_VN - Tiếng Việt
# tr_TR - Türkçe, or tr - Türkçe
# el_GR - Greek
# bg_BG - Bulgarian
# ru_RU - Russian, or ru - Russian
# sr_RS - Serbian
# uk_UA - Ukrainian
# iw_IL - Hebrew
# ar_EG - العربية
# fa_IR - فارسی
# am_ET - አማርኛ
# hi_IN - हिन्दी
# th_TH - ไทย
# ko_KR - Korean
# Customized - Custom Language
P1362=en_US

######################################################################
##     	       System Settings - Security Settings 		            ##
######################################################################
# Web/SSH Access

# Enable SSH. 0 - Yes, 1 - No. Default value is 0
# Number: 0, 1
P276=0

#SSH port
P27006=22

# Access Method. 0 - HTTP, 1 - HTTPS. Default value is 0
# Number: 0, 1
P900=0

# Port. HTTP default is 80, HTTPS default is 443
# Number: 0 - 65535
P901=80

#User Info Management
# Admin password for web interface
P2=admin

# End User Password
P196=user

#Certificate Management


######################################################################
##     	       System Settings - Audio Control					    ##
######################################################################
#Audio In

# Audio Out Device. 0 - Auto, 1 - Bluetooth, 2 - USB, 3 - HDMI. Default value is 0
# Number: 0, 1, 2, 3
P22050 = 0

# Echo Delay. 0 - -2, 10 - -1, 20 - 0, 30 - 1, 40 - 2, 50 - 3, 60 - 4, 70 - 5, 
# 80 - 6, 90 - 7, 100 - 8, 110 - 9, 120 - 10, 130 - 11, 140 - 12, 150 - 13, 
# 160 - 14, 170 - 15, 180 - 16, 190 - 17.
P22280=

#Volume

######################################################################
##     	       Device Control - Peripheral						    ##
######################################################################
# HDMI out resolution

# Screen Percent


##############################################################
##     	       Maintenance - Upgrade					    ##
##############################################################

# Firmware 

# Complete Upgrade
# Firmware Upgrade Mode.0 - TFTP, 1 - HTTP, 2 - HTTPS. Default value is 1
# Number: 0, 1, 2
P6767=1

# Firmware Server Path
P192=fw.ipvideotalk.com/gvc3212

# Firmware HTTP/HTTPS Username
P6768=

# Firmware HTTP/HTTPS Password
P6769=

# Firmware File Prefix
P232=

# Firmware File Postfix
P233=

# Config File

# Config Upgrade Mode. 0 - TFTP, 1 - HTTP, 2 - HTTPS. Default value is 2
# Number: 0, 1, 2
P212=2

# Config Server Path
P237=fm.grandstream.com/gs

# Config HTTP/HTTPS User Name
P1360=

# Config HTTP/HTTPS Password
P1361=

# Always send HTTP Basic Authentication Information. 0 - No, 1 - Yes.
# Number: 0, 1
P20713=0

# Config File Prefix
P234=

# Config File Postfix
P235=

# Authenticate Conf File. 0 - No, 1 - Yes. Default is 0.
# Number: 0, 1
P240=0

# XML Config File Password
P1359=

# Provision
# Automatic Upgrade. 0 - No, 1 - Check Every Day, 2 - Check Every Week, 3 - Check at a Period Time. Default value is 0
# Number: 0, 1, 2, 3
P194=0

# Enable Randomized Automatic Upgrade. 0 - No. 1 - Yes.
P8458=

# Automatic Upgrade Check Interval (m). Minimum 60 minutes. Default value is 10080 (7 days)
# Number: 60 - 5256000
P193=10080

# Starting Hour of the day (0-23)
# Number: 0 - 23
P285=1

# Ending Hour of the day (0-23)
# Number: 0 - 23
P8459=

# Day of the week (0-6)
# Number: 0 - 6
P286=1

# Firmware Upgrade Provisioning. Default value is 0
# 0 - Always Check When Bootup
# 1 - When F/W pre/suffix changes
# 2 - Skip the Firmware Check
# Number: 0, 1, 2
P238=0

# Upgrade With Prompt. 0 - Yes, 1 - No. Default value is 0
# Number: 0, 1
P1549=0

# Allow DHCP Option 43 and option 66 Override server. 0 - No, 1 - Yes. Default value is 1
# When set to Yes(1), it will override the configured provision path and method
# Number: 0, 1
P145=1

# Download and Process All Available Config Files. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P8467=0

#Advanced Settings

# Validate Server Certificate. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P22030=0

# Allow AutoConfig Service Access. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P7070=

# mDNS Override Server. 0 - Disable, 1 - Use Type A, 2 - Use Type SRV. Default value is 1
# Number: 0, 1, 2
P1407=1

##################################################################
##     	       Maintenance - System Diagnosis				    ##
##################################################################

# Syslog
# Syslog Protocol. 0 - UDP, 1 - SSL/TLS. Default value is 0.
# Number: 0, 1
P8402=0

# Syslog Server Address. Name of the server
# String
P207=log.ipvideotalk.com

# Syslog Level
# 0 - NONE, 1 - DEBUG, 2 - INFO, 3 - WARNING, 4 - ERROR. Default value is 0
# Number: 0, 1, 2, 3, 4
P208=0

# Syslog Keyword Filter.
# String
P22129=

# Debug
# Enable Core Dump Generation. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P29611 = 0

