############################################################################################
## Configuration template for HT813 firmware version 1.0.7.1                              ##
############################################################################################



##############################################################################
##  Advanced Settings.                                                      ##
##############################################################################

# Admin password for web interface
# Mandatory; between ascii values 33 and 126
P2 = admin

# Layer 2 QoS. 802.1Q/VLAN Tag (VLAN classification for RTP)
# Number: 0 to 4094
# Mandatory
# Reboot required
P51 = 0

# Layer 2 QoS. SIP 802.1p value (0 - 7)
# Number: 0 to 7
# Mandatory
# Reboot required
P5038 = 0

# Layer 2 QoS. RTP 802.1p value (0 - 7)
# Number: 0 to 7
# Mandatory
# Reboot required
P5042 = 0

# Black List for WAN Side. The IP address in black list can not access Web or SSH.
# String ipaddress
P28115 = 

# STUN server
# Server address
P76 = stun.mycompany.com

# Keep-alive interval (in seconds. default 20 seconds)
# Number: 10 to 160
# Mandatory
P84 = 20

# Use STUN to detect network connectivity (0 - No, 1 - Yes. default No)
# Number: 0, 1
# Mandatory
P474 = 0

# If Yes, total STUN response misses to restart DHCP client(mininum=3, default=3)
# Number: 3 to 15
# Mandatory
P475 = 3

# Use DNS to detect network connectivity
# Number: 0, 1
# 0 - No, 1 - Yes (default is No)
P1564=0

################################################################################
# Firmware Upgrade                                                             #
################################################################################
# Verify host when using HTTPS
# Number: 0, 1
# 0 - No, 1 - Yes (default is No)
P22030=0

# Firmware Upgrade and Privisioning. 0 - TFTP Upgrade, 1 - HTTP Upgrade, 2 - HTTPS Upgrade, 3 - FTP Upgrade, 4 - FTPS Update.
# Number: 0, 1, 2, 3, 4
# Mandatory
P212 = 2

# Firmware Server Path
P192 = fm.grandstream.com/gs

# Config Server Path
P237 = fm.grandstream.com/gs

# XML Config File Password
# String; between ascii values 33 and 126
P1359 = 

# HTTP/HTTPS/FTP/FTPS User Name
# String; between ascii values 33 and 126
P1360 =

# HTTP/HTTPS/FTP/FTPS Password
# String; between ascii values 33 and 126
P1361 =

# Firmware File Prefix
# String; between ascii values 33 and 126
P232 =

# Firmware File Postfix
# String; between ascii values 33 and 126
P233 =

# Config File Prefix
# String; between ascii values 33 and 126
P234 =

# Config File Postfix
# String; between ascii values 33 and 126
P235 =

# Allow DHCP Option 66 or 160 to override server. 0 - No, 1 - Yes. Default is Yes.
# When set to Yes(1), it will override the configured provision path and method.
# Number: 0, 1
# Mandatory
# Reboot required
P145 = 1

# 3CX Auto Provision. 0 - No, 1 - Yes. Default is 1 - Yes.
# Number: 0, 1
# Mandatory
P1414 = 1

# Automatic Upgrade. 0 - No, 1 - Check every () minutes, 2 - Check daily, 3 - Check weekly. Default is No.
# Number: 0, 1, 2, 3
# Mandatory
P22296 = 0

# Check for new firmware/config file every () minutes, unit is in minute, minimum 30 minutes, default is 7 days. P194 = 3
# Number: 30 to 5256000
# Mandatory
P193 = 10080

# Automatic Upgrade. Daily at start hour(0-23). P194 = 1
# Number: 0 to 23
# Mandatory
P285 = 1

# Automatic Upgrade. Daily at end hour(0-23). P194 = 1
# Number: 0 to 23
# Mandatory
P8459 = 22

# Automatic Upgrade. Weekly on day (0-6). P194 = 2
# Number: 0 to 6
# Mandatory
P286 = 1

# Randomized Automatic Upgrade. 0 - No, 1 - Yes. Default is No.
# Number: 0, 1
# Mandatory
P8458 = 0

# Use firmware pre/postfix to determine if f/w is required
# 0 = Always Check for New Firmware at Boot up
# 1 = Check New Firmware only when F/W pre/suffix changes 
# 2 = Always Skip the Firmware Check
# For Firmware only.
# Number: 0, 1, 2
# Mandatory
P238 = 0

# Disable SIP NOTIFY Authentication
# Number: 0 No, 1 Yes  (Device will not challenge NOTIFY with 401 when set to Yes) 
# Mandatory
P4428 = 0

# Authenticate Conf File
# Number: 0 No, 1 Yes  (cfg file would be authenticated before acceptance if set to Yes) 
# Mandatory
P240 = 0

# Validate Server Certificates. 0 - No, 1 - Yes, default is No. Need to reboot the device upon change the value
# Number: 0, 1
# Mandatory
P8463=0

# Trusted CA Certificates A
# String
P2386 = 

# Trusted CA Certificates B
# String
P2486 = 

# Load CA Certificates. 0 - Built-in trusted certificates, 1 - Custom trusted certificates, 2 - All trusted certificates
# Number: 0, 1, 2 
# Mandatory
P8502 = 0

# SIP TLS Certificate
# String
P280 =

# SIP TLS Private Key
# String
P279 =
	
# SIP TLS Private Key Password
# String
# Max Length: 64 characters
P281 = 

# Custom Certificate. (Private Key + Certificate)
# String
P8472 = 

# Enable TR-069. 0 - No, 1 - Yes (default is Yes)
# Number: 0, 1
# Mandatory
P1409=1

# ACS URL
#P4503 =

# ACS Username
# String
P4504 =

# ACS Password
# String
P4505 =

# Periodic Inform Enable 0 - No, 1 - Yes (default is No)
# Number: 0, 1
# Mandatory
P4506 = 0

# Periodic Inform Interval (default is 300)
# Max Length: 5 digits
P4507 = 300

# Conncetion Request Username
# String
P4511 =

# Connection Request Password
# String
P4512 =

# Connection Request Port (default is 7547)
# String
# Number: 0 - 65535
P4518 = 7547

# CPE SSL Certificate
# String
P8220 =

# CPE SSL Private Key
# String
P8221 =

# Enable SNMP. 0 - No, 1 - Yes, default value is 0.
# Number: 0, 1
# Mandatory
P21896=0

# SNMP Version. 1 - Version 1, 2 - Version 2c, 3 - Version 3. Default value is 3.
# Nmuber: 1, 2, 3
# Mandatory
P21904=3

# SNMP Port. Default is port 161
# Number: 161 or 1025 to 65535
# Mandatory
P21903=161

# SNMP Trap IP Address
# Max String Length: 64
P21897=

# SNMP Trap Port. Default value is 162.
# Number: 162 or 1025 to 65535
# Mandatory
P21898=162

# SNMP Trap Version. 1 - Version 1, 2 - Version 2c,3 - Version 3, default is Version 2c.
# Number: 1, 2, 3
# Mandatory
P21899= Version 2c

# SNMP Trap Interval. Default is 5.
# Number: 1-1440
P21901=5

# SNMPv1/v2c Community
# Max Character Number: 64
P21902 =

# SNMP Trap Community
# Max String Length: 64
P21900=

# SNMPv3 User Name
# Max Character Number: 64
P21905= 

# SNMPv3 Security Level. 0 - noAuthUser, 1 - authUser, 2 - privUser. Default value is 0.
# Number: 0, 1, 2
# Mandatory
P21910=0 

# SNMPv3 Authentication Protocol. 0 - None, 1- MD5, 2- SHA. Default value is 0.
# Number: 0, 1, 2
# Mandatory
P21906=0

# SNMP Privacy Protocol. 0 - None, 1 - DES, 2 - AES | AES128. Default value is 0.
# Number: 0, 1, 2
# Mandatory
P21907=0

# SNMPv3 Authentication Key. 
P21908=

# SNMPv3 Privacy Key
P21909=

# SNMPv3 Trap User Name
# Max Character Nmuber: 64
P21911= 

# SNMPv3 Trap Security Level. 0 - noAuthUser, 1 - authUser, 2 - privUser. Default value is 0.
# Number: 0, 1, 2
# Mandatory
P21916=0 

# SNMPv3 Trap Authentication Protocol. 0 - None, 1- MD5, 2- SHA. Default value is 0.
# Number: 0, 1, 2
# Mandatory
P21912=0

# SNMP Trap Privacy Protocol. 0 - None, 1 - DES, 2 - AES | AES128. Default value is 0.
# Number: 0, 1, 2
# Mandatory
P21913=0

# SNMPv3 Trap Authentication Key. 
P21914=

# SNMPv3 Trap Privacy Key
P21915=

# Enable RAIUS Web Access Control. 0 - No, 1 - Yes. Default value is 0.
# Nmuber: 0, 1
# Mandatory
P28107=0

# Action upon Radius Auth Server Error. 0 - Reject Access, 1 - Authenticate Locally. Default value is 1.
# Number: 0, 1
# Mandatory
P28114=1

# RADIUS Auth Server Address
# ipaddress
P28108= 

# RADIUS Auth Server Port
# Max Character Number = 64
P28109=

# RADIUS Shared Secret
# Max Character Number = 64
P28110=

# RADIUS VSA Vendor ID
# Max Character Number: 64
P28111= 

# RADIUS VSA Access Level Attribute
# Max Character Number: 64
P28112= 

# Enable DDNS. 0 - No, 1 - Yes. Default is 0.
# Number: 0, 1
# Mandatory
P28121 = 0

# DDNS Server. 0 - dyndns.org, 1 - freedns.afraid.org, 2 - zoneedit.com, 3 - no-ip.com, 4 - oray.net. 
# Number: 0, 1, 2, 3, 4
# Mandatory
P28122 = 0

# DDNS Username
# String
P28123 = 

# DDNS Password
# String
P28124 = 

# DDNS Hostname
# String
P28125 = 

# DDNS Hash
# String
P28126 = 

# System Ring Cadence
# String
P4040 = c=2000/4000;

############################################
# Call Progress Tones                      #
############################################
# Dial Tone
# String
P4000 = f1=350@-17,f2=440@-17,c=0/0;

# Ringback Tone
# String
P4001 = f1=440@-17,f2=480@-17,c=2000/4000;

# Busy Tone
# String
P4002 = f1=480@-21,f2=680@-21,c=500/500;

# Reorder Tone
# String
P4003 = f1=480@-21,f2=620@-21,c=250/250;

# Confirmation Tone
# String
P4004 = f1=350@-11,f2=440@-11,c=100/100-100/100-100/100;

# Call Waiting tone
# String
P4005 = f1=440@-13,c=300/10000;

# Prompt Tone
# String
P4041 = f1=350@-17,f2=440@-17,c=0/0;

# Prompt Tone Access Code(Key pattern to get Prompt Tone. Maximum 20 digits. No default.)
# String
P4042 = 

# Lock keypad update.  0 - No, 1 - Yes.
# Number: 0, 1
# Mandatory
P88 = 0

# Disable voice prompt. 0 - No, 1 - Yes.
# Number: 0, 1
# Mandatory
P253 = 0

# Disable Direct IP Call. 0 - No, 1 - Yes.
# Number: 0, 1
# Mandatory
P277 = 0

# Life Line Mode. 0 - Auto, 1 - Always Disconnected, 2 - Always Connected
# Number: 0, 1, 2
# Mandatory
P891 = 0

# Blacklist For Incoming Calls. Allow users to block incoming calls from specific list of numbers.Max allowed SIP numbers: 10, separated by a comma (',') 
# String: 0-9, *, #, +, comma (','), a-z, A-Z
P28127 =

# NTP Server
# Server address
P30 = pool.ntp.org

# Allow DHCP Option 42 to override NTP server. 0 - No, 1 - Yes. Default is No.
# When set to Yes(1), it will override the configured NTP server.
# Number: 0, 1
# Mandatory
P144=1

# DHCP Option 17 Enterprise Number
# Max Character Number: 5
# Mandatory
P8457=3561

# Disable Week TLS Cipher Suites. 0 – Enable Weak TLS Ciphers Suites, 1 – Disable Symmetric Encryption RC4/DES/3DES, 2 - Disable Symmetric Encryption SEED, 3 - Disable All Of The Above Weak Symmetric Encryption, 4 - Disable Symmetric Authentication MD5, 5 - Disable All Of The Above Weak Symmetric Authentication, 6 - Disable Protocol Version SSLv2/SSLv3, 7 - Disable All Of The Above Weak Protocol Version, 8 - Disable All Of The Above Weak TLS Ciphers Suites
# Number: 0-8
# Mandatory 
P8536=0

# Minimum TLS Version. 99 - Unlimited, 10 - TLS 1.0, 11 - TLS 1.1, 12 - TLS 1.2
# Number: 99, 10, 11, 12
# Mandatory
P22293=99

# Maximum TLS Version. 99 - Unlimited, 10 - TLS 1.0, 11 - TLS 1.1, 12 - TLS 1.2
# Number: 99, 10, 11, 12
# Mandatory
P22294=99

# Syslog Protocol. 0 – UDP, 1 – SSL/TLS. 
# Number: 0, 1  
# Mandatory
P8402=0 


# Syslog Server (name of the server, max length is 64 characters)
# Server address
# Reboot required
P207 = 

# Syslog Level (Default setting is NONE)
# 0 - NONE, 1 - DEBUG, 2 - INFO, 3 - WARNING, 4 - ERROR, 5 - EXTRA DEBUG
# Number: 0, 1, 2, 3, 4, 5
# Mandatory
# Reboot required
P208 = 0

# Send SIP Log (0 - No, 1 - Yes, Default set to No)
# Number: 0, 1
# Mandatory
# Reboot required
P1387 = 0

# Automatic Reboot. 0 - No, 1 - Yes, reboot every day at hour, 2 - Yes, reboot every week at day, 3 - Yes, reboot every month at day
#Number: 0,1,2,3
#Mandatory
P21929 = 0

#Hour of the Day(0-23) Defines the hour of the day to reboot the device. Will valid after configured Automatic Reboot to yes.
#Number: 0-23
#Mandatory
P21930 = 1

#Day of the Week (0-6) Defines the day of the week to reboot the device.
#Number: 0-6
#Mandatory
P21931 = 1

# Day of the Month (0-30) Defines the day of the month to reboot the device.
# Number: 0-30
# Mandatory
P28118 = 1



##############################################################################
##  FXS PORT Settings.                                                      ##
##############################################################################
# Account Active. 0 - No, 1 - Yes.
# Number: 0, 1
# Mandatory
P271 = 1

# Primary SIP Server
# Server address
P47 = sip.mycompany.com

# Failover SIP Server
# Server address
P967 = 

# Prefer Primary SIP Server. 0 - No, 1 - Yes.
# Number: 0, 1
# Mandatory
P4567 = 0

# Outbound Proxy
# Server address
P48 = proxy.mycompany.com

# Backup Outbound Proxy
# Server address
P2333 = 

# Prefer Primary Outbound Proxy. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P28096 = 0

# Allow DHCP Option 120( override SIP server )  0 - No, 1 - Yes.
# Number: 0, 1
# Mandatory
P1411=0

# SIP Transport 0 - UDP, 1 - TCP, 2 - TLS
# Number: 0, 1, 2
# Mandatory
P130 = 0

# SIP URI Scheme When Using TLS. 0 - sip, 1 - sips. Default is sips
# Number: 0, 1
# Mandatory
P2329=1

# Use Actual Ephemeral Prot in Contact with TCP/TLS. 0 - No, 1 - Yes.
# Number: 0, 1
# Mandatory
P2331=0

# NAT Traversal. 0 - No, 2 - Keep-alive, 1 - STUN, 3 - UPnP
# Number: 0, 1, 2, 3
# Mandatory
P52 = 0

# SIP User ID
# String
P35 = 

# Authentication ID
# String
P36 = 

# Authentication password
# String
P34 = 

# Name (John Doe)
# String
P3 = 

# DNS Mode. 0 - A Record, 1 - SRV, 2 - NAPTR/SRV.
# Number: 0, 1, 2,
# Mandatory
P103 = 0

# DNS SRV use Registered IP. 0 - No, 1 - Yes. Default is 0.
# Number: 0, 1
# Mandatory
P28092 = 0

# Tel URI. 0 - Disabled, 1 - User=Phone, 2 - Enabled
# Number: 0, 1, 2
# Mandatory
P63 = 0

# SIP Registration. 0 - No, 1 - Yes
# Number: 0, 1
# Mandatory
P31 = 1

# Unregister On Reboot. 0 - No, 1 - Yes
# Number: 0, 1
# Mandatory
P81 = 0

# Outgoing call without Registration. 0 - no, 1 - yes
# Number: 0, 1
# Mandatory
P109 = 1

# Register Expiration (in minutes. default 1 hour, max 45 days)
# Number: 1 to 64800
# Mandatory
P32 = 60

# Reregister before Expiration (in seconds. Default is 0 second.)
# Number: 0 to 64800
# Mandatory
P2330 = 0

# SIP Registration Failure Retry Wait Time (in seconds. Between 1-3600, default is 20)
# Number: 1 to 3600
# Mandatory
P138 = 20

# SIP Registration Failure Retry Wait Time upon 403 Forbidden. 0 second means stop retry registration. Default is 1200 sec.
# Number 0 to 3600
# Mandatory
P26002=1200

# Enable SIP OPTIONS Keep Alive. 0 - No, 1 - Yes, default is 0
# Number: 0, 1
# Mandatory
P2397=0

# SIP OPTIONS Keep Alive Interval, in seconds. Between 1-64800, default is 30
# Number: 1 to 64800
# Mandatory
P2398=30

# SIP OPTIONS Keep Alive Max Lost, Number of max lost packets for SIP OPTIONS Keep Alive before re-registration. Between 3-10, default is 3
# Number: 3 to 10
# Mandatory
P2399=3

#Layer 3 QoS SIP Diff-Serv (default 26)
#Number
#Mandatory
P5046=26

#Layer 3 QoS RTP Diff-Serv (default 46)
#Number
#Mandatory
P5050=46

# Local SIP Port (default is 5060 for UDP and TCP; 5061 for TLS)
# Number: 1 to 65535
# Mandatory
P40 = 5060

# Local RTP port (1024-65535, default 5004)
# Number: 1024 to 65535
# Mandatory
P39 = 5004 

# Use Random SIP Port. 0 - No, 1 - Yes
# Number: 0, 1
# Mandatory
P20501 = 0

# Use Random RTP Port. 0 - No, 1 - Yes
# Number: 0, 1
# Mandatory
P20505 = 0

# Enable RTCP. 0 - No, 1 - Yes
# Number: 0, 1
# Mandatory
P2392=1

# Hold Target Before Refer. 0 - No, 1 - Yes
# Number: 0, 1
# Mandatory
P26003 = 0

# Refer-To Use Target Contact. 0 - No, 1 - Yes
# Number: 0, 1
# Mandatory
P135 = 0

# Transfer on Conference Hangup. 0 - No, 1 - Yes
# Number: 0, 1
# Mandatory
P4560 = 0

# Disable Bellcore Style 3-Way Conference. 0 - No, 1 - Yes.
# Number: 0, 1
# Mandatory
P4830 = 0

# Remove OBP from Route Header. 0 - No, 1 - Yes
# Number: 0, 1
# Mandatory
P4562 =0

# Support SIP Instance ID. 0 - No, 1 - Yes
# Number: 0, 1
# Mandatory
P288 = 1

# Validate Incoming SIP Message. 0 - No, 1 - Yes
# Number: 0, 1
# Mandatory
P4340 = 0

# Check SIP User ID for incoming INVITE. 0 - No, 1 - Yes
# Number: 0, 1
# Mandatory
P258 = 0

#Authenticate incoming INVITE. 0 - No, 1 - Yes 
#Number: 0,1
P2346=0

# Authenticate server certificate domain. 0 - No, 1 - Yes, default is 0
# Number: 0, 1
# Mandatory
P2311=0

# Authenticate server certificate chain. 0 - No, 1 - Yes, default is 0
# Number: 0, 1
# Mandatory
P2367=0

# Allow Incoming SIP Messages from SIP Proxy Only 0 - No, 1 - Yes (nodirect IPcalling if Yes)
# Number: 0, 1
# Mandatory
P243 = 0

# Use Privacy Header. 0 - Default, 1 - No, 2 - Yes 
# (Default will not add Privacy header when special feature is Telkom SA or CBCOM)
# Number: 0, 1
# Mandatory
P2338 = 0

# Use P-Preferred-Identity Header. 0 - Default, 1 - No, 2 - Yes 
# (Default will not add Privacy header when special feature is Telkom SA or CBCOM)
# Number: 0, 1
# Mandatory
P2339 = 0

# Use P-Access-Network-Info Header. 0 - No, 1 - Yes. Default is 1.
# Number: 0, 1
# Mandatory
P26058 = 1

# Use P-Emergency-Info Header. 0 - No, 1 - Yes. Default is 1.
# Number: 0, 1
# Mandatory
P26059 = 1

# SIP REGISTER Contact Header Uses. 0 - LAN address, 1 - WAN address
# Number: 0, 1
# Mandatory
P4437=0

# Caller ID Fetch Order. 0 - Auto, 1 - Disable, 2 - From Header. Defaut is 0.
# Number: 0, 1, 2
# Mandatory
P2324=0

# Allow SIP Factory Reset. 0 - No, 1 - Yes. Default is 0.
# Number: 0, 1
# Mandatory
P26015=0

# SIP T1 Timeout. 
# 50 - 0.5 sec, 100 - 1 sec, 200 - 2 sec, 400 - 4 sec, 800 - 8 sec. Default 50.
# Number: 50, 100, 200, 400, 800
# Mandatory
P209 = 50

# SIP T2 Interval. 
# Value 200 - 2 sec, 400 - 4 sec, 800 - 8 sec, 1600 - 16 sec, 3200 - 32 sec. Default 400.
# Number: 200, 400, 800, 1600, 3200
# Mandatory
P250 = 400

# SIP Timer D 
# Number: 0 - 64 seconds
# Mandatory
P2387 = 0

# DTMF Payload Type
# Number
# Mandatory
P79 = 101

# Preferred DTMF method. 
# 100 - In-audio, 101 - RFC2833, 102 - SIP INFO
# Priority 1
# Number: 100, 101, 102
# Mandatory
P850 = 101

# Priority 2
# Number: 100, 101, 102
# Mandatory
P851 = 102

# Priority 3
# Number: 100, 101, 102
# Mandatory
P852 = 100

# Disable DTMF Negotiation. 0 - No, 1 - Yes 
# Number: 0, 1
# Mandatory
P4825 = 0

# Generate Continuous RFC2833 Events. 0 - No, 1 - Yes(RFC2833 events are generated until key is released) 
# Number: 0, 1
# Mandatory
P4433=0

# Send Hook Flash Event. 0 - No, 1 - Yes 
# Number: 0, 1
# Mandatory
P74 = 0

# Flash Digit Control. 0 - No, 1 - Yes(Overrides the default settings for call control when both channels are in use.) 
# Number: 0, 1
# Mandatory
P28080=0

# Enable Call Features. 0 - No, 1 - Yes 
# Number: 0, 1
# Mandatory
P191 = 1

# Offhook Auto-Dial (User ID/extension to dial automatically when offhook)
# String: 0 to 9, *, #
P71 =

# Offhook Auto-Dial Delay (default is 0)
# String: 0 to 60
P4045 = 0

# Proxy-Require 
# IP Address
P197 =

# Use NAT IP (used in SIP/SDP message if specified)
# IP Address
P101 = 

# SIP User-Agent.
# String
P29071=

# Use SIP User-Agent Postfix
# String
P4834 = 

# Distinctive Ring Tone 
# 0 - Ring Tone 1, 1 - Ring Tone 2, 2 - Ring Tone 3, 3 - Ring Tone 4, 4 - Ring Tone 5, 
# 5 - Ring Tone 6, 6 - Ring Tone 7, 7 - Ring Tone 8, 8 - Ring Tone 9, 9 - Ring Tone 10
# Distinctive Ring Tone Choice 1
# Number: 0 to 9
# Mandatory
P870 = 0

# Choice 1 incoming caller ID
# String
P871 = 

# Distinctive Ring Tone Choice 2
# Number: 0 to 9
# Mandatory
P872 = 0

# Choice 2 incoming caller ID
# String
P873 = 

# Distinctive Ring Tone Choice 3
# Number: 0 to 9
# Mandatory
P874 = 0

# Choice 3 incoming caller ID
# String
P875 = 

# Disable Call-Waiting. 0 - No, 1 - Yes
# Number: 0, 1
# Mandatory
P91 = 0

# Disable Call-Waiting Caller ID. 0 - No, 1 - Yes
# Number: 0, 1
# Mandatory
P714 = 0

# Disable Call-Waiting Tone. 0 - No, 1 - Yes
# Number: 0, 1
# Mandatory
P186 = 0

# Disable Connected Line ID. 0 = No, 1 = Yes. (If yes, Connected Line ID will not be displayed even received.)
# Number: 0, 1
# Mandatory
P20525=0

# Disable Receiver Offhook Tone. 0 - No, 1 - Yes.
# Number: 0, 1
# Mandatory
P4793 = 0

# Disable Reminder Ring for On-Hold Call. 0 - No, 1 - Yes
# Number: 0, 1
# Mandatory
P4360 = 0

# Disable Visual MWI. 0 - No, 1 - Yes
# Number: 0, 1
# Mandatory
P855 = 0

# Do Not Escape '#' as %23 in SIP URI. 0 - No, 1 - Yes
# Number: 0, 1
# Mandatory
P1406 = 0

# Disable Multiple m Line in SDP. 0 - No, 1 - Yes
# Number: 0, 1
# Mandatory
P137 = 0

# Ring Timeout. (0-300, default is 60 seconds)
# Number: 0 to 300
# Mandatory
P185 = 60

# Delayed Call Forward Wait Time. Allowed range 1-120, in seconds. Default 20 seconds.
# Number: 1 to 120
# Mandatory
P139 = 20

# No Key Entry Timeout (in seconds, default is 4 seconds)
# Number: 1 to 15
# Mandatory
P85 = 4

# Early Dial 0 - No, 1 - Yes
# Number: 0, 1
# Mandatory
P29 = 0

# Dial Plan Prefix.(this prefix string is added to each dialed number)
# String
P66 = 

# Use # as Dial Key. 0 - No, 1 - Yes (if set to Yes, "#" will function as the "(Re-)Dial" key)
# Number: 0, 1
# Mandatory
P72 = 1

# Dial Plan 
# String
P4200 = { x+ | \+x+ | *x+ | *xx*x+ }

# SUBSCRIBE for MWI. 0 - No,do not send SUBSCRIBE for Message Waiting Indication, 1 - Yes, send periodical SUBSCRIBE for Message Waiting Indication
# Number: 0, 1
# Mandatory
P99 = 0

# Send Anonymous. 0 - No, 1 - Yes  (caller ID will be blocked if set to Yes)
# Number: 0, 1
# Mandatory
P65 = 0

# Anonymous Call Rejection. 0 - No, 1 - Yes.
# Number: 0, 1
# Mandatory
P129 = 0

# Special Feature 
# 100 - Standard, 102 - BroadSoft, 108 - CBCOM, 109 - RNK, 111 - Huawei, 114 - ZTE IMS, 119 - Phone Power, 120 - TELKOM SA, 121 - Vonage, 122 - Metaswitch, 124 - CenturyLink, 126 - MTS.
# Number: 100, 102, 108, 109, 111, 114, 119, 120, 121, 122, 124, 126
# Mandatory
P198 = 100

# Enable Session Timer. 0 - No, 1 - Yes.
# Number: 0, 1
# Mandatory
P2395=1

# Session Expiration (in seconds. default 180 seconds. Allowed value: 90-64800)
# Number: 90 to 64800
# Mandatory
P260 = 180

# Minimum SE (in seconds. default 90 seconds, must be lower than or equal to P260)
# Number: 90 to 64800
# Mandatory
P261 = 90

# Caller Request Timer (Request for timer when making outbound calls) 0 - No, 1 - Yes
# Number: 0, 1
# Mandatory
P262 = 0

# Callee Request Timer (Request for timer when called. i.e. if remote party supports timer but did not request for one) 0 - No, 1 - Yes
# Number: 0, 1
# Mandatory
P263 = 0

# Force Timer (Still use timer when remote party does not support timer) 0 - No, 1 - Yes
# Number: 0, 1
# Mandatory
P264 = 0

# UAC Specify Refresher. 0 - omit, 1 - UAC, 2 - UAS
# Number: 0, 1, 2
# Mandatory
P266 = 0

# UAS Specify Refresher. 1 - UAC, 2 - UAS
# Number: 1, 2
# Mandatory
P267 = 1

# Force INVITE (Always refresh with INVITE instead of UPDATE even when remote party supports UPDATE) 0 - no, 1 - yes
# Number: 0, 1
# Mandatory
P265 = 0

# Enable 100rel. 0 - No, 1 - Yes
# Number: 0, 1
# Mandatory
P272 = 0

# Add Auth Header On Initial REGISTER. 0 - No, 1 - Yes
# Number: 0, 1
# Mandatory
P2359 = 0

# Conference URI
P2318=

################################################################################
# Codec/Voice Quality settings                                                 #
################################################################################
# Use First Matching Vocoder in 200OK SDP. 0 - No, 1 - Yes
# Number: 0, 1
# Mandatory
P4363 = 0

# Preferred Vocoder
# 0 - PCMU, 8 - PCMA, 4 - G.723, 18 - G.729, 2 - G.726-32,
# 97 - iLBC, 123 - OPUS
# Choice 1.
# Number: 0, 8, 4, 18, 2, 97, 123
# Mandatory
P57 = 0

# Choice 2. 
# Number: 0, 8, 4, 18, 2, 97, 123
# Mandatory
P58 = 8

# Choice 3. 
# Number: 0, 8, 4, 18, 2, 97, 123
# Mandatory
P59 = 4

# Choice 4. 
# Number: 0, 8, 4, 18, 2, 97, 123
# Mandatory
P60 = 18

# Choice 5. 
# Number: 0, 8, 4, 18, 2, 97, 123
# Mandatory
P61 = 2

# Choice 6. 
# Number: 0, 8, 4, 18, 2, 97, 123
# Mandatory
P62 = 97

# Choice 7. 
# Number: 0, 8, 4, 18, 2, 97, 123
# Mandatory
P46 = 123

# Voice Frames per TX. (Default 2, from 1 to 4 for G711/G726/G729)
# Number: 1 to 4
P37 = 2

# G723 rate. 0 - 6.3kbps encoding rate, 1 - 5.3kbps encoding rate
# Number: 0, 1
# Mandatory
P49 = 0

# iLBC Frame Size. 0 - 20ms(default), 1 - 30ms.
# Number: 0, 1
# Mandatory
P97 = 0

# Disable OPUS Stereo in SDP. 0 - No, 1 - Yes(remove "/2" from offer)
# Number: 0, 1
# Mandatory
P20529 = 0

# iLBC Payload Type. (between 96 and 127, default is 97).
# Number: 96-127
# Mandatory
P96=97

# OPUS Payload Type. (between 96 and 127, default is 123).
# Number: 96-127
# Mandatory
P2385=123

# VAD. 0 - No, 1 - Yes 
# Number: 0, 1
# Mandatory
P50 = 0

# Symmetric RTP. 0 - No, 1 - Yes
# Number: 0, 1
# Mandatory
P291 = 0

# FAX Mode. 0 - T.38 (Auto Detect), 1 - Pass Through
# Number: 0, 1
# Mandatory
P228 = 0

# Re-INVITE After Fax Tone Detected. 0 - Disabled, 1 - Enabled.
# Number: 0, 1
# Mandatory
P4416=1

# Jitter buffer type.  0 - Fixed, 1 - Adaptive
# Number: 0, 1
# Mandatory
P133 = 1

# Jitter buffer length. 0 - Low, 1 - Medium, 2 - High
# Number: 0, 1, 2
# Mandatory
P132 = 1

# SRTP Mode
# 0 = Disabled
# 1 = Enabled but not forced
# 2 = Enabled and forced
# Number: 0, 1, 2
# Mandatory
P183 = 0

#Crypto Life Time. 0 - Disabled, 1 - Enabled
# Number: 0, 1
# Mandatory
P2363 = 1

################################################################################
# SLIC Setting.   
# 0 - USA 1 (BELLCORE 600 ohms), 3 - USA 2 (BELLCORE 600 ohms + 2.16uF), 11 - AUSTRALIA, 5 - CHINA CO, 6 - CHINA PBX, 4 - EUROPEAN CTR21, 9 - GERMANY, 8 - INDIA/NEW ZEALAND, 2 - JAPAN CO, 7 - JAPAN PBX, 1 - STANDARD 900 ohms, 10 - UK
# Number: 0 to 11
# Mandatory
P854 = 0

# Caller ID Scheme.  
# <value=0> Bellcore/Telcordia (default)
# <value=1> ETSI-FSK during ringing	
# <value=2> ETSI-FSK prior to ringing with DTAS
# <value=3> ETSI-FSK prior to ringing with LR+DTAS
# <value=4> ETSI-FSK prior to ringing with RP
# <value=5> ETSI-DTMF during ringing
# <value=6> ETSI-DTMF prior to ringing with DTAS
# <value=7> ETSI-DTMF prior to ringing with LR+DTAS
# <value=8> ETSI-DTMF prior to ringing with RP
# <value=9> SIN 227 - BT
# <value=10> NTT Japan 
# <value=11 >DTMF Denmark prior to ringing no DTAS no LR
# <value=12 >DTMF Denmark prior to ringing with LR
# <value=13 >DTMF Sweden/Finalnd prior to ringing with LR
# <value=14 >DTMF Brazil
# <value=15 >DTMF-FSK Brazil
# Number: 0 to 15
# Mandatory
P853 = 0

# DTMF Caller ID Start Tone
# <value=0>  Default
# <value=1>  A
# <value=2>  B
# <value=3>  C
# <value=4>  D
# <value=5>  #
# Number: 0-5
# Mandatory
P4661=0

# DTMF Caller ID Stop Tone
# <value=0>  Default
# <value=1>  A
# <value=2>  B
# <value=3>  C
# <value=4>  D
# <value=5>  #
# Number: 0-5
# Mandatory
P4662=0

# Polarity Reversal.  0 - No, 1 - Yes
# Number: 0, 1
# Mandatory
P205 = 0

# Loop Current Disconnect. 0 - No, 1 - Yes
# Number: 0, 1
# Mandatory
P892 = 0

# Play busy/reorder tone before Loop Current Disconnect.  0 - No, 1 - Yes
# Number: 0, 1
# Mandatory
P21925 = 0

# Loop Current Disconnect Duration. In 100 - 10000 milliseconds range, default is 200.
# Number: 100 to 10000
# Mandatory
P856 = 200

# Enable Pulse Dialing. 0 - No, 1 - Yes. Default is 0.
# Number: 0, 1
# Mandatory
P20521 = 0

# Pulse Dialing Standard. 0 - General Standard, 1 - Swedish Standard
# Number: 0, 1
# Mandatory 
P28165=0

# Enable Hook Flash
# Number: 0, 1
# Mandatory
P4424 = 1

# Hook Flash Timing. In 40-2000 milliseconds range
# minimum
# Number: 40 to 2000
# Mandatory
P251 = 300

# maximum
# Number: 40 to 2000
# Mandatory
P252 = 1100

# On Hook Timing. (In 40-2000 milliseconds range, default is 400)
# Number: 40 to 2000
# Mandatory
P833 = 400

# Gain:
# TX 
# <value=1> +6dB
# <value=2> +4dB
# <value=3> +2dB
# <value=0> 0dB default
# <value=4> -2dB
# <value=5> -4dB
# <value=6> -6dB
# <value=7 >-8dB
# <value=8 >-10dB
# <value=9 >-12dB
# Number: 0, 1, 2, 3, 4, 5, 6, 7, 8, 9
# Mandatory
P247 = 0 

# RX 
# <value=1> +6dB
# <value=2> +4dB
# <value=3> +2dB
# <value=0> 0dB
# <value=4> -2dB
# <value=5> -4dB
# <value=6> -6dB default
# <value=7 >-8dB
# <value=8 >-10dB
# <value=9 >-12dB
# Number: 0, 1, 2, 3, 4, 5, 6, 7, 8, 9
# Mandatory
P249 = 6

# Disable Line Echo Canceller (LEC).  0 - No, 1 - Yes
# Number: 0, 1
# Mandatory
P824 = 0

# Disable Network Echo Suppressor.  0 - No, 1 - Yes
# Number: 0, 1
# Mandatory
P4441=0

# Outgoing Call Duration Limit.  (0-180 minutes, default is 0 (No Limit))
# Number: 0~180
# Mandatory
P4420=0

# Enable High Ring Power. 0 - No, 1 - Yes. Default is 0.
# Number: 0, 1
# Mandatory
P4234=0


# RFC2833 Events Count.
# Number: 2-10
# Mandatory
P28173=8

# RFC2833 End Events Count.
# Number: 2-10
# Mandatory
P28177=3

# Ring Tone 1
# String
P4010 = c=2000/4000;

# Ring Tone 2
# String
P4011 = c=2000/4000;

# Ring Tone 3
# String
P4012 = c=2000/4000;

# Ring Tone 4
# String
P4013 = c=2000/4000;

# Ring Tone 5
# String
P4014 = c=2000/4000;

# Ring Tone 6
# String
P4015 = c=2000/4000;

# Ring Tone 7
# String
P4016 = c=2000/4000;

# Ring Tone 8
# String
P4017 = c=2000/4000;

# Ring Tone 9
# String
P4018 = c=2000/4000;

# Ring Tone 10
# String
P4019 = c=2000/4000;

##############################################################################
##  FXO PORT Settings.                                                      ##
##############################################################################
# Account Active. 0 - No, 1 - Yes.
# Number: 0, 1
# Mandatory
P401 = 1

# Primary SIP Server
# Server address
P747 = sip.mycompany.com

# Failover SIP Server
# Server address
P987 = 

# Prefer Primary SIP Server. 0 - No, 1 - Yes.
# Number: 0, 1
# Mandatory
P4568 = 0

# Outbound Proxy
# Server address
P748 = proxy.mycompany.com

# Backup Outbound Proxy
# Server address
P2433 = 

# Prefer Primary Outbound Proxy. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P28097 = 0

# SIP Transport 0 - UDP, 1 - TCP, 2 - TLS
# Number: 0, 1, 2
# Mandatory
P830 = 0

# NAT Traversal. 0 - No, 2 - Keep-alive, 1 - STUN, 3 - UPnP
# Number: 0, 1, 2, 3
# Mandatory
P730 = 0

# SIP User ID
# String
P735 = 

# Authentication ID
# String
P736 = 

# Authentication password
# String
P734 = 

# Name (John Doe)
# String
P703 = 

# DNS Mode. 0 - A Record, 1 - SRV, 2 - NAPTR/SRV .
# Number: 0, 1, 2
# Mandatory
P702 = 0

# DNS SRV use Registered IP. 0 - No, 1 - Yes. Default is 0.
# Number: 0, 1
# Mandatory
P28093 = 0

# Tel URI. 0 - Disabled, 1 - User=Phone, 2 - Enabled
# Number: 0, 1, 2
# Mandatory
P763 = 0

# SIP Registration. 0 - No, 1 - Yes
# Number: 0, 1
# Mandatory
P731 = 1

# Unregister On Reboot. 0 - No, 1 - Yes
# Number: 0, 1
# Mandatory
P752 = 0

# Outgoing call without Registration. 0 - No, 1 - Yes
# Number: 0, 1
# Mandatory
P813 = 1

# Register Expiration (in minutes. default 1 hour, max 45 days)
# Number: 1 to 64800
# Mandatory
P732 = 60

# Reregister before Expiration
# Number
# Mandatory
P2430 = 0

# SIP Registration Failure Retry Wait Time
# Number: 1 to 3600
# Mandatory
P471 = 20

# SIP Registration Failure Retry Wait Time upon 403 Forbidden. 0 second means stop retry registration. Default is 1200 sec.
# Number 0 to 3600
# Mandatory
P26102=1200

Enable SIP OPTIONS Keep Alive. 0 - No, 1 - Yes, default is 0
# Number: 0, 1
# Mandatory
P2497=0

# SIP OPTIONS Keep Alive Interval, in seconds. Between 1-64800, default is 30
# Number: 1 to 64800
# Mandatory
P2498=30

# SIP OPTIONS Keep Alive Max Lost, Number of max lost packets for SIP OPTIONS Keep Alive before re-registration. Between 3-10, default is 3
# Number: 3 to 10
# Mandatory
P2499=3

#Layer 3 QoS SIP Diff-Serv (default 26)
#Number
#Mandatory
P5047=26

#Layer 3 QoS RTP Diff-Serv (default 46)
#Number
#Mandatory
P5051=46

# Local SIP port (default 5062)
# Number: 1 to 65535
# Mandatory
P740 = 5062

# Local RTP port (1024-65535, default 5012)
# Number: 1024 to 65535
# Mandatory
P739 = 5012

# Use Random SIP Port. 0 - No, 1 - Yes
# Number: 0, 1
# Mandatory
P20502 = 0

# Use Random RTP Port. 0 - No, 1 - Yes
# Number: 0, 1
# Mandatory
P20506 = 0

# Enable RTCP. 0 - No, 1 - Yes
# Number: 0, 1
# Mandatory
P2492=1

# Remove OBP from Route Header. 0 - No, 1 - Yes
# Number: 0, 1
# Mandatory
P4563 =0

# Support SIP Instance ID. 0 - No, 1 - Yes
# Number: 0, 1
# Mandatory
P489 = 1

# Validate Incoming SIP Message. 0 - No, 1 - Yes
# Number: 0, 1
# Mandatory
P4341 = 0

# Check SIP User ID for incoming INVITE. 0 - No, 1 - Yes(no direct IP calling if Yes)
# Number: 0, 1
# Mandatory
P449 = 0

#Authenticate incoming INVITE 
#Number: 0,1
P2446=0

# Authenticate server certificate domain. 0 - No, 1 - Yes, default is 0
# Number: 0, 1
# Mandatory
P2411=0

# Authenticate server certificate chain. 0 - No, 1 - Yes, default is 0
# Number: 0, 1
# Mandatory
P2467=0

# Allow Incoming SIP Messages from SIP Proxy Only 0 - No, 1 - Yes (no direct IP calling if Yes)
# Number: 0, 1
# Mandatory
P743 = 0

# Use Privacy Header. 0 - Default, 1 - No, 2 - Yes 
# (Default will not add Privacy header when special feature is Telkom SA or CBCOM)
# Number: 0, 1
# Mandatory
P2438 = 0

# Use P-Preferred-Identity Header. 0 - Default, 1 - No, 2 - Yes 
# (Default will not add Privacy header when special feature is Telkom SA or CBCOM)
# Number: 0, 1
# Mandatory
P2439 = 0

# Use P-Access-Network-Info Header. 0 - No, 1 - Yes. Default is 1.
# Number: 0, 1
# Mandatory
P26158 = 1

# Use P-Emergency-Info Header. 0 - No, 1 - Yes. Default is 1.
# Number: 0, 1
# Mandatory
P26159 = 1

# SIP REGISTER Contact Header Uses. 0 - LAN address, 1 - WAN address
# Number: 0, 1, 2
# Mandatory
P4438=0

# Allow SIP Factory Reset. 0 - No, 1 - Yes. Default is 0.
# Number: 0, 1
# Mandatory
P26115=0

# SIP T1 Timeout. 
# 50 - 0.5 sec, 100 - 1 sec, 200 - 2 sec, 400 - 4 sec, 800 - 8 sec. Default 50.
# Number: 50, 100, 200, 400, 800
# Mandatory
P440 = 50

# SIP T2 Interval. 
# 200 - 2 sec, 400 - 4 sec, 800 - 8 sec, 1600 - 16 sec, 3200 - 32 sec. Default 400.
# Number: 200, 400, 800, 1600, 3200
# Mandatory
P441 = 400

# SIP Timer D 
# Number: 0 - 64 seconds
# Mandatory
P2487 = 0

# DTMF Payload Type
# Number: 96 to 127
# Mandatory
P779 = 101

# Preferred DTMF method. 100 - In-Audio, 101 - RFC2833, 102 - SIP INFO
# Priority 1
# Number: 100, 101, 102
# Mandatory
P860 = 101

# Priority 2
# Number: 100, 101, 102
# Mandatory
P861 = 102

# Priority 3
# Number: 100, 101, 102
# Mandatory
P862 = 100

# Disable DTMF Negotiation. 0 - No (default, negotiate with peer), 1 - Yes (use above DTMF order without negotiation)
# Number: 0, 1
# Mandatory
P4826 = 0

# Generate Continuous RFC2833 Events. 0 - No, 1 - Yes(RFC2833 events are generated until key is released) 
# Number: 0, 1
# Mandatory
P4434=0

# Flash Digit Control. 0 - No, 1 - Yes(Overrides the default settings for call control when both channels are in use.) 
# Number: 0, 1
# Mandatory
P28081=0

# Proxy-Require 
# IP Address
P792 =

# Use NAT IP (used in SIP/SDP message if specified)
# IP Address
P866 = 

# SIP User-Agent.
# String
P29171=

# Use SIP User-Agent Postfix for FXO
# String
P4835 = 

# Do Not Escape '#' as %23 in SIP URI. 0 - No, 1 - Yes
# Number: 0, 1
# Mandatory
P4895 = 0

# Disable Multiple m Line in SDP. 0 - No, 1 - Yes
# Number: 0, 1
# Mandatory
P487 = 0

# Ring Timeout. (0-300, default is 60 seconds)
# Number: 0 to 300
# Mandatory
P816 = 60

# Early Dial. 0 - No, 1 - Yes (use "Yes" only if proxy supports 484 response)
# Number: 0, 1
# Mandatory
P729 = 0

# Dial Plan Prefix.(this prefix string is added to each dialed number)
# String
P766 = 

# Use # as Dial Key. 0 - No, 1 - Yes (if set to Yes, "#" will function as the "(Re-)Dial" key)
# Number: 0, 1
# Mandatory
P772 = 1

# Dial Plan 
# String
P4201 = { x+ | \+x+ | *x+ | *xx*x+ }

# SUBSCRIBE for MWI. 0 - No,do not send SUBSCRIBE for Message Waiting Indication, 1 - Yes, send periodical SUBSCRIBE for Message Waiting Indication
# Number: 0, 1
# Mandatory
P709 = 0

# Anonymous Call Rejection. 0 - No, 1 - Yes.
# Number: 0, 1
# Mandatory
P446 = 0

# Special Feature 
# STANDARD = 100, BROADSOFT = 102, CBCOM =108, RNK = 109, HUAWEI = 111, China_Mobile = 113, ZTE_IMS = 114, PHONEPOWER = 119, TELKOM_SA = 120, VONAGE = 121, Metaswitch = 122, CenturyLink = 124, MTS = 126
# Number: 100, 102, 108, 109, 111, 113, 114, 119, 120, 121, 122, 124, 126
P767 = 100

# Session Expiration (in seconds. default 180 seconds. Allowed value: 90-64800)
# Number: 90 to 64800
# Mandatory
P434 = 180

# Minimum SE (in seconds. default 90 seconds, must be lower than or equal to P260)
# Number: 90 to 64800
# Mandatory
P427 = 90

# Caller Request Timer (Request for timer when calling) 0 - No, 1 - Yes
# Number: 0, 1
# Mandatory
P428 = 0

# Callee Request Timer (Request for timer when called. i.e. if remote party supports timer but did not request for one) 0 - No, 1 - Yes
# Number: 0, 1
# Mandatory
P429 = 0

# Force Timer (Still use timer when remote party does not support timer) 0 - No, 1 - Yes
# Number: 0, 1
# Mandatory
P430 = 0

# UAC Specify Refresher. 0 - omit, 1 - UAC, 2 - UAS
# Number: 0, 1, 2
# Mandatory
P432 = 0

# UAS Specify Refresher. 1 - UAC, 2 - UAS
# Number: 1, 2
# Mandatory
P433 = 1

# Force INVITE (Always refresh with INVITE instead of UPDATE even when remote party supports UPDATE) 0 - No, 1 - Yes
# Number: 0, 1
# Mandatory
P431 = 0

# INVITE Ring-No-Answer Timeout(sec). 5-300 seconds. Default 40 seconds.
# Number: 5 to 300
# Mandatory
P848 = 40

# Enable 100rel. 0 - No, 1 - Yes
# Number: 0, 1
# Mandatory
P435 = 0

# Add Auth Header On Initial REGISTER. 0 - No, 1 - Yes
# Number: 0, 1
# Mandatory
P2459 = 0

################################################################################
# Codec/Voice Quality settings                                                 #
################################################################################
# Use First Matching Vocoder in 200OK SDP. 0 - No, 1 - Yes
# Number: 0, 1
# Mandatory
P4364 = 0

# Preferred Vocoder
#  0 - PCMU, 8 - PCMA, 4 - G.723, 18 - G.729, 2 - G.726-32, 97 - iLBC, 123 - OPUS
# Choice 1.
# Number: 0, 2, 4, 8, 18, 97, 123
# Mandatory 
P757 = 0

# Choice 2. 
# Number: 0, 2, 4, 8, 18, 97, 123
# Mandatory
P758 = 8

# Choice 3.
# Number: 0, 2, 4, 8, 18, 97, 123
# Mandatory
P759 = 4

# Choice 4. 
# Number: 0, 2, 4, 8, 18, 97, 123
# Mandatory
P760 = 18

# Choice 5. 
# Number: 0, 2, 4, 8, 18, 97, 123
# Mandatory
P761 = 2

# Choice 6. 
# Number: 0, 2, 4, 8, 18, 97, 123
# Mandatory
P762 = 97

# Choice 7. 
# Number: 0, 2, 4, 8, 18, 97, 123
# Mandatory
P814 = 123

# Voice Frames per TX. (Default 2, from 1 to 4 for G711/G726/G729)
# Number: 1, 2, 3, 4
P737 = 2

# G723 rate. 0 - 6.3kbps encoding rate, 1 - 5.3kbps encoding rate
# Number: 0, 1
# Mandatory
P749 = 0

# iLBC Frame Size. 0 - 20ms(default), 1 - 30ms.
# Number: 0, 1
# Mandatory
P705 = 0

# Disable OPUS Stereo in SDP. 0 - No, 1 - Yes(remove "/2" from offer)
# Number: 0, 1
# Mandatory
P20530 = 0

# iLBC payload type. (between 96 and 127, default is 97).
# Number: 96 to 127
# Mandatory
P704 = 97

# VAD. 0 - No, 1 - Yes 
# Number: 0, 1
# Mandatory
P750 = 0

# Symmetric RTP. 0 - No, 1 - Yes
# Number: 0, 1
# Mandatory
P460 = 0

# FAX Mode. 0 - T.38 (Auto Detect), 1 - Pass Through
# Number: 0, 1
# Mandatory
P710 = 0

# Re-INVITE After Fax Tone Detected. 0 - Disabled, 1 - Enabled.
# Number: 0, 1
# Mandatory
P4417=1

# Jitter buffer type.  0 - Fixed, 1 - Adaptive
# Number: 0, 1
# Mandatory
P831 = 1

# Jitter buffer length. 0 - Low, 1 - Medium, 2 - High
# Number: 0, 1, 2
# Mandatory
P832 = 1

# SRTP Mode
# 0 = Disabled
# 1 = Enabled but not forced
# 2 = Enabled and forced
# Number: 0, 1, 2
# Mandatory
P443 = 0

#Crypto Life Time. 0 - Disabled, 1 - Enabled
# Number: 0, 1
# Mandatory
P2463 = 1

# Caller ID Scheme.  
# <value=0> Bellcore/Telcordia (default)
# <value=1> ETSI-FSK during ringing	
# <value=2> ETSI-FSK prior to ringing with DTAS
# <value=3> ETSI-FSK prior to ringing with LR
# <value=4> ETSI-FSK prior to ringing with RP
# <value=5> ETSI-DTMF during ringing
# <value=6> ETSI-DTMF prior to ringing with DTAS
# <value=7> ETSI-DTMF prior to ringing with LR
# <value=8> ETSI-DTMF prior to ringing with RP
# <value=9> SIN 227 - BT
# <value=10> NTT Japan 
# <value=11> DTMF Denmark prior to ringing no DTAS no LR
# <value=12> DTMF Denmark prior to ringing with LR
# <value=13> DTMF Sweden/Finalnd prior to ringing with LR
# <value=14> DTMF Brazil
# <value=15 >DTMF-FSK Brazil
# Number: 0 to 15
# Mandatory
P863 = 0

# DTMF Caller ID Start Tone
# <value=0>  Default
# <value=1>  A
# <value=2>  B
# <value=3>  C
# <value=4>  D
# <value=5>  #
# Number: 0-5
# Mandatory
P4663=0

# DTMF Caller ID Stop Tone
# <value=0>  Default
# <value=1>  A
# <value=2>  B
# <value=3>  C
# <value=4>  D
# <value=5>  #
# Number: 0-5
# Mandatory
P4664=0

# FSK Caller ID Minimum RX Level. (-96 - 0dB. Default -40dB)
# Range: -96 to 0
# Mandatory
P845 = -40

# FSK Caller ID Seizure Bits. 0 - 800 bits. Default 70.
# Number: 0 to 800
# Mandatory
P846 = 70

# FSK Caller ID Mark Bits. 1 - 800 bits. Default 40.
# Number: 1 to 800
# Mandatory
P847 = 40

# Caller ID Transport Type. 0 = Relay via SIP From, 1 = Relay via SIP P-Asserted-Identity, 2 = Send Anonymous, 3 = Disable, 4 = Relay via SIP P-Preferred-Identity
# Number: 0, 1, 2, 3, 4
# Mandatory
P839 = 0

# Send Hook Flash To PSTN (If Yes, hook flash will be sent to PSTN upon receiving flash event from RFC2833 or SIP INFO). 0 - No, 1 - Yes
# Number: 0, 1
# Mandatory
P837 = 0 

# Hook Flash Duration (ms). In 300-1500 milliseconds range.minimum = 300, maximum = 1500, default = 600
# Number: 300 to 1500
# Mandatory
P838 = 600

# Gain:
# TX 
# <value=1> +6dB
# <value=2> +4dB
# <value=3> +2dB
# <value=0> 0dB default
# <value=4> -2dB
# <value=5> -4dB
# <value=6> -6dB
# <value=7 >-8dB
# <value=8 >-10dB
# <value=9 >-12dB
# Number: 0, 1, 2, 3, 4, 5, 6, 7, 8, 9
# Mandatory
P248 = 0 

# RX 
# <value=1> +6dB
# <value=2> +4dB
# <value=3> +2dB
# <value=0> 0dB default
# <value=4> -2dB
# <value=5> -4dB
# <value=6> -6dB 
# Number: 0, 1, 2, 3, 4, 5, 6
P283 = 0

# Disable Line Echo Canceller (LEC).  0 - No, 1 - Yes
# Number: 0, 1
# Mandatory
P825 = 0

# Disable Network Echo Suppressor.  0 - No, 1 - Yes
# Number: 0, 1
# Mandatory
P4442=0

# Outgoing Call Duration Limit.  (0-180 minutes, default is 0 (No Limit))
# Number: 0~180
# Mandatory
P4421=0

# FXO Termination Settings
# Enable Current Disconnect 0 - No, 1 - Yes
# Number: 0, 1
# Mandatory
P893 = 1

# Current Disconnect Threshold (50 - 800 milliseconds. Default 100 milliseconds)
# Number: 50 to 800
# Mandatory
P764 = 100

# Enable PSTN Disconnect Tone Detection 0 - No, 1 - Yes (If set to yes, the following Tone is used as the disconnect signal)
# Number: 0, 1
# Mandatory
P712 = 0

# PSTN Disconnect Tone 
# String
P841 = f1=480@-32,f2=620@-32,c=500/500;

# Enable Polarity Reversal. 0 - No, 1 - Yes. Default is 0.
# Number: 0, 1
# Mandatory
P28101 = 0

# AC Termination Model. 0 - Country Based, 1 - Impedance Based, 2 - Auto- Detected
# Number: 0, 1
# Mandatory
P899 = 0

# Country Based
#0 - USA, 15 - ARGENTINA, 1 - AUSTRIA, 13 - AUSTRALIA/NEW ZEALAND, 2 - BELGIUM, 16 - BRAZIL, 17 - CANADA, 14 - CHINA, 18 - DENMARK, 3 - FINLAND, 4 - FRANCE, 5 - GERMANY, 6 - GREECE, 19 - INDIA, 20 - INDONESIA, 7 - ITALY
#8 - JAPAN, 21 - MALAYSIA, 22 - MEXICO, 23 - MOROCCO, 24 - NETHERLANDS, 9 - NORWAY, 25 - PERU, 26 - PORTUGAL, 27 - Russia, 28 - Singapore, 10 - SPAIN, 11 - SWEDEN, 29 - SWITZELAND, 12 - UK
# Number: 0 to 28
# Mandatory
P864 = 0

# Impedance Based
#30 - 600R - 600 ohms
#31 - 600C - 600 ohms + 2.16uF
#32 - 900R - 900 ohms
#33 - 900C - 900 ohms + 2.16uF
#34 - COMPLEX1 - 220 ohms + (820 ohms || 115nF)
#35 - COMPLEX2 - 270 ohms + (750 ohms || 150nF)
#36 - COMPLEX3 - 370 ohms + (620 ohms || 310nF)
#37 - COMPLEX4 - 600R, 270 ohms + (750 ohms || 150nF)
#38 - COMPLEX5 - 320 ohms + (1050 ohms || 230nF)
#39 - COMPLEX6 - 350 ohms + (1000 ohms || 210nF)
#40 - COMPLEX7 - 200 ohms + (680 ohms || 100nF)
#41 - COMPLEX8 - 370 ohms + (820 ohms || 110nF)
#42 - COMPLEX9 - 275 ohms + (780 ohms || 115nF)
#43 - COMPLEX10 - 120 ohms + (820 ohms || 110nF)
# Number: 30 to 43
# Mandatory
P849 = 30

# Number of Rings. (1-50, Default 4),(Number of rings for a PSTN incoming call before FXO port answers to accept VoIP number)
# Number: 1 to 50
# Mandatory
P798 = 4

# PSTN Ring Thru FXS. 0-No, 1 - Yes
# Number: 0, 1
# Mandatory
P842 = 1

# PSTN Ring Thru Delay   (1-10sec, Default 4)
# Number: 1 to 10
# Mandatory
P843 = 4

# PSTN Ring Timeout (2-10 seconds. Default 6 seconds)
# Used to detect PSTN hangup when FXO port is not answered
# Number: 2 to 10
# Mandatory
P3630 = 6

# PSTN Idle Wait Timeout between Outgoing Calls. (0-10 seconds. Default 4 seconds)
# Number: 0-10
# Mandatory
P4356 = 4

################################################################################
# Channel Dialing                                                              #
################################################################################
# DTMF Digit Length (40-127 milliseconds, Default 100 milliseconds)
# Number: 40 to 127
# Mandatory
P3300 = 100

# DTMF Dial Pause (40-127 milliseconds, Default 100 milliseconds)
# Number: 40 to 127
# Mandatory
P3302 = 100

# First Digit Timeout (1-20 sec., Default 10 seconds)
# Number: 1 to 20
# Mandatory
P840 = 10

# Inter-Digit Timeout (1-15 sec., Default 4 seconds)
# Number: 1 to 15
# Mandatory
P292 = 4

# Wait for Dial-Tone. 0 - No, 1 - Yes
# Number: 0, 1
# Mandatory
P3303 = 1

# Stage Method. 1 - One stage dialing, 2 - Two stage dialing
# Number: 1, 2
# Mandatory
P3304 = 2

# Min Delay Before Dial PSTN Number.
# Number: 50 - 65000
# Mandatory
P3206 = 500

##############################################################################
##  Basic Settings.                                                         ##
##############################################################################
# New End User Password
# String
#P196 = 123

# New Viewer Password. Default is viewer.
# Max Character Number: 30
# P28113=viewer 

# Web Session Timeout. In 1 to 60 minutes range. Default value is 10
# Number: 1 to 60
# Mandatory
P28116 = 10

# Web Access Attempt Limit. Default value is 5
# Number: 1 to 10
# Mandatory
P28117 = 5

# Web Lockout Duration. In 0 to 60 minutes range. Default value is 15
# Number: 0 to 60
# Mandatory
P1683 = 15

# Web Access Mode. 0 - HTTPS, 1 - HTTP.
# Number: 0, 1
# Mandatory
P1650 = 1

# HTTP Web Port. Default HTTP is 80.
# Number: 1 to 65535
# Mandatory
P901=80

# HTTPS Web Port. Defaut HTTPS port is 443.
# Number: 1 to 65535
# Mandatory
P27010=443

# Disable SSH. 1 - Yes, 0 - No.
# Number: 0, 1
# Mandatory
P276=0

# SSH Port. Default SSH port is 22.
# String
# Mandatory
P27006 = 22

# Disable Telnet
# Number: 0 , 1. 0 - NO, 1 - Yes
# Mandatory
P28120 = 1

# Telnet Port. default is 23. Cannot be the same as SSH Port.
# Number
# Mandatory
P28128 = 23

# WAN Side Web/SSH Access. 0 - No, 1 - Yes , 2 - Auto (WAN side access will be rejected if set to No)
# Default is 2 - Auto. When set to Auto, if the device is using public IP address, WAN side HTTP/SSH access will be disabled; 
# if the device is using private IP address, it will be enabled.
# Number: 0,1,2 
# Mandatory 
P190 = 0

# White List for WAN Side. Only the IP address in white list can access Web and SSH.
# String ipaddress
P20701=

# Black List for WAN Side. The IP address in black list can not access Web or SSH.
# String ipaddress
P20702=

# Internet Protocol. 0 - Both, prefer IPv4, 1 - Both, prefer IPv6, 2 - IPv4 Only, 3 - IPv6 Only. Default is IPv4 Only
# Number: 0, 1, 2, 3
# Mandatory
P1415 = 2

# IPv4 Address. 0 - DHCP, 2 - PPPoE, 1 - Static IP 
# Number: 0, 1, 2
# Mandatory
# Reboot required
P8 = 0

################################################################################
# DHCP
# DHCP Hostname, DHCP option 12. Max length allowed is 32 bytes.
# Reboot required
P146 = 

# DHCP Vendor Class ID, DHCP option 60. Max length allowed is 32 bytes.
# Reboot required
P148 = HT8XX

# DHCP domain name
# String
P147 = 

################################################################################
# PPPoE
# PPPoE account ID
# String
# Reboot required
#P82 =

# PPPoE password
# String
# Reboot required
#P83 =

# PPPoE Service Name
# String
# Reboot required
#P269 = 

# 1st Preferred DNS server
# Number: 0 to 255
# Reboot required
#P92 = 0
#P93 = 0
#P94 = 0
#P95 = 0

# 2nd Preferred DNS server
# Number: 0 to 255
#P5026=0
#P5027=0
#P5028=0
#P5029=0

# 3rd Preferred DNS server
# Number: 0 to 255
#P5030=0
#P5031=0
#P5032=0
#P5033=0

# 4th Preferred DNS server
# Number: 0 to 255
#P5034=0
#P5035=0
#P5036=0
#P5037=0

################################################################################
# Static IP
# IP Address. Ignore if DHCP or PPPoE is used
# Number: 0 to 255
# Reboot required
#P9 = 192
#P10 = 168
#P11 = 0
#P12 = 160

# Subnet mask. Ignore if DHCP or PPPoE is used
# Number: 0 to 255
# Reboot required
#P13 = 255
#P14 = 255
#P15 = 0
#P16 = 0

# Router. Ignore if DHCP or PPPoE is used
# Number: 0 to 255
# Reboot required
#P17 = 0
#P18 = 0
#P19 = 0
#P20 = 0

# DNS 1. Ignore if DHCP or PPPoE is used
# Number: 0 to 255
# Reboot required
#P21 = 0
#P22 = 0
#P23 = 0
#P24 = 0

# DNS 2. Ignore if DHCP or PPPoE is used
# Number: 0 to 255
# Reboot required
#P25 = 0
#P26 = 0
#P27 = 0
#P28 = 0

# IPv6 Address type. 0 - dynamically assigned via DHCP, 1 - statically Configured. Default is 0.
# Number: 0, 1
# Mandatory
P1419 = 0

# IPv6 Address type: Statically configured. 0 - Full Static, 1 - Prefix Static
# Number: 0, 1
# Mandatory
P1426 = 0

# Full Static: Static IPv6 Address
P1420 =

# Full Static: IPv6 Prefix Length
P1421 =

# Prefix Static: IPv6 Prefix(64bits)
# Max Character Number : 40
P1422 = 

# DNS Server 1 for IPv6 Address
# String: a-z, A-Z, 0-9, ".", ":", "[", "]"
P1424 =

# DNS Server 2 for IPv6 Address
# String: a-z, A-Z, 0-9, ".", ":", "[", "]"
P1425 =

# Preferred DNS Server for IPv6 Address
# String: a-z, A-Z, 0-9, ".", ":", "[", "]"
P1423 =

################################################################################
#Time Zone. Offset in minutes to GMT
# <value=TZA+12> GMT-12:00 (International Date Line West)
# <value=TZB+11> GMT-11:00 (Midway Island, Samoa)
# <value=HAW10> GMT-10:00 (US Hawaiian Time)
# <value=AKST9AKDT> GMT-09:00 (US Alaska Time)
# <value=PST8PDT> GMT-08:00 (US Pacific Time, Los Angeles)
# <value=PST8PDT,M4.1.0,M10.5.0> GMT-08:00 (Baja California)
# <value=MST7MDT> GMT-07:00 (US Mountain Time, Denver)
# <value=MST7> GMT-07:00 (Mountain Time (Arizona, no DST))
# <value=MST7MDT,M4.1.0,M10.5.0> GMT-07:00 (Chihuahua, La Paz, Mazatlan)
# <value=CST6CDT> GMT-06:00 (Central Time)
# <value=CST+6> GMT-06:00 (Central America)
# <value=CST6CDT,M4.1.0,M10.5.0> GMT-06:00 (Guadalajara, Mexico City, Monterrey)
# <value=EST5EDT> GMT-05:00 (Eastern Time)
# <value=EST5> GMT-05:00 (Eastern Time without daylight saving)
# <value=TZf+4:30> GMT-04:30 (Caracas)
# <value=AST4ADT> GMT-04:00 (Atlantic Time)
# <value=AST4ADT,M4.1.0/00:01:00,M10.5.0/00:01:00> GMT-04:00 (Atlantic Time (New Brunswick))
# <value=NST+3:30NDT+2:30,M4.1.0/00:01:00,M10.5.0/00:01:00> GMT-03:30 (Newfoundland Time)
# <value=TZK+3> GMT-03:00 (Greenland)
# <value=BRST+3BRDT+2,M10.3.0,M2.3.0> GMT-03:00 (Brazil, Sao Paulo)
# <value=UTC+3> GMT-02:00 (Argentina)
# <value=TZL+2> GMT-02:00 (Mid-Atlantic)
# <value=TZM+1> GMT-01:00 (Azores, Cape Verde Is.)
# <value=TZN+0> GMT (Edinburgh, Casablanca, Monrovia)
# <value=GMT+0BST-1,M3.5.0/01:00:00,M10.5.0/02:00:00> GMT (London, Great Britain)
# <value=WET-0WEST-1,M3.5.0/01:00:00,M10.5.0/02:00:00> GMT (Lisbon, Portugal)
# <value=GMT+0IST-1,M3.5.0/01:00:00,M10.5.0/02:00:00> GMT (Dublin, Ireland)
# <value=TZO-1> GMT+01:00 (Paris, Vienna, Warsaw)
# <value=CET-1CEST-2,M3.5.0/02:00:00,M10.5.0/03:00:00> GMT+01:00 (Roma, Paris, Madrid, Prague, Berlin, Budapest, Amsterdam, Barcelona)
# <value=TZO-1> GMT+01:00 (Brussels, Belgium)
# <value=TZP-2> GMT+02:00 (Israel, Cairo, Athens, Istanbul, Bucharest)
# <value=EET-2EEST-3,M3.5.0/03:00:00,M10.5.0/04:00:00> GMT+02:00 (Helsinki, Athens, Tallinn)
# <value=EET-2EEST,M3.5.0/3,M10.5.0/4> GMT+02:00 (Kyiv, Ukraine)
# <value=TZQ-3> GMT+03:00 (Kuwait, Baghdad, Tehran, Nairobi)
# <value=MSK-3MSD,M3.5.0/2,M10.5.0/3> GMT+03:00 (Moscow, Russia)
# <value=MST-3MDT,M3.5.0/2,M10.5.0/3> GMT+03:00 (St.Petersburg, Russia)
# <value=TZR-4> GMT+04:00 (Abu Dhabi, Baku)
# <value=TZS-5> GMT+05:00 (Islamabad, Ekaterinburg, Karachi, Tashkent)
# <value=TZT-5:30> GMT+05:30 (Chennai, New Delhi, Mumbai)
# <value=TZU-5:45> GMT+05:45 (Kathmandu)
# <value=TZV-6> GMT+06:00 (Almaty, Astana, Dhaka, Novosibirsk)
# <value=TZW-6:30> GMT+06:30 (Rangoon)
# <value=TZX-7> GMT+07:00 (Bankok, Hanoi, Krasnoyarsk)
# <value=WIB-7> GMT+07:00 (Jakarta)
# <value=TZY-8> GMT+08:00 (Beijing, Taipei, Kuala Lumpur, Irkutsk)
# <value=SGT-8> GMT+08:00 (Singapore)
# <value=ULAT-8> GMT+08:00 (Ulaanbaatar, Mongolia)
# <value=WST-8> GMT+08:00 (Perth)
# <value=TZZ-9> GMT+09:00 (Japan, Korea, Yakutsk)
# <value=CST-9:30CDT-10:30,M10.5.0/02:00:00,M3.5.0/03:00:00> GMT+09:30 (Adelaide)
# <value=CST-9:30> GMT+09:30 (Darwin)
# <value=TZb-10> GMT+10:00 (Guam)
# <value=EST-10EDT-11,M10.1.0/02:00:00,M3.5.0/03:00:00> GMT+10:00 (Hobart)
# <value=EST-10EDT-11,M10.5.0/02:00:00,M3.5.0/03:00:00> GMT+10:00 (Sydney, Melbourne, Canberra)
# <value=EST-10> GMT+10:00 (Brisbane)
# <value=TZc-11> GMT+11:00 (Magadan, Solomon Is., New Caledonia)
# <value=NZST-12NZDT-13,M10.1.0/02:00:00,M3.3.0/03:00:00> GMT+12:00 (Auckland, Wellington)
# <value=TZd-12> GMT+12:00 (Fiji)
# <value=TZe-13> GMT+13:00 (Nuku'alofa)
# <value=customize> Using self-defined Time Zone
# Number: a-z, A-Z, ;, +
# Mandatory
# Reboot required
P64 = customize

# Self-Defined Time Zone
# Number: a-z, A-Z, ;, +
# Mandatory
# Reboot required
P246 = MTZ+6MDT+5,M3.2.0,M11.1.0

# Allow DHCP server to set Time Zone. 0 - No, 1 - Yes
# Number: 0, 1
# Mandatory
P143=1

# Language. 0 - English, 4 - Chinese, 10 - Spanish IVR
# Number: 0, 4, 10
# Mandatory
P342 = 0

################################################################################
# NAT/DHCP Server Information & Configuration                                  #
################################################################################
# Device Mode. 0 -NAT Router, 1 - Bridge, 2 - WAN Only
# Number: 0, 1, 2
# Mandatory
# Reboot required
P231 = 0

# NAT maximum ports. range: 0 - 4096, default is 1024
# Number: 0 to 4096
# Mandatory
# Reboot required
P896 = 1024

# NAT TCP timeout. range: 0 - 3600, default is 3600
# Number: 0 to 3600
# Mandatory
# Reboot required
P897 = 3600

# NAT UDP timeout. range: 0 - 3600, default is 300
# Number: 0 to 3600
# Mandatory
# Reboot required
P898 = 300

# Uplink bandwidth. 
#<value=0> Disabled
#<value=2> 128k
#<value=3> 256k
#<value=4> 512k
#<value=5> 1M
#<value=8> 2M
#<value=9> 3M
#<value=6> 4M
#<value=10> 5M
#<value=7> 10M
#<value=11> 15M
# Number: 0, 2 to 11
# Mandatory
# Reboot required
P867 = 0

# Downlink bandwidth.
#<value=0> Disabled
#<value=2> 128k
#<value=3> 256k
#<value=4> 512k
#<value=5> 1M
#<value=8> 2M
#<value=9> 3M
#<value=6> 4M
#<value=10> 5M
#<value=7> 10M
#<value=11> 15M
# Number: 0, 2 to 11
# Mandatory
# Reboot required
P868 = 0

# Enable UPnP support. 0 - No, 1 - Yes
# Number: 0, 1
# Mandatory
P890 = 0

# Reply to ICMP on WAN port. 0 - No, 1 - Yes (Unit will not respond to PING from WAN side if set to No)
# Number: 0, 1
# Mandatory
P189 = 0

# Cloned WAN MAC Addr:
# hex format
P115 =
P116 =
P117 =
P118 =
P119 =
P120 =

# Enable LAN DHCP. 0 - No, 1 - Yes
# Number: 0, 1
# Mandatory
P5001 = 1

# LAN DHCP Base IP. (base IP for the LAN port, default is 192.168.2.1)
# Reboot required
#P111 = 192.168.2.1

# LAN DHCP Start IP. (default is 192.168.2.100) 
# ipaddress
# Mandatory
P5002 = 192.168.2.100

# LAN DHCP End IP. (default is 192.168.2.199)
# ipaddress
# Mandatory
P5003 = 192.168.2.199

# LAN Subnet Mask (default is 255.255.255.0)
# Mandatory
# Reboot required
P110 = 255.255.255.0

# DHCP IP Lease Time. (in units of hours, default is 120 hours or 5 days)
# Mandatory
P112 = 120

# DMZ IP
# IP Address
P113 = 

################################################################################
# Port Forwarding Settings.                                                    #
################################################################################
#############  Choice 1 ####################################
# WAN Port
# Number
P150 = 0 

# LAN IP
# IP Address
P158 =

# LAN Port
# Number
P166 = 0 

# Protocol.  0 - UDP Only, 1 - TCP Only, 2 - TCP and UDP.
# Number: 0, 1, 2
# Mandatory
P174 = 0 

#############  Choice 2 ####################################
# WAN Port
# Number
P151 = 0

# LAN IP
# IP Address
P159 =

# LAN Port
# Number
P167 = 0 

# Protocol.  0 - UDP Only, 1 - TCP Only, 2 - TCP and UDP.
# Number: 0, 1, 2
# Mandatory
P175 = 0

#############  Choice 3 ####################################
# WAN Port
# Number
P152 = 0 

# LAN IP
# IP Address
P160 =

# LAN Port
# Number
P168 = 0 

# Protocol.  0 - UDP Only, 1 - TCP Only, 2 - TCP and UDP.
# Number: 0, 1, 2
# Mandatory
P176 = 0

#############  Choice 4 ####################################
# WAN Port
# Number
P153 = 0

# LAN IP
# IP Address
P161 =

# LAN Port
# Number
P169 = 0

# Protocol.  0 - UDP Only, 1 - TCP Only, 2 - TCP and UDP.
# Number: 0, 1, 2
# Mandatory
P177 = 0

#############  Choice 5 ####################################
# WAN Port
# Number: 1 to 65535
P154 = 0

# LAN IP
# IP Address
P162 =

# LAN Port
# Number: 1 to 65535
P170 = 0

# Protocol.  0 - UDP Only, 1 - TCP Only, 2 - TCP and UDP.
# Number: 0, 1, 2
# Mandatory
P178 = 0

#############  Choice 6 ####################################
# WAN Port
# Number: 1 to 65535
P155 = 0

# LAN IP
# IP Address
P163 =

# LAN Port
# Number: 1 to 65535
P171 = 0

# Protocol.  0 - UDP Only, 1 - TCP Only, 2 - TCP and UDP.
# Number: 0, 1, 2
# Mandatory
P179 = 0

#############  Choice 7 ####################################
# WAN Port
# Number: 1 to 65535
P156 = 0

# LAN IP
# IP Address
P164 =

# LAN Port
# Number: 1 to 65535
P172 = 0

# Protocol.  0 - UDP Only, 1 - TCP Only, 2 - TCP and UDP.
# Number: 0, 1, 2
# Mandatory
P180 = 0

#############  Choice 8 ####################################
# WAN Port
# Number: 1 to 65535
P157 = 0

# LAN IP
# IP Address
P165 = 

# LAN Port
# Number: 1 to 65535
P173 = 0 

# Protocol.  0 - UDP Only, 1 - TCP Only, 2 - TCP and UDP.
# Number: 0, 1, 2
# Mandatory
P181 =  0

################################################################################
# PSTN Access Code (Default value *00)
# String
P195 = *00

# PIN for VoIP-To-PSTN calls (maximum 8 digits)
# String
P794 = 

# PIN for PSTN-To-VOIP calls (maximum 8 digits)
# String
P795 = 

# Unconditional Call forward to PSTN (VoIP calls will be forwarded to the specified PSTN number)
# String
P796 = 

# Unconditional call forward to VoIP
# SIP User ID
# String
P3305 = 

# SIP Server
# Server address
P3306 = 

# SIP Destination Port
# Number: 1 to 65535
P3307 = 5060