##########################################################################################
## Configuration Template For GRP260x Firmware Version 1.0.1.18   ##
##########################################################################################

####################################################################
# Accounts                                                        ##
####################################################################
####################################################################
# Account 1                                                       ##
####################################################################
###############################################################
# Account 1/General Settings
###############################################################
###############################################################
# Account 1/General Settings/Account Register
###############################################################

# Account Active. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P271 = 0

# Account Name
# String
P270 =

# SIP Server
# String
P47 =

# Secondary SIP Server
# String
P2312 =

# SIP User ID
# String
P35 =

# SIP Authentication ID
# String
P36 =

# SIP Authentication Password
# String
P34 =

# Name
# String
P3 =

# Tel URI. 0 - Disabled, 1 - User=Phone, 2 - Enabled. Default is 0
# Number: 0, 1, 2
# Mandatory
P63 = 0

# Voicemail Access Number
# String
P33 =

# BLF Server
# String
P2375 = 

# Account Display
# Number: 0, 1. 0 - User Name, 1 - User ID. Default is 0
# Mandatory
P2380 = 0

###############################################################
# Account 1/General Settings/Network Settings
###############################################################

# Outbound Proxy
# String
P48 =

# Secondary Outbound Proxy
# String
P2333 = 

# DNS Mode. 0 - A Record, 1 - SRV, 2 - NAPTR/SRV, 3 - Use Configured IP. Default is 0
# Number: 0, 1, 2, 3
# Mandatory
P103 = 0

# DNS SRV Failover Mode. 0 - Default, 1 - Saved one until DNS TTL, 2 - Saved one until no response. Default is 0
# Number: 0,1,2
# Mandatory
P26040 = 0

# Primary IP. Maximum 15 characters
# String
P2308 =

# Backup IP 1
# String
P2309 =

# Backup IP 2
# String
P2310 =

# NAT Traversal. 0 - No, 1 - STUN, 2 - keep alive, 3 - UPnP, 4 - Auto, 5 - VPN. Default is 4.
# Number: 0, 1, 2, 3, 4, 5
# Mandatory
P52 = 4

# Proxy-Require (A SIP extension to enable firewall penetration). Max length is 64 characters
# String
P197 =

# Use SBC. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P26090 = 0

###############################################################
# Account 1/SIP Settings
###############################################################
###############################################################
# Account 1/SIP Settings/Basic Settings
###############################################################
# SIP Registration. 0 - No, 1 - Yes. Default is 1
# Number: 0, 1
# Mandatory
P31 = 1

# Unregister On Reboot. 0 - No, 1 - Yes, 2 - Instance. Default is 0
# Number: 0, 1, 2
# Mandatory
P81 = 0

# Register Expiration (in minutes). Default is 60. Max about 45 days
# Number: 1 - 64800
# Mandatory
P32 = 60

# Subscribe Expiration (in minutes). Default is 60. Max about 45 days
# Number: 1 - 64800
# Mandatory
P26051 = 60

# Re-register Before Expiration (in seconds). Default is 0 seconds
# Number: 0 - 64800
# Mandatory
P2330 = 0

# Registration Retry Wait Time (in seconds). Default is 20
# Number: 1 - 3600
# Mandatory
P138 = 20

# Add Auth Header On Initial REGISTER. Default is 0
# Number: 0, 1
# Mandatory
P2359 = 0

# Enable OPTIONS Keep Alive. 0 - No, 1 - Yes. Default is 0
# Number: 0,1
# Mandatory
P2397 = 0

# OPTIONS Keep Alive Interval. Default is 30
# Number
# Mandatory
P2398 = 30

# OPTIONS Keep-Alive Max Tries. Default is 3
# Number
# Mandatory
P2399 = 3

# SUBSCRIBE for MWI. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P99 = 0

# SUBSCRIBE for Registration. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P2319 = 0

# Use Privacy Header
# 0 - Default, 1 - No, 2 - Yes. Default is 0
# Number: 0, 1, 2
# Mandatory
P2338 = 0

# Use P-Preferred-Identity Header
# 0 - Default, 1 - No, 2 - Yes. Default is 0
# Number: 0, 1, 2
# Mandatory
P2339 = 0

# Use X-Grandstream-PBX Header
# 0 - No, 1 - Yes. Default is 1
# Number: 0, 1
# Mandatory
P26054 = 1

# Use P-Access-Network-Info Header
# 0 - No, 1 - Yes. Default is 1
# Number: 0, 1
# Mandatory
P26058 = 1

# Use P-Emergency-Info Header
# 0 - No, 1 - Yes. Default is 1
# Number: 0, 1
# Mandatory
P26059 = 1

# Use MAC Header
# 0 - No, 1 - Only for REGISTER, 2 - Yes to all SIP. Default is 0
# Number: 0, 1, 2
# Mandatory
P29090 = 0

# Add MAC in User-Agent
# 0 - No, 1 - Yes except REGISTER, 2 - Yes to all SIP. Default is 0
# Number: 0, 1, 2
# Mandatory
P26061 = 0

# SIP Transport. 0 - UDP, 1 - TCP, 2 - TLS/TCP. Default is 0
# Number: 0, 1, 2
# Mandatory
P130 = 0

# SIP Listening Mode. 
# 0 - Transport Only, 1 - Dual, 2 - Dual (BLF Enforced), 3 - Dual (Secured). Default is 0
# Number: 0,1,2,3
# Mandatory
P26024 = 0

# Local SIP Port. Default is 5060
# Number
# Mandatory
P40 = 5060

# SIP URI Scheme when using TLS. 0 - sip, 1 - sips. Default is 1
# Number: 0, 1
# Mandatory
P2329 = 1

# Use Actual Ephemeral Port in Contact with TCP/TLS. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P2331 = 0

# Support SIP Instance ID. 0 - No, 1 - Yes. Default is 1
# Number: 0, 1
# Mandatory
P288 = 1

# SIP T1 Timeout. RFC 3261 T1 value (RTT estimate)
# 50 - 0.5 sec, 100 - 1 sec, 200 - 2 sec. Default is 50
# Number: 50, 100, 200
# Mandatory	
P209 = 50

# SIP T2 Timeout. RFC 3261 T2 value. The maximum retransmit interval for non-INVITE requests and INVITE responses
# 200 - 2 sec, 400 - 4 sec, 800 - 8 sec. Default is 400
# Number: 200, 400, 800
# Mandatory
P250 = 400

# Outbound Proxy Mode. 0 - in route, 1 - not in route, 2 - always send to
# Number: 0, 1, 2
# Mandatory
P2305 = 0

# Enable 100rel. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P272 = 0

###############################################################
# Account 1/SIP Settings/Session Timer
###############################################################
# Enable Session Timer. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P2395 = 0

# Session Expiration (in seconds). Default is 180
# Number: 90 - 64800
# Mandatory
P260 = 180

# Min-SE (in seconds). Default is 90.
# Number: 90 - 64800
# Mandatory
P261 = 90

# Caller Request Timer (Request for timer when calling). 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P262 = 0

# Callee Request Timer (Request for timer when called. i.e. if remote party supports timer but did not request for one)
# 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P263 = 0

# Force Timer (Still use timer when remote party does not support timer). 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P264 = 0

# UAC Specify Refresher. 0 - Omit, 1 - UAC, 2 - UAS. Default is 1
# Number: 0 - 2
# Mandatory
P266 = 1

# UAS Specify Refresher. 1 - UAC, 2 - UAS. Default is 1
# Number: 1, 2
# Mandatory
P267 = 1

# Force INVITE (Always refresh with INVITE instead of UPDATE even when remote party supports UPDATE).
# 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P265 = 0

###############################################################
# Account 1/Codec Settings
###############################################################
###############################################################
# Account 1/Codec Settings/Audio
###############################################################
# Preferred Vocoder
# 0 - PCMU, 2 - G.726-32, 4 - G.723.1, 8 - PCMA, 9 - G.722, 18 - G.729A/B, 98 - iLBC, 123 - OPUS
# choice 1. Default is 0
# Number: 0, 2, 4, 8, 9, 18, 98, 123
# Mandatory
P57 = 0

# choice 2. Default is 8
# Number: 0, 2, 4, 8, 9, 18, 98, 123 
# Mandatory
P58 = 8

# choice 3. Default is 4
# Number: 0, 2, 4, 8, 9, 18, 98, 123
# Mandatory
P59 = 4

# choice 4. Default is 18
# Number: 0, 2, 4, 8, 9, 18, 98, 123
# Mandatory
P60 = 18

# choice 5. Default is 9
# Number: 0, 2, 4, 8, 9, 18, 98, 123
# Mandatory
P61 = 9

# choice 6. Default is 98
# Number: 0, 2, 4, 8, 9, 18, 98, 123
# Mandatory
P62 = 98

# choice 7. Default is 2
# Number: 0, 2, 4, 8, 9, 18, 98, 123
# Mandatory
P46 = 2

# choice 8. Default is 125
# Number: 0, 2, 4, 8, 9, 18, 98, 123
# Mandatory
P98 = 123

# Codec Negotiation Priority. 0 - Caller, 1 - Callee. Default is 1
# Number: 0, 1
# Mandatory
P29061 = 1

# Use First Matching Vocoder in 200OK SDP. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P2348 = 0

# iLBC Frame Size. 0 - 20ms, 1 - 30ms. Default is 1
# Number: 0, 1
# Mandatory
P97 = 1

# iLBC Payload Type. Default is 97
# Number: 96 - 127
# Mandatory
P96 = 97

# G.726-32 Packing Mode. 0 - ITU, 1 - IETF. Default is 0
# Number: 0, 1
# Mandatory
P2323 = 0

# G.726-32 Dynamic Payload Type. Default is 127
# Number: 96 - 127
# Mandatory
P2365 = 127

# OPUS Payload Type. Default is 123
# Number: 96 - 127
# Mandatory
P2385 = 123

# Send DTMF: In-audio. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P2301 = 0

# Send DTMF: Via RTP (RFC2833). 0 - No, 1 - Yes. Default is 1
# Number: 0, 1
# Mandatory
P2302 = 1

# Send DTMF: Via SIP INFO. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P2303 = 0

# DTMF Payload Type. Default is 101
# Number: 96 - 127
# Mandatory
P79 = 101

# Enable Audio RED with FEC. Default is 1.
# Number: 0, 1
# Mandatory
P26073 = 1

# Audio FEC Payload Type. Default is 121.
# Number: 96-126
# Mandatory
P26074 = 121

# Audio RED Payload Type. Default is 124.
# Number: 96-126
# Mandatory
P26075 = 124

# Silence Suppression. 0 - No, 1 - Yes. Default is 0
# Number: 0,1
# Mandatory
P50 = 0

# Jitter Buffer Type. 0 - Fixed, 1 - Adaptive. Default is 1
# Number: 0, 1
# Mandatory
P133 = 1

# Jitter Buffer Length. 0 - 100ms, 1 - 200ms, 2 - 300ms, 3 - 400ms, 4 - 500ms, 5 - 600ms, 6 - 700ms, 7 - 800ms
# Default is 2
# Number: 0, 1, 2, 3, 4, 5, 6, 7
# Mandatory
P132 = 2

# Voice Frames per TX (up to 10/20/32/64 frames for G711/G726/G723/other codecs respectively). Default is 2
# Number: 1 - 6
# Mandatory
P37 = 2

# G723 Rate. 0 - 6.3kbps encoding rate, 1 - 5.3kbps encoding rate. Default is 1
# Number: 0, 1
# Mandatory
P49 = 1

###############################################################
# Account 1/Codec Settings/RTP Settings
###############################################################
# SRTP Mode. 0 - Disabled, 1 - Enabled but not forced, 2 - Enabled and forced, 3 - Optional. Default is 0
# Number: 0, 1, 2, 3
# Mandatory
P183 = 0

# SRTP Key Length. 0 - AES 128&256 bit, 1 - AES 128 bit, 2 - AES 256 bit. Default is 0
# Default is 0
# Number: 0,1
# Mandatory
P2383 = 0

# Crypto Life Time
# 0 - No, 1 - Yes. Default is 1
# Number: 0, 1
# Mandatory
P2363 = 1

# VQ RTCP-XR
# VQ RTCP-XR Collector Name.
# String
P26093 =

# VQ RTCP-XR Collector Address.
# String
P26094 =

# VQ RTCP-XR Collector Port
# String
P26095 = 5060

# Symmetric RTP. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P291 = 0

# RTP Timeout (s). Default is 30.
# Number: 0, 6 - 600.
# Mandatory
P29068 = 0

###############################################################
# Account 1/Call Settings
###############################################################
###############################################################
# Account 1/Call Settings/Call Features
###############################################################
# Auto Answer. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P90 = 0

# Custom Alert-Info for Auto Answer.
# String
P2356 = 

# Allow Auto Answer by Call-Info/Alert-Info. 0 - No, 1 - Yes. Default is 1
# Number: 0, 1
# Mandatory
P298 = 1

# Allow Barging by Call-Info/Alert-Info. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P26019 = 0

# Send Anonymous (caller ID will be blocked if set to Yes). 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P65 = 0

# Anonymous Call Rejection. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P129 = 0

# Call Log. 0 - Log All Calls, 1 - Log Incoming/Outgoing only (missed calls NOT recorded), 2 - Disable Call Log. Default is 0
# Number: 0, 1, 2
# Mandatory
P182 = 0

# Transfer on Conference Hangup. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P2304 = 0

# Key as Send. 0 - Disabled, 1 - Pound (#), 2 - Star (*). Default is 1
# Number: 0, 1, 2
# Mandatory
P72 = 1

# Record Key Default Function. 0 - Record On, 1 - Record Off
P29066 = 0

# Call Recording On
# String
P26028 = 

# Call Recording Off
# String
P26029 = 

# Enable Recovery on Blind Transfer. 0 - Yes, 1 - No. Default is 0
# Number: 0, 1
# Mandatory
P2384 = 0

# Blind Transfer Wait Timeout. Default is 30
# Number: 30 - 300
# Mandatory
P26070 = 30

# No Key Entry Timeout (in seconds). Default is 4
# Number: 1 - 15
# Mandatory
P85 = 4

# Ring Timeout (in seconds). Default is 60
# Number: 30 - 3600
# Mandatory
P1328 = 60

# Refer-To Use Target Contact. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P135 = 0

# RFC2543 Hold. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P26062= 0

# Disable Call Waiting. 0 - Default, 1 - No, 2 - Yes. Default is 0
# Number: 0, 1, 2
# Mandatory
P26063 = 0

###############################################################
# Account 1/Call Settings/Dial Plan
###############################################################
# Dial Plan Prefix
# String 
P66 =

# Bypass Dial Plan
# String: contact,incoming,outgoing,dialing,mpk,api
P2382 = mpk

# Dial Plan. Default value is { x+ | \+x+ | *x+ | *xx*x+ }
# String
# Mandatory
P290 = { x+ | \+x+ | *x+ | *xx*x+ }

###############################################################
# Account 1/Call Settings/Call Display
###############################################################
# Caller ID Display. 0 - Auto, 1 - Disabled, 2 - From Header. Default is 2
# Number: 0, 1, 2
# Mandatory
P2324 = 2

# Callee ID Display. 0 - Auto, 1 - Disabled, 2 - To Header. Default is 0
# Number: 0, 1, 2
# Mandatory
P26025 = 0

###############################################################
# Account 1/Call Settings/Ringtone
###############################################################
# Account Ring Tone. 0 - system, 1 - ring1, 2 - ring2, 3 - ring3, 4 - ring4, 5 - ring5, 6 - ring6, 7 - Doorbell, 8 - silent. Default is 0
# Number: 0-8, more if using custom ringtone
# Mandatory
P104 = 0

# Ignore Alert-Infor header
# 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P26018 = 0

# Matching Incoming Caller ID. Matching Rule 1
# String
P1488 = 

# Matching Rule 1 Distinctive Ringtone
# 0 - system, 1 - ring1, 2 - ring2, 3 - ring3, 4 - ring4, 5 - ring5, 6 - ring6, 7 - Doorbell, 8 - silent. Default is 0
# Number: 0-8, more if using custom ringtone
# Mandatory
P1489 = 0

# Matching Incoming Caller ID. Matching Rule 2
# String
P1490 = 

# Matching Rule 2 Distinctive Ringtone
# 0 - system, 1 - ring1, 2 - ring2, 3 - ring3, 4 - ring4, 5 - ring5, 6 - ring6, 7 - Doorbell, 8 - silent. Default is 0
# Number: 0-8, more if using custom ringtone
# Mandatory
P1491 = 0

# Matching Incoming Caller ID. Matching Rule 3
# String
P1492 =

# Matching Rule 3 Distinctive Ringtone
# 0 - system, 1 - ring1, 2 - ring2, 3 - ring3, 4 - ring4, 5 - ring5, 6 - ring6, 7 - Doorbell, 8 - silent. Default is 0
# Number: 0-8, more if using custom ringtone
# Mandatory
P1493 = 0

# Matching Incoming Caller ID. Matching Rule 4
# String
P6716 = 

# Matching Rule 4 Distinctive Ringtone
# 0 - system, 1 - ring1, 2 - ring2, 3 - ring3, 4 - ring4, 5 - ring5, 6 - ring6, 7 - Doorbell, 8 - silent. Default is 0
# Number: 0-8, more if using custom ringtone
# Mandatory
P6717 = 0

# Matching Incoming Caller ID. Matching Rule 5
# String
P6718 = 

# Matching Rule 5 Distinctive Ringtone
# 0 - system, 1 - ring1, 2 - ring2, 3 - ring3, 4 - ring4, 5 - ring5, 6 - ring6, 7 - Doorbell, 8 - silent. Default is 0
# Number: 0-8, more if using custom ringtone
# Mandatory
P6719 = 0

# Matching Incoming Caller ID. Matching Rule 6
# String
P6720 = 

# Matching Rule 6 Distinctive Ringtone
# 0 - system, 1 - ring1, 2 - ring2, 3 - ring3, 4 - ring4, 5 - ring5, 6 - ring6, 7 - Doorbell, 8 - silent. Default is 0
# Number: 0-8, more if using custom ringtone
# Mandatory
P6721 = 0

# Matching Incoming Caller ID. Matching Rule 7
# String
P26064 = 

# Matching Rule 7 Distinctive Ringtone
# 0 - system, 1 - ring1, 2 - ring2, 3 - ring3, 4 - ring4, 5 - ring5, 6 - ring6, 7 - Doorbell, 8 - silent. Default is 0
# Number: 0-8, more if using custom ringtone
# Mandatory
P26065 = 0

# Matching Incoming Caller ID. Matching Rule 8
# String
P26066 = 

# Matching Rule 8 Distinctive Ringtone
# 0 - system, 1 - ring1, 2 - ring2, 3 - ring3, 4 - ring4, 5 - ring5, 6 - ring6, 7 - Doorbell, 8 - silent. Default is 0
# Number: 0-8, more if using custom ringtone
# Mandatory
P26067 = 0

# Matching Incoming Caller ID. Matching Rule 9
# String
P26068 = 

# Matching Rule 9 Distinctive Ringtone
# 0 - system, 1 - ring1, 2 - ring2, 3 - ring3, 4 - ring4, 5 - ring5, 6 - ring6, 7 - Doorbell, 8 - silent. Default is 0
# Number: 0-8, more if using custom ringtone
# Mandatory
P26069 = 0

# Matching Incoming Caller ID. Matching Rule 10
# String
P26096 = 

# Matching Rule 10 Distinctive Ringtone
# 0 - system, 1 - ring1, 2 - ring2, 3 - ring3, 4 - ring4, 5 - ring5, 6 - ring6, 7 - Doorbell, 8 - silent. Default is 0
# Number: 0-8, more if using custom ringtone
# Mandatory
P26097 = 0

###############################################################
# Account 1/Advanced Settings
###############################################################
###############################################################
# Account 1/Advanced Settings/Security Settings
###############################################################
# Check Domain Certificates. When set to Yes/Enabled, domain certificate will be checked as defined in RFC5922
# 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P2311 = 0

# Validate Certification Chain. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P2367 = 0

# Validate Incoming SIP Messages. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P2306 = 0

# Omit charset=UTF-8 in MESSAGE. 0 - Disabled, 1 - Enabled. Default is 0
# Number: 0, 1
# Mandatory
P2355 = 0

# Allow Unsolicited REFER. 0 - Disabled, 1 - Enabled, 2 - Enabled/Force Auth. Default is 0
# Number: 0, 1, 2
# Mandatory
P26023 = 0

# Accept Incoming SIP from Proxy Only. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P2347 = 0

# Check SIP User ID for incoming INVITE. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P258 = 0

# Allow SIP Reset
# 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P26015 = 0

# Authenticate Incoming INVITE. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P2346 = 0

###############################################################
# Account 1/Advanced Settings/MOH
###############################################################
# On Hold Reminder Tone. 0 - Disabled, 1 - Enable. Default is 1
# Number: 0, 1
# Mandatory
P26006 = 1

# Music On Hold URI
# String
P2350 =

###############################################################
# Account 1/Advanced Settings/Advanced Features
###############################################################
# Special Feature. 100 - Standard, 101 - Nortel MCS, 102- Broadsoft, 108 - CBCOM, 
# 109 - RNK, 110 - Sylantro, 117 - Huawei IMS, 119 - Phonepower, 120 - UCM Call Center
# Default is 100
# Number: 100, 101, 102, 108, 109, 110, 117, 119, 120
# Mandatory
P198 = 100

# Feature Key Synchronization. 0 - Disabled, 1 - Enabled. Default is 0
# Number: 0, 1
# Mandatory
P2325 = 0

# Conference URI
# String
P2318 =

# Broadsoft
# Broadsoft Call Center. 0 - Disabled, 1 - Enabled. Default is 0
# Number: 0, 1
# Mandatory
P2341 = 0

# Hoteling Event. 0 - Disabled, 1 - Enabled. Default is 0
# Number: 0, 1
# Mandatory
P2342 = 0

# Call Center Status. 0 - Disabled, 1 - Enabled. Default is 0
# Number: 0, 1
# Mandatory
P2343 = 0

# Broadsoft Executive Assistant. 0 - Disabled, 1 - Enabled. Default is 0
# Number: 0, 1
# Mandatory
P2364 = 0

# Broadsoft Call Park. 0 - Disabled, 1 - Enabled. Default is 0
# Number: 0, 1
# Mandatory
P2388 = 0

###############################################################
# Account 1/Advanced Settings/BLF(Busy Lamp Field)  2604 only
###############################################################
# Presence Eventlist URI
# String
P26084 =

# Eventlist BLF URI
# String
P134 =

# Auto Provision Eventlists. 0 - Disabled, 1 - BLF Eventlist, 2 - Presence Eventlist. Default is 0
# Number:0,1,2
# Mandatory
P2389 = 0

# BLF Call-pickup. 0 - Auto, 1 - Force BLF Call-pickup by prefix, 2 - Disabled. Default is 0
# Number: 0, 1, 2
# Mandatory
P6752 = 0

# BLF Call-pickup Prefix. Default is **
# String
# Mandatory
P1347 = **

# Call Pickup Barge-In Code
# String
P26046 = 

# PUBLISH for Presence. 0 - Disabled, 1 - Enabled. Default is 0
# Number: 0, 1
# Mandatory
P188 = 0

###############################################################
# Account 1/SCA
###############################################################
# Enable SCA (Shared Call Appearance)
# Number: -1, 32. -1 - Disabled, 32 - Enabled
# Mandatory
P1363 = 0

# Line-Seize Timeout (in seconds). Default is 15
# Number: 15 - 60
# Mandatory
P2313 = 15

###############################################################
# Account 1/Feature Codes
###############################################################
#Enable Local Call Features.  0 - No, 1 - Yes. Default is 1
#Number: 0, 1 
#Mandatory
P191 = 1

#Do Not Disturb (DND) - On
# String
P2344 = 

#Do Not Disturb (DND) - Off
# String
P2345 =

# Call Forward Always - On
# String
P26013 = 

# Call Forward Always - Off
# String
P26014 = 

# Call Forward Always - Target
# String
P29092 = 

# Call Forward Busy - On
# String
P26009 = 

# Call Forward Busy - Off
# String
P26010 = 

# Call Forward Busy - Target
# String
P29093 = 

# Call Forward No Answer - On
#String
P26011 = 

# Call Forward No Answer - Off
#String
P26012 = 

# Call Forward No Answer - Target
#String
P29094 = 

# Call Forward No Answer Timeout (s). Default is 12
# Number: 1 - 120
# Mandatory
P139 = 12

####################################################################
# Account 2                                                       ##
####################################################################
###############################################################
# Account 2/General Settings
###############################################################
###############################################################
# Account 2/General Settings/Account Register
###############################################################
# Account Active. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P401 = 0

# Account Name
# String
P417 =

# SIP Server
# String
P402 =

# Secondary SIP Server
# String
P2412 =

# SIP User ID
# String
P404 =

# SIP Authentication ID
# String
P405 =

# SIP Authentication Password
# String
P406 =

# Name
# String
P407 =

# TEL URI. 0 - Disabled, 1 - User=Phone, 2 - Enabled. Default is 0
# Number: 0, 1, 2
# Mandatory
P409 = 0

# Voicemail Access Number
# String
P426 =

# BLF Server
# String
P2475 = 

# Account Display
# Number: 0, 1. 0 - User Name, 1 - User ID. Default is 0
# Mandatory
P2480 = 0

###############################################################
# Account 2/General Settings/Network Settings
###############################################################
# Outbound Proxy
# String
P403 =

# Backup Outbound Proxy
# String
P2433 = 

# DNS Mode. 0 - A Record, 1 - SRV, 2 - NAPTR/SRV, 3 - Use Configured IP. Default is 0
# Number: 0, 1, 2, 3
# Mandatory
P408 = 0

# DNS SRV Failover Mode. 0 - Default, 1 - Saved one until DNS TTL, 2 - Saved one until no response. Default is 0
# Number: 0,1,2
# Mandatory
P26140 = 0

# Primary IP. Maximum 15 characters
# String
P2408 =

# Backup IP 1
# String
P2409 =

# Backup IP 2
# String
P2410 =

# NAT Traversal. 0 - No, 1 - STUN, 2 - keep alive, 3 - UPnP, 4 - Auto, 5 - VPN. Default is 4.
# Number: 0, 1, 2, 3, 4, 5
# Mandatory
P414 = 4

# Proxy-Require (A SIP extension to enable firewall penetration). Max length is 64 characters
# String
P418 =

# Use SBC. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P26190 = 0

###############################################################
# Account 2/SIP Settings
###############################################################
###############################################################
# Account 2/SIP Settings/Basic Settings
###############################################################
# SIP Registration. 0 - No, 1 - Yes. Default is 1
# Number: 0, 1
# Mandatory
P410 = 1

# Unregister On Reboot. 0 - No, 1 - Yes, 2 - Instance. Default is 0
# Number: 0, 1, 2
# Mandatory
P411 = 0

# Register Expiration (in minutes). Default is 60. Max about 45 days
# Number: 1 - 64800
# Mandatory
P412 = 60

# Subscribe Expiration (in minutes). Default is 60. Max about 45 days
# Number: 1 - 64800
# Mandatory
P26151 = 60

# Reregister Before Expiration (in seconds). Default is 0 seconds
# Number: 0 - 64800
# Mandatory
P2430 = 0

# SIP Registration Failure Retry Wait Time (in seconds). Default is 20
# Number: 1 - 3600
# Mandatory
P471 = 20

# Add Auth Header On Initial REGISTER. Default is 0
# Number: 0, 1
# Mandatory
P2459 = 0

# Enable OPTIONS Keep Alive. 0 - No, 1 - Yes. Default is 0
# Number: 0,1
# Mandatory
P2497 = 0

# OPTIONS Keep Alive Interval. Default is 30
# Number
# Mandatory
P2498 = 30

# OPTIONS Keep Alive Max Lost. Default is 3
# Number
# Mandatory
P2499 = 3

# SUBSCRIBE for MWI. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P415 = 0

# SUBSCRIBE for Registration. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P2419 = 0

# Use Privacy Header
# 0 - Default, 1 - No, 2 - Yes. Default is 0
# Number: 0, 1, 2
# Mandatory
P2438 = 0

# Use P-Preferred-Identity Header
# 0 - Default, 1 - No, 2 - Yes. Default is 0
# Number: 0, 1, 2
# Mandatory
P2439 = 0

# Use X-Grandstream-PBX Header
# 0 - No, 1 - Yes. Default is 1
# Number: 0, 1
# Mandatory
P26154 = 1

# Use P-Access-Network-Info Header
# 0 - No, 1 - Yes. Default is 1
# Number: 0, 1
# Mandatory
P26158 = 1

# Use P-Emergency-Info Header
# 0 - No, 1 - Yes. Default is 1
# Number: 0, 1
# Mandatory
P26159 = 1

# Use MAC Header
# 0 - No, 1 - Only for REGISTER, 2 - Yes to all SIP. Default is 0
# Number: 0, 1, 2
# Mandatory
P29190 = 0

# Add MAC in User-Agent
# 0 - No, 1 - Yes except REGISTER, 2 - Yes to all SIP. Default is 0
# Number: 0, 1, 2
# Mandatory
P26161 = 0

# SIP Transport. 0 - UDP, 1 - TCP, 2 - TLS/TCP. Default is 0
# Number: 0, 1, 2
# Mandatory
P448 = 0

# SIP Listening Mode. 
# 0 - Transport Only, 1 - Dual, 2 - Dual (BLF Enforced), 3 - Dual (Secured). Default is 0
# Number: 0,1,2,3
# Mandatory
P26124 = 0

# Local SIP Port. Default is 5062
# Number
# Mandatory
P413 = 5062

# SIP URI Scheme when using TLS. 0 - sip, 1 - sips. Default is 1
# Number: 0, 1
# Mandatory
P2429 = 1

# Use Actual Ephemeral Port in Contact with TCP/TLS. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P2431 = 0

# Support SIP Instance ID. 0 - No, 1 - Yes. Default is 1
# Number: 0, 1
# Mandatory
P489 = 1

# SIP T1 Timeout. RFC 3261 T1 value (RTT estimate)
# 50 - 0.5 sec, 100 - 1 sec, 200 - 2 sec. Default is 50
# Number: 50, 100, 200
# Mandatory	
P440 = 50

# SIP T2 Timeout. RFC 3261 T2 value. The maximum retransmit interval for non-INVITE requests and INVITE responses
# 200 - 2 sec, 400 - 4 sec, 800 - 8 sec. Default is 400
# Number: 200, 400, 800
# Mandatory
P441 = 400

# Outbound Proxy Mode. 0 - in route, 1 - not in route, 2 - always send to
# Number: 0, 1, 2
# Mandatory
P2405 = 0

# Enable 100rel. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P435 = 0

###############################################################
# Account 2/SIP Settings/Session Timer
###############################################################
# Enable Session Timer. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P2495 = 0

# Session Expiration (in seconds). Default is 180
# Number: 90 - 64800
# Mandatory
P434 = 180

# Minimum SE (in seconds). Default is 90. This value must be lower than or equal to P260
# Number: 90 - 64800
# Mandatory
P427 = 90

# Caller Request Timer (Request for timer when calling). 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P428 = 0

# Callee Request Timer (Request for timer when called. i.e. if remote party supports timer but did not request for one)
# 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P429 = 0

# Force Timer (Still use timer when remote party does not support timer). 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P430 = 0

# UAC Specify Refresher. 0 - Omit, 1 - UAC, 2 - UAS. Default is 1
# Number: 0 - 2
# Mandatory
P432 = 1

# UAS Specify Refresher. 1 - UAC, 2 - UAS. Default is 1
# Number: 1, 2
# Mandatory
P433 = 1

# Force INVITE (Always refresh with INVITE instead of UPDATE even when remote party supports UPDATE).
# 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P431 = 0

###############################################################
# Account 2/Codec Settings
###############################################################
###############################################################
# Account 2/Codec Settings/Audio
###############################################################
# Preferred Vocoder
# 0 - PCMU, 2 - G.726-32, 4 - G.723.1, 8 - PCMA, 9 - G.722, 18 - G.729A/B, 98 - iLBC, 123 - OPUS
# choice 1. Default is 0
# Number: 0, 2, 4, 8, 9, 18, 98, 123
# Mandatory
P451 = 0

# choice 2. Default is 8
# Number: 0, 2, 4, 8, 9, 18, 98, 123
# Mandatory
P452 = 8

# choice 3. Default is 4
# Number: 0, 2, 4, 8, 9, 18, 98, 123
# Mandatory
P453 = 4

# choice 4. Default is 18
# Number: 0, 2, 4, 8, 9, 18, 98, 123
# Mandatory
P454 = 18

# choice 5. Default is 9
# Number: 0, 2, 4, 8, 9, 18, 98, 123
# Mandatory
P455 = 9

# choice 6. Default is 98
# Number: 0, 2, 4, 8, 9, 18, 98, 123
# Mandatory
P456 = 98

# choice 7. Default is 2
# Number: 0, 2, 4, 8, 9, 18, 98, 123
# Mandatory
P457 = 2

# choice 8. Default is 123
# Number: 0, 2, 4, 8, 9, 18, 98, 123
# Mandatory
P458 = 123

# Codec Negotiation Priority. 0 - Caller, 1 - Callee. Default is 1
# Number: 0, 1
# Mandatory
P29161 = 1

# Use First Matching Vocoder in 200OK SDP. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P2448 = 0

# iLBC Frame Size. 0 - 20ms, 1 - 30ms. Default is 1
# Number: 0, 1
# Mandatory
P495 = 1

# iLBC Payload Type. Default is 97
# Number: 96 - 127
# Mandatory
P494 = 97

# G.726-32 Packing Mode. 0 - ITU, 1 - IETF. Default is 0
# Number: 0, 1
# Mandatory
P2423 = 0

# G.726-32 Dynamic Payload Type. Default is 127
# Number: 96 - 127
# Mandatory
P2465 = 127

# OPUS Payload Type. Default is 123
# Number: 96 - 127
# Mandatory
P2485 = 123

# Send DTMF: In-audio. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P2401 = 0

# Send DTMF: Via RTP (RFC2833). 0 - No, 1 - Yes. Default is 1
# Number: 0, 1
# Mandatory
P2402 = 1

# Send DTMF: Via SIP INFO. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P2403 = 0

# DTMF Payload Type. Default is 101
# Number: 96 - 127
# Mandatory
P496 = 101

# Enable Audio RED with FEC. Default is 1.
# Number: 0, 1
# Mandatory
P26173 = 1

# Audio FEC Payload Type. Default is 121.
# Number: 96-126
# Mandatory
P26174 = 121

# Audio RED Payload Type. Default is 124.
# Number: 96-126
# Mandatory
P26175 = 124

# Silence Suppression. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P485 = 0

# Jitter Buffer Type. 0 - Fixed, 1 - Adaptive. Default is 1
# Number: 0, 1
# Mandatory
P498 = 1

# Jitter Buffer Length. 0 - 100ms, 1 - 200ms, 2 - 300ms, 3 - 400ms, 4 - 500ms, 5 - 600ms, 6 - 700ms, 7 - 800ms
# Default is 2
# Number: 0, 1, 2, 3, 4, 5, 6, 7
# Mandatory
P497 = 2

# Voice Frames per TX (up to 10/20/32/64 frames for G711/G726/G723/other codecs respectively). Default is 2
# Number: 1 - 6
# Mandatory
P486 = 2

# G723 Rate. 0 - 6.3kbps encoding rate, 1 - 5.3kbps encoding rate. Default is 1
# Number: 0, 1
# Mandatory
P493 = 1

###############################################################
# Account 2/Codec Settings/RTP Settings
###############################################################
# SRTP Mode. 0 - Disabled, 1 - Enabled but not forced, 2 - Enabled and forced, 3 - Optional. Default is 0
# Number: 0, 1, 2, 3
# Mandatory
P443 = 0

# SRTP Key Length. 0 - AES 128&256 bit, 1 - AES 128 bit, 2 - AES 256 bit. Default is 0
# Default is 0
# Number: 0,1
# Mandatory
P2483 = 0

# Crypto Life Time
# 0 - No, 1 - Yes. Default is 1
# Number: 0, 1
# Mandatory
P2463 = 1

# VQ RTCP-XR
# VQ RTCP-XR Collector Name.
# String
P26193 =

# VQ RTCP-XR Collector Address.
# String
P26194 =

# VQ RTCP-XR Collector Port
# String
P26195 = 5060

# Symmetric RTP. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P460 = 0

# RTP Timeout (s). Default is 30.
# Number: 0, 6 - 600.
# Mandatory
P29168 = 0

###############################################################
# Account 2/Call Settings
###############################################################
###############################################################
# Account 2/Call Settings/Call Features
###############################################################
# Auto Answer. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P425 = 0

# Custom Alert-Info for Auto Answer.
# String
P2456 = 

# Allow Auto Answer by Call-Info/Alert-Info. 0 - No, 1 - Yes. Default is 1
# Number: 0, 1
# Mandatory
P438 = 1

# Allow Barging by Call-Info/Alert-Info. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P26119 = 0

# Send Anonymous (caller ID will be blocked if set to Yes). 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P421 = 0

# Intercept Anonymous Calls. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P446 = 0

# Call History. 0 - Log All Calls, 1 - Log Incoming/Outgoing only (missed calls NOT recorded), 2 - Disable Call Log. Default is 0
# Number: 0, 1, 2
# Mandatory
P442 = 0

# Transfer on Conference Hangup. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P2404 = 0

# Key as Send. 0 - Disabled, 1 - Pound (#), 2 - Star (*). Default is 1
# Number: 0, 1, 2
# Mandatory
P492 = 1

# Record Key Default Function. 0 - Record On, 1 - Record Off
P29166 = 0

# Call Recording On
# String
P26128 = 

# Call Recording Off
# String
P26129 = 

# Enable Recovery on Blind Transfer. 0 - Yes, 1 - No. Default is 0
# Number: 0, 1
# Mandatory
P2484 = 0

# Blind Transfer Wait Timeout. Default is 30
# Number: 30 - 300
# Mandatory
P26170 = 30

# No Key Entry Timeout (in seconds). Default is 4
# Number: 1 - 15
# Mandatory
P491 = 4

# Ring Timeout (in seconds). Default is 60
# Number: 30 - 3600
# Mandatory
P476 = 60

# Refer-To Use Target Contact. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P469 = 0

# RFC2543 Hold. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P26162= 0

# Disable Call Waiting. 0 - Default, 1 - No, 2 - Yes. Default is 0
# Number: 0, 1, 2
# Mandatory
P26163 = 0

###############################################################
# Account 2/Call Settings/Dial Plan
###############################################################
# Dial Plan Prefix
# String 
P419 =

# Bypass Dial Plan
# String: contact,incoming,outgoing,dialing,mpk,api
P2482 = mpk

# Dial Plan. Default is { x+ | \+x+ | *x+ | *xx*x+ }
# String
# Mandatory
P459= { x+ | \+x+ | *x+ | *xx*x+ }

###############################################################
# Account 2/Call Settings/Call Display
###############################################################
# Caller ID Display. 0 - Auto, 1 - Disabled, 2 - From Header. Default is 2
# Number: 0, 1, 2
# Mandatory
P2424 = 2

# Callee ID Display. 0 - Auto, 1 - Disabled, 2 - To Header. Default is 0
# Number: 0, 1, 2
# Mandatory
P26125 = 0

###############################################################
# Account 2/Call Settings/Ringtone
###############################################################
# Account Ring Tone. 
# 0 - system, 1 - ring1, 2 - ring2, 3 - ring3, 4 - ring4, 5 - ring5, 6 - ring6, 7 - Doorbell, 8 - silent. Default is 0
# Number: 0-8, more if using custom ringtone
# Mandatory
P423 = 0

# Matching Incoming Caller ID. Matching Rule 1
# String
P1494 = 

# Matching Rule 1 Distinctive Ringtone
# 0 - system, 1 - ring1, 2 - ring2, 3 - ring3, 4 - ring4, 5 - ring5, 6 - ring6, 7 - Doorbell, 8 - silent. Default is 0
# Number: 0-8, more if using custom ringtone
# Mandatory
P1495 = 0

# Matching Incoming Caller ID. Matching Rule 2
# String
P1496 = 

# Matching Rule 2 Distinctive Ringtone
# 0 - system, 1 - ring1, 2 - ring2, 3 - ring3, 4 - ring4, 5 - ring5, 6 - ring6, 7 - Doorbell, 8 - silent. Default is 0
# Number: 0-8, more if using custom ringtone
# Mandatory
P1497 = 0

# Matching Incoming Caller ID. Matching Rule 3
# String
P1498 =

# Matching Rule 3 Distinctive Ringtone
# 0 - system, 1 - ring1, 2 - ring2, 3 - ring3, 4 - ring4, 5 - ring5, 6 - ring6, 7 - Doorbell, 8 - silent. Default is 0
# Number: 0-8, more if using custom ringtone
# Mandatory
P1499 = 0

# Matching Incoming Caller ID. Matching Rule 4
# String
P6722 = 

# Matching Rule 4 Distinctive Ringtone
# 0 - system, 1 - ring1, 2 - ring2, 3 - ring3, 4 - ring4, 5 - ring5, 6 - ring6, 7 - Doorbell, 8 - silent. Default is 0
# Number: 0-8, more if using custom ringtone
# Mandatory
P6723 = 0

# Matching Incoming Caller ID. Matching Rule 5
# String
P6724 = 

# Matching Rule 5 Distinctive Ringtone
# 0 - system, 1 - ring1, 2 - ring2, 3 - ring3, 4 - ring4, 5 - ring5, 6 - ring6, 7 - Doorbell, 8 - silent. Default is 0
# Number: 0-8, more if using custom ringtone
# Mandatory
P6725 = 0

# Matching Incoming Caller ID. Matching Rule 6
# String
P6726 = 

# Matching Rule 6 Distinctive Ringtone
# 0 - system, 1 - ring1, 2 - ring2, 3 - ring3, 4 - ring4, 5 - ring5, 6 - ring6, 7 - Doorbell, 8 - silent. Default is 0
# Number: 0-8, more if using custom ringtone
# Mandatory
P6727 = 0

# Matching Incoming Caller ID. Matching Rule 7
# String
P26164 = 

# Matching Rule 7 Distinctive Ringtone
# 0 - system, 1 - ring1, 2 - ring2, 3 - ring3, 4 - ring4, 5 - ring5, 6 - ring6, 7 - Doorbell, 8 - silent. Default is 0
# Number: 0-8, more if using custom ringtone
# Mandatory
P26165 = 0

# Matching Incoming Caller ID. Matching Rule 8
# String
P26166 = 

# Matching Rule 8 Distinctive Ringtone
# 0 - system, 1 - ring1, 2 - ring2, 3 - ring3, 4 - ring4, 5 - ring5, 6 - ring6, 7 - Doorbell, 8 - silent. Default is 0
# Number: 0-8, more if using custom ringtone
# Mandatory
P26167 = 0

# Matching Incoming Caller ID. Matching Rule 9
# String
P26168 = 

# Matching Rule 9 Distinctive Ringtone
# 0 - system, 1 - ring1, 2 - ring2, 3 - ring3, 4 - ring4, 5 - ring5, 6 - ring6, 7 - Doorbell, 8 - silent. Default is 0
# Number: 0-8, more if using custom ringtone
# Mandatory
P26169 = 0

# Matching Incoming Caller ID. Matching Rule 10
# String
P26196 = 

# Matching Rule 10 Distinctive Ringtone
# 0 - system, 1 - ring1, 2 - ring2, 3 - ring3, 4 - ring4, 5 - ring5, 6 - ring6, 7 - Doorbell, 8 - silent. Default is 0
# Number: 0-8, more if using custom ringtone
# Mandatory
P26197 = 0

###############################################################
# Account 2/Advanced Settings
###############################################################
###############################################################
# Account 2/Advanced Settings/Security Settings
###############################################################
# Check Domain Certificates. When set to Yes/Enabled, domain certificate will be checked as defined in RFC5922
# 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P2411 = 0

# Validate Certification Chain. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P2467 = 0

# Validate Incoming Messages. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P2406 = 0

# Omit charset=UTF-8 in MESSAGE. 0 - Disabled, 1 - Enabled. Default is 0
# Number: 0, 1
# Mandatory
P2455 = 0

# Allow Unsolicited REFER. 0 - Disabled, 1 - Enabled, 2 - Enabled/Force Auth. Default is 0
# Number: 0, 1, 2
# Mandatory
P26123 = 0

# Accept Incoming SIP from Proxy Only. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P2447 = 0

# Check SIP User ID for Incoming INVITE. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P449 = 0

# Allow SIP Reset
# 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P26115 = 0

# Authenticate Incoming INVITE. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P2446 = 0

###############################################################
# Account 2/Advanced Settings/MOH
###############################################################
# On Hold Reminder Tone. 0 - Disabled, 1 - Enable. Default is 1
# Number: 0, 1
# Mandatory
P26106 = 1

# Music On Hold URI
# String
P2450 =

###############################################################
# Account 2/Advanced Settings/Advanced Features
###############################################################
# Special Feature. 100 - Standard, 101 - Nortel MCS, 102- Broadsoft, 108 - CBCOM, 
# 109 - RNK, 110 - Sylantro, 117 - Huawei IMS, 119 - Phonepower, 120 - UCM Call Center
# Default is 100
# Number: 100, 101, 102, 108, 109, 110, 117, 119, 120
# Mandatory
P424 = 100

# Feature Key Synchronization. 0 - Disabled, 1 - Enabled. Default is 0.
# Number: 0, 1
# Mandatory
P2425 = 0

# Conference URI
# String
P2418 =

# Broadsoft
# Broadsoft Call Center. 0 - Disabled, 1 - Enabled. Default is 0
# Number: 0, 1
# Mandatory
P2441 = 0

# Hoteling Event. 0 - Disabled, 1 - Enabled. Default is 0
# Number: 0, 1
# Mandatory
P2442 = 0

# Call Center Status. 0 - Disabled, 1 - Enabled. Default is 0
# Number: 0, 1
# Mandatory
P2443 = 0

# Broadsoft Executive Assistant. 0 - Disabled, 1 - Enabled. Default is 0
# Number: 0, 1
# Mandatory
P2464 = 0

# Broadsoft Call Park. 0 - Disabled, 1 - Enabled. Default is 0
# Number: 0, 1
# Mandatory
P2488 = 0

###############################################################
# Account 2/Advanced Settings/BLF(Busy Lamp Field)  2604 only
###############################################################
# Presence Eventlist URI
# String
P26184 =

# Eventlist BLF URI
# String
P444 = 

# Auto Provision Eventlists. 0 - Disabled, 1 - BLF Eventlist, 2 - Presence Eventlist. Default is 0
# Number:0,1,2
# Mandatory
P2489 = 0

# BLF Call-pickup. 0 - Auto, 1 - Force BLF Call-pickup by prefix, 2 - Disabled. Default is 0
# Number: 0, 1, 2
# Mandatory
P6753 = 0

# BLF Call-pickup Prefix. Default is **
# String
# Mandatory
P481 = **

# Call Pickup Barge-In Code
# String
P26146 = 

# PUBLISH for Presence. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P488 = 0

###############################################################
# Account 2/SCA
###############################################################
# Enable SCA (Shared Call Appearance)
# Number: -1, 32. -1 - Disabled, 32 - Enabled
# Mandatory
P1365 = 0

# Line-Seize Timeout (in seconds). Default is 15
# Number: 15 - 60
# Mandatory
P2413 = 15

###############################################################
# Account 2/Feature Codes
###############################################################
#Enable Local Call Features.  0 - No, 1 - Yes. Default is 1
#Number: 0, 1 
#Mandatory
P420 = 1

#Do Not Disturb (DND) - On
# String
P2444 = 

#Do Not Disturb (DND) - Off
# String
P2445 =

# Call Forward Always - On
# String
P26113 = 

# Call Forward Always - Off
# String
P26114 = 

# Call Forward Always - Target
# String
P29192 = 

#Call Forward Busy - On
# String
P26109 = 

#Call Forward Busy - Off
# String
P26110 = 

#Call Forward Busy - Target
# String
P29193 = 

#Call Forward No Answer - On
#String
P26111 = 

#Call Forward No Answer - Off
#String
P26112 = 

#Call Forward No Answer - Target
#String
P29194 = 

# Call Forward No Answer Timeout (s). Default is 12
# Number: 1 - 120
# Mandatory
P470 = 12

####################################################################
# Account 3(GRP2602/2603/2604 only)                               ##
####################################################################
###############################################################
# Account 3/General Settings
###############################################################
###############################################################
# Account 3/General Settings/Account Register
###############################################################
# Account Active. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P501 = 0

# Account Name
# String
P517 =

# SIP Server
# String
P502 =

# Secondary SIP Server
# String
P2512 =

# SIP User ID
# String
P504 =

# SIP Authentication ID
# String
P505 =

# SIP Authentication Password
# String
P506 =

# Name
# String
P507 =

# TEL URI. 0 - Disabled, 1 - User=Phone, 2 - Enabled. Default is 0
# Number: 0, 1, 2
# Mandatory
P509 = 0

# Voicemail Access Number
# String
P526 =

# BLF Server
# String
P2575 = 

# Account Display
# Number: 0, 1. 0 - User Name, 1 - User ID. Default is 0
# Mandatory
P2580 = 0

###############################################################
# Account 3/General Settings/Network Settings
###############################################################
# Outbound Proxy
# String
P503 =

# Backup Outbound Proxy
# String
P2533 = 

# DNS Mode. 0 - A Record, 1 - SRV, 2 - NAPTR/SRV, 3 - Use Configured IP. Default is 0
# Number: 0, 1, 2, 3
# Mandatory
P508 = 0

# DNS SRV Failover Mode. 0 - Default, 1 - Saved one until DNS TTL, 2 - Saved one until no response. Default is 0
# Number: 0,1,2
# Mandatory
P26240 = 0

# Primary IP. Maximum 15 characters
# String
P2508 =

# Backup IP 1
# String
P2509 =

# Backup IP 2
# String
P2510 =

# NAT Traversal. 0 - No, 1 - STUN, 2 - keep alive, 3 - UPnP, 4 - Auto, 5 - VPN. Default is 4.
# Number: 0, 1, 2, 3, 4, 5
# Mandatory
P514 = 4

# Proxy-Require (A SIP extension to enable firewall penetration). Max length is 64 characters
# String
P518 =

# Use SBC. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P26290 = 0

###############################################################
# Account 3/SIP Settings
###############################################################
###############################################################
# Account 3/SIP Settings/Basic Settings
###############################################################
# SIP Registration. 0 - No, 1 - Yes. Default is 1
# Number: 0, 1
# Mandatory
P510 = 1

# Unregister On Reboot. 0 - No, 1 - Yes, 2 - Instance. Default is 0
# Number: 0, 1, 2
# Mandatory
P511 = 0

# Register Expiration (in minutes). Default is 60. Max about 45 days
# Number: 1 - 64800
# Mandatory
P512 = 60

# Subscribe Expiration (in minutes). Default is 60. Max about 45 days
# Number: 1 - 64800
# Mandatory
P26251 = 60

# Reregister Before Expiration (in seconds). Default is 0 seconds
# Number: 0 - 64800
# Mandatory
P2530 = 0

# SIP Registration Failure Retry Wait Time (in seconds). Default is 20
# Number: 1 - 3600
# Mandatory
P571 = 20

# Add Auth Header On Initial REGISTER. Default is 0
# Number: 0, 1
# Mandatory
P2559 = 0

# Enable OPTIONS Keep Alive. 0 - No, 1 - Yes. Default is 0
# Number: 0,1
# Mandatory
P2597 = 0

# OPTIONS Keep Alive Interval. Default is 30
# Number
# Mandatory
P2598 = 30

# OPTIONS Keep Alive Max Lost. Default is 3
# Number
# Mandatory
P2599 = 3

# SUBSCRIBE for MWI. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P515 = 0

# SUBSCRIBE for Registration. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P2519 = 0

# Use Privacy Header
# 0 - Default, 1 - No, 2 - Yes. Default is 0
# Number: 0, 1, 2
# Mandatory
P2538 = 0

# Use P-Preferred-Identity Header
# 0 - Default, 1 - No, 2 - Yes. Default is 0
# Number: 0, 1, 2
# Mandatory
P2539 = 0

# Use X-Grandstream-PBX Header
# 0 - No, 1 - Yes. Default is 1
# Number: 0, 1
# Mandatory
P26254 = 1

# Use P-Access-Network-Info Header
# 0 - No, 1 - Yes. Default is 1
# Number: 0, 1
# Mandatory
P26258 = 1

# Use P-Emergency-Info Header
# 0 - No, 1 - Yes. Default is 1
# Number: 0, 1
# Mandatory
P26259 = 1

# Use MAC Header
# 0 - No, 1 - Only for REGISTER, 2 - Yes to all SIP. Default is 0
# Number: 0, 1, 2
# Mandatory
P29290 = 0

# Add MAC in User-Agent
# 0 - No, 1 - Yes except REGISTER, 2 - Yes to all SIP. Default is 0
# Number: 0, 1, 2
# Mandatory
P26261 = 0

# SIP Transport. 0 - UDP, 1 - TCP, 2 - TLS/TCP. Default is 0
# Number: 0, 1, 2
# Mandatory
P548 = 0

# SIP Listening Mode. 
# 0 - Transport Only, 1 - Dual, 2 - Dual (BLF Enforced), 3 - Dual (Secured). Default is 0
# Number: 0,1,2,3
# Mandatory
P26224 = 0

# Local SIP Port. Default is 5064
# Number
# Mandatory
P513 = 5064

# SIP URI Scheme when using TLS. 0 - sip, 1 - sips. Default is 1
# Number: 0, 1
# Mandatory
P2529 = 1

# Use Actual Ephemeral Port in Contact with TCP/TLS. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P2531 = 0

# Support SIP Instance ID. 0 - No, 1 - Yes. Default is 1
# Number: 0, 1
# Mandatory
P589 = 1

# SIP T1 Timeout. RFC 3261 T1 value (RTT estimate)
# 50 - 0.5 sec, 100 - 1 sec, 200 - 2 sec. Default is 50
# Number: 50, 100, 200
# Mandatory	
P540 = 50

# SIP T2 Timeout. RFC 3261 T2 value. The maximum retransmit interval for non-INVITE requests and INVITE responses
# 200 - 2 sec, 400 - 4 sec, 800 - 8 sec. Default is 400
# Number: 200, 400, 800
# Mandatory
P541 = 400

# Outbound Proxy Mode. 0 - in route, 1 - not in route, 2 - always send to
# Number: 0, 1, 2
# Mandatory
P2505 = 0

# Enable 100rel. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P535 = 0

###############################################################
# Account 3/SIP Settings/Session Timer
###############################################################
# Enable Session Timer. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P2595 = 0

# Session Expiration (in seconds). Default is 180
# Number: 90 - 64800
# Mandatory
P534 = 180

# Minimum SE (in seconds). Default is 90. This value must be lower than or equal to P260
# Number: 90 - 64800
# Mandatory
P527 = 90

# Caller Request Timer (Request for timer when calling). 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P528 = 0

# Callee Request Timer (Request for timer when called. i.e. if remote party supports timer but did not request for one)
# 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P529 = 0

# Force Timer (Still use timer when remote party does not support timer). 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P530 = 0

# UAC Specify Refresher. 0 - Omit, 1 - UAC, 2 - UAS. Default is 1
# Number: 0 - 2
# Mandatory
P532 = 1

# UAS Specify Refresher. 1 - UAC, 2 - UAS. Default is 1
# Number: 1, 2
# Mandatory
P533 = 1

# Force INVITE (Always refresh with INVITE instead of UPDATE even when remote party supports UPDATE).
# 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P531 = 0

###############################################################
# Account 3/Codec Settings
###############################################################
###############################################################
# Account 3/Codec Settings/Audio
###############################################################
# Preferred Vocoder
# 0 - PCMU, 2 - G.726-32, 4 - G.723.1, 8 - PCMA, 9 - G.722, 18 - G.729A/B, 98 - iLBC, 123 - OPUS
# choice 1. Default is 0
# Number: 0, 2, 4, 8, 9, 18, 98, 123
# Mandatory
P551 = 0

# choice 2. Default is 8
# Number: 0, 2, 4, 8, 9, 18, 98, 123
# Mandatory
P552 = 8

# choice 3. Default is 4
# Number: 0, 2, 4, 8, 9, 18, 98, 123
# Mandatory
P553 = 4

# choice 4. Default is 18
# Number: 0, 2, 4, 8, 9, 18, 98, 123
# Mandatory
P554 = 18

# choice 5. Default is 9
# Number: 0, 2, 4, 8, 9, 18, 98, 123
# Mandatory
P555 = 9

# choice 6. Default is 98
# Number: 0, 2, 4, 8, 9, 18, 98, 123
# Mandatory
P556 = 98

# choice 7. Default is 2
# Number: 0, 2, 4, 8, 9, 18, 98, 123
# Mandatory
P557 = 2

# choice 8. Default is 123
# Number: 0, 2, 4, 8, 9, 18, 98, 123
# Mandatory
P558 = 123

# Codec Negotiation Priority. 0 - Caller, 1 - Callee. Default is 1
# Number: 0, 1
# Mandatory
P29261 = 1

# Use First Matching Vocoder in 200OK SDP. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P2548 = 0

# iLBC Frame Size. 0 - 20ms, 1 - 30ms. Default is 1
# Number: 0, 1
# Mandatory
P595 = 1

# iLBC Payload Type. Default is 97
# Number: 96 - 127
# Mandatory
P594 = 97

# G.726-32 Packing Mode. 0 - ITU, 1 - IETF. Default is 0
# Number: 0, 1
# Mandatory
P2523 = 0

# G.726-32 Dynamic Payload Type. Default is 127
# Number: 96 - 127
# Mandatory
P2565 = 127

# OPUS Payload Type. Default is 123
# Number: 96 - 127
# Mandatory
P2585 = 123

# Send DTMF: In-audio. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P2501 = 0

# Send DTMF: Via RTP (RFC2833). 0 - No, 1 - Yes. Default is 1
# Number: 0, 1
# Mandatory
P2502 = 1

# Send DTMF: Via SIP INFO. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P2503 = 0

# DTMF Payload Type. Default is 101
# Number: 96 - 127
# Mandatory
P596 = 101

# Enable Audio RED with FEC. Default is 1.
# Number: 0, 1
# Mandatory
P26273 = 1

# Audio FEC Payload Type. Default is 121.
# Number: 96-126
# Mandatory
P26274 = 121

# Audio RED Payload Type. Default is 124.
# Number: 96-126
# Mandatory
P26275 = 124

# Silence Suppression. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P585 = 0

# Jitter Buffer Type. 0 - Fixed, 1 - Adaptive. Default is 1
# Number: 0, 1
# Mandatory
P598 = 1

# Jitter Buffer Length. 0 - 100ms, 1 - 200ms, 2 - 300ms, 3 - 400ms, 4 - 500ms, 5 - 600ms, 6 - 700ms, 7 - 800ms
# Default is 2
# Number: 0, 1, 2, 3, 4, 5, 6, 7
# Mandatory
P597 = 2

# Voice Frames per TX (up to 10/20/32/64 frames for G711/G726/G723/other codecs respectively). Default is 2
# Number: 1 - 6
# Mandatory
P586 = 2

# G723 Rate. 0 - 6.3kbps encoding rate, 1 - 5.3kbps encoding rate. Default is 1
# Number: 0, 1
# Mandatory
P593 = 1

###############################################################
# Account 3/Codec Settings/RTP Settings
###############################################################
# SRTP Mode. 0 - Disabled, 1 - Enabled but not forced, 2 - Enabled and forced, 3 - Optional. Default is 0
# Number: 0, 1, 2, 3
# Mandatory
P543 = 0

# SRTP Key Length. 0 - AES 128&256 bit, 1 - AES 128 bit, 2 - AES 256 bit. Default is 0
# Default is 0
# Number: 0,1
# Mandatory
P2583 = 0

# Crypto Life Time
# 0 - No, 1 - Yes. Default is 1
# Number: 0, 1
# Mandatory
P2563 = 1

# VQ RTCP-XR
# VQ RTCP-XR Collector Name.
# String
P26293 =

# VQ RTCP-XR Collector Address.
# String
P26294 =

# VQ RTCP-XR Collector Port
# String
P26295 = 5060

# Symmetric RTP. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P560 = 0

# RTP Timeout (s). Default is 30.
# Number: 0, 6 - 600.
# Mandatory
P29268 = 0

###############################################################
# Account 3/Call Settings
###############################################################
###############################################################
# Account 3/Call Settings/Call Features
###############################################################
# Auto Answer. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P525 = 0

# Custom Alert-Info for Auto Answer.
# String
P2556 = 

# Allow Auto Answer by Call-Info/Alert-Info. 0 - No, 1 - Yes. Default is 1
# Number: 0, 1
# Mandatory
P538 = 1

# Allow Barging by Call-Info/Alert-Info. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P26219 = 0

# Send Anonymous (caller ID will be blocked if set to Yes). 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P521 = 0

# Intercept Anonymous Calls. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P546 = 0

# Call History. 0 - Log All Calls, 1 - Log Incoming/Outgoing only (missed calls NOT recorded), 2 - Disable Call Log. Default is 0
# Number: 0, 1, 2
# Mandatory
P542 = 0

# Transfer on Conference Hangup. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P2504 = 0

# Key as Send. 0 - Disabled, 1 - Pound (#), 2 - Star (*). Default is 1
# Number: 0, 1, 2
# Mandatory
P592 = 1

# Record Key Default Function. 0 - Record On, 1 - Record Off
P29266 = 0

# Call Recording On
# String
P26228 = 

# Call Recording Off
# String
P26229 = 

# Enable Recovery on Blind Transfer. 0 - Yes, 1 - No. Default is 0
# Number: 0, 1
# Mandatory
P2584 = 0

# Blind Transfer Wait Timeout. Default is 30
# Number: 30 - 300
# Mandatory
P26270 = 30

# No Key Entry Timeout (in seconds). Default is 4
# Number: 1 - 15
# Mandatory
P591 = 4

# Ring Timeout (in seconds). Default is 60
# Number: 30 - 3600
# Mandatory
P576 = 60

# Refer-To Use Target Contact. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P569 = 0

# RFC2543 Hold. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P26262= 0

# Disable Call Waiting. 0 - Default, 1 - No, 2 - Yes. Default is 0
# Number: 0, 1, 2
# Mandatory
P26263 = 0

###############################################################
# Account 3/Call Settings/Dial Plan
###############################################################
# Dial Plan Prefix
# String 
P519 =

# Bypass Dial Plan
# String: contact,incoming,outgoing,dialing,mpk,api
P2582 = mpk

# Dial Plan. Default is { x+ | \+x+ | *x+ | *xx*x+ }
# String
# Mandatory
P559= { x+ | \+x+ | *x+ | *xx*x+ }

###############################################################
# Account 3/Call Settings/Call Display
###############################################################
# Caller ID Display. 0 - Auto, 1 - Disabled, 2 - From Header. Default is 2
# Number: 0, 1, 2
# Mandatory
P2524 = 2

# Callee ID Display. 0 - Auto, 1 - Disabled, 2 - To Header. Default is 0
# Number: 0, 1, 2
# Mandatory
P26225 = 0

###############################################################
# Account 3/Call Settings/Ringtone
###############################################################
# Account Ring Tone. 
# 0 - system, 1 - ring1, 2 - ring2, 3 - ring3, 4 - ring4, 5 - ring5, 6 - ring6, 7 - Doorbell, 8 - silent. Default is 0
# Number: 0-8, more if using custom ringtone
# Mandatory
P523 = 0

# Matching Incoming Caller ID. Matching Rule 1
# String
P1500 = 

# Matching Rule 1 Distinctive Ringtone
# 0 - system, 1 - ring1, 2 - ring2, 3 - ring3, 4 - ring4, 5 - ring5, 6 - ring6, 7 - Doorbell, 8 - silent. Default is 0
# Number: 0-8, more if using custom ringtone
# Mandatory
P1501 = 0

# Matching Incoming Caller ID. Matching Rule 2
# String
P1502 = 

# Matching Rule 2 Distinctive Ringtone
# 0 - system, 1 - ring1, 2 - ring2, 3 - ring3, 4 - ring4, 5 - ring5, 6 - ring6, 7 - Doorbell, 8 - silent. Default is 0
# Number: 0-8, more if using custom ringtone
# Mandatory
P1503 = 0

# Matching Incoming Caller ID. Matching Rule 3
# String
P1504 =

# Matching Rule 3 Distinctive Ringtone
# 0 - system, 1 - ring1, 2 - ring2, 3 - ring3, 4 - ring4, 5 - ring5, 6 - ring6, 7 - Doorbell, 8 - silent. Default is 0
# Number: 0-8, more if using custom ringtone
# Mandatory
P1505 = 0

# Matching Incoming Caller ID. Matching Rule 4
# String
P6728 = 

# Matching Rule 4 Distinctive Ringtone
# 0 - system, 1 - ring1, 2 - ring2, 3 - ring3, 4 - ring4, 5 - ring5, 6 - ring6, 7 - Doorbell, 8 - silent. Default is 0
# Number: 0-8, more if using custom ringtone
# Mandatory
P6729 = 0

# Matching Incoming Caller ID. Matching Rule 5
# String
P6730 = 

# Matching Rule 5 Distinctive Ringtone
# 0 - system, 1 - ring1, 2 - ring2, 3 - ring3, 4 - ring4, 5 - ring5, 6 - ring6, 7 - Doorbell, 8 - silent. Default is 0
# Number: 0-8, more if using custom ringtone
# Mandatory
P6731 = 0

# Matching Incoming Caller ID. Matching Rule 6
# String
P6732 = 

# Matching Rule 6 Distinctive Ringtone
# 0 - system, 1 - ring1, 2 - ring2, 3 - ring3, 4 - ring4, 5 - ring5, 6 - ring6, 7 - Doorbell, 8 - silent. Default is 0
# Number: 0-8, more if using custom ringtone
# Mandatory
P6733 = 0

# Matching Incoming Caller ID. Matching Rule 7
# String
P26264 = 

# Matching Rule 7 Distinctive Ringtone
# 0 - system, 1 - ring1, 2 - ring2, 3 - ring3, 4 - ring4, 5 - ring5, 6 - ring6, 7 - Doorbell, 8 - silent. Default is 0
# Number: 0-8, more if using custom ringtone
# Mandatory
P26265 = 0

# Matching Incoming Caller ID. Matching Rule 8
# String
P26266 = 

# Matching Rule 8 Distinctive Ringtone
# 0 - system, 1 - ring1, 2 - ring2, 3 - ring3, 4 - ring4, 5 - ring5, 6 - ring6, 7 - Doorbell, 8 - silent. Default is 0
# Number: 0-8, more if using custom ringtone
# Mandatory
P26267 = 0

# Matching Incoming Caller ID. Matching Rule 9
# String
P26268 = 

# Matching Rule 9 Distinctive Ringtone
# 0 - system, 1 - ring1, 2 - ring2, 3 - ring3, 4 - ring4, 5 - ring5, 6 - ring6, 7 - Doorbell, 8 - silent. Default is 0
# Number: 0-8, more if using custom ringtone
# Mandatory
P26269 = 0

# Matching Incoming Caller ID. Matching Rule 10
# String
P26296 = 

# Matching Rule 10 Distinctive Ringtone
# 0 - system, 1 - ring1, 2 - ring2, 3 - ring3, 4 - ring4, 5 - ring5, 6 - ring6, 7 - Doorbell, 8 - silent. Default is 0
# Number: 0-8, more if using custom ringtone
# Mandatory
P26297 = 0

###############################################################
# Account 3/Advanced Settings
###############################################################
###############################################################
# Account 3/Advanced Settings/Security Settings
###############################################################
# Check Domain Certificates. When set to Yes/Enabled, domain certificate will be checked as defined in RFC5922
# 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P2511 = 0

# Validate Certification Chain. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P2567 = 0

# Validate Incoming Messages. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P2506 = 0

# Omit charset=UTF-8 in MESSAGE. 0 - Disabled, 1 - Enabled. Default is 0
# Number: 0, 1
# Mandatory
P2555 = 0

# Allow Unsolicited REFER. 0 - Disabled, 1 - Enabled, 2 - Enabled/Force Auth. Default is 0
# Number: 0, 1, 2
# Mandatory
P26223 = 0

# Accept Incoming SIP from Proxy Only. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P2547 = 0

# Check SIP User ID for Incoming INVITE. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P549 = 0

# Allow SIP Reset
# 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P26215 = 0

# Authenticate Incoming INVITE. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P2546 = 0

###############################################################
# Account 3/Advanced Settings/MOH
###############################################################
# On Hold Reminder Tone. 0 - Disabled, 1 - Enable. Default is 1
# Number: 0, 1
# Mandatory
P26206 = 1

# Music On Hold URI
# String
P2550 =

###############################################################
# Account 3/Advanced Settings/Advanced Features
###############################################################
# Special Feature. 100 - Standard, 101 - Nortel MCS, 102- Broadsoft, 108 - CBCOM, 
# 109 - RNK, 110 - Sylantro, 117 - Huawei IMS, 119 - Phonepower, 120 - UCM Call Center
# Default is 100
# Number: 100, 101, 102, 108, 109, 110, 117, 119, 120
# Mandatory
P524 = 100

# Feature Key Synchronization. 0 - Disabled, 1 - Enabled. Default is 0.
# Number: 0, 1
# Mandatory
P2525 = 0

# Conference URI
# String
P2518 =

# Broadsoft
# Broadsoft Call Center. 0 - Disabled, 1 - Enabled. Default is 0
# Number: 0, 1
# Mandatory
P2541 = 0

# Hoteling Event. 0 - Disabled, 1 - Enabled. Default is 0
# Number: 0, 1
# Mandatory
P2542 = 0

# Call Center Status. 0 - Disabled, 1 - Enabled. Default is 0
# Number: 0, 1
# Mandatory
P2543 = 0

# Broadsoft Executive Assistant. 0 - Disabled, 1 - Enabled. Default is 0
# Number: 0, 1
# Mandatory
P2564 = 0

# Broadsoft Call Park. 0 - Disabled, 1 - Enabled. Default is 0
# Number: 0, 1
# Mandatory
P2588 = 0

###############################################################
# Account 3/Advanced Settings/BLF(Busy Lamp Field)  2604 only
###############################################################
# Presence Eventlist URI
# String
P26284 =

# Eventlist BLF URI
# String
P544 = 

# Auto Provision Eventlists. 0 - Disabled, 1 - BLF Eventlist, 2 - Presence Eventlist. Default is 0
# Number:0,1,2
# Mandatory
P2589 = 0

# BLF Call-pickup. 0 - Auto, 1 - Force BLF Call-pickup by prefix, 2 - Disabled. Default is 0
# Number: 0, 1, 2
# Mandatory
P6754 = 0

# BLF Call-pickup Prefix. Default is **
# String
# Mandatory
P581 = **

# Call Pickup Barge-In Code
# String
P26246 = 

# PUBLISH for Presence. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P588 = 0

###############################################################
# Account 3/SCA
###############################################################
# Enable SCA (Shared Call Appearance)
# Number: -1, 32. -1 - Disabled, 32 - Enabled
# Mandatory
P1367 = 0

# Line-Seize Timeout (in seconds). Default is 15
# Number: 15 - 60
# Mandatory
P2513 = 15

###############################################################
# Account 3/Feature Codes
###############################################################
#Enable Local Call Features.  0 - No, 1 - Yes. Default is 1
#Number: 0, 1 
#Mandatory
P520 = 1

#Do Not Disturb (DND) - On
# String
P2544 = 

#Do Not Disturb (DND) - Off
# String
P2545 =

# Call Forward Always - On
# String
P26213 = 

# Call Forward Always - Off
# String
P26214 = 

# Call Forward Always - Target
# String
P29292 = 

#Call Forward Busy - On
# String
P26209 = 

#Call Forward Busy - Off
# String
P26210 = 

#Call Forward Busy - Target
# String
P29293 = 

#Call Forward No Answer - On
#String
P26211 = 

#Call Forward No Answer - Off
#String
P26212 = 

#Call Forward No Answer - Target
#String
P29294 = 

# Call Forward No Answer Timeout (s). Default is 12
# Number: 1 - 120
# Mandatory
P570 = 12

####################################################################
# Account 4(GRP2602/2603/2604 only)                               ##
####################################################################
###############################################################
# Account 4/General Settings
###############################################################
###############################################################
# Account 4/General Settings/Account Register
###############################################################
# Account Active. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P601 = 0

# Account Name
# String
P617 =

# SIP Server
# String
P602 =

# Secondary SIP Server
# String
P2612 =

# SIP User ID
# String
P604 =

# SIP Authentication ID
# String
P605 =

# SIP Authentication Password
# String
P606 =

# Name
# String
P607 =

# TEL URI. 0 - Disabled, 1 - User=Phone, 2 - Enabled. Default is 0
# Number: 0, 1, 2
# Mandatory
P609 = 0

# Voicemail Access Number
# String
P626 =

# BLF Server
# String
P2675 = 

# Account Display
# Number: 0, 1. 0 - User Name, 1 - User ID. Default is 0
# Mandatory
P2680 = 0

###############################################################
# Account 4/General Settings/Network Settings
###############################################################
# Outbound Proxy
# String
P603 =

# Backup Outbound Proxy
# String
P2633 = 

# DNS Mode. 0 - A Record, 1 - SRV, 2 - NAPTR/SRV, 3 - Use Configured IP. Default is 0
# Number: 0, 1, 2, 3
# Mandatory
P608 = 0

# DNS SRV Failover Mode. 0 - Default, 1 - Saved one until DNS TTL, 2 - Saved one until no response. Default is 0
# Number: 0,1,2
# Mandatory
P26340 = 0

# Primary IP. Maximum 15 characters
# String
P2608 =

# Backup IP 1
# String
P2609 =

# Backup IP 2
# String
P2610 =

# NAT Traversal. 0 - No, 1 - STUN, 2 - keep alive, 3 - UPnP, 4 - Auto, 5 - VPN. Default is 4.
# Number: 0, 1, 2, 3, 4, 5
# Mandatory
P614 = 4

# Proxy-Require (A SIP extension to enable firewall penetration). Max length is 64 characters
# String
P618 =

# Use SBC. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P26390 = 0

###############################################################
# Account 4/SIP Settings
###############################################################
###############################################################
# Account 4/SIP Settings/Basic Settings
###############################################################
# SIP Registration. 0 - No, 1 - Yes. Default is 1
# Number: 0, 1
# Mandatory
P610 = 1

# Unregister On Reboot. 0 - No, 1 - Yes, 2 - Instance. Default is 0
# Number: 0, 1, 2
# Mandatory
P611 = 0

# Register Expiration (in minutes). Default is 60. Max about 45 days
# Number: 1 - 64800
# Mandatory
P612 = 60

# Subscribe Expiration (in minutes). Default is 60. Max about 45 days
# Number: 1 - 64800
# Mandatory
P26351 = 60

# Reregister Before Expiration (in seconds). Default is 0 seconds
# Number: 0 - 64800
# Mandatory
P2630 = 0

# SIP Registration Failure Retry Wait Time (in seconds). Default is 20
# Number: 1 - 3600
# Mandatory
P671 = 20

# Add Auth Header On Initial REGISTER. Default is 0
# Number: 0, 1
# Mandatory
P2659 = 0

# Enable OPTIONS Keep Alive. 0 - No, 1 - Yes. Default is 0
# Number: 0,1
# Mandatory
P2697 = 0

# OPTIONS Keep Alive Interval. Default is 30
# Number
# Mandatory
P2698 = 30

# OPTIONS Keep Alive Max Lost. Default is 3
# Number
# Mandatory
P2699 = 3

# SUBSCRIBE for MWI. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P615 = 0

# SUBSCRIBE for Registration. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P2619 = 0

# Use Privacy Header
# 0 - Default, 1 - No, 2 - Yes. Default is 0
# Number: 0, 1, 2
# Mandatory
P2638 = 0

# Use P-Preferred-Identity Header
# 0 - Default, 1 - No, 2 - Yes. Default is 0
# Number: 0, 1, 2
# Mandatory
P2639 = 0

# Use X-Grandstream-PBX Header
# 0 - No, 1 - Yes. Default is 1
# Number: 0, 1
# Mandatory
P26354 = 1

# Use P-Access-Network-Info Header
# 0 - No, 1 - Yes. Default is 1
# Number: 0, 1
# Mandatory
P26358 = 1

# Use P-Emergency-Info Header
# 0 - No, 1 - Yes. Default is 1
# Number: 0, 1
# Mandatory
P26359 = 1

# Use MAC Header
# 0 - No, 1 - Only for REGISTER, 2 - Yes to all SIP. Default is 0
# Number: 0, 1, 2
# Mandatory
P29390 = 0

# Add MAC in User-Agent
# 0 - No, 1 - Yes except REGISTER, 2 - Yes to all SIP. Default is 0
# Number: 0, 1, 2
# Mandatory
P26361 = 0

# SIP Transport. 0 - UDP, 1 - TCP, 2 - TLS/TCP. Default is 0
# Number: 0, 1, 2
# Mandatory
P648 = 0

# SIP Listening Mode. 
# 0 - Transport Only, 1 - Dual, 2 - Dual (BLF Enforced), 3 - Dual (Secured). Default is 0
# Number: 0,1,2,3
# Mandatory
P26324 = 0

# Local SIP Port. Default is 5066
# Number
# Mandatory
P613 = 5066

# SIP URI Scheme when using TLS. 0 - sip, 1 - sips. Default is 1
# Number: 0, 1
# Mandatory
P2629 = 1

# Use Actual Ephemeral Port in Contact with TCP/TLS. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P2631 = 0

# Support SIP Instance ID. 0 - No, 1 - Yes. Default is 1
# Number: 0, 1
# Mandatory
P689 = 1

# SIP T1 Timeout. RFC 3261 T1 value (RTT estimate)
# 50 - 0.5 sec, 100 - 1 sec, 200 - 2 sec. Default is 50
# Number: 50, 100, 200
# Mandatory	
P640 = 50

# SIP T2 Timeout. RFC 3261 T2 value. The maximum retransmit interval for non-INVITE requests and INVITE responses
# 200 - 2 sec, 400 - 4 sec, 800 - 8 sec. Default is 400
# Number: 200, 400, 800
# Mandatory
P641 = 400

# Outbound Proxy Mode. 0 - in route, 1 - not in route, 2 - always send to
# Number: 0, 1, 2
# Mandatory
P2605 = 0

# Enable 100rel. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P635 = 0

###############################################################
# Account 4/SIP Settings/Session Timer
###############################################################
# Enable Session Timer. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P2695 = 0

# Session Expiration (in seconds). Default is 180
# Number: 90 - 64800
# Mandatory
P634 = 180

# Minimum SE (in seconds). Default is 90. This value must be lower than or equal to P260
# Number: 90 - 64800
# Mandatory
P627 = 90

# Caller Request Timer (Request for timer when calling). 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P628 = 0

# Callee Request Timer (Request for timer when called. i.e. if remote party supports timer but did not request for one)
# 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P629 = 0

# Force Timer (Still use timer when remote party does not support timer). 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P630 = 0

# UAC Specify Refresher. 0 - Omit, 1 - UAC, 2 - UAS. Default is 1
# Number: 0 - 2
# Mandatory
P632 = 1

# UAS Specify Refresher. 1 - UAC, 2 - UAS. Default is 1
# Number: 1, 2
# Mandatory
P633 = 1

# Force INVITE (Always refresh with INVITE instead of UPDATE even when remote party supports UPDATE).
# 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P631 = 0

###############################################################
# Account 4/Codec Settings
###############################################################
###############################################################
# Account 4/Codec Settings/Audio
###############################################################
# Preferred Vocoder
# 0 - PCMU, 2 - G.726-32, 4 - G.723.1, 8 - PCMA, 9 - G.722, 18 - G.729A/B, 98 - iLBC, 123 - OPUS
# choice 1. Default is 0
# Number: 0, 2, 4, 8, 9, 18, 98, 123
# Mandatory
P651 = 0

# choice 2. Default is 8
# Number: 0, 2, 4, 8, 9, 18, 98, 123
# Mandatory
P652 = 8

# choice 3. Default is 4
# Number: 0, 2, 4, 8, 9, 18, 98, 123
# Mandatory
P653 = 4

# choice 4. Default is 18
# Number: 0, 2, 4, 8, 9, 18, 98, 123
# Mandatory
P654 = 18

# choice 5. Default is 9
# Number: 0, 2, 4, 8, 9, 18, 98, 123
# Mandatory
P655 = 9

# choice 6. Default is 98
# Number: 0, 2, 4, 8, 9, 18, 98, 123
# Mandatory
P656 = 98

# choice 7. Default is 2
# Number: 0, 2, 4, 8, 9, 18, 98, 123
# Mandatory
P657 = 2

# choice 8. Default is 123
# Number: 0, 2, 4, 8, 9, 18, 98, 123
# Mandatory
P658 = 123

# Codec Negotiation Priority. 0 - Caller, 1 - Callee. Default is 1
# Number: 0, 1
# Mandatory
P29361 = 1

# Use First Matching Vocoder in 200OK SDP. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P2648 = 0

# iLBC Frame Size. 0 - 20ms, 1 - 30ms. Default is 1
# Number: 0, 1
# Mandatory
P695 = 1

# iLBC Payload Type. Default is 97
# Number: 96 - 127
# Mandatory
P694 = 97

# G.726-32 Packing Mode. 0 - ITU, 1 - IETF. Default is 0
# Number: 0, 1
# Mandatory
P2623 = 0

# G.726-32 Dynamic Payload Type. Default is 127
# Number: 96 - 127
# Mandatory
P2665 = 127

# OPUS Payload Type. Default is 123
# Number: 96 - 127
# Mandatory
P2685 = 123

# Send DTMF: In-audio. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P2601 = 0

# Send DTMF: Via RTP (RFC2833). 0 - No, 1 - Yes. Default is 1
# Number: 0, 1
# Mandatory
P2602 = 1

# Send DTMF: Via SIP INFO. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P2603 = 0

# DTMF Payload Type. Default is 101
# Number: 96 - 127
# Mandatory
P696 = 101

# Enable Audio RED with FEC. Default is 1.
# Number: 0, 1
# Mandatory
P26373 = 1

# Audio FEC Payload Type. Default is 121.
# Number: 96-126
# Mandatory
P26374 = 121

# Audio RED Payload Type. Default is 124.
# Number: 96-126
# Mandatory
P26375 = 124

# Silence Suppression. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P685 = 0

# Jitter Buffer Type. 0 - Fixed, 1 - Adaptive. Default is 1
# Number: 0, 1
# Mandatory
P698 = 1

# Jitter Buffer Length. 0 - 100ms, 1 - 200ms, 2 - 300ms, 3 - 400ms, 4 - 500ms, 5 - 600ms, 6 - 700ms, 7 - 800ms
# Default is 2
# Number: 0, 1, 2, 3, 4, 5, 6, 7
# Mandatory
P697 = 2

# Voice Frames per TX (up to 10/20/32/64 frames for G711/G726/G723/other codecs respectively). Default is 2
# Number: 1 - 6
# Mandatory
P686 = 2

# G723 Rate. 0 - 6.3kbps encoding rate, 1 - 5.3kbps encoding rate. Default is 1
# Number: 0, 1
# Mandatory
P693 = 1

###############################################################
# Account 4/Codec Settings/RTP Settings
###############################################################
# SRTP Mode. 0 - Disabled, 1 - Enabled but not forced, 2 - Enabled and forced, 3 - Optional. Default is 0
# Number: 0, 1, 2, 3
# Mandatory
P643 = 0

# SRTP Key Length. 0 - AES 128&256 bit, 1 - AES 128 bit, 2 - AES 256 bit. Default is 0
# Default is 0
# Number: 0,1
# Mandatory
P2683 = 0

# Crypto Life Time
# 0 - No, 1 - Yes. Default is 1
# Number: 0, 1
# Mandatory
P2663 = 1

# VQ RTCP-XR
# VQ RTCP-XR Collector Name.
# String
P26393 =

# VQ RTCP-XR Collector Address.
# String
P26394 =

# VQ RTCP-XR Collector Port
# String
P26395 = 5060

# Symmetric RTP. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P660 = 0

# RTP Timeout (s). Default is 30.
# Number: 0, 6 - 600.
# Mandatory
P29368 = 0

###############################################################
# Account 4/Call Settings
###############################################################
###############################################################
# Account 4/Call Settings/Call Features
###############################################################
# Auto Answer. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P625 = 0

# Custom Alert-Info for Auto Answer.
# String
P2656 = 

# Allow Auto Answer by Call-Info/Alert-Info. 0 - No, 1 - Yes. Default is 1
# Number: 0, 1
# Mandatory
P638 = 1

# Allow Barging by Call-Info/Alert-Info. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P26319 = 0

# Send Anonymous (caller ID will be blocked if set to Yes). 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P621 = 0

# Intercept Anonymous Calls. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P646 = 0

# Call History. 0 - Log All Calls, 1 - Log Incoming/Outgoing only (missed calls NOT recorded), 2 - Disable Call Log. Default is 0
# Number: 0, 1, 2
# Mandatory
P642 = 0

# Transfer on Conference Hangup. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P2604 = 0

# Key as Send. 0 - Disabled, 1 - Pound (#), 2 - Star (*). Default is 1
# Number: 0, 1, 2
# Mandatory
P692 = 1

# Record Key Default Function. 0 - Record On, 1 - Record Off
P29366 = 0

# Call Recording On
# String
P26328 = 

# Call Recording Off
# String
P26329 = 

# Enable Recovery on Blind Transfer. 0 - Yes, 1 - No. Default is 0
# Number: 0, 1
# Mandatory
P2684 = 0

# Blind Transfer Wait Timeout. Default is 30
# Number: 30 - 300
# Mandatory
P26370 = 30

# No Key Entry Timeout (in seconds). Default is 4
# Number: 1 - 15
# Mandatory
P691 = 4

# Ring Timeout (in seconds). Default is 60
# Number: 30 - 3600
# Mandatory
P676 = 60

# Refer-To Use Target Contact. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P669 = 0

# RFC2543 Hold. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P26362= 0

# Disable Call Waiting. 0 - Default, 1 - No, 2 - Yes. Default is 0
# Number: 0, 1, 2
# Mandatory
P26363 = 0

###############################################################
# Account 4/Call Settings/Dial Plan
###############################################################
# Dial Plan Prefix
# String 
P619 =

# Bypass Dial Plan
# String: contact,incoming,outgoing,dialing,mpk,api
P2682 = mpk

# Dial Plan. Default is { x+ | \+x+ | *x+ | *xx*x+ }
# String
# Mandatory
P659= { x+ | \+x+ | *x+ | *xx*x+ }

###############################################################
# Account 4/Call Settings/Call Display
###############################################################
# Caller ID Display. 0 - Auto, 1 - Disabled, 2 - From Header. Default is 2
# Number: 0, 1, 2
# Mandatory
P2624 = 2

# Callee ID Display. 0 - Auto, 1 - Disabled, 2 - To Header. Default is 0
# Number: 0, 1, 2
# Mandatory
P26325 = 0

###############################################################
# Account 4/Call Settings/Ringtone
###############################################################
# Account Ring Tone. 
# 0 - system, 1 - ring1, 2 - ring2, 3 - ring3, 4 - ring4, 5 - ring5, 6 - ring6, 7 - Doorbell, 8 - silent. Default is 0
# Number: 0-8, more if using custom ringtone
# Mandatory
P623 = 0

# Matching Incoming Caller ID. Matching Rule 1
# String
P1506 = 

# Matching Rule 1 Distinctive Ringtone
# 0 - system, 1 - ring1, 2 - ring2, 3 - ring3, 4 - ring4, 5 - ring5, 6 - ring6, 7 - Doorbell, 8 - silent. Default is 0
# Number: 0-8, more if using custom ringtone
# Mandatory
P1507 = 0

# Matching Incoming Caller ID. Matching Rule 2
# String
P1508 = 

# Matching Rule 2 Distinctive Ringtone
# 0 - system, 1 - ring1, 2 - ring2, 3 - ring3, 4 - ring4, 5 - ring5, 6 - ring6, 7 - Doorbell, 8 - silent. Default is 0
# Number: 0-8, more if using custom ringtone
# Mandatory
P1509 = 0

# Matching Incoming Caller ID. Matching Rule 3
# String
P1510 =

# Matching Rule 3 Distinctive Ringtone
# 0 - system, 1 - ring1, 2 - ring2, 3 - ring3, 4 - ring4, 5 - ring5, 6 - ring6, 7 - Doorbell, 8 - silent. Default is 0
# Number: 0-8, more if using custom ringtone
# Mandatory
P1511 = 0

# Matching Incoming Caller ID. Matching Rule 4
# String
P6734 = 

# Matching Rule 4 Distinctive Ringtone
# 0 - system, 1 - ring1, 2 - ring2, 3 - ring3, 4 - ring4, 5 - ring5, 6 - ring6, 7 - Doorbell, 8 - silent. Default is 0
# Number: 0-8, more if using custom ringtone
# Mandatory
P6735 = 0

# Matching Incoming Caller ID. Matching Rule 5
# String
P6736 = 

# Matching Rule 5 Distinctive Ringtone
# 0 - system, 1 - ring1, 2 - ring2, 3 - ring3, 4 - ring4, 5 - ring5, 6 - ring6, 7 - Doorbell, 8 - silent. Default is 0
# Number: 0-8, more if using custom ringtone
# Mandatory
P6737 = 0

# Matching Incoming Caller ID. Matching Rule 6
# String
P6738 = 

# Matching Rule 6 Distinctive Ringtone
# 0 - system, 1 - ring1, 2 - ring2, 3 - ring3, 4 - ring4, 5 - ring5, 6 - ring6, 7 - Doorbell, 8 - silent. Default is 0
# Number: 0-8, more if using custom ringtone
# Mandatory
P6739 = 0

# Matching Incoming Caller ID. Matching Rule 7
# String
P26364 = 

# Matching Rule 7 Distinctive Ringtone
# 0 - system, 1 - ring1, 2 - ring2, 3 - ring3, 4 - ring4, 5 - ring5, 6 - ring6, 7 - Doorbell, 8 - silent. Default is 0
# Number: 0-8, more if using custom ringtone
# Mandatory
P26365 = 0

# Matching Incoming Caller ID. Matching Rule 8
# String
P26366 = 

# Matching Rule 8 Distinctive Ringtone
# 0 - system, 1 - ring1, 2 - ring2, 3 - ring3, 4 - ring4, 5 - ring5, 6 - ring6, 7 - Doorbell, 8 - silent. Default is 0
# Number: 0-8, more if using custom ringtone
# Mandatory
P26367 = 0

# Matching Incoming Caller ID. Matching Rule 9
# String
P26368 = 

# Matching Rule 9 Distinctive Ringtone
# 0 - system, 1 - ring1, 2 - ring2, 3 - ring3, 4 - ring4, 5 - ring5, 6 - ring6, 7 - Doorbell, 8 - silent. Default is 0
# Number: 0-8, more if using custom ringtone
# Mandatory
P26369 = 0

# Matching Incoming Caller ID. Matching Rule 10
# String
P26396 = 

# Matching Rule 10 Distinctive Ringtone
# 0 - system, 1 - ring1, 2 - ring2, 3 - ring3, 4 - ring4, 5 - ring5, 6 - ring6, 7 - Doorbell, 8 - silent. Default is 0
# Number: 0-8, more if using custom ringtone
# Mandatory
P26397 = 0

###############################################################
# Account 4/Advanced Settings
###############################################################
###############################################################
# Account 4/Advanced Settings/Security Settings
###############################################################
# Check Domain Certificates. When set to Yes/Enabled, domain certificate will be checked as defined in RFC5922
# 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P2611 = 0

# Validate Certification Chain. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P2667 = 0

# Validate Incoming Messages. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P2606 = 0

# Omit charset=UTF-8 in MESSAGE. 0 - Disabled, 1 - Enabled. Default is 0
# Number: 0, 1
# Mandatory
P2655 = 0

# Allow Unsolicited REFER. 0 - Disabled, 1 - Enabled, 2 - Enabled/Force Auth. Default is 0
# Number: 0, 1, 2
# Mandatory
P26323 = 0

# Accept Incoming SIP from Proxy Only. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P2647 = 0

# Check SIP User ID for Incoming INVITE. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P649 = 0

# Allow SIP Reset
# 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P26315 = 0

# Authenticate Incoming INVITE. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P2646 = 0

###############################################################
# Account 4/Advanced Settings/MOH
###############################################################
# On Hold Reminder Tone. 0 - Disabled, 1 - Enable. Default is 1
# Number: 0, 1
# Mandatory
P26306 = 1

# Music On Hold URI
# String
P2650 =

###############################################################
# Account 4/Advanced Settings/Advanced Features
###############################################################
# Special Feature. 100 - Standard, 101 - Nortel MCS, 102- Broadsoft, 108 - CBCOM, 
# 109 - RNK, 110 - Sylantro, 117 - Huawei IMS, 119 - Phonepower, 120 - UCM Call Center
# Default is 100
# Number: 100, 101, 102, 108, 109, 110, 117, 119, 120
# Mandatory
P624 = 100

# Feature Key Synchronization. 0 - Disabled, 1 - Enabled. Default is 0.
# Number: 0, 1
# Mandatory
P2625 = 0

# Conference URI
# String
P2618 =

# Broadsoft
# Broadsoft Call Center. 0 - Disabled, 1 - Enabled. Default is 0
# Number: 0, 1
# Mandatory
P2641 = 0

# Hoteling Event. 0 - Disabled, 1 - Enabled. Default is 0
# Number: 0, 1
# Mandatory
P2642 = 0

# Call Center Status. 0 - Disabled, 1 - Enabled. Default is 0
# Number: 0, 1
# Mandatory
P2643 = 0

# Broadsoft Executive Assistant. 0 - Disabled, 1 - Enabled. Default is 0
# Number: 0, 1
# Mandatory
P2664 = 0

# Broadsoft Call Park. 0 - Disabled, 1 - Enabled. Default is 0
# Number: 0, 1
# Mandatory
P2688 = 0

###############################################################
# Account 4/Advanced Settings/BLF(Busy Lamp Field)  2604 only
###############################################################
# Presence Eventlist URI
# String
P26384 =

# Eventlist BLF URI
# String
P644 = 

# Auto Provision Eventlists. 0 - Disabled, 1 - BLF Eventlist, 2 - Presence Eventlist. Default is 0
# Number:0,1,2
# Mandatory
P2689 = 0

# BLF Call-pickup. 0 - Auto, 1 - Force BLF Call-pickup by prefix, 2 - Disabled. Default is 0
# Number: 0, 1, 2
# Mandatory
P6755 = 0

# BLF Call-pickup Prefix. Default is **
# String
# Mandatory
P681 = **

# Call Pickup Barge-In Code
# String
P26346 = 

# PUBLISH for Presence. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P688 = 0

###############################################################
# Account 4/SCA
###############################################################
# Enable SCA (Shared Call Appearance)
# Number: -1, 32. -1 - Disabled, 32 - Enabled
# Mandatory
P1369 = 0

# Line-Seize Timeout (in seconds). Default is 15
# Number: 15 - 60
# Mandatory
P2613 = 15

###############################################################
# Account 4/Feature Codes
###############################################################
#Enable Local Call Features.  0 - No, 1 - Yes. Default is 1
#Number: 0, 1 
#Mandatory
P620 = 1

#Do Not Disturb (DND) - On
# String
P2644 = 

#Do Not Disturb (DND) - Off
# String
P2645 =

# Call Forward Always - On
# String
P26313 = 

# Call Forward Always - Off
# String
P26314 = 

# Call Forward Always - Target
# String
P29392 = 

#Call Forward Busy - On
# String
P26309 = 

#Call Forward Busy - Off
# String
P26310 = 

#Call Forward Busy - Target
# String
P29393 = 

#Call Forward No Answer - On
#String
P26311 = 

#Call Forward No Answer - Off
#String
P26312 = 

#Call Forward No Answer - Target
#String
P29394 = 

# Call Forward No Answer Timeout (s). Default is 12
# Number: 1 - 120
# Mandatory
P670 = 12

####################################################################
# Account 5(GRP2603/2604 only)                                    ##
####################################################################
###############################################################
# Account 5/General Settings
###############################################################
###############################################################
# Account 5/General Settings/Account Register
###############################################################
# Account Active. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P701 = 0

# Account Name
# String
P717 =

# SIP Server
# String
P702 =

# Secondary SIP Server
# String
P2712 =

# SIP User ID
# String
P704 =

# SIP Authentication ID
# String
P705 =

# SIP Authentication Password
# String
P706 =

# Name
# String
P707 =

# TEL URI. 0 - Disabled, 1 - User=Phone, 2 - Enabled. Default is 0
# Number: 0, 1, 2
# Mandatory
P709 = 0

# Voicemail Access Number
# String
P726 =

# BLF Server
# String
P2775 = 

# Account Display
# Number: 0, 1. 0 - User Name, 1 - User ID. Default is 0
# Mandatory
P2780 = 0

###############################################################
# Account 5/General Settings/Network Settings
###############################################################
# Outbound Proxy
# String
P703 =

# Backup Outbound Proxy
# String
P2733 = 

# DNS Mode. 0 - A Record, 1 - SRV, 2 - NAPTR/SRV, 3 - Use Configured IP. Default is 0
# Number: 0, 1, 2, 3
# Mandatory
P708 = 0

# DNS SRV Failover Mode. 0 - Default, 1 - Saved one until DNS TTL, 2 - Saved one until no response. Default is 0
# Number: 0,1,2
# Mandatory
P26440 = 0

# Primary IP. Maximum 15 characters
# String
P2708 =

# Backup IP 1
# String
P2709 =

# Backup IP 2
# String
P2710 =

# NAT Traversal. 0 - No, 1 - STUN, 2 - keep alive, 3 - UPnP, 4 - Auto, 5 - VPN. Default is 4.
# Number: 0, 1, 2, 3, 4, 5
# Mandatory
P714 = 4

# Proxy-Require (A SIP extension to enable firewall penetration). Max length is 64 characters
# String
P718 =

# Use SBC. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P26490 = 0

###############################################################
# Account 5/SIP Settings
###############################################################
###############################################################
# Account 5/SIP Settings/Basic Settings
###############################################################
# SIP Registration. 0 - No, 1 - Yes. Default is 1
# Number: 0, 1
# Mandatory
P710 = 1

# Unregister On Reboot. 0 - No, 1 - Yes, 2 - Instance. Default is 0
# Number: 0, 1, 2
# Mandatory
P711 = 0

# Register Expiration (in minutes). Default is 60. Max about 45 days
# Number: 1 - 64800
# Mandatory
P712 = 60

# Subscribe Expiration (in minutes). Default is 60. Max about 45 days
# Number: 1 - 64800
# Mandatory
P26451 = 60

# Reregister Before Expiration (in seconds). Default is 0 seconds
# Number: 0 - 64800
# Mandatory
P2730 = 0

# SIP Registration Failure Retry Wait Time (in seconds). Default is 20
# Number: 1 - 3600
# Mandatory
P771 = 20

# Add Auth Header On Initial REGISTER. Default is 0
# Number: 0, 1
# Mandatory
P2759 = 0

# Enable OPTIONS Keep Alive. 0 - No, 1 - Yes. Default is 0
# Number: 0,1
# Mandatory
P2797 = 0

# OPTIONS Keep Alive Interval. Default is 30
# Number
# Mandatory
P2798 = 30

# OPTIONS Keep Alive Max Lost. Default is 3
# Number
# Mandatory
P2799 = 3

# SUBSCRIBE for MWI. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P715 = 0

# SUBSCRIBE for Registration. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P2719 = 0

# Use Privacy Header
# 0 - Default, 1 - No, 2 - Yes. Default is 0
# Number: 0, 1, 2
# Mandatory
P2738 = 0

# Use P-Preferred-Identity Header
# 0 - Default, 1 - No, 2 - Yes. Default is 0
# Number: 0, 1, 2
# Mandatory
P2739 = 0

# Use X-Grandstream-PBX Header
# 0 - No, 1 - Yes. Default is 1
# Number: 0, 1
# Mandatory
P26454 = 1

# Use P-Access-Network-Info Header
# 0 - No, 1 - Yes. Default is 1
# Number: 0, 1
# Mandatory
P26458 = 1

# Use P-Emergency-Info Header
# 0 - No, 1 - Yes. Default is 1
# Number: 0, 1
# Mandatory
P26459 = 1

# Use MAC Header
# 0 - No, 1 - Only for REGISTER, 2 - Yes to all SIP. Default is 0
# Number: 0, 1, 2
# Mandatory
P29490 = 0

# Add MAC in User-Agent
# 0 - No, 1 - Yes except REGISTER, 2 - Yes to all SIP. Default is 0
# Number: 0, 1, 2
# Mandatory
P26461 = 0

# SIP Transport. 0 - UDP, 1 - TCP, 2 - TLS/TCP. Default is 0
# Number: 0, 1, 2
# Mandatory
P748 = 0

# SIP Listening Mode. 
# 0 - Transport Only, 1 - Dual, 2 - Dual (BLF Enforced), 3 - Dual (Secured). Default is 0
# Number: 0,1,2,3
# Mandatory
P26424 = 0

# Local SIP Port. Default is 5068
# Number
# Mandatory
P713 = 5068

# SIP URI Scheme when using TLS. 0 - sip, 1 - sips. Default is 1
# Number: 0, 1
# Mandatory
P2729 = 1

# Use Actual Ephemeral Port in Contact with TCP/TLS. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P2731 = 0

# Support SIP Instance ID. 0 - No, 1 - Yes. Default is 1
# Number: 0, 1
# Mandatory
P789 = 1

# SIP T1 Timeout. RFC 3261 T1 value (RTT estimate)
# 50 - 0.5 sec, 100 - 1 sec, 200 - 2 sec. Default is 50
# Number: 50, 100, 200
# Mandatory	
P740 = 50

# SIP T2 Timeout. RFC 3261 T2 value. The maximum retransmit interval for non-INVITE requests and INVITE responses
# 200 - 2 sec, 400 - 4 sec, 800 - 8 sec. Default is 400
# Number: 200, 400, 800
# Mandatory
P741 = 400

# Outbound Proxy Mode. 0 - in route, 1 - not in route, 2 - always send to
# Number: 0, 1, 2
# Mandatory
P2705 = 0

# Enable 100rel. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P735 = 0

###############################################################
# Account 5/SIP Settings/Session Timer
###############################################################
# Enable Session Timer. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P2795 = 0

# Session Expiration (in seconds). Default is 180
# Number: 90 - 64800
# Mandatory
P734 = 180

# Minimum SE (in seconds). Default is 90. This value must be lower than or equal to P260
# Number: 90 - 64800
# Mandatory
P727 = 90

# Caller Request Timer (Request for timer when calling). 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P728 = 0

# Callee Request Timer (Request for timer when called. i.e. if remote party supports timer but did not request for one)
# 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P729 = 0

# Force Timer (Still use timer when remote party does not support timer). 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P730 = 0

# UAC Specify Refresher. 0 - Omit, 1 - UAC, 2 - UAS. Default is 1
# Number: 0 - 2
# Mandatory
P732 = 1

# UAS Specify Refresher. 1 - UAC, 2 - UAS. Default is 1
# Number: 1, 2
# Mandatory
P733 = 1

# Force INVITE (Always refresh with INVITE instead of UPDATE even when remote party supports UPDATE).
# 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P731 = 0

###############################################################
# Account 5/Codec Settings
###############################################################
###############################################################
# Account 5/Codec Settings/Audio
###############################################################
# Preferred Vocoder
# 0 - PCMU, 2 - G.726-32, 4 - G.723.1, 8 - PCMA, 9 - G.722, 18 - G.729A/B, 98 - iLBC, 123 - OPUS
# choice 1. Default is 0
# Number: 0, 2, 4, 8, 9, 18, 98, 123
# Mandatory
P751 = 0

# choice 2. Default is 8
# Number: 0, 2, 4, 8, 9, 18, 98, 123
# Mandatory
P752 = 8

# choice 3. Default is 4
# Number: 0, 2, 4, 8, 9, 18, 98, 123
# Mandatory
P753 = 4

# choice 4. Default is 18
# Number: 0, 2, 4, 8, 9, 18, 98, 123
# Mandatory
P754 = 18

# choice 5. Default is 9
# Number: 0, 2, 4, 8, 9, 18, 98, 123
# Mandatory
P755 = 9

# choice 6. Default is 98
# Number: 0, 2, 4, 8, 9, 18, 98, 123
# Mandatory
P756 = 98

# choice 7. Default is 2
# Number: 0, 2, 4, 8, 9, 18, 98, 123
# Mandatory
P757 = 2

# choice 8. Default is 123
# Number: 0, 2, 4, 8, 9, 18, 98, 123
# Mandatory
P758 = 123

# Codec Negotiation Priority. 0 - Caller, 1 - Callee. Default is 1
# Number: 0, 1
# Mandatory
P29461 = 1

# Use First Matching Vocoder in 200OK SDP. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P2748 = 0

# iLBC Frame Size. 0 - 20ms, 1 - 30ms. Default is 1
# Number: 0, 1
# Mandatory
P795 = 1

# iLBC Payload Type. Default is 97
# Number: 96 - 127
# Mandatory
P794 = 97

# G.726-32 Packing Mode. 0 - ITU, 1 - IETF. Default is 0
# Number: 0, 1
# Mandatory
P2723 = 0

# G.726-32 Dynamic Payload Type. Default is 127
# Number: 96 - 127
# Mandatory
P2765 = 127

# OPUS Payload Type. Default is 123
# Number: 96 - 127
# Mandatory
P2785 = 123

# Send DTMF: In-audio. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P2701 = 0

# Send DTMF: Via RTP (RFC2833). 0 - No, 1 - Yes. Default is 1
# Number: 0, 1
# Mandatory
P2702 = 1

# Send DTMF: Via SIP INFO. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P2703 = 0

# DTMF Payload Type. Default is 101
# Number: 96 - 127
# Mandatory
P796 = 101

# Enable Audio RED with FEC. Default is 1.
# Number: 0, 1
# Mandatory
P26473 = 1

# Audio FEC Payload Type. Default is 121.
# Number: 96-126
# Mandatory
P26474 = 121

# Audio RED Payload Type. Default is 124.
# Number: 96-126
# Mandatory
P26475 = 124

# Silence Suppression. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P785 = 0

# Jitter Buffer Type. 0 - Fixed, 1 - Adaptive. Default is 1
# Number: 0, 1
# Mandatory
P798 = 1

# Jitter Buffer Length. 0 - 100ms, 1 - 200ms, 2 - 300ms, 3 - 400ms, 4 - 500ms, 5 - 600ms, 6 - 700ms, 7 - 800ms
# Default is 2
# Number: 0, 1, 2, 3, 4, 5, 6, 7
# Mandatory
P797 = 2

# Voice Frames per TX (up to 10/20/32/64 frames for G711/G726/G723/other codecs respectively). Default is 2
# Number: 1 - 6
# Mandatory
P786 = 2

# G723 Rate. 0 - 6.3kbps encoding rate, 1 - 5.3kbps encoding rate. Default is 1
# Number: 0, 1
# Mandatory
P793 = 1

###############################################################
# Account 5/Codec Settings/RTP Settings
###############################################################
# SRTP Mode. 0 - Disabled, 1 - Enabled but not forced, 2 - Enabled and forced, 3 - Optional. Default is 0
# Number: 0, 1, 2, 3
# Mandatory
P743 = 0

# SRTP Key Length. 0 - AES 128&256 bit, 1 - AES 128 bit, 2 - AES 256 bit. Default is 0
# Default is 0
# Number: 0,1
# Mandatory
P2783 = 0

# Crypto Life Time
# 0 - No, 1 - Yes. Default is 1
# Number: 0, 1
# Mandatory
P2763 = 1

# VQ RTCP-XR
# VQ RTCP-XR Collector Name.
# String
P26493 =

# VQ RTCP-XR Collector Address.
# String
P26494 =

# VQ RTCP-XR Collector Port
# String
P26495 = 5060

# Symmetric RTP. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P760 = 0

# RTP Timeout (s). Default is 30.
# Number: 0, 6 - 600.
# Mandatory
P29468 = 0

###############################################################
# Account 5/Call Settings
###############################################################
###############################################################
# Account 5/Call Settings/Call Features
###############################################################
# Auto Answer. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P725 = 0

# Custom Alert-Info for Auto Answer.
# String
P2756 = 

# Allow Auto Answer by Call-Info/Alert-Info. 0 - No, 1 - Yes. Default is 1
# Number: 0, 1
# Mandatory
P738 = 1

# Allow Barging by Call-Info/Alert-Info. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P26419 = 0

# Send Anonymous (caller ID will be blocked if set to Yes). 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P721 = 0

# Intercept Anonymous Calls. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P746 = 0

# Call History. 0 - Log All Calls, 1 - Log Incoming/Outgoing only (missed calls NOT recorded), 2 - Disable Call Log. Default is 0
# Number: 0, 1, 2
# Mandatory
P742 = 0

# Transfer on Conference Hangup. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P2704 = 0

# Key as Send. 0 - Disabled, 1 - Pound (#), 2 - Star (*). Default is 1
# Number: 0, 1, 2
# Mandatory
P792 = 1

# Record Key Default Function. 0 - Record On, 1 - Record Off
P29466 = 0

# Call Recording On
# String
P26428 = 

# Call Recording Off
# String
P26429 = 

# Enable Recovery on Blind Transfer. 0 - Yes, 1 - No. Default is 0
# Number: 0, 1
# Mandatory
P2784 = 0

# Blind Transfer Wait Timeout. Default is 30
# Number: 30 - 300
# Mandatory
P26470 = 30

# No Key Entry Timeout (in seconds). Default is 4
# Number: 1 - 15
# Mandatory
P791 = 4

# Ring Timeout (in seconds). Default is 60
# Number: 30 - 3600
# Mandatory
P776 = 60

# Refer-To Use Target Contact. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P769 = 0

# RFC2543 Hold. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P26462= 0

# Disable Call Waiting. 0 - Default, 1 - No, 2 - Yes. Default is 0
# Number: 0, 1, 2
# Mandatory
P26463 = 0

###############################################################
# Account 5/Call Settings/Dial Plan
###############################################################
# Dial Plan Prefix
# String 
P719 =

# Bypass Dial Plan
# String: contact,incoming,outgoing,dialing,mpk,api
P2782 = mpk

# Dial Plan. Default is { x+ | \+x+ | *x+ | *xx*x+ }
# String
# Mandatory
P759= { x+ | \+x+ | *x+ | *xx*x+ }

###############################################################
# Account 5/Call Settings/Call Display
###############################################################
# Caller ID Display. 0 - Auto, 1 - Disabled, 2 - From Header. Default is 2
# Number: 0, 1, 2
# Mandatory
P2724 = 2

# Callee ID Display. 0 - Auto, 1 - Disabled, 2 - To Header. Default is 0
# Number: 0, 1, 2
# Mandatory
P26425 = 0

###############################################################
# Account 5/Call Settings/Ringtone
###############################################################
# Account Ring Tone. 
# 0 - system, 1 - ring1, 2 - ring2, 3 - ring3, 4 - ring4, 5 - ring5, 6 - ring6, 7 - Doorbell, 8 - silent. Default is 0
# Number: 0-8, more if using custom ringtone
# Mandatory
P723 = 0

# Matching Incoming Caller ID. Matching Rule 1
# String
P1512 = 

# Matching Rule 1 Distinctive Ringtone
# 0 - system, 1 - ring1, 2 - ring2, 3 - ring3, 4 - ring4, 5 - ring5, 6 - ring6, 7 - Doorbell, 8 - silent. Default is 0
# Number: 0-8, more if using custom ringtone
# Mandatory
P1513 = 0

# Matching Incoming Caller ID. Matching Rule 2
# String
P1514 = 

# Matching Rule 2 Distinctive Ringtone
# 0 - system, 1 - ring1, 2 - ring2, 3 - ring3, 4 - ring4, 5 - ring5, 6 - ring6, 7 - Doorbell, 8 - silent. Default is 0
# Number: 0-8, more if using custom ringtone
# Mandatory
P1515 = 0

# Matching Incoming Caller ID. Matching Rule 3
# String
P1516 =

# Matching Rule 3 Distinctive Ringtone
# 0 - system, 1 - ring1, 2 - ring2, 3 - ring3, 4 - ring4, 5 - ring5, 6 - ring6, 7 - Doorbell, 8 - silent. Default is 0
# Number: 0-8, more if using custom ringtone
# Mandatory
P1517 = 0

# Matching Incoming Caller ID. Matching Rule 4
# String
P6740 = 

# Matching Rule 4 Distinctive Ringtone
# 0 - system, 1 - ring1, 2 - ring2, 3 - ring3, 4 - ring4, 5 - ring5, 6 - ring6, 7 - Doorbell, 8 - silent. Default is 0
# Number: 0-8, more if using custom ringtone
# Mandatory
P6741 = 0

# Matching Incoming Caller ID. Matching Rule 5
# String
P6742 = 

# Matching Rule 5 Distinctive Ringtone
# 0 - system, 1 - ring1, 2 - ring2, 3 - ring3, 4 - ring4, 5 - ring5, 6 - ring6, 7 - Doorbell, 8 - silent. Default is 0
# Number: 0-8, more if using custom ringtone
# Mandatory
P6743 = 0

# Matching Incoming Caller ID. Matching Rule 6
# String
P6744 = 

# Matching Rule 6 Distinctive Ringtone
# 0 - system, 1 - ring1, 2 - ring2, 3 - ring3, 4 - ring4, 5 - ring5, 6 - ring6, 7 - Doorbell, 8 - silent. Default is 0
# Number: 0-8, more if using custom ringtone
# Mandatory
P6745 = 0

# Matching Incoming Caller ID. Matching Rule 7
# String
P26464 = 

# Matching Rule 7 Distinctive Ringtone
# 0 - system, 1 - ring1, 2 - ring2, 3 - ring3, 4 - ring4, 5 - ring5, 6 - ring6, 7 - Doorbell, 8 - silent. Default is 0
# Number: 0-8, more if using custom ringtone
# Mandatory
P26465 = 0

# Matching Incoming Caller ID. Matching Rule 8
# String
P26466 = 

# Matching Rule 8 Distinctive Ringtone
# 0 - system, 1 - ring1, 2 - ring2, 3 - ring3, 4 - ring4, 5 - ring5, 6 - ring6, 7 - Doorbell, 8 - silent. Default is 0
# Number: 0-8, more if using custom ringtone
# Mandatory
P26467 = 0

# Matching Incoming Caller ID. Matching Rule 9
# String
P26468 = 

# Matching Rule 9 Distinctive Ringtone
# 0 - system, 1 - ring1, 2 - ring2, 3 - ring3, 4 - ring4, 5 - ring5, 6 - ring6, 7 - Doorbell, 8 - silent. Default is 0
# Number: 0-8, more if using custom ringtone
# Mandatory
P26469 = 0

# Matching Incoming Caller ID. Matching Rule 10
# String
P26496 = 

# Matching Rule 10 Distinctive Ringtone
# 0 - system, 1 - ring1, 2 - ring2, 3 - ring3, 4 - ring4, 5 - ring5, 6 - ring6, 7 - Doorbell, 8 - silent. Default is 0
# Number: 0-8, more if using custom ringtone
# Mandatory
P26497 = 0

###############################################################
# Account 5/Advanced Settings
###############################################################
###############################################################
# Account 5/Advanced Settings/Security Settings
###############################################################
# Check Domain Certificates. When set to Yes/Enabled, domain certificate will be checked as defined in RFC5922
# 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P2711 = 0

# Validate Certification Chain. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P2767 = 0

# Validate Incoming Messages. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P2706 = 0

# Omit charset=UTF-8 in MESSAGE. 0 - Disabled, 1 - Enabled. Default is 0
# Number: 0, 1
# Mandatory
P2755 = 0

# Allow Unsolicited REFER. 0 - Disabled, 1 - Enabled, 2 - Enabled/Force Auth. Default is 0
# Number: 0, 1, 2
# Mandatory
P26423 = 0

# Accept Incoming SIP from Proxy Only. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P2747 = 0

# Check SIP User ID for Incoming INVITE. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P749 = 0

# Allow SIP Reset
# 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P26415 = 0

# Authenticate Incoming INVITE. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P2746 = 0

###############################################################
# Account 5/Advanced Settings/MOH
###############################################################
# On Hold Reminder Tone. 0 - Disabled, 1 - Enable. Default is 1
# Number: 0, 1
# Mandatory
P26406 = 1

# Music On Hold URI
# String
P2750 =

###############################################################
# Account 5/Advanced Settings/Advanced Features
###############################################################
# Special Feature. 100 - Standard, 101 - Nortel MCS, 102- Broadsoft, 108 - CBCOM, 
# 109 - RNK, 110 - Sylantro, 117 - Huawei IMS, 119 - Phonepower, 120 - UCM Call Center
# Default is 100
# Number: 100, 101, 102, 108, 109, 110, 117, 119, 120
# Mandatory
P724 = 100

# Feature Key Synchronization. 0 - Disabled, 1 - Enabled. Default is 0.
# Number: 0, 1
# Mandatory
P2725 = 0

# Conference URI
# String
P2718 =

# Broadsoft
# Broadsoft Call Center. 0 - Disabled, 1 - Enabled. Default is 0
# Number: 0, 1
# Mandatory
P2741 = 0

# Hoteling Event. 0 - Disabled, 1 - Enabled. Default is 0
# Number: 0, 1
# Mandatory
P2742 = 0

# Call Center Status. 0 - Disabled, 1 - Enabled. Default is 0
# Number: 0, 1
# Mandatory
P2743 = 0

# Broadsoft Executive Assistant. 0 - Disabled, 1 - Enabled. Default is 0
# Number: 0, 1
# Mandatory
P2764 = 0

# Broadsoft Call Park. 0 - Disabled, 1 - Enabled. Default is 0
# Number: 0, 1
# Mandatory
P2788 = 0

###############################################################
# Account 5/Advanced Settings/BLF(Busy Lamp Field)  2604 only
###############################################################
# Presence Eventlist URI
# String
P26484 =

# Eventlist BLF URI
# String
P744 = 

# Auto Provision Eventlists. 0 - Disabled, 1 - BLF Eventlist, 2 - Presence Eventlist. Default is 0
# Number:0,1,2
# Mandatory
P2789 = 0

# BLF Call-pickup. 0 - Auto, 1 - Force BLF Call-pickup by prefix, 2 - Disabled. Default is 0
# Number: 0, 1, 2
# Mandatory
P6756 = 0

# BLF Call-pickup Prefix. Default is **
# String
# Mandatory
P781 = **

# Call Pickup Barge-In Code
# String
P26446 = 

# PUBLISH for Presence. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P788 = 0

###############################################################
# Account 5/SCA
###############################################################
# Enable SCA (Shared Call Appearance)
# Number: -1, 32. -1 - Disabled, 32 - Enabled
# Mandatory
P1371 = 0

# Line-Seize Timeout (in seconds). Default is 15
# Number: 15 - 60
# Mandatory
P2713 = 15

###############################################################
# Account 5/Feature Codes
###############################################################
#Enable Local Call Features.  0 - No, 1 - Yes. Default is 1
#Number: 0, 1 
#Mandatory
P720 = 1

#Do Not Disturb (DND) - On
# String
P2744 = 

#Do Not Disturb (DND) - Off
# String
P2745 =

# Call Forward Always - On
# String
P26413 = 

# Call Forward Always - Off
# String
P26414 = 

# Call Forward Always - Target
# String
P29492 = 

#Call Forward Busy - On
# String
P26409 = 

#Call Forward Busy - Off
# String
P26410 = 

#Call Forward Busy - Target
# String
P29493 = 

#Call Forward No Answer - On
#String
P26411 = 

#Call Forward No Answer - Off
#String
P26412 = 

#Call Forward No Answer - Target
#String
P29494 = 

# Call Forward No Answer Timeout (s). Default is 12
# Number: 1 - 120
# Mandatory
P770 = 12

####################################################################
# Account 6(GRP2603/2604 only)                                    ##
####################################################################
###############################################################
# Account 6/General Settings
###############################################################
###############################################################
# Account 6/General Settings/Account Register
###############################################################
# Account Active. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P801 = 0

# Account Name
# String
P817 =

# SIP Server
# String
P802 =

# Secondary SIP Server
# String
P2812 =

# SIP User ID
# String
P804 =

# SIP Authentication ID
# String
P805 =

# SIP Authentication Password
# String
P806 =

# Name
# String
P807 =

# TEL URI. 0 - Disabled, 1 - User=Phone, 2 - Enabled. Default is 0
# Number: 0, 1, 2
# Mandatory
P809 = 0

# Voicemail Access Number
# String
P826 =

# BLF Server
# String
P2875 = 

# Account Display
# Number: 0, 1. 0 - User Name, 1 - User ID. Default is 0
# Mandatory
P2880 = 0

###############################################################
# Account 6/General Settings/Network Settings
###############################################################
# Outbound Proxy
# String
P803 =

# Backup Outbound Proxy
# String
P2833 = 

# DNS Mode. 0 - A Record, 1 - SRV, 2 - NAPTR/SRV, 3 - Use Configured IP. Default is 0
# Number: 0, 1, 2, 3
# Mandatory
P808 = 0

# DNS SRV Failover Mode. 0 - Default, 1 - Saved one until DNS TTL, 2 - Saved one until no response. Default is 0
# Number: 0,1,2
# Mandatory
P26540 = 0

# Primary IP. Maximum 15 characters
# String
P2808 =

# Backup IP 1
# String
P2809 =

# Backup IP 2
# String
P2810 =

# NAT Traversal. 0 - No, 1 - STUN, 2 - keep alive, 3 - UPnP, 4 - Auto, 5 - VPN. Default is 4.
# Number: 0, 1, 2, 3, 4, 5
# Mandatory
P814 = 4

# Proxy-Require (A SIP extension to enable firewall penetration). Max length is 64 characters
# String
P818 =

# Use SBC. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P26590 = 0

###############################################################
# Account 6/SIP Settings
###############################################################
###############################################################
# Account 6/SIP Settings/Basic Settings
###############################################################
# SIP Registration. 0 - No, 1 - Yes. Default is 1
# Number: 0, 1
# Mandatory
P810 = 1

# Unregister On Reboot. 0 - No, 1 - Yes, 2 - Instance. Default is 0
# Number: 0, 1, 2
# Mandatory
P811 = 0

# Register Expiration (in minutes). Default is 60. Max about 45 days
# Number: 1 - 64800
# Mandatory
P812 = 60

# Subscribe Expiration (in minutes). Default is 60. Max about 45 days
# Number: 1 - 64800
# Mandatory
P26551 = 60

# Reregister Before Expiration (in seconds). Default is 0 seconds
# Number: 0 - 64800
# Mandatory
P2830 = 0

# SIP Registration Failure Retry Wait Time (in seconds). Default is 20
# Number: 1 - 3600
# Mandatory
P871 = 20

# Add Auth Header On Initial REGISTER. Default is 0
# Number: 0, 1
# Mandatory
P2859 = 0

# Enable OPTIONS Keep Alive. 0 - No, 1 - Yes. Default is 0
# Number: 0,1
# Mandatory
P2897 = 0

# OPTIONS Keep Alive Interval. Default is 30
# Number
# Mandatory
P2898 = 30

# OPTIONS Keep Alive Max Lost. Default is 3
# Number
# Mandatory
P2899 = 3

# SUBSCRIBE for MWI. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P815 = 0

# SUBSCRIBE for Registration. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P2819 = 0

# Use Privacy Header
# 0 - Default, 1 - No, 2 - Yes. Default is 0
# Number: 0, 1, 2
# Mandatory
P2838 = 0

# Use P-Preferred-Identity Header
# 0 - Default, 1 - No, 2 - Yes. Default is 0
# Number: 0, 1, 2
# Mandatory
P2839 = 0

# Use X-Grandstream-PBX Header
# 0 - No, 1 - Yes. Default is 1
# Number: 0, 1
# Mandatory
P26554 = 1

# Use P-Access-Network-Info Header
# 0 - No, 1 - Yes. Default is 1
# Number: 0, 1
# Mandatory
P26558 = 1

# Use P-Emergency-Info Header
# 0 - No, 1 - Yes. Default is 1
# Number: 0, 1
# Mandatory
P26559 = 1

# Use MAC Header
# 0 - No, 1 - Only for REGISTER, 2 - Yes to all SIP. Default is 0
# Number: 0, 1, 2
# Mandatory
P29590 = 0

# Add MAC in User-Agent
# 0 - No, 1 - Yes except REGISTER, 2 - Yes to all SIP. Default is 0
# Number: 0, 1, 2
# Mandatory
P26561 = 0

# SIP Transport. 0 - UDP, 1 - TCP, 2 - TLS/TCP. Default is 0
# Number: 0, 1, 2
# Mandatory
P848 = 0

# SIP Listening Mode. 
# 0 - Transport Only, 1 - Dual, 2 - Dual (BLF Enforced), 3 - Dual (Secured). Default is 0
# Number: 0,1,2,3
# Mandatory
P26524 = 0

# Local SIP Port. Default is 5070
# Number
# Mandatory
P813 = 5070

# SIP URI Scheme when using TLS. 0 - sip, 1 - sips. Default is 1
# Number: 0, 1
# Mandatory
P2829 = 1

# Use Actual Ephemeral Port in Contact with TCP/TLS. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P2831 = 0

# Support SIP Instance ID. 0 - No, 1 - Yes. Default is 1
# Number: 0, 1
# Mandatory
P889 = 1

# SIP T1 Timeout. RFC 3261 T1 value (RTT estimate)
# 50 - 0.5 sec, 100 - 1 sec, 200 - 2 sec. Default is 50
# Number: 50, 100, 200
# Mandatory	
P840 = 50

# SIP T2 Timeout. RFC 3261 T2 value. The maximum retransmit interval for non-INVITE requests and INVITE responses
# 200 - 2 sec, 400 - 4 sec, 800 - 8 sec. Default is 400
# Number: 200, 400, 800
# Mandatory
P841 = 400

# Outbound Proxy Mode. 0 - in route, 1 - not in route, 2 - always send to
# Number: 0, 1, 2
# Mandatory
P2805 = 0

# Enable 100rel. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P835 = 0

###############################################################
# Account 6/SIP Settings/Session Timer
###############################################################
# Enable Session Timer. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P2895 = 0

# Session Expiration (in seconds). Default is 180
# Number: 90 - 64800
# Mandatory
P834 = 180

# Minimum SE (in seconds). Default is 90. This value must be lower than or equal to P260
# Number: 90 - 64800
# Mandatory
P827 = 90

# Caller Request Timer (Request for timer when calling). 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P828 = 0

# Callee Request Timer (Request for timer when called. i.e. if remote party supports timer but did not request for one)
# 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P829 = 0

# Force Timer (Still use timer when remote party does not support timer). 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P830 = 0

# UAC Specify Refresher. 0 - Omit, 1 - UAC, 2 - UAS. Default is 1
# Number: 0 - 2
# Mandatory
P832 = 1

# UAS Specify Refresher. 1 - UAC, 2 - UAS. Default is 1
# Number: 1, 2
# Mandatory
P833 = 1

# Force INVITE (Always refresh with INVITE instead of UPDATE even when remote party supports UPDATE).
# 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P831 = 0

###############################################################
# Account 6/Codec Settings
###############################################################
###############################################################
# Account 6/Codec Settings/Audio
###############################################################
# Preferred Vocoder
# 0 - PCMU, 2 - G.726-32, 4 - G.723.1, 8 - PCMA, 9 - G.722, 18 - G.729A/B, 98 - iLBC, 123 - OPUS
# choice 1. Default is 0
# Number: 0, 2, 4, 8, 9, 18, 98, 123
# Mandatory
P851 = 0

# choice 2. Default is 8
# Number: 0, 2, 4, 8, 9, 18, 98, 123
# Mandatory
P852 = 8

# choice 3. Default is 4
# Number: 0, 2, 4, 8, 9, 18, 98, 123
# Mandatory
P853 = 4

# choice 4. Default is 18
# Number: 0, 2, 4, 8, 9, 18, 98, 123
# Mandatory
P854 = 18

# choice 5. Default is 9
# Number: 0, 2, 4, 8, 9, 18, 98, 123
# Mandatory
P855 = 9

# choice 6. Default is 98
# Number: 0, 2, 4, 8, 9, 18, 98, 123
# Mandatory
P856 = 98

# choice 7. Default is 2
# Number: 0, 2, 4, 8, 9, 18, 98, 123
# Mandatory
P857 = 2

# choice 8. Default is 123
# Number: 0, 2, 4, 8, 9, 18, 98, 123
# Mandatory
P858 = 123

# Codec Negotiation Priority. 0 - Caller, 1 - Callee. Default is 1
# Number: 0, 1
# Mandatory
P29561 = 1

# Use First Matching Vocoder in 200OK SDP. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P2848 = 0

# iLBC Frame Size. 0 - 20ms, 1 - 30ms. Default is 1
# Number: 0, 1
# Mandatory
P895 = 1

# iLBC Payload Type. Default is 97
# Number: 96 - 127
# Mandatory
P894 = 97

# G.726-32 Packing Mode. 0 - ITU, 1 - IETF. Default is 0
# Number: 0, 1
# Mandatory
P2823 = 0

# G.726-32 Dynamic Payload Type. Default is 127
# Number: 96 - 127
# Mandatory
P2865 = 127

# OPUS Payload Type. Default is 123
# Number: 96 - 127
# Mandatory
P2885 = 123

# Send DTMF: In-audio. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P2801 = 0

# Send DTMF: Via RTP (RFC2833). 0 - No, 1 - Yes. Default is 1
# Number: 0, 1
# Mandatory
P2802 = 1

# Send DTMF: Via SIP INFO. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P2803 = 0

# DTMF Payload Type. Default is 101
# Number: 96 - 127
# Mandatory
P896 = 101

# Enable Audio RED with FEC. Default is 1.
# Number: 0, 1
# Mandatory
P26573 = 1

# Audio FEC Payload Type. Default is 121.
# Number: 96-126
# Mandatory
P26574 = 121

# Audio RED Payload Type. Default is 124.
# Number: 96-126
# Mandatory
P26575 = 124

# Silence Suppression. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P885 = 0

# Jitter Buffer Type. 0 - Fixed, 1 - Adaptive. Default is 1
# Number: 0, 1
# Mandatory
P898 = 1

# Jitter Buffer Length. 0 - 100ms, 1 - 200ms, 2 - 300ms, 3 - 400ms, 4 - 500ms, 5 - 600ms, 6 - 700ms, 7 - 800ms
# Default is 2
# Number: 0, 1, 2, 3, 4, 5, 6, 7
# Mandatory
P897 = 2

# Voice Frames per TX (up to 10/20/32/64 frames for G711/G726/G723/other codecs respectively). Default is 2
# Number: 1 - 6
# Mandatory
P886 = 2

# G723 Rate. 0 - 6.3kbps encoding rate, 1 - 5.3kbps encoding rate. Default is 1
# Number: 0, 1
# Mandatory
P893 = 1

###############################################################
# Account 6/Codec Settings/RTP Settings
###############################################################
# SRTP Mode. 0 - Disabled, 1 - Enabled but not forced, 2 - Enabled and forced, 3 - Optional. Default is 0
# Number: 0, 1, 2, 3
# Mandatory
P843 = 0

# SRTP Key Length. 0 - AES 128&256 bit, 1 - AES 128 bit, 2 - AES 256 bit. Default is 0
# Default is 0
# Number: 0,1
# Mandatory
P2883 = 0

# Crypto Life Time
# 0 - No, 1 - Yes. Default is 1
# Number: 0, 1
# Mandatory
P2863 = 1

# VQ RTCP-XR
# VQ RTCP-XR Collector Name.
# String
P26593 =

# VQ RTCP-XR Collector Address.
# String
P26594 =

# VQ RTCP-XR Collector Port
# String
P26595 = 5060

# Symmetric RTP. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P860 = 0

# RTP Timeout (s). Default is 30.
# Number: 0, 6 - 600.
# Mandatory
P29568 = 0

###############################################################
# Account 6/Call Settings
###############################################################
###############################################################
# Account 6/Call Settings/Call Features
###############################################################
# Auto Answer. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P825 = 0

# Custom Alert-Info for Auto Answer.
# String
P2856 = 

# Allow Auto Answer by Call-Info/Alert-Info. 0 - No, 1 - Yes. Default is 1
# Number: 0, 1
# Mandatory
P838 = 1

# Allow Barging by Call-Info/Alert-Info. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P26519 = 0

# Send Anonymous (caller ID will be blocked if set to Yes). 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P821 = 0

# Intercept Anonymous Calls. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P846 = 0

# Call History. 0 - Log All Calls, 1 - Log Incoming/Outgoing only (missed calls NOT recorded), 2 - Disable Call Log. Default is 0
# Number: 0, 1, 2
# Mandatory
P842 = 0

# Transfer on Conference Hangup. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P2804 = 0

# Key as Send. 0 - Disabled, 1 - Pound (#), 2 - Star (*). Default is 1
# Number: 0, 1, 2
# Mandatory
P892 = 1

# Record Key Default Function. 0 - Record On, 1 - Record Off
P29566 = 0

# Call Recording On
# String
P26528 = 

# Call Recording Off
# String
P26529 = 

# Enable Recovery on Blind Transfer. 0 - Yes, 1 - No. Default is 0
# Number: 0, 1
# Mandatory
P2884 = 0

# Blind Transfer Wait Timeout. Default is 30
# Number: 30 - 300
# Mandatory
P26570 = 30

# No Key Entry Timeout (in seconds). Default is 4
# Number: 1 - 15
# Mandatory
P891 = 4

# Ring Timeout (in seconds). Default is 60
# Number: 30 - 3600
# Mandatory
P876 = 60

# Refer-To Use Target Contact. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P869 = 0

# RFC2543 Hold. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P26562= 0

# Disable Call Waiting. 0 - Default, 1 - No, 2 - Yes. Default is 0
# Number: 0, 1, 2
# Mandatory
P26563 = 0

###############################################################
# Account 6/Call Settings/Dial Plan
###############################################################
# Dial Plan Prefix
# String 
P819 =

# Bypass Dial Plan
# String: contact,incoming,outgoing,dialing,mpk,api
P2882 = mpk

# Dial Plan. Default is { x+ | \+x+ | *x+ | *xx*x+ }
# String
# Mandatory
P859= { x+ | \+x+ | *x+ | *xx*x+ }

###############################################################
# Account 6/Call Settings/Call Display
###############################################################
# Caller ID Display. 0 - Auto, 1 - Disabled, 2 - From Header. Default is 2
# Number: 0, 1, 2
# Mandatory
P2824 = 2

# Callee ID Display. 0 - Auto, 1 - Disabled, 2 - To Header. Default is 0
# Number: 0, 1, 2
# Mandatory
P26525 = 0

###############################################################
# Account 6/Call Settings/Ringtone
###############################################################
# Account Ring Tone. 
# 0 - system, 1 - ring1, 2 - ring2, 3 - ring3, 4 - ring4, 5 - ring5, 6 - ring6, 7 - Doorbell, 8 - silent. Default is 0
# Number: 0-8, more if using custom ringtone
# Mandatory
P823 = 0

# Matching Incoming Caller ID. Matching Rule 1
# String
P1518 = 

# Matching Rule 1 Distinctive Ringtone
# 0 - system, 1 - ring1, 2 - ring2, 3 - ring3, 4 - ring4, 5 - ring5, 6 - ring6, 7 - Doorbell, 8 - silent. Default is 0
# Number: 0-8, more if using custom ringtone
# Mandatory
P1519 = 0

# Matching Incoming Caller ID. Matching Rule 2
# String
P1520 = 

# Matching Rule 2 Distinctive Ringtone
# 0 - system, 1 - ring1, 2 - ring2, 3 - ring3, 4 - ring4, 5 - ring5, 6 - ring6, 7 - Doorbell, 8 - silent. Default is 0
# Number: 0-8, more if using custom ringtone
# Mandatory
P1521 = 0

# Matching Incoming Caller ID. Matching Rule 3
# String
P1522 =

# Matching Rule 3 Distinctive Ringtone
# 0 - system, 1 - ring1, 2 - ring2, 3 - ring3, 4 - ring4, 5 - ring5, 6 - ring6, 7 - Doorbell, 8 - silent. Default is 0
# Number: 0-8, more if using custom ringtone
# Mandatory
P1523 = 0

# Matching Incoming Caller ID. Matching Rule 4
# String
P6746 = 

# Matching Rule 4 Distinctive Ringtone
# 0 - system, 1 - ring1, 2 - ring2, 3 - ring3, 4 - ring4, 5 - ring5, 6 - ring6, 7 - Doorbell, 8 - silent. Default is 0
# Number: 0-8, more if using custom ringtone
# Mandatory
P6747 = 0

# Matching Incoming Caller ID. Matching Rule 5
# String
P6748 = 

# Matching Rule 5 Distinctive Ringtone
# 0 - system, 1 - ring1, 2 - ring2, 3 - ring3, 4 - ring4, 5 - ring5, 6 - ring6, 7 - Doorbell, 8 - silent. Default is 0
# Number: 0-8, more if using custom ringtone
# Mandatory
P6749 = 0

# Matching Incoming Caller ID. Matching Rule 6
# String
P6750 = 

# Matching Rule 6 Distinctive Ringtone
# 0 - system, 1 - ring1, 2 - ring2, 3 - ring3, 4 - ring4, 5 - ring5, 6 - ring6, 7 - Doorbell, 8 - silent. Default is 0
# Number: 0-8, more if using custom ringtone
# Mandatory
P6751 = 0

# Matching Incoming Caller ID. Matching Rule 7
# String
P26564 = 

# Matching Rule 7 Distinctive Ringtone
# 0 - system, 1 - ring1, 2 - ring2, 3 - ring3, 4 - ring4, 5 - ring5, 6 - ring6, 7 - Doorbell, 8 - silent. Default is 0
# Number: 0-8, more if using custom ringtone
# Mandatory
P26565 = 0

# Matching Incoming Caller ID. Matching Rule 8
# String
P26566 = 

# Matching Rule 8 Distinctive Ringtone
# 0 - system, 1 - ring1, 2 - ring2, 3 - ring3, 4 - ring4, 5 - ring5, 6 - ring6, 7 - Doorbell, 8 - silent. Default is 0
# Number: 0-8, more if using custom ringtone
# Mandatory
P26567 = 0

# Matching Incoming Caller ID. Matching Rule 9
# String
P26568 = 

# Matching Rule 9 Distinctive Ringtone
# 0 - system, 1 - ring1, 2 - ring2, 3 - ring3, 4 - ring4, 5 - ring5, 6 - ring6, 7 - Doorbell, 8 - silent. Default is 0
# Number: 0-8, more if using custom ringtone
# Mandatory
P26569 = 0

# Matching Incoming Caller ID. Matching Rule 10
# String
P26596 = 

# Matching Rule 10 Distinctive Ringtone
# 0 - system, 1 - ring1, 2 - ring2, 3 - ring3, 4 - ring4, 5 - ring5, 6 - ring6, 7 - Doorbell, 8 - silent. Default is 0
# Number: 0-8, more if using custom ringtone
# Mandatory
P26597 = 0

###############################################################
# Account 6/Advanced Settings
###############################################################
###############################################################
# Account 6/Advanced Settings/Security Settings
###############################################################
# Check Domain Certificates. When set to Yes/Enabled, domain certificate will be checked as defined in RFC5922
# 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P2811 = 0

# Validate Certification Chain. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P2867 = 0

# Validate Incoming Messages. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P2806 = 0

# Omit charset=UTF-8 in MESSAGE. 0 - Disabled, 1 - Enabled. Default is 0
# Number: 0, 1
# Mandatory
P2855 = 0

# Allow Unsolicited REFER. 0 - Disabled, 1 - Enabled, 2 - Enabled/Force Auth. Default is 0
# Number: 0, 1, 2
# Mandatory
P26523 = 0

# Accept Incoming SIP from Proxy Only. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P2847 = 0

# Check SIP User ID for Incoming INVITE. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P849 = 0

# Allow SIP Reset
# 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P26515 = 0

# Authenticate Incoming INVITE. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P2846 = 0

###############################################################
# Account 6/Advanced Settings/MOH
###############################################################
# On Hold Reminder Tone. 0 - Disabled, 1 - Enable. Default is 1
# Number: 0, 1
# Mandatory
P26506 = 1

# Music On Hold URI
# String
P2850 =

###############################################################
# Account 6/Advanced Settings/Advanced Features
###############################################################
# Special Feature. 100 - Standard, 101 - Nortel MCS, 102- Broadsoft, 108 - CBCOM, 
# 109 - RNK, 110 - Sylantro, 117 - Huawei IMS, 119 - Phonepower, 120 - UCM Call Center
# Default is 100
# Number: 100, 101, 102, 108, 109, 110, 117, 119, 120
# Mandatory
P824 = 100

# Feature Key Synchronization. 0 - Disabled, 1 - Enabled. Default is 0.
# Number: 0, 1
# Mandatory
P2825 = 0

# Conference URI
# String
P2818 =

# Broadsoft
# Broadsoft Call Center. 0 - Disabled, 1 - Enabled. Default is 0
# Number: 0, 1
# Mandatory
P2841 = 0

# Hoteling Event. 0 - Disabled, 1 - Enabled. Default is 0
# Number: 0, 1
# Mandatory
P2842 = 0

# Call Center Status. 0 - Disabled, 1 - Enabled. Default is 0
# Number: 0, 1
# Mandatory
P2843 = 0

# Broadsoft Executive Assistant. 0 - Disabled, 1 - Enabled. Default is 0
# Number: 0, 1
# Mandatory
P2864 = 0

# Broadsoft Call Park. 0 - Disabled, 1 - Enabled. Default is 0
# Number: 0, 1
# Mandatory
P2888 = 0

###############################################################
# Account 6/Advanced Settings/BLF(Busy Lamp Field)  2604 only
###############################################################
# Presence Eventlist URI
# String
P26584 =

# Eventlist BLF URI
# String
P844 = 

# Auto Provision Eventlists. 0 - Disabled, 1 - BLF Eventlist, 2 - Presence Eventlist. Default is 0
# Number:0,1,2
# Mandatory
P2889 = 0

# BLF Call-pickup. 0 - Auto, 1 - Force BLF Call-pickup by prefix, 2 - Disabled. Default is 0
# Number: 0, 1, 2
# Mandatory
P6757 = 0

# BLF Call-pickup Prefix. Default is **
# String
# Mandatory
P881 = **

# Call Pickup Barge-In Code
# String
P26546 = 

# PUBLISH for Presence. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P888 = 0

###############################################################
# Account 6/SCA
###############################################################
# Enable SCA (Shared Call Appearance)
# Number: -1, 32. -1 - Disabled, 32 - Enabled
# Mandatory
P1373 = 0

# Line-Seize Timeout (in seconds). Default is 15
# Number: 15 - 60
# Mandatory
P2813 = 15

###############################################################
# Account 6/Feature Codes
###############################################################
#Enable Local Call Features.  0 - No, 1 - Yes. Default is 1
#Number: 0, 1 
#Mandatory
P820 = 1

#Do Not Disturb (DND) - On
# String
P2844 = 

#Do Not Disturb (DND) - Off
# String
P2845 =

# Call Forward Always - On
# String
P26513 = 

# Call Forward Always - Off
# String
P26514 = 

# Call Forward Always - Target
# String
P29592 = 

#Call Forward Busy - On
# String
P26509 = 

#Call Forward Busy - Off
# String
P26510 = 

#Call Forward Busy - Target
# String
P29593 = 

#Call Forward No Answer - On
#String
P26511 = 

#Call Forward No Answer - Off
#String
P26512 = 

#Call Forward No Answer - Target
#String
P29594 = 

# Call Forward No Answer Timeout (s). Default is 12
# Number: 1 - 120
# Mandatory
P870 = 12

####################################################################
# Phone Settings                                                  ##
####################################################################
####################################################################
# General Settings                                                ##
####################################################################
####################################################################
# General Settings/Basic Settings                                 
####################################################################
# Local RTP Port. Default is 5004
# Number: 1024 - 65400. Must be even number
# Mandatory
P39 = 5004

# Local RTP Port Range. Default is 200
# Number: 48 - 10000
# Mandatory
P29610 = 200

# Use Random Port. 0 - No, 1 - Yes. Default is 1
# Number: 0, 1
# Mandatory
P78 = 1

# Keep-Alive Interval (in seconds). Default is 20
# Number: 10 - 160
# Mandatory
P84 = 20

# STUN server
# String
P76 =

# Use NAT IP. This will enable our SIP client to use this IP in the SIP/SDP message. Example 64.3.153.50
# String: a-z, A-Z, 0-9, ".", ":"
P101 =

# Delay Registration. Default is 0.
# Number: 0 - 90
# Mandatory
P8359 = 0

# Test Password Strength. Default is 0.
# Number: 0, 1. 0 - No, 1 - Yes. 
P8468 = 0

# Enable Outbound Notification. Default is 1.
# Number: 0, 1. 0 - No, 1 - Yes. 
P32062 = 1

####################################################################
# General Settings/Public Mode                             
####################################################################
# Enable Public Mode. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P1345 = 0

# Public Mode Username Prefix
# String
P8470 = 

# Public Mode Username Suffix
# String
P8471 = 

####################################################################
# Call Settings                                 
####################################################################
# Key Mode. 1 - Line Mode, 2 - Account Mode. Default is 2
# Number: 1, 2
# Mandatory
P8369 = 2

# Click-To-Dial Feature. 0 - Disabled, 1 - Enabled. Default is 0
# Number: 0, 1
# Mandatory
P1561 = 0

# Enable Call Waiting. 0 - Yes, 1 - No. Default is 0
# Number: 0, 1
# Mandatory
P91 = 0

# Hold Call Before Completing Transfer. 0 - No, 1 - Yes. Default is 1
# Number: 0, 1
P8466 = 1

# Hold Call before Adding Conferee. 0 - No, 1 - Yes. Default is 1
# Number: 0, 1
P22346 = 1

# Enable DND Feature. 0 - No, 1 - Yes. Default is 1
# Number: 0, 1
# Mandatory
P8446 = 1

# Mute Key Functions While Idle. 0 - DND, 1 - Idle Mute, 2 - Disabled. Default is 0
# Number: 0,1,2
# Mandatory
P1565 = 0

# GRP2604 Only
# Enable Sending DTMF via specific MPKs. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P1339 = 0

# Preferred Default Account. 
# 0 - Account 1, 1 - Account 2, 2 - Account 3, 3 - Account 4, 4 - Account 5, 5 - Account 6.
# Number: 0 - 5. Default is 0.
# Mandatory
P29612 = 0

# Off-hook Auto Dial
# String
P71 =

# Off-hook Auto Dial Delay
# Number: 0 - 10
P8388 = 4

# Off-hook/On-hook Timeout (in seconds). Default is 30
# Number: 10 - 60
# Mandatory
P1485 = 30

# Enable Live DialPad. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P8350 = 0

# Live Keypad Expiration. Default is 5
# Number: 2 - 15. 
# Mandatory
P8351 = 5

# Bypass Dial Plan Through Call History and Directories. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P6758 = 0

# Do not Escape '#' as 23% in SIP URL. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P1406 = 0

# Return Code When Refusing Incoming Call. Default is 0
# Number: 0,1,2,3. 0 - Busy(486), 1 - Temporarily Unavailable(480), 2 - Not Found(404), 3 - Decline(603).
# Mandatory
P8360 = 0

# Return Code When Enable DND. Default is 1
# Number: 0,1,2,3. 0 - Busy(486), 1 - Temporarily Unavailable(480), 2 - Not Found(404), 3 - Decline(603).
# Mandatory
P8361 = 1

# Allow Incoming Call Before Ringing.  0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P29609 = 0

# User-Agent Prefix
# String
P8358 = 

####################################################################
# Ringtone                                 
####################################################################
### Call Progress Tones ###
# Syntax: f1=val,f2=val[,c=on1/off1[-on2/off2[-on3/off3]]]; 
# (Frequencies are in Hz and cadence on and off are in 10ms) 

# System Ringtone
# String
# Mandatory
P345 = f1=440,f2=480,c=200/400;

# Dial Tone
# String
# Mandatory
P343 = f1=350,f2=440;

# Second Dial Tone
# String
# Mandatory
P2909 = f1=350,f2=440;

# Message Waiting
# String
# Mandatory
P344 = f1=350,f2=440,c=10/10;

# Ring Back Tone
# String
# Mandatory
P346 = f1=440,f2=480,c=200/400;

# Call Waiting Tone
# String
# Mandatory
P347 = f1=440,f2=440,c=25/525;

# Call-Waiting Tone Gain. 0 - Low, 1 - Medium, 2 - High. Default is 0
# Number: 0, 1, 2
# Mandatory
P1555 = 0

# Busy Tone
# String
# Mandatory
P348 = f1=480,f2=620,c=50/50;

# Reorder Tone
# String
# Mandatory
P349 = f1=480,f2=620,c=25/25;

# Lock Speaker Volume. 0 - No, 1 - Ring, 2 - Talk, 3 - Both. Default is 0
# Number: 0, 1, 2, 3
# Mandatory
P8392 = 0

##############################################################################
##  Multicast Paging
##############################################################################
# Multicast Paging Function. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P22208 = 0

# Allowed in DND Mode. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P8381 = 0

# Paging Barge. 0 - Disable, 1 - priority 1, 2 - priority 2, 3 - priority 3, 
# 4 - priority 4, 5 - priority 5, 6 - priority 6, 7 - priority 7, 8 - priority 8,
# 9 - priority 9, 10 - priority 10. Default is 0.
# Number: 0 - 10
# Mandatory
P1566 = 0

# Paging Priority Active. 0 - Disabled, 1 - Enabled
# Number: 0, 1
# Mandatory
P1567 = 1

# Multicase Channel Number
# Number: 0 - 50 (0 for normal RTP packets, 1-50 for Polycom multicast format packets). Default is 0
P8454 = 0

# Multicast Paging Codec. 18 - G.729A/B, 0 - PCMU, 8 - PCMA, 2 - G.726-32, 9 - G.722, 98 - iLBC, 4- G.723.1
# Number: 18, 0, 8, 2, 9, 98, 4. Default is 9.
# Mandatory
P1568 = 9

# Multicast Sender ID
# String
P8455 = 

### Multicast Listening ### 
# Priority 1
# Listening Address
# String
P1569 = 

# Label
# String
P1570 = 

# Priority 2
# Listening Address
# String
P1571 = 

# Label
# String
P1572 = 

# Priority 3
# Listening Address
# String
P1573 = 

# Label
# String
P1574 = 

# Priority 4
# Listening Address
# String
P1575 = 

# Label
# String
P1576 = 

# Priority 5
# Listening Address
# String
P1577 = 

# Label
# String
P1578 = 

# Priority 6
# Listening Address
# String
P1579 = 

# Label
# String
P1580 = 

# Priority 7
# Listening Address
# String
P1581 = 

# Label
# String
P1582 = 

# Priority 8
# Listening Address
# String
P1583 = 

# Label
# String
P1584 = 

# Priority 9
# Listening Address
# String
P1585 = 

# Label
# String
P1586 = 

# Priority 10
# Listening Address
# String
P1587 = 

# Label
# String
P1588 = 

####################################################################
# Network Settings                                                ##
####################################################################
####################################################################
# Ethernet Settings                                               ##
####################################################################
# Internet Protocol. 0 - Both, prefer IPv4, 1 - Both, prefer IPv6, 2 - IPv4 Only, 3 - IPv6 Only. Default is 2
# Number: 0, 1, 2, 3
# Mandatory
P1415 = 2

####################################################################
# Ethernet Settings/IPv4 Address                                 
####################################################################
# IPv4 Address. 0 - DHCP, 1 - Static IP, 2 - PPPoE. Default is 0
# Number: 0, 1, 2
# Mandatory
P8 = 0

# Host name, DHCP option 12. Max length allowed is 64 characters
# String
P146 =

# Vendor Class ID, DHCP option 60. Max length allowed is 64 characters
# String
# For GRP2601, Default value is Grandstream GRP2601.
# P148 = Grandstream GRP2601
 
# For GRP2602, Default value is Grandstream GRP2602.
# P148 = Grandstream GRP2602

# For GRP2603, Default value is Grandstream GRP2603.
# P148 = Grandstream GRP2603

# For GRP2604, Default value is Grandstream GRP2604.
# P148 = Grandstream GRP2604

# DNS 1 Server. Ignore if DHCP or PPPoE is used
# Number: 0 - 255
P21 = 0

# Number: 0 - 255
P22 = 0

# Number: 0 - 255
P23 = 0

# Number: 0 - 255
P24 = 0

# DNS 2 Server. Ignore if DHCP or PPPoE is used
# Number: 0 - 255
P25 = 0

# Number: 0 - 255
P26 = 0

# Number: 0 - 255
P27 = 0

# Number: 0 - 255
P28 = 0

# Preferred DNS server.  (if specified).
# Number: 0 - 255
P92 = 0

# Number: 0 - 255
P93 = 0

# Number: 0 - 255
P94 = 0

# Number: 0 - 255
P95 = 0

##########################################
# Statically Configured
##########################################
# IP Address. Ignore if DHCP or PPPoE is used
# Number: 0 - 255
P9 = 192

# Number: 0 - 255
P10 = 168

# Number: 0 - 255
P11 = 0

# Number: 0 - 255
P12 = 160

# Subnet mask. Ignore if DHCP or PPPoE is used
# Number: 0 - 255
P13 = 255

# Number: 0 - 255
P14 = 255

# Number: 0 - 255
P15 = 0

# Number: 0 - 255
P16 = 0

# Gateway. Ignore if DHCP or PPPoE is used
# Number: 0 - 255
P17 = 0

# Number: 0 - 255
P18 = 0

# Number: 0 - 255
P19 = 0

# Number: 0 - 255
P20 = 0

##########################################
# PPPoE
##########################################
# PPPoE Account ID
# String
P82 =

# PPPoE Password
# String
# Cannot contain ` or "
P83 =

# PPPoE Service Name
# String 
P269 =

####################################################################
# Ethernet Settings/IPv6 Address                                 
####################################################################
# IPv6 Address. 0 - Auto Configured, 1 - Statically Configured. Default is 0.
# Number: 0, 1
# Mandatory
P1419 = 0

# IPv6 Static Mode: Statically configured. 0 - Full Static, 1 - Prefix Static. Default is 0.
# Number: 0, 1
P1426 = 0

# Full Static: Static IPv6 Address
P1420 =

# Full Static: IPv6 Prefix Length
P1421 =

# Prefix Static: IPv6 Prefix (64bits)
P1422 =

# DNS Server 1 for IPv6 Address
# String: a-z, A-Z, 0-9, ".", ":", "[", "]"
P1424 =

# DNS Server 2 for IPv6 Address
# String: a-z, A-Z, 0-9, ".", ":", "[", "]"
P1425 =

# Preferred DNS Server for IPv6 Address
# String: a-z, A-Z, 0-9, ".", ":", "[", "]"
P1423 =

####################################################################
# Ethernet Settings/802.1X                                 
####################################################################
# 802.1X Mode. 0 - Disable, 1 - EAP-MD5. 2 - EAP-TLS, 3 - EAP-PEAPv0/MSCHAPv2. Default is 0
# Number: 0, 1, 2, 3
# Mandatory
P7901 = 0

# 802.1X Identity. Max length allowed is 64 characters
# String
P7902 = 

# MD5 Password. Max length allowed is 64 characters
# String
P7903 =

# 802.1X CA Certificate
# String
# P8439 =

# 802.1X Client Certificate
# String
# P8440 =

####################################################################
# OpenVPN Settings                                                ##
####################################################################
# OpenVPN Enable.  0 - No, 1 - Yes. Default is 0
# Number: 0, 1 
# Mandatory
P7050 = 0

# OpenVPN Server Address
# String
P7051 =

# OpenVPN Port. Default is 1194
# Number
# Mandatory
P7052 = 1194

# OpenVPN Transport.  0 - UDP, 1 - TCP. Default is 0
#Number: 0, 1 
#Mandatory
P2912 = 0

# OpenVPN Cipher Method. 0 - Blowfish, 1 - AES-128, 2 - AES-256, 3 - Triple-DES. Default is 0
# Number: 0, 1, 2, 3 
# Mandatory
P8396 = 0

# OpenVPN Username
# String
P8394 =

# OpenVPN Password
# String
P8395 =

# Additional Options
# String
P8460 = 

####################################################################
# Advanced Settings                                               ##
####################################################################
####################################################################
# Advanced Settings/Advanced Network Settings      
####################################################################
# Enable LLDP.  0 - Disabled, 1 - Enabled. Default is 1
# Number: 0, 1
# Mandatory
P1684 = 1

# LLDP TX Interval. Default is 60 
# Number: 1 - 3600
# Mandatory
P22122 = 60

# Enable CDP.   0 - Disabled, 1 - Enabled. Default is 1
# Number: 0, 1
# Mandatory
P22119 = 1

# Layer 3 QoS for SIP
# Number:0 - 63
# Mandatory
P1558 = 26

# Layer 3 QoS for RTP
# Number:0 - 63
# Mandatory
P1559 = 46

# Enable DHCP VLAN. 0 - Disable, 1 - Enable. Default is 0.
# Number: 0,1
# Mandatory
P8300 = 0

# Enable Manual VLAN Configuration. 0 - Disable, 1 - Enable. Default is 1.
# Number: 0,1
# Mandatory
P22174 = 1

# Layer 2 QoS 802.1Q/VLAN Tag (VLAN classification for RTP). Default is 0
# Number: 0 - 4094
# Mandatory
P51 = 0

# Layer 2 QoS 802.1p Priority Value (0 - 7). Default is 0
# Number: 0 - 7
# Mandatory
P87 = 0

# Maximum Transmission Unit(MTU). Default is 1500
# Number: 576 - 1500
# Mandatory
P244 = 1500

####################################################################
# Advanced Settings/PC Port Mode      
####################################################################
# PC Port Mode. 0 - Enable But Not Mirrored, 1 - Disabled, 2 - Enabled and Mirrored. Default is 0
# Number: 0, 1, 2
# Mandatory
P1348 = 0

# PC Port VLAN Tag. Default is 0 
# Number: 0 - 4094
#Mandatory
P229 = 0

# PC Port Priority Value. Default is 0 
# Number: 0 - 7
# Mandatory
P230 = 0

####################################################################
# Advanced Settings/Proxy      
####################################################################
# HTTP Proxy
# String
P1552 =

# HTTPS Proxy
# String
P1553 =

# Bypass Proxy for
# String
P22011 = 

####################################################################
# Advanced Settings/Remote Control      
####################################################################
# Action URI Support. 0 - Disabled, 1 - Enabled
# Number: 0, 1. Default is 1
# Mandatory
P32050 = 1

# Remote Control Popup Window Support. 0 - Disabled, 1 - Enabled
# Number: 0, 1. Default is 1
# Mandatory
P32051 = 1

# Action URI Allowed IP List
# String
P32052 = 

# CSTA Control. 0 - Disabled, 1 - Enabled
# Number: 0, 1. Default is 0
# Mandatory
P32053 = 0

####################################################################
# Advanced Settings/CTI Settings(GRP2603/2604 Only)
####################################################################
# Affinity Support. 0 - Disabled, 1 - Enabled
# Number: 0, 1. Default is 0
# Mandatory
P8334 = 0

# Preferred Account. 0 - Account 1, 1 - Account 2, 2 - Account 3, 3 - Account 4, 4 - Account 5, 5 - Account 6
# Number: 0 - 5. Default is 0
# Mandatory
P8335 = 0

####################################################################
# SNMP Settings                                                   ##
####################################################################
# Enable SNMP. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P21896 = 0

# Version. 1 - Version 1, 2 - Version 2, 3 - Version 3. Default is 3
# Number: 1, 2, 3
# Mandatory
P21904 = 3

# Port
# Number. Default is 161.
# Mandatory
P21903 = 161

# Community
# String
P21902 =

# Security Level
# Number: 0 - noAuthUser, 1 - authUser, 2 - privUser. Default is 0
# Mandatory
P21910 = 0

# SNMP Username
# Strings
P21905 = 

# Authentication Protocol
# Number: 0 - None, 1 - MD5, 2 - SHA. Default is 0
# Mandatory
P21906 = 0

# Privacy Protocol
# Number: 0 - None, 1 - DES, 2 - AES. Default is 0
# Mandatory
P21907 = 0

# Authentication Key
# String
P21908 = 

# Privacy Key
# String 
P21909 = 

# SNMP Trap Version
# Number: 1, 2. 1 - Version 1, 2 - Version 2, 3 - Version 3. Default is 2
P21899 = 2

# SNMP Trap IP
# String
P21897 = 

# SNMP Trap Port
# Number: 1025 - 65535. Default is 162
P21898 = 162

# SNMP Trap Interval
# Number: 1 - 1440. Default is 5
P21901 = 5

# SNMP Trap Community
# String
P21900 = 

# SNMP Trap Username
# String
P21911 = 

# Trap Security Level
# Number: 0 - noAuthUser, 1 - authUser, 2 - privUser. Default is 0
# Mandatory
P21916 = 0

# Trap Authentication Protocol
# Number: 0 - None, 1 - MD5, 2 - SHA. Default is 0
# Mandatory
P21912 = 0

# Trap Privacy Protocol
# Number: 0 - None, 1 - DES, 2 - AES. Default is 0
# Mandatory
P21913 = 0

# Trap Authentication Key
# String
P21914 = 

# Trap Privacy Key
# String
P21915 = 

####################################################################
# Programmable Keys                                               ##
####################################################################
####################################################################
# Multi-Purpose Keys                                              ##
####################################################################
####################################################################
# Multi-Purpose Keys/Key Settings            GRP2604 only                           
####################################################################
# MPK 1
####################################################################
# Key Mode.
# Number: -1 - 9, 11, 12, 15, 16, 17, 19, 20 - 23, 28, 29
# None (-1), SpeedDial (0), BLF (1), PresenceWatcher (2), EventlistBLF (3), SpeedDialViaActiveAccount (4)
# DialDTMF (5), VoiceMail (6), CallReturn (7), Transfer (8), CallPark (9), , LDAPSearch (11)
# Conference (12), CallLog (15), MonitoredCallPark (16), Menu (17), Information (19), Message (20), 
# Forward (21), DND (22), Redial (23), EventListPresence (28), Provision (29)
P323 = -1

# Account. 0 - Account 1, 1 - Account 2, 2 - Account 3, 3 - Account 4, 4 - Account 5, 5 - Account 6
# Number: 0, 1, 2, 3, 4, 5
# Mandatory
P301 = 0

# Description. Max length allowed is 256 characters.
# String
P302 =

# Value.  Max length allowed is 256 characters.
# String
P303 =

####################################################################
# MPK 2
####################################################################
# Key Mode.
# Number: -1 - 9, 11, 12, 15, 16, 17, 19, 20 - 23, 28, 29
# None (-1), SpeedDial (0), BLF (1), PresenceWatcher (2), EventlistBLF (3), SpeedDialViaActiveAccount (4)
# DialDTMF (5), VoiceMail (6), CallReturn (7), Transfer (8), CallPark (9), , LDAPSearch (11)
# Conference (12), CallLog (15), MonitoredCallPark (16), Menu (17), Information (19), Message (20), 
# Forward (21), DND (22), Redial (23), EventListPresence (28), Provision (29)
P324 = -1

# Account. 0 - Account 1, 1 - Account 2, 2 - Account 3, 3 - Account 4, 4 - Account 5, 5 - Account 6
# Number: 0, 1, 2, 3, 4, 5
# Mandatory
P304 = 0

# Description. Max length allowed is 256 characters.
# String
P305 =

# Value.  Max length allowed is 256 characters.
# String
P306 =

####################################################################
# MPK 3
####################################################################
# Key Mode.
# Number: -1 - 9, 11, 12, 15, 16, 17, 19, 20 - 23, 28, 29
# None (-1), SpeedDial (0), BLF (1), PresenceWatcher (2), EventlistBLF (3), SpeedDialViaActiveAccount (4)
# DialDTMF (5), VoiceMail (6), CallReturn (7), Transfer (8), CallPark (9), , LDAPSearch (11)
# Conference (12), CallLog (15), MonitoredCallPark (16), Menu (17), Information (19), Message (20), 
# Forward (21), DND (22), Redial (23), EventListPresence (28), Provision (29)
P325 = -1

# Account. 0 - Account 1, 1 - Account 2, 2 - Account 3, 3 - Account 4, 4 - Account 5, 5 - Account 6
# Number: 0, 1, 2, 3, 4, 5
# Mandatory
P307 = 0

# Description. Max length allowed is 256 characters.
# String
P308 =

# Value.  Max length allowed is 256 characters.
# String
P309 =

####################################################################
# MPK 4
####################################################################
# Key Mode.
# Number: -1 - 9, 11, 12, 15, 16, 17, 19, 20 - 23, 28, 29
# None (-1), SpeedDial (0), BLF (1), PresenceWatcher (2), EventlistBLF (3), SpeedDialViaActiveAccount (4)
# DialDTMF (5), VoiceMail (6), CallReturn (7), Transfer (8), CallPark (9), , LDAPSearch (11)
# Conference (12), CallLog (15), MonitoredCallPark (16), Menu (17), Information (19), Message (20), 
# Forward (21), DND (22), Redial (23), EventListPresence (28), Provision (29)
P326 = -1

# Account. 0 - Account 1, 1 - Account 2, 2 - Account 3, 3 - Account 4, 4 - Account 5, 5 - Account 6
# Number: 0, 1, 2, 3, 4, 5
# Mandatory
P310 = 0

# Description. Max length allowed is 256 characters.
# String
P311 =

# Value.  Max length allowed is 256 characters.
# String
P312 =

####################################################################
# MPK 5
####################################################################
# Key Mode.
# Number: -1 - 9, 11, 12, 15, 16, 17, 19, 20 - 23, 28, 29
# None (-1), SpeedDial (0), BLF (1), PresenceWatcher (2), EventlistBLF (3), SpeedDialViaActiveAccount (4)
# DialDTMF (5), VoiceMail (6), CallReturn (7), Transfer (8), CallPark (9), , LDAPSearch (11)
# Conference (12), CallHistory (15), MonitoredCallPark (16), Menu (17), Information (19), Message (20), 
# Forward (21), DND (22), Redial (23), EventListPresence (28), Provision (29)
P327 = -1

# Account. 0 - Account 1, 1 - Account 2, 2 - Account 3, 3 - Account 4, 4 - Account 5, 5 - Account 6
# Number: 0, 1, 2, 3, 4, 5
# Mandatory
P313 = 0

# Description. Max length allowed is 256 characters.
# String
P314 =

# Value.  Max length allowed is 256 characters.
# String
P315 =

####################################################################
# MPK 6
####################################################################
# Key Mode.
# Number: -1 - 9, 11, 12, 15, 16, 17, 19, 20 - 23, 28, 29
# None (-1), SpeedDial (0), BLF (1), PresenceWatcher (2), EventlistBLF (3), SpeedDialViaActiveAccount (4)
# DialDTMF (5), VoiceMail (6), CallReturn (7), Transfer (8), CallPark (9), , LDAPSearch (11)
# Conference (12), CallLog (15), MonitoredCallPark (16), Menu (17), Information (19), Message (20), 
# Forward (21), DND (22), Redial (23), EventListPresence (28), Provision (29)
P328 = -1

# Account. 0 - Account 1, 1 - Account 2, 2 - Account 3, 3 - Account 4, 4 - Account 5, 5 - Account 6
# Number: 0, 1, 2, 3, 4, 5
# Mandatory
P316 = 0

# Description. Max length allowed is 256 characters.
# String
P317 =

# Value.  Max length allowed is 256 characters.
# String
P318 =

####################################################################
# MPK 7
####################################################################
# Key Mode.
# Number: -1 - 9, 11, 12, 15, 16, 17, 19, 20 - 23, 28, 29
# None (-1), SpeedDial (0), BLF (1), PresenceWatcher (2), EventlistBLF (3), SpeedDialViaActiveAccount (4)
# DialDTMF (5), VoiceMail (6), CallReturn (7), Transfer (8), CallPark (9), , LDAPSearch (11)
# Conference (12), CallLog (15), MonitoredCallPark (16), Menu (17), Information (19), Message (20), 
# Forward (21), DND (22), Redial (23), EventListPresence (28), Provision (29)
P329 = -1

# Account. 0 - Account 1, 1 - Account 2, 2 - Account 3, 3 - Account 4, 4 - Account 5, 5 - Account 6
# Number: 0, 1, 2, 3, 4, 5
# Mandatory
P319 = 0

# Description. Max length allowed is 256 characters.
# String
P320 =

# Value.  Max length allowed is 256 characters.
# String
P321 =

####################################################################
# MPK 8
####################################################################
# Key Mode.
# Number: -1 - 9, 11, 12, 15, 16, 17, 19, 20 - 23, 28, 29
# None (-1), SpeedDial (0), BLF (1), PresenceWatcher (2), EventlistBLF (3), SpeedDialViaActiveAccount (4)
# DialDTMF (5), VoiceMail (6), CallReturn (7), Transfer (8), CallPark (9), , LDAPSearch (11)
# Conference (12), CallLog (15), MonitoredCallPark (16), Menu (17), Information (19), Message (20), 
# Forward (21), DND (22), Redial (23), EventListPresence (28), Provision (29)
P353 = -1

# Account. 0 - Account 1, 1 - Account 2, 2 - Account 3, 3 - Account 4, 4 - Account 5, 5 - Account 6
# Number: 0, 1, 2, 3, 4, 5
# Mandatory
P354 = 0

# Description. Max length allowed is 256 characters.
# String
P355 =

# Value.  Max length allowed is 256 characters.
# String
P356 =

####################################################################
# MPK 9
####################################################################
# Key Mode.
# Number: -1 - 9, 11, 12, 15, 16, 17, 19, 20 - 23, 28, 29
# None (-1), SpeedDial (0), BLF (1), PresenceWatcher (2), EventlistBLF (3), SpeedDialViaActiveAccount (4)
# DialDTMF (5), VoiceMail (6), CallReturn (7), Transfer (8), CallPark (9), , LDAPSearch (11)
# Conference (12), CallLog (15), MonitoredCallPark (16), Menu (17), Information (19), Message (20), 
# Forward (21), DND (22), Redial (23), EventListPresence (28), Provision (29)
P357 = -1

# Account. 0 - Account 1, 1 - Account 2, 2 - Account 3, 3 - Account 4, 4 - Account 5, 5 - Account 6
# Number: 0, 1, 2, 3, 4, 5
# Mandatory
P358 = 0

# Description. Max length allowed is 256 characters.
# String
P359 =

# Value.  Max length allowed is 256 characters.
# String
P360 =

####################################################################
# MPK 10
####################################################################
# Key Mode.
# Number: -1 - 9, 11, 12, 15, 16, 17, 19, 20 - 23, 28, 29
# None (-1), SpeedDial (0), BLF (1), PresenceWatcher (2), EventlistBLF (3), SpeedDialViaActiveAccount (4)
# DialDTMF (5), VoiceMail (6), CallReturn (7), Transfer (8), CallPark (9), , LDAPSearch (11)
# Conference (12), CallLog (15), MonitoredCallPark (16), Menu (17), Information (19), Message (20), 
# Forward (21), DND (22), Redial (23), EventListPresence (28), Provision (29)
P361 = -1

# Account. 0 - Account 1, 1 - Account 2, 2 - Account 3, 3 - Account 4, 4 - Account 5, 5 - Account 6
# Number: 0, 1, 2, 3, 4, 5
# Mandatory
P362 = 0

# Description. Max length allowed is 256 characters.
# String
P363 =

# Value.  Max length allowed is 256 characters.
# String
P364 =

####################################################################
# Multi-Purpose Keys/Basic Settings            GRP2604 only                           
####################################################################
# Transfer Mode via MPK. 0 - Blind Transfer, 1 - Attended Transfer, 2 - New Call. Default is 0
# Number: 0, 1, 2
# Mandatory
P8390 = 0

# Enable transfer via non-Transfer MPK. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P22162 = 0

####################################################################
# Idle Screen Softkeys                                            ##
####################################################################
# Custom Idle Screen Softkey Layout
# Number: 0 - No, 1 - Yes
P2939 = 0

####################################################################
# Custom Softkey 1     
####################################################################
# Key Mode
# Number: 0, 4, 6
# SpeedDial (0), SpeedDialViaActiveAccount (4), VoiceMail (6)
P2987 = 

# Account. 0 - Account 1, 1 - Account 2, 2 - Account 3, 3 - Account 4, 4 - Account 5, 5 - Account 6
# Number: 0, 1, 2, 3, 4, 5
# Mandatory
P2988 = 0

# Label. Max length allowed is 256 characters.
# String
P2989 =

# Value.  Max length allowed is 256 characters.
# String
P2990 =

####################################################################
# Custom Softkey 2   
####################################################################
# Key Mode
# Number: 0, 4, 6
# SpeedDial (0), SpeedDialViaActiveAccount (4), VoiceMail (6)
P2991 = 

# Account. 0 - Account 1, 1 - Account 2, 2 - Account 3, 3 - Account 4, 4 - Account 5, 5 - Account 6
# Number: 0, 1, 2, 3, 4, 5
# Mandatory
P2992 = 0

# Label. Max length allowed is 256 characters.
# String
P2993 =

# Value.  Max length allowed is 256 characters.
# String
P2994 =

####################################################################
# Custom Softkey 3
####################################################################
# Key Mode
# Number: 0, 4, 6
# SpeedDial (0), SpeedDialViaActiveAccount (4), VoiceMail (6)
P2995 = 

# Account. 0 - Account 1, 1 - Account 2, 2 - Account 3, 3 - Account 4, 4 - Account 5, 5 - Account 6
# Number: 0, 1, 2, 3, 4, 5
# Mandatory
P2996 = 0

# Label. Max length allowed is 256 characters.
# String
P2997 =

# Value.  Max length allowed is 256 characters.
# String
P2998 =

####################################################################
# Custom Idle Screen Softkey Layout
####################################################################
# String:Custom-Menu,Custom-History,Custom-BS-History,Custom-Contacts,Custom-BS-Contacts,Custom-LDAP-Contacts,Custom-DND,Custom-Redial,Custom-CallReturn
# Custom-Paging,ParkedCalls,Custom-BS-CallCenter,Custom-BS-EXEC-Asst,Custom1,Custom2,Custom3
P8348 = Custom-Menu,Custom-History,Custom-Contacts,Custom-Redial,Custom-DND

####################################################################
# Call Screen Softkeys                                            ##
####################################################################
# Custom Call Screen Softkey Layout
# Number: 0 - No, 1 - Yes
P2923 = 0

# Enforce Softkey Layout Position
# Number: 0 - No, 1 - Yes
P2924 = 0

####################################################################
# Custom Softkey 1     
####################################################################
# Key Mode
# Number: 0, 4, 6
# SpeedDial (0), SpeedDialViaActiveAccount (4), VoiceMail (6)
P8475 = 

# Label. Max length allowed is 256 characters.
# String
P8476 =

# Value.  Max length allowed is 256 characters.
# String
P8477 =

####################################################################
# Custom Softkey 2   
####################################################################
# Key Mode
# Number: 0, 4, 6
# SpeedDial (0), SpeedDialViaActiveAccount (4), VoiceMail (6)
P8478 = 

# Label. Max length allowed is 256 characters.
# String
P8479 =

# Value.  Max length allowed is 256 characters.
# String
P8480 =

####################################################################
# Custom Softkey 3
####################################################################
# Key Mode
# Number: 0, 4, 6
# SpeedDial (0), SpeedDialViaActiveAccount (4), VoiceMail (6)
P8481 = 

# Label. Max length allowed is 256 characters.
# String
P8482 =

# Value.  Max length allowed is 256 characters.
# String
P8483 =

####################################################################
# Custom Call Screen Softkey Layout
####################################################################
# Softkey layout in dialing state
# String: EndCall,Backspace,Dial,Custom-Contacts,Custom-History,Custom1,Custom2,Custom3
P2925 = EndCall,Backspace,Dial,Custom-Contacts,Custom-History

# Softkey layout in ringing state
# String: Answer,Reject,Forward,Custom-Silence,Custom1,Custom2,Custom3
P2926 = Answer,Reject,Forward,Custom-Silence

# Softkey layout in calling state
# String: EndCall,ConfCall,Custom1,Custom2,Custom3
P2927 = EndCall,ConfCall

# Softkey layout in call connected state
# String: EndCall,ConfCall,NewCall,Swap,Transfer,Record,Custom-Hold,Custom-NoiseShield,DialDTMF,Custom1,Custom2,Custom3
P2928 = EndCall,ConfCall,NewCall,Swap,Transfer,Record,Custom-Hold,Custom-NoiseShield,DialDTMF

# Softkey layout in on hold state
# String: EndCall,Resume,NewCall,ConfCall,Swap,Transfer,Custom1,Custom2,Custom3
P2929 = EndCall,Resume,NewCall,ConfCall,Swap,Transfer

# Softkey layout in call failed state
# String: EndCall,Redial,Custom1,Custom2,Custom3
P2930 = EndCall,Redial

# Softkey layout in transfer state
# String: Cancel,Backspace,Transfer,Custom-Contacts,Custom-History,Custom1,Custom2,Custom3
P2931 = Cancel,Backspace,Transfer,Custom-Contacts,Custom-History

# Softkey layout in conference state
# String: Cancel,Dial,Backspace,Custom-Contacts,Custom-History,Custom1,Custom2,Custom3
P2932 = Cancel,Dial,Backspace,Custom-Contacts,Custom-History

# Softkey layout in conference connected state
# String: EndCall,ConfRoom,Custom-Hold,Add,Custom-NoiseShield,Custom1,Custom2,Custom3
P2933 = EndCall,ConfRoom,Custom-Hold,Add,Custom-NoiseShield

# Softkey layout in onhook dialing state
# String: EndCall,Backspace,Dial,Custom-Contacts,Custom-History,Custom1,Custom2,Custom3
P2935 = EndCall,Backspace,Dial,Custom-Contacts,Custom-History

####################################################################
# System Settings                                                 ##
####################################################################
####################################################################
# Time And Language                                               ##
####################################################################
####################################################################
# Time And Language/Date and Time      
####################################################################
# NTP Server
# String
P30 = pool.ntp.org

# Secondary NTP Server
# String
P8333 = 

# NTP Update Interval
# String
# Number: 5 - 1440. Default is 1440 
P5005 = 1440

# Allow DHCP Option 42 to override NTP server. 0 - No, 1 - Yes. Default is 0
# When set to Yes(1), it will override the configured NTP server
# Number: 0, 1
# Mandatory
P144 = 0

# Time Zone

# Web GUI Option										P Value
# Automatic												auto
# GMT-12:00 (International Date Line West)				TAZ+12
# GMT-11:00 (Midway Island, Samoa) 						TAB+11
# GMT-10:00 (US Hawaiian Time) 							HAW10
# GMT-9:00 (US Alaska Time) 							AKST9AKDT
# GMT-8:00 (US Pacific Time, Los Angeles)				PST8PDT
# GMT-08:00 (Baja California)							PST8PDT,M3.2.0,M11.1.0
# GMT-07:00 (US Mountain Time, Denver) 					MST7MDT
# GMT-07:00 (Mountain Time (Arizona, no DST)) 			MST7
# GMT-07:00 (Chihuahua, La Paz, Mazatlan)				MST7MDT,M4.1.0,M10.5.0  
# GMT-06:00 (Central Time) 								CST6CDT
# GMT-06:00 (Central America) 							CST+6
# GMT-06:00 (Guadalajara, Mexico City, Monterrey)		CST6CDT,M4.1.0,M10.5.0
# GMT-05:00 (Eastern Time)								EST5EDT
# GMT-05:00 (Eastern Time without daylight saving) 		EST5
# GMT-04:30 (Caracas) 									TZf+4:30
# GMT-04:00 (Atlantic Time) 							AST4ADT
# GMT-04:00 (Atlantic Time (New Brunswick)) 			AST4ADT,M3.2.0,M11.1.0
# GMT-04:00 (Santiago, Chile)							CLT4CLST,M9.1.6/24:00,M4.1.6/24:00
# GMT-03:30 (Newfoundland Time)							NST+3:30NDT+2:30,M4.1.0/00:01:00,M10.5.0/00:01:00
# GMT-03:00 (Greenland) 								TZK+3
# GMT-03:00 (Brazil, Sao Paulo) 						BRST+3BRDT+2,M11.1.0,M2.3.0
# GMT-02:00 (Argentina) 								UTC+3 
# GMT-02:00 (Mid-Atlantic) 								TZL+2
# GMT-01:00 (Azores, Cape Verdi Is.) 					TZM+1
# GMT (Edinburgh, Casablanca, Monrovia) 				TZN+0
# GMT (London, Great Britain) 							GMT+0BST-1,M3.5.0/01:00:00,M10.5.0/02:00:00
# GMT (Lisbon, Portugal) 								WET-0WEST-1,M3.5.0/01:00:00,M10.5.0/02:00:00
# GMT (Dublin, Ireland) 								GMT+0IST-1,M3.5.0/01:00:00,M10.5.0/02:00:00
# GMT+01:00 (Paris, Vienna, Warsaw, Roma, Madrid, Prague, Berlin, Budapest, Amsterdam, Belgium)   CET-1CEST-2,M3.5.0/02:00:00,M10.5.0/03:00:00
# GMT+02:00 (Israel, Cairo, Athens, Istanbul, Buchrest) TZP-2
# GMT+02:00 (Helsinki, Athens, Tallinn) 				EET-2EEST-3,M3.5.0/03:00:00,M10.5.0/04:00:00
# GMT+02:00 (Kyiv, Ukraine) 							EET-2EEST,M3.5.0/3,M10.5.0/4 
# GMT+03:00 (Kuwait, Baghdad, Tehran, Nairobi) 			TZQ-3
# GMT+03:00 (Moscow, Russia) 							MSK-3
# GMT+04:00 (Abu Dhabi, Baku) 							TZR-4
# GMT+05:00 (Islamabad, Ekaterinburg, Karachi, Tashkent)TZS-5
# GMT+05:30 (Chennai, New Delhi, Mumbai) 				TZT-5:30
# GMT+05:45 (Kathmandu) 								TZU-5:45
# GMT+06:00 (Almaty, Astana, Dhaka, Novosibirsk) 		TZV-6
# GMT+06:30 (Rangoon) 									TZW-6:30
# GMT+07:00 (Bankok, Hanoi, Krasnoyarsk) 				TZX-7
# GMT+07:00 (Jakarta) 									WIB-7
# GMT+08:00 (Beijing, Taipei, Kuala Lumpur, Irkutsk) 	TZY-8
# GMT+08:00 (Singapore) 								SGT-8
# GMT+08:00 (Ulaanbaatar, Mongolia) 					ULAT-8
# GMT+08:00 (Perth) 									WST-8
# GMT+09:00 (Japan, Korea, Yakutsk) 					TZZ-9
# GMT+09:30 (Adelaide) 									CST-9:30CDT-10:30,M10.1.0/02:00:00,M4.1.0/03:00:00
# GMT+09:30 (Darwin) 									CST-9:30 
# GMT+10:00 (Guam) 										TZb-10
# GMT+10:00 (Hobart) 									EST-10EDT-11,M10.1.0/02:00:00,M4.1.0/03:00:00
# GMT+10:00 (Sydney, Melbourne, Canberra) 				EST-10EDT-11,M10.1.0/02:00:00,M4.1.0/03:00:00
# GMT+10:00 (Brisbane) 									EST-10
# GMT+11:00 (Magadan, Solomon Is., New Caledonia) 		TZc-11
# GMT+12:00 (Auckland, Wellington) 						NZST-12NZDT-13,M9.5.0/02:00:00,M4.1.0/03:00:00
# GMT+12:00 (Fiji) 										TZd-12
# GMT+13:00 (Nuku'alofa) 								TZe-13
# Self-Defined Time Zone								customize

# String
# Mandatory
P64 = auto

# Allow DHCP Option 2 to Override Time Zone Setting
# Number: 0, 1
P143 = 1

# Self Defined Time Zone. Max length allowed is 64 characters
# String
# Mandatory
P246 = MTZ+6MDT+5,M4.1.0,M11.1.0

# Date Display Format
# 0: yyyy-mm-dd      eg. 2011-10-31
# 1: mm-dd-yyyy      eg. 10-31-2011
# 2: dd-mm-yyyy      eg. 31-10-2011
# 3: dddd, MMMM dd   eg. Monday, October 31
# Number: 0, 1, 2, 3
# Mandatory
P102 = 0

# Time Display Format. 0 - 12 Hour, 1 - 24 Hour
# Number: 0, 1
# Mandatory
P122 = 0

####################################################################
# Time And Language/Language      
####################################################################
# Display Language. Default is auto
# ar - Arabic, ca - Catalan, cz - Czech, de - Deutsh
# en - English, es - Spanish, fr - Francais
# he - Hebrew, hr - Hrvatski, hu - Magyar 
# it - Italiano, ja - japanese, ko - korean, lv - latvian
# nl - Dutch, pl - Polski, pt - Portugue
# ru - Russian, sl - Slovenian, se - Svenska, tr - Turkish
# zh-tw - traditional chinese, zh - simplified chinese, auto - Automatic
# Downloaded Language
# String
# Mandatory
P1362 = auto

####################################################################
# Security Settings                                               ##
####################################################################
####################################################################
# Security Settings/"Web/SSH Access"      
####################################################################
####################################################################
# Security Settings/"Web/SSH Access"/SSH Access      
####################################################################
# Enable SSH. 0 - Yes, 1 - No. Default is 0
# Number: 0, 1
P276 = 0

####################################################################
# Security Settings/Web/SSH Access/Keypad Mode      
####################################################################
# Configuration Via Keypad Menu. 0 - Unrestricted, 1 - Basic settings only, 2 - Constraint mode, 3 - Locked Mode. Default is 0
# Number: 0, 1, 2, 3
# Mandatory
P1357 = 0

####################################################################
# Security Settings/"Web/SSH Access"/Web Access      
####################################################################
# HTTP Web Port. Default is 80
# Number
# Mandatory
P22120 = 80

# HTTPS Web Port. Default is 443
# Number
# Mandatory
P22121 = 443

# Web Access Mode. 0 - HTTPS, 1 - HTTP, 2 - Disabled, 3 - Both HTTP and HTTPS. Default is 3
# Number: 0, 1, 2, 3
# Mandatory
P1650 = 3

# Web Access Control. 0 - None, 1 - Whitelist, 2 - Blacklist. Default is 0
# Number: 0, 1, 2, 3
# Mandatory
P22374 = 0

# Web Access Control List
# String
P22375 = 

# Web Session Timeout(in minutes)
# Number: 2 - 60. Default is 10
P28116 = 10

# Enable User Web Access. 0 - Disabled, 1 - Enabled. Default is 1
# Number: 0, 1
# Mandatory
P8469 = 1

# Validate Server Certificates. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P8463 = 0

# Web/Restrict mode Lockout Duration (0-60 minutes). Default is 5
# Number: 0-60
P1683 = 5

# Web Session Attempt Limit
# Number: 1 - 10. Default is 5
P28117 = 5

####################################################################
# Security Settings/User Info Management      
####################################################################
# User Password
# String: a-z, A-Z, 0-9
# P196 =

# Admin Password
# String: a-z, A-Z, 0-9
# P2 = 

####################################################################
# Security Settings/Client Certificate
####################################################################
# SIP TLS Certificate
# String: a-z, A-Z, 0-9
# P280 =

# SIP TLS Private Key
# String: a-z, A-Z, 0-9
# P279 =

# SIP TLS Private Key Password
# String: a-z, A-Z, 0-9
P281 = 

####################################################################
# Security Settings/Trusted CA Certificates
####################################################################
# Load CA Certificates. 0 - Default Certificates, 1 - Custom Certificates, 2 - All Certificates
# Number: 0, 1, 2. Default is 0
P8502 = 0

##############################################################################
##  Maintenance/Security Settings/Keypad Lock  ##
##############################################################################
# Enable Keypad Locking. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P1382 = 0

# Keypad Lock Type. 0 - All Keys, 1 - Functional Keys. Default is 0
# Number: 0, 1
# Mandatory
P8383 = 0

# Password to Lock/Unlock
# String
P1383 = 

# Keypad Lock Timer. Default is 0
# Number
# Mandatory
P8384 = 0

# Emergency. Default is 112, 911, 110.
# String
P8385 = 112, 911, 110

####################################################################
# Preferences                                                     ##
####################################################################
####################################################################
# Preferences/LCD&LED                                               
####################################################################
# Backlight Brightness
# Active. Default is 8.
# Number: 0-8
# Mandatory
P334 = 8

# Idle. Default is 1.
# Number: 0 - 8
# Mandatory
P335 = 1

# Active Backlight Timeout. Default is 1
# Number: 1 - 90
# Mandatory
P8356 = 1

# Disable Missed Call Backlight. 0 - No, 1 - Yes, 2 - Yes, but flash MWI LED. Default is 0
# Number: 0, 1, 2
# Mandatory
P351 = 0

# New Message LED Indicator. 0 - Blinking, 1 - Off, 2 - Solid. Default is 0
# Number: 0, 1, 2
# Mandatory
P8371 = 0

####################################################################
# Preferences/Audio Control                                           
####################################################################
####################################################################
# Headset                                       
####################################################################
# HEADSET Key Mode. 0 - Default Mode, 1 - Toggle Headset/Speaker. Default is 0
# Number: 0, 1
# Mandatory
P1312 = 0

# Headset Type. 0 - Normal, 1 - Plantronics EHS, 2 - Jabra EHS, 3 - Sennheiser EHS. Default is 0
# Number: 0, 1, 2, 3
# Mandatory
P1487 = 0

# Always Ring Speaker. 0 - No, 1 - Yes, both, 2 - Yes, speaker only. Default is 0
# Number: 0, 1, 2
# Mandatory
P1439 = 0

# Headset TX gain(dB). 1 - -6, 0 - 0, 2 - +6. Default is 0
# Number: 0, 1, 2
# Mandatory
P1301 = 0

# Headset RX gain(dB). 1 - -6, 0 - 0, 2 - +6. Default is 0
# Number: 0, 1, 2
# Mandatory
P1302 = 0

# Enable Headset Noise Shield. 0 - Disable, 1 - Moderate Headset, 2 - Loud Headset, 3 - Thin Headset
# Number: 0, 1, 2, 3
# Mandatory
P8563 = 1

####################################################################
# Handset                                         
####################################################################
# Handset TX gain(dB). 1 - -6, 0 - 0, 2 - +6. Default is 0
# Number: 0, 1, 2
# Mandatory
P1464 = 0

# Enable EDRC Feature. Default is 1.0 - Disable, 1 - High Shielding, 2 - Soft Shielding
# Number: 0, 1, 2
# Mandatory
P8538 = 1

####################################################################
# TR-069                                                          ##
####################################################################
# Enable TR-069
# Number: 0, 1
# Mandatory
P1409 = 0

# ACS URL
# String
P4503 = https://acs.gdms.cloud

# TR-069 Username
# String
P4504 =

# TR-069 Password
# String
P4505 =

# Periodic Inform Enable. 0 - No, 1 - Yes. Default is 1
# Number: 0, 1
# Mandatory
P4506 = 1

# Periodic Inform Interval. Default is 60.
# Number
P4507 = 60

# Connection Request Username	
# String: a-z, A-Z, 0-9
P4511 =

# Connection Request Password	
# String: a-z, A-Z, 0-9
P4512 =

# Connection Request Port. Default is 7547.
# Number
P4518 = 7547

# CPE SSL Certificate
# String: a-z, A-Z, 0-9
P8220 =

# CPE SSL Private Key
# String: a-z, A-Z, 0-9
P8221 =

# Start TR-069 at Random Time. 0 - Disabled, 1 - Enabled. Default is 0
# Number: 0, 1
# Mandatory
P8487 = 0

####################################################################
# Maintenance                                                     ##
####################################################################
####################################################################
# Upgrade and Provisioning                                        ##
####################################################################
####################################################################
# Upgrade and Provisioning/Firmware
####################################################################
####################################################################
# Upgrade and Provisioning/Firmware/Upgrade via Network
####################################################################
# Firmware Upgrade Via. 0 - TFTP,  1 - HTTP, 2 - HTTPS, 3 - FTP, 4 - FTPS. Default is 1. 
# Number: 0, 1, 2, 3, 4
# Mandatory
P6767 = 1

# Firmware Server Path
# String
P192 = fm.grandstream.com/gs

# Firmware HTTP/HTTPS Username
# String
P6768 = 

# Firmware HTTP/HTTPS Password
# String
P6769 = 

# Firmware File Prefix
# String
P232 =

# Firmware File Postfix
# String
P233 =

####################################################################
# Upgrade and Provisioning/Config File
####################################################################
####################################################################
# Upgrade and Provisioning/Config File/Configure via Network
####################################################################
# Config Upgrade Via. 0 - TFTP,  1 - HTTP, 2 - HTTPS, 3 - FTP, 4 - FTPS. Default is 2
# Number: 0, 1, 2, 3, 4
# Mandatory
P212 = 2

# Config Server Path
# String
P237 = fm.grandstream.com/gs

# Config HTTP/HTTPS User Name
# String
P1360 =

# Config HTTP/HTTPS Password
# String
P1361 =

# Always Authenticate Before Challenge. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P20713 = 0

# Config File Prefix
# String
P234 =

# Config File Postfix
# String
P235 =

# Authenticate Conf File. 0 - No, 1 - Yes. Default is No
# Number: 0, 1
# Mandatory
P240 = 0

# XML Config File Password
# String
P1359 = 

####################################################################
# Upgrade and Provisioning/Provision
####################################################################
####################################################################
# Upgrade and Provisioning/Auto Upgrade
####################################################################
# Automatic Upgrade. 
# 0 - No, 
# 1 - Yes, check for upgrade every () minute,
# 2 - Yes, check for upgrade every day,
# 3 - Yes, check for upgrade every week,
# Default is No
# Number: 0, 1, 2, 3
# Mandatory
P194 = 0

# Automatic Upgrade Check Interval (m). Default is 10080.
# Number: 60-86400
# Mandatory
P193 = 10080

# Hour of the Day--Start (0-23). Default is 1
# Number: 0 - 23
P285 = 1

# Hour of the Day--End (-1, 0-23). Default is 0
# Number: -1, 0 - 23
P8459 = 0

# Day of the Week (0-6). Default is 1
# Number: 0-6
P286 = 1

# Start Upgrade at Random Time. 0 - No, 1 - Yes. Default is No
# Number: 0, 1
# Mandatory
P8458 = 0

# Firmware Upgrade and Provisioning
# 0 - Always check for new firmware
# 1 - Check new firmware only when F/W pre/suffix changes
# 2 - Always skip the firmware check
# Number: 0, 1, 2
# Mandatory
P238 = 0

# Firmware Upgrade Confirmation. 0 - No, 1 - Yes. Default is 1
# Number: 0,1
# Mandatory
P8375 = 1

####################################################################
# Upgrade and Provisioning/DHCP Option
####################################################################
# Allow DHCP Option 43 and Option 66 to override server. 0 - No, 1 - Yes, 2 - Prefer, fallback when failed. Default is 1
# When set to Yes(1), it will override the configured provision path and method
# Number: 0, 1, 2
# Mandatory
P145 = 1

# Allow DHCP Option 120 to Override SIP Server
# 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P1411 = 0

# Additional Override DHCP Option. 0 - None,  1 - Option 150,  2 - Option 160. Default is 0
# Number: 0, 1, 2
# Mandatory
P8337 = 0

####################################################################
# Upgrade and Provisioning/Provision/Config Provision
####################################################################
# Download and Process ALL Available Config Files. 0 - No, 1 - Yes. Default is No
# Number: 0, 1
# Mandatory
P8467 = 0

# User Protection. 0 - Off, 1 - On. Default is Off
# Number: 0, 1
# Mandatory
P9996 = 0

# 3CX Auto Provision. 0 - No, 1 - Yes. Default is Yes
# Number: 0, 1
# Mandatory
P1414 = 1

####################################################################
# Upgrade and Provisioning/Advanced Settings
####################################################################
# Validate Hostname in Certificate. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
P22030 = 0

# Enable SIP NOTIFY Authentication. 0 - Yes, 1 - No. Default is 1
# Number: 0,1
# Mandatory
P4428 = 0

####################################################################
# System Diagnosis                                                ##
####################################################################
####################################################################
# System Diagnosis/Syslog
####################################################################
# Syslog Protocol. 0 - UDP, 1 - SSL/TLS. Default is 0
# Number: 0, 1
# Mandatory
P8402 = 0

# Syslog Server (name of the server, max length is 64 characters)
# String
P207 =

# Syslog Level. 0 - NONE, 1 - DEBUG, 2 - INFO, 3 - WARNING, 4 - ERROR. Default is 0
# Number: 0, 1, 2, 3, 4
# Mandatory
P208 = 0

# Syslog Keyword Filtering
# String
P22129 = 

# Send SIP Log. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P1387 = 0

####################################################################
# System Diagnosis/Packet Capture
####################################################################
# With RTP Packets. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P6007 = 0

##############################################################################
# System Diagnosis/Outbound Notification
##############################################################################
######################################################################################
# Action URL
######################################################################################
# Setup Completed. 
# String
P8304 = 

# Registered.
# String
P8305 = 

# Unregistered.
# String
P8306 = 

# Off-Hook.
# String
P8308 = 

# On-Hook.
# String
P8309 = 

# Incoming Call.
# String
P8310 = 

# Outgoing Call
# String
P8311 = 

# Missed Call
# String
P8312 = 

# Established Call
# String 
P8313 = 

# Terminated Call
# String
P8314 = 

# Enable DND
# String
P8316 = 

# Disable DND
# String
P8317 = 

# Enable Call Forward
# String
P8318 = 

# Disable Call Forward
# String
P8319 = 

# Blind Transfer
# String
P8320 = 

# Attended Transfer
# String
P8321 = 

# Hold Call
# String
P8324 = 

# Unhold Call
# String
P8325 = 

####################################################################
# Voice Monitoring                                                ##
####################################################################
####################################################################
# Voice Monitoring/Session Report
####################################################################
# VQ RTCP-XR Session Report. 0 - Disabled, 1 - Enabled. Default is 0
# Number: 0, 1
P8489 = 0

####################################################################
# Voice Monitoring/Interval Report
####################################################################
# VQ RTCP-XR Interval Report. 0 - Disabled, 1 - Enabled. Default is 0
# Number: 0, 1
P8490 = 0

# VQ RTCP-XR Interval Report Period. 1 - 5, 2 - 10, 3 - 15, 4 - 20. Default is 4
# Number: 1, 2, 3, 4
P8491 = 4

####################################################################
# Voice Monitoring/Alert Report
####################################################################
# Warning Threshold for Moslq
# String
P8492 = 0

# Critical Threshold for Moslq
# String
P8493 = 0

# Warning Threshold for Delay
# String
P8494 = 0

# Critical Threshold for Delay
# String
P8495 = 0

####################################################################
# Application                                                     ##
####################################################################
####################################################################
# Application/Web Service
####################################################################
# Use Auto Location Service. 0 - No, 1 - Yes. Default is 1
# Number: 0, 1
# Mandatory
P8338 = 1

####################################################################
# Application/Contacts
####################################################################
####################################################################
# Application/Contacts/Phonebook Management
####################################################################
# Enable Phonebook XML Download. # 0 - Disabled, 1 - Enabled, use HTTP, 2 - Enabled, use TFTP, 3 - Enabled, use HTTPS. Default is 0
# Number: 0, 1, 2, 3
# Mandatory
P330 = 0

# HTTP/HTTPS User Name
# String
P6713 =

# HTTP/HTTPS Password
# String
P6714 =

# Phonebook XML Server Path
# This is a string of up to 256 characters that should contain a path to the XML file. It MUST be in the host/path format.
# For example: directory.grandstream.com/engineering
# String
P331 =

# Phonebook Download Interval (in minutes)
# Valid value range is 5-720. Default is 0 for disabled
# Number: 0, 5-720; 
P332 = 0

# Remove Manually-edited Entries on Download. 0 - No, 1 - Yes. Default is 1
# Number: 0, 1
# Mandatory
P333 = 1

# Import Group Method. 0 - Replace, 1 - Append. Default is 0
# Number: 0, 1
# Mandatory
P8462 = 0

# Sort Phonebook by. 0 - Last Name, 1 - First Name. Default is 0
# Number: 0, 1
# Mandatory
P2914 = 0

# Default Search Mode. 0 - Quick match, 1 - Exact match. Default is 0
# Number: 0, 1.
# Mandatory
P2970 = 0

####################################################################
# Application/LDAP
####################################################################
# LDAP Protocol. 0 - LDAP, 1 - LDAPS
# Number: 0,1
# Mandatory
P8037 = 0

# LDAP Server Address, up to 256 characters can be used. It can be IP address or Domain name
# String
P8020 = 

# LDAP Server Port. Default is 389.
# Number: 1 - 65535
P8021 = 389

# Base DN. The LDAP search base refers to the location in the directory where the search is requested to begin
# Example 1: dc=grandstream,dc=com
# Example 2: ou=Boston, dc=grandstream,dc=com
# String
P8022 =

# Username. The bind "Username" for querying LDAP servers. Some LDAP servers allow anonymous binds in which case the setting can be left blank
# String
P8023 =

# Password. The bind "Password" for querying LDAP servers. And the field can be left blank if the LDAP server allows anonymous binds
# String
P8024 =

# LDAP Number Filter
# LDAP name filter is the filter used for name look ups. Please refer to user manual for examples
# String
P8025 =

# LDAP Name Filter
# LDAP name filter is the filter used for name look ups. Please refer to user manual for examples
# String
P8026 =

# LDAP Version. Protocol version for the phone when send the bind requests
# 2 - version 2, 3 - version 3. Default is 3
# Mandatory
P8027 = 3

# LDAP Name Attributes. This setting specifies the "name" attributes of each record which are returned in the LDAP search result
# The setting allows the users to configure multiple space separated name attributes
# String
P8028 =

# LDAP Number Attributes. This setting specifies the "number" attributes of each record which are returned in the LDAP search result
# The setting allows the users to configure multiple space separated number attributes
# String
P8029 =

# LDAP Display Name. The entry information to be shown on phone LCD. Grandstream phones will display up to 3 fields
# String
P8030 =

# Max Hits. The setting specifies the maximum number of results to be returned by the LDAP server
# If the value is set to 0, server will return all search results. Default is 50
# Number: 0 - 32000
# Mandatory
P8031 = 50

# Search Timeout (in seconds). Default is 30
# The setting specifies how long the server should process the request and client waits for server to return
# Number: 0 - 180
# Mandatory
P8032 = 30

# Sort Results. This setting is used for sorting searching result. Default is 0
# Number: 0, 1. 0 - No, 1 - Yes. Default is 0
# Mandatory
P8033 = 0

# LDAP Lookup
# Incoming calls. 0 - No, 1 - Yes. Default is 0
P8035 = 0

# Outgoing calls. 0 - No, 1 - Yes. Default is 0
P8034 = 0

# Lookup Display Name
# String
P8036 =

# LDAP Dialing Default Account
# -1 - Auto, 0 - Account 1, 1 - Account 2, 2 - Account 3, 3 - Account 4, 4 - Account 5, 5 - Account 6
# Number: -1, 0, 1, 2, 3, 4, 5
P22039 = -1

# Exact Match Search. . 0 - No, 1 - Yes. Default is 0
# Mandatory
P8505 = 0

####################################################################
# External Service                                                ##
####################################################################
####################################################################
# External Service/GDS
####################################################################
###############################################################
# Order 1
###############################################################
# Service Type. 1 - Others, 0 - GDS. Default is 1.
# Number: 1, 0
# Mandatory: 1
P32000 = 1

# Account
# 0 - Account 1, 1 - Account 2, 2 - Account 3, 3 - Account 4, 4 - Account 5, 5 - Account 6
# Number: 0, 1, 2, 3, 4, 5. Default is 0.
# Mandatory
P32001 = 0

# System Identification
# String
P32002 = 

# System Number
# String
P32003 = 

# Access Password
# String
P32004 = 

# System Ringtone
# 0 - system, 1 - ring1, 2 - ring2, 3 - ring3, 4 - ring4, 5 - ring5, 6 - ring6, 7 - Doorbell, 8 - silent. Default is 0
# Number: 0-8, more if using custom ringtone. Default is 7.
P22241 = 7

###############################################################
# Order 2
###############################################################
# Service Type. 1 - Others, 0 - GDS. Default is 1.
# Number: 1, 0
# Mandatory: 1
P32005 = 1

# Account
# 0 - Account 1, 1 - Account 2, 2 - Account 3, 3 - Account 4, 4 - Account 5, 5 - Account 6
# Number: 0, 1, 2, 3, 4, 5. Default is 0.
# Mandatory
P32006 = 0

# System Identification
# String
P32007 = 

# System Number
# String
P32008 = 

# Access Password
# String
P32009 = 

# System Ringtone
# 0 - system, 1 - ring1, 2 - ring2, 3 - ring3, 4 - ring4, 5 - ring5, 6 - ring6, 7 - Doorbell, 8 - silent. Default is 0
# Number: 0-8, more if using custom ringtone. Default is 7.
P22242 = 7

###############################################################
# Order 3
###############################################################
# Service Type. 1 - Others, 0 - GDS. Default is 1.
# Number: 1, 0
# Mandatory: 1
P32010 = 1

# Account
# 0 - Account 1, 1 - Account 2, 2 - Account 3, 3 - Account 4, 4 - Account 5, 5 - Account 6
# Number: 0, 1, 2, 3, 4, 5. Default is 0.
# Mandatory
P32011 = 0

# System Identification
# String
P32012 = 

# System Number
# String
P32013 = 

# Access Password
# String
P32014 = 

# System Ringtone
# 0 - system, 1 - ring1, 2 - ring2, 3 - ring3, 4 - ring4, 5 - ring5, 6 - ring6, 7 - Doorbell, 8 - silent. Default is 0
# Number: 0-8, more if using custom ringtone. Default is 7.
P22243 = 7

###############################################################
# Order 4
###############################################################
# Service Type. 1 - Others, 0 - GDS. Default is 1.
# Number: 1, 0
# Mandatory: 1
P32015 = 1

# Account
# 0 - Account 1, 1 - Account 2, 2 - Account 3, 3 - Account 4, 4 - Account 5, 5 - Account 6
# Number: 0, 1, 2, 3, 4, 5. Default is 0.
# Mandatory
P32016 = 0

# System Identification
# String
P32017 = 

# System Number
# String
P32018 = 

# Access Password
# String
P32019 = 

# System Ringtone
# 0 - system, 1 - ring1, 2 - ring2, 3 - ring3, 4 - ring4, 5 - ring5, 6 - ring6, 7 - Doorbell, 8 - silent. Default is 0
# Number: 0-8, more if using custom ringtone. Default is 7.
P22244 = 7

###############################################################
# Order 5
###############################################################
# Service Type. 1 - Others, 0 - GDS. Default is 1.
# Number: 1, 0
# Mandatory: 1
P32020 = 1

# Account
# 0 - Account 1, 1 - Account 2, 2 - Account 3, 3 - Account 4, 4 - Account 5, 5 - Account 6
# Number: 0, 1, 2, 3, 4, 5. Default is 0.
# Mandatory
P32021 = 0

# System Identification
# String
P32022 = 

# System Number
# String
P32023 = 

# Access Password
# String
P32024 = 

# System Ringtone
# 0 - system, 1 - ring1, 2 - ring2, 3 - ring3, 4 - ring4, 5 - ring5, 6 - ring6, 7 - Doorbell, 8 - silent. Default is 0
# Number: 0-8, more if using custom ringtone. Default is 7.
P22245 = 7

###############################################################
# Order 6
###############################################################
# Service Type. 1 - Others, 0 - GDS. Default is 1.
# Number: 1, 0
# Mandatory: 1
P32025 = 1

# Account
# 0 - Account 1, 1 - Account 2, 2 - Account 3, 3 - Account 4, 4 - Account 5, 5 - Account 6
# Number: 0, 1, 2, 3, 4, 5. Default is 0.
# Mandatory
P32026 = 0

# System Identification
# String
P32027 = 

# System Number
# String
P32028 = 

# Access Password
# String
P32029 = 

# System Ringtone
# 0 - system, 1 - ring1, 2 - ring2, 3 - ring3, 4 - ring4, 5 - ring5, 6 - ring6, 7 - Doorbell, 8 - silent. Default is 0
# Number: 0-8, more if using custom ringtone. Default is 7.
P22246 = 7

###############################################################
# Order 7
###############################################################
# Service Type. 1 - Others, 0 - GDS. Default is 1.
# Number: 1, 0
# Mandatory: 1
P32030 = 1

# Account
# 0 - Account 1, 1 - Account 2, 2 - Account 3, 3 - Account 4, 4 - Account 5, 5 - Account 6
# Number: 0, 1, 2, 3, 4, 5. Default is 0.
# Mandatory
P32031 = 0

# System Identification
# String
P32032 = 

# System Number
# String
P32033 = 

# Access Password
# String
P32034 = 

# System Ringtone
# 0 - system, 1 - ring1, 2 - ring2, 3 - ring3, 4 - ring4, 5 - ring5, 6 - ring6, 7 - Doorbell, 8 - silent. Default is 0
# Number: 0-8, more if using custom ringtone. Default is 7.
P22247 = 7

###############################################################
# Order 8
###############################################################
# Service Type. 1 - Others, 0 - GDS. Default is 1.
# Number: 1, 0
# Mandatory: 1
P32035 = 1

# Account
# 0 - Account 1, 1 - Account 2, 2 - Account 3, 3 - Account 4, 4 - Account 5, 5 - Account 6
# Number: 0, 1, 2, 3, 4, 5. Default is 0.
# Mandatory
P32036 = 0

# System Identification
# String
P32037 = 

# System Number
# String
P32038 = 

# Access Password
# String
P32039 = 

# System Ringtone
# 0 - system, 1 - ring1, 2 - ring2, 3 - ring3, 4 - ring4, 5 - ring5, 6 - ring6, 7 - Doorbell, 8 - silent. Default is 0
# Number: 0-8, more if using custom ringtone. Default is 7.
P22248 = 7

###############################################################
# Order 9
###############################################################
# Service Type. 1 - Others, 0 - GDS. Default is 1.
# Number: 1, 0
# Mandatory: 1
P32040 = 1

# Account
# 0 - Account 1, 1 - Account 2, 2 - Account 3, 3 - Account 4, 4 - Account 5, 5 - Account 6
# Number: 0, 1, 2, 3, 4, 5. Default is 0.
# Mandatory
P32041 = 0

# System Identification
# String
P32042 = 

# System Number
# String
P32043 = 

# Access Password
# String
P32044 = 

# System Ringtone
# 0 - system, 1 - ring1, 2 - ring2, 3 - ring3, 4 - ring4, 5 - ring5, 6 - ring6, 7 - Doorbell, 8 - silent. Default is 0
# Number: 0-8, more if using custom ringtone. Default is 7.
P22249 = 7

###############################################################
# Order 10
###############################################################
# Service Type. 1 - Others, 0 - GDS. Default is 1.
# Number: 1, 0
# Mandatory: 1
P32045 = 1

# Account
# 0 - Account 1, 1 - Account 2, 2 - Account 3, 3 - Account 4, 4 - Account 5, 5 - Account 6
# Number: 0, 1, 2, 3, 4, 5. Default is 0.
# Mandatory
P32046 = 0

# System Identification
# String
P32047 = 

# System Number
# String
P32048 = 

# Access Password
# String
P32049 = 

# System Ringtone
# 0 - system, 1 - ring1, 2 - ring2, 3 - ring3, 4 - ring4, 5 - ring5, 6 - ring6, 7 - Doorbell, 8 - silent. Default is 0
# Number: 0-8, more if using custom ringtone. Default is 7.
P22250 = 7

####################################################################
# External Service/Call Center
####################################################################
# Wrap-up Countdown (m). Default is 6.
# Number
P22378 = 6

####################################################################
# External Service/Broadsoft XSI
####################################################################
####################################################################
# Authentication Login
####################################################################
# XSI
# Server
# String
P1591 =

# Port
# Number
P1592 =

# XSI Actions Path
# String
P2937 =

# XSI Authentication Type. 0 - Login Credentials, 1 - SIP Credentials, 2 - Account 1, 3 - Account 2, 4 - Account 3, 5 - Account 4, 6 - Account 5, 7 - Account 6. 
# Number: 0, 1, 2, 3, 4, 5, 6, 7. Default is 0.
# Mandatory
P22054 = 0

# Login Credentials
# BroadWorks User ID
# String
P1593 = 

# Login Password
# String
P1594 = 

# Aut0 Login. 0 - No, 1 - Yes. Default is 0.
# Number: 0, 1
# Mandatory
P22379 = 0

####################################################################
# Service Settings
####################################################################
# Sort Phonebook by. 0 - Last Name, 1 - First Name. Default is 0.
# Number: 0, 1
# Mandatory
P22131 = 0

# Broadsoft Directory Update Interval(m)
# Number: 0, 5-4320
# Mandatory
P8362 = 4320

# Broadsoft Contacts Download Limit.
# Number: 0-2000. Default is 1000
# Mandatory
P8464 = 1000

# Broadsoft Contacts Search Limit
# Number: 0 - 2000. Default is 100
P8465 = 100

####################################################################
# Network Directories
####################################################################
### Group Directory ###
# Disabled/Enabled. 0 - Disabled, 1 - Enabled.
# Number: 0, 1. Default is 0
# Mandatory
P2971 = 0

# Name. 
# String
P2972 = 

### Enterprise Directory ###
# Disabled/Enabled. 0 - Disabled, 1 - Enabled.
# Number: 0, 1. Default is 0
# Mandatory
P2973 = 0

# Name. 
# String
P2974 = 

### Group Common ###
# Disabled/Enabled. 0 - Disabled, 1 - Enabled.
# Number: 0, 1. Default is 0
# Mandatory
P2975 = 0

# Name. 
# String
P2976 = 

### Enterprise Common ###
# Disabled/Enabled. 0 - Disabled, 1 - Enabled.
# Number: 0, 1. Default is 0
# Mandatory
P2977 = 0

# Name. 
# String
P2978 =

### Personal Directory ###
# Disabled/Enabled. 0 - Disabled, 1 - Enabled.
# Number: 0, 1. Default is 0
# Mandatory
P2979 = 0

# Name. 
# String
P2980 =

### Missed Call Log ### 
# Disabled/Enabled. 0 - Disabled, 1 - Enabled.
# Number: 0, 1. Default is 0
# Mandatory
P2981 = 0

# Name. 
# String
P2982 =

### Placed Call Log ### 
# Disabled/Enabled. 0 - Disabled, 1 - Enabled.
# Number: 0, 1. Default is 0
# Mandatory
P2983 = 0

# Name. 
# String
P2984 =

### Received Call Log ### 
# Disabled/Enabled. 0 - Disabled, 1 - Enabled.
# Number: 0, 1. Default is 0
# Mandatory
P2985 = 0

# Name. 
# String
P2986 =
