################################################################################################
## Configuration Template For WP820 Version 1.0.7.15                                          ##
################################################################################################

####################################################################
# Account Settings                                                ##
####################################################################
####################################################################
# Account 1                                                       ##
####################################################################
###############################################################
# Account 1/General Settings
###############################################################
# Account Registration

# Account Active. 0 - No, 1 - Yes. Default is 1
# Number: 0, 1
# Mandatory
P271 = 1

# Account Name
# String
P270 =

# SIP Server
# String
P47 =

# Secondary SIP Server
# String
P50602 =
P50702 =
P50802 =
P50902 =

# SIP User ID
# String
P35 =

# SIP Authenticate ID
# String
P36 =

# SIP Authenticate Password
# String
P34 =

# Name
# String
P3 =

# TEL URI. 0 - Disabled, 1 - User=Phone, 2 - Enabled. Default is 0
# Number: 0, 1, 2
# Mandatory
P63 = 0

# Voice Mail Access Number
# String
P33 =

# Network Settings

# Outbound Proxy
# String
P48 =

# Secondary Outbound Proxy
# String
P2333 = 

# DNS Mode. 0 - A Record, 1 - SRV, 2 - NAPTR/SRV. Default is 0
# Number: 0, 1, 2, 3
# Mandatory
P103 = 0

# DNS SRV Fail-over Mode. 0 - Default, 1 - Saved one until DNS TTL, 2 - Saved one until no response. Default is 0
# Number: 0,1,2
# Mandatory
P26040 = 0

# NAT Traversal. 0 - No, 1 - STUN, 2 - keep alive, 4 - Auto, 5 - VPN. Default is 0.
# Number: 0, 1, 2, 3, 4, 5
# Mandatory
P52 = 0

# Proxy-Require (A SIP extension to enable firewall penetration). Max length is 64 characters
# String
P197 =

###############################################################
# Account 1/SIP Settings
###############################################################
# SIP Basic Settings

# SIP Registration. 0 - No, 1 - Yes. Default is 1
# Number: 0, 1
# Mandatory
P31 = 1

# Unregister On Reboot. 0 - No, 1 - Yes, 2 - Instance. Default is 2
# Number: 0, 1
# Mandatory
P81 = 2

# Register Expiration (in minutes). Default is 60. Max about 45 days
# Number: 1 - 64800
# Mandatory
P32 = 60

# Subscribe Expiration (in minutes). Default is blank.
# Number: 1 - 64800
P26051 =

# Re-register Before Expiration (in seconds). Default is 0 second
# Number: 0 - 64800
# Mandatory
P2330 = 0

# Registration Retry Wait Time (in seconds). Default is 20
# Number: 1 - 3600
# Mandatory
P138 = 20

# Add Auth Header On Initial REGISTER
# 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P2359 = 0

# Enable OPTIONS Keep Alive. 0 - No, 1 - Yes. Default is 0
# Number: 0,1
# Mandatory
P2397 = 0

# SIP OPTIONS Keep Alive Interval (s). Default is 30
# Number: 1 - 64800
# Mandatory
P2398 = 30

# SIP OPTIONS Keep Alive Max Tries. Default is 3
# Number: 3 - 10
# Mandatory
P2399 = 3

# SUBSCRIBE for MWI (Whether or not send SUBSCRIBE for Message Waiting Indication). 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P99 = 0

# Use Privacy Header
# 0 - Default, 1 - No, 2 - Yes. Default is 0
# Number: 0, 1, 2
# Mandatory
P2338 = 0

# Use P-Preferred-Identity Header
# 0 - Default, 1 - No, 2 - Yes. Default is 0
# Number: 0, 1, 2
# Mandatory
P2339 = 0

# Use P-Access-Network-Info Header. 0 - No, 1 - Yes. Default is 0.
# Number: 0, 1
P26058 = 0

# Use P-Emergency-Info header. 0 - No, 1 - Yes. Default is 0.
# Number: 0, 1
P26059 = 0

# Use MAC Header. 0 - No, 1 - Yes except REGISTER, 2 - Yes to all SIP. Default is 0.
# Number: 0, 1, 2
P29090 = 2

# Add MAC in User-Agent. 0 - No, 1 - Yes except REGISTER, 2 - Yes to all SIP. Default is 0.
# Number: 0, 1, 2
P26061 = 1

# SIP Transport. 0 - UDP, 1 - TCP, 2 - TLS/TCP. Default is 0
# Number: 0, 1, 2
# Mandatory
P130 = 0

# Local SIP Port. Default is 5060
# Number: 0 - 65535
# Mandatory
P40 = 5060

# SIP URI Scheme when using TLS. 0 - sip, 1 - sips. Default is 0
# Number: 0, 1
# Mandatory
P2329 = 0

# Use Actual Ephemeral Port in Contact with TCP/TLS. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P2331 = 0

# Support SIP Instance ID. 0 - No, 1 - Yes. Default is 1
# Number: 0, 1
# Mandatory
P288 = 1

# SIP T1 Timeout. RFC 3261 T1 value (RTT estimate)
# 50 - 0.5 sec, 100 - 1 sec, 200 - 2 sec. Default is 50
# Number: 50, 100, 200
# Mandatory	
P209 = 50

# SIP T2 Interval
# 200 - 2 sec, 400 - 4 sec, 800 - 8 sec. Default is 400
# Number: 200, 400, 800
# Mandatory
P250 = 400

# SIP Timer D Interval
# Number: 0 - 64
# Mandatory
P2387 = 0

# Remove OBP from Route. 0 - Disable, 1 - Enable, 2 - Always. Default is 0 
# Number: 0, 1, 2 
# Mandatory
P2305 = 0

# Enable 100rel. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P272 = 0

# Enable Session Timer/ Session Expiration(s).  In seconds. Default value is 180 seconds.
# By default,  Session Timer is Enabled.  Session Timer is disabled if the value is 0.
# Number: 0 or 90 - 64800
P260 = 180

# Minimum SE (in seconds). Default is 90. This value must be lower than or equal to P260
# Number: 90 - 64800
# Mandator
P261 = 90

# UAC Specify Refresher. 0 - Omit, 1 - UAC, 2 - UAS. Default is 0
# Number: 0, 1, 2
# Mandatory
P266 = 0

# UAS Specify Refresher. 1 - UAC, 2 - UAS. Default is 1
# Number: 1, 2
# Mandatory
P267 = 1

# Caller Request Timer (Request for timer when calling). 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P262 = 0

# Callee Request Timer (Request for timer when called. i.e. if remote party supports timer but did not request for one)
# 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P263 = 0

# Force Timer (Still use timer when remote party does not support timer). 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P264 = 0

# Force INVITE (Always refresh with INVITE instead of UPDATE even when remote party supports UPDATE).
# 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P265 = 0

###############################################################
# Account 1/Codec Settings
###############################################################
# Account 1/Preferred Vocoder

# Preferred Vocoder   
# 0 - PCMU, 8 - PCMA, 9 - G722, 18 - G729A/B, 98 - iLBC, 123 - Opus
# Number: 0, 8, 9, 18, 98, 123     

# (For selected Vocoder)
# choice 1. Default is 0
# Number: 0, 8, 9, 18, 98, 123
# Mandatory
P57 = 0

# choice 2. Default is 8
# Number: 0, 8, 9, 18, 98, 123
# Mandatory
P58 = 8

# choice 3. Default is 9
# Number: 0, 8, 9, 18, 98, 123
# Mandatory
P59 = 9

# choice 4. Default is 9
# Number: 0, 8, 9, 18, 98, 123
# Mandatory
P60 = 9

# choice 5. Default is 9
# Number: 0, 8, 9, 18, 98, 123
# Mandatory
P61 = 9

# choice 6. Default is 9
# Number: 0, 8, 9, 18, 98, 123
# Mandatory
P62 = 9

# choice 7. Default is 9
# Number: 0, 8, 9, 18, 98, 123
# Mandatory
P46 = 9

# choice 8. Default is 9
# Number: 0, 8, 9, 18, 98, 123
# Mandatory
P98 = 9

# Codec Negotiation Priority. 0 - Caller, 1 - Callee. Default is 1
# Number: 0, 1
# Mandatory
P29061 = 1

# Use First Matching Vocoder in 200OK SDP. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P2348 = 0

# iLBC Frame Size. 0 - 20ms, 1 - 30ms. Default is 1
# Number: 0, 1
# Mandatory
P97 = 1

# OPUS Payload Type. Default is 123
# Number: 96 - 127
# Mandatory
P2385 = 123

# Send DTMF: In-audio. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P2301 = 0

# Send DTMF: Via RTP (RFC2833). 0 - No, 1 - Yes. Default is 1
# Number: 0, 1
# Mandatory
P2302 = 1

# Send DTMF: Via SIP INFO. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P2303 = 0

# DTMF Payload Type. Default is 101
# Number: 96 - 127
# Mandatory
P79 = 101

# Enable Audio RED with FEC. 0 - Disabled, 1 - Enabled. Default is 0
# Number: 0, 1
# Mandatory
P26073 = 0

# Audio FEC Payload Type. Default is 121
# Number: 96 to 127 (extra limit:  97, 98, 99, 127 are invalid values, and the value can't be the same as the Audio RED Payload Type)
# Mandatory
P26074 = 121

# Audio RED Payload Type. Default is 124 
# Number: 96 to 127 (extra limit:  97, 98, 99, 127 are invalid values, and the value can't be the same as the Audio FEC Payload Type)
# Mandatory
P26075 = 124

# Silence Suppression. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P50 = 0

# Voice Frames per TX (up to 10/20/32/64 frames for G711/G726/G723/other codecs respectively). Default is 2
# Number: 1 - 64
# Mandatory
P37 = 2

# Account 1/Preferred Video Codec

# Preferred Video Codec. 99 - H264. Default is 99. 
# Number: 99
P295 = 99

# Enable Video FEC. 0 - No, 1 - Yes. Default value is 1.
# Number: 0, 1
P2393 = 1

# Enable RFC5168 Support. 0 - No, 1 - Yes. Default value is 1.
# Number: 0, 1
P1331 = 1

# FEC Payload Type. Default value is 120.
# Number: 96 - 126
P2394 = 120

# H.264 Image Size. 9 - 720P, 1 - VGA, 5 - CIF, 4 - 4CIF, 0 - QVGA, 6 - QCIF. Default value is 9
# Number: 9, 1, 5, 4, 0, 6
P2307 = 9

# Video Bit Rate. 32 - 32 kbps, 64 - 64 kbps, 96 - 96 kbps, 128 - 128 kbps, 160 - 160 kbps, 192 - 192 kbps
# 210 - 210 kbps, 256 - 256 kbps, 384 - 384 kbps, 512 - 512 kbps, 640 - 640 kbps, 768 - 768 kbps
# 1024 - 1024 kbps, 1280 - 1280 kbps, 1536 - 1536 kbps, 2048 - 2048 kbps. Default value is 2048.
# Number: 32,64,96,128,160,192,210,256,384,512,640,768,1024,1280,1536,2048
P2315 = 2048

# SDP Bandwidth Attribute. 0 - Standard, 1 - Media Level, 2 - Session Level, 3 - None. Default value is Media Level.
# Number: 0, 1, 2, 3
P2360 = 1

# Account 1/RTP Settings

# SRTP Mode. 0 - Disabled, 1 - Enabled but not forced, 2 - Enabled and forced. Default is 0
# Number: 0, 1, 2
# Mandatory
P183 = 0

# SRTP Key Length. 0 - AES 128&256 bit, 1 - AES 128 bit, 2 - AES 256 bit. Default is 0
# Default is 0
# Number: 0, 1, 2
# Mandatory
P2383 = 0

# Enable SRTP Key Life Time. 0 - No, 1 - Yes. Default is 1
# Number: 0, 1
# Mandatory
P2363 = 1

# RTCP Destination
# Strings
P2390 = 

# Symmetric RTP. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P291 = 0

# RTP IP Filter. 0 - Disable, 1 - IP Only, 2 - IP and Port. Default is 0
# Number: 0, 1, 2
# Mandatory
P26026 = 0

# RTP Timeout (in seconds). Default is 30.
# Number: 0 - 600
P29068 = 30

###############################################################
# Account 1/Call Settings
###############################################################
# Call Features

# Start Video Automatically. 0 - Disable, 1 - Enable. Default is 1.
# Number: 0, 1
P2314 = 0

# Auto Answer.  0 - No, 1 - Yes, 2 - Enable Intercom/Paging 
# Number: 0, 1, 2. Default is 0
# Mandatory
P90 = 0 

# Play warning tone for Auto Answer Intercom. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P26072 = 0

# Intercom Barging. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P26019 = 0

# Send Anonymous (caller ID will be blocked if set to Yes). 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P65 = 0

# Anonymous Call Rejection. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P129 = 0

# Call Log. 0 - Log All Calls, 1 - Log Incoming/Outgoing only (Missed calls NOT recorded), 2 - Disable Call Log, 3 - Do Not Prompt Missed Call. Default is 0
# Number: 0, 1, 2
# Mandatory
P182 = 0

# Enable Call Features.  0 - No, 1 - Yes. Default is 0
# Number: 0, 1 
# Mandatory
P191 = 0

# Mute on Answer Intercom Call. 0 - Off, 1 - On. Default is 1.
# Number: 0, 1
P26071 = 0

# Transfer on 3 Way Conference Hangup.  0 - Disabled, 1 - Enabled. Default is 0
# Number: 0, 1 
# Mandatory
P2304 = 0

# Use # As Dial Key. 0 - No, 1 - Yes
# Number: 0, 1
# Mandatory
P72 = 1

# DND Call Feature On
# String
P2344 = 

# DND Call Feature Off
# String
P2345 = 

# No Key Entry Timeout (in seconds). Default is 4
# Number: 1 - 15
# Mandatory
P85 = 4

# Ring Timeout (in seconds). Default is 60
# Number: 10 - 300
# Mandatory
P1328 = 60

# Refer-To Use Target Contact. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P135 = 0

# RFC2543 Hold. 0 - No, 1 - Yes. Default is 1
# Number: 0, 1
# Mandatory
P26062 = 0

# Call Forward Type (Cannot be provisioned by config template currently)

# Dial Plan

# Dial Plan Prefix
# String
P66 = 

# Disable DialPlan. 0 - No Selection, 1 - Dial Page, 2 - Contact, 4 - Incoming Call History, 8 -  Outgoing Call History. 
# If need to check multiple selections, add the specific values for each selections together. Default value is 0
# Number: 0-31
P2382 = 0

# Dial Plan. Default is { x+ | \+x+ | *x+ | *xx*x+ | x+*x+*x+*x+ | x+*x+*x+*x+#x+ }.
# String
# Mandatory
P290 = { x+ | \+x+ | *x+ | *xx*x+ | x+*x+*x+*x+ | x+*x+*x+*x+#x+ }

# Caller IDs

# Caller ID Display. 0 - Auto, 1 - Disabled, 2 - From Header. Default is 0
# Number: 0, 1, 2
# Mandatory
P2324 = 0

##########################Ringtone Value Table###################################
# Default						content://settings/system/ringtone
# Silent						ringtone_silence
# Andromeda						/system/media/audio/ringtones/ANDROMEDA.ogg
# Aquila						/system/media/audio/ringtones/Aquila.ogg
# Argo Navi						/system/media/audio/ringtones/ArgoNavis.ogg
# Atria							/system/media/audio/ringtones/Atria.ogg
# Backroad						/system/media/audio/ringtones/Backroad.ogg
# Beat Plucker					/system/media/audio/ringtones/BeatPlucker.ogg
# Bell Phone					/system/media/audio/ringtones/Ring_Classic_02.ogg
# Bentley Dubs					/system/media/audio/ringtones/BentleyDubs.ogg
# Big Easy						/system/media/audio/ringtones/Big_Easy.ogg
# Bird Loop						/system/media/audio/ringtones/BirdLoop.ogg
# Bollywood						/system/media/audio/ringtones/Bollywood.ogg
# BoÃ¶tes						/system/media/audio/ringtones/BOOTES.ogg
# Bus' a Move					/system/media/audio/ringtones/BussaMove.ogg
# Cairo							/system/media/audio/ringtones/Cairo.ogg
# Calypso Steel					/system/media/audio/ringtones/Calypso_Steel.ogg
# Canis Major					/system/media/audio/ringtones/CANISMAJOR.ogg
# Caribbean Ice					/system/media/audio/ringtones/CaribbeanIce.ogg
# Carina						/system/media/audio/ringtones/Carina.ogg
# Cassiopeia					/system/media/audio/ringtones/CASSIOPEIA.ogg
# Centaurus						/system/media/audio/ringtones/Centaurus.ogg
# Champagne Edition				/system/media/audio/ringtones/Champagne_Edition.ogg
# Chimey Phone					/system/media/audio/ringtones/Ring_Synth_02.ogg
# Club Cubano					/system/media/audio/ringtones/Club_Cubano.ogg
# Crayon Rock					/system/media/audio/ringtones/CrayonRock.ogg
# Crazy Dream					/system/media/audio/ringtones/CrazyDream.ogg
# Curve Ball Blend				/system/media/audio/ringtones/CurveBall.ogg
# Cygnus						/system/media/audio/ringtones/Cygnus.ogg
# Dancin' Fool					/system/media/audio/ringtones/DancinFool.ogg
# Digital Phone					/system/media/audio/ringtones/Ring_Digital_02.ogg
# Ding							/system/media/audio/ringtones/Ding.ogg
# DingDong						/system/media/audio/ringtones/DingDong.wav
# Don' Mess Wiv It				/system/media/audio/ringtones/DonMessWivIt.ogg
# Draco							/system/media/audio/ringtones/Draco.ogg
# Dream Theme					/system/media/audio/ringtones/DreamTheme.ogg
# Eastern Sky					/system/media/audio/ringtones/Eastern_Sky.ogg
# Enter the Nexus				/system/media/audio/ringtones/Enter_the_Nexus.ogg
# Eridani						/system/media/audio/ringtones/Eridani.ogg
# Ether Shake					/system/media/audio/ringtones/EtherShake.ogg
# Flutey Phone					/system/media/audio/ringtones/Ring_Synth_04.ogg
# Free Flight					/system/media/audio/ringtones/FreeFlight.ogg
# Friendly Ghost				/system/media/audio/ringtones/FriendlyGhost.ogg
# Funk Y'all					/system/media/audio/ringtones/Funk_Yall.ogg
# Game Over Guitar				/system/media/audio/ringtones/GameOverGuitar.ogg
# Gimme Mo' Town				/system/media/audio/ringtones/Gimme_Mo_Town.ogg
# Girtab						/system/media/audio/ringtones/Girtab.ogg
# Glacial Groove				/system/media/audio/ringtones/Glacial_Groove.ogg
# Growl							/system/media/audio/ringtones/Growl.ogg
# Halfway Home					/system/media/audio/ringtones/HalfwayHome.ogg
# Hydra							/system/media/audio/ringtones/Hydra.ogg
# Insert Coin					/system/media/audio/ringtones/InsertCoin.ogg
# Kuma							/system/media/audio/ringtones/Kuma.ogg
# Loopy Lounge					/system/media/audio/ringtones/LoopyLounge.ogg
# Love Flute					/system/media/audio/ringtones/LoveFlute.ogg
# Lyra							/system/media/audio/ringtones/Lyra.ogg
# Machina						/system/media/audio/ringtones/Machina.ogg
# Medieval Jaunt				/system/media/audio/ringtones/MidEvilJaunt.ogg
# Mildly Alarming				/system/media/audio/ringtones/MildlyAlarming.ogg
# Nairobi						/system/media/audio/ringtones/Nairobi.ogg
# Nassau						/system/media/audio/ringtones/Nassau.ogg
# New Player					/system/media/audio/ringtones/NewPlayer.ogg
# No Limits						/system/media/audio/ringtones/No_Limits.ogg
# Noisey One					/system/media/audio/ringtones/Noises1.ogg
# Organ Dub						/system/media/audio/ringtones/OrganDub.ogg
# Orion							/system/media/audio/ringtones/Orion.ogg
# Paradise Island				/system/media/audio/ringtones/Paradise_Island.ogg
# Pegasus						/system/media/audio/ringtones/Pegasus.ogg
# Perseus						/system/media/audio/ringtones/PERSEUS.ogg
# Playa							/system/media/audio/ringtones/Playa.ogg
# Pyxis							/system/media/audio/ringtones/Pyxis.ogg
# Rasalas						/system/media/audio/ringtones/Rasalas.ogg
# Revelation					/system/media/audio/ringtones/Revelation.ogg
# Rigel							/system/media/audio/ringtones/Rigel.ogg
# Road Trip						/system/media/audio/ringtones/Road_Trip.ogg
# Romancing The Tone			/system/media/audio/ringtones/RomancingTheTone.ogg
# Safari						/system/media/audio/ringtones/Safari.ogg
# Savannah						/system/media/audio/ringtones/Savannah.ogg
# Scarabaeus					/system/media/audio/ringtones/Scarabaeus.ogg
# Sceptrum						/system/media/audio/ringtones/Sceptrum.ogg
# Seville						/system/media/audio/ringtones/Seville.ogg
# She's All That				/system/media/audio/ringtones/Shes_All_That.ogg
# Silky Way						/system/media/audio/ringtones/SilkyWay.ogg
# Sitar Versus Sitar			/system/media/audio/ringtones/SitarVsSitar.ogg
# Solarium						/system/media/audio/ringtones/Solarium.ogg
# Springy Jalopy				/system/media/audio/ringtones/SpringyJalopy.ogg
# Steppin' Out					/system/media/audio/ringtones/Steppin_Out.ogg
# Terminated					/system/media/audio/ringtones/Terminated.ogg
# Terrible Twos					/system/media/audio/ringtones/Noises2.ogg
# Testudo						/system/media/audio/ringtones/Testudo.ogg
# Themos						/system/media/audio/ringtones/Themos.ogg
# Third Eye						/system/media/audio/ringtones/Third_Eye.ogg
# Thriller Three				/system/media/audio/ringtones/Noises3.ogg
# Thunderfoot					/system/media/audio/ringtones/Thunderfoot.ogg
# Twirl Away					/system/media/audio/ringtones/TwirlAway.ogg
# Ursa Minor					/system/media/audio/ringtones/URSAMINOR.ogg
# UrsaMinor						/system/media/audio/ringtones/UrsaMinor.ogg
# Very Alarmed					/system/media/audio/ringtones/VeryAlarmed.ogg
# Vespa							/system/media/audio/ringtones/Vespa.ogg
# World							/system/media/audio/ringtones/World.ogg
# Zeta							/system/media/audio/ringtones/Zeta.ogg
# bellcore-dr1					/system/media/audio/ringtones/bellcore-dr1.ogg
# bellcore-dr2					/system/media/audio/ringtones/bellcore-dr2.ogg
# bellcore-dr3					/system/media/audio/ringtones/bellcore-dr3.ogg
# bellcore-dr4					/system/media/audio/ringtones/bellcore-dr4.ogg
# bellcore-dr5					/system/media/audio/ringtones/bellcore-dr5.ogg
# speaker						/system/media/audio/ringtones/speaker.wav

# Ring Tones

# Account Ring Tone
# Mandatory
P104 = content://settings/system/ringtone

# Ignore Alert-Info header
# 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P26018 = 0

# Match Incoming Caller ID Rule 1
# String
P1488 = 

# Distinctive Ringtone Rule 1
# String
P1489 = content://settings/system/ringtone

# Match Incoming Caller ID Rule 2
# String
P1490 = 

# Distinctive Ringtone Rule 2
# String
P1491 = content://settings/system/ringtone

# Match Incoming Caller ID Rule 3
# String
P1492 =

# Distinctive Ringtone Rule 3
# String
P1493 = content://settings/system/ringtone

# Match Incoming Caller ID Rule 4
# String
P6716 = 

# Distinctive Ringtone Rule 4
# String
P6717 = content://settings/system/ringtone

# Match Incoming Caller ID Rule 5
# String
P6718 = 

# Distinctive Ringtone Rule 5
# String
P6719 = content://settings/system/ringtone

# Match Incoming Caller ID Rule 6
# String
P6720 =

# Distinctive Ringtone Rule 6
# String
P6721 = content://settings/system/ringtone

# Match Incoming Caller ID Rule 7
# String
P26064 =

# Distinctive Ringtone Rule 7 
# String
P26065 = content://settings/system/ringtone

# Match Incoming Caller ID Rule 8
# String
P26066 =

# Distinctive Ringtone Rule 8 
# String
P26067 = content://settings/system/ringtone

# Match Incoming Caller ID Rule 9
# String
P26068 =

# Distinctive Ringtone Rule 9
# String
P26069 = content://settings/system/ringtone

# Match Incoming Caller ID Rule 10
# String
P26096 =

# Distinctive Ringtone Rule 10 
# String
P26097 = content://settings/system/ringtone

###############################################################
# Account 1/Advanced Settings
###############################################################
# Security Settings

# Check Domain Certificates. When set to Yes/Enabled, domain certificate will be checked as defined in RFC5922
# 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P2311 = 0

# Validate Certification Chain. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P2367 = 0

# Validate Incoming Messages. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P2306 = 0

# Allow Unsolicited REFER. 0 - Disabled, 1 - Enabled, 2 - Enabled/Force Auth. Default is 0
# Number: 0, 1, 2
# Mandatory
P26023 = 0

# Only Accept SIP Requests from Known Servers. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P2347 = 0

# Check SIP User ID for incoming INVITE. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P258 = 0

# Allow SIP Reset
# 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P26015 = 0

# Authenticate Incoming INVITE. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P2346 = 0

# SIP Realm Used for Challenge INVITE & NOTIFY
# Strings
P26021 =

# MOH
# Enable Local MOH
# 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P2357 = 0

# Advanced Features

# Special Feature. Default is 100
# 100 - Standard, 102 - Broadsoft, 113 - China Mobile
# 114 - ZTE IMS, 115 - Mobotix, 116 - ZTE NGN, 117 - Huawei IMS, 122 - Metaswitch, 123 - NEC, 125 - WorldStone
# Number: 100, 102, 113, 114, 115, 116, 117, 122, 123, 125
# Mandatory
P198 = 100

# Feature Key Synchronization. 0 – Disable, 1 – BroadSoft/Metaswitch. Default is 0.
# Number: 0, 1
P2325 = 1

# Allow Sync Phonebook via SIP Notify. 0 - No, 1 - Yes. Default is 1.
# Number: 0, 1
P26099 = 1

####################################################################
# Account 2                                                       ##
####################################################################
###############################################################
# Account 2/General Settings
###############################################################
# Account Registration

# Account Active. 0 - No, 1 - Yes. Default is 1
# Number: 0, 1
# Mandatory
P401 = 1

# Account Name
# String
P417 =

# SIP Server
# String
P402 =

# Secondary SIP Server
# String
P51102 =
P51202 =
P51302 =
P51402 =

# SIP User ID
# String
P404 =

# SIP Authenticate ID
# String
P405 =

# SIP Authenticate Password
# String
P406 =

# Name
# String
P407 =

# TEL URI. 0 - Disabled, 1 - User=Phone, 2 - Enabled. Default is 0
# Number: 0, 1, 2
# Mandatory
P409 = 0

# Voice Mail Access Number
# String
P426 =

# Network Settings

# Outbound Proxy
# String
P403 =

# Secondary Outbound Proxy
# String
P2433 = 

# DNS Mode. 0 - A Record, 1 - SRV, 2 - NAPTR/SRV. Default is 0
# Number: 0, 1, 2, 3
# Mandatory
P408 = 0

# DNS SRV Fail-over Mode. 0 - Default, 1 - Saved one until DNS TTL, 2 - Saved one until no response. Default is 0
# Number: 0,1,2
# Mandatory
P26140 = 0

# NAT Traversal. 0 - No, 1 - STUN, 2 - keep alive, 4 - Auto, 5 - VPN. Default is 0.
# Number: 0, 1, 2, 3, 4, 5
# Mandatory
P414 = 0

# Proxy-Require (A SIP extension to enable firewall penetration). Max length is 64 characters
# String
P418 =

###############################################################
# Account 2/SIP Settings
###############################################################
# SIP Basic Settings

# SIP Registration. 0 - No, 1 - Yes. Default is 1
# Number: 0, 1
# Mandatory
P410 = 1

# Unregister On Reboot. 0 - No, 1 - Yes, 2 - Instance. Default is 0
# Number: 0, 1
# Mandatory
P411 = 0

# Register Expiration (in minutes). Default is 60. Max about 45 days
# Number: 1 - 64800
# Mandatory
P412 = 60

# Subscribe Expiration (in minutes). Default is blank.
# Number: 1 - 64800
P26151 =

# Re-register Before Expiration (in seconds). Default is 0 second
# Number: 0 - 64800
# Mandatory
P2430 = 0

# Registration Retry Wait Time (in seconds). Default is 20
# Number: 1 - 3600
# Mandatory
P471 = 20

# Add Auth Header On Initial REGISTER
# 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P2459 = 0

# Enable OPTIONS Keep Alive. 0 - No, 1 - Yes. Default is 0
# Number: 0,1
# Mandatory
P2497 = 0

# SIP OPTIONS Keep Alive Interval (s). Default is 30
# Number: 1 - 64800
# Mandatory
P2498 = 30

# SIP OPTIONS Keep Alive Max Tries. Default is 3
# Number: 3 - 10
# Mandatory
P2499 = 3

# SUBSCRIBE for MWI (Whether or not send SUBSCRIBE for Message Waiting Indication). 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P415 = 0

# Use Privacy Header
# 0 - Default, 1 - No, 2 - Yes. Default is 0
# Number: 0, 1, 2
# Mandatory
P2438 = 0

# Use P-Preferred-Identity Header
# 0 - Default, 1 - No, 2 - Yes. Default is 0
# Number: 0, 1, 2
# Mandatory
P2439 = 0

# Use P-Access-Network-Info Header. 0 - No, 1 - Yes. Default is 0.
# Number: 0, 1
P26158 = 0

# Use P-Emergency-Info header. 0 - No, 1 - Yes. Default is 0.
# Number: 0, 1
P26159 = 0

# Use MAC Header. 0 - No, 1 - Yes except REGISTER, 2 - Yes to all SIP. Default is 0.
# Number: 0, 1, 2
P29190 = 2

# Add MAC in User-Agent. 0 - No, 1 - Yes except REGISTER, 2 - Yes to all SIP. Default is 0.
# Number: 0, 1, 2
P26161 = 2

# SIP Transport. 0 - UDP, 1 - TCP, 2 - TLS/TCP. Default is 0
# Number: 0, 1, 2
# Mandatory
P448 = 0

# Local SIP Port. Default is 5062
# Number: 0 - 65535
# Mandatory
P413 = 5062

# SIP URI Scheme when using TLS. 0 - sip, 1 - sips. Default is 1
# Number: 0, 1
# Mandatory
P2429 = 1

# Use Actual Ephemeral Port in Contact with TCP/TLS. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P2431 = 0

# Support SIP Instance ID. 0 - No, 1 - Yes. Default is 1
# Number: 0, 1
# Mandatory
P489 = 1

# SIP T1 Timeout. RFC 3261 T1 value (RTT estimate)
# 50 - 0.5 sec, 100 - 1 sec, 200 - 2 sec. Default is 50
# Number: 50, 100, 200
# Mandatory	
P440 = 50

# SIP T2 Interval
# 200 - 2 sec, 400 - 4 sec, 800 - 8 sec. Default is 400
# Number: 200, 400, 800
# Mandatory
P441 = 400

# SIP Timer D Interval
# Number: 0 - 64
# Mandatory
P2487 = 0

# Remove OBP from Route. 0 - Disable, 1 - Enable, 2 - Always. Default is 0 
# Number: 0, 1, 2 
# Mandatory
P2405 = 0

# Enable 100rel. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P435 = 0 

# Enable Session Timer/ Session Expiration(s).  In seconds. Default value is 180 seconds.
# By default,  Session Timer is Enabled.  Session Timer is disabled if the value is 0.
# Number: 0 or 90 - 64800
P434 = 180

# Minimum SE (in seconds). Default is 90. This value must be lower than or equal to P260
# Number: 90 - 64800
# Mandator
P427 = 90

# UAC Specify Refresher. 0 - omit, 1 - UAC, 2 - UAS. Default is 0
# Number: 0, 1, 2
# Mandatory
P432 = 0

# UAS Specify Refresher. 1 - UAC, 2 - UAS. Default is 1
# Number: 1, 2
# Mandatory
P433 = 1

# Caller Request Timer (Request for timer when calling). 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P428 = 0

# Callee Request Timer (Request for timer when called. i.e. if remote party supports timer but did not request for one)
# 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P429 = 0

# Force Timer (Still use timer when remote party does not support timer). 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P430 = 0

# Force INVITE (Always refresh with INVITE instead of UPDATE even when remote party supports UPDATE).
# 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P431 = 0

###############################################################
# Account 2/Codec Settings
###############################################################
# Preferred Vocoder   
# 0 - PCMU, 8 - PCMA, 9 - G722, 18 - G729A/B, 98 - iLBC, 123 - Opus
# Number: 0, 8, 9, 18, 98, 123     

# (For selected Vocoder)
# choice 1. Default is 0
# Number: 0, 8, 9, 18, 98, 123
# Mandatory
P451 = 0

# choice 2. Default is 8
# Number: 0, 8, 9, 18, 98, 123
# Mandatory
P452 = 8

# choice 3. Default is 9
# Number: 0, 8, 9, 18, 98, 123
# Mandatory
P453 = 9

# choice 4. Default is 9
# Number: 0, 8, 9, 18, 98, 123
# Mandatory
P454 = 9

# choice 5. Default is 9
# Number: 0, 8, 9, 18, 98, 123
# Mandatory
P455 = 9

# choice 6. Default is 9
# Number: 0, 8, 9, 18, 98, 123
# Mandatory
P456 = 9

# choice 7. Default is 9
# Number: 0, 8, 9, 18, 98, 123
P457 = 9

# choice 8. Default is 9
# Number: 0, 8, 9, 18, 98, 123
P458 = 9

# Codec Negotiation Priority. 0 - Caller, 1 - Callee. Default is 1
# Number: 0, 1
# Mandatory
P29161 = 1

# Use First Matching Vocoder in 200OK SDP. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P2448 = 0

# iLBC Frame Size. 0 - 20ms, 1 - 30ms. Default is 1
# Number: 0, 1
# Mandatory
P495 = 1

# OPUS Payload Type. Default is 123
# Number: 96 - 127
# Mandatory
P2485 = 123

# Send DTMF: In-audio. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P2401 = 0

# Send DTMF: Via RTP (RFC2833). 0 - No, 1 - Yes. Default is 1
# Number: 0, 1
# Mandatory
P2402 = 1

# Send DTMF: Via SIP INFO. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P2403 = 0

# DTMF Payload Type. Default is 101
# Number: 96 - 127
# Mandatory
P496 = 101

# Enable Audio RED with FEC. 0 - Disabled, 1 - Enabled. Default is 0
# Number: 0, 1
# Mandatory
P26173 = 0

# Audio FEC Payload Type. Default is 121
# Number: 96 to 127 (extra limit:  97, 98, 99, 127 are invalid values, and the value can't be the same as the Audio RED Payload Type)
# Mandatory
P26174 = 121

# Audio RED Payload Type. Default is 124 
# Number:96 to 127 (extra limit:  97, 98, 99, 127 are invalid values, and the value can't be the same as the Audio FEC Payload Type)
# Mandatory
P26175 = 124

# Silence Suppression. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P485 = 0

# Voice Frames per TX (up to 10/20/32/64 frames for G711/G726/G723/other codecs respectively). Default is 2
# Number: 1 - 64
# Mandatory
P486 = 2

# Account 2/Preferred Video Codec

# Preferred Video Codec. 99 - H264. Default is 99. 
# Number: 99
P464 = 99

# Enable Video FEC. 0 - No, 1 - Yes. Default value is 1.
# Number: 0, 1
P2493 = 1

# Enable RFC5168 support. 0 - No, 1 - Yes. Default value is 1.
# Number: 0, 1
P478 = 1

# FEC Payload Type. Default value is 120.
# Number: 96 - 126
P2494 = 120

# H.264 Image Size. 9 - 720P, 1 - VGA, 5 - CIF, 4 - 4CIF, 0 - QVGA, 6 - QCIF. Default value is 9
# Number: 9, 1, 5, 4, 0, 6
P2407 = 9

# Video Bit Rate. 32 - 32 kbps, 64 - 64 kbps, 96 - 96 kbps, 128 - 128 kbps, 160 - 160 kbps, 192 - 192 kbps
# 210 - 210 kbps, 256 - 256 kbps, 384 - 384 kbps, 512 - 512 kbps, 640 - 640 kbps, 768 - 768 kbps
# 1024 - 1024 kbps, 1280 - 1280 kbps, 1536 - 1536 kbps, 2048 - 2048 kbps. Default value is 2048.
# Number: 32,64,96,128,160,192,210,256,384,512,640,768,1024,1280,1536,2048
P2415 = 2048

# SDP Bandwidth Attribute. 0 - Standard, 1 - Media Level, 2 - Session Level, 3 - None. Default value is Media Level.
# Number: 0, 1, 2, 3
P2460 = 1

# Account 2/RTP Settings

# SRTP Mode. 0 - Disabled, 1 - Enabled but not forced, 2 - Enabled and forced. Default is 0
# Number: 0, 1, 2
# Mandatory
P443 = 0

# SRTP Key Length. 0 - AES 128&256 bit, 1 - AES 128 bit, 2 - AES 256 bit. Default is 0
# Default is 0
# Number: 0, 1, 2
# Mandatory
P2483 = 0

# Enable SRTP Key Life Time. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P2463 = 0

# RTCP Destination
# Strings
P2490 = 

# Symmetric RTP. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P460 = 0

# RTP IP Filter. 0 - Disable, 1 - IP Only, 2 - IP and Port. Default is 0
# Number: 0, 1, 2
# Mandatory
P26126 = 0

# RTP Timeout (in seconds). Default is 30.
# Number: 0 - 600
P29168 = 30

###############################################################
# Account 2/Call Settings
###############################################################
# Call Features

# Start Video Automatically. 0 - Disable, 1 - Enable. Default is 1.
# Number: 0, 1
P2414 = 0

# Auto Answer.  0 - No, 1 - Yes, 2 - Enable Intercom/Paging 
# Number: 0, 1, 2. Default is 0
# Mandatory
P425 = 0

# Play warning tone for Auto Answer Intercom. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P26172 = 0

# Intercom Barging. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P26119 = 0

# Send Anonymous (caller ID will be blocked if set to Yes). 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P421 = 0

# Anonymous Call Rejection. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P446 = 0

# Call Log. 0 - Log All Calls, 1 - Log Incoming/Outgoing only (Missed calls NOT recorded), 2 - Disable Call Log, 3 - Do Not Prompt Missed Call. Default is 0
# Number: 0, 1, 2
# Mandatory
P442 = 0

# Enable Call Features.  0 - No, 1 - Yes. Default is 1
# Number: 0, 1 
# Mandatory
P420 = 0

# Mute on Answer Intercom Call. 0 - Off, 1 - On. Default is 1.
# Number: 0, 1
P26171 = 0

# Transfer on 3 Way Conference Hangup.  0 - Disabled, 1 - Enabled. Default is 0
# Number: 0, 1
# Mandatory
P2404 = 0

# Use # As Dial Key. 0 - No, 1 - Yes
# Number: 0, 1
# Mandatory
P492 = 1

# DND Call Feature On
# String
P2444 = 

# DND Call Feature Off
# String
P2445 = 

# No Key Entry Timeout (in seconds). Default is 4
# Number: 1 - 15
# Mandatory
P491 = 4

# Ring Timeout (in seconds). Default is 60
# Number: 10 - 300
# Mandatory
P476 = 60

# Refer-To Use Target Contact. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P469 = 0

# RFC2543 Hold. 0 - No, 1 - Yes. Default is 1
# Number: 0, 1
# Mandatory
P26162 = 0

# Call Forward Type (Cannot be provisioned by config template currently)

# Dial Plan

# Dial Plan Prefix
# String
P419 = 

# Disable DialPlan. 0 - No Selection, 1 - Dial Page, 2 - Contact, 4 - Incoming Call History, 8 -  Outgoing Call History. 
# If need to check multiple selections, add the specific values for each selections together. Default value is 0
# Number: 0-31
P2482 = 0

# Dial Plan. Default is { x+ | \+x+ | *x+ | *xx*x+ | x+*x+*x+*x+ | x+*x+*x+*x+#x+ }
# String
# Mandatory
P459 = { x+ | \+x+ | *x+ | *xx*x+ | x+*x+*x+*x+ | x+*x+*x+*x+#x+ }

# Caller IDs

# Caller ID Display. 0 - Auto, 1 - Disabled, 2 - From Header. Default is 0
# Number: 0, 1, 2
# Mandatory
P2424 = 0

##########################Ringtone Value Table###################################
# Default						content://settings/system/ringtone
# Silent						ringtone_silence
# Andromeda						/system/media/audio/ringtones/ANDROMEDA.ogg
# Aquila						/system/media/audio/ringtones/Aquila.ogg
# Argo Navis					/system/media/audio/ringtones/ArgoNavis.ogg
# Atria							/system/media/audio/ringtones/Atria.ogg
# Backroad						/system/media/audio/ringtones/Backroad.ogg
# Beat Plucker					/system/media/audio/ringtones/BeatPlucker.ogg
# Bell Phone					/system/media/audio/ringtones/Ring_Classic_02.ogg
# Bentley Dubs					/system/media/audio/ringtones/BentleyDubs.ogg
# Big Easy						/system/media/audio/ringtones/Big_Easy.ogg
# Bird Loop						/system/media/audio/ringtones/BirdLoop.ogg
# Bollywood						/system/media/audio/ringtones/Bollywood.ogg
# BoÃ¶tes						/system/media/audio/ringtones/BOOTES.ogg
# Bus' a Move					/system/media/audio/ringtones/BussaMove.ogg
# Cairo							/system/media/audio/ringtones/Cairo.ogg
# Calypso Steel					/system/media/audio/ringtones/Calypso_Steel.ogg
# Canis Major					/system/media/audio/ringtones/CANISMAJOR.ogg
# Caribbean Ice					/system/media/audio/ringtones/CaribbeanIce.ogg
# Carina						/system/media/audio/ringtones/Carina.ogg
# Cassiopeia					/system/media/audio/ringtones/CASSIOPEIA.ogg
# Centaurus						/system/media/audio/ringtones/Centaurus.ogg
# Champagne Edition				/system/media/audio/ringtones/Champagne_Edition.ogg
# Chimey Phone					/system/media/audio/ringtones/Ring_Synth_02.ogg
# Club Cubano					/system/media/audio/ringtones/Club_Cubano.ogg
# Crayon Rock					/system/media/audio/ringtones/CrayonRock.ogg
# Crazy Dream					/system/media/audio/ringtones/CrazyDream.ogg
# Curve Ball Blend				/system/media/audio/ringtones/CurveBall.ogg
# Cygnus						/system/media/audio/ringtones/Cygnus.ogg
# Dancin' Fool					/system/media/audio/ringtones/DancinFool.ogg
# Digital Phone					/system/media/audio/ringtones/Ring_Digital_02.ogg
# Ding							/system/media/audio/ringtones/Ding.ogg
# DingDong						/system/media/audio/ringtones/DingDong.wav
# Don' Mess Wiv It				/system/media/audio/ringtones/DonMessWivIt.ogg
# Draco							/system/media/audio/ringtones/Draco.ogg
# Dream Theme					/system/media/audio/ringtones/DreamTheme.ogg
# Eastern Sky					/system/media/audio/ringtones/Eastern_Sky.ogg
# Enter the Nexus				/system/media/audio/ringtones/Enter_the_Nexus.ogg
# Eridani						/system/media/audio/ringtones/Eridani.ogg
# Ether Shake					/system/media/audio/ringtones/EtherShake.ogg
# Flutey Phone					/system/media/audio/ringtones/Ring_Synth_04.ogg
# Free Flight					/system/media/audio/ringtones/FreeFlight.ogg
# Friendly Ghost				/system/media/audio/ringtones/FriendlyGhost.ogg
# Funk Y'all					/system/media/audio/ringtones/Funk_Yall.ogg
# Game Over Guitar				/system/media/audio/ringtones/GameOverGuitar.ogg
# Gimme Mo' Town				/system/media/audio/ringtones/Gimme_Mo_Town.ogg
# Girtab						/system/media/audio/ringtones/Girtab.ogg
# Glacial Groove				/system/media/audio/ringtones/Glacial_Groove.ogg
# Growl							/system/media/audio/ringtones/Growl.ogg
# Halfway Home					/system/media/audio/ringtones/HalfwayHome.ogg
# Hydra							/system/media/audio/ringtones/Hydra.ogg
# Insert Coin					/system/media/audio/ringtones/InsertCoin.ogg
# Kuma							/system/media/audio/ringtones/Kuma.ogg
# Loopy Lounge					/system/media/audio/ringtones/LoopyLounge.ogg
# Love Flute					/system/media/audio/ringtones/LoveFlute.ogg
# Lyra							/system/media/audio/ringtones/Lyra.ogg
# Machina						/system/media/audio/ringtones/Machina.ogg
# Medieval Jaunt				/system/media/audio/ringtones/MidEvilJaunt.ogg
# Mildly Alarming				/system/media/audio/ringtones/MildlyAlarming.ogg
# Nairobi						/system/media/audio/ringtones/Nairobi.ogg
# Nassau						/system/media/audio/ringtones/Nassau.ogg
# New Player					/system/media/audio/ringtones/NewPlayer.ogg
# No Limits						/system/media/audio/ringtones/No_Limits.ogg
# Noisey One					/system/media/audio/ringtones/Noises1.ogg
# Organ Dub						/system/media/audio/ringtones/OrganDub.ogg
# Orion							/system/media/audio/ringtones/Orion.ogg
# Paradise Island				/system/media/audio/ringtones/Paradise_Island.ogg
# Pegasus						/system/media/audio/ringtones/Pegasus.ogg
# Perseus						/system/media/audio/ringtones/PERSEUS.ogg
# Playa							/system/media/audio/ringtones/Playa.ogg
# Pyxis							/system/media/audio/ringtones/Pyxis.ogg
# Rasalas						/system/media/audio/ringtones/Rasalas.ogg
# Revelation					/system/media/audio/ringtones/Revelation.ogg
# Rigel							/system/media/audio/ringtones/Rigel.ogg
# Road Trip						/system/media/audio/ringtones/Road_Trip.ogg
# Romancing The Tone			/system/media/audio/ringtones/RomancingTheTone.ogg
# Safari						/system/media/audio/ringtones/Safari.ogg
# Savannah						/system/media/audio/ringtones/Savannah.ogg
# Scarabaeus					/system/media/audio/ringtones/Scarabaeus.ogg
# Sceptrum						/system/media/audio/ringtones/Sceptrum.ogg
# Seville						/system/media/audio/ringtones/Seville.ogg
# She's All That				/system/media/audio/ringtones/Shes_All_That.ogg
# Silky Way						/system/media/audio/ringtones/SilkyWay.ogg
# Sitar Versus Sitar			/system/media/audio/ringtones/SitarVsSitar.ogg
# Solarium						/system/media/audio/ringtones/Solarium.ogg
# Springy Jalopy				/system/media/audio/ringtones/SpringyJalopy.ogg
# Steppin' Out					/system/media/audio/ringtones/Steppin_Out.ogg
# Terminated					/system/media/audio/ringtones/Terminated.ogg
# Terrible Twos					/system/media/audio/ringtones/Noises2.ogg
# Testudo						/system/media/audio/ringtones/Testudo.ogg
# Themos						/system/media/audio/ringtones/Themos.ogg
# Third Eye						/system/media/audio/ringtones/Third_Eye.ogg
# Thriller Three				/system/media/audio/ringtones/Noises3.ogg
# Thunderfoot					/system/media/audio/ringtones/Thunderfoot.ogg
# Twirl Away					/system/media/audio/ringtones/TwirlAway.ogg
# Ursa Minor					/system/media/audio/ringtones/URSAMINOR.ogg
# UrsaMinor						/system/media/audio/ringtones/UrsaMinor.ogg
# Very Alarmed					/system/media/audio/ringtones/VeryAlarmed.ogg
# Vespa							/system/media/audio/ringtones/Vespa.ogg
# World							/system/media/audio/ringtones/World.ogg
# Zeta							/system/media/audio/ringtones/Zeta.ogg
# bellcore-dr1					/system/media/audio/ringtones/bellcore-dr1.ogg
# bellcore-dr2					/system/media/audio/ringtones/bellcore-dr2.ogg
# bellcore-dr3					/system/media/audio/ringtones/bellcore-dr3.ogg
# bellcore-dr4					/system/media/audio/ringtones/bellcore-dr4.ogg
# bellcore-dr5					/system/media/audio/ringtones/bellcore-dr5.ogg
# speaker						/system/media/audio/ringtones/speaker.wav

# Ring Tones
# Account Ring Tone. Default is 0
# Mandatory
P423 = content://settings/system/ringtone

# Ignore Alert-Info header
# 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P26118 = 0

# Match Incoming Caller ID Rule 1
# String
P1494 = 

# Distinctive Ringtone Rule 1
# String
P1495 = content://settings/system/ringtone

# Match Incoming Caller ID Rule 2
# String
P1496 = 

# Distinctive Ringtone Rule 2
# String
P1497 = content://settings/system/ringtone

# Match Incoming Caller ID Rule 3
# String
P1498 =

# Distinctive Ringtone Rule 3
# String
P1499 = content://settings/system/ringtone

# Match Incoming Caller ID Rule 4
# String
P6722 = 

# Distinctive Ringtone Rule 4
# String
P6723 = content://settings/system/ringtone

# Match Incoming Caller ID Rule 5
# String
P6724 = 

# Distinctive Ringtone Rule 5
# String
P6725 = content://settings/system/ringtone

# Match Incoming Caller ID Rule 6
# String
P6726 =

# Distinctive Ringtone Rule 6 
# String
P6727 = content://settings/system/ringtone

# Match Incoming Caller ID Rule 7
# String
P26164 =

# Distinctive Ringtone Rule 7
# String
P26165 = content://settings/system/ringtone

# Match Incoming Caller ID Rule 8
# String
P26166 =

# Distinctive Ringtone Rule 8
# String
P26167 = content://settings/system/ringtone

# Match Incoming Caller ID Rule 9
# String
P26168 =

# Distinctive Ringtone Rule 9
# String
P26169 = content://settings/system/ringtone

# Match Incoming Caller ID Rule 10
# String
P26196 =

# Distinctive Ringtone Rule 10
# String
P26197 = content://settings/system/ringtone

###############################################################
# Account 2/Advanced Settings
###############################################################
# Security Settings

# Check Domain Certificates. When set to Yes/Enabled, domain certificate will be checked as defined in RFC5922
# 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P2411 = 0

# Validate Certification Chain. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P2467 = 0

# Validate Incoming Messages. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P2406 = 0

# Allow Unsolicited REFER. 0 - Disabled, 1 - Enabled, 2 - Enabled/Force Auth. Default is 0
# Number: 0, 1, 2
# Mandatory
P26123 = 0

# Only Accept SIP Requests from Known Servers. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P2447 = 0

# Check SIP User ID for incoming INVITE. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P449 = 0

# Allow SIP Reset
# 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P26115 = 0

# Authenticate Incoming INVITE. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P2446 = 0

# SIP Realm Used for Challenge INVITE & NOTIFY 
# Strings
P26121 = 

# MOH
# Enable Local MOH
# 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P2457 = 0

# Advanced Features

# Special Feature. Default is 100
# 100 - Standard, 102 - Broadsoft, 113 - China Mobile
# 114 - ZTE IMS, 115 - Mobotix, 116 - ZTE NGN, 117 - Huawei IMS, 122 - Metaswitch, 123 - NEC, 125 - WorldStone
# Number: 100, 102, 113, 114, 115, 116, 117, 122, 123, 125
# Mandatory
P424 = 100

# Feature Key Synchronization. 0 – Disable, 1 – BroadSoft/Metaswitch. Default is 0.
# Number: 0, 1
P2425 = 1

# Allow Sync Phonebook via SIP Notify. 0 - No, 1 - Yes. Default is 1.
# Number: 0, 1
P26199 = 1

####################################################################
# Phone Settings                                                 ##
####################################################################
####################################################################
# Phone Settings/General Settings/Basic Settings                 ##
####################################################################
# Local RTP port. Default is 50040
# Number: 50040 - 65400. Must be even number
# Mandatory
P39 = 50040

# Use Random Port. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P78 = 0

# Disable in-call DTMF display. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P338 = 0

# Keep-Alive Interval (in seconds). 
# Number: 10 - 160
# String
P84 = 20

# STUN server. Default is stun.ipvideotalk.com
# String
P76 = stun.ipvideotalk.com

# Use NAT IP. This will enable our SIP client to use this IP in the SIP/SDP message. Example 64.3.153.50
# String: a-z, A-Z, 0-9, ".", ":"
P101 =

####################################################################
# Phone Settings/General Settings/Guest Features                  ##
####################################################################
# Guest Login. 0 - Disabled, 1 - Enabled.
# Number: 0, 1. Default is 0.
# Mandatory
P22015 = 0

# Guest Login Timeout. 0 - Never, 60 - 1 hour, 120 - 2 hours, 240 - 4hours, 480 - 8 hours.
# Number: 0, 60, 120, 240, 480. Default is 0.
P22016 = 0

# Guest Login PIN Code
# String
P22019 = 

# SIP Domain
# Server Alias / Server List
# String
# The value should be json format string like this: {"alias":"aa","servers":["192.168.130.11","192.168.130.145"]};{"alias":"bb","servers":["192.168.130.123"]}
# P22017

####################################################################
# Phone Settings/Call Settings                   				  ##
####################################################################
# Enable Video Call. 0 - Yes, 1 - No. Default is 0.
# Number: 0, 1
P22091 = 0

# Default Video Zoom Area. Default is 0.
# Number: 0 - 9
P22324 = 5

# Enable Call Waiting. 0 - Yes, 1 - No. Default is 0
# Number: 0, 1
# Mandatory
P91 = 0

# Enable Call Waiting Tone. 0 - Yes, 1 - No. Default is 0
# Number: 0, 1
# Mandatory
P186 = 0

# Enable DND Reminder Ring. 0 - Enable, 1 - Disabled. Default is 0
# Number: 0, 1
# Mandatory
P1486 = 0

# Enable Transfer. 0 - Yes, 1 - No. Default is 0
# Number: 0, 1
# Mandatory
P1341 = 0

# Hold Call Before Completing Transfer. 0 - Disabled, 1 - Enabled. Default value is 1.
# Number: 0, 1
P8466 = 1

# Enable Conference. 0 - Yes, 1 - No. Default is 0
# Number: 0, 1
# Mandatory
P1311 = 0

# Auto Mute on Entry. 0 - Disable, 1 - Auto Mute on Incoming Call, 2 - Auto Mute on Outgoing Call, 3 - Auto Mute on Incoming & Outgoing Call.
# Number: 0, 1, 2, 3. Default is 0.
P29607 = 0

# Always Ring Speaker. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P1439 = 0

# Offhook Auto Dial
# String
P71 = 

# Offhook Auto Dial Delay (s)
# Number: 0 - 60
P8388 = 

# Offhook/Onhook Timeout (s). Default is 30.
# Number: 10 - 60
# Mandatory
P1485 = 30

# Off-cradle Pickup
# Number: 0 - Disable, 1 - Enable. Default is 0.
# Mandatory
P30120 = 0

# On-cradle Hangup
# Number: 0 - Disable, 1 - Enable. Default is 0.
# Mandatory
P30140 = 0

# Number Of Accounts The Virtual Account Group Register
# Number: 1 - 5
P22133 = 2

# Filter Characters. Default is [()-]
# String
P22012 = [()-]

# Escape '#' as 23% in SIP URL. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P1406 = 1

# Enable Noise Shield. 0 - No, 1 - Yes. Default is 0. 
# Number: 0, 1 
P25110 = 0

# Rejected Call Notification. 0 - Off, 1 - On. Default is 0.
# Number: 0, 1
P8393 = 0

# Enable In-call Recording. 0 - Disable, 1 - Enable. Default is 1.
# Number: 0, 1
P22318 = 0
####################################################################
# Phone Settings/Ring Tone                                        ##
####################################################################
# Auto Config CPT by Region. 0 - Disabled, 1 - Enabled.  Default value is 0
# Number: 0, 1
P22041 = 0

# Dial Tone
# String
P4000 = f1=350,f2=440,c=0/0;

# Second Dial Tone
# String
# P2909 = f1=350,f2=440,c=0/0;

# Ring Back Tone
# String
P4001 = f1=440,f2=480,c=2000/4000;

# Busy Tone
# String
P4002 = f1=480,f2=620,c=500/500;

# Reorder Tone
# String
P4003 = f1=480,f2=620,c=250/250;

# Confirmation Tone
# String
P4004 = f1=350,f2=440,c=100/100-100/100-100/100;

# Call-Waiting Tone
# String
P4005 = f1=440,c=300/2000-300/2000-0/0;

# Call-Waiting Tone Gain. 0 - Low, 1 - Medium, 2 - High. Default is 0
# Number: 0, 1, 2
# Mandatory
P1555 = 0

# Default Ring Cadence
# String
P4040 = c=2000/4000;

####################################################################
# Phone Settings/Video Settings                                   ##
####################################################################
# Video Frame Rate. 5 - 5 frames/second,  15 - 15 frames/second, 25 - 25 frames/second, 30 - 30 frames/second, 29 - Variable frames rate. Default value is 15
# Number: 5, 15, 25, 29, 30
P904 = 15

# Video Display Mode. 0 - Original proportion, 1 - Equal proportional cutting, 2 - Proportional add black edge. Default value is 1
# Number: 0, 1, 2
P921 = 1

# Enable Frame Skipping in Video Decoder. 0 - No, 1 - Yes, default is 1.
# Number: 0, 1
P22008 = 1

####################################################################
# Phone Settings/PTT/Multicast Settings				              ##
####################################################################
# General Settings

# Allow PTT/Paging When Lock Screen Status. 0 - Disable, 1 - Enable. Default is 0.
# Number: 0, 1
P22325 = 1

# IGMP keep-alive internal. Default is 30.
# Number: 0 - 120
P22251 = 30

# PTT Config

# Enable/Disable PTT. 0 - Disable, 1 - Enable. Default is 0.
# Number: 0, 1
# Mandatory
P22177 = 0

# PTT payload size (ms). 10, 20, 30, 40, 50, 60. Default is 30.
# Number: 10, 20, 30, 40, 50, 60
# Mandatory 
P22178 = 30

# PTT accept when busy. 0 - Disable, 1 - Enable. Default is 0.
# Number: 0, 1
# Mandatory
P22179 = 0

# PTT audio codecs. 0 - G711, 1 - G722, 2 - Opus. Default is 0.
# Number: 0, 1, 2
# Mandatory
P22180 = 0

# Emergency PTT/Paging Volume. 1-8. Default is 8.
# Number: 1-8
# Mandatory
P22181 = 8

# PTT caller ID
# String
P22182 = channel(*)

# PTT multicast address and port
# String
P22183 = 224.0.1.116:5001

# PTT channel default. 1-25. Default is 1.
# Number: 1-25
# Mandatory
P22184 = 1

# PTT channel priority. 1-25. Default is 24.
# Number: 1-25
# Mandatory
P22185 = 24

# PTT channel emergency. 1-25. Default is 25.
# Number: 1-25
# Mandatory
P22186 = 25

# PTT channel available
# String
# Example: 1100000000000000000000011 means Channels 0,1,24,25 (each digit is a channel, 0 means disable, 1 means enable)
P22187 = 1100000000000000000000011

# PTT channel join group
# String
# Example: 1100000000000000000000011 means Channels 0,1,24,25 (each digit is a channel, 0 means disable, 1 means enable)
P22188 = 1100000000000000000000011

# PTT channel transmittable
# String
# Example: 1100000000000000000000011 means Channels 0,1,24,25 (each digit is a channel, 0 means disable, 1 means enable)
P22189 = 1111111111111111111111111

# PTT channel subscribe
# String
# Example: 1100000000000000000000011 means Channels 0,1,24,25 (each digit is a channel, 0 means disable, 1 means enable)
P22190 = 1111111111111111111111111

# PTT recent channel.
# Number: 1-25
# Mandatory
# P22191

# PTT channel label
# Usage: Use ^ to separate the channel labels. E.g. Label1^Label2^Label3
# String
P22192 =

# Paging default mode. 0 - Multicast paging, 1 - PTT, 2 - Group Paging
# Number: 0, 1, 2
# Mandatory
P22193 = 1

# Group Paging Config

# Enable/Disable group paging. 0 - Disable, 1 - Enable. Default is 0.
# Number: 0, 1
# Mandatory
P22194 = 0

# Paging payload size (ms). 10, 20, 30, 40, 50, 60. Default is 30.
# Number: 10, 20, 30, 40, 50, 60
# Mandatory
P22195 = 30

# Paging accept when busy. 0 - Disable, 1 - Enable. Default is 0.
# Number: 0, 1
# Mandatory
P22196 = 0

# Paging audio codecs. 0 - G711, 1 - G722, 2 - Opus. Default is 0.
# Number: 0, 1, 2
# Mandatory
P22197 = 0

# Paging caller ID
# String
P22198 = channel(*)

# Paging channel default. 26-50. Default is 26.
# Number: 26-50
# Mandatory
P22199 = 26

# Paging channel priority. 26-50. Default is 49.
# Number: 26-50
# Mandatory
P22200 = 49

# Paging emergency channel. 26-50. Default is 50.
# Number: 26-50
# Mandatory
P22201 = 50

# Paging recent channel
# Number: 26-50
# Mandatory
# P22202

# Paging channel available
# String
# Example: 1100000000000000000000011 means Channels 0,1,24,25 (each digit is a channel, 0 means disable, 1 means enable)
P22203 = 1100000000000000000000011

# Paging channel join group
# String
# Example: 1100000000000000000000011 means Channels 0,1,24,25 (each digit is a channel, 0 means disable, 1 means enable)
P22204 = 1100000000000000000000011

# Paging channel transmittable
# String
# Example: 1100000000000000000000011 means Channels 0,1,24,25 (each digit is a channel, 0 means disable, 1 means enable)
P22205 = 1111111111111111111111111

# Paging channel subscribe
# String
# Example: 1100000000000000000000011 means Channels 0,1,24,25 (each digit is a channel, 0 means disable, 1 means enable)
P22206 = 1111111111111111111111111

# Group Paging channel label
# Usage: Use ^ to separate the channel labels. E.g. Label1^Label2^Label3
# String
P22207 =

# Multicast paging         

# Paging Barge. 0 - Disable, 1 - priority 1, 2 - priority 2, 3 - priority 3, 
# 4 - priority 4, 5 - priority 5, 6 - priority 6, 7 - priority 7, 8 - priority 8,
# 9 - priority 9, 10 - priority 10. Default is 0.
# Number: 0 - 10
# Mandatory
P1566 = 0

# Paging Priority Active. 0 - Disabled, 1 - Enabled
# Number: 0, 1
# Mandatory
P1567 = 0

# Multicast Paging Codec.  0 - PCMU, 8 - PCMA, 2 - G.726-32, 9 - G.722, 18 - G.729A/B, 98 - iLBC, 123 - Opus
# Number: 0, 8, 2, 9, 18, 98， 123. Default is 0.
# Mandatory
P1568 = 0

# Enable/Disable Multicast paging. 0 - Disable, 1 - Enable. Default is 0.
# Number: 0, 1
# Mandatory
P22208 = 0

# Priority 1
# Listening Address and Port
# String
P1569 = 

# Label
# String
P1570 = 

# Priority 2
# Listening Address and Port
# String
P1571 = 

# Label
# String
P1572 = 

# Priority 3
# Listening Address and Port
# String
P1573 = 

# Label
# String
P1574 = 

# Priority 4
# Listening Address and Port
# String
P1575 = 

# Label
# String
P1576 = 

# Priority 5
# Listening Address and Port
# String
P1577 = 

# Label
# String
P1578 = 

# Priority 6
# Listening Address and Port
# String
P1579 = 

# Label
# String
P1580 = 

# Priority 7
# Listening Address and Port
# String
P1581 = 

# Label
# String
P1582 = 

# Priority 8
# LListening Address and Port
# String
P1583 = 

# Label
# String
P1584 = 

# Priority 9
# Listening Address and Port
# String
P1585 = 

# Label
# String
P1586 = 

# Priority 10
# Listening Address and Port
# String
P1587 = 

# Label
# String
P1588 = 

###############################################################
# Network Settings/Bluetooth         
###############################################################
# Device Name
# String
# (P-value TBA)
#
# Bluetooth Headset Mode
# Number: 0, 1
# (P-value TBA)
#
# Bluetooth Function
# Number: 0, 1
# (P-value TBA)

####################################################################
# Network Settings/Wi-Fi Settings/Wi-Fi Basics                    ##
####################################################################
# IP mode. 0 - Both, prefer IPv4, 1 - Both, prefer IPv6, 2 - IPv4 Only, 3 - IPv6 Only. Default is 2.
# Number: 0, 1, 2, 3
P22233 = 0

# Wi-Fi Signal Warning. 0 - Disable, 1 - Level 1, 2 - Level 2, 3 - Level 3, 4 - Level 4, 5 - Level 5. Default is 3.
# Number: 0 - 5
P22322 = 5

# Wi-Fi Function. 0 - Disabled, 1 - Enabled.  Default value is 1
# Number: 0, 1
# Mandatory
# P7800 = 1

# WiFi Band. 2.4G & 5G - P25420=1 P25421=1, 2.4G - P25420=1 P25421=0, 5G - P25420=0 P25421=1. Default is P25420=1 P25421=1.
# Number: 0, 1
# P25420 = 1
# P25421 = 1

####################################################################
# Network Settings/Wi-Fi Settings/Add Network                     ##
####################################################################
# ESSID
# String
# P7812 = wp_master

# Password
# String
# P7830 = wp!987@dmin

# Security Mode for Hidden SSID. 0 - None, 1 - WEP, 2 - WPA/WPA2 PSK, 3 - WPA Enterprise.  Default value is 2.
# Number: 0, 1, 2, 3
# P7814 = 2

# EAP Method (WPA Enterprise). 0 - PEAP, 1 - TLS, 2 - TTLS, 3 - PWD. Default is 0.
# Number: 0 - 3
# P83004 = 0

# Phase 2 Authentication (WPA Enterprise). 0 - None, 1 - PAP, 2 - MSCHAP, 3 - MSCHAPV2, 4 - GTC. Default is 0.
# Number: 0 - 4
# P83013 = 0

# CA Certificate (WPA Enterprise). 
# String
# P83011 =

# User Certificate (WPA Enterprise). 
# String
# P83010 =

# Identity (WPA Enterprise). 
# String
# P83014 =

# Anonymous identity (WPA Enterprise). 
# String
# P83012 =

# Password (WPA Enterprise). 
# String
# P83015 =
####################################################################
# Network Settings/Wi-Fi Settings/Advanced Settings               ##
####################################################################
# Country Code (World version device only. Locked device cannot change country code.)
# Use ISO 3166-1 alpha-2 code for country value
# For example, United States of America - US
# P7831 = US

# Host Name (Option 12)
# String
# P146 =

# Vendor Class ID (Option 60)
# String
# P148 = Grandstream WP820

# Channel Mode. (Blank) - Auto, (Any value) - Customize. Default is blank.
# 2.4G: Channel 1 - 2412, Channel 2 - 2417, Channel 3 - 2422, Channel 4 - 2427, Channel 5 - 2432, Channel 6 - 2437,
# Channel 7 - 2442, Channel 8 - 2447, Channel 9 - 2452, Channel 10 - 2457, Channel 11 - 2462
# 5G: Channel 36 - 5180, Channel 40 - 5200, Channel 44 - 5220, Channel 48 - 5240, Channel 52 - 5260, Channel 56 - 5280, 
# Channel 60 - 5300, Channel 64 - 5320, Channel 100 - 5340, Channel 104 - 5360, Channel 108 - 5380, Channel 112 - 5400,
# Channel 116 - 5420, Channel 120 - 5440, Channel 124 - 5460, Channel 128 - 5480, Channel 132 - 5500, Channel 136 - 5520,
# Channel 140 - 5540, Channel 144 - 5560, Channel 149 - 5580, Channel 153 - 5600, Channel 157 - 5620, Channel 161 - 5640,
# Channel 165 - 5660.
# Separate channel values by comma e.g "2412,2417,5180,5200"
# String
# P22288 =

####################################################################
# Network Settings/Wi-Fi Settings/Wi-Fi Roaming                   ##
####################################################################
# Good Signal Scanning Interval
# Number: 1 - 65535
# P22230 = 600

# Poor Signal Scanning Interval
# Number: 1 - 65535
# P22231 = 5

# Roaming signal threshold
# Number: -100 - -30
# P22232 = -70

####################################################################
# Network Settings/OpenVPN® Settings                              ##
####################################################################
# OpenVPN Enable.  0 - No, 1 - Yes. Default is 0
# Number: 0, 1 
# Mandatory
# P7050 = 0

# OpenVPN Mode. 0 - Simple Mode, 1 - Expert Mode.
# Number: 0, 1
# P22292 = 0

# Enable OpenVPN® Comp-lzo. 0 - On, 1 - Off. Default is 0.
# Number: 0, 1
# P8508 = 0

# OpenVPN Server Address
# String
# P7051 =

# OpenVPN Port. Default is 1194.
# Number
# P7052 = 1194

# OpenVPN Transport.  0 - UDP, 1 - TCP. Default is 0
# Number: 0, 1 
# Mandatory
# P2912 = 0

# OpenVPN CA
# String
# P9902 =

# OpenVPN Client Certificate
# String
# P9903 =

# OpenVPN Client Private Key
# String
# P9904 =

# OpenVPN Cipher Method. 0 - Blowfish, 1 - AES-128, 2 - AES-256, 3 - Triple-DES. Default is 0
# Number: 0, 1, 2, 3 
# Mandatory
# P8396 = 0

# OpenVPN Username
# String
# P8394 =

# OpenVPN Password
# String
# P8395 =

####################################################################
# Network Settings/Advanced Network Settings                      ##
####################################################################
# Preferred DNS 1
# Number: 0 - 255
# P92 = 

# Number: 0 - 255
# P93 = 

# Number: 0 - 255
# P94 = 

# Number: 0 - 255
# P95 = 

# Preferred DNS 2
# Number: 0 - 255
# P5026 = 

# Number: 0 - 255
# P5027 = 

# Number: 0 - 255
# P5028 = 

# Number: 0 - 255
# P5029 = 

# Layer 3 QoS for SIP. 0-63. Default is 26.
# Number: 0-63
# Mandatory
# P1558 = 26

# Layer 3 QoS for Audio. 0-63. Default is 46.
# Number: 0-63
# Mandatory
# P1559 = 46

# HTTP/HTTPS User-Agent
# String
# P1541 = 

# SIP User-Agent
# String
# P26027 = 

# Proxy

# HTTP/HTTPS Proxy Hostname and port
# e.g.  If the HTTP/HTTPS Proxy Hostname is gs, HTTP/HTTPS Proxy Port is 8082， the P1552 = gs:8082
# P1552 =

# Bypass Proxy For 
# String
# P22011

# Remote Control

# CSTA Control. 0 - Off, 1 - On. Default is 0.
# Number: 0, 1
# P32053 = 0

####################################################################
# System Settings/Time and Language/Time Settings                 ##
####################################################################
# Assign NTP Server Address 
# String
P30 = pool.ntp.org

# DHCP Option 42 to override NTP server. 0 - No, 1 - Yes. Default is 1
# When set to Yes(1), it will override the configured NTP server
# Number: 0, 1
# Mandatory
P144 = 1

# DHCP Option 2 to override Time Zone setting. 0 - No, 1 - Yes. Default is 1
# When set to Yes(1), it will override the configured Time Zone setting if available 
# Number: 0, 1
# Mandatory
P143 = 1

# Time Zone
# Web GUI Option       			   							    P Value            							
# GMT-11:00(Midway Island)             							Pacific/Midway
# GMT-10:00(Honolulu)                    						Pacific/Honolulu
# GMT-8:00(Anchorage)                     						America/Anchorage
# GMT-8:00(Los Angeles)               							America/Los_Angeles
# GMT-8:00(Tijuana)                    							America/Tijuana
# GMT-7:00(Phoenix)												America/Phoenix
# GMT-7:00(Chihuahua)                  							America/Chihuahua
# GMT-7:00(Denver)										        America/Denver
# GMT-6:00(Costa Rica)            							    America/Costa_Rica
# GMT-6:00(Regina)										        America/Regina
# GMT-6:00(Chicago)               							    America/Chicago     
# GMT-6:00(Mexico City)              							America/Mexico_City
# GMT-5:00(Bogota)												America/Bogota
# GMT-5:00(New York)                                            America/New_York
# GMT-4:00(Caracas)											    America/Caracas
# GMT-4:00(Barbados)                           	                America/Barbados
# GMT-4:00(Manaus)												America/Manaus
# GMT-4:00(Halifax)                           	                America/Halifax
# GMT-4:00(Santiago)											America/Santiago
# GMT-3:00(Recife)  											America/Recife
# GMT-3:00(Sao Paulo)                                			America/Sao_Paulo
# GMT-3:00(Buenos Aires)										America/Buenos_Aires
# GMT-3:00(Montevideo)											America/Montevideo
# GMT-2:30(America/St_Johns)									America/St_Johns
# GMT-2:00(Nuuk)												America/Godthab
# GMT-2:00(South_Georgia)                            			Atlantic/South_Georgia
# GMT-1:00(Cape Verde Islands)									Atlantic/Cape_Verde
# GMT+0:00(Azores)                                  			Atlantic/Azores
# GMT+1:00(Casablanca)                              			Africa/Casablanca
# GMT+0:00(London)                                  			Europe/London
# GMT+1:00(Brazzaville)											Africa/Brazzaville
# GMT+1:00(Amsterdam)											Europe/Amsterdam
# GMT+1:00(Belgrade)											Europe/Belgrade
# GMT+1:00(Brussels)											Europe/Brussels
# GMT+1:00(Madrid)												Europe/Madrid
# GMT+1:00(Sarajevo)											Europe/Sarajevo
# GMT+2:00(Windhoek)											Africa/Windhoek
# GMT+2:00(Cairo)												Africa/Cairo
# GMT+2:00(Harare)												Africa/Harare
# GMT+2:00(Amman)										        Asia/Amman
# GMT+2:00(Athens)												Europe/Athens
# GMT+3:00(Istanbul)											Europe/Istanbul
# GMT+2:00(Beirut)												Asia/Beirut
# GMT+2:00(Helsinki)											Europe/Helsinki
# GMT+2:00(Jerusalem)											Asia/Jerusalem
# GMT+3:00(Minsk)												Europe/Minsk
# GMT+3:00(Baghdad)												Asia/Baghdad
# GMT+3:00(Moscow)												Europe/Moscow
# GMT+3:00(Kuwait)												Asia/Kuwait
# GMT+3:00(Nairobi)												Africa/Nairobi
# GMT+3:30(Tehran)												Asia/Tehran
# GMT+4:00(Baku)												Asia/Baku
# GMT+4:00(Tbilisi)												Asia/Tbilisi
# GMT+4:00(Yerevan)												Asia/Yerevan
# GMT+4:00(Dubai)												Asia/Dubai
# GMT+4:30(Kabul)												Asia/Kabul
# GMT+5:00(Karachi)									            Asia/Karachi
# GMT+5:00(Ural'sk)												Asia/Oral
# GMT+5:00(Yekaterinburg)										Asia/Yekaterinburg
# GMT+5:30(Kolkata)												Asia/Calcutta
# GMT+5:30(Colombo)											    Asia/Colombo
# GMT+5:45(Kathmandu)											Asia/Katmandu
# GMT+6:00(Almaty)												Asia/Almaty
# GMT+6:30(Rangoon)												Asia/Rangoon
# GMT+7:00(Krasnoyarsk)											Asia/Krasnoyarsk
# GMT+7:00(Bangkok)												Asia/Bangkok
# GMT+7:00(Jakarta)												Asia/Jakarta
# GMT+8:00(Shanghai)											Asia/Shanghai
# GMT+8:00(Hong Kong)											Asia/Hong_Kong
# GMT+8:00(Irkutsk)												Asia/Irkutsk
# GMT+8:00(Kuala Lumpur)										Asia/Kuala_Lumpur
# GMT+8:00(Perth)												Australia/Perth
# GMT+8:00(Taipei)                                				Asia/Taipei
# GMT+9:00(Seoul)												Asia/Seoul
# GMT+9:00(Tokyo)										        Asia/Tokyo
# GMT+9:00(Yakutsk)												Asia/Yakutsk
# GMT+9:30(Darwin)												Australia/Darwin
# GMT+10:00(Brisbane)											Australia/Brisbane
# GMT+10:00(Vladivostok)										Asia/Vladivostok
# GMT+10:00(Guam)												Pacific/Guam
# GMT+9:30(Adelaide)											Australia/Adelaide
# GMT+10:00(Hobart)												Australia/Hobart
# GMT+10:00(Sydney)								       	        Australia/Sydney
# GMT+11:00(Magadan)											Asia/Magadan
# GMT+11:00(Noumea)								                Pacific/Noumea
# GMT+12:00(Majuro)                                             Pacific/Majuro
# GMT+12:00(Fiji)												Pacific/Fiji
# GMT+12:00(Auckland)											Pacific/Auckland
# GMT+13:00(Tonga)                                              Pacific/Tongatapu

# Time Zone
P64 = America/Los_Angeles

# Time Display Format. 0 - 12 Hour, 1 - 24 Hour
# Number: 0, 1
# Mandatory
P122 = 0

# Date Display Format. 3 - Normal(YYYY/M/D), 0 - YYYY/MM/DD, 1 - MM/DD/YYYY, 2 - DD/MM/YYYY.  Default value is 3.
# Number: 0, 1, 2, 3
# Mandatory
P102 = 3

####################################################################
# System Settings/Time and Language/Language                      ##
####################################################################
# Language
# Language. Configure the language to be displayed on LCD
# Note: for some languages that have 2 codes avaiable, both are working
# ja_JP - 日本語
# zh_TW - 中文 (繁體), or zh-tw - 中文 (繁體)
# zh_CN - 中文 (简体), or zh - 中文 (简体)
# de_DE - Deutsch
# en_US - English (United States), en - English (United States)
# es_ES - Español (España)
# fr_FR - Français, fr - Français
# it_IT - Italiano, or it - Italiano
# nl_NL - Nederlands, or nld - Nederlands
# pl_PL - Polski, or pl - Polski
# pt_PT - Português (Portugal)
# sl_SI - Slovenšcina
# tr_TR - Türkçe, or tr - Türkçe
# ru_RU - Russian, or ru - Russian
# uk_UA - Ukrainian
# iw_IL - Hebrew
# ar_EG - العربية
# Customized - Custom Language
P1362 = en_US

####################################################################
# System Settings/Security Settings/Web/SSH Access                ##
####################################################################
# Enable SSH. 0 - Yes, 1 - No. Default is 0.
# Number: 0, 1
P276 = 0

# SSH Port. Default is 22. 
# Number 1 - 65535
P27006 = 22

# Web Access Method. 0 - HTTP, 1 - HTTPS. Default value is 0
# Number: 0, 1
P900 = 0

# Web Port. Default is 443.(By default, HTTP uses port 80 and HTTPS uses port 443.)
# Number
# Mandatory
P901 = 80

# Configuration Via Keypad Menu. 0 - Unrestricted, 1 - Basic settings only, 2 - Constraint mode, 3 - Basic settings & Network settings. Default is 0
# Number: 0, 1, 2, 3
# Mandatory
P1357 = 0

# User Login Timeout (in minutes). Default is 15.
# Number: 0 - 60
P28116 = 60

####################################################################
# System Settings/Security Settings/User Info Management          ##
####################################################################
# New Admin Password. Default is admin.
# String
P2 = 

# New User Password. Default is 123.
# String
P196 =

####################################################################
# System Settings/Security Settings/TLS                           ##
####################################################################
# Minimum TLS Version. 10 - 1.0, 11 - 1.1, 12 - 1.2. Default is 11.
# Number: 10, 11, 12
P22293 = 10

# Maximum TLS Version. 10 - 1.0, 11 - 1.1, 12 - 1.2, 99 - No limit. Default is 99.
# Number: 10, 11, 12, 99
P22294 = 12

# SIP TLS Certificate
# String: a-z, A-Z, 0-9
# P280 =

# SIP TLS Private Key
# String: a-z, A-Z, 0-9
# P279 =

# SIP TLS Private Key Password
# String: a-z, A-Z, 0-9
# P281 = 

####################################################################
# System Settings/Security Settings/Certificate Management        ##
####################################################################
# CA Certificate

# Trusted CA Certificate 1
# String
# P2386 =

# Trusted CA Certificate 2
# String
# P2486 =

# Trusted CA Certificate 3
# String
# P2586 =

# Trusted CA Certificate 4
# String
# P2686 =

# Trusted CA Certificate 5
# String
# P2786 =

# Trusted CA Certificate 6
# String
# P2886 =

# User Certificate
# (P-value TBA)

# Custom Certificate

# Custom Certificate
# String
# P8472 = 

###############################################################
# System Settings/Security Settings/Lock Screen Settings           
###############################################################
# Screen Lock Function. 0 - Off, 1 - On. Default is 0.
# Number: 0, 1
P22235 = 0

# Screen Lock Password.
# String
P1383 =

###############################################################
# System Settings->Preferences->Sound
###############################################################
# Silent Mode. 0 - Disable, 1 - Enable. Default is 0.
# Number: 0, 1
P22319 = 1

# Vibrate Mode. 0 - Disable, 1 - Enable. Default is 0.
# Number: 0, 1
P22320 = 1

# Charging tone. 0 - Disable, 1 - Enable. Default is 0.
# Number: 0, 1
P22224 = 0

# Low Battery Warning Tone. 0 - Disable, 1 - Enable. Default is 1.
# Number: 0, 1
P22321 = 0

# Voicemail Notification Tone. 0 - Disable, 1 - Enable. Default is 1.
# Number: 0, 1
P22323 = 0

# Ringtone Volume
# (P-value TBA)

# Media Volume
# (P-value TBA)

# Alarm Volume
# (P-value TBA)

# Default Ringtone
# (P-value TBA)

# Notification Tone
# (P-value TBA)

####################################################################
# System Settings/Preferences/LCD & LED Management                ##
####################################################################
# LED Management

# Enable Missed Call Indicator. 0 - Yes, 1 - No. Default is 0.
# Number: 0, 1
P1691 = 0

# Enable MWI Indicator. 0 - Yes, 1 - No. Default is 0.
# Number: 0, 1
P1692 = 0

# Enable New Message Indicator. 0 - Yes, 1 - No. Default is 0.
# Number: 0, 1
P1693 = 0

# Keypad backlight. 0 - Disable, 1 - Enable. Default is 0.
# Number: 0, 1
P22234 = 0

# Brightness. Default is 182.
# Number: 1 - 255
P910 = 182

# Timeout. 0 - Never, 15 - 15 Seconds, 30 - 30 Seconds, 60 - 1 Minute, 120 - 2 Minutes, 300 - 5 Minutes, 600 - 10 Minutes, 1800 - 30 Minutes. Default is 60.
# Number: 0, 15, 30, 60, 120, 300, 600, 1800
P1412 = 60

# Font Size. 0 - Small, 1 - Standard, 2 - Large. Default is 1.
# Number: 0, 1, 2
P22275 = 2

####################################################################
# System Settings/Preferences/Gesture Control                     ##
####################################################################
# Flip phone 

# Reject incoming call. 1 - Reject, 2 - Reject with SMS, 3 - Off Default is 3.
# Number: 1, 2, 3
P22225 = 3

# Reply content
# not_convenient - Sorry, I can't answer the phone now.
# call_later - I am not available now. I'll call you later.
# in_metting - Sorry, I'm in a meeting.
# in_a_call - I am on another call right now and will call you back later.
# customize - Customize
# P22228 = not_convenient

# Customize (Reply Content)
# String
# P22274 = 

# Pick up the phone

# Ringtone. 1 - Mute, 2 - Ringing Down, 3 - Off. Default is 3. 
P22226 = 3

# Alarm Ringtone. 1 - Mute, 2 - Ringing Down, 3 - Off. Default is 3. 
P22227 = 3
####################################################################
# System Settings/Preferences/Button Customization                ##
####################################################################
# WP8xx main screen left softkey. 0 - Call history, 1 - Menu , 2 - Settings , 3 - Contacts , 4 - Voicemail, 5 - DND. Default is 0.
# Number: 0 - 5
P22252 = 0

# WP8xx main screen center softkey. 0 - Call history, 1 - Menu , 2 - Settings , 3 - Contacts , 4 - Voicemail, 5 - DND. Default is 1.
# Number: 0 - 5
P22253 = 1

# WP8xx main screen right softkey. 0 - Call history, 1 - Menu , 2 - Settings , 3 - Contacts , 4 - Voicemail, 5 - DND. Default is 2
# Number: 0 - 5
P22254 = 2

# WP8xx call screen left softkey. 0 - Option, 1 - Transfer, 2 - Hold, 3 - Mute, 4 - New Call, 5 - Conference, 6 - Record. Default is 0.
# Number: 0 - 6
P22255 = 0

# WP8xx call screen center softkey. 0 - Option, 1 - Transfer, 2 - Hold, 3 - Mute, 4 - New Call, 5 - Conference, 6 - Record. Default is 1.
# Number: 0 - 6
P22256 = 1

# WP8xx call screen right softkey. 0 - Option, 1 - Transfer, 2 - Hold, 3 - Mute, 4 - New Call, 5 - Conference, 6 - Record. Default is 2. 
# Number: 0 - 6
P22257 = 2

# Multi-function button customization. 0 - PTT/Paging, 1 - Mute, 2 - SAFE/Panic Call, 3 - Speed Dial. Default is 0.
# Number: 0, 1, 2, 3
P22258 = 0

# Multi-function Button - Speed dial account. 0 - Account 1, 1 - Account 2. Default is 0.
# Number: 0, 1
P23051 = 0

# Multi-function Button - Speed dial number. 
# String (numbers only)
P23053 =

####################################################################
# System Settings/TR069                                           ##
####################################################################
# Enable TR-069. 0 - Disabled, 1 - Enabled.
# Number: 0, 1
# Mandatory
# Reboot
P1409 = 0

# ACS URL
# String 
P4503 =

# TR-069 Username
# String
P4504 =

# TR-069 Password
# String
P4505 =

# Periodic Inform Enable. 0 - No, 1 - Yes. Default is 0.
# Number: 0, 1
P4506 = 0

# Periodic Inform Interval. Default is 86400.
# Number
P4507 = 86400

# Connection Request Username	
# String: a-z, A-Z, 0-9
P4511 =

# Connection Request Password	
# String: a-z, A-Z, 0-9
P4512 =

# Connection Request Port. 
# Number
P4518 = 

# CPE Cert File
# String
P8220 = 

# CPE Cert Key
# String
P8221 = 

####################################################################
# Maintenance/Upgrade/Firmware                                    ##
####################################################################
# Complete Upgrade. 0 - No, 1 - Yes. Default is 0.
# Pupgradeall = 0

# Firmware
# Firmware Upgrade Via. 0 - TFTP,  1 - HTTP, 2 - HTTPS. Default is 2.
# Number: 0, 1, 2
# Mandatory
P6767 = 2

# Firmware Server Path
# String
P192 = fm.grandstream.com/gs

# Firmware HTTP/HTTPS User Name
# String
P6768 = 

# Firmware HTTP/HTTPS Password
# String
P6769 = 

# Firmware File Prefix
# String
P232 =

# Firmware File Postfix
# String
P233 =

####################################################################
# Maintenance/Upgrade/Config File                                ##
####################################################################
# Config Via. 0 - TFTP,  1 - HTTP, 2 - HTTPS. Default is 2.
# Number: 0, 1, 2
# Mandatory
P212 = 2

# Config Server Path
# String
P237 = fm.grandstream.com/gs

# Config HTTP/HTTPS User Name
# String
P1360 =

# Config HTTP/HTTPS Password
# String
P1361 =

# Always send HTTP Basic Authentication Information. 0 - Disable, 1 - Enable. Default is 0. 
# Number: 0, 1
# Mandatory
P20713 = 0

# Config File Prefix
# String
P234 =

# Config File Postfix
# String
P235 =

# Authenticate Conf File. 0 - No, 1 - Yes. Default is No
# Number: 0, 1
# Mandatory
P240 = 0

# XML Config File Password
# String
P1359 =

####################################################################
# Maintenance/Upgrade/Provision                                   ##
####################################################################
# Automatic Upgrade. 0 - No, 1 - Check Every Day, 2 - Check Every Week, 3 - Check at a Period Time. Default value is 0
# Number: 0, 1, 2, 3
P194 = 0

# Enable Randomized Automatic Upgrade. 0 - Disable, 1 - Enable. Default is 0.
# Number: 0, 1
P8458 = 1

# Automatic Upgrade Check Interval (m). Minimum 60 minutes. Default value is 10080 (7 days)
# Number: 60 - 5256000
P193 = 10080

# Starting/Ending Hour of the Day(0-23)
# Number: 0 - 23
P285 = 1
P8459 = 

# Day of the Week (0-6)
# Number: 0 - 6
P286 = 1

# Firmware Upgrade and Provisioning
# 0 - Always Check at bootup
# 1 - When Firmware/Config file pre/suffix changes
# 2 - Skip the Firmware Check
# Number: 0, 1, 2
# Mandatory
P238 = 0

# Upgrade With Prompt. 0 - Enable, 1 - Disable. Default value is 0.
# Number: 0, 1
P1549 = 0

# DHCP Option

# Allow DHCP Option 43, 160 and 66 Override Server. 0 - No, 1 - Yes, 2 - Prefer, fallback when failed. Default is 1.
# When set to Yes(1), it will override the configured provision path and method
# Number: 0, 1, 2
# Mandatory
P145 = 2

# Allow DHCP Option 120 to Override SIP Server
# 0 - No, 1 - Yes. Default is 1
# Number: 0, 1
# Mandatory
P1411 = 1

# Allow DHCP Option 242 (Avaya IP Phones). 0 - Disabled, 1 - Enabled. Default value is 1.
# Number: 0, 1
P22053 = 1

# Config Provision

# Download and Process All Available Config Files. 0 - No, 1 - Yes. Default is 0.
# 0 - No, If set to 1, WP820 will only download all the XML config files for provisioning: cfg.xml, cfg${max}.xml and cfgwp820.xml.  
# P8467 has higher priority than P8501 when set to 1.
# Number: 0, 1
# P8467 = 0

# List config file name in the preferred order separated by “;”. For example:
# cfg$mac;cfg$mac.xml;cfg$product.xml;cfg.xml
# String
# P8501

#PNP (3CX) Auto Provision. 0 - No, 1 - Yes. Default is 1.
P1414 = 1

####################################################################
# Maintenance/Upgrade/Advanced Settings                           ##
####################################################################
# Enable SIP NOTIFY Authentication. 1 - No, 0 - Yes. Default is 1
# Number: 0,1
# Mandatory
P4428 = 1

# Validate Server Certificates. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P22030 = 0

# mDNS Override Server. 0 - Disable, 1 - Use Type A, 2 - Use Type SRV. Default value is 1.
# Number: 0, 1, 2
# Mandatory
# Reboot
P1407 = 1

####################################################################
# Maintenance/System Diagnosis/Syslog                             ##
####################################################################
# Syslog Protocol. 0 - UDP, 1 - SSL/TLS. Default is 0
# Number: 0, 1
# Mandatory
P8402 = 0

# Syslog Server (name of the server, max length is 64 characters)
# Default is log.ipvideotalk.com
# String
P207 = log.ipvideotalk.com

# Syslog Level. 0 - NONE, 1 - DEBUG, 2 - INFO, 3 - WARNING, 4 - ERROR. Default is 0
# Number: 0, 1, 2, 3, 4
# Mandatory
P208 = 0

# Send SIP log. Default is 1.
# Number: 0, 1
P1387 = 1

# Syslog Keyword Filtering
# String
P22129 = 

####################################################################
# Maintenance/System Diagnosis/Logcat                             ##
####################################################################
# Log Tag (Not stored in pvalue)

# Log Priority (Not stored in pvalue)

####################################################################
# Maintenance/System Diagnosis/Debug                              ##
####################################################################
# One-click debugging
# Debug Info List (Not stored in pvalue)

# Core Dump
# Enable Core Dump Generation. 0 - Disabled, 1 - Enabled.
# Number: 0, 1. Default is 0
P29611 = 0

# Core Dump List (Not stored in pvalue)

# Record
# Recording List (Not stored in pvalue)

# Screenshot
# Screenshot List (Not stored in pvalue)


####################################################################
# Maintenance/System Diagnosis/Traceroute                         ##
####################################################################
# Target Host (Not stored in pvalue)

####################################################################
# Maintenance/Event Notification (Not stored in pvalue)           ##
####################################################################
# Boot Completed

# Incoming Call

# Outgoing Call

# Missed Call

# Connected 

# Disconnected

# DND On

# DND Off

# Forward On

# Forward Off

# Blind Transfer

# Attended Transfer

# Hold

# Unhold

# Log On

# Log Off

# Register

# Unregister

####################################################################
# Application/Contacts/General Settings                           ##
####################################################################
# Sort Phonebook by. 0 - Last Name. 1 - First Name. Default is 0
# Number: 0, 1
# Mandatory 
P2914 = 0

######################################################################
# Application/Contacts/Import/Export Contacts(Not stored in pvalue) ##
######################################################################

####################################################################
# Application/Contacts/Download Contacts                          ##
####################################################################
# Clear The Old List       0 - disabled, 1 or 2 - enabled
# Clear Old History Mode   1 - Clear all,  2 - Keep Local Contacts
# Note:'Clear The Old List ' and 'Clear Old History Mode' both set by P1435.
# P1435=0,  'Clear The Old List' is disabled.
# P1435=1,  'Clear The Old List' is enabled and 'Clear Old History Mode' is 'Clear all'.
# P1435=2,  'Clear The Old List' is enabled and 'Clear Old History Mode' is 'Keep Local Contacts'.
P1435 = 0

# Replace Duplicate Items    0 - disabled, 1 or 2 - enabled
# Replace Duplicate Entries Mode    1 - Replace by name,  2 - Replace by number
# 'Replace Duplicate Items ' and 'Replace Duplicate Entries Mode' both set by P1435.
# P1436=0,  'Replace Duplicate Items' is disabled.
# P1436=1,  'Replace Duplicate Items' is enabled and 'Replace Duplicate Entries Mode' is 'Replace by name'.
# P1436=2,  'Replace Duplicate Items' is enabled and 'Replace Duplicate Entries Mode' is 'Replace by number'.
# Number: 0, 1, 2
P1436 = 0

# Download Mode. 0 - No, 1 - YES, HTTP, 2 - YES, TFTP, 3 - Yes, HTTPS. Default is 0
# Number: 0, 1, 2, 3
# Mandatory
P330 = 0

# File Encoding
# GBK, UTF-8, UTF-16, UTF-32, Big5, Big5-HKSCS, Shift-JIS, ISO 2022-JP, KOI8-R, ISO8859-1, ISO8859-15, Windows-1251, EUC-KR
# P1681

# Download Server
# String
P331 =

# HTTP/HTTPS User name
# String
P6713 =

# HTTP/HTTPS Password
# String
P6714 =

# Automatic Download Interval. 0 - None, 5 - 5 min, 30 - 30 min, 60 - 1 Hour, 120 - 2 Hours, 240 - 4 Hours, 360 - 6 Hours, 480 - 8 Hours, 720 - 12 Hours. Default is 0.
# Number: 0, 5, 30, 60, 120, 240, 360, 480, 720
# Mandatory
P332 = 0

####################################################################
# Application/LDAP Phonebook                                      ##
####################################################################
# Connection Mode. 0 - LDAP, 1 - LDAPS. Default Value is 0
# Number : 0, 1
P8037 = 0

# Server Address
# LDAP Server Address, up to 256 characters can be used. It can be IP address or Domain name
# String
P8020 =

# Port
# Number: 1 - 65535. Default value is 389
P8021 = 389

# Base DN. The LDAP search base refers to the location in the directory where the search is requested to begin
# Example 1: dc=grandstream,dc=com
# Example 2: ou=Boston,dc=grandstream,dc=com
# String
P8022 =

# User Name. The bind "Username" for querying LDAP servers. Some LDAP servers allow anonymous binds in which case the setting can be left blank
# String
P8023 =

# Password. The bind "Password" for querying LDAP servers. And the field can be left blank if the LDAP server allows anonymous binds
# String
P8024 =

# LDAP Name Attributes. This setting specifies the "name" attributes of each record which are returned in the LDAP search result
# The setting allows the users to configure multiple space separated name attributes
# String
P8028 =

# LDAP Number Attributes. This setting specifies the "number" attributes of each record which are returned in the LDAP search result
# The setting allows the users to configure multiple space separated number attributes
# String
P8029 =

# LDAP Name Filter
# LDAP name filter is the filter used for name look ups. Please refer to usermanual for examples
# String
P8026 =

# LDAP Number Filter
# LDAP name filter is the filter used for number look ups. Please refer to usermanual for examples
# String
P8025 =

# Search Field Filter. 0 - All filter, 1 - Name Filter, 2 - Number Filter. Default is 0.
# Number: 0, 1, 2
# Pldap_search_field = 0

# LDAP Displaying Name Attributes. The entry information to be shown on phone LCD. Grandstream phones will display up to 3 fields
# String
P8030 =

# Max Hits. The setting specifies the maximum number of results to be returned by the LDAP server
# If the value is set to 0, server will return all search results. Default is 50
# Number: 0 - 32000
P8031 = 50

# Search Timeout (in seconds). Default is 4
# The setting specifies how long the server should process the request and client waits for server to return
# Number: 0 - 180
P8032 = 4

# LDAP Lookup For Dial. 0 - No, 1 - Yes. Default is 0
P8034 = 0

# LDAP Lookup For Incoming Calls. 0 - No, 1 - Yes. Default is 0
P8035 = 0

# LDAP Dialing Default Account. -1 - Default, 0 - Account 1, 1 - Account 2. Default is 0
# Number: -1 - 1
P22039 = -1

####################################################################
# Value-added Service/Door System                                 ##
####################################################################
# 10 GDS entries are supported. For each setting, the first P-value is for GDS1 and the last P-value is for GDS10.

# Door System Type. 0 - GDS, 1 - Others. Default is 0. (Also enables GDS 1-10)
# Number: 0, 1
P32001 = 1
P32006 = 1
P32011 = 1
P32016 = 1
P32021 = 1
P32026 = 1
P32031 = 1
P32036 = 1
P32041 = 1
P32046 = 1

# Door System Name
# String
# P32002 =
# P32007 =
# P32012 =
# P32017 =
# P32022 =
# P32027 =
# P32032 =
# P32037 =
# P32042 =
# P32047 =

# System Number
# String
# P32003 =
# P32008 =
# P32013 =
# P32018 =
# P32023 =
# P32028 =
# P32033 =
# P32038 =
# P32043 =
# P32048 =

# Access Password
# String
# P32004 =
# P32009 =
# P32014 =
# P32019 =
# P32024 =
# P32029 =
# P32034 =
# P32039 =
# P32044 =
# P32049 =

# System Ringtone (see ringtone value table).
# String
# P22241 = /system/media/audio/ringtones/DingDong.wav
# P22242 = /system/media/audio/ringtones/DingDong.wav
# P22243 = /system/media/audio/ringtones/DingDong.wav
# P22244 = /system/media/audio/ringtones/DingDong.wav
# P22245 = /system/media/audio/ringtones/DingDong.wav
# P22246 = /system/media/audio/ringtones/DingDong.wav
# P22247 = /system/media/audio/ringtones/DingDong.wav
# P22248 = /system/media/audio/ringtones/DingDong.wav
# P22249 = /system/media/audio/ringtones/DingDong.wav
# P22250 = /system/media/audio/ringtones/DingDong.wav

####################################################################
# Value-added Service/BroadSoft Directories/XSI Service Settings  ##
####################################################################
# Authentication Type. 0 - SIP Credentials, 1 - Login Credentials. Default is 1.
# Number: 0, 1
P22054 = 1

# Server
# String
P1591 = 

# Port
# Number: 0 - 65535
P1592 = 80

# Action Path
# String
P2937 = 

# BroadWorks User ID
# String
P22034 = 

# Login Password
# String
P22103 = 

# Broadsoft Directory & Call Logs Update Interval. Default is 1800.
# Number: 60 - 2147483647
# (P-value TBA)

# BroadSoft Directory Hits
# Number: 1 - 1000
P22014 = 

# Associated Broadsoft Account. 0 - Account 1, 1 - Account 2. Default is 0.
# Number: 0, 1
xsi_call_accountid = 1

# BroadSoft Directory Order
# (P-value TBA)

####################################################################
# Value-added Service/BroadSoft Directories/Network Directories   ##
####################################################################
# Group Directory
# Enable/Disable. Default is 1.
# Number: 0, 1
P2971 = 0

# Name
# String
P2972 = 

# Enterprise Directory
# Enable/Disable. Default is 1.
# Number: 0, 1
P2973 = 0

# Name
# String
P2974 = 

# Group Common
# Enable/Disable. Default is 1.
# Number: 0, 1
P2975 = 0

# Name
# String
P2976 = 

# Enterprise Common
# Enable/Disable. Default is 1.
# Number: 0, 1
P2977 = 0

# Name
# String
P2978 = 

# Personal Directory
# Enable/Disable. Default is 1.
# Number: 0, 1
P2979 = 0

# Name
# String
P2980 = 

# Missed Call Log
# Enable/Disable. Default is 1.
# Number: 0, 1
P2981 = 0

# Name
# String
P2982 = 

# Placed Call Log
# Enable/Disable. Default is 1.
# Number: 0, 1
P2983 = 0

# Name
# String
P2984 = 

# Received Call Log
# Enable/Disable. Default is 1.
# Number: 0, 1
P2985 = 0

# Name
# String
P2986 = 

####################################################################
# Value-added Service/SAFE/Panic Call                             ##
####################################################################
# WP8xx safety monitoring. 0 - off, 1 - on. Default is 0.
# P22259 = 0

# WP8xx no-movement sensitivity. 0 - Disable, 1 - Level 1 (lowest), 2 - Level 2, 3 - Level 3, 4 - Level 4, 5 - Level 5, 6 - Level 6, 7 - Level 7 (highest). Default 0.  
# Number: 0 - 7
# P22260 = 0

# WP8xx no-movement timeout. Default is 5.  
# Number: 5 - 300
# P22261 = 5

# WP8xx tilt sensitivity. 0 - Disable, 1 - Level 1 (lowest), 2 - Level 2, 3 - Level 3, 4 - Level 4, 5 - Level 5, 6 - Level 6, 7 - Level 7 (highest). Default 0.
# Number: 0 - 7
# P22262 = 0

# WP8xx tilt timeout 
# Number: 5 - 300
# P22263 = 5 

# WP8xx running sensitivity. 0 - Disable, 1 - Level 1 (lowest), 2 - Level 2, 3 - Level 3, 4 - Level 4, 5 - Level 5, 6 - Level 6, 7 - Level 7 (highest). Default 0.
# Number: 0 - 7
# P22264 = 0

# WP8xx running timeout 
# Number: 5 - 300
# P22265 = 5

# WP8xx snooze timeout 
# Number: 0 - 300
# P22266 = 0

# WP8xx warning timeout 
# Numnber: 5 - 60
# P22267 = 5

# WP8xx panic call silent alarm. 0 - Off, 1 - On. Default is 1.
# Number: 0, 1
# P22268 = 1

# WP8xx emergency call. 0 - Off, 1 - On. Default is 1.
# Number: 0, 1
# P22269 = 1 

# Associated Account. 0 - Account 1, 1 - Account 2. Default is 0.
# Number: 0, 1
# P22277 = 0

# Emergency Dial Force Speaker. 0 - Off, 1 - On. Default is 0.
# Number: 0, 1
# P22273 = 0

# WP8xx emergency call number
# String
# P22270 =

##################################Warning Tone Value Table##################################
# Web GUI Option                            Value
# Adara										/system/media/audio/notifications/Adara.ogg
# Aldebaran									/system/media/audio/notifications/Aldebaran.ogg
# Altair									/system/media/audio/notifications/Altair.ogg
# Alya										/system/media/audio/notifications/Alya.ogg
# Antares									/system/media/audio/notifications/Antares.ogg
# Antimony									/system/media/audio/notifications/Antimony.ogg
# Arcturus									/system/media/audio/notifications/Arcturus.ogg
# Argon										/system/media/audio/notifications/Argon.ogg
# Beat Box Android							/system/media/audio/notifications/Beat_Box_Android.ogg
# Bellatrix									/system/media/audio/notifications/Bellatrix.ogg
# Beryllium									/system/media/audio/notifications/Beryllium.ogg
# Betegeuse									/system/media/audio/notifications/Betegeuse.ogg
# Caffeinated Rattlesnake					/system/media/audio/notifications/CaffeineSnake.ogg
# Canopus									/system/media/audio/notifications/Canopus.ogg
# Capella									/system/media/audio/notifications/Capella.ogg
# Captain's Log								/system/media/audio/notifications/F1_New_MMS.ogg
# Castor									/system/media/audio/notifications/Castor.ogg
# Ceti Alpha								/system/media/audio/notifications/CetiAlpha.ogg
# Cobalt									/system/media/audio/notifications/Cobalt.ogg
# Cricket									/system/media/audio/notifications/Cricket.ogg
# Dear Deer									/system/media/audio/notifications/DearDeer.ogg
# Deneb										/system/media/audio/notifications/Deneb.ogg
# Doink										/system/media/audio/notifications/Doink.ogg
# Don't Panic								/system/media/audio/notifications/DontPanic.ogg
# Drip										/system/media/audio/notifications/Drip.ogg
# Electra									/system/media/audio/notifications/Electra.ogg
# Fluorine									/system/media/audio/notifications/Fluorine.ogg
# Fomalhaut									/system/media/audio/notifications/Fomalhaut.ogg
# Gallium									/system/media/audio/notifications/Gallium.ogg
# Heaven									/system/media/audio/notifications/Heaven.ogg
# Helium									/system/media/audio/notifications/Helium.ogg
# Highwire									/system/media/audio/notifications/Highwire.ogg
# Hojus										/system/media/audio/notifications/Hojus.ogg
# Iridium									/system/media/audio/notifications/Iridium.ogg
# Krypton									/system/media/audio/notifications/Krypton.ogg
# Kzurb Sonar								/system/media/audio/notifications/KzurbSonar.ogg
# Lalande									/system/media/audio/notifications/Lalande.ogg
# Look At Me								/system/media/audio/notifications/F1_New_SMS.ogg
# Merope									/system/media/audio/notifications/Merope.ogg
# Mira										/system/media/audio/notifications/Mira.ogg
# Missed It									/system/media/audio/notifications/F1_MissedCall.ogg
# Moonbeam									/system/media/audio/notifications/moonbeam.ogg
# On The Hunt								/system/media/audio/notifications/OnTheHunt.ogg
# Palladium									/system/media/audio/notifications/Palladium.ogg
# Pixie Dust								/system/media/audio/notifications/pixiedust.ogg
# Pizzicato									/system/media/audio/notifications/pizzicato.ogg
# Plastic Pipe 								/system/media/audio/notifications/Plastic_Pipe.ogg
# Polaris									/system/media/audio/notifications/Polaris.ogg
# Pollux									/system/media/audio/notifications/Pollux.ogg
# Procyon									/system/media/audio/notifications/Procyon.ogg
# Proxima									/system/media/audio/notifications/Proxima.ogg
# Radon										/system/media/audio/notifications/Radon.ogg
# Regulus									/system/media/audio/notifications/regulus.ogg
# Rubidium									/system/media/audio/notifications/Rubidium.ogg
# Selenium									/system/media/audio/notifications/Selenium.ogg
# Shaula									/system/media/audio/notifications/Shaula.ogg
# Sirius									/system/media/audio/notifications/sirius.ogg
# Sirrah									/system/media/audio/notifications/Sirrah.ogg
# Space Seed								/system/media/audio/notifications/SpaceSeed.ogg
# Spica										/system/media/audio/notifications/Spica.ogg
# Strontium									/system/media/audio/notifications/Strontium.ogg
# Syrma										/system/media/audio/notifications/Syrma.ogg
# Ta Da										/system/media/audio/notifications/TaDa.ogg
# Talitha									/system/media/audio/notifications/Talitha.ogg
# Tejat										/system/media/audio/notifications/Tejat.ogg
# Thallium									/system/media/audio/notifications/Thallium.ogg
# Thinkerbell								/system/media/audio/notifications/Tinkerbell.ogg
# Tweeters									/system/media/audio/notifications/tweeters.ogg
# Upsilon									/system/media/audio/notifications/Upsilon.ogg
# Vega										/system/media/audio/notifications/vega.ogg
# Voila										/system/media/audio/notifications/Voila.ogg
# Xenon										/system/media/audio/notifications/Xenon.ogg
# Zirconium									/system/media/audio/notifications/Zirconium.ogg
#
# WP8xx warning tone. Default is Xenon.
# P22271 = /system/media/audio/notifications/Xenon.ogg

##################################Alarm Tone Value Table##################################
# Argon										/system/media/audio/alarms/Argon.ogg
# Barium									/system/media/audio/alarms/Barium.ogg
# BeeBeep Alarm								/system/media/audio/alarms/Alarm_Beep_02.ogg
# Beep-Beep-Beep Alarm						/system/media/audio/alarms/Alarm_Beep_03.ogg
# Buzzer Alarm								/system/media/audio/alarms/Alarm_Buzzer.ogg
# Carbon									/system/media/audio/alarms/Carbon.ogg
# Cesium									/system/media/audio/alarms/Alarm_Classic.ogg
# Fermium									/system/media/audio/alarms/Fermium.ogg
# Hassium									/system/media/audio/alarms/Hassium.ogg
# Hellium									/system/media/audio/alarms/Helium.ogg
# Krypton									/system/media/audio/alarms/Krypton.ogg
# Neon										/system/media/audio/alarms/Neon.ogg
# Neptunium									/system/media/audio/alarms/Neptunium.ogg
# Nobelium									/system/media/audio/alarms/Nobelium.ogg
# Osmium									/system/media/audio/alarms/Osmium.ogg
# Oxygen									/system/media/audio/alarms/Oxygen.ogg
# Piezo Alarm								/system/media/audio/alarms/Alarm_Beep_01.ogg
# Platinum									/system/media/audio/alarms/Platinum.ogg
# Plutonium									/system/media/audio/alarms/Plutonium.ogg
# Rooster Alarm								/system/media/audio/alarms/Alarm_Rooster_02.ogg
# Scandium									/system/media/audio/alarms/Scandium.ogg
#
# WP8xx alarm tone. Default is Oxygen. 
# P22272 = /system/media/audio/alarms/Oxygen.ogg

####################################################################
# Handset/Speed Dial                                              ##
####################################################################
# Key 0 SpeedDial Account Index. 0 - Account 1, 1 - Account 2. Default is 0. 
# Number: 0, 1
# P23001 = 0 

# Key 0 SpeedDial Number
# String
# P23003 =

# Key 2 SpeedDial Account Index. 0 - Account 1, 1 - Account 2. Default is 0.
# Number: 0, 1
# P23011 = 0

# Key 2 SpeedDial Number
# String
# P23013 =

# Key 3 SpeedDial Account Index. 0 - Account 1, 1 - Account 2. Default is 0.
# Number: 0, 1
# P23016 = 0

# Key 3 SpeedDial Number
# String
# P23018 =

# Key 4 SpeedDial Account Index. 0 - Account 1, 1 - Account 2. Default is 0.
# Number: 0, 1
# P23021 = 0

# Key 4 SpeedDial Number
# String
# P23023 =

# Key 5 SpeedDial Account Index. 0 - Account 1, 1 - Account 2. Default is 0.
# Number: 0, 1
# P23026 = 0

# Key 5 SpeedDial Number
# String
# P23028 =

# Key 6 SpeedDial Account Index. 0 - Account 1, 1 - Account 2. Default is 0.
# Number: 0, 1
# P23031 = 0

# Key 6 SpeedDial Number
# String
# P23033 =

# Key 7 SpeedDial Account Index. 0 - Account 1, 1 - Account 2. Default is 0.
# Number: 0, 1
# P23036 = 0

# Key 7 SpeedDial Number
# String
# P23038 =

# Key 8 SpeedDial Account Index. 0 - Account 1, 1 - Account 2. Default is 0.
# Number: 0, 1
# P23041 = 0

# Key 8 SpeedDial Number
# String
# P23043 =

# Key 9 SpeedDial Account Index. 0 - Account 1, 1 - Account 2. Default is 0.
# Number: 0, 1
# P23046 = 0

# Key 9 SpeedDial Number
# String
# P23048 =

####################################################################
# Handset/Basic Setting/Display                                   ##
####################################################################
# LCD Font Size. 0 - Small, 1 - Normal, 2 - Large. Default is 1.
# Number: 0, 1, 2
# P22275 = 1