###############################################################################################
####            Configuration Template for Grandstream Wave                                ####
###############################################################################################
##############################################################################
##  Account 1 Settings                                                      ##
##############################################################################
#######################################################################
##  Account 1 General Settings                                       ##
#######################################################################
# Account Active. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P271 = 1

# Account Name
P270 =

# SIP Server
P47 =

# SIP User ID
P35 = 

# SIP Authentication ID
P36 = 

# SIP Authentication Password
P34 = 

# Voice Mail Access Number
P33 =

# Name (Display Name, e.g., John Doe)
P3 = 
#######################################################################
##  Account 1 Network Settings                                       ##
#######################################################################
# Outbound Proxy
P48 =

# Secondary Outbound Proxy
P2333 =

# DNS Mode. 0 - A Record, 1 - SRV, 2 - NAPTR/SRV. Default value is 0
# Number: 0, 1, 2
P103 = 0

# NAT Traversal. 0 - NAT No, 1 - STUN, 2 - Keep-alive, 3 - UPnP, 4 - Auto. Default value is 2
# Number: 0, 1, 2, 3, 4
P52 = 2

# Proxy-Require
P197 =
#######################################################################
##  Account 1 SIP Settings                                           ##
#######################################################################
# Unregister Before New Registration. 0 - Do Not Unregister, 1 - Unregister All, 2 - Unregister Single. Default value is 2
# Number: 0, 1, 2
P81 = 2

# Register Expiration (m). In minutes. Default value is 60
# Number: 0 - 64800
P32 = 60

# Local SIP Port. Default value is 5060
# Number: 5 - 65535
P40 = 5060

# Enable Session Timer/ Session Expiration(s).  In seconds. Default value is 180 seconds.
# By default,  Session Timer is Enabled.  Session Timer is disabled if the value is 0.
# Number: 0 or 90 - 64800
P260 = 180

# Min-SE(s). Default value is 90 seconds
# Number: 90 - 64800
P261 = 90

# UAC Specify Refresher. 0 - Omit, 1 - UAC, 2 - UAS. Default value is 0
# Number: 0, 1, 2
P266 = 0

# UAS Specify Refresher. 1 - UAC, 2 - UAS. Default value is 1
# Number: 1, 2
P267 = 1

# Force INVITE. Always refresh with INVITE instead of UPDATE even when remote party supports UPDATE
# 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P265 = 0

# Caller Request Timer. Request for timer when calling
# 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P262 = 0

# Callee Request Timer
# Request for timer when being called (i.e., if remote party supports timer but did not request for one)
# 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P263 = 0

# Force Timer. Still use timer when remote party does not support timer
# 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P264 = 0

# SIP Transport
# 0 - UDP , 1 - TCP, 2 - TLS. Default value is 0
# Number: 0, 1, 2
P130 = 0

# Only Accept SIP Requests from Known Servers
# 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P2347 = 0

# Check SIP User ID for Incoming INVITE
# 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P258 = 0
#######################################################################
##  Account 1 Codec Settings                                         ##
#######################################################################

# DTMF: in audio. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P2301 = 0

# DTMF: via RFC2833. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P2302 = 1

# DTMF: via SIP INFO. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P2303 = 0

# Preferred Vocoder
# First codec. -1 - NONE, 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 97 - iLBC, 123 - Opus, 3 - GSM. Default value is 0
# Number: -1, 0, 8, 9, 2, 97, 123, 3
P57 = 0

# Second codec. -1 - NONE, 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 97 - iLBC, 123 - Opus, 3 - GSM. Default value is 8
# Number: -1, 0, 8, 9, 2, 97, 123, 3
P58 = 8

# Third codec. -1 - NONE, 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 97 - iLBC, 123 - Opus, 3 - GSM. Default value is -1
# Number: -1, 0, 8, 9, 2, 97, 123, 3
P59 = -1

# Forth codec. -1 - NONE, 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 97 - iLBC, 123 - Opus, 3 - GSM. Default value is -1
# Number: -1, 0, 8, 9, 2, 97, 123, 3
P60 = -1

# Fifth codec. -1 - NONE, 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 97 - iLBC, 123 - Opus, 3 - GSM. Default value is -1
# Number: -1, 0, 8, 9, 2, 97, 123, 3
P61 = -1

# Sixth codec. -1 - NONE, 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 97 - iLBC, 123 - Opus, 3 - GSM. Default value is -1
# Number: -1, 0, 8, 9, 2, 97, 123, 3
P62 = -1

# Seventh codec. -1 - NONE, 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 97 - iLBC, 123 - Opus, 3 - GSM. Default value is -1
# Number: -1, 0, 8, 9, 2, 97, 123, 3
P63 = -1

# H.264 Image Size. 9 - 720P, 1 - VGA, 5 - CIF, 0 - QVGA, 6 - QCIF. Default value is 1
# Number: 9, 1, 5, 0, 6
P2307 = 1

# Video Bit Rate. 32 - 32 kbps, 64 - 64 kbps, 96 - 96 kbps, 128 - 128 kbps, 160 - 160 kbps, 192 - 192 kbps
# 210 - 210 kbps, 256 - 256 kbps, 384 - 384 kbps, 512 - 512 kbps, 640 - 640 kbps, 768 - 768 kbps
# 1024 - 1024 kbps. Default value is 512.
# Number: 32, 64, 96, 128, 160, 192, 210, 256, 384, 512, 640, 768, 1024.
P2315 = 512

# SDP Bandwidth Attribute. Default value is 1
# 0 - Standard, 1 - Media Level, 2 - Session Level, 3 - None
# Number: 0, 1, 2, 3
P2360 = 1

# H.264 Payload Type. Default value is 99
# Number
P293 = 99

# SRTP Mode. Default value is 0. 0 - Disable, 1 - Enable but not forced, 2 - Enable and forced.
# Number: 0, 1, 2
P183 = 0

# Enable SRTP Key Lifetime. 0 - No, 1 - Yes.
# Number: 0,1
P2363 = 1
#######################################################################
##  Account 1 Call Settings                                          ##
#######################################################################
# Dial Plan Prefix
# String
P66 =

# Dial Plan. Default value is { x+ | \+x+ | *x+ | *xx*x+ }
P290 = { x+ | \+x+ | *x+ | *xx*x+ }

# Auto Answer. 0 - No, 1 - Yes, 2 - Enable Intercom/Paging. Default value is 0
# Number: 0, 1, 2
P90 = 0

# Use # as Dial Key. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P72 = 1

# No Answer Timeout (s). Default value is 20
# Number: 1 - 120
P139 = 20
##############################################################################
##  Account 2 Settings                                                      ##
##############################################################################
#######################################################################
##  Account 2 General Settings                                       ##
#######################################################################

# Account Active. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P401 = 0

# Account Name
P417 =

# SIP Server
P402 = 

# SIP User ID
P404 = 

# SIP Authenticate ID
P405 = 

# SIP Authenticate Password
P406 = 

# Voice Mail UserID
P426 =

# Name (Display name, e.g., John Doe)
P407 = 

#######################################################################
##  Account 2 Network Settings                                       ##
#######################################################################

# Outbound Proxy
P403 =

# Secondary Outbound Proxy
P2433 =

# DNS Mode. 0 - A Record, 1 - SRV, 2 - NAPTR/SRV. Default value is 0
# Number: 0, 1, 2
P408 = 0

# NAT Traversal. 0 - No, 1 - STUN, 2 - Keep-alive, 3 - UPnP, 4 - Auto. Default value is 2
# Number: 0, 1, 2, 3, 4, 5
P414 = 2

# Proxy-Require
P418 =

#######################################################################
##  Account 2 SIP Settings                                           ##
#######################################################################

# Unregister Before New Registration. 0 - Do Not Unregister, 1 - Unregister All, 2 - Unregister Single. Default value is 2
# Number: 0, 1, 2
P411 = 2

# Register Expiration (m). In minutes. Default value is 60
# Number: 0 - 64800
P412 = 60

# Local SIP Port. Default value is 5062
# Number: 5 - 65535
P413 = 5062

# Session Expiration. In seconds. Default value is 180 seconds
# Number: 90 - 64800
P434 = 180

# Min-SE (s). Default value is 90 seconds
# Number: 90 - 64800
P427 = 90

# UAC Specify Refresher. 0 - Omit, 1 - UAC, 2 - UAS. Default value is 0
# Number: 0, 1, 2
P432 = 0

# UAS Specify Refresher. 1 - UAC, 2 - UAS. Default value is 1
# Number: 1, 2
P433 = 1

# Force INVITE (Always refresh with INVITE instead of UPDATE even when remote party supports UPDATE)
# 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P431 = 0

# Caller Request Timer (Request for timer when calling). 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P428 = 0

# Callee Request Timer (Request for timer when being called, i.e. if remote party supports timer but did not request for one)
# 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P429 = 0

# Force Timer (Still use timer when remote party does not support timer). 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P430 = 0

# SIP Transport. 0 - UDP, 1 - TCP, 2 - TLS. Default value is 0
# Number: 0, 1, 2
P448 = 0

# Only Accept SIP Requests from Known Servers. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P2447 = 0

# Check SIP User ID for Incoming INVITE
# 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P449 = 0
#######################################################################
##  Account 2 Codec Settings                                         ##
#######################################################################

# DTMF: in audio. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P2401 = 0

# DTMF: via RFC2833. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P2402 = 1

# DTMF: via SIP INFO. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P2403 = 0

# Preferred Vocoder
# First codec. -1 - NONE, 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 97 - iLBC, 123 - Opus, 3 - GSM. Default value is 0
# Number: -1, 0, 8, 9, 2, 97, 123, 3
P451 = 0

# Second codec. -1 - NONE, 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 97 - iLBC, 123 - Opus, 3 - GSM. Default value is 8
# Number: -1, 0, 8, 9, 2, 97, 123, 3
P452 = 8

# Third codec. -1 - NONE, 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 97 - iLBC, 123 - Opus, 3 - GSM. Default value is -1
# Number: -1, 0, 8, 9, 2, 97, 123, 3
P453 = -1

# Forth codec. -1 - NONE, 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 97 - iLBC, 123 - Opus, 3 - GSM. Default value is -1
# Number: -1, 0, 8, 9, 2, 97, 123, 3
P454 = -1

# Fifthcodec. -1 - NONE, 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 97 - iLBC, 123 - Opus, 3 - GSM. Default value is -1
# Number: -1, 0, 8, 9, 2, 97, 123, 3
P455 = -1

# Sixth codec. -1 - NONE, 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 97 - iLBC, 123 - Opus, 3 - GSM. Default value is -1
# Number: -1, 0, 8, 9, 2, 97, 123, 3
P456 = -1

# Seventh codec. -1 - NONE, 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 97 - iLBC, 123 - Opus, 3 - GSM. Default value is -1
# Number: -1, 0, 8, 9, 2, 97, 123, 3
P457 = -1

# H.264 Image Size. 9 - 720P, 1 - VGA, 5 - CIF, 0 - QVGA, 6 - QCIF. Default value is 1
# Number: 9, 1, 5, 0, 6
P2407 = 1

# Video Bit Rate. 32 - 32 kbps, 64 - 64 kbps, 96 - 96 kbps, 128 - 128 kbps, 160 - 160 kbps, 192 - 192 kbps
# 210 - 210 kbps, 256 - 256 kbps, 384 - 384 kbps, 512 - 512 kbps, 640 - 640 kbps, 768 - 768 kbps
# 1024 - 1024 kbps. Default value is 512.
# Number: 32, 64, 96, 128, 160, 192, 210, 256, 384, 512, 640, 768, 1024.
P2415 = 512

# SDP Bandwidth Attribute. Default value is 1
# 0 - Standard, 1 - Media Level, 2 - Session Level, 3 - None
P2460 = 1

# H.264 Payload Type
P462 = 99

# SRTP Mode. Default value is 0. 0 - Disable, 1 - Enable but not forced, 2 - Enable and forced.
# Number: 0, 1, 2.
P443 = 0

# Enable SRTP Key Lift Time. 0 - No, 1 - Yes.
# Number: 0,1
P2463 = 1

#######################################################################
##  Account 2 Call Settings                                          ##
#######################################################################

# Dial Plan Prefix
# String
P419 =

# Dial Plan. Default value is { x+ | \+x+ | *x+ | *xx*x+ }
P459 = { x+ | \+x+ | *x+ | *xx*x+ }

# Auto Answer. 0 - No, 1 - Yes, 2 - Enable Intercom/Paging. Default value is 0
# Number: 0, 1, 2
P425 = 0

# Use # as Dial Key. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P492 = 1

# No Answer Timeout (s). Default value is 20
# Number: 1 - 120.
P470 = 20
##############################################################################
##  Account 3 Settings                                                      ##
##############################################################################

#######################################################################
##  Account 3 General Settings                                       ##
#######################################################################

# Account Active. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P501 = 0

# Account Name
P517 =

# SIP Server
P502 =

# SIP User ID
P504 =

# SIP Authenticate ID
P505 =

# SIP Authenticate Password
P506 =

# Voice Mail UserID
P526 =

# Name (Display name: John Doe)
P507 =

# Show Account Name Only. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P2580 = 0

#######################################################################
##  Account 3 Network Settings                                       ##
#######################################################################

# Outbound Proxy
P503 =

# Secondary Outbound Proxy
P2533 =

# DNS Mode  0 - A Record, 1 - SRV, 2 - NAPTR/SRV. Default is 0
# Number: 0, 1, 2.
P508 = 0

# NAT Traversal. 0 - No, 1 - STUN, 2 - Keep-alive, 3 - UPnP, 4 - Auto. Default value is 2
# Number: 0, 1, 2, 3, 4
P514 = 2

# Proxy-Require
P518 =

#######################################################################
##  Account 3 SIP Settings                                           ##
#######################################################################

# Unregister Before New Registration. 0 - Do Not Unregister, 1 - Unregister All, 2 - Unregister Single. Default value is 2
# Number: 0, 1, 2
P511 = 2

# Register Expiration (m). In minutes. Default value is 60
# Number: 0 - 64800
P512 = 60

# Local SIP Port. Default value is 5064
# Number: 5 - 65535
P513 = 5064

# Session Expiration. In seconds. Default value is 180 seconds
# Number: 90 - 64800
P534 = 180

# Min-SE (s). Default value is 90 seconds
# Number: 5 - 65535
P527 = 90

# UAC Specify Refresher. 0 - Omit, 1 - UAC, 2 - UAS. Default value is 0
# Number: 0, 1, 2
P532 = 0

# UAS Specify Refresher. 1 - UAC, 2 - UAS. Default value is 1
# Number: 1, 2
P533 = 1

# Force INVITE (Always refresh with INVITE instead of UPDATE even when remote party supports UPDATE)
# 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P531 = 0

# Caller Request Timer (Request for timer when calling)
# 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1.
P528 = 0

# Callee Request Timer. Request for timer when called (i.e. if remote party supports timer but did not request for one)
# 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P529 = 0

# Force Timer (Still use timer when remote party does not support timer). 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P530 = 0

# SIP Transport. 0 - UDP, 1 - TCP, 2 - TLS. Default value is 0
# Number: 0, 1, 2
P548 = 0

# Only Accept SIP Requests from Known Servers. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P2547 = 0

# Check SIP User ID for Incoming INVITE
# 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P549 = 0
#######################################################################
##  Account 3 Codec Settings                                         ##
#######################################################################

# DTMF: in audio. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P2501 = 0

# DTMF: in RFC2833. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P2502 = 1

# DTMF: in SIP INFO. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P2503 = 0

# Preferred Vocoder
# First codec. -1 - NONE, 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 97 - iLBC, 123 - Opus, 3 - GSM. Default value is 0
# Number: -1, 0, 8, 9, 2, 97, 123, 3
P551 = 0

# Second codec. -1 - NONE, 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 97 - iLBC, 123 - Opus, 3 - GSM. Default value is 8
# Number: -1, 0, 8, 9, 2, 97, 123, 3
P552 = 8

# Third codec. -1 - NONE, 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 97 - iLBC, 123 - Opus, 3 - GSM. Default value is -1
# Number: -1, 0, 8, 9, 2, 97, 123, 3
P553 = -1

# Forth codec. -1 - NONE, 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 97 - iLBC, 123 - Opus, 3 - GSM. Default value is -1
# Number: -1, 0, 8, 9, 2, 97, 123, 3
P554 = -1

# Fifth codec. -1 - NONE, 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 97 - iLBC, 123 - Opus, 3 - GSM. Default value is -1
# Number: -1, 0, 8, 9, 2, 97, 123, 3
P555 = -1

# Sixth codec. -1 - NONE, 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 97 - iLBC, 123 - Opus, 3 - GSM. Default value is -1
# Number: -1, 0, 8, 9, 2, 97, 123, 3
P556 = -1

# Seventh codec. -1 - NONE, 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 97 - iLBC, 123 - Opus, 3 - GSM. Default value is -1
# Number: -1, 0, 8, 9, 2, 97, 123, 3
P557 = -1

# H.264 Image Size. 9 - 720P, 1 - VGA, 5 - CIF, 0 - QVGA, 6 - QCIF. Default value is 1
# Number: 9, 1, 5, 0, 6
P2507 = 1

# Video Bit Rate. 32 - 32 kbps, 64 - 64 kbps, 96 - 96 kbps, 128 - 128 kbps, 160 - 160 kbps, 192 - 192 kbps
# 210 - 210 kbps, 256 - 256 kbps, 384 - 384 kbps, 512 - 512 kbps, 640 - 640 kbps, 768 - 768 kbps
# 1024 - 1024 kbps. Default value is 512.
# Number: 32, 64, 96, 128, 160, 192, 210, 256, 384, 512, 640, 768, 1024.
P2515 = 2048

# SDP Bandwidth Attribute. Default value is 1
# 0 - Standard, 1 - Media Level, 2 - Session Level, 3 - None
P2560 = 1

# H.264 Payload Type
P562 = 99

# SRTP Mode. Default value is 0. 0 - Disable, 1 - Enable but not forced, 2 Enable and forced.
# Number: 0, 1, 2.
P543 = 0

# Enable SRTP Key Lift Time. 0 - No, 1 - Yes.
# Number: 0,1
P2563 = 1

#######################################################################
##  Account 3 Call Settings                                          ##
#######################################################################

# Dial Plan Prefix
# String
P519 =

# Dial Plan. Default value is { x+ | \+x+ | *x+ | *xx*x+ }
P559 = { x+ | \+x+ | *x+ | *xx*x+ }

# Auto Answer. 0 - No, 1 - Yes, 2 - Enable Intercom/Paging. Default value is 0
# Number: 0, 1, 2
P525 = 0

# Use # as Dial Key. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P592 = 1 

# No Answer Timeout (s). Default value is 20
# Number: 1 - 120
P570 = 20
##############################################################################
##  Account 4 Settings                                                      ##
##############################################################################

#######################################################################
##  Account 4 General Settings                                       ##
#######################################################################

# Account Active. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P601 = 

# Account Name
P617 =

# SIP Server
P602 =

# SIP User ID
P604 =

# SIP Authenticate ID
P605 =

# SIP Authenticate Password
P606 =

# Voice Mail UserID
P626 =

# Name (Display Name, e.g., John Doe)
P607 =

# Show Account Name Only. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P2680 = 0

#######################################################################
##  Account 4 Network Settings                                       ##
#######################################################################

# Outbound Proxy
P603 =

# Secondary Outbound Proxy
P2633 =

# DNS Mode. 0 - A Record, 1 - SRV, 2 - NAPTR/SRV. Default value is 0
# Number: 0, 1, 2
P608 = 0

# NAT Traversal. 0 - NAT No, 1 - STUN, 2 - Keep-alive, 3 - UPnP, 4 - Auto. Default value is 2
# Number: 0, 1, 2, 3, 4, 5
P614 = 2

# Proxy-Require
P618 =

#######################################################################
##  Account 4 SIP Settings                                           ##
#######################################################################

# Unregister Before New Registration. 0 - Do Not Unregister, 1 - Unregister All, 2 - Unregister Single. Default value is 2
# Number: 0, 1, 2
P611 = 2

# Register Expiration (m). In minutes. Default value is 60
# Number: 0 - 64800
P612 = 60

# Local SIP Port. Default value is 5066
# Number: 5 - 65535
P613 = 5066

# Session Expiration. In seconds. Default value is 180 seconds
# Number: 90 - 64800
P634 = 180

# Min-SE (s). Default value is 90 seconds
# Number: 90 - 64800
P627 = 90

# UAC Specify Refresher. 0 - Omit, 1 - UAC, 2 - UAS. Default value is 0
# Number: 0, 1, 2
P632 = 0

# UAS Specify Refresher. 1 - UAC, 2 - UAS. Default value is 1
# Number: 1, 2
P633 = 1

# Force INVITE. Always refresh with INVITE instead of UPDATE even when remote party supports UPDATE
# 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P631 = 0

# Caller Request Timer. Request for timer when calling. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P628 = 0

# Callee Request Timer. Request for timer when being called (i.e., if remote party supports timer but did not request for one)
# 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P629 = 0

# Force Timer. Still use timer when remote party does not support timer
# 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P630 = 0

# SIP Transport. 0 - UDP , 1 - TCP, 2 - TLS. Default value is 0
# Number: 0, 1, 2
P648 = 0

# Only Accept SIP Requests from Known Servers. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P2647 = 0

# Check SIP User ID for Incoming INVITE
# 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P649 = 0
#######################################################################
##  Account 4 Codec Settings                                         ##
#######################################################################

# DTMF: in audio. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P2601 = 0

# DTMF: via RFC2833. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P2602 = 1

# DTMF: via SIP INFO. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P2603 = 0

# Preferred Vocoder
# First codec. -1 - NONE, 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 97 - iLBC, 123 - Opus, 3 - GSM. Default value is 0
# Number: -1, 0, 8, 9, 2, 97, 123, 3
P651 = 0

# Second codec. -1 - NONE, 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 97 - iLBC, 123 - Opus, 3 - GSM. Default value is 8
# Number: -1, 0, 8, 9, 2, 97, 123, 3
P652 = 8

# Third codec. -1 - NONE, 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 97 - iLBC, 123 - Opus, 3 - GSM. Default value is -1
# Number: -1, 0, 8, 9, 2, 97, 123, 3
P653 = -1

# Forth codec. -1 - NONE, 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 97 - iLBC, 123 - Opus, 3 - GSM. Default value is -1
# Number: -1, 0, 8, 9, 2, 97, 123, 3
P654 = -1

# Fifth codec. -1 - NONE, 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 97 - iLBC, 123 - Opus, 3 - GSM. Default value is -1
# Number: -1, 0, 8, 9, 2, 97, 123, 3
P655 = -1

# Sixth codec. -1 - NONE, 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 97 - iLBC, 123 - Opus, 3 - GSM. Default value is -1
# Number: -1, 0, 8, 9, 2, 97, 123, 3
P656 = -1

# Seventh codec. -1 - NONE, 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 97 - iLBC, 123 - Opus, 3 - GSM. Default value is -1
# Number: -1, 0, 8, 9, 2, 97, 123, 3
P657 = -1

# H.264 Image Size. 9 - 720P, 1 - VGA, 5 - CIF, 0 - QVGA, 6 - QCIF. Default value is 1
# Number: 9, 1, 5, 4, 0, 6
P2607 = 1

# Video Bit Rate. 32 - 32 kbps, 64 - 64 kbps, 96 - 96 kbps, 128 - 128 kbps, 160 - 160 kbps, 192 - 192 kbps
# 210 - 210 kbps, 256 - 256 kbps, 384 - 384 kbps, 512 - 512 kbps, 640 - 640 kbps, 768 - 768 kbps
# 1024 - 1024 kbps. Default value is 512.
# Number: 32, 64, 96, 128, 160, 192, 210, 256, 384, 512, 640, 768, 1024.
P2615 = 512

# SDP Bandwidth Attribute. Default value is 1
# 0 - Standard, 1 - Media Level, 2 - Session Level, 3 - None
P2660 = 1

# H.264 Payload Type
P662 = 99

# SRTP Mode. Default value is 0. 0 - Disable, 1 - Enable but not forced, 2 Enable and forced.
# Number: 0, 1, 2.
P643 = 0

# Enable SRTP Key Lift Time. 0 - No, 1 - Yes.
# Number: 0,1
P2663 = 1

#######################################################################
##  Account 4 Call Settings                                          ##
#######################################################################

# Dial Plan Prefix
# String
P619 =

# Dial Plan. Default value is { x+ | \+x+ | *x+ | *xx*x+ }
P659 = { x+ | \+x+ | *x+ | *xx*x+ }

# Auto Answer. 0 - No, 1 - Yes, 2 - Enable Intercom/Paging. Default value is 0
# Number: 0, 1, 2
P625 = 0

# Use # as Dial Key. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P692 = 1

# No Answer Timeout (s). Default value is 20
# Number: 1 - 120
P670 = 20
##############################################################################
##  Account 5 Settings                                                      ##
##############################################################################

#######################################################################
##  Account 5 General Settings                                       ##
#######################################################################

# Account Active. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P1701 = 

# Account Name
P1717 =

# SIP Server
P1702 =

# SIP User ID
P1704 =

# SIP Authenticate ID
P1705 =

# SIP Authenticate Password
P1706 =

# Voice Mail UserID
P1726 =

# Name (Display name, e.g., John Doe)
P1707 =

# Show Account Name Only. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P2780 = 0

#######################################################################
##  Account 5 Network Settings                                       ##
#######################################################################

# Outbound Proxy
P1703 =

# Secondary Outbound Proxy
P2733 =

# DNS Mode. 0 - A Record, 1 - SRV, 2 - NAPTR/SRV. Default value is 0
# Number: 0, 1, 2.
P1708 = 0

# NAT Traversal. 0 - No, 1 - STUN, 2 - Keep-alive, 3 - UPnP, 4 - Auto. Default value is 2
# Number: 0, 1, 2, 3, 4
P1714 = 2

# Proxy-Require
P1718 =

#######################################################################
##  Account 5 SIP Settings                                           ##
#######################################################################

# Unregister Before New Registration. 0 - Do Not Unregister, 1 - Unregister All, 2 - Unregister Single. Default value is 2
# Number: 0, 1, 2
P1711 = 2

# Register Expiration (m). In minutes. Default value is 60
# Number: 0 - 64800
P1712 = 60

# Local SIP Port. Default value is 5068
# Number: 5 - 65535
P1713 = 5068

# SUBSCRIBE for MWI. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P1715 = 0

# Session Expiration. In seconds. Default value is 180 seconds
# Number: 90 - 64800
P1734 = 180

# Min-SE (s). Default value is 90 seconds
# Number is 90 - 64800
P1727 = 90

# UAC Specify Refresher. 0 - Omit, 1 - UAC, 2 - UAS. Default value is 0
# Number: 0, 1, 2
P1732 = 0

# UAS Specify Refresher. 1 - UAC, 2 - UAS. Default value is 1
# Number: 1, 2
P1733 = 1

# Force INVITE (Always refresh with INVITE instead of UPDATE even when remote party supports UPDATE)
# 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P1731 = 0

# Caller Request Timer (Request for timer when calling). 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P1728 = 0

# Callee Request Timer (Request for timer when being called, i.e. if remote party supports timer but did not request for one)
# 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P1729 = 0

# Force Timer (Still use timer when remote party does not support timer). 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P1730 = 0

# SIP Transport. 0 - UDP, 1 - TCP, 2 - TLS. Default value is 0
# Number: 0, 1, 2
P1748 = 0

# Only Accept SIP Requests from Known Servers. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P2747 = 0

# Check SIP User ID for Incoming INVITE
# 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P1749 = 0
#######################################################################
##  Account 5 Codec Settings                                         ##
#######################################################################

# DTMF: in audio. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P2701 = 0

# DTMF: via RFC2833. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P2702 = 1

# DTMF: via SIP INFO. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P2703 = 0

# Preferred Vocoder
# First codec. -1 - NONE, 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 97 - iLBC, 123 - Opus, 3 - GSM. Default value is 0
# Number: -1, 0, 8, 9, 2, 97, 123, 3
P1751 = 0

# Second codec. -1 - NONE, 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 97 - iLBC, 123 - Opus, 3 - GSM. Default value is 8
# Number: -1, 0, 8, 9, 2, 97, 123, 3
P1752 = 8

# Third codec. -1 - NONE, 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 97 - iLBC, 123 - Opus, 3 - GSM. Default value is -1
# Number: -1, 0, 8, 9, 2, 97, 123, 3
P1753 = -1

# Forth codec. -1 - NONE, 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 97 - iLBC, 123 - Opus, 3 - GSM. Default value is -1
# Number: -1, 0, 8, 9, 2, 97, 123, 3
P1754 = -1

# Fifth codec. -1 - NONE, 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 97 - iLBC, 123 - Opus, 3 - GSM. Default value is -1
# Number: -1, 0, 8, 9, 2, 97, 123, 3
P1755 = -1

# Sixth codec. -1 - NONE, 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 97 - iLBC, 123 - Opus, 3 - GSM. Default value is -1
# Number: -1, 0, 8, 9, 2, 97, 123, 3
P1756 = -1

# Seventh codec. -1 - NONE, 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 97 - iLBC, 123 - Opus, 3 - GSM. Default value is -1
# Number: -1, 0, 8, 9, 2, 97, 123, 3
P1757 = -1

# H.264 Image Size. 9 - 720P, 1 - VGA, 5 - CIF, 0 - QVGA, 6 - QCIF. Default value is 1
# Number: 9, 1, 5, 0, 6
P2707 = 1

# Video Bit Rate. 32 - 32 kbps, 64 - 64 kbps, 96 - 96 kbps, 128 - 128 kbps, 160 - 160 kbps, 192 - 192 kbps
# 210 - 210 kbps, 256 - 256 kbps, 384 - 384 kbps, 512 - 512 kbps, 640 - 640 kbps, 768 - 768 kbps
# 1024 - 1024 kbps. Default value is 512.
# Number: 32, 64, 96, 128, 160, 192, 210, 256, 384, 512, 640, 768, 1024.
P2715 = 512

# SDP Bandwidth Attribute. Default value is 1
# 0 - Standard, 1 - Media Level, 2 - Session Level, 3 - None
P2760 = 1

# H.264 Payload Type
P1762 = 99

# SRTP Mode. Default value is 0. 0 - Disable, 1 - Enable but not forced, 2 Enable and forced.
# Number: 0, 1, 2.
P1743 = 0

# Enable SRTP Key Lift Time. 0 - No, 1 - Yes.
# Number: 0,1
P2763 = 1

#######################################################################
##  Account 5 Call Settings                                          ##
#######################################################################

# Dial Plan Prefix
# String
P1719 =

# Dial Plan Maxlength: unlimited, default is allow all { x+ | *x+ | *xx*x+ }
P1759 = { x+ | \+x+ | *x+ | *xx*x+ }

# Auto Answer. 0 - No, 1 - Yes, 2 - Enable Intercom/Paging. Default value is 0
# Number: 0, 1, 2
P1725 = 0

# Use # as Dial Key. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P1792 = 1

# No Answer Timeout (s). Default value is 20
# Number: 1 - 120
P1770 = 20
##############################################################################
##  Account 6 Settings                                                      ##
##############################################################################

#######################################################################
##  Account 6 General Settings                                       ##
#######################################################################

# Account Active. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P1801 = 1

# Account Name
P1817 = 

# SIP Server
P1802 = 

# SIP User ID
P1804 = 

# SIP Authenticate ID
P1805 =

# SIP Authenticate Password
P1806 =

# Voice Mail UserID
P1826 =

# Name (Display name :John Doe)
P1807 =

# Show Account Name Only. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P2880 = 0

#######################################################################
##  Account 6 Network Settings                                       ##
#######################################################################

# Outbound Proxy
P1803 =

# Secondary Outbound Proxy
P2833 =

# DNS Mode. 0 - A Record, 1 - SRV, 2 - NAPTR/SRV. Default is 0
# Number: 0, 1, 2
P1808 = 0

# NAT Traversal. 0 - No, 1 - STUN, 2 - Keep-alive, 3 - UPnP, 4 - Auto. Default value is 2
# Number: 0, 1, 2, 3, 4
P1814 = 2

# Proxy-Require
P1818 =

#######################################################################
##  Account 6 SIP Settings                                           ##
#######################################################################

# Unregister Before New Registration. 0 - Do Not Unregister, 1 - Unregister All, 2 - Unregister Single. Default value is 2
# Number: 0, 1, 2
P1811 = 2

# Register Expiration (m). In minutes. Default value is 60
# Number: 0 - 64800
P1812 = 60

# Local SIP Port. Default value is 5070
# Number: 5-65535
P1813 = 5070

# Session Expiration (in seconds). Default value is 180 seconds
# Number: 90 - 64800
P1834 = 180

# Min-SE (s). Default value is 90 seconds
# Number: 5 - 65535
P1827 = 90

# UAC Specify Refresher. 0 - Omit, 1 - UAC, 2 - UAS. Default value is 0
# Number: 0, 1, 2
P1832 = 0

# UAS Specify Refresher. 1 - UAC, 2 - UAS. Default value is 1
# Number: 1, 
P1833 = 1

# Force INVITE (Always refresh with INVITE instead of UPDATE even when remote party supports UPDATE)
# 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P1831 = 0

# Caller Request Timer (Request for timer when calling)
# 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P1828 = 0

# Callee Request Timer. Request for timer when called (i.e. if remote party supports timer but did not request for one)
# 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P1829 = 0

# Force Timer (Still use timer when remote party does not support timer). 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P1830 = 0

# SIP Transport. 0 - UDP, 1 - TCP, 2 - TLS. Default value is 0
# Number: 0, 1, 2
P1848 = 0

# Only Accept SIP Requests from Known Servers. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P2847 = 0

# Check SIP User ID for Incoming INVITE
# 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P1849 = 0
#######################################################################
##  Account 6 Codec Settings                                         ##
#######################################################################

# DTMF: in audio. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P2801 = 0

# DTMF: in RFC2833. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P2802 = 1

# DTMF: in SIP INFO. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P2803 = 0

# Preferred Vocoder
# First codec. -1 - NONE, 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 97 - iLBC, 123 - Opus, 3 - GSM. Default value is 0
# Number: -1, 0, 8, 9, 2, 97, 123, 3
P1851 = 0

# Second codec. -1 - NONE, 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 97 - iLBC, 123 - Opus, 3 - GSM. Default value is 8
# Number: -1, 0, 8, 9, 2, 97, 123, 3
P1852 = 8

# Third codec. -1 - NONE, 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 97 - iLBC, 123 - Opus, 3 - GSM. Default value is -1
# Number: -1, 0, 8, 9, 2, 97, 123, 3
P1853 = -1

# Forth codec. -1 - NONE, 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 97 - iLBC, 123 - Opus, 3 - GSM. Default value is -1
# Number: -1, 0, 8, 9, 2, 97, 123, 3
P1854 = -1

# Fifth codec. -1 - NONE, 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 97 - iLBC, 123 - Opus, 3 - GSM. Default value is -1
# Number: -1, 0, 8, 9, 2, 97, 123, 3
P1855 = -1

# Sixth codec. -1 - NONE, 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 97 - iLBC, 123 - Opus, 3 - GSM. Default value is -1
# Number: -1, 0, 8, 9, 2, 97, 123, 3
P1856 = -1

# Seventh codec. -1 - NONE, 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 97 - iLBC, 123 - Opus, 3 - GSM. Default value is -1
# Number: -1, 0, 8, 9, 2, 97, 123, 3
P1857 = -1

# H.264 Image Size. 9 - 720P, 1 - VGA, 5 - CIF, 0 - QVGA, 6 - QCIF. Default value is 1
# Number: 9, 1, 5, 0, 6
P2807 = 1

# Video Bit Rate. 32 - 32 kbps, 64 - 64 kbps, 96 - 96 kbps, 128 - 128 kbps, 160 - 160 kbps, 192 - 192 kbps
# 210 - 210 kbps, 256 - 256 kbps, 384 - 384 kbps, 512 - 512 kbps, 640 - 640 kbps, 768 - 768 kbps
# 1024 - 1024 kbps. Default value is 512.
# Number: 32, 64, 96, 128, 160, 192, 210, 256, 384, 512, 640, 768, 1024.
P2815 = 512

# SDP Bandwidth Attribute. Default value is 1
# 0 - Standard, 1 - Media Level, 2 - Session Level, 3 - None
P2860 = 1

# H.264 Payload Type
P1862 = 99

# SRTP Mode. Default value is 0. 0 - Disable, 1 - Enable but not forced, 2 Enable and forced.
# Number: 0, 1, 2.
P1843 = 0

# Enable SRTP Key Lift Time. 0 - No, 1 - Yes.
# Number: 0,1
P2863 = 1

#######################################################################
##  Account 6 Call Settings                                          ##
#######################################################################
# Dial Plan Prefix
# String
P1819 =

# Dial Plan. Default value is { x+ | \+x+ | *x+ | *xx*x+ }
P1859 = { x+ | \+x+ | *x+ | *xx*x+ }

# Auto Answer. 0 - No, 1 - Yes, 2 - Enable Intercom/Paging. Default value is 0
# Number: 0, 1
P1825 = 0

# Use # as Dial Key. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P1892 = 1 

# No Answer Timeout (s). Default value is 20
# Number: 1 - 120
P1870 = 20
##############################################################################
##  Advanced Settings                                                       ##
##############################################################################

#######################################################################
##  Advanced Settings - Audio Settings                               ##
#######################################################################
# Noise Rduction Level. 0 - Low, 1 - Middle, 2 - High. Default value is 1.
# Number: 0, 1, 2
P2358 = 1

#######################################################################
##  Advanced Settings -> Network Settings                            ##
#######################################################################
# Use Random Port. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P78 = 1

# STUN Server
P76 = stun.ipvideotalk.com

# Layer 3 QoS for SIP. Default value is 48
P1558 = 48

# Layer 3 QoS for Audio. Default value is 48
P1559 = 48

#######################################################################
##  Advanced Settings - Other Settings                               ##
#######################################################################

# Config Server Path
P237 = labtest1.grandstream.com/William

# LDAP Lookup For Dial. 0 - No, 1 - Yes. Default is 0
P8034 = 1

# LDAP Lookup For Incoming Calls. 0 - No, 1 - Yes. Default is 0
P8035 = 1

# Server Address, up to 256 characters can be used. It can be IP address or Domain name
# String
P8020 =

# Port. Default value is 389
# Number: 1 - 65535
P8021 = 389

# Base DN. The LDAP search base refers to the location in the directory where the search is requested to begin
# Example 1: dc=grandstream,dc=com
# Example 2: ou=Boston, dc=grandstream,dc=com
# String
P8022 =

# User Name. The bind "Username" for querying LDAP servers. Some LDAP servers allow anonymous binds in which case the setting can be left blank
# String
P8023 =

# Password. The bind "Password" for querying LDAP servers. And the field can be left blank if the LDAP server allows anonymous binds
# String
P8024 =

# LDAP Name Attributes. This setting specifies the "name" attributes of each record which are returned in the LDAP search result
# The setting allows the users to configure multiple space separated name attributes
# String
P8028 =

# LDAP Number Attributes. This setting specifies the "number" attributes of each record which are returned in the LDAP search result
# The setting allows the users to configure multiple space separated number attributes
# String
P8029 =

# LDAP Name Filter
# LDAP name filter is the filter used for name look ups. Please refer to usermanual for examples
# String
P8026 =

# LDAP Number Filter
# LDAP name filter is the filter used for number look ups. Please refer to usermanual for examples
# String
P8025 =

# LDAP Displaying Name Attributes. The entry information to be shown on phone LCD. Grandstream Wave will display up to 3 fields
# String
P8030 =

# Max Hits. The setting specifies the maximum number of results to be returned by the LDAP server
# If the value is set to 0, server will return all search results. Default is 100
# Number: 0 - 32000
P8031 = 100

# Search Timeout (in milliseconds). Default is 10000
# The setting specifies how long the server should process the request and client waits for server to return
P8032 = 10000

# Connection Mode. 0 - LDAP, 1 - LDAPS. Default Value is 0
# Number : 0, 1
P8037 = 0


