################################################################################################
##                General Configuration Template for GDS3710 Door System         			  ##
##                        (Firmware Version:   1.0.7.8)                                       ##
################################################################################################

################################################################################################
##                              Door System Settings                                          ##
################################################################################################

	##### ALMOUT1 Feature #####
	## P15450
	## value: 0/1 (0:Alarm Output  1:Open Door)
	
	##### ALMOUT1 Status #####
	## P15470
	## value: 0/1 (0:Normal Close	1:Normal Open)
	
	##### Control Options #####
	## P15467
	## value: 0/1/2/3 (0:Door 1  1:Door 2  2:Door 1 & Door 2  3:None)
	
	##### Wiegand Control Options #####
	## P15468
	## value: 0/1/2/3 (0:Door 1  1:Door 2  2:Door 1 & Door 2  3:None)
	
	##### Delay before Unlock(s) #####
	## P14100
	## value: 0 - 20 (Integer)
	
	##### Delay before Unlock(s) (For the second door)#####
	## P15465
	## value: 0 - 20 (Integer)
	
	##### Unlock Holding Time(s) #####
	## P14101
	## value: 1 - 20 (Integer)
	
	##### Unlock Holding Time(s) (For the second door)#####
	## P15466
	## value: 1 - 20 (Integer)
	
	##### Min. Interval of Swiping Card(ms) #####
	## P14829
	## value: 0 - 2000 (Integer)
	
	##### Number of Snapshots when Door Opened #####
	## P15474
	## value: 0 - 4 and no more than 'Unlock Action Holding Time' value (Integer)
	
	##### Number of Snapshots when Door Opened (For the second door) #####
	## P15475
	## value: 0 - 4 and no more than 'Unlock Action Holding Time (For the second door)' value (Integer)
	
	##### Snapshot when Door Opened -- via FTP  #####
	## P14103
	## value: 0/1 (0:Disable  1:Enable)
	
	##### Snapshot when Door Opened -- via Enail  #####
	## P15471
	## value: 0/1 (0:Disable  1:Enable)
	
	##### Snapshot when Doorbell Pressed -- via FTP #####
	## P15420
	## value: 0/1 (0:Disable  1:Enable)
	
	##### Snapshot when Doorbell Pressed -- via Email #####
	## P15409
	## value: 0/1 (0:Disable  1:Enable)
	
	##### Call Mode #####
	## P14856
	## value: 0/1 (0:Virtual Number 1:SIP Number)
	
	##### Doorbell Mode #####
	## P14827
	## value: 0/1/2 (0:Call Doorbell Number 1:Control Doorbell Output 2:Both of the above)
	
	##### Door Bell Call Mode #####
	## P15434
	## value: 0/1 (0:Serial Hunting 1:Parallel Hunting)

	##### Number Called When Door Bell Pressed #####
	## P10462
	## value: A pure digital string. Example: 6688
	
	##### Maximum Number of Dialed Digits #####
	## P15419
	## value: 0 - 20 (Integer)	Default 0
	
	##### No Key Input Timeout(s) #####
	## P15436
	## value: 1 - 15  (Integer)
	
	##### Press Doorbell Schedule #####
	## P15418
	## value: 0 - 10 profile. (Integer) Default 0
	
	##### Remote PIN to Open the Door #####
	## P10457
	## value: A pure digital string, MAX length is 8. Example: 6688
	
	##### Remote PIN to Open the Door (For the second door)#####
	## P15460
	## value: A pure digital string, MAX length is 8. Example: 6688
	
	##### Local PIN Type #####
	## P10464
	## value: 0/1/2 (0:Private Card PIN  1:Unified PIN  2:Card + Private PIN)
	
	##### Unified PIN Open Door Options #####
	## P15461
	## value: 0/1/2/3 (0:Door 1  1:Door 2  2:Door 1 & Door 2  3:None)
	
	##### Local PIN to Open the Door #####
	## P10463
	## value: A pure digital string, MAX length is 8. Example: 6688
	
	##### Enable Guest PIN #####
	## P14850
	## value: 0/1 (0:Disable  1:Enable)

	##### Guest PIN #####
	## P14851
	## value: A pure digital string, MAX length is 8. Example: 6688
	
	##### Guest PIN Open Door Options #####
	## P15462
	## value: 0/1/2/3 (0:Door 1  1:Door 2  2:Door 1 & Door 2  3:None)
	
	##### Guest PIN Duration Start Time #####
	## P14852
	## value: A pure digital string, Example: 2017/02/28 02:31:56 value:20170228023156
	
	##### Guest PIN Duration End Time #####
	## P14853
	## value: A pure digital string, Example: 2017/02/28 02:31:56 value:20170228023156
	
	##### Disable Auto Answer #####
	## P14580
	## value: 0/1 	(0:Disable  1:Enable)
	
	##### Enable Doorbell Button to Hang Up Call #####
	## P14582
	## value: 0/1 	(0:Disable  1:Enable)
	
	##### Disable Keypad (except Doorbell Button) #####
	## P15421
	## value: 0/1 	(0:Disable  1:Enable)
	
	##### Enable On Hook After Remote Unlock #####
	## P15422
	## value: 0/1 	(0:Disable  1:Enable)
	
	##### Enable HTTP API Remote Open Door #####
	## P15424
	## value: 0/1 	(0:Disable  1:Enable  default 0)
	
	##### Open Door IDCode Valid Time #####
	## P15428
	## value: 5 - 300 (s) . (Integer)  Default 30
	
	##### Enable DTMF Open Door #####
	## P14858
	## value: 0/1 	(0:Disable  1:Enable)
	
	##### Card Issuing Mode Effective Time #####
	## P15423
	## value: 1 - 1440 (Integer)
	
	##### Enable Key Blue Light #####
	## P14800
	## value: 0/1 	(0:Disable  1:Enable)
	
	##### Enable Background Light #####
	## P14801
	## value: 0/1	(0:Disable  1:Enable)
	
	##### Enable Blue Doorbell Light #####
	## P14562
	## value: 0/1	(0:Disable  1:Enable)
	
	##### Blue Doorbell Light Lighting Start Time #####
	## P14560
	## value: A pure digital string, MAX length is 6. Example: 125900 -> 12:59:00
	
	##### Blue Doorbell Light Lighting End Time #####
	## P14561
	## value: A pure digital string, MAX length is 6. Example: 125900 -> 12:59:00
	
	##### Enable Blue Keypad Light #####
	## P15500
	## value: 0/1	(0:Disable  1:Enable)
	
	##### Blue Keypad Light Lighting Start Time #####
	## P15501
	## value: A pure digital string, MAX length is 6. Example: 125900 -> 12:59:00
	
	##### Blue Keypad Light Lighting End Time #####
	## P15502
	## value: A pure digital string, MAX length is 6. Example: 125900 -> 12:59:00
	
	##### Central Mode #####
	## P15301
	## value: 0/1	(0:Disable  1:Enable)
	
	##### Key Tone Type #####
	## P14340
	## value: 0/1/2	(0:Default 1:DTMF 2:Mute)

	##### Wiegand Input Enable #####
	## P14120
	## value: 0/1	(0:Disable  1:Enable)
	
	##### Wiegand Output #####
	## P14121
	## value: 0/1/2	(0:Disabled  1:Relay and  Local Authentication  2:Relay and Bypass Local)
	
	######################################  Keep Door Open   ######################################
	##### Keep Door Open #####
	## P15429
	## value: 0: Disable  1:Immediate Open Door  2:Schedule Open Door
	
	##### Emergency PIN to Disable Keep Door Open #####
	## P15435
	## value: Digital string. Max.Length=8
	
	##### Length(m) to Keep Door Open #####
	## P15430
	## value: 5 - 480	(Integer)
	
	##### Schedule Start Time #####
	## P15211
	## value: Digital string. Example:20180516000000
	
	##### Schedule End Time #####
	## P15212
	## value: Digital string. Example:20180516000000
	
	##### Holiday Mode #####
	## P15506
	## value: 0 - 10
	
	##### Schedule Table #####
	## P15213
	## value: string. Format:door_sch,0@start_time@end_time,  Example:door_sch,0@0000@2359,
	
	
	##### Keep Door Open (For the second door)#####
	## P15455
	## value: 0: Disable  1:Immediate Open Door  2:Schedule Open Door
	
	##### Emergency PIN to Disable Keep Door Open (For the second door) #####
	## P15472
	## value: Digital string. Max.Length=8
	
	##### Length(m) to Keep Door Open(min) (For the second door)#####
	## P15456
	## value: 5 - 480	(Integer)
	
	##### Schedule Start Time (For the second door)#####
	## P15457
	## value: Digital string. Example:20180516000000
	
	##### Schedule End Time (For the second door)#####
	## P15458
	## value: Digital string. Example:20180516000000
	
	##### Holiday Mode #####
	## P15507
	## value: 0 - 10
	
	##### Schedule Table (For the second door)#####
	## P15459
	## value: string. Format:door_sch,0@start_time@end_time,  Example:door_sch,0@0000@2359,

	######################################  Group Settings   ######################################
	##### Group string #####
	## P15300
	## value: Format:index@scheduleX@name. Example:1@1@info,2@1@test,
	
	
	######################################  Schedule Settings   ######################################
	##### Schedule string 0 #####
	## P15200
	## value: Format: name@holiday_mode,weekday@start_time@end_time,weekday@start_time@end_time,
	## Example: rest@0,0@1200@1300,
	
	##### Schedule string 1 #####
	## P15201
	## value: Format: name@holiday_mode,weekday@start_time@end_time,weekday@start_time@end_time,
	## Example: rest@0,0@1200@1300,
	
	##### Schedule string 2 #####
	## P15202
	## value: Format: name@holiday_mode,weekday@start_time@end_time,weekday@start_time@end_time,
	## Example: rest@0,0@1200@1300,
	
	##### Schedule string 3 #####
	## P15203
	## value: Format: name@holiday_mode,weekday@start_time@end_time,weekday@start_time@end_time,
	## Example: rest@0,0@1200@1300,
	
	##### Schedule string 4 #####
	## P15204
	## value: Format: name@holiday_mode,weekday@start_time@end_time,weekday@start_time@end_time,
	## Example: rest@0,0@1200@1300,
	
	##### Schedule string 5 #####
	## P15205
	## value: Format: name@holiday_mode,weekday@start_time@end_time,weekday@start_time@end_time,
	## Example: rest@0,0@1200@1300,
	
	##### Schedule string 6 #####
	## P15206
	## value: Format: name@holiday_mode,weekday@start_time@end_time,weekday@start_time@end_time,
	## Example: rest@0,0@1200@1300,
	
	##### Schedule string 7 #####
	## P15207
	## value: Format: name@holiday_mode,weekday@start_time@end_time,weekday@start_time@end_time,
	## Example: rest@0,0@1200@1300,
	
	##### Schedule string 8 #####
	## P15208
	## value: Format: name@holiday_mode,weekday@start_time@end_time,weekday@start_time@end_time,
	## Example: rest@0,0@1200@1300,
	
	##### Schedule string 9 #####
	## P15209
	## value: Format: name@holiday_mode,weekday@start_time@end_time,weekday@start_time@end_time,
	## Example: rest@0,0@1200@1300,
	
	
	######################################  Holiday Settings   ######################################
	##### Holiday string 1 #####
	## P15250
	## value: Format: name,start_date@end_date, Example: hahaha,20170708@20170910,
	
	##### Holiday string 2 #####
	## P15251
	## value: Format: name,start_date@end_date, Example: hahaha,20170708@20170910,
	
	##### Holiday string 3 #####
	## P15252
	## value: Format: name,start_date@end_date, Example: hahaha,20170708@20170910,
	
	##### Holiday string 4 #####
	## P15253
	## value: Format: name,start_date@end_date, Example: hahaha,20170708@20170910,
	
	##### Holiday string 5 #####
	## P15254
	## value: Format: name,start_date@end_date, Example: hahaha,20170708@20170910,
	
	##### Holiday string 6 #####
	## P15255
	## value: Format: name,start_date@end_date, Example: hahaha,20170708@20170910,
	
	##### Holiday string 7 #####
	## P15256
	## value: Format: name,start_date@end_date, Example: hahaha,20170708@20170910,
	
	##### Holiday string 8 #####
	## P15257
	## value: Format: name,start_date@end_date, Example: hahaha,20170708@20170910,
	
	##### Holiday string 9 #####
	## P15258
	## value: Format: name,start_date@end_date, Example: hahaha,20170708@20170910,
	
	##### Holiday string 10 #####
	## P15259
	## value: Format: name,start_date@end_date, Example: hahaha,20170708@20170910,
	
################################################################################################
##                              System Settings                                               ##
################################################################################################	

######			    			  Date & Time 											  ######

# TimeZone
# 1  --GMT-12 		(Eniwetok, Kwajalein)
# 2  --GMT-11 		(Midway Isl., Samoa)
# 3  --GMT-10 		(Hawaii, Aleutian Isl.)
# 4  --GMT-09  		(Alaska)
# 5  --GMT-08  		(Las Vegas, San Francisco, Vancouver)
# 6  --GMT-07  		(Calgary, Denver, Salt Lake City)
# 7  --GMT-06  		(Chicago, Dallas, Mexico City)
# 8  --GMT-05  		(Cuba)
# 9  --GMT-05  		(New York, Toronto, Washington DC)
# 10 --GMT-04  		(Paraguay)
# 11 --GMT-04  		(Chile)
# 12 --GMT-04  		(Charlottetown, Manaus)
# 55 --GMT-04  		(Charlottetown, Manaus)
# 13 --GMT-03  		(Brazilia, Sao Paulo)
# 14 --GMT-02  		(Noronha, Mid-Atlantic)
# 15 --GMT-01  		(Azores, Cap Verde Isl.)
# 16 --GMT-00  		(Dublin, Lisbon, London, Reykjavik)
# 17 --GMT+01  		(Amsterdam, Berlin, Rome, Stockholm)
# 18 --GMT+02  		(Athens, Helsinki, Istanbul, Riga)
# 19 --GMT+02  		(Egypt)
# 20 --GMT+02  		(Israel)
# 21 --GMT+02  		(Lebanon)
# 22 --GMT+02  		(Syria)
# 23 --GMT+03  		(Moscow, Riyadh)
# 24 --GMT+03  		(Iraq)
# 25 --GMT+03:30  	(Iran)
# 26 --GMT+04  		(Abu Dubai, Baku)
# 27 --GMT+04:30  	(Kabul)
# 28 --GMT+05  		(Islamabad, Karachi, Tashkent)
# 29 --GMT+05:30  	(Bombay, Calcutta, New Delhi)
# 30 --GMT+06  		(Novosibirsk, Omsk)
# 31 --GMT+07  		(Bangkok, Hanoi, Jakarta)
# 32 --GMT+08  		(Beijing, Hong Kong, Shanghai, Taipei, Taiwan)
# 33 --GMT+09  		(Osaka, Sapporo, Tokyo)
# 34 --GMT+09:30  	(Adelaide, Darwin)
# 35 --GMT+10 		(Hobart)
# 36 --GMT+10 		(Canberra, Melbourne, Sydney)
# 37 --GMT+11 		(Solomon Isl.)
# 38 --GMT+12 		(Auckland, Wellington)
# 56 --GMT+13 		(Auckland, Wellington)

	
	##### Allow DHCP Option 42 to override NTP server #####
	## P144
	## value: 0:Disable  1:Enable
	
	##### Time Zone #####
	## P64
	## value: TimeZone option	(Integer)
	
	##### Enable Daylight Saving Time #####
	## P10004
	## value: 0/1	(0:Disable  1:Enable)
	
	##### Daylight Saving Time String #####
	## P10005
	## example:
	## GMT-08:00MDT-09:00,M4.1.2/11:00:00,M5.4.3/11:00:00
	## Format: current zone -- Head with "GMT-"  DST zone -- Head with "MDT-"
	
	##### Enable NTP #####
	## P5006
	## value: 0/1	(0:Disable  1:Enable)
	
	##### NTP Server #####
	## P30
	## value: String and MAX length is 255 .
	
	##### DST #####
	## P10005
	## value: DST string.
	
	##### Update Interval(m) #####
	## P10006
	## value: 60 - 1440 (Integer)

######			    			  Network Settings 									  ######	

	##### IP Address Mode #####
	## P8
	## value: 0/1 (0:DHCP  1:Static IP)
	
	##### IP Address segment1 #####
	## P9
	## value: 0 - 255 (Integer)
	
	##### IP Address segment2 #####
	## P10
	## value: 0 - 255 (Integer)
	
	##### IP Address segment3 #####
	## P11
	## value: 0 - 255 (Integer)
	
	##### IP Address segment4 #####
	## P12
	## value: 0 - 255 (Integer)
	
	##### Subnet Mask segment1 #####
	## P13
	## value: 0 - 255 (Integer)
	
	##### Subnet Mask segment2 #####
	## P14
	## value: 0 - 255 (Integer)
	
	##### Subnet Mask segment3 #####
	## P15
	## value: 0 - 255 (Integer)
	
	##### Subnet Mask segment4 #####
	## P16
	## value: 0 - 255 (Integer)

	##### Gateway segment1 #####
	## P17
	## value: 0 - 255 (Integer)
	
	##### Gateway segment2 #####
	## P18
	## value: 0 - 255 (Integer)
	
	##### Gateway segment3 #####
	## P19
	## value: 0 - 255 (Integer)
	
	##### Gateway segment4 #####
	## P20
	## value: 0 - 255 (Integer)

	##### DNS Address Type #####
	## P10107
	## value: 0/1	(0:Dynamic  1:Static DNS)

	##### DNS Server 1 segment1 #####
	## P21
	## value: 0 - 255 (Integer)
	
	##### DNS Server 1 segment2 #####
	## P22
	## value: 0 - 255 (Integer)
	
	##### DNS Server 1 segment3 #####
	## P23
	## value: 0 - 255 (Integer)
	
	##### DNS Server 1 segment4 #####
	## P24
	## value: 0 - 255 (Integer)
	
	##### DNS Server 2 segment1 #####
	## P25
	## value: 0 - 255 (Integer)
	
	##### DNS Server 2 segment2 #####
	## P26
	## value: 0 - 255 (Integer)
	
	##### DNS Server 2 segment3 #####
	## P27
	## value: 0 - 255 (Integer)
	
	##### DNS Server 2 segment4 #####
	## P28
	## value: 0 - 255 (Integer)
	
	##### LLDP Enable #####
	## P1684
	## value: 0/1	(0:Disable  1:Enable)
	
	##### Layer 2 QoS 802.1Q/VLAN Tag #####
	## P51
	## value: 0 - 4094 (Integer)
	
	##### Layer 2 QoS 802.1Q p Priority Value #####
	## P87
	## value: 0 - 7 (Integer)
	
######			 			Access Settings 					######

	##### Web Connection Mode #####
	## P12054
	## value: 0/1	(0:HTTP  1:HTTPS)
	
	##### Web Access Port #####
	## P901
	## value: 80 - 65535	(Integer)
	
	##### RTSP Port #####
	## P903
	## value: 554 - 65535 & no equal Web Access Port. (Integer)
	
	##### User Login Timeout(min) #####
	## P12056
	## value: 3 - 60 (Integer)
	
	##### Max Times Consecutively Login Error #####
	## P14832
	## value: 3 - 10 (Integer)
	
	##### Login Error Lock Time (min) #####
	## P14834
	## value: 3 - 10 (Integer)

	##### Disable Web Access #####
	## P15473
	## value: 0/1	(0:Disable  1:Enable)
	
	##### Enable UPnP Discovery #####
	## P12053
	## value: 0/1	(0:Disable  1:Enable)
	
	##### Enable Anonymous LiveView #####
	## P15469
	## value: 0/1	(0:Disable  1:Enable)
	
	##### Enable SSH  #####
	## P276 
	## value: 0/1	(0:Disable  1:Enable)
	
	##### SSH Port   #####
	## P27006
	## value: 22 or 444-65535, default 22	(Integer)
	
	##### GDSManager Configuration Password   #####
	## P15505
	## value: String & MAX length is 32
	
	
######			 			User Management 					######
	##### admin PW  #####
	## P2
	## value: String (Rule: [^!#%(-*,.0-9=@-Z_-z|~&*]) Max.length=32
	
################################################################################################
##                                 SIP Settings                                               ##
################################################################################################	

######			 				          Account 1 		       						  ######
	
	##### Account Active #####
	## P271
	## value: 0/1  (0:Disable  1:Enable)
	
	##### Account Name #####
	## P3
	## value: String & MAX length is 64
	
	##### SIP Server #####
	## P47
	## value: String & MAX length is 255
	
	##### Outbound Proxy #####
	## P48
	## value: String & MAX length is 255
	
	##### Backup Outbound Proxy #####
	## P2333
	## value: String & MAX length is 255
	
	##### DNS Mode #####
	## P103
	## value: 0/1/2  (0: A Record  1: SRV  2: NAPTR/SRV)
	
	##### SIP User ID #####
	## P35
	## value: String & MAX length is 255
	
	##### Authenticate ID #####
	## P36
	## value: String & MAX length is 255
	
	##### Password #####
	## P34
	## value: String & MAX length is 255
	
	##### TEL URI #####
	## P63
	## value: 0/1/2	(0:Disabled  1:User=phone  2:Enabled)
	
	
	##### Registration Expiration(m) #####
	## P32
	## value: 1 - 64800. Default 60.
	
	##### Re-register before Expiration (s)  #####
	## P2330
	## value: 1 - 64800. Default 0.
	
	##### Local SIP Port #####
	## P40
	## value: 81 - 65535. Default 5062.
	
	##### SIP Transport #####
	## P130
	## value: 0/1/2  (0: UDP  1: TCP  2: TLS/TCP)
	
	##### Stream #####
	## P15480
	## value: 0/1/2  (0: Stream 1  1: Stream 2  2: Stream 3)
	
	##### Enable DTMF RFC2833 #####
	## P2302
	## value: 0/1   (0: Disable  1: Enable)
	
	##### Enable DTMF SIP_INFO #####
	## P2303
	## value: 0/1   (0: Disable  1: Enable)
	
	##### DTMF Payload Type #####
	## P79
	## value: 96 - 127 default 101
	
	##### Unregister On Reboot #####
	## P81
	## value: 0/1   (0: Disable  1: Enable)
	
	##### NAT Traversal #####
	## P52
	## value: 0/1/2/3/4   (0: No  1: STUN  2: Keep Alive  3: UPnP  4: Auto)
	
	##### Enable SRTP #####
	## P183
	## value: 0/1   (0: Disable  1: Enable but No Forced  2: Enable and Forced)
	
	##### Special Feature #####
	## P100
	## value: 100/102/129   (100: Standard  102: Broadsoft  129: Telefonica Spain)
	
	##### Outbound Proxy Mode #####
	## P2305
	## value: 0/1/2		(0: In Route  1: Not In Route  2: Always Send To)
	
	##### Enable RTCP #####
	## P2492
	## value: 0/1/2   (0: Disable  1: RTCP  2: RTCP-XR)
	
	##### H.264 Payload Type #####
	## P462
	## value: 96 - 127 and no include 101

	##### Accept Incoming SIP from Proxy Only #####
	## P2447
	## value: 0/1/2   (0: Disable  1: Enable)
	
	##### Preferred Vocoder 1 #####
	## P57
	## value: 0:PCMU  8:PCMA  9:G.722  18:G.729A/B
	
	##### Preferred Vocoder 2 #####
	## P58
	## value: 0:PCMU  8:PCMA  9:G.722  18:G.729A/B
	
	##### Preferred Vocoder 3 #####
	## P59
	## value: 0:PCMU  8:PCMA  9:G.722  18:G.729A/B
	
	##### Preferred Vocoder 4 #####
	## P60
	## value: 0:PCMU  8:PCMA  9:G.722  18:G.729A/B
	
	##### Voice Frames Per TX #####
	## P37
	## value: 1 - 64
	

######			 				          Account 2 		       						  ######

	##### Account Active #####
	## P401
	## value: 0/1  (0:Disable  1:Enable)
	
	##### Account Name #####
	## P407
	## value: String & MAX length is 64
	
	##### SIP Server #####
	## P402
	## value: String & MAX length is 255
	
	##### Outbound Proxy #####
	## P403
	## value: String & MAX length is 255
	
	##### Backup Outbound Proxy #####
	## P2433
	## value: String & MAX length is 255
	
	##### DNS Mode #####
	## P408
	## value: 0/1/2  (0: A Record  1: SRV  2: NAPTR/SRV)
	
	##### SIP User ID #####
	## P404
	## value: String & MAX length is 255
	
	##### Authenticate ID #####
	## P405
	## value: String & MAX length is 255
	
	##### Password #####
	## P406
	## value: String & MAX length is 255
	
	##### TEL URI #####
	## P409
	## value: 0/1/2	(0:Disabled  1:User=phone  2:Enabled)
	
	
	
	##### Registration Expiration(m) #####
	## P412
	## value: 1 - 64800. Default 60.
	
	##### Re-register before Expiration (s)  #####
	## P2430
	## value: 1 - 64800. Default 0.
	
	##### Local SIP Port #####
	## P413
	## value: 81 - 65535. Default 5062.
	
	##### SIP Transport #####
	## P448
	## value: 0/1/2  (0: UDP  1: TCP  2: TLS/TCP)
	
	##### Stream #####
	## P8000
	## value: 0/1/2  (0: Stream 1  1: Stream 2  2: Stream 3)
	
	##### Enable DTMF RFC2833 #####
	## P2402
	## value: 0/1   (0: Disable  1: Enable)
	
	##### Enable DTMF SIP_INFO #####
	## P2403
	## value: 0/1   (0: Disable  1: Enable)
	
	##### DTMF Payload Type #####
	## P496
	## value: 96 - 127 default 101
	
	##### Unregister On Reboot #####
	## P411
	## value: 0/1   (0: Disable  1: Enable)
	
	##### NAT Traversal #####
	## P414
	## value: 0/1/2/3/4   (0: No  1: STUN  2: Keep Alive  3: UPnP  4: Auto)
	
	##### Enable SRTP #####
	## P443
	## value: 0/1   (0: Disable  1: Enable but No Forced  2: Enable and Forced)
	
	##### Special Feature #####
	## P424
	## value: 100/102   (100: Standard  1: Broadsoft)
	
	##### Outbound Proxy Mode #####
	## P2405
	## value: 0/1/2		(0: In Route  1: Not In Route  2: Always Send To)
	
	##### Enable RTCP #####
	## P2392
	## value: 0/1/2   (0: Disable  1: RTCP  2: RTCP-XR)
	
	##### H.264 Payload Type #####
	## P293
	## value: 96 - 127 and no include 101
	
	##### Accept Incoming SIP from Proxy Only #####
	## P2347
	## value: 0/1   (0: Disable  1: Enable)
	
	##### Preferred Vocoder 1 #####
	## P451
	## value: 0:PCMU  8:PCMA  9:G.722  18:G.729A/B
	
	##### Preferred Vocoder 2 #####
	## P452
	## value: 0:PCMU  8:PCMA  9:G.722  18:G.729A/B
	
	##### Preferred Vocoder 3 #####
	## P453
	## value: 0:PCMU  8:PCMA  9:G.722  18:G.729A/B
	
	##### Preferred Vocoder 3 #####
	## P454
	## value: 0:PCMU  8:PCMA  9:G.722  18:G.729A/B
	
	##### Voice Frames Per TX #####
	## P486
	## value: 1 - 64
	
	
######			 				   Account 3 		       					  ######
	
	##### Account Active #####
	## P501
	## value: 0/1  (0:Disable  1:Enable)
	
	##### Account Name #####
	## P507
	## value: String & MAX length is 64
	
	##### SIP Server #####
	## P502
	## value: String & MAX length is 255
	
	##### Outbound Proxy #####
	## P503
	## value: String & MAX length is 255
	
	##### Backup Outbound Proxy #####
	## P2533
	## value: String & MAX length is 255
	
	##### DNS Mode #####
	## P508
	## value: 0/1/2  (0: A Record  1: SRV  2: NAPTR/SRV)
	
	##### SIP User ID #####
	## P504
	## value: String & MAX length is 255
	
	##### Authenticate ID #####
	## P505
	## value: String & MAX length is 255
	
	##### Password #####
	## P506
	## value: String & MAX length is 255
	
	##### TEL URI #####
	## P509
	## value: 0/1/2	(0:Disabled  1:User=phone  2:Enabled)
	
	
	
	##### Registration Expiration(m) #####
	## P512
	## value: 1 - 64800. Default 60.
	
	##### Re-register before Expiration (s)  #####
	## P2530
	## value: 1 - 64800. Default 0.
	
	##### Local SIP Port #####
	## P513
	## value: 81 - 65535. Default 5062.
	
	##### SIP Transport #####
	## P548
	## value: 0/1/2  (0: UDP  1: TCP  2: TLS/TCP)
	
	##### Stream #####
	## P5481
	## value: 0/1/2  (0: Stream 1  1: Stream 2  2: Stream 3)
	
	##### Enable DTMF RFC2833 #####
	## P2502
	## value: 0/1   (0: Disable  1: Enable)
	
	##### Enable DTMF SIP_INFO #####
	## P2503
	## value: 0/1   (0: Disable  1: Enable)
	
	##### DTMF Payload Type #####
	## P596
	## value: 96 - 127 default 101
	
	##### Unregister On Reboot #####
	## P511
	## value: 0/1   (0: Disable  1: Enable)
	
	##### NAT Traversal #####
	## P514
	## value: 0/1/2/3/4   (0: No  1: STUN  2: Keep Alive  3: UPnP  4: Auto)
	
	##### Enable SRTP #####
	## P543
	## value: 0/1   (0: Disable  1: Enable but No Forced  2: Enable and Forced)
	
	##### Special Feature #####
	## P524
	## value: 100/102   (100: Standard  1: Broadsoft)
	
	##### Outbound Proxy Mode #####
	## P2505
	## value: 0/1/2		(0: In Route  1: Not In Route  2: Always Send To)
	
	##### Enable RTCP #####
	## P2592
	## value: 0/1/2   (0: Disable  1: RTCP  2: RTCP-XR)
	
	##### H.264 Payload Type #####
	## P562
	## value: 96 - 127 and no include 101
	
	##### Accept Incoming SIP from Proxy Only #####
	## P2547
	## value: 0/1/2   (0: Disable  1: Enable)
	
	##### Preferred Vocoder 1 #####
	## P551
	## value: 0:PCMU  8:PCMA  9:G.722  18:G.729A/B
	
	##### Preferred Vocoder 2 #####
	## P552
	## value: 0:PCMU  8:PCMA  9:G.722  18:G.729A/B
	
	##### Preferred Vocoder 3 #####
	## P553
	## value: 0:PCMU  8:PCMA  9:G.722  18:G.729A/B
	
	##### Preferred Vocoder 4 #####
	## P554
	## value: 0:PCMU  8:PCMA  9:G.722  18:G.729A/B
	
	##### Voice Frames Per TX #####
	## P586
	## value: 1 - 64


######			 				   Account 4 		       					  ######

	##### Account Active #####
	## P601
	## value: 0/1  (0:Disable  1:Enable)
	
	##### Account Name #####
	## P607
	## value: String & MAX length is 64
	
	##### SIP Server #####
	## P602
	## value: String & MAX length is 255
	
	##### Outbound Proxy #####
	## P603
	## value: String & MAX length is 255
	
	##### Backup Outbound Proxy #####
	## P2633
	## value: String & MAX length is 255
	
	##### DNS Mode #####
	## P608
	## value: 0/1/2  (0: A Record  1: SRV  2: NAPTR/SRV)
	
	##### SIP User ID #####
	## P604
	## value: String & MAX length is 255
	
	##### Authenticate ID #####
	## P605
	## value: String & MAX length is 255
	
	##### Password #####
	## P606
	## value: String & MAX length is 255
	
	##### TEL URI #####
	## P609
	## value: 0/1/2	(0:Disabled  1:User=phone  2:Enabled)
	
	
	
	##### Registration Expiration(m) #####
	## P612
	## value: 1 - 64800. Default 60.
	
	##### Re-register before Expiration (s)  #####
	## P2630
	## value: 1 - 64800. Default 0.
	
	##### Local SIP Port #####
	## P613
	## value: 81 - 65535. Default 5062.
	
	##### SIP Transport #####
	## P648
	## value: 0/1/2  (0: UDP  1: TCP  2: TLS/TCP)
	
	##### Stream #####
	## P15482
	## value: 0/1/2  (0: Stream 1  1: Stream 2  2: Stream 3)
	
	##### Enable DTMF RFC2833 #####
	## P2602
	## value: 0/1   (0: Disable  1: Enable)
	
	##### Enable DTMF SIP_INFO #####
	## P2603
	## value: 0/1   (0: Disable  1: Enable)
	
	##### DTMF Payload Type #####
	## P696
	## value: 96 - 127 default 101
	
	##### Unregister On Reboot #####
	## P611
	## value: 0/1   (0: Disable  1: Enable)
	
	##### NAT Traversal #####
	## P614
	## value: 0/1/2/3/4   (0: No  1: STUN  2: Keep Alive  3: UPnP  4: Auto)
	
	##### Enable SRTP #####
	## P643
	## value: 0/1   (0: Disable  1: Enable but No Forced  2: Enable and Forced)
	
	##### Special Feature #####
	## P624
	## value: 100/102   (100: Standard  1: Broadsoft)
	
	##### Outbound Proxy Mode #####
	## P2605
	## value: 0/1/2		(0: In Route  1: Not In Route  2: Always Send To)
	
	##### Enable RTCP #####
	## P2692
	## value: 0/1/2   (0: Disable  1: RTCP  2: RTCP-XR)
	
	##### H.264 Payload Type #####
	## P662
	## value: 96 - 127 and no include 101
	
	##### Accept Incoming SIP from Proxy Only #####
	## P2647
	## value: 0/1/2   (0: Disable  1: Enable)
	
	##### Preferred Vocoder 1 #####
	## P651
	## value: 0:PCMU  8:PCMA  9:G.722  18:G.729A/B
	
	##### Preferred Vocoder 2 #####
	## P652
	## value: 0:PCMU  8:PCMA  9:G.722  18:G.729A/B
	
	##### Preferred Vocoder 3 #####
	## P653
	## value: 0:PCMU  8:PCMA  9:G.722  18:G.729A/B
	
	##### Preferred Vocoder 4 #####
	## P654
	## value: 0:PCMU  8:PCMA  9:G.722  18:G.729A/B
	
	##### Voice Frames Per TX #####
	## P686
	## value: 1 - 64
	
	
######			 				   Phone Settings		       					  ######
	
	##### STUN Server #####
	## P76
	## value: String & MAX length is 255
	
	##### Local RTP Port #####
	## P39
	## value: 1 - 65535 & no equal 6789 (Integer).
	
	##### User Random Port #####
	## P78
	## value: 0/1	(0:Disable  1:Enable)
	
	##### Auto On-Hook Timer(second) #####
	## P10451
	## value: 0 - 65535  (Integer).
	
	##### Ring Timeout(second) #####
	## P14847
	## value: 0 - 90  (Integer).
	
	##### SIP TLS Certificate #####
	## P280
	## value: String
	
	##### SIP TLS Private Key #####
	## P279
	## value: String
	
	##### Enable Direct IP Call #####
	## P10453
	## value: 0/1	(0:Disable  1:Enable)
	
	##### Enable two-way SIP Calling #####
	## P8001
	## value: 0/1	(0:Disable  1:Enable)
	
	##### SIP Proxy Compatibility Mode #####
	## P8003
	## value: 0/1	(0:Disable  1:Enable)
	
	##### SIP Packetization Compatibility Mode #####
	## P957
	## value: 0/1	(0:Disable  1:Enable)
	
	##### Enable Multi-channel Call Mode #####
	## P15427
	## value: 0/1	(0:Disable default  1:Enable)
	
	##### Allow Reset via SIP NOTIFY #####
	## P15476
	## value: 0/1	(0:Disable default  1:Enable)
	
	##### Enable Session Timer #####
	## P2495
	## value: 0/1	(0: Disable  1: Enable)
	

######			 				   Account 1 White List 		 		       						  ######

	##### Enable White Number List #####
	## P10410
	## value: 0/1	(0:Disable  1:Enable)
	
	##### Phone Number #####
	## P10411
	## value: String. (Format:123,4567,)
	
######			 				   Account 2 White List 		 		       						  ######

	##### Enable White Number List #####
	## P10454
	## value: 0/1	(0:Disable  1:Enable)
	
	##### Phone Number #####
	## P10460
	## value: String. (Format:123,4567,)
	
######			 				   Account 3 White List 		 		       						  ######

	##### Enable White Number List #####
	## P10420
	## value: 0/1	(0:Disable  1:Enable)
	
	##### Phone Number #####
	## P10421
	## value: String. (Format:123,4567,)
	
######			 				   Account 4 White List 		 		       						  ######

	##### Enable White Number List #####
	## P10430
	## value: 0/1	(0:Disable  1:Enable)
	
	##### Phone Number #####
	## P10431
	## value: String. (Format:123,4567,)
	
################################################################################################
##                            Video & Audio Settings                                          ##
################################################################################################

######			 				  Video Settings	 		       						  ######
	
	##### Stream 1 Preferred Video Codec #####
	## P12306
	## value: 96/26	(96:H264  26:MJPEG)
	
	##### Stream 1 Profile #####
	## P12313
	## value: 0/1/2	(0:Baseline 1:Main Profile 2:Hight Profile)
	
	##### Stream 1 Resolution #####
	## P12307
	## value: 1025/1022	(1025:1920*1080 1022:1280*720)
	
	##### Stream 1 Bit Rate(kbps) #####
	## P12315
	## value: 1024/2048/4096
	
	##### Stream 1 Frame Rate(fps) #####
	## P12904
	## value: 5/10/15(If CMOS is Low Hight). 5/10/15/20/25/30(Others))
	
	##### Stream 1 Bit Rate Control #####
	## P12924
	## value: 0/1	(0:CBR 1:VBR)
	
	##### Stream 1 Image Quality #####
	## P12311
	## value: 
	
	##### Stream 1 I-frame Interval #####
	## P12312
	## value: 1 - 100	(Integer)
	
################################################################################################
	
	##### Stream 2 Preferred Video Codec #####
	## P12706
	## value: 96/26	(96:H264  26:MJPEG)
	
	##### Stream 2 Profile #####
	## P12713
	## value: 0/1/2	(0:Baseline 1:Main Profile 2:Hight Profile)
	
	##### Stream 2 Resolution #####
	## P12707
	## value: 1022/1/1010	(1022:1280*720 1:640*480 1010:480*272)
	
	##### Stream 2 Bit Rate(kbps) #####
	## P12708
	## value: 256/512/1024
	
	##### Stream 2 Frame Rate(fps) #####
	## P12709
	## value: 5/10/15(If CMOS is Low Hight). 5/10/15/20/25/30(Others))
	
	##### Stream 2 Bit Rate Control #####
	## P12710
	## value: 0/1	(0:CBR 1:VBR)
	
	##### Stream 2 Image Quality #####
	## P12711
	## value: 
	
	##### Stream 2 I-frame Interval #####
	## P12712
	## value: 1 - 100	(Integer)
	
################################################################################################

	##### Stream 3 Preferred Video Codec #####
	## P13106
	## value: 96/26	(96:H264  26:MJPEG)
	
	##### Stream 3 Profile #####
	## P13113
	## value: 0/1/2	(0:Baseline 1:Main Profile 2:Hight Profile)
	
	##### Stream 3 Resolution #####
	## P13107
	## value: 1008/0	(1008:352*240 0:320*240)
	
	##### Stream 3 Bit Rate(kbps) #####
	## P13108
	## value: 128/256/512
	
	##### Stream 3 Frame Rate(fps) #####
	## P13109
	## value: 5/10/15(If CMOS is Low Hight). 5/10/15/20/25/30(Others))
	
	##### Stream 3 Bit Rate Control #####
	## P13110
	## value: 0/1	(0:CBR 1:VBR)
	
	##### Stream 3 Image Quality #####
	## P13111
	## value: 
	
	##### Stream 3 I-frame Interval #####
	## P13112
	## value: 1 - 100	(Integer)
	
######			 				  OSD Settings	 		       						  ######

	##### Enable Display Time #####
	## P10044
	## value: 0/1 	(0:Disable  1:Enable)
	
	##### Enable Display Text #####
	## P10045
	## value: 0/1	(0:Disable  1:Enable)
	
	##### OSD Date Format #####
	## P10001
	## value: 0/1/2	(0:YYY-MM-DD 1:MM/DD/YYYY 2:DD MM YYYY)
	
	##### OSD Time Format #####
	## P10007
	## value: 0/1	(0:24H 1:12H)
	
	##### OSD Text #####
	## P10040
	## value: String & Max length is 32
	
	##### OSD Date/Time Position #####
	## P10041
	## value: 0/1/2/3	(0:Top Left 1:Bottom Left 2:Top Right 3:Bottom Right)
	
	##### OSD Text Position #####
	## P10046
	## value: 0/1/2/3	(0:Top Left 1:Bottom Left 2:Top Right 3:Bottom Right)
	
######			 				  CMOS Settings	 		       						  ######
	
	##### CMOS Mode #####
	## P10572
	## value: 1/2/3	(1:Normal 2:Low Light 3:WDR)
	
	##### CMOS LDC #####
	## P10573
	## value: 0/1	(0:OFF 1:ON)
	
	##### LDC Rate #####
	## P14565
	## value: 7: 0.7,  8: 0.8,  9: 0.9,  10: 1.0,  11: 1.1,  12: 1.2,  13: 1.3
	
	##### CMOS Power Frequency #####
	## P12314
	## value: 0/1	(0:50HZ 1:60HZ)
	
	##### CMOS Shutter Speed #####
	## P10503
	## value: 0/30/60/125/250/500/1000/2000/10000	(0:auto 30:1/30 60:1/60 125:1/125 250:1/250 500:1/500 1000:1/1000 2000:1/2000 10000:1/10000)
	
	
######			 				  Audio Settings	        						 ######

	##### Preferred Audio Codec #####
	## P14000
	## value: 1/2/4	(1:PCMU 2:PCMA 4:G722)
	
	##### System Volume #####
	## P14003
	## value:  
	## 		If Preferred Audio Codec is not G722 -- 0/1/2/3/4/5/6	(0:0 1:68 2:73 3:78 4:83 5:87 6:93)
	## 		If Preferred Audio Codec is G722 -- 0/1/2/3/4/5/6		(0:0 1:82 2:86 3:89 4:92 5:94 6:96)
	
	##### Doorbell Volume #####
	## P14835
	## value:  
	## 		If Preferred Audio Codec is not G722 -- 0/1/2/3/4/5/6	(0:0 1:68 2:73 3:78 4:83 5:87 6:93)
	## 		If Preferred Audio Codec is G722 -- 0/1/2/3/4/5/6		(0:0 1:82 2:86 3:89 4:92 5:94 6:96)
	
	##### Enable Custom Doorbell Ringtone #####
	## P15499
	## value: 0/1	(0:Disable  1:Enable)
	
######			 				  Privacy Masks    	 		       						      ######
	##### Privacy Mask Region #####
	## P14225
	## Format: (Enable/Disable@x1,y1,x2,y2; 0<=x1<=x2<=704 & 0<=y1<=y2<=576 
	## Example: 0@0,0,10,10;0@20,20,40,40;1@80,80,100,100;1@120,120,150,150;
	

###   P VALUE MISSING HERE, PLEASE ADD THEM !!!

################################################################################################
##                            Alarm Config                                                    ##
################################################################################################

######			 			  Alarm Events Config     		       						  ######

	##### Enable Motion Detection #####
	## P10250
	## value: 0/1	(0:Disable  1:Enable)
	
	##### Alarm Sensitivity #####
	## P14223
	## value: 0 - 100	(Integer)
	
	##### Select Alarm Schedule #####
	## P14221
	## value: 0 - 10	(Integer)
	
	##### Select Alarm Action Profile #####
	## P14222
	## value: 0 - 10	(Integer)
	
	##### MD regions #####
	## P14224
	## Format: [X0,Y0,X1,Y1] 0 <= X0 <= 32  0 <= Y0 <= 24  0 <= X1 <= 32  0 <= Y1 <= 24  X0 < X1  Y0 < Y1
	## Example: [0,0,0,0],[0,0,0,0],[0,0,0,0],[0,0,0,0],[0,0,0,0],[0,0,0,0],[0,0,0,0],[0,0,0,0]
	
	##### Digital Input 1 #####
	## P14320
	## value: 0/1/2/3		(0:Disable 1:Alarm Input 2:Open Door 3:Abnormal Door Control)
	
	##### Digit Input 1 Open Door Options #####
	## P15451
	## value: 0/1/2/3 (0:Door 1  1:Door 2  2:Door 1 & Door 2  3:None)
	
	##### Digit Input 1 Abnormal Door Control Options #####
	## P15508
	## value: 0/1 (0:Door 1  1:Door 2)
	
	##### Digit Input 1 Status #####
	## P15431
	## value: 0/1	(0:Normal Open	1:Normal Close)

	##### Digital Input 1 -> Select Alarm Schedule 1 #####
	## P14321
	## value: 0 - 10	(Integer)
	
	##### Digital Input 1 -> Select Alarm Action Profile 1 #####
	## P14322
	## value: 1 - 10	(Integer)
	
	##### Digital Input 2 #####
	## P14325
	## value: 0/1/2/3		(0:Disable 1:Alarm Input 2:Open Door 3:Abnormal Door Control)
	
	##### Digit Input 2 Open Door Options #####
	## P15452
	## value: 0/1/2/3 (0:Door 1  1:Door 2  2:Door 1 & Door 2  3:None)
	
	#### Digit Input 2 Abnormal Door Control Options #####
	## P15509
	## value: 0/1 (0:Door 1  1:Door 2)
	
	##### Digit Input 2 Status #####
	## P15432
	## value: 0/1	(0:Normal Open	1:Normal Close)

	##### Digital Input 2 -> Select Alarm Schedule 2 #####
	## P14326
	## value: 0 - 10	(Integer)
	
	##### Digital Input 2 -> Select Alarm Action Profile 2 #####
	## P14327
	## value: 1 - 10	(Integer)
	
	##### Alarm Output Duration(s) #####
	## P14341
	## value: 5/15/30/60/180/300	(Integer)
	
	##### Enable Silently Alarm Mode #####
	## P14568
	## Format:enable@DI@MD@Tamper@Passwd_Err   Exmaple: 0@1@1@0@1)
	
	##### Enable Hostage Code #####
	## P10467
	## value: 0/1	(0:Disable  1:Enable)

	##### Hostage Code #####
	## P10466
	## value: A pure digital string, MAX length is 8. Example: 6688
	
	##### Hostage Code Alarm Action Profile #####
	## P10468
	## value: 1 - 10	(Integer)
	
	##### Enable Tamper Alarm #####
	## P14350
	## value: 0/1	(0:Disable  1:Enable)
	
	##### Tamper Alarm Action Profile #####
	## P14355
	## value: 1 - 10	(Integer)
	
	##### Enable Keypad Input Error Alarm #####
	## P14825
	## value: 0/1	(0:Disable  1:Enable  Define:1)
	
	##### Keypad Input Error Alarm profile #####
	## P14826
	## value: 1 - 10	(Integer)
	
	##### Enable Non-scheduled Access Alarm #####
	## P15407
	## value: 0/1	(0:Disable  1:Enable  Define:1)
	
	##### Non-scheduled Access Alarm profile #####
	## P15408
	## value: 1 - 10	(Integer)

######			 				  Alarm Schedule	 		       						  ######

	##### schedule 1 #####
	## P14200
	## value: String  (Format:name,Date@start_time@end_time. example:schedule1,0@0000@1011,0@1100@2300)
	
	##### schedule 2 #####
	## P14201
	## value: String  (Format:name,Date@start_time@end_time. example:schedule1,0@0000@1011,0@1100@2300)
	
	##### schedule 3 #####
	## P14202
	## value: String  (Format:name,Date@start_time@end_time. example:schedule1,0@0000@1011,0@1100@2300)
	
	##### schedule 4 #####
	## P14203
	## value: String  (Format:name,Date@start_time@end_time. example:schedule1,0@0000@1011,0@1100@2300)
	
	##### schedule 5 #####
	## P14204
	## value: String  (Format:name,Date@start_time@end_time. example:schedule1,0@0000@1011,0@1100@2300)
	
	##### schedule 6 #####
	## P14205
	## value: String  (Format:name,Date@start_time@end_time. example:schedule1,0@0000@1011,0@1100@2300)
	
	##### schedule 7 #####
	## P14206
	## value: String  (Format:name,Date@start_time@end_time. example:schedule1,0@0000@1011,0@1100@2300)
	
	##### schedule 8 #####
	## P14207
	## value: String  (Format:name,Date@start_time@end_time. example:schedule1,0@0000@1011,0@1100@2300)
	
	##### schedule 9 #####
	## P14208
	## value: String  (Format:name,Date@start_time@end_time. example:schedule1,0@0000@1011,0@1100@2300)
	
	##### schedule 10 #####
	## P14209
	## value: String  (Format:name,Date@start_time@end_time. example:schedule1,0@0000@1011,0@1100@2300)
	
######			 				  Alarm Action	 		       						   ######

	##### Alarm Action Profile 1 #####
	## P14300
	## value: String  (Format:profileName@Alarm-Center,Sound,Sip,Output,Email,JPEG, example:night@1,1,1,0,1,0,)
	
	##### Alarm Action Profile 2 #####
	## P14301
	## value: String  (Format:profileName@Alarm-Center,Sound,Sip,Output,Email,JPEG, example:night@1,1,1,0,1,0,)
	
	##### Alarm Action Profile 3 #####
	## P14302
	## value: String  (Format:profileName@Alarm-Center,Sound,Sip,Output,Email,JPEG, example:night@1,1,1,0,1,0,)
	
	##### Alarm Action Profile 4 #####
	## P14303
	## value: String  (Format:profileName@Alarm-Center,Sound,Sip,Output,Email,JPEG, example:night@1,1,1,0,1,0,)
	
	##### Alarm Action Profile 5 #####
	## P14304
	## value: String  (Format:profileName@Alarm-Center,Sound,Sip,Output,Email,JPEG, example:night@1,1,1,0,1,0,)
	
	##### Alarm Action Profile 6 #####
	## P14305
	## value: String  (Format:profileName@Alarm-Center,Sound,Sip,Output,Email,JPEG, example:night@1,1,1,0,1,0,)
	
	##### Alarm Action Profile 7 #####
	## P14306
	## value: String  (Format:profileName@Alarm-Center,Sound,Sip,Output,Email,JPEG, example:night@1,1,1,0,1,0,)
	
	##### Alarm Action Profile 8 #####
	## P14307
	## value: String  (Format:profileName@Alarm-Center,Sound,Sip,Output,Email,JPEG, example:night@1,1,1,0,1,0,)
	
	##### Alarm Action Profile 9 #####
	## P14308
	## value: String  (Format:profileName@Alarm-Center,Sound,Sip,Output,Email,JPEG, example:night@1,1,1,0,1,0,)
	
	##### Alarm Action Profile 10 #####
	## P14309
	## value: String  (Format:profileName@Alarm-Center,Sound,Sip,Output,Email,JPEG, example:night@1,1,1,0,1,0,)
	
######			 				  Alarm Phone List 	 		       						  ######

	##### Alarm Phone List #####
	## P10471
	## value: 0/1/2/3/4  (0: Auto  1: Account 1  2: Account 2  3: Account 3  4: Account 4 )
	
	##### Alarm Phone List #####
	## P10459
	## value: String  (Example:1122,3344,5566, Don't forget the last ',')
	
################################################################################################
##                           Email & FTP Settings                                             ##
################################################################################################
	
######			 			 Email Settings     	 		       						  ######
	
	############### Email Settings ###############
	##### SMTP Server #####
	## P10121
	## value: String  (Example: smtp.google.com)
	
	##### SMTP Server Port #####
	## P10122
	## value: 0 - 65535  (Integer)
	
	##### From E-Mail Address #####
	## P10123
	## value: A valid email address (String)
	
	##### Sender User Name #####
	## P10127
	## value: String. Max length 63.
	
	##### Sender Password #####
	## P10128
	## value: String. Max length 63.
	
	##### Password Recovery Email #####
	## P10124
	## value: A valid email address (String)
	
	##### Alarm Receive Email 1 #####
	## P14348
	## value: A valid email address (String)
	
	##### Alarm Receive Email 2 #####
	## P14349
	## value: A valid email address (String)
	
	##### SSL #####
	## P10129
	## value: 0/1	(0:Disable  1:Enable)
	
######			 			 FTP & Central Storage	         						  ######
	
	##### Storage Server Type #####
	## P14113
	## value: 0/1	(0:FTP 1:Central Storage)
	
	##### FTP Server #####
	## P14114
	## value: String (Example: 192.168.0.160)
	
	##### FTP Server Port #####
	## P14115
	## value: 0 - 65535 (Integer)
	
	##### FTP User Name #####
	## P14116
	## value: String. Max length is 63.
	
	##### FTP Path #####
	## P14118
	## value: A valid path	(String)

################################################################################################
##                           Maintenance                                                      ##
################################################################################################

######			 		     Upgrade      	       						                  ######
	##### Firmware Upgrade Via #####
	## P6767
	## value: 0/1/2		(0:TFTP  1:HTTP  2:HTTPS)
	
	##### Firmware Server Path #####
	## P192
	## value: (String)
	
	##### Firmware HTTP/HTTS User Name #####
	## P6768
	## value: (String)
	
	##### Firmware HTTP/HTTS Password #####
	## P6769
	## value: (String)
	
	##### Firmware Upgrade File Prefix #####
	## P232
	## value: (String)
	
	##### Firmware Upgrade File Postfix #####
	## P233
	## value: (String)
		
	##### Config Upgrade Via #####
	## P212
	## value: 0/1/2		(0:TFTP  1:HTTP  2:HTTPS)
	
	##### Config Server Path #####
	## P237
	## value: (String)
	
	##### Config HTTP/HTTS User Name #####
	## P1360
	## value: (String)
	
	##### Config HTTP/HTTS Password #####
	## P1361
	## value: (String)
	
	##### Config Upgrade File Prefix #####
	## P234
	## value: (String)
	
	##### Config Upgrade File Postfix #####
	## P235
	## value: (String)
	
	##### XML Config File Password #####
	## P1359
	## value: String.
	
	##### Validate Server Certificates #####
	## P8463
	## value: 0/1	(0:Disable  1:Enable)
	
	##### DHCP Option 66 Override Server #####
	## P145
	## value: 0/1	(0:Disable  1:Enable)
	
	##### Zero Config #####
	## P1414
	## value: 0/1	(0:Disable  1:Enable)
	
	##### Enable DHCP Option 120 Override SIP Server #####
	## P1411
	## value: 0/1	(0:Disable  1:Enable)
	
	##### Automatic Upgrade #####
	## P194
	## value: 0/1	(0:No  1:Yes,check for upgrade periodic  2:Yes,check for upgrade every day  3:Yes,check for upgrade every week)
	
	##### Automatic Upgrade Interval(minutes) #####
	## P193
	## value: 60 - 525600	(Integer)
	
	##### Randomized Automatic Upgrade #####
	## P8458
	## value: 0/1  (0:Disable  1:Enable)
	
	##### Hour of the Day  – Start Time #####
	## P285
	## value: 0 -- 23  (Integer)
	
	##### Hour of the Day – End Time #####
	## P8459
	## value: 0 -- 23  (Integer)
	
	##### Day of the Week  – Week #####
	## P286
	## value: 0 -- 6  (Integer)
	
	
	
	
	
	
######			 		   Debug Log   	       						                  ######

	##### Debug Log Server #####
	## P207
	## value: A valid server path	(String)
	
	##### Debug Log Level #####
	## P208
	## value: 0/1/2/3/4	(0:None 1:Debug 2:Info 3:Warning 4:Error)
	
	
	
######						System Health Alert													######
	
	##### Enable System Health Alert ####
	## P15490
	## value: 0/1	(0:Disable  1:Enable)
	
	##### Delivery Method ####
	## P15491
	## value: 0/1	(0:Real-time  1:Periodic)
	
	##### Alert Interval(m) ####
	## P15492
	## value: 1 - 10080
	
	##### Email Title ####
	## P15496
	## value: string  MAX Length 256
	
	##### SIP Registration Status ####
	## P15493
	## value: 0/1	(0:Disable  1:Enable)
	
	##### System Running Status ####
	## P15494
	## value: 0/1	(0:Disable  1:Enable)
	
	##### System Temperature ####
	## P15495
	## value: 0/1	(0:Disable  1:Enable)
	
######			 		   Event Notification   	       						                  ######
	##### Enable Event Notification #####
	## P15410
	## value: 0: Disable  1: Enable
	
	##### Event Notification Type #####
	## P15417
	## value: 1:HTTP 2:HTTPS
	
	##### HTTP Server URL #####
	## P15413
	## value: string Max.length=256. Format http://ip:port/path. Such as http://192.100.10.10:80/
	
	##### HTTP Server Username #####
	## P15414
	## value: string Max.length=128 . 
	
	##### HTTP Server Password #####
	## P15415
	## value: string Max.length=128 . 
	
	##### URL Template #####
	## P15416
	## value: string Max.length=1024 . Example:{"mac":"${MAC}","content":"${WARNING_MSG}"}
	
	######
	
######			 		   Trusted CA Cerificates   	       						      ######
	##### Trusted CA Cerificates 1 #####
	## P8433
	## value: string max.length=4096
	
	##### Trusted CA Cerificates 2 #####
	## P8434
	## value: string max.length=4096
	
	##### Trusted CA Cerificates 3 #####
	## P8435
	## value: string max.length=4096
	
	##### Trusted CA Cerificates 4 #####
	## P8436
	## value: string max.length=4096
	
	##### Trusted CA Cerificates 5 #####
	## P8437
	## value: string max.length=4096
	
	##### Trusted CA Cerificates 6 #####
	## P8438
	## value: string max.length=4096
	
	##### Custom Certificate  #####
	## P8475
	## value: string max.length=4096

################################################################################################
##                End of the Configuration Template for GDS3710 Door System        			  ##
##                           (Firmware Version:   1.0.7.8)                                    ##
################################################################################################
