################################################################################################
## Configuration Template For GXP1610/1620/1625/1628/1630 Firmware Version 1.0.5.3            ##
################################################################################################

####################################################################
# Account Settings                                                ##
####################################################################

####################################################################
# Account 1                                                       ##
####################################################################

##########################################
# Account 1/General Settings
##########################################

# Account Active. 0 - No, 1 - Yes. Default is 1
# Number: 0, 1
# Mandatory
P271 = 1

# Account Name
# String
P270 =

# SIP Server
# String
P47 =

# Secondary SIP Server
# String
P2312 =


# Outbound Proxy
# String
P48 =


# Backup Outbound Proxy
# String
P2333 = 

# BLF Server
# String
P2375 =

# SIP User ID
# String
P35 =

# Authenticate ID
# String
P36 =

# Authenticate Password
# String
P34 =

# Name
# String
P3 =

# Voice Mail Access Number
# String
P33 =

# Account Display
# Number: 0 - User Name, 1 - User ID. Default is 0.
# Mandatory
P2380 = 0

##########################################
# Account 1/Network Settings
##########################################
# DNS Mode. 0 - A Record, 1 - SRV, 2 - NAPTR/SRV, 3 - Use Configured IP. Default is 0
# Number: 0, 1, 2, 3
# Mandatory
P103 = 0

# Primary IP. Maximum 15 characters
# String
P2308 =

# Backup IP 1
# String
P2309 =

# Backup IP 2
# String
P2310 =

# NAT Traversal. 0 - No, 1 - STUN, 2 - keep alive, 3 - UPnP, 4 - Auto, 5 - VPN. Default is 0.
# Number: 0, 1, 2, 3, 4, 5
# Mandatory
P52 = 0

# Proxy-Require (A SIP extension to enable firewall penetration). Max length is 64 characters
# String
P197 =

# Use SBC. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P26090 = 0

##########################################
# Account 1/SIP Settings/Basic Settings
##########################################
# TEL URI. 0 - Disabled, 1 - User=Phone, 2 - Enabled. Default is 0
# Number: 0, 1, 2
# Mandatory
P63 = 0

# SIP Registration. 0 - No, 1 - Yes. Default is 1
# Number: 0, 1
# Mandatory
P31 = 1

# Unregister On Reboot. 0 - No, 1 - All, 2-Instance. Default is 0
# Number: 0, 1
# Mandatory
P81 = 0

# Register Expiration (in minutes). Default is 60. Max about 45 days
# Number: 1 - 64800
# Mandatory
P32 = 60

# Subscribe Expiration (in minutes). Default is 60. Max about 45 days
# Number: 1 - 64800
# Mandatory
P26051 = 60

# Reregister Before Expiration (in seconds). Default is 0 second
# Number: 0 - 64800
# Mandatory
P2330 = 0

# Enable OPTIONS Keep Alive
# Number: 0, 1
# Mandatory
P2397 = 0

# OPTIONS Keep Alive Interval (in seconds). Default is 30 seconds
# Number
# Mandatory
P2398 = 30

# OPTIONS Keep Alive Max Lost (number of max lost packets). Default is 3
# Number
# Mandatory
P2399 = 3

# Local SIP Port. Default is 5060
# Number
# Mandatory
P40 = 5060

# SIP Registration Failure Retry Wait Time (in seconds). Default is 20
# Number: 1 - 3600
# Mandatory
P138 = 20

# SIP T1 Timeout. RFC 3261 T1 value (RTT estimate)
# 50 - 0.5 sec, 100 - 1 sec, 200 - 2 sec. Default is 50
# Number: 50, 100, 200
# Mandatory
P209 = 50

# SIP T2 Timeout. RFC 3261 T2 value. The maximum retransmit interval for non-INVITE requests and INVITE responses
# 200 - 2 sec, 400 - 4 sec, 800 - 8 sec. Default is 400
# Number: 200, 400, 800
# Mandatory
P250 = 400

# Switch Backup Proxy on No Response. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P26092 = 0

# SIP Transport. 0 - UDP, 1 - TCP, 2 - TLS/TCP. Default is 0
# Number: 0, 1, 2
# Mandatory
P130 = 0

# SIP URI Scheme when using TLS. 0 - sip, 1 - sips. Default is 1
# Number: 0, 1
# Mandatory
P2329 = 1

# Use Actual Ephemeral Port in Contact with TCP/TLS. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P2331 = 0

# Outbound Proxy Mode. 0 - in route, 1 - not in route, 2 - always send to. Default is 0
# Number: 0, 1, 2
# Mandatory
P2305 = 0

# Support SIP Instance ID. 0 - No, 1 - Yes. Default is 1
# Number: 0, 1
# Mandatory
P288 = 1

# SUBSCRIBE for MWI. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P99 = 0

# SUBSCRIBE for Registration. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P2319 = 0

# Enable 100rel. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P272 = 0

# Callee ID Display. 0 - Auto, 1 - Disabled, 2 - To Header. Default is 0
# Number: 0, 1, 2
# Mandatory 
P26025 = 0

# Caller ID Display. 0 - Auto, 1 - Disabled, 2 - From Header. Default is 0
# Number: 0, 1, 2
# Mandatory
P2324 = 0

# Ignore Alert-Info header
# 0 - No, 1 - Yes. Default is 0
# Number 0,1
# Mandatory
P26018 = 0

# Add Auth Header On Initial REGISTER
# 0 - No, 1 - Yes. Default is 0
# Number 0,1
# Mandatory
P2359 = 0 

###########################################
# Account 1/SIP Settings/Custom SIP Headers
###########################################
# Use Privacy Header
# 0 - Default, 1 - No, 2 - Yes. Default is 0
# Number: 0, 1, 2
# Mandatory
P2338 = 0

# Use P-Preferred-Identity Header
# 0 - Default, 1 - No, 2 - Yes. Default is 0
# Number: 0, 1, 2
# Mandatory
P2339 = 0

# Use X-Grandstream-PBX Header
# 0 - No, 1 - Yes. Default is 1
# Number: 0, 1
# Mandatory
P26054 = 1

# Use P-Access-Network-Info Header
# 0 - No, 1 - Yes. Default is 1
# Number: 0, 1
# Mandatory
P26058 = 1

# Use P-Emergency-Info Header
# 0 - No, 1 - Yes. Default is 1
# Number: 0, 1
# Mandatory
P26059 = 1

# Use MAC Header
# 0 - No, 1 - Yes except REGISTER, 2 - Yes to all SIP. Default is 0
# Number: 0, 1, 2
# Mandatory
P26061 = 0

##########################################
# Account 1/SIP Settings/Advanced Features
##########################################
# Line-seize Timeout (in seconds). Default is 15
# Number: 15-60
# Mandatory
P2313 = 15

# Eventlist BLF URI. For GXP1630/1628 only
# String
P134 = 

# Auto Provision Eventlist BLFs. For GXP1630/1628 only. 0 - disabled, 1 - enabled. 
# Number: 0, 1
# Default is 0
# Mandatory
P2389 = 0

# Conference URI
# String
P2318 =

# Music On Hold URI
# String
P2350 =

# Force BLF Call-pickup by prefix. For GXP1630/1628 only. 0 - No, 1 - Yes. Default is 0 
# Number: 0, 1
# Mandatory
P6752 = 0

# BLF Call-pickup Prefix. For GXP1630/1628 only.
# String. Defaule is "**"
P1347 = **

# Call Pickup Barge-In Code. For GXP1630/1628 only.
# String 
P26046 =

# PUBLISH for Presence. 0 - No, 1 - Yes. For GXP1630/1628 only.
# Number: 0, 1
# Default is 0
# Mandatory
P188 = 0

# Enable User Presence Subscription
# Number: 0 - No, 1 - Yes. Default is 0.
# Mandatory
P2353 = 0

# Hide Login Soft Key On Auto User Presence Subscription
# Number: 0 - No, 1 - Yes. Default is 1.
# Mandatory
P2354 = 1

# Auto User Presence ID
# String
P2351 =

# Auto User Presence Password
# String
P2352 =

# Special Feature. 100 - Standard, 101 - Nortel MCS, 102- Broadsoft, 108 - CBCOM, 
# 109 - RNK, 110 - Sylantro, 117 - Huawei IMS, 119 - Phonepower
# Default is 100
# Number: 100, 101, 102, 108, 109, 110, 117, 119
# Mandatory
P198 = 100

# Broadsoft Call Center. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P2341 = 0

# Hoteling Event. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P2342 = 0

# Call Center Status. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P2343 = 0

# Feature Key Synchronization. 0 - Disabled, 1 - Enabled. Default is 0
# Number: 0, 1
# Mandatory
P2325 = 0

# Broadsoft Call Park
# Number 0 - Disabled, 1 - Enabled. Default is 0
# Mandatory
P2388 = 0

##########################################
# Account 1/SIP Settings/Session Timer
##########################################
# Enable Session Timer. 0 - No, 1 - Yes. Default is 1
# Number: 0, 1
# Mandatory
P2395 = 1

# Session Expiration (in seconds). Default is 180
# Number: 90 - 64800
# Mandatory
P260 = 180

# Minimum SE (in seconds). Default is 90. This value must be lower than or equal to P260
# Number: 90 - 64800
# Mandatory
P261 = 90

# Caller Request Timer (Request for timer when calling). 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P262 = 0

# Callee Request Timer (Request for timer when called. i.e. if remote party supports timer but did not request for one)
# 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P263 = 0

# Force Timer (Still use timer when remote party does not support timer). 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P264 = 0

# UAC Specify Refresher. 0 - omit, 1 - UAC, 2 - UAS. Default is 0
# Number: 0, 1, 2
# Mandatory
P266 = 0

# UAS Specify Refresher. 1 - UAC, 2 - UAS. Default is 1
# Number: 1, 2
# Mandatory
P267 = 1

# Force INVITE (Always refresh with INVITE instead of UPDATE even when remote party supports UPDATE).
# 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P265 = 0

###########################################
# Account 1/SIP Settings/Security Settings
###########################################
# Check Domain Certificates. When set to Yes/Enabled, domain certificate will be checked as defined in RFC5922
# 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P2311 = 0

# Validate Certification Chain. 0 - No, 1 - Yes. Default is 0
# NUmber: 0, 1
# Mandatory
P2367 = 0

# Validate Incoming Messages. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P2306 = 0

# Check SIP User ID for incoming INVITE. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P258 = 0

# Accept Incoming SIP from Proxy Only. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P2347 = 0

# Authenticate Incoming INVITE. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P2346 = 0

##########################################
# Account 1/Audio Settings
##########################################
# Send DTMF: In-audio. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P2301 = 0

# Send DTMF: Via RTP (RFC2833). 0 - No, 1 - Yes. Default is 1
# Number: 0, 1
# Mandatory
P2302 = 1

# Send DTMF: Via SIP INFO. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P2303 = 0

# DTMF Payload Type. Default is 101
# Number: 96 - 127
# Mandatory
P79 = 101

# Preferred Vocoder
# 0 - PCMU, 2 - G.726-32, 4 - G.723.1, 8 - PCMA, 9 - G.722, 18 - G.729A/B, 98 - iLBC
# choice 1. Default is 0
# Number: 0, 2, 4, 8, 9, 18, 98
# Mandatory
P57 = 0

# choice 2. Default is 8
# Number: 0, 2, 4, 8, 9, 18, 98
# Mandatory
P58 = 8

# choice 3. Default is 18
# Number: 0, 2, 4, 8, 9, 18, 98
# Mandatory
P59 = 18

# choice 4. Default is 9
# Number: 0, 2, 4, 8, 9, 18, 98
# Mandatory
P60 = 9

# choice 5. Default is 2
# Number: 0, 2, 4, 8, 9, 18, 98
# Mandatory
P61 = 2

# choice 6. Default is 2
# Number: 0, 2, 4, 8, 9, 18, 98
# Mandatory
P62 = 2

# choice 7. Default is 2
# Number: 0, 2, 4, 8, 9, 18, 98
# Mandatory
P46 = 2

# Use First Matching Vocoder in 200OK SDP. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P2348 = 0

# Codec Negotiation Priority. 0 - Caller, 1 - Callee. Default is 1
# Number: 0, 1
# Mandatory
P29061 = 1

# Disable Multiple m line in SDP. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P137 = 0

# SRTP Mode. 0 - Disabled, 1 - Enabled but not forced, 2 - Enabled and forced, 3 - Optional. Default is 0
# Number: 0, 1, 2, 3
# Mandatory
P183 = 0

# Symmetric RTP. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P291 = 0

# Silence Suppression. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P50 = 0

# Voice Frames per TX (up to 10/20/32/64 frames for G711/G726/G723/other codecs respectively). Default is 2
# Number: 1 - 64
# Mandatory
P37 = 2

# G723 Rate. 0 - 6.3kbps, 1 - 5.3 kbps. Default is 0
# Number: 0, 1
# Mandatory
P49 = 0

# G.726-32 Packing Mode. 0 - ITU, 1 - IETF. Default is 0
# Number: 0, 1
# Mandatory
P2323 = 0

# iLBC Frame Size, 0 - 20ms, 1 - 30ms. Default is 1.
# Number: 0, 1
# Mandatory
P97 = 1

# iLBC Payload Type, Default is 97
# Number: 96 - 127
# Mandatory
P96 = 97

# Jitter Buffer Type. 0 - Fixed, 1 - Adaptive. Default is 1
# Number: 0, 1
# Mandatory
P133 = 1

# Jitter Buffer Length. 0 - 100ms, 1 - 200ms, 2 - 300ms, 3 - 400ms, 4 - 500ms, 5 - 600ms, 6 - 700ms, 7 - 800ms
# Default is 2
# Number: 0, 1, 2, 3, 4, 5, 6, 7
# Mandatory
P132 = 2

# Hide Vocodec. 0 - No, 1 - Yes. Default is 0.
# Number: 0, 1
# Mandatory
P26047 = 0

##########################################
# Account 1/Call Settings
##########################################
# Early Dial (use "Yes" only if proxy supports 484 response). 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P29 = 0

# Dial Plan Prefix
# String 
P66 =

# Dial Plan. Default is { x+ | *x+ | *xx*x+ }
# String
# Mandatory
P290 = { x+ | *x+ | *xx*x+ }

# Bypass Dial Plan. Default is Mpk
# String: Contact, Call History Incoming Call, Call History Outgoing Call, Dialing Page, Mpk, Api
# P2382 = Mpk

# Call Log. 0 - Log All, 1 - Log Incoming/Outgoing only (Missed calls NOT recorded), 2 - Disable Call Log. Default is 0
# Number: 0, 1, 2
# Mandatory
P182 = 0

# Send Anonymous (caller ID will be blocked if set to Yes). 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P65 = 0

# Anonymous Call Rejection. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P129 = 0

# Auto Answer. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P90 = 0

# Auto Answer Numbers
# String
P29064 = 

# Refer-To Use Target Contact. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P135 = 0

# Transfer on conference Hang-Up. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P2304 = 0

# Disable Recovery on Blind Transfer, 0 - No, 1- Yes. Default is 0
# Number: 0, 1
# Mandatory
P2384 = 0

# Blind Transfer Wait Timeout, in seconds. Default is 30
# Number: 30 - 300
P26070 = 30

# No Key Entry Timeout (in seconds). Default is 4
# Number: 1 - 15
# Mandatory
P85 = 4

# Key as Send. 0 - Disable, 1 - Pound (#). Default is 1
# Number: 0, 1
# Mandatory
P72 = 1

# On Hold Reminder Tone.  0 - Disabled, 1 - Enabled. Default is 0
# Number: 0, 1
# Mandatory
P26006 = 0

# Call Recording ON
# String
P26028 =

# Call Recording OFF
# String
P26029 =

# Hide Dialing Password - Prefix for Dialing Password
# String
P26049 =

# Hide Dialing Password - Password Length. Default is 0.
# Number: 1 - 32
P26050 = 0

# Remote Info Display
# 0 - Name and Number, 1 - Number, 2 - Name. Default is 0
# Number: 0, 1, 2
P26076 = 0

# Hide Remote User ID - Call Type. 0 - None of Call, 1 - Incoming Calls, 2 - Outgoing Calls, 3 - Both Directions. Default is 0
# Number: 0 - 3
P26043 = 0

# Hide Remote User ID - Length
# Number: 0 ... N
P26044 = 0

# Account Ring Tone. 0 - System Ringtone, 1 - Custom Ringtone 1, 2 - Custom Ringtone 2, 3 - Custom Ringtone 3
# 6 - Custom Ringtone 4, 7 - Custom Ringtone 5, 8 - Custom Ringtone 6, 9 - Custom Ringtone 7, 10 - Custom Ringtone 8
# 11 - Custom Ringtone 9, 12 - Custom Ringtone 10, 4 - Silent, 5 - Default Ringtone
# Default is 5
# Number: 0 - 12
# Mandatory
P104 = 5

# Matching Incoming Caller ID. Matching Rule 1
# String
P1488 = 

# Matching Rule 1 Distinctive Ringtone
# 0 - System Ringtone, 1 - Custom Ringtone 1, 2 - Custom Ringtone 2, 3 - Custom Ringtone 3
# 6 - Custom Ringtone 4, 7 - Custom Ringtone 5, 8 - Custom Ringtone 6, 9 - Custom Ringtone 7, 10 - Custom Ringtone 8
# 11 - Custom Ringtone 9, 12 - Custom Ringtone 10, 4 - Silent, 5 - Default Ringtone
# Default is 0
# Number: 0 - 12
# Mandatory
P1489 = 0

# Matching Incoming Caller ID. Matching Rule 2
# String
P1490 = 

# Matching Rule 2 Distinctive Ringtone
# 0 - System Ringtone, 1 - Custom Ringtone 1, 2 - Custom Ringtone 2, 3 - Custom Ringtone 3
# 6 - Custom Ringtone 4, 7 - Custom Ringtone 5, 8 - Custom Ringtone 6, 9 - Custom Ringtone 7, 10 - Custom Ringtone 8
# 11 - Custom Ringtone 9, 12 - Custom Ringtone 10, 4 - Silent, 5 - Default Ringtone
# Default is 0
# Number: 0 - 12
# Mandatory
P1491 = 0

# Matching Incoming Caller ID. Matching Rule 3
# String
P1492 =

# Matching Rule 3 Distinctive Ringtone
# 0 - System Ringtone, 1 - Custom Ringtone 1, 2 - Custom Ringtone 2, 3 - Custom Ringtone 3
# 6 - Custom Ringtone 4, 7 - Custom Ringtone 5, 8 - Custom Ringtone 6, 9 - Custom Ringtone 7, 10 - Custom Ringtone 8
# 11 - Custom Ringtone 9, 12 - Custom Ringtone 10, 4 - Silent, 5 - Default Ringtone
# Default is 0
# Number: 0 - 12
# Mandatory
P1493 = 0

# Matching Incoming Caller ID. Matching Rule 4
# String
P6716 = 

# Matching Rule 4 Distinctive Ringtone
# 0 - System Ringtone, 1 - Custom Ringtone 1, 2 - Custom Ringtone 2, 3 - Custom Ringtone 3
# 6 - Custom Ringtone 4, 7 - Custom Ringtone 5, 8 - Custom Ringtone 6, 9 - Custom Ringtone 7, 10 - Custom Ringtone 8
# 11 - Custom Ringtone 9, 12 - Custom Ringtone 10, 4 - Silent, 5 - Default Ringtone
# Default is 0
# Number: 0 - 12
# Mandatory
P6717 = 0

# Matching Incoming Caller ID. Matching Rule 5
# String
P6718 = 

# Matching Rule 5 Distinctive Ringtone
# 0 - System Ringtone, 1 - Custom Ringtone 1, 2 - Custom Ringtone 2, 3 - Custom Ringtone 3
# 6 - Custom Ringtone 4, 7 - Custom Ringtone 5, 8 - Custom Ringtone 6, 9 - Custom Ringtone 7, 10 - Custom Ringtone 8
# 11 - Custom Ringtone 9, 12 - Custom Ringtone 10, 4 - Silent, 5 - Default Ringtone
# Default is 0
# Number: 0 - 12
# Mandatory
P6719 = 0

# Matching Incoming Caller ID. Matching Rule 6
# String
P6720 = 

# Matching Rule 6 Distinctive Ringtone
# 0 - System Ringtone, 1 - Custom Ringtone 1, 2 - Custom Ringtone 2, 3 - Custom Ringtone 3
# 6 - Custom Ringtone 4, 7 - Custom Ringtone 5, 8 - Custom Ringtone 6, 9 - Custom Ringtone 7, 10 - Custom Ringtone 8
# 11 - Custom Ringtone 9, 12 - Custom Ringtone 10, 4 - Silent, 5 - Default Ringtone
# Default is 0
# Number: 0 - 12
# Mandatory
P6721 = 0

# Matching Incoming Caller ID. Matching Rule 7
# String
P26064 = 

# Matching Rule 7 Distinctive Ringtone
# 0 - System Ringtone, 1 - Custom Ringtone 1, 2 - Custom Ringtone 2, 3 - Custom Ringtone 3
# 6 - Custom Ringtone 4, 7 - Custom Ringtone 5, 8 - Custom Ringtone 6, 9 - Custom Ringtone 7, 10 - Custom Ringtone 8
# 11 - Custom Ringtone 9, 12 - Custom Ringtone 10, 4 - Silent, 5 - Default Ringtone
# Default is 0
# Number: 0 - 12
# Mandatory
P26065 = 0

# Matching Incoming Caller ID. Matching Rule 8
# String
P26066 = 

# Matching Rule 8 Distinctive Ringtone
# 0 - System Ringtone, 1 - Custom Ringtone 1, 2 - Custom Ringtone 2, 3 - Custom Ringtone 3
# 6 - Custom Ringtone 4, 7 - Custom Ringtone 5, 8 - Custom Ringtone 6, 9 - Custom Ringtone 7, 10 - Custom Ringtone 8
# 11 - Custom Ringtone 9, 12 - Custom Ringtone 10, 4 - Silent, 5 - Default Ringtone
# Default is 0
# Number: 0 - 12
# Mandatory
P26067 = 0

# Matching Incoming Caller ID. Matching Rule 9
# String
P26068 = 

# Matching Rule 9 Distinctive Ringtone
# 0 - System Ringtone, 1 - Custom Ringtone 1, 2 - Custom Ringtone 2, 3 - Custom Ringtone 3
# 6 - Custom Ringtone 4, 7 - Custom Ringtone 5, 8 - Custom Ringtone 6, 9 - Custom Ringtone 7, 10 - Custom Ringtone 8
# 11 - Custom Ringtone 9, 12 - Custom Ringtone 10, 4 - Silent, 5 - Default Ringtone
# Default is 0
# Number: 0 - 12
# Mandatory
P26069 = 0

# Matching Incoming Caller ID. Matching Rule 10
# String
P26096 = 

# Matching Rule 10 Distinctive Ringtone
# 0 - System Ringtone, 1 - Custom Ringtone 1, 2 - Custom Ringtone 2, 3 - Custom Ringtone 3
# 6 - Custom Ringtone 4, 7 - Custom Ringtone 5, 8 - Custom Ringtone 6, 9 - Custom Ringtone 7, 10 - Custom Ringtone 8
# 11 - Custom Ringtone 9, 12 - Custom Ringtone 10, 4 - Silent, 5 - Default Ringtone
# Default is 0
# Number: 0 - 12
# Mandatory
P26097 = 0

# Ring Timeout (in seconds). Default is 60
# Number: 30 - 3600
# Mandatory
P1328 = 60

#####################################################
# Account 1/Intercom Settings
#####################################################
# Allow Auto Answer by Call-Info/Alert-Info. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P298 = 0

# Mute on answer Intercom call. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P26071 = 0

# Play warning tone for Auto Answer Intercom. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P26072 = 0

# Custom Call-Info for Auto Answer
# String
P2356 = 

#####################################################
# Account 1/Feature Codes
#####################################################
# Enable Local Call Features.  0 - No, 1 - Yes. Default is 1
# Number: 0, 1
# Mandatory
P191 = 1

# DND Call Feature ON
# String
P2344 =

# DND Call Feature OFF
# String
P2345 =

# Call Forward Unconditionally (All) ON
# String
P26013 =

# Call Forward Unconditionally (All) - OFF
# String
P26014 =

# Call Forward Busy - ON
# String
P26009 =

# Call Forward Busy - OFF
# String
P26010 =

# Call Forward Delayed (No Answer) - ON
# String
P26011 =

# Call Forward Delayed (No Answer) - OFF
# String
P26012 =

# Delayed Call Forward Wait Time
# Number: 1 - 120. Default is 20.
# Mandatory
P139 = 20

####################################################################
# Account 2  - GXP1620/1625/1628/1630 only
####################################################################
##########################################
# Account 2/General Settings
##########################################
# Account Active. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P401 = 1

# Account Name
# String
P417 =

# SIP Server
# String
P402 =

# Secondary SIP Server
# String
P2412 =

# Outbound Proxy
# String
P403 =

# Backup Outbound Proxy
# String 
P2433 = 

# BLF Server
# String
P2475 =

# SIP User ID
# String
P404 =

# Authenticate ID
# String
P405 =

# Authenticate Password
# String
P406 =

# Name
# String
P407 =

# Voice Mail Access Number
# String
P426 =

# Account Display
# Number: 0 - User Name, 1 - User ID. Default is 0.
# Mandatory
P2480 = 0

##########################################
# Account 2/Network Settings
##########################################
# DNS Mode. 0 - A Record, 1 - SRV, 2 - NAPTR/SRV, 3 - Use Configured IP. Default is 0
# Number: 0, 1, 2, 3
# Mandatory
P408 = 0

# Primary IP. Maximum 15 characters
# String
P2408 =

# Backup IP 1
# String
P2409 =

# Backup IP 2
# String
P2410 =

# NAT Traversal. 0 - No, 1 - STUN, 2 - keep alive, 3 - UPnP, 4 - Auto, 5 - VPN. Default is 0.
# Number: 0, 1, 2, 3, 4, 5
# Mandatory
P414 = 0

# Proxy-Require (A SIP extension to enable firewall penetration). Max length is 64 characters
# String
P418 =

# Use SBC. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P26190 = 0

##########################################
# Account 2/SIP Settings/Basic Settings
##########################################
# TEL URI. 0 - Disabled, 1 - User=Phone, 2 - Enabled. Default is 0
# Number: 0, 1, 2
# Mandatory
P409 = 0

# SIP Registration. 0 - No, 1 - Yes. Default is 1
# Number: 0, 1
# Mandatory
P410 = 1

# Unregister On Reboot. 0 - No, 1 - All, 2 - Instace. Default is 0
# Number: 0, 1
# Mandatory
P411 = 0

# Register Expiration (in minutes). Default is 60. Max about 45 days
# Number: 1 - 64800
# Mandatory
P412 = 60

# Subscribe Expiration (in minutes). Default is 60. Max about 45 days
# Number: 1 - 64800
# Mandatory
P26151 = 60

# Reregister Before Expiration (in seconds). Default is 0 second
# Number: 0 - 64800
# Mandatory
P2430 = 0

# Enable OPTIONS Keep Alive
# Number: 0, 1
# Mandatory
P2497 = 0

# OPTIONS Keep Alive Interval (in seconds). Default is 30 seconds
# Number
# Mandatory
P2498 = 30

# OPTIONS Keep Alive Max Lost (number of max lost packets). Default is 3
# Number
# Mandatory
P2499 = 3

# Local SIP Port. Default is 5062
# Number
# Mandatory
P413 = 5062

# SIP Registration Failure Retry Wait Time (in seconds). Default is 20
# Number: 1 - 3600
# Mandatory
P471 = 20

# SIP T1 Timeout. RFC 3261 T1 value (RTT estimate)
# 50 - 0.5 sec, 100 - 1 sec, 200 - 2 sec. Default is 50
# Number: 50, 100, 200
# Mandatory
P440 = 50

# SIP T2 Timeout. RFC 3261 T2 value. The maximum retransmit interval for non-INVITE requests and INVITE responses
# 200 - 2 sec, 400 - 4 sec, 800 - 8 sec. Default is 400
# Number: 200, 400, 800
# Mandatory
P441 = 400

# Switch Backup Proxy on No Response. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P26192 = 0

# SIP Transport. 0 - UDP, 1 - TCP, 2 - TLS/TCP. Default is 0
# Number: 0, 1, 2
# Mandatory
P448 = 0

# SIP URI Scheme when using TLS. 0 - sip, 1 - sips. Default is 1
# Number: 0, 1
# Mandatory
P2429 = 1

# Use Actual Ephemeral Port in Contact with TCP/TLS. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P2431 = 0

# Outbound Proxy Mode. 0 - in route, 1 - not in route, 2 - always send to. Default is 0
# Number: 0, 1, 2
# Mandatory
P2405 = 0

# Support SIP Instance ID. 0 - No, 1 - Yes. Default is 1
# Number: 0, 1
# Mandatory
P489 = 1

# SUBSCRIBE for MWI. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P415 = 0

# SUBSCRIBE for Registration. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P2419 = 0

# Enable 100rel. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P435 = 0

# Callee ID Display. 0 - Auto, 1 - Disabled, 2 - To Header. Default is 0
# Number: 0, 1, 2
# Mandatory 
P26125 = 0

# Caller ID Display. 0 - Auto, 1 - Disabled, 2 - From Header. Default is 0
# Number: 0, 1, 2
# Mandatory
P2424 = 0

# Ignore Alert-Info header
# 0 - No, 1 - Yes. Default is 0
# Number 0,1
# Mandatory
P26118 = 0

# Add Auth Header On Initial REGISTER
# 0 - No, 1 - Yes. Default is 0
# Number 0,1
# Mandatory
P2459 = 0 

############################################
# Account 2/SIP Settings/Custom SIP Headers
############################################
# Use Privacy Header
# 0 - Default, 1 - No, 2 - Yes. Default is 0
# Number: 0, 1, 2
# Mandatory
P2438 = 0

# Use P-Preferred-Identity Header
# 0 - Default, 1 - No, 2 - Yes. Default is 0
# Number: 0, 1, 2
# Mandatory
P2439 = 0

# Use X-Grandstream-PBX Header
# 0 - No, 1 - Yes. Default is 1
# Number: 0, 1
# Mandatory
P26154 = 1

# Use P-Access-Network-Info Header
# 0 - No, 1 - Yes. Default is 1
# Number: 0, 1
# Mandatory
P26158 = 1

# Use P-Emergency-Info Header
# 0 - No, 1 - Yes. Default is 1
# Number: 0, 1
# Mandatory
P26159 = 1

# Use MAC Header
# 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P26161 = 0

##########################################
# Account 2/SIP Settings/Advanced Features
##########################################
# Line-seize Timeout (in seconds). Default is 15
# Number: 15-60
# Mandatory
P2413 = 15

# Eventlist BLF URI. For GXP1630/1628 only. 
# String
P444 = 

# Auto Provision Eventlist BLFs. For GXP1630/1628 only. 0 - disabled, 1 - enabled
# Number: 0, 1
# Default is 0
# Mandatory
P2489 = 0

# Conference URI
# String
P2418 =

# Music On Hold URI
# String
P2450 =

# Force BLF Call-pickup by prefix. For GXP1630/1628 only. 0 - No, 1 - Yes. Default is 0 
# Number: 0, 1
# Mandatory
P6753 = 0

# BLF Call-pickup Prefix. For GXP1630/1628 only.
# String. Defaule is "**"
P481 = **

# Call Pickup Barge-In Code. For GXP1630/1628 only.
# String 
P26146 =

# PUBLISH for Presence. For GXP1630/1628 only. 0 - No, 1 - Yes
# Number: 0, 1
# Default is 0
# Mandatory
P488 = 0

# Enable User Presence Subscription
# Number: 0 - No, 1 - Yes. Default is 0.
# Mandatory
P2453 = 0

# Hide Login Soft Key On Auto User Presence Subscription
# Number: 0 - No, 1 - Yes. Default is 1.
# Mandatory
P2454 = 1

# Auto User Presence ID
# String
P2451 =

# Auto User Presence Password
# String
P2452 = 

# Special Feature. 100 - Standard, 101 - Nortel MCS, 102- Broadsoft, 108 - CBCOM, 
# 109 - RNK, 110 - Sylantro, 117 - Huawei IMS, 119 - Phonepower
# Default is 100
# Number: 100, 101, 102, 108, 109, 110, 117, 119
# Mandatory
P424 = 100

# Broadsoft Call Center. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P2441 = 0

# Hoteling Event. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P2442 = 0

# Call Center Status. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P2443 = 0

# Feature Key Synchronization. 0 - Disabled, 1 - Enabled. Default is 0
# Number: 0, 1
# Mandatory
P2425 = 0

# Broadsoft Call Park
# Number: 0,1 - Default is 0
# Mandatory
P2488 = 0 

##########################################
# Account 2/SIP Settings/Session Timer
##########################################
# Enable Session Timer. 0 - No, 1 - Yes. Default is 1
# Number: 0, 1
# Mandatory
P2495 = 1

# Session Expiration (in seconds). Default is 180
# Number: 90 - 64800
# Mandatory
P434 = 180

# Minimum SE (in seconds). Default is 90. This value must be lower than or equal to P434
# Number: 90 - 64800
# Mandatory
P427 = 90

# Caller Request Timer (Request for timer when calling). 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P428 = 0

# Callee Request Timer (Request for timer when called. i.e. if remote party supports timer but did not request for one)
# 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P429 = 0

# Force Timer (Still use timer when remote party does not support timer). 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P430 = 0

# UAC Specify Refresher. 0 - omit, 1 - UAC, 2 - UAS. Default is 0
# Number: 0, 1, 2
# Mandatory
P432 = 0

# UAS Specify Refresher. 1 - UAC, 2 - UAS. Default is 1
# Number: 1, 2
# Mandatory
P433 = 1

# Force INVITE (Always refresh with INVITE instead of UPDATE even when remote party supports UPDATE).
# 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P431 = 0

############################################
# Account 2/SIP Settings/Security Settings
############################################
# Check Domain Certificates. When set to Yes/Enabled, domain certificate will be checked as defined in RFC5922
# 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P2411 = 0

# Validate Certification Chain. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P2467 = 0

# Validate Incoming Messages. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P2406 = 0

# Check SIP User ID for incoming INVITE. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P449 = 0

# Accept Incoming SIP from Proxy Only. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P2447 = 0

# Authenticate Incoming INVITE. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P2446 = 0

##########################################
# Account 2/Audio Settings
##########################################
# Send DTMF: In-audio. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P2401 = 0

# Send DTMF: Via RTP (RFC2833). 0 - No, 1 - Yes. Default is 1
# Number: 0, 1
# Mandatory
P2402 = 1

# Send DTMF: Via SIP INFO. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P2403 = 0

# DTMF Payload Type. Default is 101
# Number: 96 - 127
# Mandatory
P496 = 101

# Preferred Vocoder
# 0 - PCMU, 2 - G.726-32, 4 - G.723.1, 8 - PCMA, 9 - G.722, 18 - G.729A/B, 98 - iLBC
# choice 1. Default is 0
# Number: 0, 2, 4, 8, 9, 18, 98
# Mandatory
P451 = 0

# choice 2. Default is 8
# Number: 0, 2, 4, 8, 9, 18, 98
# Mandatory
P452 = 8

# choice 3. Default is 18
# Number: 0, 2, 4, 8, 9, 18, 98
# Mandatory
P453 = 18

# choice 4. Default is 9
# Number: 0, 2, 4, 8, 9, 18, 98
# Mandatory
P454 = 9

# choice 5. Default is 2
# Number: 0, 2, 4, 8, 9, 18, 98
# Mandatory
P455 = 2

# choice 6. Default is 2
# Number: 0, 2, 4, 8, 9, 18, 98
# Mandatory
P456 = 2

# choice 7. Default is 2
# Number: 0, 2, 4, 8, 9, 18, 98
# Mandatory
P457 = 2

# Use First Matching Vocoder in 200OK SDP. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P2448 = 0

# Codec Negotiation Priority. 0 - Caller, 1 - Callee. Default is 1
# Number: 0, 1
# Mandatory
P29161 = 1

# Disable Multiple m line in SDP. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P487 = 0

# SRTP Mode. 0 - Disabled, 1 - Enabled but not forced, 2 - Enabled and forced, 3 - Optional. Default is 0
# Number: 0, 1, 2, 3
# Mandatory
P443 = 0

# Symmetric RTP. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P460 = 0

# Silence Suppression. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P485 = 0

# Voice Frames per TX (up to 10/20/32/64 frames for G711/G726/G723/other codecs respectively). Default is 2
# Number: 1 - 64
# Mandatory
P486 = 2

# G723 Rate. 0 - 6.3kbps, 1 - 5.3kbps. Default is 0-23
# Number: 0, 1
# Mandatory
P493 = 0

# G.726-32 Packing Mode. 0 - ITU, 1 - IETF. Default is 0
# Number: 0, 1
# Mandatory
P2423 = 0

# iLBC Frame Size, Default is 1. 0 - 20ms, 1 - 30ms. 
# Number: 0, 1
# Mandatory
P495 = 1

# iLBC Payload Type, Default is 97
# Number: 96 - 127
# Mandatory
P494 = 97

# Jitter Buffer Type. 0 - Fixed, 1 - Adaptive. Default is 1
# Number: 0, 1
# Mandatory
P498 = 1

# Jitter Buffer Length. 0 - 100ms, 1 - 200ms, 2 - 300ms, 3 - 400ms, 4 - 500ms, 5 - 600ms, 6 - 700ms, 7 - 800ms
# Default is 2
# Number: 0, 1, 2, 3, 4, 5, 6, 7
# Mandatory
P497 = 2

# Hide Vocoder. 0 - No, 1 - Yes. Default is 0.
# Number: 0, 1
# Mandatory
P26147 = 0

##########################################
# Account 2/Call Settings
##########################################
# Early Dial (use "Yes" only if proxy supports 484 response). 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P422 = 0

# Dial Plan Prefix
# String 
P419 =

# Dial Plan. Default is { x+ | *x+ | *xx*x+ }
# String
# Mandatory
P459 = { x+ | *x+ | *xx*x+ }

# Bypass Dial Plan. Default is Mpk
# String: Contact, Call History Incoming Call, Call History Outgoing Call, Dialing Page, Mpk, Api
# P2482 = Mpk

# Call Log. 0 - Log All, 1 - Log Incoming/Outgoing only (Missed calls NOT recorded), 2 - Disable Call Log. Default is 0
# Number: 0, 1, 2
# Mandatory
P442 = 0

# Send Anonymous (caller ID will be blocked if set to Yes). 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P421 = 0

# Anonymous Call Rejection. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P446 = 0

# Auto Answer. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P425 = 0

# Auto Answer Numbers
# String
P29164 = 

# Refer-To Use Target Contact. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P469 = 0

# Transfer on conference Hang-Up. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P2404 = 0

# Disable Recovery on Blind Transfer, 0 - No, 1- Yes. Default is 0
# Number: 0, 1
# Mandatory
P2484 = 0

# Blind Transfer Wait Timeout, in seconds. Default is 30
# Number: 30 to 300
P26170 = 30

# No Key Entry Timeout (in seconds). Default is 4
# Number: 1 - 15
# Mandatory
P491 = 4

# Key As Send. 0 - Disable, 1 - Pound (#). Default is 1
# Number: 0, 1
# Mandatory
P492 = 1

# On Hold Reminder Tone.  0 - Disabled, 1 - Enabled. Default is 0
# Number: 0, 1
# Mandatory
P26106 = 0

# Call Recording ON
# String
P26128 =

# Call Recording OFF
# String
P26129 =

# Hide Dialing Password - Prefix for Dialing Password
# String
P26149 = 

# Hide Dialing Password - Password Length. Default is 0.
# Number: 0 - 32
P26150 = 0

# Remote Info Display
# 0 - Name and Number, 1 - Number, 2 - Name. Default is 0
# Number: 0, 1, 2
P26176 = 0

# Hide Remote User ID - Call Type. 0 - None of Call, 1 - Incoming Calls, 2 - Outgoing Calls, 3 - Both Directions. Default is 0.
# Number: 0 - 3
# Mandatory
P26143 = 0

# Hide Remote User ID - Length
# Number: 0 ... N
P26144 = 0

# Account Ring Tone. 0 - System Ringtone, 1 - Custom Ringtone 1, 2 - Custom Ringtone 2, 3 - Custom Ringtone 3
# 6 - Custom Ringtone 4, 7 - Custom Ringtone 5, 8 - Custom Ringtone 6, 9 - Custom Ringtone 7, 10 - Custom Ringtone 8
# 11 - Custom Ringtone 9, 12 - Custom Ringtone 10, 4 - Silent, 5 - Default Ringtone
# Default is 5
# Number: 0 - 12
P423 = 5

# Matching Incoming Caller ID. Matching Rule 1
# String
P1494 = 

# Matching Rule 1 Distinctive Ringtone
# 0 - System Ringtone, 1 - Custom Ringtone 1, 2 - Custom Ringtone 2, 3 - Custom Ringtone 3
# 6 - Custom Ringtone 4, 7 - Custom Ringtone 5, 8 - Custom Ringtone 6, 9 - Custom Ringtone 7, 10 - Custom Ringtone 8
# 11 - Custom Ringtone 9, 12 - Custom Ringtone 10, 4 - Silent, 5 - Default Ringtone
# Default is 0
# Number: 0 - 12
# Mandatory
P1495 = 0

# Matching Incoming Caller ID. Matching Rule 2
# String
P1496 = 

# Matching Rule 2 Distinctive Ringtone
# 0 - System Ringtone, 1 - Custom Ringtone 1, 2 - Custom Ringtone 2, 3 - Custom Ringtone 3
# 6 - Custom Ringtone 4, 7 - Custom Ringtone 5, 8 - Custom Ringtone 6, 9 - Custom Ringtone 7, 10 - Custom Ringtone 8
# 11 - Custom Ringtone 9, 12 - Custom Ringtone 10, 4 - Silent, 5 - Default Ringtone
# Default is 0
# Number: 0 - 12
# Mandatory
P1497 = 0

# Matching Incoming Caller ID. Matching Rule 3
# String
P1498 =

# Matching Rule 3 Distinctive Ringtone
# 0 - System Ringtone, 1 - Custom Ringtone 1, 2 - Custom Ringtone 2, 3 - Custom Ringtone 3
# 6 - Custom Ringtone 4, 7 - Custom Ringtone 5, 8 - Custom Ringtone 6, 9 - Custom Ringtone 7, 10 - Custom Ringtone 8
# 11 - Custom Ringtone 9, 12 - Custom Ringtone 10, 4 - Silent, 5 - Default Ringtone
# Default is 0
# Number: 0 - 12
# Mandatory
P1499 = 0

# Matching Incoming Caller ID. Matching Rule 4
# String
P6722 = 

# Matching Rule 4 Distinctive Ringtone
# 0 - System Ringtone, 1 - Custom Ringtone 1, 2 - Custom Ringtone 2, 3 - Custom Ringtone 3
# 6 - Custom Ringtone 4, 7 - Custom Ringtone 5, 8 - Custom Ringtone 6, 9 - Custom Ringtone 7, 10 - Custom Ringtone 8
# 11 - Custom Ringtone 9, 12 - Custom Ringtone 10, 4 - Silent, 5 - Default Ringtone
# Default is 0
# Number: 0 - 12
# Mandatory
P6723 = 0

# Matching Incoming Caller ID. Matching Rule 5
# String
P6724 = 

# Matching Rule 5 Distinctive Ringtone
# 0 - System Ringtone, 1 - Custom Ringtone 1, 2 - Custom Ringtone 2, 3 - Custom Ringtone 3
# 6 - Custom Ringtone 4, 7 - Custom Ringtone 5, 8 - Custom Ringtone 6, 9 - Custom Ringtone 7, 10 - Custom Ringtone 8
# 11 - Custom Ringtone 9, 12 - Custom Ringtone 10, 4 - Silent, 5 - Default Ringtone
# Default is 0
# Number: 0 - 12
# Mandatory
P6725 = 0

# Matching Incoming Caller ID. Matching Rule 6
# String
P6726 = 

# Matching Rule 6 Distinctive Ringtone
# 0 - System Ringtone, 1 - Custom Ringtone 1, 2 - Custom Ringtone 2, 3 - Custom Ringtone 3
# 6 - Custom Ringtone 4, 7 - Custom Ringtone 5, 8 - Custom Ringtone 6, 9 - Custom Ringtone 7, 10 - Custom Ringtone 8
# 11 - Custom Ringtone 9, 12 - Custom Ringtone 10, 4 - Silent, 5 - Default Ringtone
# Default is 0
# Number: 0 - 12
# Mandatory
P6727 = 0

# Matching Incoming Caller ID. Matching Rule 7
# String
P26164 = 

# Matching Rule 7 Distinctive Ringtone
# 0 - System Ringtone, 1 - Custom Ringtone 1, 2 - Custom Ringtone 2, 3 - Custom Ringtone 3
# 6 - Custom Ringtone 4, 7 - Custom Ringtone 5, 8 - Custom Ringtone 6, 9 - Custom Ringtone 7, 10 - Custom Ringtone 8
# 11 - Custom Ringtone 9, 12 - Custom Ringtone 10, 4 - Silent, 5 - Default Ringtone
# Default is 0
# Number: 0 - 12
# Mandatory
P26165 = 0

# Matching Incoming Caller ID. Matching Rule 8
# String
P26166 = 

# Matching Rule 8 Distinctive Ringtone
# 0 - System Ringtone, 1 - Custom Ringtone 1, 2 - Custom Ringtone 2, 3 - Custom Ringtone 3
# 6 - Custom Ringtone 4, 7 - Custom Ringtone 5, 8 - Custom Ringtone 6, 9 - Custom Ringtone 7, 10 - Custom Ringtone 8
# 11 - Custom Ringtone 9, 12 - Custom Ringtone 10, 4 - Silent, 5 - Default Ringtone
# Default is 0
# Number: 0 - 12
# Mandatory
P26167= 0

# Matching Incoming Caller ID. Matching Rule 9
# String
P26168 = 

# Matching Rule 9 Distinctive Ringtone
# 0 - System Ringtone, 1 - Custom Ringtone 1, 2 - Custom Ringtone 2, 3 - Custom Ringtone 3
# 6 - Custom Ringtone 4, 7 - Custom Ringtone 5, 8 - Custom Ringtone 6, 9 - Custom Ringtone 7, 10 - Custom Ringtone 8
# 11 - Custom Ringtone 9, 12 - Custom Ringtone 10, 4 - Silent, 5 - Default Ringtone
# Default is 0
# Number: 0 - 12
# Mandatory
P26169 = 0

# Matching Incoming Caller ID. Matching Rule 10
# String
P26196 = 

# Matching Rule 10 Distinctive Ringtone
# 0 - System Ringtone, 1 - Custom Ringtone 1, 2 - Custom Ringtone 2, 3 - Custom Ringtone 3
# 6 - Custom Ringtone 4, 7 - Custom Ringtone 5, 8 - Custom Ringtone 6, 9 - Custom Ringtone 7, 10 - Custom Ringtone 8
# 11 - Custom Ringtone 9, 12 - Custom Ringtone 10, 4 - Silent, 5 - Default Ringtone
# Default is 0
# Number: 0 - 12
# Mandatory
P26197 = 0

# Ring Timeout (in seconds). Default is 60
# Number: 30 - 3600
# Mandatory
P476 = 60

####################################################
# Account 2/Intercom Settings
####################################################
# Allow Auto Answer by Call-Info/Alert-Info. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P438 = 0

# Mute on answer Intercom call. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P26171 = 0

# Play warning tone for Auto Answer Intercom. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P26172 = 0

# Custom Call-Info for Auto Answer.
# String
P2456 = 

#####################################################
# Account 2/Feature Codes
#####################################################
# Enable Local Call Features.  0 - No, 1 - Yes. Default is 1
# Number: 0, 1
# Mandatory
P420 = 1

# DND Call Feature ON
# String
P2444 =

# DND Call Feature OFF
# String
P2445 =

# Call Forward Unconditionally (All) ON
# String
P26113 =

# Call Forward Unconditionally (All) - OFF
# String
P26114 =

# Call Forward Busy - ON
# String
P26109 =

# Call Forward Busy - OFF
# String
P26110 =

# Call Forward Delayed (No Answer) - ON
# String
P26111 =

# Call Forward Delayed (No Answer) - OFF
# String
P26112 =

# Delayed Call Forward Wait Time
# Number: 1 - 120. Default is 20.
# Mandatory
P470 = 20

####################################################################
# Account 3  - GXP1630 only
####################################################################
##########################################
# Account 3/General Settings
##########################################
# Account Active. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P501 = 1

# Account Name
# String
P517 =

# SIP Server
# String
P502 =

# Secondary SIP Server
# String
P2512 =

# Outbound Proxy
# String
P503 =

# Backup Outbound Proxy
# String 
P2533 = 

# BLF Server
# String
P2575 = 

# SIP User ID
# String
P504 =

# Authenticate ID
# String
P505 =

# Authenticate Password
# String
P506 =

# Name
# String
P507 =

# Voice Mail Access Number
# String
P526 =

# Account Display
# Number: 0 - User Name, 1 - User ID. Default is 0.
# Mandatory
P2580 = 0

##########################################
# Account 3/Network Settings
##########################################
# DNS Mode. 0 - A Record, 1 - SRV, 2 - NAPTR/SRV, 3 - Use Configured IP. Default is 0
# Number: 0, 1, 2, 3
# Mandatory
P508 = 0

# Primary IP. Maximum 15 characters
# String
P2508 =

# Backup IP 1
# String
P2509 =

# Backup IP 2
# String
P2510 =

# NAT Traversal. 0 - No, 1 - STUN, 2 - keep alive, 3 - UPnP, 4 - Auto, 5 - VPN. Default is 0.
# Number: 0, 1, 2, 3, 4, 5
# Mandatory
P514 = 0

# Proxy-Require (A SIP extension to enable firewall penetration). Max length is 64 characters
# String
P518 =

# Use SBC. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P26290 = 0

##########################################
# Account 3/SIP Settings/Basic Settings
##########################################
# TEL URI. 0 - Disabled, 1 - User=Phone, 2 - Enabled. Default is 0
# Number: 0, 1, 2
# Mandatory
P509 = 0

# SIP Registration. 0 - No, 1 - Yes. Default is 1
# Number: 0, 1
# Mandatory
P510 = 1

# Unregister On Reboot. 0 - No, 1 - All, 2 - Instace. Default is 0
# Number: 0, 1
# Mandatory
P511 = 0

# Register Expiration (in minutes). Default is 60. Max about 45 days
# Number: 1 - 64800
# Mandatory
P512 = 60

# Subscribe Expiration (in minutes). Default is 60. Max about 45 days
# Number: 1 - 64800
# Mandatory
P26251 = 60

# Reregister Before Expiration (in seconds). Default is 0 second
# Number: 0 - 64800
# Mandatory
P2530 = 0

# Enable OPTIONS Keep Alive
# Number: 0, 1
# Mandatory
P2597 = 0

# OPTIONS Keep Alive Interval (in seconds). Default is 30 seconds
# Number
# Mandatory
P2598 = 30

# OPTIONS Keep Alive Max Lost (number of max lost packets). Default is 3
# Number
# Mandatory
P2599 = 3

# Local SIP Port. Default is 5064
# Number
# Mandatory
P513 = 5064

# SIP Registration Failure Retry Wait Time (in seconds). Default is 20
# Number: 1 - 3600
# Mandatory
P571 = 20

# SIP T1 Timeout. RFC 3261 T1 value (RTT estimate)
# 50 - 0.5 sec, 100 - 1 sec, 200 - 2 sec. Default is 50
# Number: 50, 100, 200
# Mandatory
P540 = 50

# SIP T2 Timeout. RFC 3261 T2 value. The maximum retransmit interval for non-INVITE requests and INVITE responses
# 200 - 2 sec, 400 - 4 sec, 800 - 8 sec. Default is 400
# Number: 200, 400, 800
# Mandatory
P541 = 400

# SIP Transport. 0 - UDP, 1 - TCP, 2 - TLS/TCP. Default is 0
# Number: 0, 1, 2
# Mandatory
P548 = 0

# SIP URI Scheme when using TLS. 0 - sip, 1 - sips. Default is 1
# Number: 0, 1
# Mandatory
P2529 = 1

# Use Actual Ephemeral Port in Contact with TCP/TLS. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P2531 = 0

# Outbond Proxy Mode. 0 - in route, 1 - not in route, 2 - always send to. Default is 0
# Number: 0, 1, 2
# Mandatory
P2505 = 0

# Support SIP Instace ID. 0 - No, 1 - Yes. Default is 1
# Number: 0, 1
# Mandatory
P589 = 1

# SUBSCRIBE for MWI. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P515 = 0

# SUBSCRIBE for Registration. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P2519 = 0

# Enable 100rel. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P535 = 0

# Caller ID Display. 0 - Auto, 1 - Disabled, 2 - From Header. Default is 0
# Number: 0, 1, 2
# Mandatory
P2524 = 0

# Ignore Alert-Info header
# 0 - No, 1 - Yes. Default is 0
# Number 0,1
# Mandatory
P26218 = 0

# Add Auth Header On Initial REGISTER
# 0 - No, 1 - Yes. Default is 0
# Number 0,1
# Mandatory
P2559 = 0 

############################################
# Account 3/SIP Settings/Custom SIP Headers
############################################
# Use Privacy Header
# 0 - Default, 1 - No, 2 - Yes. Default is 0
# Number: 0, 1, 2
# Mandatory
P2538 = 0

# Use P-Preferred-Identity Header
# 0 - Default, 1 - No, 2 - Yes. Default is 0
# Number: 0, 1, 2
# Mandatory
P2539 = 0

# Use X-Grandstream-PBX Header
# 0 - No, 1 - Yes. Default is 1
# Number: 0, 1
# Mandatory
P26254 = 1

# Use P-Access-Network-Info Header
# 0 - No, 1 - Yes. Default is 1
# Number: 0, 1
# Mandatory
P26258 = 1

# Use P-Emergency-Info Header
# 0 - No, 1 - Yes. Default is 1
# Number: 0, 1
# Mandatory
P26259 = 1

# Use MAC Header
# 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P26261 = 0

##########################################
# Account 3/SIP Settings/Advanced Features
##########################################
# Line-seize Timeout (in seconds). Default is 15
# Number: 15-60
# Mandatory
P2513 = 15

# Eventlist BLF URI. For GXP1630/1628 only. 
# String
P544 = 

# Auto Provision Eventlist BLFs. For GXP1630/1628 only. 0 - disabled, 1 - enabled
# Number: 0, 1
# Default is 0
# Mandatory
P2589 = 0

# Conference URI
# String
P2518 =

# Music On Hold URI
# String
P2550 =

# Force BLF Call-pickup by prefix. For GXP1630/1628 only. 0 - No, 1 - Yes. Default is 0 
# Number: 0, 1
# Mandatory
P6754 = 0

# BLF Call-pickup Prefix. For GXP1630/1628 only. 
# String. Defaule is "**"
P581 = **

# Call Pickup Barge-In Code. For GXP1630/1628 only.
# String 
P26246 =

# PUBLISH for Presence. For GXP1630/1628 only. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P588 = 0

# Enable User Presence Subscription
# Number: 0 - No, 1 - Yes. Default is 0.
# Mandatory
P2553 = 0

# Hide Login Soft Key On Auto User Presence Subscription
# Number: 0 - No, 1 - Yes. Default is 1.
# Mandatory
P2554 = 1

# Auto User Presence ID
# String
P2551 =

# Auto User Presence Password
# String
P2552 =

# Special Feature. 100 - Standard, 101 - Nortel MCS, 102- Broadsoft, 108 - CBCOM, 
# 109 - RNK, 110 - Sylantro, 117 - Huawei IMS, 119 - Phonepower
# Default is 100
# Number: 100, 101, 102, 108, 109, 110, 117, 119
# Mandatory
P524 = 100

# Broadsoft Call Center. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P2541 = 0

# Hoteling Event. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P2542 = 0

# Call Center Status. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P2543 = 0

# Feature Key Synchronization. 0 - Disabled, 1 - Enabled. Default is 0
# Number: 0, 1
# Mandatory
P2525 = 0

# Broadsoft Call Park
# Number: 0,1 - Default is 0
# Mandatory
P2588 = 0 

##########################################
# Account 3/SIP Settings/Session Timer
##########################################
# Enable Session Timer. 0 - No, 1 - Yes. Default is 1
# Number: 0, 1
# Mandatory
P2595 = 1

# Session Expiration (in seconds). Default is 180
# Number: 90 - 64800
# Mandatory
P534 = 180

# Minimum SE (in seconds). Default is 90. This value must be lower than or equal to P434
# Number: 90 - 64800
# Mandatory
P527 = 90

# Caller Request Timer (Request for timer when calling). 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P528 = 0

# Callee Request Timer (Request for timer when called. i.e. if remote party supports timer but did not request for one)
# 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P529 = 0

# Force Timer (Still use timer when remote party does not support timer). 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P530 = 0

# UAC Specify Refresher. 0 - omit, 1 - UAC, 2 - UAS. Default is 0
# Number: 0, 1, 2
# Mandatory
P532 = 0

# UAS Specify Refresher. 1 - UAC, 2 - UAS. Default is 1
# Number: 1, 2
# Mandatory
P533 = 1

# Force INVITE (Always refresh with INVITE instead of UPDATE even when remote party supports UPDATE).
# 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P531 = 0


##########################################
# Account 3/SIP Settings/Security Settings
##########################################
# Check Domain Certificates. When set to Yes/Enabled, domain certificate will be checked as defined in RFC5922
# 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P2511 = 0

# Validate Certification Chain. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P2567 = 0

# Validate Incoming Messages. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P2506 = 0

# Check SIP User ID for incoming INVITE. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P549 = 0

# Accept Incoming SIP from Proxy Only. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P2547 = 0

# Authenticate Incoming INVITE. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P2546 = 0

##########################################
# Account 3/Audio Settings
##########################################
# Send DTMF: In-audio. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P2501 = 0

# Send DTMF: Via RTP (RFC2833). 0 - No, 1 - Yes. Default is 1
# Number: 0, 1
# Mandatory
P2502 = 1

# Send DTMF: Via SIP INFO. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P2503 = 0

# DTMF Payload Type. Default is 101
# Number: 96 - 127
# Mandatory
P596 = 101

# Preferred Vocoder
# 0 - PCMU, 2 - G.726-32, 4 - G.723.1, 8 - PCMA, 9 - G.722, 18 - G.729A/B, 98 - iLBC
# choice 1. Default is 0
# Number: 0, 2, 4, 8, 9, 18, 98
# Mandatory
P551 = 0

# choice 2. Default is 8
# Number: 0, 2, 4, 8, 9, 18, 98
# Mandatory
P552 = 8

# choice 3. Default is 18
# Number: 0, 2, 4, 8, 9, 18, 98
# Mandatory
P553 = 18

# choice 4. Default is 9
# Number: 0, 2, 4, 8, 9, 18, 98
# Mandatory
P554 = 9

# choice 5. Default is 2
# Number: 0, 2, 4, 8, 9, 18, 98
# Mandatory
P555 = 2

# choice 6. Default is 2
# Number: 0, 2, 4, 8, 9, 18, 98
# Mandatory
P556 = 2

# choice 7. Default is 2
# Number: 0, 2, 4, 8, 9, 18, 98
# Mandatory
P557 = 2

# Use First Matching Vocoder in 200OK SDP. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P2548 = 0

# Codec Negotiation Priority. 0 - Caller, 1 - Callee. Default is 1
# Number: 0, 1
# Mandatory
P29261 = 1

# Disable Multiple m line in SDP. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P587 = 0

# SRTP Mode. 0 - Disabled, 1 - Enabled but not forced, 2 - Enabled and forced, 3 - Optional. Default is 0
# Number: 0, 1, 2, 3
# Mandatory
P543 = 0

# Symmetric RTP. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P560 = 0

# Silence Suppression. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P585 = 0

# Voice Frames per TX (up to 10/20/32/64 frames for G711/G726/G723/other codecs respectively). Default is 2
# Number: 1 - 64
# Mandatory
P586 = 2

# G723 Rate. 0 - 6.3kbps, 1 - 5.3 kbps. Default is 0
# Number: 0, 1
# Mandatory
P593 = 0

# G.726-32 Packing Mode. 0 - ITU, 1 - IETF. Default is 0
# Number: 0, 1
# Mandatory
P2523 = 0

# iLBC Frame Size, Default is 1. 0 - 20ms, 1 - 30ms. 
# Number: 0, 1
# Mandatory
P595 = 1

# iLBC Payload Type, Default is 97
# Number: 96 - 127
# Mandatory
P594 = 97

# Jitter Buffer Type. 0 - Fixed, 1 - Adaptive. Default is 1
# Number: 0, 1
# Mandatory
P598 = 1

# Jitter Buffer Length. 0 - 100ms, 1 - 200ms, 2 - 300ms, 3 - 400ms, 4 - 500ms, 5 - 600ms, 6 - 700ms, 7 - 800ms
# Default is 2
# Number: 0, 1, 2, 3, 4, 5, 6, 7
# Mandatory
P597 = 2

# Hide Vocodec. 0 - No, 1 - Yes. Default is 0.
# Number: 0, 1
# Mandatory
P26247 = 0

##########################################
# Account 3/Call Settings
##########################################
# Early Dial (use "Yes" only if proxy supports 484 response). 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P522 = 0

# Dial Plan Prefix
# String 
P519 =

# Dial Plan. Default is { x+ | *x+ | *xx*x+ }
# String
# Mandatory
P559 = { x+ | *x+ | *xx*x+ }

# Bypass Dial Plan. Default is Mpk
# String: Contact, Call History Incoming Call, Call History Outgoing Call, Dialing Page, Mpk, Api
# P2582 = Mpk

# Call Log. 0 - Log All, 1 - Log Incoming/Outgoing only (Missed calls NOT recorded), 2 - Disable Call Log. Default is 0
# Number: 0, 1, 2
# Mandatory
P542 = 0

# Send Anonymous (caller ID will be blocked if set to Yes). 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P521 = 0

# Anonymous Call Rejection. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P546 = 0

# Auto Answer. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P525 = 0

# Auto Answer Numbers
# String
P29264 = 

# Refer-To Use Target Contact. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P569 = 0

# Transfer on conference Hang-Up. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P2504 = 0

# Disable Recovery on Blind Transfer, 0 - No, 1- Yes. Default is 0
# Number: 0, 1
# Mandatory
P2584 = 0

# Blind Transfer Wait Timeout, in seconds. Default is 30
# Number: 30 to 300
P26270 = 30

# No Key Entry Timeout (in seconds). Default is 4
# Number: 1 - 15
# Mandatory
P591 = 4

# Key As Send. 0 - Disabled, 1 - Pound (#). Default is 1
# Number: 0, 1
# Mandatory
P592 = 1

# On Hold Reminder Tone.  0 - Disabled, 1 - Enabled. Default is 0
# Number: 0, 1
# Mandatory
P26206 = 0

# Call Recording ON
# String
P26228 =

# Call Recording OFF
# String
P26229 =

# Hide Password - Prefix for Dialing Password.
# String
P26249 =

# Hide Password - Password Length. Default is 0.
# Number: 0 - 32
P26250 = 0

# Remote Info Display
# 0 - Name and Number, 1 - Number, 2 - Name. Default is 0
# Number: 0, 1, 2
P26276 = 0

# Hide Remote User ID - Call Type. 0 - None of Call, 1 - Incoming Calls, 2 - Outgoing Calls, 3 - Both Directions. Default is 0-23
# Number: 0 - 3
# Mandatory
P26243 = 0

# Hide Remote User ID - Length
# Number: 0 ... N
P26244 = 0

# Account Ring Tone. 0 - System Ringtone, 1 - Custom Ringtone 1, 2 - Custom Ringtone 2, 3 - Custom Ringtone 3
# 6 - Custom Ringtone 4, 7 - Custom Ringtone 5, 8 - Custom Ringtone 6, 9 - Custom Ringtone 7, 10 - Custom Ringtone 8
# 11 - Custom Ringtone 9, 12 - Custom Ringtone 10, 4 - Silent, 5 - Default Ringtone
# Default is 5
# Number: 0 - 12
P523 = 5

# Matching Incoming Caller ID. Matching Rule 1
# String
P1500 = 

# Matching Rule 1 Distinctive Ringtone
# 0 - System Ringtone, 1 - Custom Ringtone 1, 2 - Custom Ringtone 2, 3 - Custom Ringtone 3
# 6 - Custom Ringtone 4, 7 - Custom Ringtone 5, 8 - Custom Ringtone 6, 9 - Custom Ringtone 7, 10 - Custom Ringtone 8
# 11 - Custom Ringtone 9, 12 - Custom Ringtone 10, 4 - Silent, 5 - Default Ringtone
# Default is 0
# Number: 0 - 12
# Mandatory
P1501 = 0

# Matching Incoming Caller ID. Matching Rule 2
# String
P1502 = 

# Matching Rule 2 Distinctive Ringtone
# 0 - System Ringtone, 1 - Custom Ringtone 1, 2 - Custom Ringtone 2, 3 - Custom Ringtone 3
# 6 - Custom Ringtone 4, 7 - Custom Ringtone 5, 8 - Custom Ringtone 6, 9 - Custom Ringtone 7, 10 - Custom Ringtone 8
# 11 - Custom Ringtone 9, 12 - Custom Ringtone 10, 4 - Silent, 5 - Default Ringtone
# Default is 0
# Number: 0 - 12
# Mandatory
P1503 = 0

# Matching Incoming Caller ID. Matching Rule 3
# String
P1504 =


# Matching Rule 3 Distinctive Ringtone
# 0 - System Ringtone, 1 - Custom Ringtone 1, 2 - Custom Ringtone 2, 3 - Custom Ringtone 3
# 6 - Custom Ringtone 4, 7 - Custom Ringtone 5, 8 - Custom Ringtone 6, 9 - Custom Ringtone 7, 10 - Custom Ringtone 8
# 11 - Custom Ringtone 9, 12 - Custom Ringtone 10, 4 - Silent, 5 - Default Ringtone
# Default is 0
# Number: 0 - 12
# Mandatory
P1505 = 0

# Matching Incoming Caller ID. Matching Rule 4
# String
P6728 = 

# Matching Rule 4 Distinctive Ringtone
# 0 - System Ringtone, 1 - Custom Ringtone 1, 2 - Custom Ringtone 2, 3 - Custom Ringtone 3
# 6 - Custom Ringtone 4, 7 - Custom Ringtone 5, 8 - Custom Ringtone 6, 9 - Custom Ringtone 7, 10 - Custom Ringtone 8
# 11 - Custom Ringtone 9, 12 - Custom Ringtone 10, 4 - Silent, 5 - Default Ringtone
# Default is 0
# Number: 0 - 12
# Mandatory
P6729 = 0

# Matching Incoming Caller ID. Matching Rule 5
# String
P6730 = 

# Matching Rule 5 Distinctive Ringtone
# 0 - System Ringtone, 1 - Custom Ringtone 1, 2 - Custom Ringtone 2, 3 - Custom Ringtone 3
# 6 - Custom Ringtone 4, 7 - Custom Ringtone 5, 8 - Custom Ringtone 6, 9 - Custom Ringtone 7, 10 - Custom Ringtone 8
# 11 - Custom Ringtone 9, 12 - Custom Ringtone 10, 4 - Silent, 5 - Default Ringtone
# Default is 0
# Number: 0 - 12
# Mandatory
P6731 = 0

# Matching Incoming Caller ID. Matching Rule 6
# String
P6732 = 

# Matching Rule 6 Distinctive Ringtone
# 0 - System Ringtone, 1 - Custom Ringtone 1, 2 - Custom Ringtone 2, 3 - Custom Ringtone 3
# 6 - Custom Ringtone 4, 7 - Custom Ringtone 5, 8 - Custom Ringtone 6, 9 - Custom Ringtone 7, 10 - Custom Ringtone 8
# 11 - Custom Ringtone 9, 12 - Custom Ringtone 10, 4 - Silent, 5 - Default Ringtone
# Default is 0
# Number: 0 - 12
# Mandatory
P6733 = 0

# Matching Incoming Caller ID. Matching Rule 7
# String
P26264 = 

# Matching Rule 7 Distinctive Ringtone
# 0 - System Ringtone, 1 - Custom Ringtone 1, 2 - Custom Ringtone 2, 3 - Custom Ringtone 3
# 6 - Custom Ringtone 4, 7 - Custom Ringtone 5, 8 - Custom Ringtone 6, 9 - Custom Ringtone 7, 10 - Custom Ringtone 8
# 11 - Custom Ringtone 9, 12 - Custom Ringtone 10, 4 - Silent, 5 - Default Ringtone
# Default is 0
# Number: 0 - 12
# Mandatory
P26265 = 0

# Matching Incoming Caller ID. Matching Rule 8
# String
P26266 = 

# Matching Rule 8 Distinctive Ringtone
# 0 - System Ringtone, 1 - Custom Ringtone 1, 2 - Custom Ringtone 2, 3 - Custom Ringtone 3
# 6 - Custom Ringtone 4, 7 - Custom Ringtone 5, 8 - Custom Ringtone 6, 9 - Custom Ringtone 7, 10 - Custom Ringtone 8
# 11 - Custom Ringtone 9, 12 - Custom Ringtone 10, 4 - Silent, 5 - Default Ringtone
# Default is 0
# Number: 0 - 12
# Mandatory
P26267 = 0

# Matching Incoming Caller ID. Matching Rule 9
# String
P26268 = 

# Matching Rule 9 Distinctive Ringtone
# 0 - System Ringtone, 1 - Custom Ringtone 1, 2 - Custom Ringtone 2, 3 - Custom Ringtone 3
# 6 - Custom Ringtone 4, 7 - Custom Ringtone 5, 8 - Custom Ringtone 6, 9 - Custom Ringtone 7, 10 - Custom Ringtone 8
# 11 - Custom Ringtone 9, 12 - Custom Ringtone 10, 4 - Silent, 5 - Default Ringtone
# Default is 0
# Number: 0 - 12
# Mandatory
P26269 = 0

# Matching Incoming Caller ID. Matching Rule 10
# String
P26296 = 

# Matching Rule 10 Distinctive Ringtone
# 0 - System Ringtone, 1 - Custom Ringtone 1, 2 - Custom Ringtone 2, 3 - Custom Ringtone 3
# 6 - Custom Ringtone 4, 7 - Custom Ringtone 5, 8 - Custom Ringtone 6, 9 - Custom Ringtone 7, 10 - Custom Ringtone 8
# 11 - Custom Ringtone 9, 12 - Custom Ringtone 10, 4 - Silent, 5 - Default Ringtone
# Default is 0
# Number: 0 - 12
# Mandatory
P26297 = 0

# Ring Timeout (in seconds). Default is 60
# Number: 30 - 3600
# Mandatory
P576 = 60

###############################################################
# Account 3/Intercom Settings
###############################################################
# Allow Auto Answer by Call-Info/Alert-Info. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P538 = 0

# Mute on answer Intercom call. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P26271 = 0

# Play warning tone for Auto Answer Intercom. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P26272 = 0

# Custom Call-Info for Auto Answer.
# String
P2556 = 

#####################################################
# Account 3/Feature Codes
#####################################################
# Enable Local Call Features.  0 - No, 1 - Yes. Default is 1
# Number: 0, 1
# Mandatory
P520 = 1

# DND Call Feature ON
# String
P2544 =

# DND Call Feature OFF
# String
P2545 =

# Call Forward Unconditionally (All) ON
# String
P26213 =

# Call Forward Unconditionally (All) - OFF
# String
P26214 =

# Call Forward Busy - ON
# String
P26209 =

# Call Forward Busy - OFF
# String
P26210 =

# Call Forward Delayed (No Answer) - ON
# String
P26211 =

# Call Forward Delayed (No Answer) - OFF
# String
P26212 =

# Delayed Call Forward Wait Time
# Number: 1 - 120. Default is 20.
# Mandatory
P570 = 20

##############################################################################
## Network/Basic Settings                                                   ##
##############################################################################

# Internet Protocol. 0 - Both, Prefer IPv4, 1 - Both, Prefer IPv6, 2 - IPv4 Only, 3 - IPv6 Only. Default is 0
# Number: 0, 1, 2, 3
# Mandatory
P1415 = 0

# IP Address Mode. 0 - DHCP, 1 - Static IP, 2 - PPPoE. Default is 0
# Number: 0, 1, 2
# Mandatory
P8 = 0

##########################################
# DHCP
##########################################
# Host name, DHCP option 12. Max length allowed is 64 characters
# String
P146 =

# Vendor Class ID, DHCP option 60. Max length allowed is 64 characters
# Default value for GXP1610 - Grandstream GXP1610
# Default value for GXP1620 - Grandstream GXP1620
# Default value for GXP1625 - Grandstream GXP1625
# Default value for GXP1625 - Grandstream GXP1628
# Default value for GXP1625 - Grandstream GXP1630
# String
# Cannot be empty
# P148 =  

##########################################
# PPPoE
##########################################
# PPPoE Account ID
# String
P82 =

# PPPoE Password
# String
# Cannot contain ` or "
P83 =

# PPPoE Service Name
# String 
P269 =

##########################################
# Statically Configured
##########################################
# IP Address. Ignore if DHCP or PPPoE is used
# Number: 0 - 255
P9 = 192

# Number: 0 - 255
P10 = 168

# Number: 0 - 255
P11 = 0

# Number: 0 - 255
P12 = 160

# Subnet mask. Ignore if DHCP or PPPoE is used
# Number: 0 - 255
P13 = 255

# Number: 0 - 255
P14 = 255

# Number: 0 - 255
P15 = 255

# Number: 0 - 255
P16 = 0

# Gateway. Ignore if DHCP or PPPoE is used
# Number: 0 - 255
P17 = 0

# Number: 0 - 255
P18 = 0

# Number: 0 - 255
P19 = 0

# Number: 0 - 255
P20 = 0

# DNS 1 Server. Ignore if DHCP or PPPoE is used
# Number: 0 - 255
P21 = 0

# Number: 0 - 255
P22 = 0

# Number: 0 - 255
P23 = 0

# Number: 0 - 255
P24 = 0

# DNS 2 Server. Ignore if DHCP or PPPoE is used
# Number: 0 - 255
P25 = 0

# Number: 0 - 255
P26 = 0

# Number: 0 - 255
P27 = 0

# Number: 0 - 255
P28 = 0

# Preferred DNS server.  (if specified).
# Number: 0 - 255
P92 = 0

# Number: 0 - 255
P93 = 0

# Number: 0 - 255
P94 = 0

# Number: 0 - 255
P95 = 0

# IPv6 Address type. 0 - Auto Configured, 1 - Statically Configured. Default is 0.
# Number: 0, 1
# Mandatory
P1419 = 0

# IPv6 Address type: Statically configured. 0 - Full Static, 1 - Prefix Static
# Number: 0, 1
P1426 = 0

# Full Static: Static IPv6 Address
P1420 =

# Full Static: IPv6 Prefix Length
P1421 =

# Prefix Static: IPv6 Prefix (64bits)
P1422 =

# DNS Server 1 for IPv6 Address
# String: a-z, A-Z, 0-9, ".", ":", "[", "]"
P1424 =

# DNS Server 2 for IPv6 Address
# String: a-z, A-Z, 0-9, ".", ":", "[", "]"
P1425 =

# Preferred DNS Server for IPv6 Address
# String: a-z, A-Z, 0-9, ".", ":", "[", "]"
P1423 =

##############################################################################
## Network/Advanced Settings
##############################################################################
# 802.1X Mode. 0 - disable, 1 - EAP-MD5, 2 - EAP-TLS, 3 - EAP-PEAPv0/MSCHAPv2. Default is 0
# Number: 0, 1, 2, 3
# Mandatory
P7901 = 0

# 802.1X Identity. Max length allowed is 64 characters
# String
P7902 = 

# MD5 Password. Max length allowed is 64 characters
# String
P7903 =

# HTTP Proxy
# String
P1552 =

# HTTPS Proxy
# String
P1553 =

# Layer 3 QoS for SIP. Default is 26
# Number: 0 - 63
# Mandatory
P1558 = 26

# Layer 3 QoS for RTP. Default is 46
# Number: 0 - 63
# Mandatory
P1559 = 46

# Enable DHCP VLAN, 0 - Disable, 1 - Enable. Default is 0
# Number: 0, 1
# Mandatory
P8300 = 0

# Enable Manual VLAN Configuration. 0 - Disable, 1 - Enable. Default is 1
# Number: 0, 1
# Mandatory
P22174 = 1

# Layer 2 QoS. 802.1Q/VLAN Tag (VLAN classification for RTP). Default is 0
# Number: 0 - 4094
# Mandatory
P51 = 0

# Layer 2 QoS. 802.1p priority value (0 - 7). Default is 0
# Number: 0 - 7
# Mandatory
P87 = 0

# PC Port Mode. 0 - Enable, 1 - Disabled, 2 - Mirrored. Default is 0
# Number: 0, 1, 2
# Mandatory
P1348 = 0

# PC Port VLAN Tag. Default is 0
# Mandatory
P229 = 0

# PC Port Priority Value. Default is 0
# Mandatory
P230 = 0

# Enable CDP.   0 - Disabled, 1 - Enabled. Default is 0
# Number: 0, 1
# Mandatory
P22119 = 0

# Enable LLDP.  0 - Disabled, 1 - Enabled. Default is 1
# Number: 0, 1
# Mandatory
P1684 = 1

# Maximum Transmission Unit (MTU) in bytes, default is 1500 bytes
# Number
# Mandatory
P244 = 1500

##############################################################################
##  Network/Remote Control
##############################################################################
# CSTA Control. 0 - Disabled, 1 - Enabled
# Number: 0, 1. Default is 0
# Mandatory
P32053 = 0

##############################################################################
## Network/OpenVPN Settings
##############################################################################
# OpenVPN Enable. 0 - No, 1 - Yes, default is 0
# Number
# Mandatory
P7050 = 0

# OpenVPN Server Address
# String
P7051 = 

# OpenVPN Port. Default is 1194
# Number
# Mandatory
P7052 = 1194

# OpenVPN Transport.  0 - UDP, 1 - TCP Default is 0
# Number: 0, 1 
# Mandatory
P2912 = 0

# OpenVPN CA
# String
P9902 = 

# OpenVPN Certificate
# String
P9903 = 

# OpenVPN Client Key
# String
P9904 = 

# OpenVPN Cipher Method
# Number: 0 - Blowfish, 1 - AES-128, 2 - AES-256, 3 - Triple-DES. Default is 0.  
P8396 = 0

# OpenVPN Username
# String
P8394 =

# OpenVPN Password
# String
P8395 =

# OpenVPN Comp-lzo. 0 - No, 1 - Yes. Default is 1
# Number: 0, 1
# Mandatory
P8508 = 1

# Additional Options
# String
P8460 =

#####################################################
# Network/SNMP Settings
#####################################################
# Enable SNMP
# Number: 0 - No, 1 - Yes. Default is 0.
# Mandatory
P21896 = 0

# Version. 1 - Version 1, 2 - Version 2, 3 - Version 3. Default is 3
# Number: 1, 2, 3
# Mandatory
P21904 = 3

# Port
# Number
P21903 = 161

# SNMP Trap IP
# String
P21897 =

# SNMP Trap Port
# Number: 1025 - 65535. Default is 162.
# Mandatory
P21898 = 162

# SNMP Trap Interval
# Number: 1 - 1440. Default is 5.
# Mandatory
P21901 = 5

# SNMP Trap Version
# Number: 1 - Version 1, 2 - Version 2, 3 - Version 3. Default is 2
# Mandatory
P21899 = 2

# Community
# String
P21902 =

# SNMP Trap Community
# String
P21900 =

# SNMP Username
# String
P21905 =

# Security Level. 0 - noAuthUser, 1 - authUser, 2 - privUser. Default is 0
# Number: 0, 1, 2
# Mandatory
P21910 = 0

# Authentication Protocol. 0 - None, 1 - MD5, 2 - SHA. Default is 0
# Number: 0, 1, 2
# Mandatory
P21906 = 0

# Privacy Protocol. 0 - None, 1 - DES, 2 - AES. Default is 0
# Number: 0, 1, 2
# Mandatory
P21907 = 0

# Authentication Key
# String
P21908 =

# Private Key
# String
P21909 =

# SNMP Trap Username
# String
P21911 =

# Trap Security Level. 0 - noAuthUser, 1 - authUser, 2 - privUser. Default is 0
# Number: 0, 1, 2
# Mandatory
P21916 = 0

# Trap Authentication Protocol. 0 - None, 1 - MD5, 2 - SHA. Default is 0
# Number: 0, 1, 2
# Mandatory
P21912 = 0

# Trap Privacy Protocol. 0 - None, 1 - DES, 2 - AES. Default is 0
# Number: 0, 1, 2
# Mandatory
P21913 = 0

# Trap Authentication Key
# String
P21914 =

# Trap Private Key
# String
P21915 =

##############################################################################
##  Maintenance/ Web Access
##############################################################################
# New User Password
# String: a-z, A-Z, 0-9
# P196 =

# New Admin password for web interface
# String: a-z, A-Z, 0-9
# P2 = 

##############################################################################
##  Maintenance/Upgrade and Provisioning
##############################################################################
# Firmware Upgrade and Provisioning
# 0 - Always Check For New Firmware
# 1 - Check New Firmware only when F/W pre/suffix changes
# 2 - Always Skip the Firmware Check
# Number: 0, 1, 2
# Mandatory
P238 = 0

# Always Authenticate Before Challenge. 0 - No,  1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P20713 = 0

# Validate Hostname in Certificate. 0 - No,  1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P22030 = 0

# Allow DHCP Option 43 and Option 66 to override server. 0 - No, 1 - Yes. Default is 1
# When set to Yes(1), it will override the configured provision path and method
# Number: 0, 1
# Mandatory
P145 = 1

# Additional Override DHCP option
# 0 - None, 1 - Option 150, 2 - Option 160
# Number: 0, 1, 2
# Mandatory
P8337 = 0

# Allow DHCP Option 120 to Override SIP Server
# 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P1411 = 0

# 3CX Auto Provision. 0 - No, 1 - Yes. Default is 1
# Number: 0, 1
# Mandatory
P1414 = 1

# Automatic Upgrade
# 0 - No, 
# 1 - Yes, check for upgrade based on minute(s) setting,
# 2 - Yes, check for upgrade based on Hour of Day setting,
# 3 - Yes, check for upgrade based on Day of Week setting,
# Default is No.
# Number: 0, 1, 2, 3
# Mandatory
P194 = 0

# Randomized Automatic Upgrade. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P8458 = 0

# Check for new firmware every () minutes. Default is 7 days.
# Number: 60-86400
# Mandatory
P193 = 10080

# Hour of the Day (0-23). Default is 1
# Number: 0 - 23
# Mandatory
P285 = 1

# Day of the Week (0-6). Default is 1
# Number: 0-6
# Mandatory
P286 = 1

# Disable SIP NOTIFY Authentication. 0 -No, 1 - Yes. Default is 0.
# Number: 0, 1
# Mandatory
P4428 = 0

# Firmware Upgrade Confirmation. 0 - No, 1 - Yes. Default is 1.
# Number: 0, 1
# Mandatory
P8375 = 1

# Config Upgrade Via. 0 - TFTP,  1 - HTTP, 2 - HTTPS, 3 - FTP, 4 - FTPS. Default is 1
# Number: 0, 1, 2, 3, 4
# Mandatory
P212 = 1

# Config Server Path
# String
P237 = fm.grandstream.com/gs

# Config HTTP/HTTPS User Name
# String
P1360 =

# Config HTTP/HTTPS Password
# String
P1361 =

# Config File Prefix
# String
P234 =

# Config File Postfix
# String
P235 =

# XML Config File Password
# String
P1359 =

# Authenticate Conf File. 0 - No, 1 - Yes. Default is No
# Number: 0, 1
# Mandatory
P240 = 0

# Firmware Upgrade Via. 0 - TFTP,  1 - HTTP, 2 - HTTPS, 3 - FTP, 4 - FTPS. Default is 1
# Number: 0, 1, 2, 3, 4
# Mandatory
P6767 = 1

# Firmware Server Path
# String
P192 = fm.grandstream.com/gs

# Firmware HTTP/HTTPS User Name
# String
P6768 =

# Firmware HTTP/HTTPS Password
# String
P6769 =

# Firmware File Prefix
# String
P232 =

# Firmware File Postfix
# String
P233 =

##############################################################################
##  Maintenance/Syslog
##############################################################################
# Syslog Protocol
# 0 - UDP, 1 - SSL/TLS. Default is 0
# Number: 0, 1
# Mandatory
P8402 = 0

# Syslog Server (name of the server, max length is 64 characters)
# String
P207 =

# Syslog Level. 0 - NONE, 1 - DEBUG, 2 - INFO, 3 - WARNING, 4 - ERROR. Default is 0
# Number: 0, 1 , 2, 3, 4
# Mandatory
P208 = 0

# Syslog Keyword Filtering
# String
P22129 = 

# Send SIP Log. 0 - Do not send SIP log in Syslog, 1 - Send SIP log in Syslog if configured and set to DEBUG level. Default is 0
# Number: 0, 1
# Mandatory
P1387 = 0

##############################################################################
##  Maintenance/Language
##############################################################################
# Display Language. Default is auto
# ar - Arabic, cs - Czech, de - Deutsh
# en - English, es - Spanish, fr - Francais
# he - Hebrew, hr - Hrvatski, hu - Magyar 
# it - Italiano, ja - japanese, ko - korean
# lv - Latvian, nl - Dutch, pl - Polski, pt - Portugue
# ru - Russian, sl - Slovenian, se - Svenska
# tr - Turkish, zh-tw - traditional chinese, 
# zh - simplified chinese, auto - Automatic
# gxp - Downloaded Language
# String
# Mandatory
P1362 = auto

# Language File postfix (for Downloaded Language)
# String
P399 =

##############################################################################
##  Maintenance/Action URL
##############################################################################
# Setup Completed
# String
P8304 = 

# Registered
# String
P8305 = 

# Unregistered 
# String
P8306 = 

# Register Failed
# String
P8307 =

# Off Hook
# String 
P8308 = 

# On Hook 
# String 
P8309 = 

# Incoming Call
# String
P8310 = 

# Outgoing Call
# String
P8311 = 

# Missed Call
# String 
P8312 = 

# Answered Call
# String
P22171 =

# Rejected Call
# String
P8315 =

# Forwarded Call
# String
P22172 =

# Established Call
# String
P8313 = 

# Terminated Call
# String
P8314 = 

# Open DND
# String
P8316 = 

# Close DND
# String 
P8317 = 

# Open Forward
# String
P8318 = 

# Close Forward 
# String
P8319 = 

# Open Unconditional Forward
# String
P22164 = 

# Close Unconditional Forward
# String
P22165 = 

# Open Busy Forward
# String
P22166 = 

# Close Busy Forward
# String
P22167 = 

# Open No Answer Forward
# String
P22168 = 

# Close No Answer Forward
# String
P22169 = 

# Blind Transfer
# String
P8320 = 

# Attended Transfer
# String
P8321 = 

# Hold Call
# String
P8324 = 

# Unhold Call
# String
P8325 = 

# Open Syslog
# String
P8330 = 

# Close Syslog
# String
P8331 = 

# IP Change
# String
P22170 =

# Auto-Provision Finish
# String
P8332 =

##############################################################################
##  Maintenance/TR-069
##############################################################################
# ACS URL
# String
P4503 =

# TR-069 Username
# String
P4504 =

# TR-069 Password
# String
P4505 =

# Periodic Inform Enable. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P4506 = 0

# Periodic Inform Interval
# Number
P4507 = 86400

# Connection Request Username	
# String: a-z, A-Z, 0-9
P4511 =

# Connection Request Password	
# String: a-z, A-Z, 0-9
P4512 =

# Connection Request Port
# Number
P4518 = 7547

# CPE SSL Certificate
# String: a-z, A-Z, 0-9
P8220 =

# CPE SSL Private Key
# String: a-z, A-Z, 0-9
P8221 =

# Randomized TR069 Startup. 0 - Disabled, 1 - Enabled. Default is 0
# Number: 0, 1
# Mandatory
P8487 = 0

##########################################
##  Maintenance/Security Settings/Security
##########################################
# Configuration Via Keypad Menu. 0 - Unrestricted, 1 - Basic settings only, 2 - Constraint mode, 3 - Locked mode. Default is 0
# Number: 0, 1, 2, 3
# Mandatory
P1357 = 0

# Enable STAR key Keypad locking. 0 - No, 1 - Yes. Default is 1
# Number: 0, 1
# Mandatory
P1382 = 0

# Keypad Lock Type. 0 - Full, 1 - Functional. Default is 0
# Number: 0, 1
# Mandatory
P8383 = 0

# Password to lock/unlock (0-9 only)
# Number
P1383 =

# Emergency Numbers
# String
P8385 = 

# Keypad Lock Timer
# Number: 0 - 3600
P8384 = 

# Validate Server Certificates. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P8463 = 0

# SIP TLS Certificate
# String: a-z, A-Z, 0-9
#P280 =

# SIP TLS Private Key
# String: a-z, A-Z, 0-9
#P279 =

# SIP TLS Private Key Password
# String: a-z, A-Z, 0-9
P281 = s1pphone

# Web Access Mode. 0 - HTTPS, 1 - HTTP, 2 - Disabled. Default is 1
# Number: 0, 1, 2
# Mandatory
P1650 = 1

# Enable User Web Access. 0 - Disabled, 1 - Enabled. Default is 1
# Number: 0, 1
# Mandatory
P8469 = 1

# HTTP Web Port. Default is 80
# Number: 60 - 65535
# Mandatory
P22120 = 80

# HTTPS Web Port. Default is 443
# Number: 60 - 65535
# Mandatory
P22121 = 443

# Disable SSH. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
P276 = 0

# Web/Keypad/Restrict mode Lockout Duration (0-60 minutes). Default is 5
# Number: 0-60
P1683 = 5

# Web Session Timeout. Default is 10.
# Number: 2-60
# Mandatory
P28116 = 10

# Web Access Attempt Limit. Default is 5.
# Number: 1-10
# Mandatory
P28117 = 5

# Minimum TLS Version. 10 - TLS 1.0, 11 - TLS 1.1, 12 - TLS 1.2. Default is 11.
# Number: 10, 11, 12
# Mandatory
P22293 = 11

# Maximum TLS Version. 99 - Unlimited, 10 - TLS 1.0, 11 - TLS 1.1, 12 - TLS 1.2. Default is 99
# Number: 99, 10, 11, 12
# Mandatory
P22294 = 99

# Enable/Disable Weak Ciphers. Default is 0
# 0 - Enable Weak TLS Ciphers Suites
# 1 - Disable Symmetric Encryption RC4/DES/3DES
# 2 - Disable Symmetric Encryption SEED
# 3 - Disable All Weak Symmetric Encryption
# 4 - Disable Symmetric Authentication MD5
# 5 - Disable All Weak TLS Cipher Suites
# Number: 0 - 5
P8536 = 0

########################################################
##  Maintenance/Security Settings/Trusted CA Certificate
########################################################
# Trusted CA Certificate
# String
P8433 =
P8434 =
P8435 =
P8436 =
P8437 =
P8438 = 

# Load CA Certificates. 0 - Default Certificates, 1 - Custom Certificates, 2- All Certificates. Default is 2
# Number: 0, 1, 2
P8502 = 2

##############################################################################
##  Phonebook/Phonebook Management
##############################################################################
# Enable Phonebook XML Download. # 0 - No, 1 - YES, HTTP, 2 - YES, TFTP, 3 - Yes, HTTPS. Default is 0
# Number: 0, 1, 2, 3
# Mandatory
P330 = 0

# HTTP/HTTPS User name
# String
P6713 =

# HTTP/HTTPS Password
# String
P6714 =

# Phonebook XML Server Path
# This is a string of up to 256 characters that should contain a path to the XML file. It MUST be in the host/path format.
# For example: directory.grandstream.com/engineering
# String
P331 =

# Phonebook Download Interval (in minutes)
# Valid value range is 5-720. Default is 0 for disabled
# Number: 0, 5-720; 
P332 = 0

# Remove Manually-edited entries on Download. 0 - No, 1 - Yes. Default is 1
# Number: 0, 1
# Mandatory
P333 = 1

# Import Group Method. 0 - Replace, 1 - Append. Default is 0
# Number: 0, 1
# Mandatory
P8462 = 0

# Sort Phonebook by. 0 - Last Name. 1 - First Name. Default is 0
# Number: 0, 1
# Mandatory 
P2914 = 0

# Phonebook Key Function. 0 - Default, 1 - LDAP Search, 2 - Local Phonebook, 3 - Local Group, 4 - Broadsoft Phonebook.
# Number: 0, 1, 2, 3, 4.
# Mandatory
P1526 = 0

##############################################################################
##  Phonebook/LDAP
##############################################################################
# LDAP Directory
# LDAP Protocol. 0 - LDAP, 1 - LDAPS. Default is 0.
# Number: 0, 1
P8370 = 0

# LDAP Server Address, up to 256 characters can be used. It can be IP address or Domain name
# String
P8020 = 

# LDAP Server Port. Default is 389.
# Number: 1 - 65535
P8021 = 389

# Base. The LDAP search base refers to the location in the directory where the search is requested to begin
# Example 1: dc=grandstream,dc=com
# value i 2: ou=Boston, dc=grandstream,dc=com
# String
P8022 =

# User name. The bind "Username" for querying LDAP servers. Some LDAP servers allow anonymous binds in which case the setting can be left blank
# String
P8023 =

# Password. The bind "Password" for querying LDAP servers. And the field can be left blank if the LDAP server allows anonymous binds
# String
P8024 =

# LDAP Number Filter
# LDAP name filter is the filter used for name look ups. Please refer to usermanual for examples
# String
P8025 =

# LDAP Name Filter
# LDAP name filter is the filter used for name look ups. Please refer to usermanual for examples
# String
P8026 =

# LDAP Version. Protocol version for the phone when send the bind requests
# 2 - version 2, 3 - version 3. Default is 3
# Mandatory
P8027 = 3

# LDAP Name Attributes. This setting specifies the "name" attributes of each record which are returned in the LDAP search result
# The setting allows the users to configure multiple space separated name attributes
# String
P8028 =

# LDAP Number Attributes. This setting specifies the “number” attributes of each record which are returned in the LDAP search result
# The setting allows the users to configure multiple space separated number attributes
# String
P8029 =

# LDAP Display Name. The entry information to be shown on phone LCD. Grandstream phones will display up to 3 fields
# String
P8030 =

# Max Hits. The setting specifies the maximum number of results to be returned by the LDAP server
# If the value is set to 0, server will return all search results. Default is 50
# Number: 0 - 32000
# Mandatory
P8031 = 50

# Search Timeout (in seconds). Default is 30
# The setting specifies how long the server should process the request and client waits for server to return
# Number: 0 - 180
# Mandatory
P8032 = 30

# Sort Results. This setting is used for sorting searching result. 0 - no, 1 - yes. Default is 0
# Number: 0, 1
# Mandatory
P8033 = 0

# LDAP Lookup
# Incoming calls. 0 - No, 1 - Yes. Default is 0
P8035 = 0

# Outgoing calls. 0 - No, 1 - Yes. Default is 0
P8034 = 0

# Lookup Display Name
# String
P8036 =

##############################################################################
##  Settings/General Settings
##############################################################################
# Local RTP port. Default is 5004
# Number: 1024 - 65535. Must be even number
# Mandatory
P39 = 5004

# Local RTP port range
# Number: 48 - 10000. Default is 200.
P29610 = 200

# Use Random Port. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P78 = 0

# Keep-alive interval (in seconds). Default is 20
# Number: 10 - 160
# Mandatory
P84 = 20

# Use NAT IP. This will enable our SIP client to use this IP in the SIP/SDP message. Example 64.3.153.50
# String: a-z, A-Z, 0-9, ".", ":"
P101 =

# STUN server
# String
P76 =

# Public Mode. 0 - No. 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P1345 = 0

# Enable Fix For RTP Timestamp Jump
# Number: 0 - No, 1 - Yes. Default is 0. 
P8389 = 0

# Test Password Strength. Default is 0.
# Number: 0, 1. 0 - No, 1 - Yes. 
P8468 = 0

# DNS Cache Refresh Time, in minutes. Default is 30
# Number: 5 - 1440
P4208 =

##############################################################################
##  Settings/Call Features
##############################################################################
# Onhook Dial Barging. Default is 1
# Number: 0 - Disabled, 1 - Enabled.
# Mandatory
P8397 = 1

# Off-hook Auto Dial
# String
P71 =

# Off-hook Auto Dial Delay
# Number: 0 - 30
# Mandatory
P8388 = 0

# Off-hook timeout (in seconds). Default is 30
# Number: 10 - 60
# Mandatory
P1485 = 30

# Enable Live DialPad.
# Number: 0 - No, 1 - Yes. Default is 0.
# Mandatory
P8350 = 0

# Live DialPad Expire Time
# Number: 2 - 15. Default is 5.
# Mandatory
P8351 = 5

# Busy Tone Expiration
# Number: 0 - 60. Default is 30.
P8443 = 30

# Enable Automatic Redial
# Number: 0 - No, 1 - Yes. Default is 0.
# Mandatory
P8353 = 0

# Automatic Redial Times
# Number: 1 - 100. Default is 10.
# Mandatory
P8354 = 10

# Automatic Redial Interval
# Number: 1 - 360. Default is 20.
# Mandatory
P8355 = 20

# Intercom Key Mode. 0 - Intercom, 1 - Multicast Paging. Default is 0.
# Number: 0, 1
# Mandatory
P22123 = 0

# Intercom User ID
# String
P1303 =

# Intercom Multicast Paging Address
# String
P22124 = 

# Intercom Multicast Paging Label
# String
P22125 = 

# Bypass Dial Plan Through Call History and Directories
# Number: 0,1. Default is 0
# Mandatory
P6758 = 0

# Disable Call Waiting. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P91 = 0

# Disable Call-Waiting Tone. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P186 = 0

# Ring For Call Waiting
# Number: 0 - No, 1 - Yes. Default is 0.
# Mandatory
P22102 = 0

# Disable Busy Tone on Remote Disconnect. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P6762 = 0

# Disable Direct IP Call. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P1310 = 0

# Use Quick IP Call mode. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P184 = 0

# Disable Conference. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P1311 = 0

# Disable in-call DTMF Display. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P338 = 0

# Enable Sending DTMF via Specific MPKs. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P1339 = 0

# Mute Key Functions While Idle. 0 - DND, 1 - Idle Mute, 2 - Disabled. Default is 0
# Number: 0, 1, 2
# Mandatory
P1565 = 0

# Disable Transfer. 0 - No, 1 - Yes. Defauls is 0
# Number: 0, 1
# Mandatory
P1341 = 0

# In-call Dial Number on pressing transfer key
# String
P1525 =

# Attended Transfer Mode
# Number: 0 - Static, 1 - Dynamic. Default is 0.
# Mandatory
P1376 =

# Do not escape '#' as 23% in SIP URL. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P1406 = 0

# Use Pound # For Redial. 0 - No, 1 - Yes. Default is 1
# Number: 0, 1
# Mandatory
P8504 = 1

# Click-To-Dial Feature. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P1561 = 0

# Call History Flash Writing: 0 means this option is disabled
# Write Timeout, 30-3600, in seconds, default is 300
# Number: 30 - 3600
# Mandatory
P1433 = 300

# Max Unsaved Log, 0-500, default is 200
# Number: 0-500
# Mandatory
P1434 = 200

# User-Agent Prefix
# String
P8358 = 

# Predictive Dialing Feature. 0 - disabled, 1 - enabled. Default is 1
# Number: 0, 1
# Mandatory
P22126 = 1

# Disable Hook Switch
# Number: 0 - No, 1 - Yes, 2 - For Answering Call. Default is 0.
# Mandatory
P6763 = 0

# Show SIP Error Response. 0 - No, 1 - Yes. Default is 1.
# Number: 0, 1
# Mandatory
P8376 = 1

# Auto Answer Delay. Default is 0.
# Number: 0 - 4.
# Mandatory
P8486 = 0

# Enable Enhanced Acoustic Echo Canceller. 0 - No, 1 - Yes. Default is 1
# Number: 0, 1
# Mandatory
P22175 = 1

# Show On Hold Duration. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P8503 = 0

# Hide/Disable Reject Key. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P8511 = 0

# Enable Diversion Information Display. 0 - No, 1 - Yes. Default is 1
# Number: 0, 1
# Mandatory
P22237 = 1

####################################################################
# Blink message LED on ringing - GXP1610 only
####################################################################
# Blink message LED on ringing. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P1696 = 0
####################################################################

##############################################################################
##  Settings/Multicast Paging
##############################################################################
# Paging Barge. 0 - Disable, 1 - priority 1, 2 - priority 2, 3 - priority 3, 
# 4 - priority 4, 5 - priority 5, 6 - priority 6, 7 - priority 7, 8 - priority 8,
# 9 - priority 9, 10 - priority 10. Default is 0.
# Number: 0 - 10
# Mandatory
P1566 = 0

# Paging Priority Active. 0 - Disabled, 1 - Enabled
# Number: 0, 1
# Mandatory
P1567 = 0

# Multicast Paging Codec. 0 - PCMU, 2 - G.726-32, 4 - G.723.1, 8 - PCMA, 9 - G.722, 18 - G.729A/B
# Number: 0, 2, 4, 8, 9, 18
# Mandatory
P1568 = 0

# Multicast Channel Number. 0 - 50. Default is 0
# Number
# Mandatory
P8454 = 0

# Multicast Sender ID
# String
P8455 =

### Multicast Listening ### 
# Priority 1
# Listening Address
# String
P1569 = 

# Label
# String
P1570 = 

# Priority 2
# Listening Address
# String
P1571 = 

# Label
# String
P1572 = 

# Priority 3
# Listening Address
# String
P1573 = 

# Label
# String
P1574 = 

# Priority 4
# Listening Address
# String
P1575 = 

# Label
# String
P1576 = 

# Priority 5
# Listening Address
# String
P1577 = 

# Label
# String
P1578 = 

# Priority 6
# Listening Address
# String
P1579 = 

# Label
# String
P1580 = 

# Priority 7
# Listening Address
# String
P1581 = 

# Label
# String
P1582 = 

# Priority 8
# Listening Address
# String
P1583 = 

# Label
# String
P1584 = 

# Priority 9
# Listening Address
# String
P1585 = 

# Label
# String
P1586 = 

# Priority 10
# Listening Address
# String
P1587 = 

# Label
# String
P1588 = 

##############################################################################
##  Settings/Preferences/Audio Control
##############################################################################
# HEADSET Key Mode. 0 = Default Mode, 1 = Toggle Headset/Speaker. Default is 0
# Number: 0, 1
# Mandatory
P1312 = 0

# Headset Type. 0 - Normal, 1 - Plantronics EHS. Default is 0
# Number: 0, 1
# Mandatory
P1487 = 0

# Always Ring Speaker. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P1439 = 0

# Enable Group Listening. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P22100 = 0

# Grouop Listen with Speaker. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P22163 = 0

# Headset TX gain(db). 1 - -6, 0 - 0, 2 - +6. Default is 0
# Number: 0, 1, 2
# Mandatory
P1301 = 0

# Headset RX gain(db). 1 - -6, 0 - 0, 2 - +6. Default is 0
# Number: 0, 1, 2
# Mandatory
P1302 = 0

# Handset TX gain(db). 1 - -6, 0 - 0, 2 - +6. Default is 0
# Number: 0, 1, 2
# Mandatory
P1464 = 0

##############################################################################
##  Settings/Preferences/Date and Time
##############################################################################
# NTP Server
# String
P30 = pool.ntp.org

# Allow DHCP Option 42 to override NTP server. 0 - No, 1 - Yes. Default is 1
# When set to Yes(1), it will override the configured NTP server
# Number: 0, 1
# Mandatory
P144 = 1

# Time Zone
# Web GUI Option										P Value
# Automatic												auto
# GMT-12:00 (International Date Line West)				TZA+12
# GMT-11:00 (Midway Island, Samoa) 						TZB+11
# GMT-10:00 (US Hawaiian Time) 							HAW10
# GMT-9:00 (US Alaska Time) 							AKST9AKDT
# GMT-8:00 (US Pacific Time, Los Angeles)				PST8PDT
# GMT-08:00 (Baja California)							PST8PDT,M3.2.0,M11.1.0
# GMT-07:00 (US Mountain Time, Denver) 					MST7MDT
# GMT-07:00 (Mountain Time (Arizona, no DST)) 			MST7
# GMT-07:00 (Chihuahua, La Paz, Mazatlan)				MST7MDT,M4.1.0,M10.5.0  
# GMT-06:00 (Central Time) 								CST6CDT
# GMT-06:00 (Central America) 							CST+6
# GMT-06:00 (Guadalajara, Mexico City, Monterrey)		CST6CDT,M4.1.0,M10.5.0
# GMT-05:00 (Eastern Time)								EST5EDT
# GMT-05:00 (Eastern Time without daylight saving) 		EST5
# GMT-04:30 (Caracas) 									TZf+4:30
# GMT-04:00 (Atlantic Time) 							AST4ADT
# GMT-04:00 (Atlantic Time (New Brunswick)) 			AST4ADT,M3.2.0,M11.1.0
# GMT-03:30 (Newfoundland Time)							NST+3:30NDT+2:30,M3.2.0/00:01:00,M11.1.0/00:01:00
# GMT-03:00 (Greenland) 								TZK+3
# GMT-03:00 (Brazil, Sao Paulo) 						BRST+3BRDT+2,M10.3.0,M2.3.0
# GMT-02:00 (Argentina) 								UTC+3 
# GMT-02:00 (Mid-Atlantic) 								TZL+2
# GMT-01:00 (Azores, Cape Verdi Is.) 					TZM+1
# GMT (Edinburgh, Casablanca, Monrovia) 				TZN+0
# GMT (London, Great Britain) 							GMT+0BST-1,M3.5.0/01:00:00,M10.5.0/02:00:00
# GMT (Lisbon, Portugal) 								WET-0WEST-1,M3.5.0/01:00:00,M10.5.0/02:00:00
# GMT (Dublin, Ireland) 								GMT+0IST-1,M3.5.0/01:00:00,M10.5.0/02:00:00
# GMT+01:00 (Paris, Vienna, Warsaw, Roma, Madrid, Prague, Berlin, Budapest, Amsterdam, Belgium)   CET-1CEST-2,M3.5.0/02:00:00,M10.5.0/03:00:00
# GMT+02:00 (Israel, Cairo, Athens, Istanbul, Buchrest) TZP-2
# GMT+02:00 (Helsinki, Athens, Tallinn) 				EET-2EEST-3,M3.5.0/03:00:00,M10.5.0/04:00:00
# GMT+02:00 (Kyiv, Ukraine) 							EET-2EEST,M3.5.0/3,M10.5.0/4 
# GMT+03:00 (Kuwait, Baghdad, Tehran, Nairobi) 			TZQ-3
# GMT+03:00 (Moscow, Russia) 							MSK-3MSD,M3.5.0/2,M10.5.0/3
# GMT+03:00 (St.Petersburg, Russia) 					MST-3MDT,M3.5.0/2,M10.5.0/3
# GMT+04:00 (Abu Dhabi, Baku) 							TZR-4
# GMT+05:00 (Islamabad, Ekaterinburg, Karachi, Tashkent)TZS-5
# GMT+05:30 (Chennai, New Delhi, Mumbai) 				TZT-5:30
# GMT+05:45 (Kathmandu) 								TZU-5:45
# GMT+06:00 (Almaty, Astana, Dhaka, Novosibirsk) 		TZV-6
# GMT+06:30 (Rangoon) 									TZW-6:30
# GMT+07:00 (Bankok, Hanoi, Krasnoyarsk) 				TZX-7
# GMT+07:00 (Jakarta) 									WIB-7
# GMT+08:00 (Beijing, Taipei, Kuala Lumpur, Irkutsk) 	TZY-8
# GMT+08:00 (Singapore) 								SGT-8
# GMT+08:00 (Ulaanbaatar, Mongolia) 					ULAT-8
# GMT+08:00 (Perth) 									WST-8
# GMT+09:00 (Japan, Korea, Yakutsk) 					TZZ-9
# GMT+09:30 (Adelaide) 									CST-9:30CDT-10:30,M10.5.0/02:00:00,M3.5.0/03:00:00
# GMT+09:30 (Darwin) 									CST-9:30 
# GMT+10:00 (Guam) 										TZb-10
# GMT+10:00 (Hobart) 									EST-10EDT-11,M10.1.0/02:00:00,M3.5.0/03:00:00
# GMT+10:00 (Sydney, Melbourne, Canberra) 				EST-10EDT-11,M10.5.0/02:00:00,M3.5.0/03:00:00
# GMT+10:00 (Brisbane) 									EST-10
# GMT+11:00 (Magadan, Solomon Is., New Caledonia) 		TZc-11
# GMT+12:00 (Auckland, Wellington) 						NZST-12NZDT-13,M10.1.0/02:00:00,M3.3.0/03:00:00
# GMT+12:00 (Fiji) 										TZd-12
# GMT+13:00 (Nuku'alofa) 								TZe-13
# Self-Defined Time Zone								customize
# String
# Mandatory
P64 = auto

# Allow DHCP Option 2 to override Time Zone setting. 0 - No, 1 - Yes. Default is 1
# When set to Yes(1), it will override the configured Time Zone setting if available 
# Number: 0, 1
# Mandatory
P143 = 1

# Self Defined Time zone. Max length allowed is 64 characters
# String
# Mandatory
P246 = MTZ+6MDT+5,M4.1.0,M11.1.0

# Date Display Format
# 0: yyyy-mm-dd      eg. 2011-10-31
# 1: mm-dd-yyyy      eg. 10-31-2011
# 2: dd-mm-yyyy      eg. 31-10-2011
# 3: dddd, MMMM dd   eg. Monday, October 31
# 4: MMMM dd, dddd   eg. October 31, Monday
# Number: 0, 1, 2, 3, 4
# Mandatory
P102 = 0

# Time Display Format. 0 - 12 Hour, 1 - 24 Hour
# Number: 0, 1
# Mandatory
P122 = 0

##############################################################################
##  Settings/Preferences/LCD Display
##############################################################################
# Backlight Brightness: Active.  Valid range is 0 - 8.  GXP1620/1625/1628/1630 only
# Active. Default is 6.
# Number: 0 - 8
# Mandatory
P334 = 6

# Backlight Brightness: Idle. Valid range is 0 - 8. GXP1620/1625/1628/1630 only
# Default is 2.
# Number: 0 - 8
# Mandatory
P335 = 2

# Active Backlight Timeout. Default is 1
# Number: 1 - 90
# Mandatory
P8356 = 1

# LCD Contrast. Default is 3
# Number: 1 - 5
# Mandatory
P6771 = 3

# Disable Missed Call Backlight. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P351 = 0

# Wide Idle Screen View. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P8346 = 0

# Caller ID Display Mode. 0 - Dynamic, 1 - Static. Default is 0
# Number: 0, 1
# Mandatory
P8473 = 0

#####################################################
# Settings/Preferences/LED control
#####################################################
# Disable VM/MSG power light flash
# Number: 0 - No, 1 - Yes. Default is 0.
# Mandatory
P8371 = 0

##############################################################################
##  Settings/Preferences/Ringtone
##############################################################################
### Call Progress Tones ###
# Syntax: f1=val,f2=val[,c=on1/off1[-on2/off2[-on3/off3]]]; 
# (Frequencies are in Hz and cadence on and off are in 10ms) 

# System Ring Tone
# String
# Mandatory
P345 = f1=440,f2=480,c=200/400;

# Dial Tone
# String
# Mandatory
P343 = f1=350,f2=440;

# Second Dial Tone
# String
P2909 = f1=350,f2=440;

# Message Waiting Tone
# String
# Mandatory
P344 = f1=350,f2=440,c=10/10;

# Ring Back Tone
# String
# Mandatory
P346 = f1=440,f2=480,c=200/400;

# Call-Waiting Tone
# String
# Mandatory
P347 = f1=440,f2=440,c=25/525;

# Call-Waiting Tone Gain. 0 - Low, 1 - Medium, 2 - High. Default is 0
# Number: 0, 1, 2
# Mandatory
P1555 = 0

# Busy Tone
# String
# Mandatory
P348 = f1=480,f2=620,c=50/50;

# Reorder Tone
# String
# Mandatory
P349 = f1=480,f2=620,c=25/25;

# Speaker Ring Volume. Default is 7
# Number: 0 - 7
# Mandatory
P8352 = 7

# Notification Tone Volume
# Number: 0 - 7. Default is 4.
# Mandatory
P8399 = 4

# Lock Speaker Volume
# 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
P8392 = 0

# Default Ringtone
# 0 - System Ringtone, 1 - Custom Ringtone 1, 2 - Custom Ringtone 2, 3 - Custom Ringtone 3, 4 - Silent, 6 - Custom Ringtone 4, 7 - Custom Ringtone 5, 8 - Custom Ringtone 6, 9 - Custom Ringtone 7, 10 - Custom Ringtone 8, 11 - Custom Ringtone 9, 12 - Custom Ringtone 10
# Number: 0, 1, 2, 3, 4, 6, 7, 8, 9, 10, 11, 12. Default is 0
P8398 = 0

# Total Number of Custom Ringtone Update Default is 3
# Number: 1 - 10
P8509 = 3

##############################################################################
##  Settings/Web Service
##############################################################################
# Use Auto Location Service. 0 - No, 1 - Yes. Default is 1
# Number: 0, 1
# Mandatory
P8338 = 1

##############################################################################
##  Settings/XML Applications
##############################################################################
# Idle Screen XML Download
# 0 - disabled, 1 - enabled:HTTP, 2 - enabled:TFTP, 3 - enabled:HTTPS. Default is 0
# Number: 0, 1, 2, 3
# Mandatory
P340 = 0

# Download Screen XML At Boot-up. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P1349 = 0

# Use Custom File Name. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P1343 = 0

# Idle Screen XML Server Path
# This is a string of up to 256 characters that should contain a path to the XML file
# It MUST be in the host/path format. For example: directory.grandstream.com/engineering
# String
P341 =

# Server Path
# String
P337 = 

# Softkey Label
# String
P352 = 

##############################################################################
##  Settings/Programmable Keys/Multi-Purpose Keys Settings
##############################################################################
# Transfer Mode via VPK. 0 - Blind Transfer, 1 - Attended Transfer, 2 - New Call. Default is 0
# Number: 0, 1, 2
# Mandatory
P8390 = 0

# Enable transfer via non-Transfer MPK. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
# Mandatory
P22162 = 0

##############################################################################
##  Settings/Programmable Keys/Programmable Keys
##############################################################################

################################################################################################################################
# Key Mode 14 - Speed dial via active account, for GXP1620/1625/1628/1630 only
# Key Mode 11 - BLF, 12 - Presence Watcher, 13 - Eventlist BLF, 19 - Call Park, 26 - Monitored Call Park, for GXP1628/1630 only
################################################################################################################################

#####################################################################################
# Line Keys
######################################################################################
# Line Key 1
######################################################################################
# Key Mode. Default is 0
# 0 - Line, 1 - Shared Line, 10 - Speed Dial, 11 - BLF, 12 - Presence Watcher, 13 - Eventlist BLF, 14 - Speed Dial via active account
# 15 - Dial DTMF, 16 - Voicemail, 17 - Call Return, 18 - Transfer, 19 - Call Park, 26 - Monitored Call Park, 20 - Intercom 
# 21 - LDAP Search, 23 - Multicast Paging, 27 - GDS OpenDoor, 28 - Provision
# Number: 0, 1, 10-21, 23, 26-28
# Mandatory
P1363 = 0

# Account. 0 - Account 1, 1 - Account 2, 2 - Account 3
# Number: 0, 1, 2
# Mandatory
P1364 = 0

# Description. Max length allowed is 32 characters.
# String
P1465 =

# Value. Max length allowed is 64 characters.
# String
P1466 = 

######################################################################################
# Line Key 2
######################################################################################
# Key Mode. Default is 0
# 0 - Line, 1 - Shared Line, 10 - Speed Dial, 11 - BLF, 12 - Presence Watcher, 13 - Eventlist BLF, 14 - Speed Dial via active account
# 15 - Dial DTMF, 16 - Voicemail, 17 - Call Return, 18 - Transfer, 19 - Call Park, 26 - Monitored Call Park, 20 - Intercom 
# 21 - LDAP Search, 23 - Multicast Paging, 27 - GDS OpenDoor, 28 - Provision
# Number: 0, 1, 10-21, 23, 26-28
# Mandatory
P1365 = 0

# Account. 0 - Account 1, 1 - Account 2, 2 - Account 3
# Number: 0, 1, 2
# Mandatory 
P1366 = 0

# Description. Max length allowed is 32 characters.
# String
P1467 =

# Value. Max length allowed is 64 characters.
# String
P1468 =

######################################################################################
# Line Key 3
######################################################################################
# Key Mode. Default is 0
# 0 - Line, 1 - Shared Line, 10 - Speed Dial, 11 - BLF, 12 - Presence Watcher, 13 - Eventlist BLF, 14 - Speed Dial via active account
# 15 - Dial DTMF, 16 - Voicemail, 17 - Call Return, 18 - Transfer, 19 - Call Park, 26 - Monitored Call Park, 20 - Intercom 
# 21 - LDAP Search, 23 - Multicast Paging, 27 - GDS OpenDoor, 28 - Provision
# Number: 0, 1, 10-21, 23, 26-28
# Mandatory
P1367 = 0

# Account. 0 - Account 1, 1 - Account 2, 2 - Account 3
# Number: 0, 1, 2
# Mandatory 
P1368 = 0

# Description. Max length allowed is 32 characters.
# String
P1469 =

# Value. Max length allowed is 64 characters.
# String
P1470 =

######################################################################################
# Customizable Softkey
######################################################################################
# Softkey 1
# Mode: 0 - Default, 10 - Speed Dial, 14 - Speed Dial via Active Account, 16 - Voice Mail, 17 - Call Return, 20 - Intercom, 21 - LDAP Search. Default is 0.
# Number
# Mandatory
P2987 = 0

# Account: 0 - Account 1, 1 - Account 2, 2 - Account 3. Default is 0
# Number
# Mandatory
P2988 = 0

# Description
# String
P2989 = 

# Value
# String
P2990 = 

####################################################################
# GXP1628/1630 only
####################################################################

######################################################################################
# Multi-Purpose Keys
######################################################################################
# MPK 1
######################################################################################
# Key Mode. Default is 0
# 0 - Speed dial ,1 - Busy Lamp Field, 2 - Presence Watch, 3 - Evenlist BLF,
# 4 - Speed dial via active account, 5 - Dial DTMF, 6 - Voice mail, 7 - Call return
# 8 - Transfer, 9 - Call park, 10 - Intercom, 11 - LDAP search, 13 - Multicast paging
# 16 - Monitored Call Park, 17 - GDS OpenDoor, 18 - Provision
# Number: 0, 1, 2, 3, 4, 5, 6, 7, 8, 9, 10, 11, 13, 16, 17, 18
# Mandatory
P323 = 0

# Account. 0 - Account 1, 1 - Account 2, 2 - Account 3
# Number: 0, 1, 2
# Mandatory 
P301 = 0

# Description 
# String
P302 = 

# Value
# String
P303 = 

######################################################################################
# MPK 2
######################################################################################
# Key Mode. Default is 0
# 0 - Speed dial ,1 - Busy Lamp Field, 2 - Presence Watch, 3 - Evenlist BLF,
# 4 - Speed dial via active account, 5 - Dial DTMF, 6 - Voice mail, 7 - Call return
# 8 - Transfer, 9 - Call park, 10 - Intercom, 11 - LDAP search, 13 - Multicast paging
# 16 - Monitored Call Park, 17 - GDS OpenDoor, 18 - Provision
# Number: 0, 1, 2, 3, 4, 5, 6, 7, 8, 9, 10, 11, 13, 16, 17, 18
P324 = 0

# Account. 0 - Account 1, 1 - Account 2, 2 - Account 3
# Number: 0, 1, 2
# Mandatory 
P304 = 0

# Description 
# String
P305 = 

# Value
# String
P306 = 

######################################################################################
# MPK 3
######################################################################################
# Key Mode. Default is 0
# 0 - Speed dial ,1 - Busy Lamp Field, 2 - Presence Watch, 3 - Evenlist BLF,
# 4 - Speed dial via active account, 5 - Dial DTMF, 6 - Voice mail, 7 - Call return
# 8 - Transfer, 9 - Call park, 10 - Intercom, 11 - LDAP search, 13 - Multicast paging
# 16 - Monitored Call Park, 17 - GDS OpenDoor, 18 - Provision
# Number: 0, 1, 2, 3, 4, 5, 6, 7, 8, 9, 10, 11, 13, 16, 17, 18
P325 = 0

# Account. 0 - Account 1, 1 - Account 2, 2 - Account 3
# Number: 0, 1, 2
# Mandatory 
P307 = 0

# Description 
# String
P308 = 

# Value
# String
P309 = 

######################################################################################
# MPK 4
######################################################################################
# Key Mode. Default is 0
# 0 - Speed dial ,1 - Busy Lamp Field, 2 - Presence Watch, 3 - Evenlist BLF,
# 4 - Speed dial via active account, 5 - Dial DTMF, 6 - Voice mail, 7 - Call return
# 8 - Transfer, 9 - Call park, 10 - Intercom, 11 - LDAP search, 13 - Multicast paging
# 16 - Monitored Call Park, 17 - GDS OpenDoor, 18 - Provision
# Number: 0, 1, 2, 3, 4, 5, 6, 7, 8, 9, 10, 11, 13, 16, 17, 18
P326 = 0

# Account. 0 - Account 1, 1 - Account 2, 2 - Account 3
# Number: 0, 1, 2
# Mandatory 
P310 = 0

# Description 
# String
P311 = 

# Value
# String
P312 = 

######################################################################################
# MPK 5
######################################################################################
# Key Mode. Default is 0
# 0 - Speed dial ,1 - Busy Lamp Field, 2 - Presence Watch, 3 - Evenlist BLF,
# 4 - Speed dial via active account, 5 - Dial DTMF, 6 - Voice mail, 7 - Call return
# 8 - Transfer, 9 - Call park, 10 - Intercom, 11 - LDAP search, 13 - Multicast paging
# 16 - Monitored Call Park, 17 - GDS OpenDoor, 18 - Provision
# Number: 0, 1, 2, 3, 4, 5, 6, 7, 8, 9, 10, 11, 13, 16, 17, 18
P327 = 0

# Account. 0 - Account 1, 1 - Account 2, 2 - Account 3
# Number: 0, 1, 2
# Mandatory 
P313 = 0

# Description 
# String
P314 = 

# Value
# String
P315 = 

######################################################################################
# MPK 6
######################################################################################
# Key Mode. Default is 0
# 0 - Speed dial ,1 - Busy Lamp Field, 2 - Presence Watch, 3 - Evenlist BLF,
# 4 - Speed dial via active account, 5 - Dial DTMF, 6 - Voice mail, 7 - Call return
# 8 - Transfer, 9 - Call park, 10 - Intercom, 11 - LDAP search, 13 - Multicast paging
# 16 - Monitored Call Park, 17 - GDS OpenDoor, 18 - Provision
# Number: 0, 1, 2, 3, 4, 5, 6, 7, 8, 9, 10, 11, 13, 16, 17, 18
P328 = 0

# Account. 0 - Account 1, 1 - Account 2, 2 - Account 3
# Number: 0, 1, 2
# Mandatory 
P316 = 0

# Description 
# String
P317 = 

# Value
# String
P318 = 

######################################################################################
# MPK 7
######################################################################################
# Key Mode. Default is 0
# 0 - Speed dial ,1 - Busy Lamp Field, 2 - Presence Watch, 3 - Evenlist BLF,
# 4 - Speed dial via active account, 5 - Dial DTMF, 6 - Voice mail, 7 - Call return
# 8 - Transfer, 9 - Call park, 10 - Intercom, 11 - LDAP search, 13 - Multicast paging
# 16 - Monitored Call Park, 17 - GDS OpenDoor, 18 - Provision
# Number: 0, 1, 2, 3, 4, 5, 6, 7, 8, 9, 10, 11, 13, 16, 17, 18
P329 = 0

# Account. 0 - Account 1, 1 - Account 2, 2 - Account 3
# Number: 0, 1, 2
# Mandatory 
P319 = 0

# Description 
# String
P320 = 

# Value
# String
P321 = 

######################################################################################
# MPK 8
######################################################################################
# Key Mode. Default is 0
# 0 - Speed dial ,1 - Busy Lamp Field, 2 - Presence Watch, 3 - Evenlist BLF,
# 4 - Speed dial via active account, 5 - Dial DTMF, 6 - Voice mail, 7 - Call return
# 8 - Transfer, 9 - Call park, 10 - Intercom, 11 - LDAP search, 13 - Multicast paging
# 16 - Monitored Call Park, 17 - GDS OpenDoor, 18 - Provision
# Number: 0, 1, 2, 3, 4, 5, 6, 7, 8, 9, 10, 11, 13, 16, 17, 18
P353 = 0

# Account. 0 - Account 1, 1 - Account 2, 2 - Account 3
# Number: 0, 1, 2
# Mandatory 
P354 = 0

# Description 
# String
P355 = 

# Value
# String
P356 = 

##############################################################################
##    Settings/Broadsoft/Broadsoft Directories
##############################################################################
##############################################################################
# XSI
##############################################################################
# Server Address
# String
P1591 =  

# Port
# Number
P1592 =  

# XSI Actions Path
# String
P2937 =

# Broadsoft Contact Download Interval. 0 - Disabled. Default is 0
# Number: 0, 5-720
P8362 = 0

# XSI Authentication Type. 0 - Login Credentials, 1 - SIP, 2 - Account 1, 3 - Account 2, 4 - Account 3. Default is 0
# Number: 0, 1, 2, 3, 4
# Mandatory
P22054 = 0

##################################
# Login Credentials              
##################################
# Login Username
# String
P1593 = 

# Login Password
# String
P1594 = 

##################################
# SIP Credentials              
##################################
# SIP Username
# String
P6772 = 

# SIP User ID
# String
P22034 = 

# SIP Password
# String
P6773 = 

# Sort Phonebook by. 0 - Last Name, 1 - First Name. Default is 0
# Number: 0, 1
# Mandatory
P22131 = 0

######################################################################################
# Network Directories
######################################################################################
### Group Directory ###
# Disabled/Enabled. 0 - Disabled, 1 - Enabled.
# Number: 0, 1. Default is 0
# Mandatory
P2971 = 0

# Name
# String
P2972 = 

### Enterprise Directory ###
# Disabled/Enabled. 0 - Disabled, 1 - Enabled.
# Number: 0, 1. Default is 0
# Mandatory
P2973 = 0

# Name
# String
P2974 = 

### Group Common ###
# Disabled/Enabled. 0 - Disabled, 1 - Enabled.
# Number: 0, 1. Default is 0
# Mandatory
P2975 = 0

# Name
# String
P2976 = 

### Enterprise Common ###
# Disabled/Enabled. 0 - Disabled, 1 - Enabled.
# Number: 0, 1. Default is 0
# Mandatory
P2977 = 0

# Name
# String
P2978 =

### Personal Directory ###
# Disabled/Enabled. 0 - Disabled, 1 - Enabled.
# Number: 0, 1. Default is 0
# Mandatory
P2979 = 0

# Name
# String
P2980 =

### Missed Call Log ### 
# Disabled/Enabled. 0 - Disabled, 1 - Enabled.
# Number: 0, 1. Default is 0
# Mandatory
P2981 = 0

# Name
# String
P2982 =

### Placed Call Log ### 
# Disabled/Enabled. 0 - Disabled, 1 - Enabled.
# Number: 0, 1. Default is 0
# Mandatory
P2983 = 0

# Name
# String
P2984 =

### Received Call Log ### 
# Disabled/Enabled. 0 - Disabled, 1 - Enabled.
# Number: 0, 1. Default is 0
# Mandatory
P2985 = 0

# Name. 
# String
P2986 =

#####################################################
##  Settings/External Service
#####################################################
#####################################################
##  Grandstream Door System
#####################################################

########## No.1 ##########
# No.1 - Service Type
# Number: -1 - None, 0 - GDS. Default is 0
# Mandatory
P32000 = 0

# No.1 - Account
# Number: 0 - Account 1, 1 - Account 2, 2 - Account 3. Default is 0
# Mandatory
P32001 = 0

# No.1 - System Identification
# String
P32002 = 

# No.1 - System Number
# String
P32003 =

# No.1 - Access Password
# String
P32004 =

########## No.2 ##########
# No.2 - Service Type
# Number: -1 - None, 0 - GDS. Default is 0
# Mandatory
P32005 = 0

# No.2 - Account
# Number: 0 - Account 1, 1 - Account 2, 2 - Account 3. Default is 0
# Mandatory
P32006 = 0

# No.2 - System Identification
# String
P32007 = 

# No.2 - System Number
# String
P32008 =

# No.2 - Access Password
# String
P32009 =

########## No.3 ##########
# No.3 - Service Type
# Number: -1 - None, 0 - GDS. Default is 0
# Mandatory
P32010 = 0

# No.3 - Account
# Number: 0 - Account 1, 1 - Account 2, 2 - Account 3. Default is 0
# Mandatory
P32011 = 0

# No.3 - System Identification
# String
P32012 = 

# No.3 - System Number
# String
P32013 =

# No.3 - Access Password
# String
P32014 =

########## No.4 ##########
# No.4 - Service Type
# Number: -1 - None, 0 - GDS. Default is 0
# Mandatory
P32015 = 0

# No.4 - Account
# Number: 0 - Account 1, 1 - Account 2, 2 - Account 3. Default is 0
# Mandatory
P32016 = 0

# No.4 - System Identification
# String
P32017 = 

# No.4 - System Number
# String
P32018 =

# No.4 - Access Password
# String
P32019 =

########## No.5 ##########
# No.5 - Service Type
# Number: -1 - None, 0 - GDS. Default is 0
# Mandatory
P32020 = 0

# No.5 - Account
# Number: 0 - Account 1, 1 - Account 2, 2 - Account 3. Default is 0
# Mandatory
P32021 = 0

# No.5 - System Identification
# String
P32022 = 

# No.5 - System Number
# String
P32023 =

# No.5 - Access Password
# String
P32024 =

########## No.6 ##########
# No.6 - Service Type
# Number: -1 - None, 0 - GDS. Default is 0
# Mandatory
P32025 = 0

# No.6 - Account
# Number: 0 - Account 1, 1 - Account 2, 2 - Account 3. Default is 0
# Mandatory
P32026 = 0

# No.6 - System Identification
# String
P32027 = 

# No.6 - System Number
# String
P32028 =

# No.6 - Access Password
# String
P32029 =

########## No.7 ##########
# No.7 - Service Type
# Number: -1 - None, 0 - GDS. Default is 0
# Mandatory
P32030 = 0

# No.7 - Account
# Number: 0 - Account 1, 1 - Account 2, 2 - Account 3. Default is 0
# Mandatory
P32031 = 0

# No.7 - System Identification
# String
P32032 = 

# No.7 - System Number
# String
P32033 =

# No.7 - Access Password
# String
P32034 =

########## No.8 ##########
# No.8 - Service Type
# Number: -1 - None, 0 - GDS. Default is 0
# Mandatory
P32035 = 0

# No.8 - Account
# Number: 0 - Account 1, 1 - Account 2, 2 - Account 3. Default is 0
# Mandatory
P32036 = 0

# No.8 - System Identification
# String
P32037 = 

# No.8 - System Number
# String
P32038 =

# No.8 - Access Password
# String
P32039 =

########## No.9 ##########
# No.9 - Service Type
# Number: -1 - None, 0 - GDS. Default is 0
# Mandatory
P32040 = 0

# No.9 - Account
# Number: 0 - Account 1, 1 - Account 2, 2 - Account 3. Default is 0
# Mandatory
P32041 = 0

# No.9 - System Identification
# String
P32042 = 

# No.9 - System Number
# String
P32043 =

# No.9 - Access Password
# String
P32044 =

########## No.10 ##########
# No.10 - Service Type
# Number: -1 - None, 0 - GDS. Default is 0
# Mandatory
P32045 = 0

# No.10 - Account
# Number: 0 - Account 1, 1 - Account 2, 2 - Account 3. Default is 0
# Mandatory
P32046 = 0

# No.10 - System Identification
# String
P32047 = 

# No.10 - System Number
# String
P32048 =

# No.10 - Access Password
# String
P32049 =
