###############################################################################################
####                                                                                       ####  
####            Configuration Template for GSC3505 Firmware Version 1.0.1.5                ####
####                                                                                       ####
###############################################################################################
##############################################################################
##  Account 1 Settings                                                      ##
##############################################################################
#######################################################################
##  Account 1 General Settings                                       ##
#######################################################################
# Account Active. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P271 = 1

# Account Name
P270 =

# SIP Server
P47 = 

# SIP User ID
P35 =
 
# SIP Authentication ID
P36 =

# SIP Authentication Password
P34 =

# Tel URI. 0 - Disable, 1 - User=Phone, 2 - Enabled. Default value is 0
# Number: 0, 1, 2
P63 = 0

#######################################################################
##  Account 1 Network Settings                                       ##
#######################################################################
# Outbound Proxy
P48 =

# Secondary Outbound Proxy
P2333 =

# DNS Mode.  0 - A Record, 1 - SRV, 2 - NAPTR/SRV. Default value is 0
# Number: 0, 1, 2
P103 = 0

# DNS SRV Fail-over Mode. 0 - Default, 1 - Saved one until DNS TTL, 2 - Saved one until no response, 3 - Register first when  the invite fail-over. 
# Default value is 0
# Number
P26040 = 0

# Register Before DNS SRV Fail-over. 0 - No, 1 - Yes. Default Value is 0.
# Number: 0, 1
P29095 = 1

# NAT Traversal. 0 - NAT No, 1 - STUN, 2 - Keep-alive, 3 - UPnP, 4 - Auto, 5 - VPN. Default value is 2
# Number: 0, 1, 2, 3, 4, 5
P52 = 2

# Proxy-Require
P197 =

#######################################################################
##  Account 1 SIP Settings                                           ##
#######################################################################
# SIP Registration. 0 - No, 1 - Yes. Default is 1
# Number: 0, 1
P31 = 1

# Unregister Before New Registration. 0 - No, 1 - All, 2 -  Instance . Default value is 2
# Number: 0, 1, 2
P81 = 2

# Register Expiration (m). In minutes. Default value is 60
# Number: 60 - 64800
P32 = 60

# Subscribe Expiration (m). In minutes. Default value is blank
# Number: 0 - 64800
P26051 =

# Re-register before Expiration (s). Default Value is 0
# Number: 0 - 3600
P2330 = 0

# Registration Retry Wait Time (s). In seconds. Default value is 20
# Number: 20 - 3600
P138 = 20

# Add Auth Header On RE-REGISTER
# 0 - No, 1- Yes
P2359 = 1

# Enable SIP OPTIONS Keep Alive. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P2397 = 0

# SIP OPTIONS Keep Alive Interval(s). Default value is 30
# Number: 1 - 64800 
P2398 = 30

# SIP OPTIONS Keep Alive Maximum Tries. Default value is 3
# Number: 3 - 10
P2399 = 3

# Use Privacy Header. 0 - Default, 1 - No, 2 - Yes. Default value is 0
# Number: 0, 1, 2
P2338 = 0

# Use P-Preferred-Identity Header. 0 - Default, 1 - No, 2 - Yes. Default value is 0
# Number: 0, 1, 2
P2339 = 0

# SIP Transport. 0 - UDP, 1 - TCP, 2 - TLS. Default value is 0
# Number: 0, 1, 2
P130 = 0

# Local SIP Port. Default value is 5060
# Number: 0 or 90 - 65535
P40 = 5060

# SIP URI Scheme When Using TLS
# 0 -sip, 1 - sips. Default value is 0.
# Number: 0, 1
P2329 = 0

# Use Actual Ephemeral Port in Contact with TCP/TLS
# 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P2331 = 0

# Support SIP Instance ID
# 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P288 = 1

# SIP T1 Timeout. RFC 3261 T1 value (RTT estimate)
# 50 - 0.5 sec, 100 - 1 sec, 200 - 2 sec. Default value is 50
# Number: 50, 100, 200
P209 = 50

# SIP T2 Interval. RFC 3261 T2 value
# The maximum retransmit interval for non-INVITE requests and INVITE responses
# 200 - 2 sec, 400 - 4 sec, 800 - 8 sec. Default value is 400
# Number: 200, 400, 800.
P250 = 400

# SIP Timer D Interval (Seconds)
# Number 0-64. Default value is 0
P2387 = 0

# Remove OBP from Route
# 0 - Disable, 1 - Enable, 2 - Always. Default value is 0
# Number: 0, 1, 2
P2305 = 0

# Enable 100rel. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P272 = 0

#######################################################################
##  Account 1 Session Timer                                          ##
#######################################################################

# Enable Session Timer/ Session Expiration(s).  In seconds. Default value is 180 seconds.
# By default,  Session Timer is Enabled.  Session Timer is disabled if the value is 0.
# Number: 0 or 90 - 64800
P260 = 180

# Min-SE (s). Default value is 90 seconds
# Number: 0 or 90 - 64800
P261 = 90

# UAC Specify Refresher. 0 - Omit, 1 - UAC, 2 - UAS. Default value is 0
# Number: 0, 1, 2
P266 = 0

# UAS Specify Refresher. 1 - UAC, 2 - UAS. Default value is 1
# Number: 1, 2
P267 = 1

# Caller Request Timer. Request for timer when calling
# 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P262 = 0

# Callee Request Timer
# Request for timer when being called (i.e., if remote party supports timer but did not request for one)
# 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P263 = 0

# Force Timer. Still use timer when remote party does not support timer
# 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P264 = 0

# Force INVITE. Always refresh with INVITE instead of UPDATE even when remote party supports UPDATE
# 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P265 = 0

#######################################################################
##  Account 1 Codec Settings                                         ##
#######################################################################
# Preferred Vocoder
# First codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 103 - G722.1C, 104 - G722.1, 123 - Opus. Default value is 0
# Number: 0, 2, 8, 9, 18, 98, 103, 104, 123
P57 = 0

# Second codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 103 - G722.1C, 104 - G722.1, 123 - Opus. Default value is 8
# Number: 0, 2, 8, 9, 18, 98, 103, 104, 123
P58 = 8

# Third codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 103 - G722.1C, 104 - G722.1, 123 - Opus. Default value is 9
# Number: 0, 2, 8, 9, 18, 98, 103, 104, 123
P59 = 9

# Forth codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 103 - G722.1C, 104 - G722.1, 123 - Opus. Default value is 104
# Number: 0, 2, 8, 9, 18, 98, 103, 104, 123
P60 = 104

# Fifth codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 103 - G722.1C, 104 - G722.1, 123 - Opus. Default value is 104
# Number: 0, 2, 8, 9, 18, 98, 103, 104, 123
P61 = 104

# Sixth codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 103 - G722.1C, 104 - G722.1, 123 - Opus. Default value is 104
# Number: 0, 2, 8, 9, 18, 98, 103, 104, 123
P62 = 104

# Seventh codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 103 - G722.1C, 104 - G722.1, 123 - Opus. Default value is 104
# Number: 0, 2, 8, 9, 18, 98, 103, 104, 123
P46 = 104

# Eigth codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 103 - G722.1C, 104 - G722.1, 123 - Opus. Default value is 104
# Number: 0, 2, 8, 9, 18, 98, 103, 104, 123
P98 = 104

# Codec Negotiation Priority. 0 - Caller, 1 - Callee. Default value is 1.
# Number: 0, 1
P29061 = 1

# Use First Matching Vocoder in 200OK SDP. 0 - No, 1 - Yes. The default value is 0.
# Number: 0, 1
P2348 = 0

# iLBC Frame Size. 0 - 20 ms, 1 - 30 ms. Default value is 1.
# Number: 0, 1
P97 = 1

# G726-32 ITU Payload. 0 - 2, 1 - Dynamic. Default value is 0.
# Number: 0, 1
P2369 = 0

# G726-32 Dynamic PT. Default value is 126.
# Number
P2365 = 126

# Opus Payload Type. Default value is 123.
P2385 = 123

# DTMF: in audio. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P2301 = 0

# DTMF: via RFC2833. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P2302 = 1

# DTMF: via SIP INFO. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P2303 = 0

# DTMF Payload Type. Default value is 101
# Number: 96 - 127
P79 = 101

# Enable Audio RED with FEC. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P26073 = 0

# Audio FEC Payload Type. Default value is 121
# Number: 96 - 126
P26074 = 121

# Audio RED Payload Type. Default value is 124
# Number: 96 - 126
P26075 = 124

# Silence Suppression. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P50 = 0

# Voice Frames Per TX. Default value is 2
# Number: 1 - 64.
P37 = 2

#######################################################################
##  Account 1 RTP Settings                                           ##
#######################################################################
# SRTP Mode. 0 - Disable, 1 - Enabled but not forced, 2 - Enabled and forced. Default value is 0.
# Number: 0, 1, 2
P183 = 0

# SRTP Key Length. 0 - AES 128&256 bit, 1 - AES 128 bit, 2 - AES 256 bit. Default value is 0
#Number:0, 1, 2
P2383 = 0 

# Enable SRTP Key Life Time. 0 - No, 1 - Yes.
# Number: 0,1
P2363 = 1

# RTCP Destination
P2390 = 

# Symmetric RTP. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P291 = 0

# RTP IP Filter. 0 - Disable, 1 - IP Only, 2 - IP and Port. Default value is 0
# Number: 0, 1, 2
P26026 = 0

#######################################################################
##  Account 1 Call Settings                                          ##
#######################################################################
# Play warning tone for Auto Answer Intercom. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P26072 = 1

# Send Anonymous. 0 - No, 1 - Yes (caller ID will be blocked if set to Yes). Default value is 0
# Number: 0, 1
P65 = 0

# Intercept Anonymous Calls. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P129 = 0

# Call Log
# 0 - Log All, 1 - Log Incoming/Outgoing only (Missed Calls Not Recorded), 2 - Disable Call All, 3 - Don't Prompt Missed Call. Default value is 0
# Number: 0, 1, 2
P182 = 0

# Ring Timeout (s). Default value is 60
# Number: 0 - 300
P1328 = 60

# Refer-To Use Target Contact. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P135 = 0

# Incoming Call Rules. 0 - Block, 1 - Set Password, 2 - Auto Answer, 3 - Ringing, 4 - Disable. Default value is 4.
# Number: 0, 1, 2 ,3 ,4
P60044 = 4

# Set Password Rules. 
# Numbers
P60045

# Dial Plan Prefix
# String
P66 =

# Disable DialPlan. 0 - No Selection, 1 - Dial Page, 2 - Contact, 4 - Incoming Call History, 8 -  Outgoing Call History, 16 - MPK & Click2Dial. 
# If need to check multiple selections, add the specific values for each selections together. Default value is 0
# Number: 0-31
P2382 = 0

# DialPlan. Default value is { x+ | \+x+ | *x+ | *xx*x+ }
P290 = { x+ | \+x+ | *x+ | *xx*x+ }

# Account Ringtone. See ring tone options and value in the Ring Tone Value Table below.
P104 = content://settings/system/ringtone

# Ignore Alert-Info Header. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1
P26018 = 0

# Matching Incoming Caller ID. Matching Rule 1.
# String
P1488 =

# Matching Rule 1 Distinctive Ringtone. See ring tone options and value in the Ring Tone Value Table below.
# String
P1489 = content://settings/system/ringtone

# Matching Incoming Caller ID. Matching Rule 2.
# String
P1490 =

# Matching Rule 2 Distinctive Ringtone. See ring tone options and value in the Ring Tone Value Table below.
# String
P1491 = content://settings/system/ringtone

# Matching Incoming Caller ID. Matching Rule 3.
# String
P1492 =

# Matching Rule 3 Distinctive Ringtone. See ring tone options and value in the Ring Tone Value Table below.
# String
P1493 = content://settings/system/ringtone

############Ring Tone Value Table###############
# Web GUI Option                            Value
# Use System Ring tone                      content://settings/system/ringtone 
# Andromeda					/system/media/audio/ringtones/ANDROMEDA.ogg
# Aquila					/system/media/audio/ringtones/Aquila.ogg
# Argo Navis					/system/media/audio/ringtones/ArgoNavis.ogg
# Atria					/system/media/audio/ringtones/Atria.ogg
# Backroad					/system/media/audio/ringtones/Backroad.ogg
# Beat Plucker					/system/media/audio/ringtones/BeatPlucker.ogg
# Bell Phone					/system/media/audio/ringtones/Ring_Classic_02.ogg
# Bentley Dubs					/system/media/audio/ringtones/BentleyDubs.ogg
# Big Easy					/system/media/audio/ringtones/Big_Easy.ogg
# Bird Loop					/system/media/audio/ringtones/BirdLoop.ogg
# Bollywood					/system/media/audio/ringtones/Bollywood.ogg
# Boötes					/system/media/audio/ringtones/BOOTES.ogg
# Bus' a Move					/system/media/audio/ringtones/BussaMove.ogg
# Cairo					/system/media/audio/ringtones/Cairo.ogg
# Calypso Steel					/system/media/audio/ringtones/Calypso_Steel.ogg
# Canis Major					/system/media/audio/ringtones/CANISMAJOR.ogg
# Caribbean Ice					/system/media/audio/ringtones/CaribbeanIce.ogg
# Carina					/system/media/audio/ringtones/Carina.ogg
# Cassiopeia					/system/media/audio/ringtones/CASSIOPEIA.ogg
# Centaurus					/system/media/audio/ringtones/Centaurus.ogg
# Champagne Edition					/system/media/audio/ringtones/Champagne_Edition.ogg
# Chimey Phone					/system/media/audio/ringtones/Ring_Synth_02.ogg
# Club Cubano					/system/media/audio/ringtones/Club_Cubano.ogg
# Crayon Rock					/system/media/audio/ringtones/CrayonRock.ogg
# Crazy Dream					/system/media/audio/ringtones/CrazyDream.ogg
# Curve Ball Blend					/system/media/audio/ringtones/CurveBall.ogg
# Cygnus					/system/media/audio/ringtones/Cygnus.ogg
# Dancin' Fool					/system/media/audio/ringtones/DancinFool.ogg
# Digital Phone					/system/media/audio/ringtones/Ring_Digital_02.ogg
# Ding					/system/media/audio/ringtones/Ding.ogg
# DingDong					/system/media/audio/ringtones/DingDong.wav
# Don' Mess Wiv It					/system/media/audio/ringtones/DonMessWivIt.ogg
# Draco					/system/media/audio/ringtones/Draco.ogg
# Dream Theme					/system/media/audio/ringtones/DreamTheme.ogg
# Eastern Sky					/system/media/audio/ringtones/Eastern_Sky.ogg
# Enter the Nexus					/system/media/audio/ringtones/Enter_the_Nexus.ogg
# Eridani					/system/media/audio/ringtones/Eridani.ogg
# Ether Shake					/system/media/audio/ringtones/EtherShake.ogg
# Flutey Phone					/system/media/audio/ringtones/Ring_Synth_04.ogg
# Free Flight					/system/media/audio/ringtones/FreeFlight.ogg
# Friendly Ghost					/system/media/audio/ringtones/FriendlyGhost.ogg
# Funk Y'all					/system/media/audio/ringtones/Funk_Yall.ogg
# Game Over Guitar					/system/media/audio/ringtones/GameOverGuitar.ogg
# Gimme Mo' Town					/system/media/audio/ringtones/Gimme_Mo_Town.ogg
# Girtab					/system/media/audio/ringtones/Girtab.ogg
# Glacial Groove					/system/media/audio/ringtones/Glacial_Groove.ogg
# Growl					/system/media/audio/ringtones/Growl.ogg
# Halfway Home					/system/media/audio/ringtones/HalfwayHome.ogg
# Hydra					/system/media/audio/ringtones/Hydra.ogg
# Insert Coin					/system/media/audio/ringtones/InsertCoin.ogg
# Kuma					/system/media/audio/ringtones/Kuma.ogg
# Loopy Lounge					/system/media/audio/ringtones/LoopyLounge.ogg
# Love Flute					/system/media/audio/ringtones/LoveFlute.ogg
# Lyra					/system/media/audio/ringtones/Lyra.ogg
# Machina					/system/media/audio/ringtones/Machina.ogg
# Medieval Jaunt					/system/media/audio/ringtones/MidEvilJaunt.ogg
# Mildly Alarming					/system/media/audio/ringtones/MildlyAlarming.ogg
# Nairobi					/system/media/audio/ringtones/Nairobi.ogg
# Nassau					/system/media/audio/ringtones/Nassau.ogg
# New Player					/system/media/audio/ringtones/NewPlayer.ogg
# No Limits					/system/media/audio/ringtones/No_Limits.ogg
# Noisey One					/system/media/audio/ringtones/Noises1.ogg
# Organ Dub					/system/media/audio/ringtones/OrganDub.ogg
# Orion					/system/media/audio/ringtones/Orion.ogg
# Paradise Island					/system/media/audio/ringtones/Paradise_Island.ogg
# Pegasus					/system/media/audio/ringtones/Pegasus.ogg
# Perseus					/system/media/audio/ringtones/PERSEUS.ogg
# Playa					/system/media/audio/ringtones/Playa.ogg
# Pyxis					/system/media/audio/ringtones/Pyxis.ogg
# Rasalas					/system/media/audio/ringtones/Rasalas.ogg
# Revelation					/system/media/audio/ringtones/Revelation.ogg
# Rigel					/system/media/audio/ringtones/Rigel.ogg
# Road Trip					/system/media/audio/ringtones/Road_Trip.ogg
# Romancing The Tone					/system/media/audio/ringtones/RomancingTheTone.ogg
# Safari					/system/media/audio/ringtones/Safari.ogg
# Savannah					/system/media/audio/ringtones/Savannah.ogg
# Scarabaeus					/system/media/audio/ringtones/Scarabaeus.ogg
# Sceptrum					/system/media/audio/ringtones/Sceptrum.ogg
# Seville					/system/media/audio/ringtones/Seville.ogg
# She's All That					/system/media/audio/ringtones/Shes_All_That.ogg
# Silky Way					/system/media/audio/ringtones/SilkyWay.ogg
# Sitar Versus Sitar					/system/media/audio/ringtones/SitarVsSitar.ogg
# Solarium					/system/media/audio/ringtones/Solarium.ogg
# Springy Jalopy					/system/media/audio/ringtones/SpringyJalopy.ogg
# Steppin' Out					/system/media/audio/ringtones/Steppin_Out.ogg
# Terminated					/system/media/audio/ringtones/Terminated.ogg
# Terrible Twos					/system/media/audio/ringtones/Noises2.ogg
# Testudo					/system/media/audio/ringtones/Testudo.ogg
# Themos					/system/media/audio/ringtones/Themos.ogg
# Third Eye					/system/media/audio/ringtones/Third_Eye.ogg
# Thriller Three					/system/media/audio/ringtones/Noises3.ogg
# Thunderfoot					/system/media/audio/ringtones/Thunderfoot.ogg
# Twirl Away					/system/media/audio/ringtones/TwirlAway.ogg
# Ursa Minor					/system/media/audio/ringtones/URSAMINOR.ogg
# UrsaMinor					/system/media/audio/ringtones/UrsaMinor.ogg
# Very Alarmed					/system/media/audio/ringtones/VeryAlarmed.ogg
# Vespa					/system/media/audio/ringtones/Vespa.ogg
# World					/system/media/audio/ringtones/World.ogg
# Zeta					/system/media/audio/ringtones/Zeta.ogg
# bellcore-dr1					/system/media/audio/ringtones/bellcore-dr1.ogg
# bellcore-dr2					/system/media/audio/ringtones/bellcore-dr2.ogg
# bellcore-dr3					/system/media/audio/ringtones/bellcore-dr3.ogg
# bellcore-dr4					/system/media/audio/ringtones/bellcore-dr4.ogg
# bellcore-dr5					/system/media/audio/ringtones/bellcore-dr5.ogg
# speaker					/system/media/audio/ringtones/speaker.wav

#######################################################################
##  Account 1 Advanced Settings                                      ##
#######################################################################
# Check Domain Certificates. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P2311 = 0

# Validate Certificate Chain. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P2367 = 0

# Validate Incoming SIP Messages. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P2306 = 0

# Allow Unsolicited REFER. 0 - Disabled, 1 - Enabled, 2 - Enabled/Force Auth. Default value is 0.
# Number: 0, 1, 2
P26023 = 0

# Only Accept SIP Requests from Known Servers. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P2347 = 0

# Check SIP User ID for Incoming INVITE. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P258 = 0

# Allow SIP Reset. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P26015 = 0

# Authenticate Incoming INVITE. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P2346 = 0

# SIP Realm Used for Challenge INVITE & NOTIFY.
# String
P26021 =

# Enable Local MOH
# Number: 0, 1
P2357 = 0

# Virtual Account Group. -1 - Default,  0 - Virtual Account Group 1, 1 - Virtual Account Group 2, 2 - Virtual Account Group 3
# 3 - Virtual Account Group 4, 4 - Virtual Account Group 5, 5 - Virtual Account Group 6, 6 - Virtual Account Group 7, 7 - Virtual Account Group 8
# 8 - Virtual Account Group 9, 9 - Virtual Account Group 10, 10 - Virtual Account Group 11, 11 - Virtual Account Group 12, 12 - Virtual Account Group 13
# 13 - Virtual Account Group 14, 14 - Virtual Account Group 15, 15 - Virtual Account Group 16. Default value is -1.
# Number: -1 - 15 
P2391 = -1

# Special Feature. Default value is 100
# 100 - Standard, 102 - Broadsoft, 113 - China Mobile, 114 - ZTE IMS, 115 - Mobotix
# 116 - ZTE NGN, 117 - Huawei IMS, 123 - NEC, 125 - WorldStone, 129 - Telefonica Spain
# Number: 100, 102, 113, 114, 115, 116, 117, 123, 125, 129
P198 = 100

# Feature Key Synchronization.  0 - Disable, 0 - Broadsoft/Metaswitch. Default Value is 0.
# Number: 0, 1
# P2325 = 0

# Allow Sync Phonebook via SIP Notify. 0 - No, 1 - Yes. Default is 1.
# Number: 0, 1
P26099 = 1

##############################################################################
##  Account 2 Settings                                                      ##
##############################################################################
#######################################################################
##  Account 2 General Settings                                       ##
#######################################################################
# Account Active. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P401 = 0

# Account Name
P417 =

# SIP Server
P402 =

# SIP User ID
P404 =

# SIP Authentication ID
P405 =

# SIP Authentication Password
P406 =

# Tel URI. 0 - Disable, 1 - User=Phone, 2 - Enabled. Default value is 0
# Number: 0, 1, 2
P409 = 0

#######################################################################
##  Account 2 Network Settings                                       ##
#######################################################################
# Outbound Proxy
P403 =

# Secondary Outbound Proxy
P2433 =

# DNS Mode.  0 - A Record, 1 - SRV, 2 - NAPTR/SRV. Default value is 0
# Number: 0, 1, 2
P408 = 0

# DNS SRV Fail-over Mode. 0 - Default, 1 - Saved one until DNS TTL, 2 - Saved one until no response. Defualt value is 1
# Number
P26140 = 0

# Register Before DNS SRV Fail-over. 0 - No, 1 - Yes. Default Value is 0.
# Number: 0, 1
P29195 = 1

# NAT Traversal. 0 - NAT No, 1 - STUN, 2 - Keep-alive, 3 - UPnP, 4 - Auto, 5 - VPN. Default value is 2
# Number: 0, 1, 2, 3, 4, 5
P414 = 2

# Proxy-Require
P418 =

#######################################################################
##  Account 2 SIP Settings                                           ##
#######################################################################
# SIP Registration. 0 - No, 1 - Yes. Default is 1
# Number: 0, 1
P410 = 1

# Unregister Before New Registration. 0 - No, 1 - All, 2 -  Instance . Default value is 0
# Number: 0, 1, 2
P411 = 2

# Register Expiration (m). In minutes. Default value is 60
# Number: 60 - 64800
P412 = 60

# Subscribe Expiration (m). In minutes. Default value is blank
# Number: 0 - 64800
P26151 = 60

# Re-register before Expiration (s). Default value is 0
# Number: 0 - 3600
P2430 = 0

# Registration Retry Wait Time (s). In seconds. Default value is 20
# Number: 20 - 3600
P471 = 20

# Add Auth Header On RE-REGISTER
# 0 - No, 1- Yes
P2459 = 1

# Enable SIP OPTIONS Keep Alive. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P2497 = 0

# SIP OPTIONS Keep Alive Interval(s). Default value is 30
# Number: 1 - 64800 
P2498 = 30

# SIP OPTIONS Keep Alive Maximum Tries. Default value is 3
# Number: 3 
P2499 = 3

# Use Privacy Header. 0 - Default, 1 - No, 2 - Yes. Default value is 0
# Number: 0, 1, 2
P2438 = 0

# Use P-Preferred-Identity Header. 0 - Default, 1 - No, 2 - Yes. Default value is 0
# Number: 0, 1, 2
P2439 = 0

# SIP Transport. 0 - UDP, 1 - TCP, 2 - TLS. Default value is 0
# Number: 0, 1, 2
P448 = 0

# Local SIP Port. Default value is 5062
# Number: 0 or 90 - 65535
P413 = 5062

# SIP URI Scheme When Using TLS
# 0 -sip, 1 - sips. Default value is 0.
# Number: 0, 1
P2429 = 0

# Use Actual Ephemeral Port in Contact with TCP/TLS
# 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P2431 = 0

# Support SIP Instance ID. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P489 = 1

# SIP T1 Timeout. RFC 3261 T1 value (RTT estimate). 50 - 0.5 sec, 100 - 1 sec, 200 - 2 sec. Default value is 50
# Number: 50, 100, 200
P440 = 50

# SIP T2 Interval. RFC 3261 T2 value. The maximum retransmit interval for non-INVITE requests and INVITE responses
# 200 - 2 sec, 400 - 4 sec, 800 - 8 sec. Default value is 400
# Number: 200, 400, 800
P441 = 400

# SIP Timer D Interval (Seconds)
# Number 0-64. Default value is 0
P2487 = 0

# Remove OBP from route. 0 - Disable, 1 - Enable. Default value is 0
# Number: 0, 1
P2405 = 0

# Enable 100rel. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P435 = 0 

#######################################################################
##  Account 2 Session Timer                                          ##
#######################################################################

# Enable Session Timer/ Session Expiration(s).  In seconds. Default value is 180 seconds.
# By default,  Session Timer is Enabled.  Session Timer is disabled if the value is 0.
# Number: 0 or 90 - 64800
P434 = 180

# Min-SE (s). Default value is 90 seconds
# Number: 0 or 90 - 64800
P427 = 90

# UAC Specify Refresher. 0 - Omit, 1 - UAC, 2 - UAS. Default value is 0
# Number: 0, 1, 2
P432 = 0

# UAS Specify Refresher. 1 - UAC, 2 - UAS. Default value is 1
# Number: 1, 2
P433 = 1

# Caller Request Timer (Request for timer when calling). 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P428 = 0

# Callee Request Timer (Request for timer when being called, i.e. if remote party supports timer but did not request for one)
# 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P429 = 0

# Force Timer (Still use timer when remote party does not support timer). 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P430 = 0

# Force INVITE (Always refresh with INVITE instead of UPDATE even when remote party supports UPDATE)
# 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P431 = 0

#######################################################################
##  Account 2 Codec Settings                                         ##
#######################################################################
# Preferred Vocoder
# First codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 103 - G722.1C, 104 - G722.1, 123 - Opus. Default value is 0
# Number: 0, 2, 8, 9, 18, 98, 103, 104, 123
P451 = 0

# Second codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 103 - G722.1C, 104 - G722.1, 123 - Opus. Default value is 8
# Number: 0, 2, 8, 9, 18, 98, 103, 104, 123
P452 = 8

# Third codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 103 - G722.1C, 104 - G722.1, 123 - Opus. Default value is 9
# Number: 0, 2, 8, 9, 18, 98, 103, 104, 123
P453 = 9

# Forth codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 103 - G722.1C, 104 - G722.1, 123 - Opus. Default value is 104
# Number: 0, 2, 8, 9, 18, 98, 103, 104, 123
P454 = 104

# Fifth codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 103 - G722.1C, 104 - G722.1, 123 - Opus. Default value is 104
# Number: 0, 2, 8, 9, 18, 98, 103, 104, 123
P455 = 104

# Sixth codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 103 - G722.1C, 104 - G722.1, 123 - Opus. Default value is 104
# Number: 0, 2, 8, 9, 18, 98, 103, 104, 123
P456 = 104

# Seventh codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 103 - G722.1C, 104 - G722.1, 123 - Opus. Default value is 104
# Number: 0, 2, 8, 9, 18, 98, 103, 104, 123
P457 = 104

# Eigth codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 103 - G722.1C, 104 - G722.1, 123 - Opus. Default value is 104
# Number: 0, 2, 8, 9, 18, 98, 103, 104, 123
P458 = 104

# Codec Negotiation Priority. 0 - Caller, 1 - Callee. Default value is 1.
# Number: 0, 1
P29161 = 1

# Use First Matching Vocoder in 200OK SDP. 0 - No, 1 - Yes. The default value is 0.
# Number: 0, 1
P2448 = 0

# iLBC Frame Size. 0 - 20 ms, 1 - 30 ms. Default value is 1.
# Number: 0, 1
P495 = 1

# G726-32 ITU Payload. 0 - 2, 1 - Dynamic. Default value is 0.
# Number: 0, 1
P2469 = 0

# G726-32 Dynamic PT. Default value is 126.
# Number
P2465 = 126

# Opus Payload Type. Default value is 123.
P2485 = 123

# DTMF: in audio. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P2401 = 0

# DTMF: via RFC2833. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P2402 = 1

# DTMF: via SIP INFO. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P2403 = 0

# DTMF Payload Type. Default value is 101
# Number: 96 - 127
P496 = 101

# Enable Audio RED with FEC. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P26173 = 0

# Audio FEC Payload Type. Default value is 121
# Number: 96 - 126
P26174 = 121

# Audio RED Payload Type. Default value is 124
# Number: 96 - 126
P26175 = 124

# Silence Suppression. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P485 = 0

# Voice Frames per TX. Default value is 2
# Number: 1 - 64
P486 = 2

#######################################################################
##  Account 2 RTP Settings                                           ##
#######################################################################
# SRTP Mode. 0 - Disable, 1 - Enabled but not forced, 2 - Enabled and forced. Default value is 0
# Number: 0, 1, 2
P443 = 0

# SRTP Key Length. 0 - AES 128&256 bit, 1 - AES 128 bit, 2 - AES 256 bit. Default value is 0
#Number:0, 1, 2
P2483 = 0 

# Enable SRTP Key Life Time. 0 - No, 1 - Yes.
# Number: 0,1
P2463 = 1

# RTCP Destination
P2490 = 

# Symmetric RTP. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P460 = 0

# RTP IP Filter. 0 - Disable, 1 - IP Only, 2 - IP and Port. Default value is 0
# Number: 0, 1, 2
P26126 = 0

#######################################################################
##  Account 2 Call Settings                                          ##
#######################################################################
# Play warning tone for Auto Answer Intercom. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P26172 = 1

# Send Anonymous. 0 - No, 1 - Yes (caller ID will be blocked if set to Yes). Default value is 0
# Number: 0, 1
P421 = 0

# Intercept Anonymous Calls. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P446 = 0

# Call Log
# 0 - Log All, 1 - Log Incoming/Outgoing only (Missed Calls Not Recorded), 2 - Disable Call All, 3 - Don't Prompt Missed Call. Default value is 0
# Number: 0, 1, 2
P442 = 0

# Ring Timeout (s). Default value is 60
# Number: 0 - 300
P476 = 60

# Refer-To Use Target Contact. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P469 = 0

# Incoming Call Rules. 0 - Block, 1 - Set Password, 2 - Auto Answer, 3 - Ringing, 4 - Disable. Default value is 4.
# Number: 0, 1, 2 ,3 ,4
P60144 = 4

# Set Password Rules. 
# Numbers
P60145

# Dial Plan Prefix
# String
P419 =

# Disable DialPlan. 0 - No Selection, 1 - Dial Page, 2 - Contact, 4 - Incoming Call History, 8 -  Outgoing Call History, 16 - MPK & Click2Dial. 
# If need to check multiple selections, add the specific values for each selections together. Default value is 0
# Number: 0-31
P2482 = 0

# DialPlan. Default value is { x+ | \+x+ | *x+ | *xx*x+ }
P459 = { x+ | \+x+ | *x+ | *xx*x+ }

# Account Ringtone. See ring tone options and value in the Ring Tone Value Table below.
P423 = content://settings/system/ringtone

# Ignore Alert-Info Header. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1
P26118 = 0

# Matching Incoming Caller ID. Matching Rule 1.
# String
P1494 =

# Matching Rule 1 Distinctive Ringtone. See ring tone options and value in the Ring Tone Value Table below.
# String
P1495 = content://settings/system/ringtone

# Matching Incoming Caller ID. Matching Rule 2.
# String
P1496 =

# Matching Rule 2 Distinctive Ringtone. See ring tone options and value in the Ring Tone Value Table below.
# String
P1497 = content://settings/system/ringtone

# Matching Incoming Caller ID. Matching Rule 3.
# String
P1498 =

# Matching Rule 3 Distinctive Ringtone. See ring tone options and value in the Ring Tone Value Table below.
# String
P1499 = content://settings/system/ringtone

############Ring Tone Value Table###############
# Web GUI Option                            Value
# Use System Ring tone                      content://settings/system/ringtone 
# Andromeda					/system/media/audio/ringtones/ANDROMEDA.ogg
# Aquila					/system/media/audio/ringtones/Aquila.ogg
# Argo Navis					/system/media/audio/ringtones/ArgoNavis.ogg
# Atria					/system/media/audio/ringtones/Atria.ogg
# Backroad					/system/media/audio/ringtones/Backroad.ogg
# Beat Plucker					/system/media/audio/ringtones/BeatPlucker.ogg
# Bell Phone					/system/media/audio/ringtones/Ring_Classic_02.ogg
# Bentley Dubs					/system/media/audio/ringtones/BentleyDubs.ogg
# Big Easy					/system/media/audio/ringtones/Big_Easy.ogg
# Bird Loop					/system/media/audio/ringtones/BirdLoop.ogg
# Bollywood					/system/media/audio/ringtones/Bollywood.ogg
# Boötes					/system/media/audio/ringtones/BOOTES.ogg
# Bus' a Move					/system/media/audio/ringtones/BussaMove.ogg
# Cairo					/system/media/audio/ringtones/Cairo.ogg
# Calypso Steel					/system/media/audio/ringtones/Calypso_Steel.ogg
# Canis Major					/system/media/audio/ringtones/CANISMAJOR.ogg
# Caribbean Ice					/system/media/audio/ringtones/CaribbeanIce.ogg
# Carina					/system/media/audio/ringtones/Carina.ogg
# Cassiopeia					/system/media/audio/ringtones/CASSIOPEIA.ogg
# Centaurus					/system/media/audio/ringtones/Centaurus.ogg
# Champagne Edition					/system/media/audio/ringtones/Champagne_Edition.ogg
# Chimey Phone					/system/media/audio/ringtones/Ring_Synth_02.ogg
# Club Cubano					/system/media/audio/ringtones/Club_Cubano.ogg
# Crayon Rock					/system/media/audio/ringtones/CrayonRock.ogg
# Crazy Dream					/system/media/audio/ringtones/CrazyDream.ogg
# Curve Ball Blend					/system/media/audio/ringtones/CurveBall.ogg
# Cygnus					/system/media/audio/ringtones/Cygnus.ogg
# Dancin' Fool					/system/media/audio/ringtones/DancinFool.ogg
# Digital Phone					/system/media/audio/ringtones/Ring_Digital_02.ogg
# Ding					/system/media/audio/ringtones/Ding.ogg
# DingDong					/system/media/audio/ringtones/DingDong.wav
# Don' Mess Wiv It					/system/media/audio/ringtones/DonMessWivIt.ogg
# Draco					/system/media/audio/ringtones/Draco.ogg
# Dream Theme					/system/media/audio/ringtones/DreamTheme.ogg
# Eastern Sky					/system/media/audio/ringtones/Eastern_Sky.ogg
# Enter the Nexus					/system/media/audio/ringtones/Enter_the_Nexus.ogg
# Eridani					/system/media/audio/ringtones/Eridani.ogg
# Ether Shake					/system/media/audio/ringtones/EtherShake.ogg
# Flutey Phone					/system/media/audio/ringtones/Ring_Synth_04.ogg
# Free Flight					/system/media/audio/ringtones/FreeFlight.ogg
# Friendly Ghost					/system/media/audio/ringtones/FriendlyGhost.ogg
# Funk Y'all					/system/media/audio/ringtones/Funk_Yall.ogg
# Game Over Guitar					/system/media/audio/ringtones/GameOverGuitar.ogg
# Gimme Mo' Town					/system/media/audio/ringtones/Gimme_Mo_Town.ogg
# Girtab					/system/media/audio/ringtones/Girtab.ogg
# Glacial Groove					/system/media/audio/ringtones/Glacial_Groove.ogg
# Growl					/system/media/audio/ringtones/Growl.ogg
# Halfway Home					/system/media/audio/ringtones/HalfwayHome.ogg
# Hydra					/system/media/audio/ringtones/Hydra.ogg
# Insert Coin					/system/media/audio/ringtones/InsertCoin.ogg
# Kuma					/system/media/audio/ringtones/Kuma.ogg
# Loopy Lounge					/system/media/audio/ringtones/LoopyLounge.ogg
# Love Flute					/system/media/audio/ringtones/LoveFlute.ogg
# Lyra					/system/media/audio/ringtones/Lyra.ogg
# Machina					/system/media/audio/ringtones/Machina.ogg
# Medieval Jaunt					/system/media/audio/ringtones/MidEvilJaunt.ogg
# Mildly Alarming					/system/media/audio/ringtones/MildlyAlarming.ogg
# Nairobi					/system/media/audio/ringtones/Nairobi.ogg
# Nassau					/system/media/audio/ringtones/Nassau.ogg
# New Player					/system/media/audio/ringtones/NewPlayer.ogg
# No Limits					/system/media/audio/ringtones/No_Limits.ogg
# Noisey One					/system/media/audio/ringtones/Noises1.ogg
# Organ Dub					/system/media/audio/ringtones/OrganDub.ogg
# Orion					/system/media/audio/ringtones/Orion.ogg
# Paradise Island					/system/media/audio/ringtones/Paradise_Island.ogg
# Pegasus					/system/media/audio/ringtones/Pegasus.ogg
# Perseus					/system/media/audio/ringtones/PERSEUS.ogg
# Playa					/system/media/audio/ringtones/Playa.ogg
# Pyxis					/system/media/audio/ringtones/Pyxis.ogg
# Rasalas					/system/media/audio/ringtones/Rasalas.ogg
# Revelation					/system/media/audio/ringtones/Revelation.ogg
# Rigel					/system/media/audio/ringtones/Rigel.ogg
# Road Trip					/system/media/audio/ringtones/Road_Trip.ogg
# Romancing The Tone					/system/media/audio/ringtones/RomancingTheTone.ogg
# Safari					/system/media/audio/ringtones/Safari.ogg
# Savannah					/system/media/audio/ringtones/Savannah.ogg
# Scarabaeus					/system/media/audio/ringtones/Scarabaeus.ogg
# Sceptrum					/system/media/audio/ringtones/Sceptrum.ogg
# Seville					/system/media/audio/ringtones/Seville.ogg
# She's All That					/system/media/audio/ringtones/Shes_All_That.ogg
# Silky Way					/system/media/audio/ringtones/SilkyWay.ogg
# Sitar Versus Sitar					/system/media/audio/ringtones/SitarVsSitar.ogg
# Solarium					/system/media/audio/ringtones/Solarium.ogg
# Springy Jalopy					/system/media/audio/ringtones/SpringyJalopy.ogg
# Steppin' Out					/system/media/audio/ringtones/Steppin_Out.ogg
# Terminated					/system/media/audio/ringtones/Terminated.ogg
# Terrible Twos					/system/media/audio/ringtones/Noises2.ogg
# Testudo					/system/media/audio/ringtones/Testudo.ogg
# Themos					/system/media/audio/ringtones/Themos.ogg
# Third Eye					/system/media/audio/ringtones/Third_Eye.ogg
# Thriller Three					/system/media/audio/ringtones/Noises3.ogg
# Thunderfoot					/system/media/audio/ringtones/Thunderfoot.ogg
# Twirl Away					/system/media/audio/ringtones/TwirlAway.ogg
# Ursa Minor					/system/media/audio/ringtones/URSAMINOR.ogg
# UrsaMinor					/system/media/audio/ringtones/UrsaMinor.ogg
# Very Alarmed					/system/media/audio/ringtones/VeryAlarmed.ogg
# Vespa					/system/media/audio/ringtones/Vespa.ogg
# World					/system/media/audio/ringtones/World.ogg
# Zeta					/system/media/audio/ringtones/Zeta.ogg
# bellcore-dr1					/system/media/audio/ringtones/bellcore-dr1.ogg
# bellcore-dr2					/system/media/audio/ringtones/bellcore-dr2.ogg
# bellcore-dr3					/system/media/audio/ringtones/bellcore-dr3.ogg
# bellcore-dr4					/system/media/audio/ringtones/bellcore-dr4.ogg
# bellcore-dr5					/system/media/audio/ringtones/bellcore-dr5.ogg
# speaker					/system/media/audio/ringtones/speaker.wav

#######################################################################
##  Account 2 Advanced Settings                                      ##
#######################################################################
# Check Domain Certificates. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P2411 = 0

# Validate Certificate Chain. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P2467 = 0

# Validate Incoming SIP Messages. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P2406 = 0

# Allow Unsolicited REFER. 0 - Disabled, 1 - Enabled, 2 - Enabled/Force Auth. Default value is 0.
# Number: 0, 1, 2
P26123 = 0

# Only Accept SIP Requests from Known Servers. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P2447 = 0

# Check SIP User ID for Incoming INVITE. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P449 = 0

# Allow SIP Reset. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P26115 = 0

# Authenticate Incoming INVITE. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P2446 = 0

# SIP Realm Used for Challenge INVITE & NOTIFY.
# String
P26121 =

# Enable Local MOH
# Number: 0, 1
P2457 = 0

# Virtual Account Group. -1 - Default,  0 - Virtual Account Group 1, 1 - Virtual Account Group 2, 2 - Virtual Account Group 3
# 3 - Virtual Account Group 4, 4 - Virtual Account Group 5, 5 - Virtual Account Group 6, 6 - Virtual Account Group 7, 7 - Virtual Account Group 8
# 8 - Virtual Account Group 9, 9 - Virtual Account Group 10, 10 - Virtual Account Group 11, 11 - Virtual Account Group 12, 12 - Virtual Account Group 13
# 13 - Virtual Account Group 14, 14 - Virtual Account Group 15, 15 - Virtual Account Group 16. Default value is -1.
# Number: -1 - 15 
P2491 = -1

# Special Feature. Default value is 100
# 100 - Standard, 102 - Broadsoft, 113 - China Mobile, 114 - ZTE IMS, 115 - Mobotix
# 116 - ZTE NGN, 117 - Huawei IMS, 123 - NEC, 125 - WorldStone, 129 - Telefonica Spain
# Number: 100, 102, 113, 114, 115, 116, 117, 123, 125, 129
P424 = 100

# Feature Key Synchronization.  0 - Disable, 0 - Broadsoft/Metaswitch. Default Value is 0.
# Number: 0, 1
# P2425 = 0

# Allow Sync Phonebook via SIP Notify. 0 - No, 1 - Yes. Default is 1.
# Number: 0, 1
P26199 = 1

##############################################################################
##  Account 3 Settings                                                      ##
##############################################################################
#######################################################################
##  Account 3 General Settings                                       ##
#######################################################################
# Account Active. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P501 = 0

# Account Name
P517 =

# SIP Server
P502 =

# SIP User ID
P504 =

# SIP Authentication ID
P505 =

# SIP Authentication Password
P506 =

# Tel URI. 0 - Disable, 1 - User=Phone, 2 - Enabled. Default value is 0
# Number: 0, 1, 2
P509 = 0

#######################################################################
##  Account 3 Network Settings                                       ##
#######################################################################
# Outbound Proxy
P503 =

# Secondary Outbound Proxy
P2533 =

# DNS Mode.  0 - A Record, 1 - SRV, 2 - NAPTR/SRV. Default value is 0
# Number: 0, 1, 2
P508 = 0

# DNS SRV Fail-over Mode. 0 - Default, 1 - Saved one until DNS TTL, 2 - Saved one until no response. Defualt value is 1
# Number
P26240 = 0

# Register Before DNS SRV Fail-over. 0 - No, 1 - Yes. Default Value is 0.
# Number: 0, 1
P29295 = 1

# NAT Traversal. 0 - NAT No, 1 - STUN, 2 - Keep-alive, 3 - UPnP, 4 - Auto, 5 - VPN. Default value is 2
# Number: 0, 1, 2, 3, 4, 5
P514 = 2

# Proxy-Require
P518 =

#######################################################################
##  Account 3 SIP Settings                                           ##
#######################################################################
# SIP Registration. 0 - No, 1 - Yes. Default is 1
# Number: 0, 1
P510 = 1

# Unregister Before New Registration. 0 - No, 1 - All, 2 -  Instance . Default value is 0
# Number: 0, 1, 2
P511 = 2

# Register Expiration (m). In minutes. Default value is 60
# Number: 60 - 64800
P512 = 60

# Subscribe Expiration (m). In minutes. Default value is blank
# Number: 0 - 64800
P26251 = 60

# Re-register before Expiration (s). Default value is 0
# Number: 0 - 3600
P2530 = 0

# Registration Retry Wait Time (s). In seconds. Default value is 20
# Number: 20 - 3600
P571 = 20

# Add Auth Header On RE-REGISTER
# 0 - No, 1- Yes
P2559 = 1

# Enable SIP OPTIONS Keep Alive. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P2597 = 0

# SIP OPTIONS Keep Alive Interval(s). Default value is 30
# Number: 1 - 64800 
P2598 = 30

# SIP OPTIONS Keep Alive Maximum Tries. Default value is 3
# Number: 3 
P2599 = 3

# Use Privacy Header. 0 - Default, 1 - No, 2 - Yes. Default value is 0
# Number: 0, 1, 2
P2538 = 0

# Use P-Preferred-Identity Header. 0 - Default, 1 - No, 2 - Yes. Default value is 0
# Number: 0, 1, 2
P2539 = 0

# SIP Transport. 0 - UDP, 1 - TCP, 2 - TLS. Default value is 0
# Number: 0, 1, 2
P548 = 0

# Local SIP Port. Default value is 5064
# Number: 0 or 90 - 65535
P513 = 5064

# SIP URI Scheme When Using TLS
# 0 -sip, 1 - sips. Default value is 0.
# Number: 0, 1
P2529 = 0

# Use Actual Ephemeral Port in Contact with TCP/TLS
# 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P2531 = 0

# Support SIP Instance ID. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P589 = 1

# SIP T1 Timeout. RFC 3261 T1 value (RTT estimate)
# 50 - 0.5 sec, 100 - 1 sec, 200 - 2 sec. Default value is 50
# Number: 50, 100, 200
P540 = 50

# SIP T2 Interval. RFC 3261 T2 value. The maximum retransmit interval for non-INVITE requests and INVITE responses
# 200 - 2 sec, 400 - 4 sec, 800 - 8 sec. Default 400
# Number: 200, 400, 800
P541 = 400

# SIP Timer D Interval (Seconds)
# Number 0-64. Default value is 0
P2587 = 0

# Remove OBP from route. 0 - Disable, 1 - Enable. Default value is 0
# Number: 0, 1
P2505 = 0

# Enable 100rel. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P535 = 0

#######################################################################
##  Account 3 Session Timer                                          ##
#######################################################################
# Enable Session Timer/ Session Expiration(s).  In seconds. Default value is 180 seconds.
# By default,  Session Timer is Enabled.  Session Timer is disabled if the value is 0.
# Number: 0 or 90 - 64800
P534 = 180

# Min-SE (s). Default value is 90 seconds
# Number: 0 or 90 - 64800
P527 = 90

# UAC Specify Refresher. 0 - Omit, 1 - UAC, 2 - UAS. Default value is 0
# Number: 0, 1, 2
P532 = 0

# UAS Specify Refresher. 1 - UAC, 2 - UAS. Default value is 1
# Number: 1, 2
P533 = 1

# Caller Request Timer (Request for timer when calling)
# 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1.
P528 = 0

# Callee Request Timer. Request for timer when called (i.e. if remote party supports timer but did not request for one)
# 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P529 = 0

# Force Timer (Still use timer when remote party does not support timer). 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P530 = 0

# Force INVITE (Always refresh with INVITE instead of UPDATE even when remote party supports UPDATE)
# 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P531 = 0

#######################################################################
##  Account 3 Codec Settings                                         ##
#######################################################################
# Preferred Vocoder
# First codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 103 - G722.1C, 104 - G722.1, 123 - Opus. Default value is 0
# Number: 0, 2, 8, 9, 18, 98, 103, 104, 123
P551 = 0

# Second codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 103 - G722.1C, 104 - G722.1, 123 - Opus. Default value is 8
# Number: 0, 2, 8, 9, 18, 98, 103, 104, 123
P552 = 8

# Third codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 103 - G722.1C, 104 - G722.1, 123 - Opus. Default value is 9
# Number: 0, 2, 8, 9, 18, 98, 103, 104, 123
P553 = 9

# Forth codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 103 - G722.1C, 104 - G722.1, 123 - Opus. Default value is 104
# Number: 0, 2, 8, 9, 18, 98, 103, 104, 123
P554 = 104

# Fifth codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 103 - G722.1C, 104 - G722.1, 123 - Opus. Default value is 104
# Number: 0, 2, 8, 9, 18, 98, 103, 104, 123
P555 = 104

# Sixth codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 103 - G722.1C, 104 - G722.1, 123 - Opus. Default value is 104
# Number: 0, 2, 8, 9, 18, 98, 103, 104, 123
P556 = 104

# Seventh codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 103 - G722.1C, 104 - G722.1, 123 - Opus. Default value is 104
# Number: 0, 2, 8, 9, 18, 98, 103, 104, 123
P557 = 104

# Eigth codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 103 - G722.1C, 104 - G722.1, 123 - Opus. Default value is 104
# Number: 0, 2, 8, 9, 18, 98, 103, 104, 123
P558 = 104

# Codec Negotiation Priority. 0 - Caller, 1 - Callee. Default value is 1.
# Number: 0, 1
P29261 = 1

# Use First Matching Vocoder in 200OK SDP. 0 - No, 1 - Yes. The default value is 0.
# Number: 0, 1
P2548 = 0

# iLBC Frame Size. 0 - 20 ms, 1 - 30 ms. Default value is 1.
# Number: 0, 1
P595 = 1

# G726-32 ITU Payload. 0 - 2, 1 - Dynamic. Default value is 0.
# Number: 0, 1
P2569 = 0

# G726-32 Dynamic PT. Default value is 126.
# Number
P2565 = 126

# Opus Payload Type. Default value is 123.
P2585 = 123

# DTMF: in audio. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P2501 = 0

# DTMF: in RFC2833. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P2502 = 1

# DTMF: in SIP INFO. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P2503 = 0

# DTMF Payload Type. Default value is 101
# Number: 96 - 127
P596 = 101

# Enable Audio RED with FEC. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P26273 = 0

# Audio FEC Payload Type. Default value is 121
# Number: 96 - 126
P26274 = 121

# Audio RED Payload Type. Default value is 124
# Number: 96 - 126
P26275 = 124

# Silence Suppression. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P585 = 0

# Voice Frames per TX. Default valule is 2
# Number: 1 - 64
P586 = 2

#######################################################################
##  Account 3 RTP Settings                                           ##
#######################################################################
# SRTP Mode. 0 - Disable, 1 - Enabled but not forced, 2 - Enabled and forced. Default value is 0
# Number: 0, 1, 2
P543 = 0

# SRTP Key Length. 0 - AES 128&256 bit, 1 - AES 128 bit, 2 - AES 256 bit. Default value is 0
#Number:0, 1, 2
P2583 = 0

# Enable SRTP Key Life Time. 0 - No, 1 - Yes.
# Number: 0,1
P2563 = 1

# RTCP Destination
P2590 = 

# Symmetric RTP. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P560 = 0

# RTP IP Filter. 0 - Disable, 1 - IP Only, 2 - IP and Port. Default value is 0
# Number: 0, 1, 2
P26226 = 0

#######################################################################
##  Account 3 Call Settings                                          ##
#######################################################################
# Play warning tone for Auto Answer Intercom. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P26272 = 1

# Send Anonymous. 0 - No, 1 - Yes (caller ID will be blocked if set to Yes). Default value is 0
# Number: 0, 1
P521 = 0

# Intercept Anonymous Calls. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P546 = 0

# Call Log. 0 - Log All, 1 - Log Incoming/Outgoing only (Missed Calls Not Recorded), 2 - Disable Call All. Default value is 0
# Number: 0, 1
P542 = 0

# Ring Timeout. Default value is 60 seconds
# Number: 0 - 300
P576 = 60

# Refer-To Use Target Contact. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P569 = 0

# Incoming Call Rules. 0 - Block, 1 - Set Password, 2 - Auto Answer, 3 - Ringing, 4 - Disable. Default value is 4.
# Number: 0, 1, 2 ,3 ,4
P60244 = 4

# Set Password Rules. 
# Numbers
P60245

# Dial Plan Prefix
# String
P519 =

# Disable DialPlan. 0 - No Selection, 1 - Dial Page, 2 - Contact, 4 - Incoming Call History, 8 -  Outgoing Call History, 16 - MPK & Click2Dial. 
# If need to check multiple selections, add the specific values for each selections together. Default value is 0
# Number: 0-31
P2582 = 0

# Dial Plan. Default value is { x+ | \+x+ | *x+ | *xx*x+ }
P559 = { x+ | \+x+ | *x+ | *xx*x+ }

# Account Ringtone. See ring tone options and value in the Ring Tone Value Table below.
P523 = content://settings/system/ringtone

# Ignore Alert-Info Header. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1
P26218 = 0

# Matching Incoming Caller ID. Matching Rule 1.
# String
P1500 =

# Matching Rule 1 Distinctive Ringtone. See ring tone options and value in the Ring Tone Value Table below.
# String
P1501 = content://settings/system/ringtone

# Matching Incoming Caller ID. Matching Rule 2.
# String
P1502 =

# Matching Rule 2 Distinctive Ringtone. See ring tone options and value in the Ring Tone Value Table below.
# String
P1503 = content://settings/system/ringtone

# Matching Incoming Caller ID. Matching Rule 3.
# String
P1504 =

# Matching Rule 3 Distinctive Ringtone. See ring tone options and value in the Ring Tone Value Table below.
# String
P1505 = content://settings/system/ringtone

############Ring Tone Value Table###############
# Web GUI Option                            Value
# Use System Ring tone                      content://settings/system/ringtone 
# Andromeda					/system/media/audio/ringtones/ANDROMEDA.ogg
# Aquila					/system/media/audio/ringtones/Aquila.ogg
# Argo Navis					/system/media/audio/ringtones/ArgoNavis.ogg
# Atria					/system/media/audio/ringtones/Atria.ogg
# Backroad					/system/media/audio/ringtones/Backroad.ogg
# Beat Plucker					/system/media/audio/ringtones/BeatPlucker.ogg
# Bell Phone					/system/media/audio/ringtones/Ring_Classic_02.ogg
# Bentley Dubs					/system/media/audio/ringtones/BentleyDubs.ogg
# Big Easy					/system/media/audio/ringtones/Big_Easy.ogg
# Bird Loop					/system/media/audio/ringtones/BirdLoop.ogg
# Bollywood					/system/media/audio/ringtones/Bollywood.ogg
# Boötes					/system/media/audio/ringtones/BOOTES.ogg
# Bus' a Move					/system/media/audio/ringtones/BussaMove.ogg
# Cairo					/system/media/audio/ringtones/Cairo.ogg
# Calypso Steel					/system/media/audio/ringtones/Calypso_Steel.ogg
# Canis Major					/system/media/audio/ringtones/CANISMAJOR.ogg
# Caribbean Ice					/system/media/audio/ringtones/CaribbeanIce.ogg
# Carina					/system/media/audio/ringtones/Carina.ogg
# Cassiopeia					/system/media/audio/ringtones/CASSIOPEIA.ogg
# Centaurus					/system/media/audio/ringtones/Centaurus.ogg
# Champagne Edition					/system/media/audio/ringtones/Champagne_Edition.ogg
# Chimey Phone					/system/media/audio/ringtones/Ring_Synth_02.ogg
# Club Cubano					/system/media/audio/ringtones/Club_Cubano.ogg
# Crayon Rock					/system/media/audio/ringtones/CrayonRock.ogg
# Crazy Dream					/system/media/audio/ringtones/CrazyDream.ogg
# Curve Ball Blend					/system/media/audio/ringtones/CurveBall.ogg
# Cygnus					/system/media/audio/ringtones/Cygnus.ogg
# Dancin' Fool					/system/media/audio/ringtones/DancinFool.ogg
# Digital Phone					/system/media/audio/ringtones/Ring_Digital_02.ogg
# Ding					/system/media/audio/ringtones/Ding.ogg
# DingDong					/system/media/audio/ringtones/DingDong.wav
# Don' Mess Wiv It					/system/media/audio/ringtones/DonMessWivIt.ogg
# Draco					/system/media/audio/ringtones/Draco.ogg
# Dream Theme					/system/media/audio/ringtones/DreamTheme.ogg
# Eastern Sky					/system/media/audio/ringtones/Eastern_Sky.ogg
# Enter the Nexus					/system/media/audio/ringtones/Enter_the_Nexus.ogg
# Eridani					/system/media/audio/ringtones/Eridani.ogg
# Ether Shake					/system/media/audio/ringtones/EtherShake.ogg
# Flutey Phone					/system/media/audio/ringtones/Ring_Synth_04.ogg
# Free Flight					/system/media/audio/ringtones/FreeFlight.ogg
# Friendly Ghost					/system/media/audio/ringtones/FriendlyGhost.ogg
# Funk Y'all					/system/media/audio/ringtones/Funk_Yall.ogg
# Game Over Guitar					/system/media/audio/ringtones/GameOverGuitar.ogg
# Gimme Mo' Town					/system/media/audio/ringtones/Gimme_Mo_Town.ogg
# Girtab					/system/media/audio/ringtones/Girtab.ogg
# Glacial Groove					/system/media/audio/ringtones/Glacial_Groove.ogg
# Growl					/system/media/audio/ringtones/Growl.ogg
# Halfway Home					/system/media/audio/ringtones/HalfwayHome.ogg
# Hydra					/system/media/audio/ringtones/Hydra.ogg
# Insert Coin					/system/media/audio/ringtones/InsertCoin.ogg
# Kuma					/system/media/audio/ringtones/Kuma.ogg
# Loopy Lounge					/system/media/audio/ringtones/LoopyLounge.ogg
# Love Flute					/system/media/audio/ringtones/LoveFlute.ogg
# Lyra					/system/media/audio/ringtones/Lyra.ogg
# Machina					/system/media/audio/ringtones/Machina.ogg
# Medieval Jaunt					/system/media/audio/ringtones/MidEvilJaunt.ogg
# Mildly Alarming					/system/media/audio/ringtones/MildlyAlarming.ogg
# Nairobi					/system/media/audio/ringtones/Nairobi.ogg
# Nassau					/system/media/audio/ringtones/Nassau.ogg
# New Player					/system/media/audio/ringtones/NewPlayer.ogg
# No Limits					/system/media/audio/ringtones/No_Limits.ogg
# Noisey One					/system/media/audio/ringtones/Noises1.ogg
# Organ Dub					/system/media/audio/ringtones/OrganDub.ogg
# Orion					/system/media/audio/ringtones/Orion.ogg
# Paradise Island					/system/media/audio/ringtones/Paradise_Island.ogg
# Pegasus					/system/media/audio/ringtones/Pegasus.ogg
# Perseus					/system/media/audio/ringtones/PERSEUS.ogg
# Playa					/system/media/audio/ringtones/Playa.ogg
# Pyxis					/system/media/audio/ringtones/Pyxis.ogg
# Rasalas					/system/media/audio/ringtones/Rasalas.ogg
# Revelation					/system/media/audio/ringtones/Revelation.ogg
# Rigel					/system/media/audio/ringtones/Rigel.ogg
# Road Trip					/system/media/audio/ringtones/Road_Trip.ogg
# Romancing The Tone					/system/media/audio/ringtones/RomancingTheTone.ogg
# Safari					/system/media/audio/ringtones/Safari.ogg
# Savannah					/system/media/audio/ringtones/Savannah.ogg
# Scarabaeus					/system/media/audio/ringtones/Scarabaeus.ogg
# Sceptrum					/system/media/audio/ringtones/Sceptrum.ogg
# Seville					/system/media/audio/ringtones/Seville.ogg
# She's All That					/system/media/audio/ringtones/Shes_All_That.ogg
# Silky Way					/system/media/audio/ringtones/SilkyWay.ogg
# Sitar Versus Sitar					/system/media/audio/ringtones/SitarVsSitar.ogg
# Solarium					/system/media/audio/ringtones/Solarium.ogg
# Springy Jalopy					/system/media/audio/ringtones/SpringyJalopy.ogg
# Steppin' Out					/system/media/audio/ringtones/Steppin_Out.ogg
# Terminated					/system/media/audio/ringtones/Terminated.ogg
# Terrible Twos					/system/media/audio/ringtones/Noises2.ogg
# Testudo					/system/media/audio/ringtones/Testudo.ogg
# Themos					/system/media/audio/ringtones/Themos.ogg
# Third Eye					/system/media/audio/ringtones/Third_Eye.ogg
# Thriller Three					/system/media/audio/ringtones/Noises3.ogg
# Thunderfoot					/system/media/audio/ringtones/Thunderfoot.ogg
# Twirl Away					/system/media/audio/ringtones/TwirlAway.ogg
# Ursa Minor					/system/media/audio/ringtones/URSAMINOR.ogg
# UrsaMinor					/system/media/audio/ringtones/UrsaMinor.ogg
# Very Alarmed					/system/media/audio/ringtones/VeryAlarmed.ogg
# Vespa					/system/media/audio/ringtones/Vespa.ogg
# World					/system/media/audio/ringtones/World.ogg
# Zeta					/system/media/audio/ringtones/Zeta.ogg
# bellcore-dr1					/system/media/audio/ringtones/bellcore-dr1.ogg
# bellcore-dr2					/system/media/audio/ringtones/bellcore-dr2.ogg
# bellcore-dr3					/system/media/audio/ringtones/bellcore-dr3.ogg
# bellcore-dr4					/system/media/audio/ringtones/bellcore-dr4.ogg
# bellcore-dr5					/system/media/audio/ringtones/bellcore-dr5.ogg
# speaker					/system/media/audio/ringtones/speaker.wav

#######################################################################
##  Account 3 Advanced Settings                                      ##
#######################################################################
# Check Domain Certificates. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P2511 = 0

# Validate Certificate Chain. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P2567 = 0

# Validate Incoming SIP Messages. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P2506 = 0

# Allow Unsolicited REFER. 0 - Disabled, 1 - Enabled, 2 - Enabled/Force Auth. Default value is 0.
# Number: 0, 1, 2
P26223 = 0

# Only Accept SIP Requests from Known Servers. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P2547 = 0

# Check SIP User ID for Incoming INVITE. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P549 = 0

# Allow SIP Reset. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P26215 = 0

# Authenticate Incoming INVITE. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P2546 = 0

# SIP Realm Used for Challenge INVITE & NOTIFY.
# String
P26221 =

# Enable Local MOH
# Number: 0, 1 
P2557 = 0

# Virtual Account Group. -1 - Default,  0 - Virtual Account Group 1, 1 - Virtual Account Group 2, 2 - Virtual Account Group 3
# 3 - Virtual Account Group 4, 4 - Virtual Account Group 5, 5 - Virtual Account Group 6, 6 - Virtual Account Group 7, 7 - Virtual Account Group 8
# 8 - Virtual Account Group 9, 9 - Virtual Account Group 10, 10 - Virtual Account Group 11, 11 - Virtual Account Group 12, 12 - Virtual Account Group 13
# 13 - Virtual Account Group 14, 14 - Virtual Account Group 15, 15 - Virtual Account Group 16. Default value is -1.
# Number: -1 - 15 
P2591 = -1

# Special Feature. Default value is 100
# 100 - Standard, 102 - Broadsoft, 113 - China Mobile, 114 - ZTE IMS, 115 - Mobotix
# 116 - ZTE NGN, 117 - Huawei IMS, 123 - NEC, 125 - WorldStone, 129 - Telefonica Spain
# Number: 100, 102, 113, 114, 115, 116, 117, 123, 125, 129
P524 = 100

# Feature Key Synchronization.  0 - Disable, 0 - Broadsoft/Metaswitch. Default Value is 0.
# Number: 0, 1
# P2525 = 0

# Allow Sync Phonebook via SIP Notify. 0 - No, 1 - Yes. Default is 1.
# Number: 0, 1
P26299 = 1

##############################################################################
##  Account 4 Settings                                                      ##
##############################################################################
#######################################################################
##  Account 4 General Settings                                       ##
#######################################################################
# Account Active. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P601 = 0

# Account Name
P617 =

# SIP Server
P602 =

# SIP User ID
P604 =

# SIP Authentication ID
P605 =

# SIP Authentication Password
P606 =

# Tel URI. 0 - Disable, 1 - User=Phone, 2 - Enabled. Default value is 0
# Number: 0, 1, 2
P609 = 0

#######################################################################
##  Account 4 Network Settings                                       ##
#######################################################################
# Outbound Proxy
P603 =

# Secondary Outbound Proxy
P2633 =

# DNS Mode.  0 - A Record, 1 - SRV, 2 - NAPTR/SRV. Default value is 0
# Number: 0, 1, 2
P608 = 0

# DNS SRV Fail-over Mode. 0 - Default, 1 - Saved one until DNS TTL, 2 - Saved one until no response. Defualt value is 1
# Number
P26340 = 0

# Register Before DNS SRV Fail-over. 0 - No, 1 - Yes. Default Value is 0.
# Number: 0, 1
P29395 = 1

# NAT Traversal. 0 - NAT No, 1 - STUN, 2 - Keep-alive, 3 - UPnP, 4 - Auto, 5 - VPN. Default value is 2
# Number: 0, 1, 2, 3, 4, 5
P614 = 2

# Proxy-Require
P618 =

#######################################################################
##  Account 4 SIP Settings                                           ##
#######################################################################
# SIP Registration. 0 - No, 1 - Yes. Default is 1
# Number: 0, 1
P610 = 1

# Unregister Before New Registration. 0 - No, 1 - All, 2 -  Instance . Default value is 0
# Number: 0, 1, 2
P611 = 2

# Register Expiration (m). In minutes. Default value is 60
# Number: 60 - 64800
P612 = 60

# Subscribe Expiration (m). In minutes. Default value is blank
# Number: 0 - 64800
P26351 = 60

# Re-register before Expiration (s). Default value is 0
# Number: 0 - 3600
P2630 = 0

# Registration Retry Wait Time (s). In seconds. Default value is 20
# Number: 20 - 3600
P671 = 20

# Add Auth Header On RE-REGISTER
# 0 - No, 1- Yes
P2659 = 1

# Enable SIP OPTIONS Keep Alive. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P2697 = 0

# SIP OPTIONS Keep Alive Interval(s). Default value is 30
# Number: 1 - 64800 
P2698 = 30

# SIP OPTIONS Keep Alive Maximum Tries. Default value is 3
# Number: 3 
P2699 = 3

# Use Privacy Header. 0 - Default, 1 - No, 2 - Yes. Default value is 0
# Number: 0, 1, 2
P2638 = 0

# Use P-Preferred-Identity Header. 0 - Default, 1 - No, 2 - Yes. Default value is 0
# Number: 0, 1, 2
P2639 = 0

# SIP Transport. 0 - UDP, 1 - TCP, 2 - TLS. Default value is 0
# Number: 0, 1, 2
P648 = 0

# Local SIP Port. Default value is 5066
# Number: 0 or 90 - 65535
P613 = 5066

# SIP URI Scheme When Using TLS
# 0 -sip, 1 - sips. Default value is 0.
# Number: 0, 1
P2629 = 0

# Use Actual Ephemeral Port in Contact with TCP/TLS
# 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P2631 = 0

# Support SIP Instance ID. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P689 = 1

# SIP T1 Timeout. RFC 3261 T1 value (RTT estimate)
# 50 - 0.5 sec, 100 - 1 sec, 200 - 2 sec. Default value is 50
# Number: 50, 100, 200
P640 = 50

# SIP T2 Interval. RFC 3261 T2 value. The maximum retransmit interval for non-INVITE requests and INVITE responses
# 200 - 2 sec, 400 - 4 sec, 800 - 8 sec. Default 400
# Number: 200, 400, 800
P641 = 400

# SIP Timer D Interval (Seconds)
# Number 0-64. Default value is 0
P2687 = 0

# Remove OBP from route. 0 - Disable, 1 - Enable. Default value is 0
# Number: 0, 1
P2605 = 0

# Enable 100rel. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P635 = 0

#######################################################################
##  Account 4 Session Timer                                          ##
#######################################################################

# Enable Session Timer/ Session Expiration(s).  In seconds. Default value is 180 seconds.
# By default,  Session Timer is Enabled.  Session Timer is disabled if the value is 0.
# Number: 0 or 90 - 64800
P634 = 180

# Min-SE (s). Default value is 90 seconds
# Number: 0 or 90 - 64800
P627 = 90

# UAC Specify Refresher. 0 - Omit, 1 - UAC, 2 - UAS. Default value is 0
# Number: 0, 1, 2
P632 = 0

# UAS Specify Refresher. 1 - UAC, 2 - UAS. Default value is 1
# Number: 1, 2
P633 = 1

# Caller Request Timer (Request for timer when calling)
# 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1.
P628 = 0

# Callee Request Timer. Request for timer when called (i.e. if remote party supports timer but did not request for one)
# 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P629 = 0

# Force Timer (Still use timer when remote party does not support timer). 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P630 = 0

# Force INVITE (Always refresh with INVITE instead of UPDATE even when remote party supports UPDATE)
# 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P631 = 0

#######################################################################
##  Account 4 Codec Settings                                         ##
#######################################################################
# Preferred Vocoder
# First codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 103 - G722.1C, 104 - G722.1, 123 - Opus. Default value is 0
# Number: 0, 2, 8, 9, 18, 98, 103, 104, 123
P651 = 0

# Second codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 103 - G722.1C, 104 - G722.1, 123 - Opus. Default value is 8
# Number: 0, 2, 8, 9, 18, 98, 103, 104, 123
P652 = 8

# Third codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 103 - G722.1C, 104 - G722.1, 123 - Opus. Default value is 9
# Number: 0, 2, 8, 9, 18, 98, 103, 104, 123
P653 = 9

# Forth codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 103 - G722.1C, 104 - G722.1, 123 - Opus. Default value is 104
# Number: 0, 2, 8, 9, 18, 98, 103, 104, 123
P654 = 104

# Fifth codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 103 - G722.1C, 104 - G722.1, 123 - Opus. Default value is 104
# Number: 0, 2, 8, 9, 18, 98, 103, 104, 123
P655 = 104

# Sixth codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 103 - G722.1C, 104 - G722.1, 123 - Opus. Default value is 104
# Number: 0, 2, 8, 9, 18, 98, 103, 104, 123
P656 = 104

# Seventh codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 103 - G722.1C, 104 - G722.1, 123 - Opus. Default value is 104
# Number: 0, 2, 8, 9, 18, 98, 103, 104, 123
P657 = 104

# Eigth codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 103 - G722.1C, 104 - G722.1, 123 - Opus. Default value is 104
# Number: 0, 2, 8, 9, 18, 98, 103, 104, 123
P658 = 104

# Codec Negotiation Priority. 0 - Caller, 1 - Callee. Default value is 1.
# Number: 0, 1
P29361 = 1

# Use First Matching Vocoder in 200OK SDP. 0 - No, 1 - Yes. The default value is 0.
# Number: 0, 1
P2648 = 0

# iLBC Frame Size. 0 - 20 ms, 1 - 30 ms. Default value is 1.
# Number: 0, 1
P695 = 1

# G726-32 ITU Payload. 0 - 2, 1 - Dynamic. Default value is 0.
# Number: 0, 1
P2669 = 0

# G726-32 Dynamic PT. Default value is 126.
# Number
P2665 = 126

# Opus Payload Type. Default value is 123.
P2685 = 123

# DTMF: in audio. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P2601 = 0

# DTMF: in RFC2833. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P2602 = 1

# DTMF: in SIP INFO. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P2603 = 0

# DTMF Payload Type. Default value is 101
# Number: 96 - 127
P696 = 101

# Enable Audio RED with FEC. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P26373 = 0

# Audio FEC Payload Type. Default value is 121
# Number: 96 - 126
P26374 = 121

# Audio RED Payload Type. Default value is 124
# Number: 96 - 126
P26375 = 124

# Silence Suppression. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P685 = 0

# Voice Frames per TX. Default valule is 2
# Number: 1 - 64
P686 = 2

#######################################################################
##  Account 4 RTP Settings                                           ##
#######################################################################
# SRTP Mode. 0 - Disable, 1 - Enabled but not forced, 2 - Enabled and forced. Default value is 0
# Number: 0, 1, 2
P643 = 0

# SRTP Key Length. 0 - AES 128&256 bit, 1 - AES 128 bit, 2 - AES 256 bit. Default value is 0
#Number:0, 1, 2
P2683 = 0

# Enable SRTP Key Life Time. 0 - No, 1 - Yes.
# Number: 0,1
P2663 = 1

# RTCP Destination
P2690 = 

# Symmetric RTP. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P660 = 0

# RTP IP Filter. 0 - Disable, 1 - IP Only, 2 - IP and Port. Default value is 0
# Number: 0, 1, 2
P26326 = 0

#######################################################################
##  Account 4 Call Settings                                          ##
#######################################################################
# Play warning tone for Auto Answer Intercom. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P26372 = 1

# Send Anonymous. 0 - No, 1 - Yes (caller ID will be blocked if set to Yes). Default value is 0
# Number: 0, 1
P621 = 0

# Intercept Anonymous Calls. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P646 = 0

# Call Log. 0 - Log All, 1 - Log Incoming/Outgoing only (Missed Calls Not Recorded), 2 - Disable Call All. Default value is 0
# Number: 0, 1
P642 = 0

# Ring Timeout. Default value is 60 seconds
# Number: 0 - 300
P676 = 60

# Refer-To Use Target Contact. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P669 = 0

# Incoming Call Rules. 0 - Block, 1 - Set Password, 2 - Auto Answer, 3 - Ringing, 4 - Disable. Default value is 4.
# Number: 0, 1, 2 ,3 ,4
P60344 = 4

# Set Password Rules. 
# Numbers
P60345

# Dial Plan Prefix
# String
P619 =

# Disable DialPlan. 0 - No Selection, 1 - Dial Page, 2 - Contact, 4 - Incoming Call History, 8 -  Outgoing Call History, 16 - MPK & Click2Dial. 
# If need to check multiple selections, add the specific values for each selections together. Default value is 0
# Number: 0-31
P2682 = 0

# Dial Plan. Default value is { x+ | \+x+ | *x+ | *xx*x+ }
P659 = { x+ | \+x+ | *x+ | *xx*x+ }

# Account Ringtone. See ring tone options and value in the Ring Tone Value Table below.
P623 = content://settings/system/ringtone

# Ignore Alert-Info Header. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1
P26318 = 0

# Matching Incoming Caller ID. Matching Rule 1.
# String
P1506 =

# Matching Rule 1 Distinctive Ringtone. See ring tone options and value in the Ring Tone Value Table below.
# String
P1507 = content://settings/system/ringtone

# Matching Incoming Caller ID. Matching Rule 2.
# String
P1508 =

# Matching Rule 2 Distinctive Ringtone. See ring tone options and value in the Ring Tone Value Table below.
# String
P1509 = content://settings/system/ringtone

# Matching Incoming Caller ID. Matching Rule 3.
# String
P1510 =

# Matching Rule 3 Distinctive Ringtone. See ring tone options and value in the Ring Tone Value Table below.
# String
P1511 = content://settings/system/ringtone

############Ring Tone Value Table###############
# Web GUI Option                            Value
# Use System Ring tone                      content://settings/system/ringtone 
# Andromeda					/system/media/audio/ringtones/ANDROMEDA.ogg
# Aquila					/system/media/audio/ringtones/Aquila.ogg
# Argo Navis					/system/media/audio/ringtones/ArgoNavis.ogg
# Atria					/system/media/audio/ringtones/Atria.ogg
# Backroad					/system/media/audio/ringtones/Backroad.ogg
# Beat Plucker					/system/media/audio/ringtones/BeatPlucker.ogg
# Bell Phone					/system/media/audio/ringtones/Ring_Classic_02.ogg
# Bentley Dubs					/system/media/audio/ringtones/BentleyDubs.ogg
# Big Easy					/system/media/audio/ringtones/Big_Easy.ogg
# Bird Loop					/system/media/audio/ringtones/BirdLoop.ogg
# Bollywood					/system/media/audio/ringtones/Bollywood.ogg
# Boötes					/system/media/audio/ringtones/BOOTES.ogg
# Bus' a Move					/system/media/audio/ringtones/BussaMove.ogg
# Cairo					/system/media/audio/ringtones/Cairo.ogg
# Calypso Steel					/system/media/audio/ringtones/Calypso_Steel.ogg
# Canis Major					/system/media/audio/ringtones/CANISMAJOR.ogg
# Caribbean Ice					/system/media/audio/ringtones/CaribbeanIce.ogg
# Carina					/system/media/audio/ringtones/Carina.ogg
# Cassiopeia					/system/media/audio/ringtones/CASSIOPEIA.ogg
# Centaurus					/system/media/audio/ringtones/Centaurus.ogg
# Champagne Edition					/system/media/audio/ringtones/Champagne_Edition.ogg
# Chimey Phone					/system/media/audio/ringtones/Ring_Synth_02.ogg
# Club Cubano					/system/media/audio/ringtones/Club_Cubano.ogg
# Crayon Rock					/system/media/audio/ringtones/CrayonRock.ogg
# Crazy Dream					/system/media/audio/ringtones/CrazyDream.ogg
# Curve Ball Blend					/system/media/audio/ringtones/CurveBall.ogg
# Cygnus					/system/media/audio/ringtones/Cygnus.ogg
# Dancin' Fool					/system/media/audio/ringtones/DancinFool.ogg
# Digital Phone					/system/media/audio/ringtones/Ring_Digital_02.ogg
# Ding					/system/media/audio/ringtones/Ding.ogg
# DingDong					/system/media/audio/ringtones/DingDong.wav
# Don' Mess Wiv It					/system/media/audio/ringtones/DonMessWivIt.ogg
# Draco					/system/media/audio/ringtones/Draco.ogg
# Dream Theme					/system/media/audio/ringtones/DreamTheme.ogg
# Eastern Sky					/system/media/audio/ringtones/Eastern_Sky.ogg
# Enter the Nexus					/system/media/audio/ringtones/Enter_the_Nexus.ogg
# Eridani					/system/media/audio/ringtones/Eridani.ogg
# Ether Shake					/system/media/audio/ringtones/EtherShake.ogg
# Flutey Phone					/system/media/audio/ringtones/Ring_Synth_04.ogg
# Free Flight					/system/media/audio/ringtones/FreeFlight.ogg
# Friendly Ghost					/system/media/audio/ringtones/FriendlyGhost.ogg
# Funk Y'all					/system/media/audio/ringtones/Funk_Yall.ogg
# Game Over Guitar					/system/media/audio/ringtones/GameOverGuitar.ogg
# Gimme Mo' Town					/system/media/audio/ringtones/Gimme_Mo_Town.ogg
# Girtab					/system/media/audio/ringtones/Girtab.ogg
# Glacial Groove					/system/media/audio/ringtones/Glacial_Groove.ogg
# Growl					/system/media/audio/ringtones/Growl.ogg
# Halfway Home					/system/media/audio/ringtones/HalfwayHome.ogg
# Hydra					/system/media/audio/ringtones/Hydra.ogg
# Insert Coin					/system/media/audio/ringtones/InsertCoin.ogg
# Kuma					/system/media/audio/ringtones/Kuma.ogg
# Loopy Lounge					/system/media/audio/ringtones/LoopyLounge.ogg
# Love Flute					/system/media/audio/ringtones/LoveFlute.ogg
# Lyra					/system/media/audio/ringtones/Lyra.ogg
# Machina					/system/media/audio/ringtones/Machina.ogg
# Medieval Jaunt					/system/media/audio/ringtones/MidEvilJaunt.ogg
# Mildly Alarming					/system/media/audio/ringtones/MildlyAlarming.ogg
# Nairobi					/system/media/audio/ringtones/Nairobi.ogg
# Nassau					/system/media/audio/ringtones/Nassau.ogg
# New Player					/system/media/audio/ringtones/NewPlayer.ogg
# No Limits					/system/media/audio/ringtones/No_Limits.ogg
# Noisey One					/system/media/audio/ringtones/Noises1.ogg
# Organ Dub					/system/media/audio/ringtones/OrganDub.ogg
# Orion					/system/media/audio/ringtones/Orion.ogg
# Paradise Island					/system/media/audio/ringtones/Paradise_Island.ogg
# Pegasus					/system/media/audio/ringtones/Pegasus.ogg
# Perseus					/system/media/audio/ringtones/PERSEUS.ogg
# Playa					/system/media/audio/ringtones/Playa.ogg
# Pyxis					/system/media/audio/ringtones/Pyxis.ogg
# Rasalas					/system/media/audio/ringtones/Rasalas.ogg
# Revelation					/system/media/audio/ringtones/Revelation.ogg
# Rigel					/system/media/audio/ringtones/Rigel.ogg
# Road Trip					/system/media/audio/ringtones/Road_Trip.ogg
# Romancing The Tone					/system/media/audio/ringtones/RomancingTheTone.ogg
# Safari					/system/media/audio/ringtones/Safari.ogg
# Savannah					/system/media/audio/ringtones/Savannah.ogg
# Scarabaeus					/system/media/audio/ringtones/Scarabaeus.ogg
# Sceptrum					/system/media/audio/ringtones/Sceptrum.ogg
# Seville					/system/media/audio/ringtones/Seville.ogg
# She's All That					/system/media/audio/ringtones/Shes_All_That.ogg
# Silky Way					/system/media/audio/ringtones/SilkyWay.ogg
# Sitar Versus Sitar					/system/media/audio/ringtones/SitarVsSitar.ogg
# Solarium					/system/media/audio/ringtones/Solarium.ogg
# Springy Jalopy					/system/media/audio/ringtones/SpringyJalopy.ogg
# Steppin' Out					/system/media/audio/ringtones/Steppin_Out.ogg
# Terminated					/system/media/audio/ringtones/Terminated.ogg
# Terrible Twos					/system/media/audio/ringtones/Noises2.ogg
# Testudo					/system/media/audio/ringtones/Testudo.ogg
# Themos					/system/media/audio/ringtones/Themos.ogg
# Third Eye					/system/media/audio/ringtones/Third_Eye.ogg
# Thriller Three					/system/media/audio/ringtones/Noises3.ogg
# Thunderfoot					/system/media/audio/ringtones/Thunderfoot.ogg
# Twirl Away					/system/media/audio/ringtones/TwirlAway.ogg
# Ursa Minor					/system/media/audio/ringtones/URSAMINOR.ogg
# UrsaMinor					/system/media/audio/ringtones/UrsaMinor.ogg
# Very Alarmed					/system/media/audio/ringtones/VeryAlarmed.ogg
# Vespa					/system/media/audio/ringtones/Vespa.ogg
# World					/system/media/audio/ringtones/World.ogg
# Zeta					/system/media/audio/ringtones/Zeta.ogg
# bellcore-dr1					/system/media/audio/ringtones/bellcore-dr1.ogg
# bellcore-dr2					/system/media/audio/ringtones/bellcore-dr2.ogg
# bellcore-dr3					/system/media/audio/ringtones/bellcore-dr3.ogg
# bellcore-dr4					/system/media/audio/ringtones/bellcore-dr4.ogg
# bellcore-dr5					/system/media/audio/ringtones/bellcore-dr5.ogg
# speaker					/system/media/audio/ringtones/speaker.wav

#######################################################################
##  Account 4 Advanced Settings                                      ##
#######################################################################
# Check Domain Certificates. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P2611 = 0

# Validate Certificate Chain. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P2667 = 0

# Validate Incoming SIP Messages. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P2606 = 0

# Allow Unsolicited REFER. 0 - Disabled, 1 - Enabled, 2 - Enabled/Force Auth. Default value is 0.
# Number: 0, 1, 2
P26323 = 0

# Only Accept SIP Requests from Known Servers. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P2647 = 0

# Check SIP User ID for Incoming INVITE. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P649 = 0

# Allow SIP Reset. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P26315 = 0

# Authenticate Incoming INVITE. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P2646 = 0

# SIP Realm Used for Challenge INVITE & NOTIFY.
# String
P26321 =

# Enable Local MOH
# Number: 0, 1 
P2657 = 0

# Virtual Account Group. -1 - Default,  0 - Virtual Account Group 1, 1 - Virtual Account Group 2, 2 - Virtual Account Group 3
# 3 - Virtual Account Group 4, 4 - Virtual Account Group 5, 5 - Virtual Account Group 6, 6 - Virtual Account Group 7, 7 - Virtual Account Group 8
# 8 - Virtual Account Group 9, 9 - Virtual Account Group 10, 10 - Virtual Account Group 11, 11 - Virtual Account Group 12, 12 - Virtual Account Group 13
# 13 - Virtual Account Group 14, 14 - Virtual Account Group 15, 15 - Virtual Account Group 16. Default value is -1.
# Number: -1 - 15 
P2691 = -1

# Special Feature. Default value is 100
# 100 - Standard, 102 - Broadsoft, 113 - China Mobile, 114 - ZTE IMS, 115 - Mobotix
# 116 - ZTE NGN, 117 - Huawei IMS, 123 - NEC, 125 - WorldStone, 129 - Telefonica Spain
# Number: 100, 102, 113, 114, 115, 116, 117, 123, 125, 129
P624 = 100

# Feature Key Synchronization.  0 - Disable, 0 - Broadsoft/Metaswitch. Default Value is 0.
# Number: 0, 1
# P2625 = 0

# Allow Sync Phonebook via SIP Notify. 0 - No, 1 - Yes. Default is 1.
# Number: 0, 1
P26399 = 1

##############################################################################
##  Account 5 Settings                                                      ##
##############################################################################
#######################################################################
##  Account 5 General Settings                                       ##
#######################################################################
# Account Active. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P1701 = 0

# Account Name
P1717 =

# SIP Server
P1702 =

# SIP User ID
P1704 =

# SIP Authentication ID
P1705 =

# SIP Authentication Password
P1706 =

# Tel URI. 0 - Disable, 1 - User=Phone, 2 - Enabled. Default value is 0
# Number: 0, 1, 2
P1709 = 0

#######################################################################
##  Account 5 Network Settings                                       ##
#######################################################################
# Outbound Proxy
P1703 =

# Secondary Outbound Proxy
P2733 =

# DNS Mode.  0 - A Record, 1 - SRV, 2 - NAPTR/SRV. Default value is 0
# Number: 0, 1, 2
P1708 = 0

# DNS SRV Fail-over Mode. 0 - Default, 1 - Saved one until DNS TTL, 2 - Saved one until no response. Defualt value is 1
# Number
P26440 = 0

# Register Before DNS SRV Fail-over. 0 - No, 1 - Yes. Default Value is 0.
# Number: 0, 1
P29495 = 1

# NAT Traversal. 0 - NAT No, 1 - STUN, 2 - Keep-alive, 3 - UPnP, 4 - Auto, 5 - VPN. Default value is 2
# Number: 0, 1, 2, 3, 4, 5
P1714 = 2

# Proxy-Require
P1718 =

#######################################################################
##  Account 5 SIP Settings                                           ##
#######################################################################
# SIP Registration. 0 - No, 1 - Yes. Default is 1
# Number: 0, 1
P1710 = 1

# Unregister Before New Registration. 0 - No, 1 - All, 2 -  Instance . Default value is 0
# Number: 0, 1, 2
P1711 = 2

# Register Expiration (m). In minutes. Default value is 60
# Number: 60 - 64800
P1712 = 60

# Subscribe Expiration (m). In minutes. Default value is blank
# Number: 0 - 64800
P26451 = 60

# Re-register before Expiration (s). Default value is 0
# Number: 0 - 3600
P2730 = 0

# Registration Retry Wait Time (s). In seconds. Default value is 20
# Number: 20 - 3600
P1771 = 20

# Add Auth Header On RE-REGISTER
# 0 - No, 1- Yes
P2759 = 1

# Enable SIP OPTIONS Keep Alive. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P2797 = 0

# SIP OPTIONS Keep Alive Interval(s). Default value is 30
# Number: 1 - 64800
P2798 = 30

# SIP OPTIONS Keep Alive Maximum Tries. Default value is 3
# Number: 3 
P2799 = 3

# Use Privacy Header. 0 - Default, 1 - No, 2 - Yes. Default value is 0
# Number: 0, 1, 2
P2738 = 0

# Use P-Preferred-Identity Header. 0 - Default, 1 - No, 2 - Yes. Default value is 0
# Number: 0, 1, 2
P2739 = 0

# SIP Transport. 0 - UDP, 1 - TCP, 2 - TLS. Default value is 0
# Number: 0, 1, 2
P1748 = 0

# Local SIP Port. Default value is 5068
# Number: 0 or 90 - 65535
P1713 = 5068

# SIP URI Scheme When Using TLS
# 0 -sip, 1 - sips. Default value is 0.
# Number: 0, 1
P2729 = 0

# Use Actual Ephemeral Port in Contact with TCP/TLS
# 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P2731 = 0

# Support SIP Instance ID. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P1789 = 1

# SIP T1 Timeout. RFC 3261 T1 value (RTT estimate)
# 50 - 0.5 sec, 100 - 1 sec, 200 - 2 sec. Default value is 50
# Number: 50, 100, 200
P1740 = 50

# SIP T2 Interval. RFC 3261 T2 value. The maximum retransmit interval for non-INVITE requests and INVITE responses
# 200 - 2 sec, 400 - 4 sec, 800 - 8 sec. Default 400
# Number: 200, 400, 800
P1741 = 400

# SIP Timer D Interval (Seconds)
# Number 0-64. Default value is 0
P2787 = 0

# Remove OBP from route. 0 - Disable, 1 - Enable. Default value is 0
# Number: 0, 1
P2705 = 0

# Enable 100rel. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P1735 = 0

#######################################################################
##  Account 5 Session Timer                                          ##
#######################################################################

# Enable Session Timer/ Session Expiration(s).  In seconds. Default value is 180 seconds.
# By default,  Session Timer is Enabled.  Session Timer is disabled if the value is 0.
# Number: 0 or 90 - 64800
P1734 = 180

# Min-SE (s). Default value is 90 seconds
# Number: 0 or 90 - 64800
P1727 = 90

# UAC Specify Refresher. 0 - Omit, 1 - UAC, 2 - UAS. Default value is 0
# Number: 0, 1, 2
P1732 = 0

# UAS Specify Refresher. 1 - UAC, 2 - UAS. Default value is 1
# Number: 1, 2
P1733 = 1

# Caller Request Timer (Request for timer when calling)
# 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1.
P1728 = 0

# Callee Request Timer. Request for timer when called (i.e. if remote party supports timer but did not request for one)
# 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P1729 = 0

# Force Timer (Still use timer when remote party does not support timer). 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P1730 = 0

# Force INVITE (Always refresh with INVITE instead of UPDATE even when remote party supports UPDATE)
# 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P1731 = 0

#######################################################################
##  Account 5 Codec Settings                                         ##
#######################################################################
# Preferred Vocoder
# First codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 103 - G722.1C, 104 - G722.1, 123 - Opus. Default value is 0
# Number: 0, 2, 8, 9, 18, 98, 103, 104, 123
P1751 = 0

# Second codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 103 - G722.1C, 104 - G722.1, 123 - Opus. Default value is 8
# Number: 0, 2, 8, 9, 18, 98, 103, 104, 123
P1752 = 8

# Third codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 103 - G722.1C, 104 - G722.1, 123 - Opus. Default value is 9
# Number: 0, 2, 8, 9, 18, 98, 103, 104, 123
P1753 = 9

# Forth codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 103 - G722.1C, 104 - G722.1, 123 - Opus. Default value is 104
# Number: 0, 2, 8, 9, 18, 98, 103, 104, 123
P1754 = 104

# Fifth codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 103 - G722.1C, 104 - G722.1, 123 - Opus. Default value is 104
# Number: 0, 2, 8, 9, 18, 98, 103, 104, 123
P1755 = 104

# Sixth codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 103 - G722.1C, 104 - G722.1, 123 - Opus. Default value is 104
# Number: 0, 2, 8, 9, 18, 98, 103, 104, 123
P1756 = 104

# Seventh codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 103 - G722.1C, 104 - G722.1, 123 - Opus. Default value is 104
# Number: 0, 2, 8, 9, 18, 98, 103, 104, 123
P1757 = 104

# Eigth codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 103 - G722.1C, 104 - G722.1, 123 - Opus. Default value is 104
# Number: 0, 2, 8, 9, 18, 98, 103, 104, 123
P1758 = 104

# Codec Negotiation Priority. 0 - Caller, 1 - Callee. Default value is 1.
# Number: 0, 1
P29461 = 1

# Use First Matching Vocoder in 200OK SDP. 0 - No, 1 - Yes. The default value is 0.
# Number: 0, 1
P2748 = 0

# iLBC Frame Size. 0 - 20 ms, 1 - 30 ms. Default value is 1.
# Number: 0, 1
P1795 = 1

# G726-32 ITU Payload. 0 - 2, 1 - Dynamic. Default value is 0.
# Number: 0, 1
P2769 = 0

# G726-32 Dynamic PT. Default value is 126.
# Number
P2765 = 126

# Opus Payload Type. Default value is 123.
P2785 = 123

# DTMF: in audio. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P2701 = 0

# DTMF: in RFC2833. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P2702 = 1

# DTMF: in SIP INFO. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P2703 = 0

# DTMF Payload Type. Default value is 101
# Number: 96 - 127
P1796 = 101

# Enable Audio RED with FEC. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P26473 = 0

# Audio FEC Payload Type. Default value is 121
# Number: 96 - 126
P26474 = 121

# Audio RED Payload Type. Default value is 124
# Number: 96 - 126
P26475 = 124

# Silence Suppression. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P1785 = 0

# Voice Frames per TX. Default valule is 2
# Number: 1 - 64
P1786 = 2

#######################################################################
##  Account 5 RTP Settings                                           ##
#######################################################################
# SRTP Mode. 0 - Disable, 1 - Enabled but not forced, 2 - Enabled and forced. Default value is 0
# Number: 0, 1, 2
P1743 = 0

# SRTP Key Length. 0 - AES 128&256 bit, 1 - AES 128 bit, 2 - AES 256 bit. Default value is 0
#Number:0, 1, 2
P2783 = 0

# Enable SRTP Key Life Time. 0 - No, 1 - Yes.
# Number: 0,1
P2763 = 1

# RTCP Destination
P2790 = 

# Symmetric RTP. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P1760 = 0

# RTP IP Filter. 0 - Disable, 1 - IP Only, 2 - IP and Port. Default value is 0
# Number: 0, 1, 2
P26426 = 0

#######################################################################
##  Account 5 Call Settings                                          ##
#######################################################################
# Play warning tone for Auto Answer Intercom. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P26472 = 1

# Send Anonymous. 0 - No, 1 - Yes (caller ID will be blocked if set to Yes). Default value is 0
# Number: 0, 1
P1721 = 0

# Intercept Anonymous Calls. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P1746 = 0

# Call Log. 0 - Log All, 1 - Log Incoming/Outgoing only (Missed Calls Not Recorded), 2 - Disable Call All. Default value is 0
# Number: 0, 1
P1742 = 0

# Ring Timeout. Default value is 60 seconds
# Number: 0 - 300
P1776 = 60

# Refer-To Use Target Contact. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P1769 = 0

# Incoming Call Rules. 0 - Block, 1 - Set Password, 2 - Auto Answer, 3 - Ringing, 4 - Disable. Default value is 4.
# Number: 0, 1, 2 ,3 ,4
P60444 = 4

# Set Password Rules. 
# Numbers
P60445

# Dial Plan Prefix
# String
P1719 =

# Disable DialPlan. 0 - No Selection, 1 - Dial Page, 2 - Contact, 4 - Incoming Call History, 8 -  Outgoing Call History, 16 - MPK & Click2Dial. 
# If need to check multiple selections, add the specific values for each selections together. Default value is 0
# Number: 0-31
P2782 = 0

# Dial Plan. Default value is { x+ | \+x+ | *x+ | *xx*x+ }
P1759 = { x+ | \+x+ | *x+ | *xx*x+ }

# Account Ringtone. See ring tone options and value in the Ring Tone Value Table below.
P1723 = content://settings/system/ringtone

# Ignore Alert-Info Header. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1
P26418 = 0

# Matching Incoming Caller ID. Matching Rule 1.
# String
P1512 =

# Matching Rule 1 Distinctive Ringtone. See ring tone options and value in the Ring Tone Value Table below.
# String
P1513 = content://settings/system/ringtone

# Matching Incoming Caller ID. Matching Rule 2.
# String
P1514 =

# Matching Rule 2 Distinctive Ringtone. See ring tone options and value in the Ring Tone Value Table below.
# String
P1515 = content://settings/system/ringtone

# Matching Incoming Caller ID. Matching Rule 3.
# String
P1516 =

# Matching Rule 3 Distinctive Ringtone. See ring tone options and value in the Ring Tone Value Table below.
# String
P1517 = content://settings/system/ringtone

############Ring Tone Value Table###############
# Web GUI Option                            Value
# Use System Ring tone                      content://settings/system/ringtone 
# Andromeda					/system/media/audio/ringtones/ANDROMEDA.ogg
# Aquila					/system/media/audio/ringtones/Aquila.ogg
# Argo Navis					/system/media/audio/ringtones/ArgoNavis.ogg
# Atria					/system/media/audio/ringtones/Atria.ogg
# Backroad					/system/media/audio/ringtones/Backroad.ogg
# Beat Plucker					/system/media/audio/ringtones/BeatPlucker.ogg
# Bell Phone					/system/media/audio/ringtones/Ring_Classic_02.ogg
# Bentley Dubs					/system/media/audio/ringtones/BentleyDubs.ogg
# Big Easy					/system/media/audio/ringtones/Big_Easy.ogg
# Bird Loop					/system/media/audio/ringtones/BirdLoop.ogg
# Bollywood					/system/media/audio/ringtones/Bollywood.ogg
# Boötes					/system/media/audio/ringtones/BOOTES.ogg
# Bus' a Move					/system/media/audio/ringtones/BussaMove.ogg
# Cairo					/system/media/audio/ringtones/Cairo.ogg
# Calypso Steel					/system/media/audio/ringtones/Calypso_Steel.ogg
# Canis Major					/system/media/audio/ringtones/CANISMAJOR.ogg
# Caribbean Ice					/system/media/audio/ringtones/CaribbeanIce.ogg
# Carina					/system/media/audio/ringtones/Carina.ogg
# Cassiopeia					/system/media/audio/ringtones/CASSIOPEIA.ogg
# Centaurus					/system/media/audio/ringtones/Centaurus.ogg
# Champagne Edition					/system/media/audio/ringtones/Champagne_Edition.ogg
# Chimey Phone					/system/media/audio/ringtones/Ring_Synth_02.ogg
# Club Cubano					/system/media/audio/ringtones/Club_Cubano.ogg
# Crayon Rock					/system/media/audio/ringtones/CrayonRock.ogg
# Crazy Dream					/system/media/audio/ringtones/CrazyDream.ogg
# Curve Ball Blend					/system/media/audio/ringtones/CurveBall.ogg
# Cygnus					/system/media/audio/ringtones/Cygnus.ogg
# Dancin' Fool					/system/media/audio/ringtones/DancinFool.ogg
# Digital Phone					/system/media/audio/ringtones/Ring_Digital_02.ogg
# Ding					/system/media/audio/ringtones/Ding.ogg
# DingDong					/system/media/audio/ringtones/DingDong.wav
# Don' Mess Wiv It					/system/media/audio/ringtones/DonMessWivIt.ogg
# Draco					/system/media/audio/ringtones/Draco.ogg
# Dream Theme					/system/media/audio/ringtones/DreamTheme.ogg
# Eastern Sky					/system/media/audio/ringtones/Eastern_Sky.ogg
# Enter the Nexus					/system/media/audio/ringtones/Enter_the_Nexus.ogg
# Eridani					/system/media/audio/ringtones/Eridani.ogg
# Ether Shake					/system/media/audio/ringtones/EtherShake.ogg
# Flutey Phone					/system/media/audio/ringtones/Ring_Synth_04.ogg
# Free Flight					/system/media/audio/ringtones/FreeFlight.ogg
# Friendly Ghost					/system/media/audio/ringtones/FriendlyGhost.ogg
# Funk Y'all					/system/media/audio/ringtones/Funk_Yall.ogg
# Game Over Guitar					/system/media/audio/ringtones/GameOverGuitar.ogg
# Gimme Mo' Town					/system/media/audio/ringtones/Gimme_Mo_Town.ogg
# Girtab					/system/media/audio/ringtones/Girtab.ogg
# Glacial Groove					/system/media/audio/ringtones/Glacial_Groove.ogg
# Growl					/system/media/audio/ringtones/Growl.ogg
# Halfway Home					/system/media/audio/ringtones/HalfwayHome.ogg
# Hydra					/system/media/audio/ringtones/Hydra.ogg
# Insert Coin					/system/media/audio/ringtones/InsertCoin.ogg
# Kuma					/system/media/audio/ringtones/Kuma.ogg
# Loopy Lounge					/system/media/audio/ringtones/LoopyLounge.ogg
# Love Flute					/system/media/audio/ringtones/LoveFlute.ogg
# Lyra					/system/media/audio/ringtones/Lyra.ogg
# Machina					/system/media/audio/ringtones/Machina.ogg
# Medieval Jaunt					/system/media/audio/ringtones/MidEvilJaunt.ogg
# Mildly Alarming					/system/media/audio/ringtones/MildlyAlarming.ogg
# Nairobi					/system/media/audio/ringtones/Nairobi.ogg
# Nassau					/system/media/audio/ringtones/Nassau.ogg
# New Player					/system/media/audio/ringtones/NewPlayer.ogg
# No Limits					/system/media/audio/ringtones/No_Limits.ogg
# Noisey One					/system/media/audio/ringtones/Noises1.ogg
# Organ Dub					/system/media/audio/ringtones/OrganDub.ogg
# Orion					/system/media/audio/ringtones/Orion.ogg
# Paradise Island					/system/media/audio/ringtones/Paradise_Island.ogg
# Pegasus					/system/media/audio/ringtones/Pegasus.ogg
# Perseus					/system/media/audio/ringtones/PERSEUS.ogg
# Playa					/system/media/audio/ringtones/Playa.ogg
# Pyxis					/system/media/audio/ringtones/Pyxis.ogg
# Rasalas					/system/media/audio/ringtones/Rasalas.ogg
# Revelation					/system/media/audio/ringtones/Revelation.ogg
# Rigel					/system/media/audio/ringtones/Rigel.ogg
# Road Trip					/system/media/audio/ringtones/Road_Trip.ogg
# Romancing The Tone					/system/media/audio/ringtones/RomancingTheTone.ogg
# Safari					/system/media/audio/ringtones/Safari.ogg
# Savannah					/system/media/audio/ringtones/Savannah.ogg
# Scarabaeus					/system/media/audio/ringtones/Scarabaeus.ogg
# Sceptrum					/system/media/audio/ringtones/Sceptrum.ogg
# Seville					/system/media/audio/ringtones/Seville.ogg
# She's All That					/system/media/audio/ringtones/Shes_All_That.ogg
# Silky Way					/system/media/audio/ringtones/SilkyWay.ogg
# Sitar Versus Sitar					/system/media/audio/ringtones/SitarVsSitar.ogg
# Solarium					/system/media/audio/ringtones/Solarium.ogg
# Springy Jalopy					/system/media/audio/ringtones/SpringyJalopy.ogg
# Steppin' Out					/system/media/audio/ringtones/Steppin_Out.ogg
# Terminated					/system/media/audio/ringtones/Terminated.ogg
# Terrible Twos					/system/media/audio/ringtones/Noises2.ogg
# Testudo					/system/media/audio/ringtones/Testudo.ogg
# Themos					/system/media/audio/ringtones/Themos.ogg
# Third Eye					/system/media/audio/ringtones/Third_Eye.ogg
# Thriller Three					/system/media/audio/ringtones/Noises3.ogg
# Thunderfoot					/system/media/audio/ringtones/Thunderfoot.ogg
# Twirl Away					/system/media/audio/ringtones/TwirlAway.ogg
# Ursa Minor					/system/media/audio/ringtones/URSAMINOR.ogg
# UrsaMinor					/system/media/audio/ringtones/UrsaMinor.ogg
# Very Alarmed					/system/media/audio/ringtones/VeryAlarmed.ogg
# Vespa					/system/media/audio/ringtones/Vespa.ogg
# World					/system/media/audio/ringtones/World.ogg
# Zeta					/system/media/audio/ringtones/Zeta.ogg
# bellcore-dr1					/system/media/audio/ringtones/bellcore-dr1.ogg
# bellcore-dr2					/system/media/audio/ringtones/bellcore-dr2.ogg
# bellcore-dr3					/system/media/audio/ringtones/bellcore-dr3.ogg
# bellcore-dr4					/system/media/audio/ringtones/bellcore-dr4.ogg
# bellcore-dr5					/system/media/audio/ringtones/bellcore-dr5.ogg
# speaker					/system/media/audio/ringtones/speaker.wav

#######################################################################
##  Account 5 Advanced Settings                                      ##
#######################################################################
# Check Domain Certificates. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P2711 = 0

# Validate Certificate Chain. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P2767 = 0

# Validate Incoming SIP Messages. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P2706 = 0

# Allow Unsolicited REFER. 0 - Disabled, 1 - Enabled, 2 - Enabled/Force Auth. Default value is 0.
# Number: 0, 1, 2
P26423 = 0

# Only Accept SIP Requests from Known Servers. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P2747 = 0

# Check SIP User ID for Incoming INVITE. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P1749 = 0

# Allow SIP Reset. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P26415 = 0

# Authenticate Incoming INVITE. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P2746 = 0

# SIP Realm Used for Challenge INVITE & NOTIFY.
# String
P26421 =

# Enable Local MOH
# Number: 0, 1 
P2757 = 0

# Virtual Account Group. -1 - Default,  0 - Virtual Account Group 1, 1 - Virtual Account Group 2, 2 - Virtual Account Group 3
# 3 - Virtual Account Group 4, 4 - Virtual Account Group 5, 5 - Virtual Account Group 6, 6 - Virtual Account Group 7, 7 - Virtual Account Group 8
# 8 - Virtual Account Group 9, 9 - Virtual Account Group 10, 10 - Virtual Account Group 11, 11 - Virtual Account Group 12, 12 - Virtual Account Group 13
# 13 - Virtual Account Group 14, 14 - Virtual Account Group 15, 15 - Virtual Account Group 16. Default value is -1.
# Number: -1 - 15 
P2791 = -1

# Special Feature. Default value is 100
# 100 - Standard, 102 - Broadsoft, 113 - China Mobile, 114 - ZTE IMS, 115 - Mobotix
# 116 - ZTE NGN, 117 - Huawei IMS, 123 - NEC, 125 - WorldStone, 129 - Telefonica Spain
# Number: 100, 102, 113, 114, 115, 116, 117, 123, 125, 129
P1724 = 100

# Feature Key Synchronization.  0 - Disable, 0 - Broadsoft/Metaswitch. Default Value is 0.
# Number: 0, 1
# P2725 = 0

# Allow Sync Phonebook via SIP Notify. 0 - No, 1 - Yes. Default is 1.
# Number: 0, 1
P26499 = 1

##############################################################################
##  Account 6 Settings                                                      ##
##############################################################################
#######################################################################
##  Account 6 General Settings                                       ##
#######################################################################
# Account Active. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P1801 = 0

# Account Name
P1817 =

# SIP Server
P1802 =

# SIP User ID
P1804 =

# SIP Authentication ID
P1805 =

# SIP Authentication Password
P1806 =

# Tel URI. 0 - Disable, 1 - User=Phone, 2 - Enabled. Default value is 0
# Number: 0, 1, 2
P1809 = 0

#######################################################################
##  Account 6 Network Settings                                       ##
#######################################################################
# Outbound Proxy
P1803 =

# Secondary Outbound Proxy
P2833 =

# DNS Mode.  0 - A Record, 1 - SRV, 2 - NAPTR/SRV. Default value is 0
# Number: 0, 1, 2
P1808 = 0

# DNS SRV Fail-over Mode. 0 - Default, 1 - Saved one until DNS TTL, 2 - Saved one until no response. Defualt value is 1
# Number
P26540 = 0

# Register Before DNS SRV Fail-over. 0 - No, 1 - Yes. Default Value is 0.
# Number: 0, 1
P29595 = 1

# NAT Traversal. 0 - NAT No, 1 - STUN, 2 - Keep-alive, 3 - UPnP, 4 - Auto, 5 - VPN. Default value is 2
# Number: 0, 1, 2, 3, 4, 5
P1814 = 2

# Proxy-Require
P1818 =

#######################################################################
##  Account 6 SIP Settings                                           ##
#######################################################################
# SIP Registration. 0 - No, 1 - Yes. Default is 1
# Number: 0, 1
P1810 = 1

# Unregister Before New Registration. 0 - No, 1 - All, 2 -  Instance . Default value is 0
# Number: 0, 1, 2
P1811 = 2

# Register Expiration (m). In minutes. Default value is 60
# Number: 60 - 64800
P1812 = 60

# Subscribe Expiration (m). In minutes. Default value is blank
# Number: 0 - 64800
P26551 = 60

# Re-register before Expiration (s). Default value is 0
# Number: 0 - 3600
P2830 = 0

# Registration Retry Wait Time (s). In seconds. Default value is 20
# Number: 20 - 3600
P1871 = 20

# Add Auth Header On RE-REGISTER
# 0 - No, 1- Yes
P2859 = 1

# Enable SIP OPTIONS Keep Alive. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P2897 = 0

# SIP OPTIONS Keep Alive Interval(s). Default value is 30
# Number: 1 - 64800 
P2898 = 30

# SIP OPTIONS Keep Alive Maximum Tries. Default value is 3
# Number: 3 
P2899 = 3

# Use Privacy Header. 0 - Default, 1 - No, 2 - Yes. Default value is 0
# Number: 0, 1, 2
P2838 = 0

# Use P-Preferred-Identity Header. 0 - Default, 1 - No, 2 - Yes. Default value is 0
# Number: 0, 1, 2
P2839 = 0

# SIP Transport. 0 - UDP, 1 - TCP, 2 - TLS. Default value is 0
# Number: 0, 1, 2
P1848 = 0

# Local SIP Port. Default value is 5070
# Number: 0 or 90 - 65535
P1813 = 5070

# SIP URI Scheme When Using TLS
# 0 -sip, 1 - sips. Default value is 0.
# Number: 0, 1
P2829 = 0

# Use Actual Ephemeral Port in Contact with TCP/TLS
# 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P2831 = 0

# Support SIP Instance ID. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P1889 = 1

# SIP T1 Timeout. RFC 3261 T1 value (RTT estimate)
# 50 - 0.5 sec, 100 - 1 sec, 200 - 2 sec. Default value is 50
# Number: 50, 100, 200
P1840 = 50

# SIP T2 Interval. RFC 3261 T2 value. The maximum retransmit interval for non-INVITE requests and INVITE responses
# 200 - 2 sec, 400 - 4 sec, 800 - 8 sec. Default 400
# Number: 200, 400, 800
P1841 = 400

# SIP Timer D Interval (Seconds)
# Number 0-64. Default value is 0
P2887 = 0

# Remove OBP from route. 0 - Disable, 1 - Enable. Default value is 0
# Number: 0, 1
P2805 = 0

# Enable 100rel. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P1835 = 0

#######################################################################
##  Account 6 Session Timer                                          ##
#######################################################################

# Enable Session Timer/ Session Expiration(s).  In seconds. Default value is 180 seconds.
# By default,  Session Timer is Enabled.  Session Timer is disabled if the value is 0.
# Number: 0 or 90 - 64800
P1834 = 180

# Min-SE (s). Default value is 90 seconds
# Number: 0 or 90 - 64800
P1827 = 90

# UAC Specify Refresher. 0 - Omit, 1 - UAC, 2 - UAS. Default value is 0
# Number: 0, 1, 2
P1832 = 0

# UAS Specify Refresher. 1 - UAC, 2 - UAS. Default value is 1
# Number: 1, 2
P1833 = 1

# Caller Request Timer (Request for timer when calling)
# 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1.
P1828 = 0

# Callee Request Timer. Request for timer when called (i.e. if remote party supports timer but did not request for one)
# 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P1829 = 0

# Force Timer (Still use timer when remote party does not support timer). 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P1830 = 0

# Force INVITE (Always refresh with INVITE instead of UPDATE even when remote party supports UPDATE)
# 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P1831 = 0

#######################################################################
##  Account 6 Codec Settings                                         ##
#######################################################################
# Preferred Vocoder
# First codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 103 - G722.1C, 104 - G722.1, 123 - Opus. Default value is 0
# Number: 0, 2, 8, 9, 18, 98, 103, 104, 123
P1851 = 0

# Second codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 103 - G722.1C, 104 - G722.1, 123 - Opus. Default value is 8
# Number: 0, 2, 8, 9, 18, 98, 103, 104, 123
P1852 = 8

# Third codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 103 - G722.1C, 104 - G722.1, 123 - Opus. Default value is 9
# Number: 0, 2, 8, 9, 18, 98, 103, 104, 123
P1853 = 9

# Forth codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 103 - G722.1C, 104 - G722.1, 123 - Opus. Default value is 104
# Number: 0, 2, 8, 9, 18, 98, 103, 104, 123
P1854 = 104

# Fifth codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 103 - G722.1C, 104 - G722.1, 123 - Opus. Default value is 104
# Number: 0, 2, 8, 9, 18, 98, 103, 104, 123
P1855 = 104

# Sixth codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 103 - G722.1C, 104 - G722.1, 123 - Opus. Default value is 104
# Number: 0, 2, 8, 9, 18, 98, 103, 104, 123
P1856 = 104

# Seventh codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 103 - G722.1C, 104 - G722.1, 123 - Opus. Default value is 104
# Number: 0, 2, 8, 9, 18, 98, 103, 104, 123
P1857 = 104

# Eigth codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 103 - G722.1C, 104 - G722.1, 123 - Opus. Default value is 104
# Number: 0, 2, 8, 9, 18, 98, 103, 104, 123
P1858 = 104

# Codec Negotiation Priority. 0 - Caller, 1 - Callee. Default value is 1.
# Number: 0, 1
P29561 = 1

# Use First Matching Vocoder in 200OK SDP. 0 - No, 1 - Yes. The default value is 0.
# Number: 0, 1
P2848 = 0

# iLBC Frame Size. 0 - 20 ms, 1 - 30 ms. Default value is 1.
# Number: 0, 1
P1895 = 1

# G726-32 ITU Payload. 0 - 2, 1 - Dynamic. Default value is 0.
# Number: 0, 1
P2869 = 0

# G726-32 Dynamic PT. Default value is 126.
# Number
P2865 = 126

# Opus Payload Type. Default value is 123.
P2885 = 123

# DTMF: in audio. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P2801 = 0

# DTMF: in RFC2833. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P2802 = 1

# DTMF: in SIP INFO. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P2803 = 0

# DTMF Payload Type. Default value is 101
# Number: 96 - 127
P1896 = 101

# Enable Audio RED with FEC. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P26573 = 0

# Audio FEC Payload Type. Default value is 121
# Number: 96 - 126
P26574 = 121

# Audio RED Payload Type. Default value is 124
# Number: 96 - 126
P26575 = 124

# Silence Suppression. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P1885 = 0

# Voice Frames per TX. Default valule is 2
# Number: 1 - 64
P1886 = 2

#######################################################################
##  Account 6 RTP Settings                                           ##
#######################################################################
# SRTP Mode. 0 - Disable, 1 - Enabled but not forced, 2 - Enabled and forced. Default value is 0
# Number: 0, 1, 2
P1843 = 0

# SRTP Key Length. 0 - AES 128&256 bit, 1 - AES 128 bit, 2 - AES 256 bit. Default value is 0
#Number:0, 1, 2
P2883 = 0

# Enable SRTP Key Life Time. 0 - No, 1 - Yes.
# Number: 0,1
P2863 = 1

# RTCP Destination
P2890 = 

# Symmetric RTP. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P1860 = 0

# RTP IP Filter. 0 - Disable, 1 - IP Only, 2 - IP and Port. Default value is 0
# Number: 0, 1, 2
P26526 = 0

#######################################################################
##  Account 6 Call Settings                                          ##
#######################################################################
# Play warning tone for Auto Answer Intercom. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P26572 = 1

# Send Anonymous. 0 - No, 1 - Yes (caller ID will be blocked if set to Yes). Default value is 0
# Number: 0, 1
P1821 = 0

# Intercept Anonymous Calls. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P1846 = 0

# Call Log. 0 - Log All, 1 - Log Incoming/Outgoing only (Missed Calls Not Recorded), 2 - Disable Call All. Default value is 0
# Number: 0, 1
P1842 = 0

# Ring Timeout. Default value is 60 seconds
# Number: 0 - 300
P1876 = 60

# Refer-To Use Target Contact. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P1869 = 0

# Incoming Call Rules. 0 - Block, 1 - Set Password, 2 - Auto Answer, 3 - Ringing, 4 - Disable. Default value is 4.
# Number: 0, 1, 2 ,3 ,4
P60544 = 4

# Set Password Rules. 
# Numbers
P60545

# Dial Plan Prefix
# String
P1819 =

# Disable DialPlan. 0 - No Selection, 1 - Dial Page, 2 - Contact, 4 - Incoming Call History, 8 -  Outgoing Call History, 16 - MPK & Click2Dial. 
# If need to check multiple selections, add the specific values for each selections together. Default value is 0
# Number: 0-31
P2882 = 0

# Dial Plan. Default value is { x+ | \+x+ | *x+ | *xx*x+ }
P1859 = { x+ | \+x+ | *x+ | *xx*x+ }

# Account Ringtone. See ring tone options and value in the Ring Tone Value Table below.
P1823 = content://settings/system/ringtone

# Ignore Alert-Info Header. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1
P26518 = 0

# Matching Incoming Caller ID. Matching Rule 1.
# String
P1518 =

# Matching Rule 1 Distinctive Ringtone. See ring tone options and value in the Ring Tone Value Table below.
# String
P1519 = content://settings/system/ringtone

# Matching Incoming Caller ID. Matching Rule 2.
# String
P1520 =

# Matching Rule 2 Distinctive Ringtone. See ring tone options and value in the Ring Tone Value Table below.
# String
P1521 = content://settings/system/ringtone

# Matching Incoming Caller ID. Matching Rule 3.
# String
P1522 =

# Matching Rule 3 Distinctive Ringtone. See ring tone options and value in the Ring Tone Value Table below.
# String
P1523 = content://settings/system/ringtone

############Ring Tone Value Table###############
# Web GUI Option                            Value
# Use System Ring tone                      content://settings/system/ringtone 
# Andromeda					/system/media/audio/ringtones/ANDROMEDA.ogg
# Aquila					/system/media/audio/ringtones/Aquila.ogg
# Argo Navis					/system/media/audio/ringtones/ArgoNavis.ogg
# Atria					/system/media/audio/ringtones/Atria.ogg
# Backroad					/system/media/audio/ringtones/Backroad.ogg
# Beat Plucker					/system/media/audio/ringtones/BeatPlucker.ogg
# Bell Phone					/system/media/audio/ringtones/Ring_Classic_02.ogg
# Bentley Dubs					/system/media/audio/ringtones/BentleyDubs.ogg
# Big Easy					/system/media/audio/ringtones/Big_Easy.ogg
# Bird Loop					/system/media/audio/ringtones/BirdLoop.ogg
# Bollywood					/system/media/audio/ringtones/Bollywood.ogg
# Boötes					/system/media/audio/ringtones/BOOTES.ogg
# Bus' a Move					/system/media/audio/ringtones/BussaMove.ogg
# Cairo					/system/media/audio/ringtones/Cairo.ogg
# Calypso Steel					/system/media/audio/ringtones/Calypso_Steel.ogg
# Canis Major					/system/media/audio/ringtones/CANISMAJOR.ogg
# Caribbean Ice					/system/media/audio/ringtones/CaribbeanIce.ogg
# Carina					/system/media/audio/ringtones/Carina.ogg
# Cassiopeia					/system/media/audio/ringtones/CASSIOPEIA.ogg
# Centaurus					/system/media/audio/ringtones/Centaurus.ogg
# Champagne Edition					/system/media/audio/ringtones/Champagne_Edition.ogg
# Chimey Phone					/system/media/audio/ringtones/Ring_Synth_02.ogg
# Club Cubano					/system/media/audio/ringtones/Club_Cubano.ogg
# Crayon Rock					/system/media/audio/ringtones/CrayonRock.ogg
# Crazy Dream					/system/media/audio/ringtones/CrazyDream.ogg
# Curve Ball Blend					/system/media/audio/ringtones/CurveBall.ogg
# Cygnus					/system/media/audio/ringtones/Cygnus.ogg
# Dancin' Fool					/system/media/audio/ringtones/DancinFool.ogg
# Digital Phone					/system/media/audio/ringtones/Ring_Digital_02.ogg
# Ding					/system/media/audio/ringtones/Ding.ogg
# DingDong					/system/media/audio/ringtones/DingDong.wav
# Don' Mess Wiv It					/system/media/audio/ringtones/DonMessWivIt.ogg
# Draco					/system/media/audio/ringtones/Draco.ogg
# Dream Theme					/system/media/audio/ringtones/DreamTheme.ogg
# Eastern Sky					/system/media/audio/ringtones/Eastern_Sky.ogg
# Enter the Nexus					/system/media/audio/ringtones/Enter_the_Nexus.ogg
# Eridani					/system/media/audio/ringtones/Eridani.ogg
# Ether Shake					/system/media/audio/ringtones/EtherShake.ogg
# Flutey Phone					/system/media/audio/ringtones/Ring_Synth_04.ogg
# Free Flight					/system/media/audio/ringtones/FreeFlight.ogg
# Friendly Ghost					/system/media/audio/ringtones/FriendlyGhost.ogg
# Funk Y'all					/system/media/audio/ringtones/Funk_Yall.ogg
# Game Over Guitar					/system/media/audio/ringtones/GameOverGuitar.ogg
# Gimme Mo' Town					/system/media/audio/ringtones/Gimme_Mo_Town.ogg
# Girtab					/system/media/audio/ringtones/Girtab.ogg
# Glacial Groove					/system/media/audio/ringtones/Glacial_Groove.ogg
# Growl					/system/media/audio/ringtones/Growl.ogg
# Halfway Home					/system/media/audio/ringtones/HalfwayHome.ogg
# Hydra					/system/media/audio/ringtones/Hydra.ogg
# Insert Coin					/system/media/audio/ringtones/InsertCoin.ogg
# Kuma					/system/media/audio/ringtones/Kuma.ogg
# Loopy Lounge					/system/media/audio/ringtones/LoopyLounge.ogg
# Love Flute					/system/media/audio/ringtones/LoveFlute.ogg
# Lyra					/system/media/audio/ringtones/Lyra.ogg
# Machina					/system/media/audio/ringtones/Machina.ogg
# Medieval Jaunt					/system/media/audio/ringtones/MidEvilJaunt.ogg
# Mildly Alarming					/system/media/audio/ringtones/MildlyAlarming.ogg
# Nairobi					/system/media/audio/ringtones/Nairobi.ogg
# Nassau					/system/media/audio/ringtones/Nassau.ogg
# New Player					/system/media/audio/ringtones/NewPlayer.ogg
# No Limits					/system/media/audio/ringtones/No_Limits.ogg
# Noisey One					/system/media/audio/ringtones/Noises1.ogg
# Organ Dub					/system/media/audio/ringtones/OrganDub.ogg
# Orion					/system/media/audio/ringtones/Orion.ogg
# Paradise Island					/system/media/audio/ringtones/Paradise_Island.ogg
# Pegasus					/system/media/audio/ringtones/Pegasus.ogg
# Perseus					/system/media/audio/ringtones/PERSEUS.ogg
# Playa					/system/media/audio/ringtones/Playa.ogg
# Pyxis					/system/media/audio/ringtones/Pyxis.ogg
# Rasalas					/system/media/audio/ringtones/Rasalas.ogg
# Revelation					/system/media/audio/ringtones/Revelation.ogg
# Rigel					/system/media/audio/ringtones/Rigel.ogg
# Road Trip					/system/media/audio/ringtones/Road_Trip.ogg
# Romancing The Tone					/system/media/audio/ringtones/RomancingTheTone.ogg
# Safari					/system/media/audio/ringtones/Safari.ogg
# Savannah					/system/media/audio/ringtones/Savannah.ogg
# Scarabaeus					/system/media/audio/ringtones/Scarabaeus.ogg
# Sceptrum					/system/media/audio/ringtones/Sceptrum.ogg
# Seville					/system/media/audio/ringtones/Seville.ogg
# She's All That					/system/media/audio/ringtones/Shes_All_That.ogg
# Silky Way					/system/media/audio/ringtones/SilkyWay.ogg
# Sitar Versus Sitar					/system/media/audio/ringtones/SitarVsSitar.ogg
# Solarium					/system/media/audio/ringtones/Solarium.ogg
# Springy Jalopy					/system/media/audio/ringtones/SpringyJalopy.ogg
# Steppin' Out					/system/media/audio/ringtones/Steppin_Out.ogg
# Terminated					/system/media/audio/ringtones/Terminated.ogg
# Terrible Twos					/system/media/audio/ringtones/Noises2.ogg
# Testudo					/system/media/audio/ringtones/Testudo.ogg
# Themos					/system/media/audio/ringtones/Themos.ogg
# Third Eye					/system/media/audio/ringtones/Third_Eye.ogg
# Thriller Three					/system/media/audio/ringtones/Noises3.ogg
# Thunderfoot					/system/media/audio/ringtones/Thunderfoot.ogg
# Twirl Away					/system/media/audio/ringtones/TwirlAway.ogg
# Ursa Minor					/system/media/audio/ringtones/URSAMINOR.ogg
# UrsaMinor					/system/media/audio/ringtones/UrsaMinor.ogg
# Very Alarmed					/system/media/audio/ringtones/VeryAlarmed.ogg
# Vespa					/system/media/audio/ringtones/Vespa.ogg
# World					/system/media/audio/ringtones/World.ogg
# Zeta					/system/media/audio/ringtones/Zeta.ogg
# bellcore-dr1					/system/media/audio/ringtones/bellcore-dr1.ogg
# bellcore-dr2					/system/media/audio/ringtones/bellcore-dr2.ogg
# bellcore-dr3					/system/media/audio/ringtones/bellcore-dr3.ogg
# bellcore-dr4					/system/media/audio/ringtones/bellcore-dr4.ogg
# bellcore-dr5					/system/media/audio/ringtones/bellcore-dr5.ogg
# speaker					/system/media/audio/ringtones/speaker.wav

#######################################################################
##  Account 6 Advanced Settings                                      ##
#######################################################################
# Check Domain Certificates. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P2811 = 0

# Validate Certificate Chain. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P2867 = 0

# Validate Incoming SIP Messages. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P2806 = 0

# Allow Unsolicited REFER. 0 - Disabled, 1 - Enabled, 2 - Enabled/Force Auth. Default value is 0.
# Number: 0, 1, 2
P26523 = 0

# Only Accept SIP Requests from Known Servers. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P2847 = 0

# Check SIP User ID for Incoming INVITE. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P1849 = 0

# Allow SIP Reset. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P26515 = 0

# Authenticate Incoming INVITE. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P2846 = 0

# SIP Realm Used for Challenge INVITE & NOTIFY.
# String
P26521 =

# Enable Local MOH
# Number: 0, 1 
P2857 = 0

# Virtual Account Group. -1 - Default,  0 - Virtual Account Group 1, 1 - Virtual Account Group 2, 2 - Virtual Account Group 3
# 3 - Virtual Account Group 4, 4 - Virtual Account Group 5, 5 - Virtual Account Group 6, 6 - Virtual Account Group 7, 7 - Virtual Account Group 8
# 8 - Virtual Account Group 9, 9 - Virtual Account Group 10, 10 - Virtual Account Group 11, 11 - Virtual Account Group 12, 12 - Virtual Account Group 13
# 13 - Virtual Account Group 14, 14 - Virtual Account Group 15, 15 - Virtual Account Group 16. Default value is -1.
# Number: -1 - 15 
P2891 = -1

# Special Feature. Default value is 100
# 100 - Standard, 102 - Broadsoft, 113 - China Mobile, 114 - ZTE IMS, 115 - Mobotix
# 116 - ZTE NGN, 117 - Huawei IMS, 123 - NEC, 125 - WorldStone, 129 - Telefonica Spain
# Number: 100, 102, 113, 114, 115, 116, 117, 123, 125, 129
P1824 = 100

# Feature Key Synchronization.  0 - Disable, 0 - Broadsoft/Metaswitch. Default Value is 0.
# Number: 0, 1
# P2825 = 0

# Allow Sync Phonebook via SIP Notify. 0 - No, 1 - Yes. Default is 1.
# Number: 0, 1
P26599 = 1

##############################################################################
##  Account 7 Settings                                                      ##
##############################################################################
#######################################################################
##  Account 7 General Settings                                       ##
#######################################################################
# Account Active. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P50601 = 0

# Account Name
P50617 =

# SIP Server
P50602 =

# SIP User ID
P50604 =

# SIP Authentication ID
P50605 =

# SIP Authentication Password
P50606 =

# Tel URI. 0 - Disable, 1 - User=Phone, 2 - Enabled. Default value is 0
# Number: 0, 1, 2
P50609 = 0

#######################################################################
##  Account 7 Network Settings                                       ##
#######################################################################
# Outbound Proxy
P50603 =

# Secondary Outbound Proxy
P51633 =

# DNS Mode.  0 - A Record, 1 - SRV, 2 - NAPTR/SRV. Default value is 0
# Number: 0, 1, 2
P50608 = 0

# DNS SRV Fail-over Mode. 0 - Default, 1 - Saved one until DNS TTL, 2 - Saved one until no response. Defualt value is 1
# Number
P52640 = 0

# Register Before DNS SRV Fail-over. 0 - No, 1 - Yes. Default Value is 0.
# Number: 0, 1
P53695 = 1

# NAT Traversal. 0 - NAT No, 1 - STUN, 2 - Keep-alive, 3 - UPnP, 4 - Auto, 5 - VPN. Default value is 2
# Number: 0, 1, 2, 3, 4, 5
P50614 = 2

# Proxy-Require
P50618 =

#######################################################################
##  Account 7 SIP Settings                                           ##
#######################################################################
# SIP Registration. 0 - No, 1 - Yes. Default is 1
# Number: 0, 1
P50610 = 1

# Unregister Before New Registration. 0 - No, 1 - All, 2 -  Instance . Default value is 0
# Number: 0, 1, 2
P50611 = 2

# Register Expiration (m). In minutes. Default value is 60
# Number: 60 - 64800
P50612 = 60

# Subscribe Expiration (m). In minutes. Default value is blank
# Number: 0 - 64800
P52651 = 60

# Re-register before Expiration (s). Default value is 0
# Number: 0 - 3600
P51630 = 0

# Registration Retry Wait Time (s). In seconds. Default value is 20
# Number: 20 - 3600
P50671 = 20

# Add Auth Header On RE-REGISTER
# 0 - No, 1- Yes
P51659 = 1

# Enable SIP OPTIONS Keep Alive. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P51697 = 0

# SIP OPTIONS Keep Alive Interval(s). Default value is 30
# Number: 1 - 64800 
P51698 = 30

# SIP OPTIONS Keep Alive Maximum Tries. Default value is 3
# Number: 3 
P51699 = 3

# Use Privacy Header. 0 - Default, 1 - No, 2 - Yes. Default value is 0
# Number: 0, 1, 2
P51638 = 0

# Use P-Preferred-Identity Header. 0 - Default, 1 - No, 2 - Yes. Default value is 0
# Number: 0, 1, 2
P51639 = 0

# SIP Transport. 0 - UDP, 1 - TCP, 2 - TLS. Default value is 0
# Number: 0, 1, 2
P50648 = 0

# Local SIP Port. Default value is 5072
# Number: 0 or 90 - 65535
P50613 = 5072

# SIP URI Scheme When Using TLS
# 0 -sip, 1 - sips. Default value is 0.
# Number: 0, 1
P51629 = 0

# Use Actual Ephemeral Port in Contact with TCP/TLS
# 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P51631 = 0

# Support SIP Instance ID. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P50689 = 1

# SIP T1 Timeout. RFC 3261 T1 value (RTT estimate)
# 50 - 0.5 sec, 100 - 1 sec, 200 - 2 sec. Default value is 50
# Number: 50, 100, 200
P50640 = 50

# SIP T2 Interval. RFC 3261 T2 value. The maximum retransmit interval for non-INVITE requests and INVITE responses
# 200 - 2 sec, 400 - 4 sec, 800 - 8 sec. Default 400
# Number: 200, 400, 800
P50641 = 400

# SIP Timer D Interval (Seconds)
# Number 0-64. Default value is 0
P51687 = 0

# Remove OBP from route. 0 - Disable, 1 - Enable. Default value is 0
# Number: 0, 1
P51605 = 0

# Enable 100rel. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P50635 = 0

#######################################################################
##  Account 7 Session Timer                                          ##
#######################################################################

# Enable Session Timer/ Session Expiration(s).  In seconds. Default value is 180 seconds.
# By default,  Session Timer is Enabled.  Session Timer is disabled if the value is 0.
# Number: 0 or 90 - 64800
P50634 = 180

# Min-SE (s). Default value is 90 seconds
# Number: 0 or 90 - 64800
P50627 = 90

# UAC Specify Refresher. 0 - Omit, 1 - UAC, 2 - UAS. Default value is 0
# Number: 0, 1, 2
P50632 = 0

# UAS Specify Refresher. 1 - UAC, 2 - UAS. Default value is 1
# Number: 1, 2
P50633 = 1

# Caller Request Timer (Request for timer when calling)
# 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1.
P50628 = 0

# Callee Request Timer. Request for timer when called (i.e. if remote party supports timer but did not request for one)
# 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P50629 = 0

# Force Timer (Still use timer when remote party does not support timer). 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P50630 = 0

# Force INVITE (Always refresh with INVITE instead of UPDATE even when remote party supports UPDATE)
# 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P50631 = 0

#######################################################################
##  Account 7 Codec Settings                                         ##
#######################################################################
# Preferred Vocoder
# First codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 103 - G722.1C, 104 - G722.1, 123 - Opus. Default value is 0
# Number: 0, 2, 8, 9, 18, 98, 103, 104, 123
P50651 = 0

# Second codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 103 - G722.1C, 104 - G722.1, 123 - Opus. Default value is 8
# Number: 0, 2, 8, 9, 18, 98, 103, 104, 123
P50652 = 8

# Third codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 103 - G722.1C, 104 - G722.1, 123 - Opus. Default value is 9
# Number: 0, 2, 8, 9, 18, 98, 103, 104, 123
P50653 = 9

# Forth codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 103 - G722.1C, 104 - G722.1, 123 - Opus. Default value is 104
# Number: 0, 2, 8, 9, 18, 98, 103, 104, 123
P50654 = 104

# Fifth codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 103 - G722.1C, 104 - G722.1, 123 - Opus. Default value is 104
# Number: 0, 2, 8, 9, 18, 98, 103, 104, 123
P50655 = 104

# Sixth codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 103 - G722.1C, 104 - G722.1, 123 - Opus. Default value is 104
# Number: 0, 2, 8, 9, 18, 98, 103, 104, 123
P50656 = 104

# Seventh codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 103 - G722.1C, 104 - G722.1, 123 - Opus. Default value is 104
# Number: 0, 2, 8, 9, 18, 98, 103, 104, 123
P50657 = 104

# Eigth codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 103 - G722.1C, 104 - G722.1, 123 - Opus. Default value is 104
# Number: 0, 2, 8, 9, 18, 98, 103, 104, 123
P50658 = 104

# Codec Negotiation Priority. 0 - Caller, 1 - Callee. Default value is 1.
# Number: 0, 1
P53661 = 1

# Use First Matching Vocoder in 200OK SDP. 0 - No, 1 - Yes. The default value is 0.
# Number: 0, 1
P51648 = 0

# iLBC Frame Size. 0 - 20 ms, 1 - 30 ms. Default value is 1.
# Number: 0, 1
P50695 = 1

# G726-32 ITU Payload. 0 - 2, 1 - Dynamic. Default value is 0.
# Number: 0, 1
P51669 = 0

# G726-32 Dynamic PT. Default value is 126.
# Number
P51665 = 126

# Opus Payload Type. Default value is 123.
P51685 = 123

# DTMF: in audio. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P51601 = 0

# DTMF: in RFC2833. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P51602 = 1

# DTMF: in SIP INFO. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P51603 = 0

# DTMF Payload Type. Default value is 101
# Number: 96 - 127
P50696 = 101

# Enable Audio RED with FEC. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P52673 = 0

# Audio FEC Payload Type. Default value is 121
# Number: 96 - 126
P52674 = 121

# Audio RED Payload Type. Default value is 124
# Number: 96 - 126
P52675 = 124

# Silence Suppression. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P50685 = 0

# Voice Frames per TX. Default valule is 2
# Number: 1 - 64
P50686 = 2

#######################################################################
##  Account 7 RTP Settings                                           ##
#######################################################################
# SRTP Mode. 0 - Disable, 1 - Enabled but not forced, 2 - Enabled and forced. Default value is 0
# Number: 0, 1, 2
P50643 = 0

# SRTP Key Length. 0 - AES 128&256 bit, 1 - AES 128 bit, 2 - AES 256 bit. Default value is 0
#Number:0, 1, 2
P51683 = 0

# Enable SRTP Key Life Time. 0 - No, 1 - Yes.
# Number: 0,1
P51663 = 1

# RTCP Destination
P51690 = 

# Symmetric RTP. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P50660 = 0

# RTP IP Filter. 0 - Disable, 1 - IP Only, 2 - IP and Port. Default value is 0
# Number: 0, 1, 2
P52626 = 0

#######################################################################
##  Account 7 Call Settings                                          ##
#######################################################################
# Play warning tone for Auto Answer Intercom. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P52672 = 1

# Send Anonymous. 0 - No, 1 - Yes (caller ID will be blocked if set to Yes). Default value is 0
# Number: 0, 1
P50621 = 0

# Intercept Anonymous Calls. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P50646 = 0

# Call Log. 0 - Log All, 1 - Log Incoming/Outgoing only (Missed Calls Not Recorded), 2 - Disable Call All. Default value is 0
# Number: 0, 1
P50642 = 0

# Ring Timeout. Default value is 60 seconds
# Number: 0 - 300
P50676 = 60

# Refer-To Use Target Contact. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P50669 = 0

# Incoming Call Rules. 0 - Block, 1 - Set Password, 2 - Auto Answer, 3 - Ringing, 4 - Disable. Default value is 4.
# Number: 0, 1, 2 ,3 ,4
P60644 = 4

# Set Password Rules. 
# Numbers
P60645

# Dial Plan Prefix
# String
P50619 =

# Disable DialPlan. 0 - No Selection, 1 - Dial Page, 2 - Contact, 4 - Incoming Call History, 8 -  Outgoing Call History, 16 - MPK & Click2Dial. 
# If need to check multiple selections, add the specific values for each selections together. Default value is 0
# Number: 0-31
P51682 = 0

# Dial Plan. Default value is { x+ | \+x+ | *x+ | *xx*x+ }
P50659 = { x+ | \+x+ | *x+ | *xx*x+ }

# Account Ringtone. See ring tone options and value in the Ring Tone Value Table below.
P50623 = content://settings/system/ringtone

# Ignore Alert-Info Header. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1
P52618 = 0

# Matching Incoming Caller ID. Matching Rule 1.
# String
P52677 =

# Matching Rule 1 Distinctive Ringtone. See ring tone options and value in the Ring Tone Value Table below.
# String
P52678 = content://settings/system/ringtone

# Matching Incoming Caller ID. Matching Rule 2.
# String
P52679 =

# Matching Rule 2 Distinctive Ringtone. See ring tone options and value in the Ring Tone Value Table below.
# String
P52680 = content://settings/system/ringtone

# Matching Incoming Caller ID. Matching Rule 3.
# String
P52681 =

# Matching Rule 3 Distinctive Ringtone. See ring tone options and value in the Ring Tone Value Table below.
# String
P52682 = content://settings/system/ringtone

############Ring Tone Value Table###############
# Web GUI Option                            Value
# Use System Ring tone                      content://settings/system/ringtone 
# Andromeda					/system/media/audio/ringtones/ANDROMEDA.ogg
# Aquila					/system/media/audio/ringtones/Aquila.ogg
# Argo Navis					/system/media/audio/ringtones/ArgoNavis.ogg
# Atria					/system/media/audio/ringtones/Atria.ogg
# Backroad					/system/media/audio/ringtones/Backroad.ogg
# Beat Plucker					/system/media/audio/ringtones/BeatPlucker.ogg
# Bell Phone					/system/media/audio/ringtones/Ring_Classic_02.ogg
# Bentley Dubs					/system/media/audio/ringtones/BentleyDubs.ogg
# Big Easy					/system/media/audio/ringtones/Big_Easy.ogg
# Bird Loop					/system/media/audio/ringtones/BirdLoop.ogg
# Bollywood					/system/media/audio/ringtones/Bollywood.ogg
# Boötes					/system/media/audio/ringtones/BOOTES.ogg
# Bus' a Move					/system/media/audio/ringtones/BussaMove.ogg
# Cairo					/system/media/audio/ringtones/Cairo.ogg
# Calypso Steel					/system/media/audio/ringtones/Calypso_Steel.ogg
# Canis Major					/system/media/audio/ringtones/CANISMAJOR.ogg
# Caribbean Ice					/system/media/audio/ringtones/CaribbeanIce.ogg
# Carina					/system/media/audio/ringtones/Carina.ogg
# Cassiopeia					/system/media/audio/ringtones/CASSIOPEIA.ogg
# Centaurus					/system/media/audio/ringtones/Centaurus.ogg
# Champagne Edition					/system/media/audio/ringtones/Champagne_Edition.ogg
# Chimey Phone					/system/media/audio/ringtones/Ring_Synth_02.ogg
# Club Cubano					/system/media/audio/ringtones/Club_Cubano.ogg
# Crayon Rock					/system/media/audio/ringtones/CrayonRock.ogg
# Crazy Dream					/system/media/audio/ringtones/CrazyDream.ogg
# Curve Ball Blend					/system/media/audio/ringtones/CurveBall.ogg
# Cygnus					/system/media/audio/ringtones/Cygnus.ogg
# Dancin' Fool					/system/media/audio/ringtones/DancinFool.ogg
# Digital Phone					/system/media/audio/ringtones/Ring_Digital_02.ogg
# Ding					/system/media/audio/ringtones/Ding.ogg
# DingDong					/system/media/audio/ringtones/DingDong.wav
# Don' Mess Wiv It					/system/media/audio/ringtones/DonMessWivIt.ogg
# Draco					/system/media/audio/ringtones/Draco.ogg
# Dream Theme					/system/media/audio/ringtones/DreamTheme.ogg
# Eastern Sky					/system/media/audio/ringtones/Eastern_Sky.ogg
# Enter the Nexus					/system/media/audio/ringtones/Enter_the_Nexus.ogg
# Eridani					/system/media/audio/ringtones/Eridani.ogg
# Ether Shake					/system/media/audio/ringtones/EtherShake.ogg
# Flutey Phone					/system/media/audio/ringtones/Ring_Synth_04.ogg
# Free Flight					/system/media/audio/ringtones/FreeFlight.ogg
# Friendly Ghost					/system/media/audio/ringtones/FriendlyGhost.ogg
# Funk Y'all					/system/media/audio/ringtones/Funk_Yall.ogg
# Game Over Guitar					/system/media/audio/ringtones/GameOverGuitar.ogg
# Gimme Mo' Town					/system/media/audio/ringtones/Gimme_Mo_Town.ogg
# Girtab					/system/media/audio/ringtones/Girtab.ogg
# Glacial Groove					/system/media/audio/ringtones/Glacial_Groove.ogg
# Growl					/system/media/audio/ringtones/Growl.ogg
# Halfway Home					/system/media/audio/ringtones/HalfwayHome.ogg
# Hydra					/system/media/audio/ringtones/Hydra.ogg
# Insert Coin					/system/media/audio/ringtones/InsertCoin.ogg
# Kuma					/system/media/audio/ringtones/Kuma.ogg
# Loopy Lounge					/system/media/audio/ringtones/LoopyLounge.ogg
# Love Flute					/system/media/audio/ringtones/LoveFlute.ogg
# Lyra					/system/media/audio/ringtones/Lyra.ogg
# Machina					/system/media/audio/ringtones/Machina.ogg
# Medieval Jaunt					/system/media/audio/ringtones/MidEvilJaunt.ogg
# Mildly Alarming					/system/media/audio/ringtones/MildlyAlarming.ogg
# Nairobi					/system/media/audio/ringtones/Nairobi.ogg
# Nassau					/system/media/audio/ringtones/Nassau.ogg
# New Player					/system/media/audio/ringtones/NewPlayer.ogg
# No Limits					/system/media/audio/ringtones/No_Limits.ogg
# Noisey One					/system/media/audio/ringtones/Noises1.ogg
# Organ Dub					/system/media/audio/ringtones/OrganDub.ogg
# Orion					/system/media/audio/ringtones/Orion.ogg
# Paradise Island					/system/media/audio/ringtones/Paradise_Island.ogg
# Pegasus					/system/media/audio/ringtones/Pegasus.ogg
# Perseus					/system/media/audio/ringtones/PERSEUS.ogg
# Playa					/system/media/audio/ringtones/Playa.ogg
# Pyxis					/system/media/audio/ringtones/Pyxis.ogg
# Rasalas					/system/media/audio/ringtones/Rasalas.ogg
# Revelation					/system/media/audio/ringtones/Revelation.ogg
# Rigel					/system/media/audio/ringtones/Rigel.ogg
# Road Trip					/system/media/audio/ringtones/Road_Trip.ogg
# Romancing The Tone					/system/media/audio/ringtones/RomancingTheTone.ogg
# Safari					/system/media/audio/ringtones/Safari.ogg
# Savannah					/system/media/audio/ringtones/Savannah.ogg
# Scarabaeus					/system/media/audio/ringtones/Scarabaeus.ogg
# Sceptrum					/system/media/audio/ringtones/Sceptrum.ogg
# Seville					/system/media/audio/ringtones/Seville.ogg
# She's All That					/system/media/audio/ringtones/Shes_All_That.ogg
# Silky Way					/system/media/audio/ringtones/SilkyWay.ogg
# Sitar Versus Sitar					/system/media/audio/ringtones/SitarVsSitar.ogg
# Solarium					/system/media/audio/ringtones/Solarium.ogg
# Springy Jalopy					/system/media/audio/ringtones/SpringyJalopy.ogg
# Steppin' Out					/system/media/audio/ringtones/Steppin_Out.ogg
# Terminated					/system/media/audio/ringtones/Terminated.ogg
# Terrible Twos					/system/media/audio/ringtones/Noises2.ogg
# Testudo					/system/media/audio/ringtones/Testudo.ogg
# Themos					/system/media/audio/ringtones/Themos.ogg
# Third Eye					/system/media/audio/ringtones/Third_Eye.ogg
# Thriller Three					/system/media/audio/ringtones/Noises3.ogg
# Thunderfoot					/system/media/audio/ringtones/Thunderfoot.ogg
# Twirl Away					/system/media/audio/ringtones/TwirlAway.ogg
# Ursa Minor					/system/media/audio/ringtones/URSAMINOR.ogg
# UrsaMinor					/system/media/audio/ringtones/UrsaMinor.ogg
# Very Alarmed					/system/media/audio/ringtones/VeryAlarmed.ogg
# Vespa					/system/media/audio/ringtones/Vespa.ogg
# World					/system/media/audio/ringtones/World.ogg
# Zeta					/system/media/audio/ringtones/Zeta.ogg
# bellcore-dr1					/system/media/audio/ringtones/bellcore-dr1.ogg
# bellcore-dr2					/system/media/audio/ringtones/bellcore-dr2.ogg
# bellcore-dr3					/system/media/audio/ringtones/bellcore-dr3.ogg
# bellcore-dr4					/system/media/audio/ringtones/bellcore-dr4.ogg
# bellcore-dr5					/system/media/audio/ringtones/bellcore-dr5.ogg
# speaker					/system/media/audio/ringtones/speaker.wav

#######################################################################
##  Account 7 Advanced Settings                                      ##
#######################################################################
# Check Domain Certificates. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P51611 = 0

# Validate Certificate Chain. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P51667 = 0

# Validate Incoming SIP Messages. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P51606 = 0

# Allow Unsolicited REFER. 0 - Disabled, 1 - Enabled, 2 - Enabled/Force Auth. Default value is 0.
# Number: 0, 1, 2
P52623 = 0

# Only Accept SIP Requests from Known Servers. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P51647 = 0

# Check SIP User ID for Incoming INVITE. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P50649 = 0

# Allow SIP Reset. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P52615 = 0

# Authenticate Incoming INVITE. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P51646 = 0

# SIP Realm Used for Challenge INVITE & NOTIFY.
# String
P52621 =

# Enable Local MOH
# Number: 0, 1 
P51657 = 0

# Virtual Account Group. -1 - Default,  0 - Virtual Account Group 1, 1 - Virtual Account Group 2, 2 - Virtual Account Group 3
# 3 - Virtual Account Group 4, 4 - Virtual Account Group 5, 5 - Virtual Account Group 6, 6 - Virtual Account Group 7, 7 - Virtual Account Group 8
# 8 - Virtual Account Group 9, 9 - Virtual Account Group 10, 10 - Virtual Account Group 11, 11 - Virtual Account Group 12, 12 - Virtual Account Group 13
# 13 - Virtual Account Group 14, 14 - Virtual Account Group 15, 15 - Virtual Account Group 16. Default value is -1.
# Number: -1 - 15 
P51691 = -1

# Special Feature. Default value is 100
# 100 - Standard, 102 - Broadsoft, 113 - China Mobile, 114 - ZTE IMS, 115 - Mobotix
# 116 - ZTE NGN, 117 - Huawei IMS, 123 - NEC, 125 - WorldStone, 129 - Telefonica Spain
# Number: 100, 102, 113, 114, 115, 116, 117, 123, 125, 129
P50624 = 100

# Feature Key Synchronization.  0 - Disable, 0 - Broadsoft/Metaswitch. Default Value is 0.
# Number: 0, 1
# P51625 = 0

# Allow Sync Phonebook via SIP Notify. 0 - No, 1 - Yes. Default is 1.
# Number: 0, 1
P52699 = 1

##############################################################################
##  Account 8 Settings                                                      ##
##############################################################################
#######################################################################
##  Account 8 General Settings                                       ##
#######################################################################
# Account Active. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P50701 = 0

# Account Name
P50717 = 

# SIP Server
P50702 = 

# SIP User ID
P50704 =

# SIP Authentication ID
P50705 =

# SIP Authentication Password
P50706 =

# Tel URI. 0 - Disable, 1 - User=Phone, 2 - Enabled. Default value is 0
# Number: 0, 1, 2
P50709 = 0

#######################################################################
##  Account 8 Network Settings                                       ##
#######################################################################
# Outbound Proxy
P50703 =

# Secondary Outbound Proxy
P51733 =

# DNS Mode.  0 - A Record, 1 - SRV, 2 - NAPTR/SRV. Default value is 0
# Number: 0, 1, 2
P50708 = 0

# DNS SRV Fail-over Mode. 0 - Default, 1 - Saved one until DNS TTL, 2 - Saved one until no response. Defualt value is 1
# Number
P52740 = 0

# Register Before DNS SRV Fail-over. 0 - No, 1 - Yes. Default Value is 0.
# Number: 0, 1
P53795 = 1

# NAT Traversal. 0 - NAT No, 1 - STUN, 2 - Keep-alive, 3 - UPnP, 4 - Auto, 5 - VPN. Default value is 2
# Number: 0, 1, 2, 3, 4, 5
P50714 = 2

# Proxy-Require
P50718 =

#######################################################################
##  Account 8 SIP Settings                                           ##
#######################################################################
# SIP Registration. 0 - No, 1 - Yes. Default is 1
# Number: 0, 1
P50710 = 1

# Unregister Before New Registration. 0 - No, 1 - All, 2 -  Instance . Default value is 0
# Number: 0, 1, 2
P50711 = 2

# Register Expiration (m). In minutes. Default value is 60
# Number: 60 - 64800
P50712 = 60

# Subscribe Expiration (m). In minutes. Default value is blank
# Number: 0 - 64800
P52751 = 60

# Re-register before Expiration (s). Default value is 0
# Number: 0 - 3600
P51730 = 0

# Registration Retry Wait Time (s). In seconds. Default value is 20
# Number: 20 - 3600
P50771 = 20

# Add Auth Header On RE-REGISTER
# 0 - No, 1- Yes
P51759 = 1

# Enable SIP OPTIONS Keep Alive. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P51797 = 0

# SIP OPTIONS Keep Alive Interval(s). Default value is 30
# Number: 1 - 64800 
P51798 = 30

# SIP OPTIONS Keep Alive Maximum Tries. Default value is 3
# Number: 3 
P51799 = 3

# Use Privacy Header. 0 - Default, 1 - No, 2 - Yes. Default value is 0
# Number: 0, 1, 2
P51738 = 0

# Use P-Preferred-Identity Header. 0 - Default, 1 - No, 2 - Yes. Default value is 0
# Number: 0, 1, 2
P51739 = 0

# SIP Transport. 0 - UDP, 1 - TCP, 2 - TLS. Default value is 0
# Number: 0, 1, 2
P50748 = 0

# Local SIP Port. Default value is 5074
# Number: 0 or 90 - 65535
P50713 = 5074

# SIP URI Scheme When Using TLS
# 0 -sip, 1 - sips. Default value is 0.
# Number: 0, 1
P51729 = 0

# Use Actual Ephemeral Port in Contact with TCP/TLS
# 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P51731 = 0

# Support SIP Instance ID. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P50789 = 1

# SIP T1 Timeout. RFC 3261 T1 value (RTT estimate)
# 50 - 0.5 sec, 100 - 1 sec, 200 - 2 sec. Default value is 50
# Number: 50, 100, 200
P50740 = 50

# SIP T2 Interval. RFC 3261 T2 value. The maximum retransmit interval for non-INVITE requests and INVITE responses
# 200 - 2 sec, 400 - 4 sec, 800 - 8 sec. Default 400
# Number: 200, 400, 800
P50741 = 400

# SIP Timer D Interval (Seconds)
# Number 0-64. Default value is 0
P51787 = 0

# Remove OBP from route. 0 - Disable, 1 - Enable. Default value is 0
# Number: 0, 1
P51705 = 0

# Enable 100rel. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P50735 = 0

#######################################################################
##  Account 8 Session Timer                                          ##
#######################################################################

# Enable Session Timer/ Session Expiration(s).  In seconds. Default value is 180 seconds.
# By default,  Session Timer is Enabled.  Session Timer is disabled if the value is 0.
# Number: 0 or 90 - 64800
P50734 = 180

# Min-SE (s). Default value is 90 seconds
# Number: 0 or 90 - 64800
P50727 = 90

# UAC Specify Refresher. 0 - Omit, 1 - UAC, 2 - UAS. Default value is 0
# Number: 0, 1, 2
P50732 = 0

# UAS Specify Refresher. 1 - UAC, 2 - UAS. Default value is 1
# Number: 1, 2
P50733 = 1

# Caller Request Timer (Request for timer when calling)
# 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1.
P50728 = 0

# Callee Request Timer. Request for timer when called (i.e. if remote party supports timer but did not request for one)
# 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P50729 = 0

# Force Timer (Still use timer when remote party does not support timer). 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P50730 = 0

# Force INVITE (Always refresh with INVITE instead of UPDATE even when remote party supports UPDATE)
# 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P50731 = 0

#######################################################################
##  Account 8 Codec Settings                                         ##
#######################################################################
# Preferred Vocoder
# First codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 103 - G722.1C, 104 - G722.1, 123 - Opus. Default value is 0
# Number: 0, 2, 8, 9, 18, 98, 103, 104, 123
P50751 = 0

# Second codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 103 - G722.1C, 104 - G722.1, 123 - Opus. Default value is 8
# Number: 0, 2, 8, 9, 18, 98, 103, 104, 123
P50752 = 8

# Third codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 103 - G722.1C, 104 - G722.1, 123 - Opus. Default value is 9
# Number: 0, 2, 8, 9, 18, 98, 103, 104, 123
P50753 = 9

# Forth codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 103 - G722.1C, 104 - G722.1, 123 - Opus. Default value is 104
# Number: 0, 2, 8, 9, 18, 98, 103, 104, 123
P50754 = 104

# Fifth codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 103 - G722.1C, 104 - G722.1, 123 - Opus. Default value is 104
# Number: 0, 2, 8, 9, 18, 98, 103, 104, 123
P50755 = 104

# Sixth codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 103 - G722.1C, 104 - G722.1, 123 - Opus. Default value is 104
# Number: 0, 2, 8, 9, 18, 98, 103, 104, 123
P50756 = 104

# Seventh codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 103 - G722.1C, 104 - G722.1, 123 - Opus. Default value is 104
# Number: 0, 2, 8, 9, 18, 98, 103, 104, 123
P50757 = 104

# Eigth codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 103 - G722.1C, 104 - G722.1, 123 - Opus. Default value is 104
# Number: 0, 2, 8, 9, 18, 98, 103, 104, 123
P50758 = 104

# Codec Negotiation Priority. 0 - Caller, 1 - Callee. Default value is 1.
# Number: 0, 1
P53761 = 1

# Use First Matching Vocoder in 200OK SDP. 0 - No, 1 - Yes. The default value is 0.
# Number: 0, 1
P51748 = 0

# iLBC Frame Size. 0 - 20 ms, 1 - 30 ms. Default value is 1.
# Number: 0, 1
P50795 = 1

# G726-32 ITU Payload. 0 - 2, 1 - Dynamic. Default value is 0.
# Number: 0, 1
P51769 = 0

# G726-32 Dynamic PT. Default value is 126.
# Number
P51765 = 126

# Opus Payload Type. Default value is 123.
P51785 = 123

# DTMF: in audio. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P51701 = 0

# DTMF: in RFC2833. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P51702 = 1

# DTMF: in SIP INFO. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P51703 = 0

# DTMF Payload Type. Default value is 101
# Number: 96 - 127
P50796 = 101

# Enable Audio RED with FEC. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P52773 = 0

# Audio FEC Payload Type. Default value is 121
# Number: 96 - 126
P52774 = 121

# Audio RED Payload Type. Default value is 124
# Number: 96 - 126
P52775 = 124

# Silence Suppression. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P50785 = 0

# Voice Frames per TX. Default value is 2
# Number: 1 - 64
P50786 = 2

#######################################################################
##  Account 8 RTP Settings                                           ##
#######################################################################
# SRTP Mode. 0 - Disable, 1 - Enabled but not forced, 2 - Enabled and forced. Default value is 0
# Number: 0, 1, 2
P50743 = 0

# SRTP Key Length. 0 - AES 128&256 bit, 1 - AES 128 bit, 2 - AES 256 bit. Default value is 0
#Number:0, 1, 2
P51783 = 0 

# Enable SRTP Key Life Time. 0 - No, 1 - Yes.
# Number: 0,1
P51763 = 1

# RTCP Destination
P51790 = 

# Symmetric RTP. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P50760 = 0

# RTP IP Filter. 0 - Disable, 1 - IP Only, 2 - IP and Port. Default value is 0
# Number: 0, 1, 2
P52726 = 0
#######################################################################
##  Account 8 Call Settings                                          ##
#######################################################################
# Play warning tone for Auto Answer Intercom. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P52772 = 1

# Send Anonymous. 0 - No, 1 - Yes (caller ID will be blocked if set to Yes). Default value is 0
# Number: 0, 1
P50721 = 0

# Intercept Anonymous Calls. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P50746 = 0

# Call Log. 0 - Log All, 1 - Log Incoming/Outgoing only (Missed Calls Not Recorded), 2 - Disable Call All. Default value is 0
# Number: 0, 1
P50742 = 0

# Ring Timeout. Default value is 60 seconds
# Number: 0 - 300
P50776 = 60

# Refer-To Use Target Contact. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P50769 = 0

# Incoming Call Rules. 0 - Block, 1 - Set Password, 2 - Auto Answer, 3 - Ringing, 4 - Disable. Default value is 4.
# Number: 0, 1, 2 ,3 ,4
P60744 = 4

# Set Password Rules. 
# Numbers
P60745

# Dial Plan Prefix
# String
P50719 =

# Disable DialPlan. 0 - No Selection, 1 - Dial Page, 2 - Contact, 4 - Incoming Call History, 8 -  Outgoing Call History, 16 - MPK & Click2Dial. 
# If need to check multiple selections, add the specific values for each selections together. Default value is 0
# Number: 0-31
P51782 = 0

# Dial Plan. Default value is { x+ | \+x+ | *x+ | *xx*x+ }
P50759 = { x+ | \+x+ | *x+ | *xx*x+ }

# Account Ringtone. See ring tone options and value in the Ring Tone Value Table below.
P50723 = content://settings/system/ringtone

# Ignore Alert-Info Header. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1
P52718 = 0

# Matching Incoming Caller ID. Matching Rule 1.
# String
P52777 =

# Matching Rule 1 Distinctive Ringtone. See ring tone options and value in the Ring Tone Value Table below.
# String
P52778 = content://settings/system/ringtone

# Matching Incoming Caller ID. Matching Rule 2.
# String
P52779 =

# Matching Rule 2 Distinctive Ringtone. See ring tone options and value in the Ring Tone Value Table below.
# String
P52780 = content://settings/system/ringtone

# Matching Incoming Caller ID. Matching Rule 3.
# String
P52781 =

# Matching Rule 3 Distinctive Ringtone. See ring tone options and value in the Ring Tone Value Table below.
# String
P52782 = content://settings/system/ringtone

############Ring Tone Value Table###############
# Web GUI Option                            Value
# Use System Ring tone                      content://settings/system/ringtone 
# Andromeda					/system/media/audio/ringtones/ANDROMEDA.ogg
# Aquila					/system/media/audio/ringtones/Aquila.ogg
# Argo Navis					/system/media/audio/ringtones/ArgoNavis.ogg
# Atria					/system/media/audio/ringtones/Atria.ogg
# Backroad					/system/media/audio/ringtones/Backroad.ogg
# Beat Plucker					/system/media/audio/ringtones/BeatPlucker.ogg
# Bell Phone					/system/media/audio/ringtones/Ring_Classic_02.ogg
# Bentley Dubs					/system/media/audio/ringtones/BentleyDubs.ogg
# Big Easy					/system/media/audio/ringtones/Big_Easy.ogg
# Bird Loop					/system/media/audio/ringtones/BirdLoop.ogg
# Bollywood					/system/media/audio/ringtones/Bollywood.ogg
# Boötes					/system/media/audio/ringtones/BOOTES.ogg
# Bus' a Move					/system/media/audio/ringtones/BussaMove.ogg
# Cairo					/system/media/audio/ringtones/Cairo.ogg
# Calypso Steel					/system/media/audio/ringtones/Calypso_Steel.ogg
# Canis Major					/system/media/audio/ringtones/CANISMAJOR.ogg
# Caribbean Ice					/system/media/audio/ringtones/CaribbeanIce.ogg
# Carina					/system/media/audio/ringtones/Carina.ogg
# Cassiopeia					/system/media/audio/ringtones/CASSIOPEIA.ogg
# Centaurus					/system/media/audio/ringtones/Centaurus.ogg
# Champagne Edition					/system/media/audio/ringtones/Champagne_Edition.ogg
# Chimey Phone					/system/media/audio/ringtones/Ring_Synth_02.ogg
# Club Cubano					/system/media/audio/ringtones/Club_Cubano.ogg
# Crayon Rock					/system/media/audio/ringtones/CrayonRock.ogg
# Crazy Dream					/system/media/audio/ringtones/CrazyDream.ogg
# Curve Ball Blend					/system/media/audio/ringtones/CurveBall.ogg
# Cygnus					/system/media/audio/ringtones/Cygnus.ogg
# Dancin' Fool					/system/media/audio/ringtones/DancinFool.ogg
# Digital Phone					/system/media/audio/ringtones/Ring_Digital_02.ogg
# Ding					/system/media/audio/ringtones/Ding.ogg
# DingDong					/system/media/audio/ringtones/DingDong.wav
# Don' Mess Wiv It					/system/media/audio/ringtones/DonMessWivIt.ogg
# Draco					/system/media/audio/ringtones/Draco.ogg
# Dream Theme					/system/media/audio/ringtones/DreamTheme.ogg
# Eastern Sky					/system/media/audio/ringtones/Eastern_Sky.ogg
# Enter the Nexus					/system/media/audio/ringtones/Enter_the_Nexus.ogg
# Eridani					/system/media/audio/ringtones/Eridani.ogg
# Ether Shake					/system/media/audio/ringtones/EtherShake.ogg
# Flutey Phone					/system/media/audio/ringtones/Ring_Synth_04.ogg
# Free Flight					/system/media/audio/ringtones/FreeFlight.ogg
# Friendly Ghost					/system/media/audio/ringtones/FriendlyGhost.ogg
# Funk Y'all					/system/media/audio/ringtones/Funk_Yall.ogg
# Game Over Guitar					/system/media/audio/ringtones/GameOverGuitar.ogg
# Gimme Mo' Town					/system/media/audio/ringtones/Gimme_Mo_Town.ogg
# Girtab					/system/media/audio/ringtones/Girtab.ogg
# Glacial Groove					/system/media/audio/ringtones/Glacial_Groove.ogg
# Growl					/system/media/audio/ringtones/Growl.ogg
# Halfway Home					/system/media/audio/ringtones/HalfwayHome.ogg
# Hydra					/system/media/audio/ringtones/Hydra.ogg
# Insert Coin					/system/media/audio/ringtones/InsertCoin.ogg
# Kuma					/system/media/audio/ringtones/Kuma.ogg
# Loopy Lounge					/system/media/audio/ringtones/LoopyLounge.ogg
# Love Flute					/system/media/audio/ringtones/LoveFlute.ogg
# Lyra					/system/media/audio/ringtones/Lyra.ogg
# Machina					/system/media/audio/ringtones/Machina.ogg
# Medieval Jaunt					/system/media/audio/ringtones/MidEvilJaunt.ogg
# Mildly Alarming					/system/media/audio/ringtones/MildlyAlarming.ogg
# Nairobi					/system/media/audio/ringtones/Nairobi.ogg
# Nassau					/system/media/audio/ringtones/Nassau.ogg
# New Player					/system/media/audio/ringtones/NewPlayer.ogg
# No Limits					/system/media/audio/ringtones/No_Limits.ogg
# Noisey One					/system/media/audio/ringtones/Noises1.ogg
# Organ Dub					/system/media/audio/ringtones/OrganDub.ogg
# Orion					/system/media/audio/ringtones/Orion.ogg
# Paradise Island					/system/media/audio/ringtones/Paradise_Island.ogg
# Pegasus					/system/media/audio/ringtones/Pegasus.ogg
# Perseus					/system/media/audio/ringtones/PERSEUS.ogg
# Playa					/system/media/audio/ringtones/Playa.ogg
# Pyxis					/system/media/audio/ringtones/Pyxis.ogg
# Rasalas					/system/media/audio/ringtones/Rasalas.ogg
# Revelation					/system/media/audio/ringtones/Revelation.ogg
# Rigel					/system/media/audio/ringtones/Rigel.ogg
# Road Trip					/system/media/audio/ringtones/Road_Trip.ogg
# Romancing The Tone					/system/media/audio/ringtones/RomancingTheTone.ogg
# Safari					/system/media/audio/ringtones/Safari.ogg
# Savannah					/system/media/audio/ringtones/Savannah.ogg
# Scarabaeus					/system/media/audio/ringtones/Scarabaeus.ogg
# Sceptrum					/system/media/audio/ringtones/Sceptrum.ogg
# Seville					/system/media/audio/ringtones/Seville.ogg
# She's All That					/system/media/audio/ringtones/Shes_All_That.ogg
# Silky Way					/system/media/audio/ringtones/SilkyWay.ogg
# Sitar Versus Sitar					/system/media/audio/ringtones/SitarVsSitar.ogg
# Solarium					/system/media/audio/ringtones/Solarium.ogg
# Springy Jalopy					/system/media/audio/ringtones/SpringyJalopy.ogg
# Steppin' Out					/system/media/audio/ringtones/Steppin_Out.ogg
# Terminated					/system/media/audio/ringtones/Terminated.ogg
# Terrible Twos					/system/media/audio/ringtones/Noises2.ogg
# Testudo					/system/media/audio/ringtones/Testudo.ogg
# Themos					/system/media/audio/ringtones/Themos.ogg
# Third Eye					/system/media/audio/ringtones/Third_Eye.ogg
# Thriller Three					/system/media/audio/ringtones/Noises3.ogg
# Thunderfoot					/system/media/audio/ringtones/Thunderfoot.ogg
# Twirl Away					/system/media/audio/ringtones/TwirlAway.ogg
# Ursa Minor					/system/media/audio/ringtones/URSAMINOR.ogg
# UrsaMinor					/system/media/audio/ringtones/UrsaMinor.ogg
# Very Alarmed					/system/media/audio/ringtones/VeryAlarmed.ogg
# Vespa					/system/media/audio/ringtones/Vespa.ogg
# World					/system/media/audio/ringtones/World.ogg
# Zeta					/system/media/audio/ringtones/Zeta.ogg
# bellcore-dr1					/system/media/audio/ringtones/bellcore-dr1.ogg
# bellcore-dr2					/system/media/audio/ringtones/bellcore-dr2.ogg
# bellcore-dr3					/system/media/audio/ringtones/bellcore-dr3.ogg
# bellcore-dr4					/system/media/audio/ringtones/bellcore-dr4.ogg
# bellcore-dr5					/system/media/audio/ringtones/bellcore-dr5.ogg
# speaker					/system/media/audio/ringtones/speaker.wav

#######################################################################
##  Account 8 Advanced Settings                                      ##
#######################################################################
# Check Domain Certificates. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P51711 = 0

# Validate Certificate Chain. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P51767 = 0

# Validate Incoming SIP Messages. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P51706 = 0

# Allow Unsolicited REFER. 0 - Disabled, 1 - Enabled, 2 - Enabled/Force Auth. Default value is 0.
# Number: 0, 1, 2
P52723 = 0

# Only Accept SIP Requests from Known Servers. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P51747 = 0

# Check SIP User ID for Incoming INVITE. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P50749 = 0

# Allow SIP Reset. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P52715 = 0

# Authenticate Incoming INVITE. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P51746 = 0

# SIP Realm Used for Challenge INVITE & NOTIFY.
# String
P52721 =

# Enable Local MOH
# Number: 0, 1 
P51757 = 0

# Virtual Account Group. -1 - Default,  0 - Virtual Account Group 1, 1 - Virtual Account Group 2, 2 - Virtual Account Group 3
# 3 - Virtual Account Group 4, 4 - Virtual Account Group 5, 5 - Virtual Account Group 6, 6 - Virtual Account Group 7, 7 - Virtual Account Group 8
# 8 - Virtual Account Group 9, 9 - Virtual Account Group 10, 10 - Virtual Account Group 11, 11 - Virtual Account Group 12, 12 - Virtual Account Group 13
# 13 - Virtual Account Group 14, 14 - Virtual Account Group 15, 15 - Virtual Account Group 16. Default value is -1.
# Number: -1 - 15 
P51791 = -1

# Special Feature. Default value is 100
# 100 - Standard, 102 - Broadsoft, 113 - China Mobile, 114 - ZTE IMS, 115 - Mobotix
# 116 - ZTE NGN, 117 - Huawei IMS, 123 - NEC, 125 - WorldStone, 129 - Telefonica Spain
# Number: 100, 102, 113, 114, 115, 116, 117, 123, 125, 129
P50724 = 100

# Feature Key Synchronization.  0 - Disable, 0 - Broadsoft/Metaswitch. Default Value is 0.
# Number: 0, 1
# P51725 = 0

# Allow Sync Phonebook via SIP Notify. 0 - No, 1 - Yes. Default is 1.
# Number: 0, 1
P52799 = 1

##############################################################################
##  Account 9 Settings                                                      ##
##############################################################################
#######################################################################
##  Account 9 General Settings                                       ##
#######################################################################
# Account Active. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P50801 = 0

# Account Name
P50817 = 

# SIP Server
P50802 = 

# SIP User ID
P50804 =

# SIP Authentication ID
P50805 =

# SIP Authentication Password
P50806 =

# Tel URI. 0 - Disable, 1 - User=Phone, 2 - Enabled. Default value is 0
# Number: 0, 1, 2
P50809 = 0

#######################################################################
##  Account 9 Network Settings                                       ##
#######################################################################
# Outbound Proxy
P50803 =

# Secondary Outbound Proxy
P51833 =

# DNS Mode.  0 - A Record, 1 - SRV, 2 - NAPTR/SRV. Default value is 0
# Number: 0, 1, 2
P50808 = 0

# DNS SRV Fail-over Mode. 0 - Default, 1 - Saved one until DNS TTL, 2 - Saved one until no response. Defualt value is 1
# Number
P52840 = 0

# Register Before DNS SRV Fail-over. 0 - No, 1 - Yes. Default Value is 0.
# Number: 0, 1
P53895 = 1

# NAT Traversal. 0 - NAT No, 1 - STUN, 2 - Keep-alive, 3 - UPnP, 4 - Auto, 5 - VPN. Default value is 2
# Number: 0, 1, 2, 3, 4, 5
P50814 = 2

# Proxy-Require
P50818 =

#######################################################################
##  Account 9 SIP Settings                                           ##
#######################################################################
# SIP Registration. 0 - No, 1 - Yes. Default is 1
# Number: 0, 1
P50810 = 1

# Unregister Before New Registration. 0 - No, 1 - All, 2 -  Instance . Default value is 0
# Number: 0, 1, 2
P50811 = 2

# Register Expiration (m). In minutes. Default value is 60
# Number: 60 - 64800
P50812 = 60

# Subscribe Expiration (m). In minutes. Default value is blank
# Number: 0 - 64800
P52851 = 60

# Re-register before Expiration (s). Default value is 0
# Number: 0 - 3600
P51830 = 0

# Registration Retry Wait Time (s). In seconds. Default value is 20
# Number: 20 - 3600
P50871 = 20

# Add Auth Header On RE-REGISTER
# 0 - No, 1- Yes
P51859 = 1

# Enable SIP OPTIONS Keep Alive. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P51897 = 0

# SIP OPTIONS Keep Alive Interval(s). Default value is 30
# Number: 1 - 64800 
P51898 = 30

# SIP OPTIONS Keep Alive Maximum Tries. Default value is 3
# Number: 3 
P51899 = 3

# Use Privacy Header. 0 - Default, 1 - No, 2 - Yes. Default value is 0
# Number: 0, 1, 2
P51838 = 0

# Use P-Preferred-Identity Header. 0 - Default, 1 - No, 2 - Yes. Default value is 0
# Number: 0, 1, 2
P51839 = 0

# SIP Transport. 0 - UDP, 1 - TCP, 2 - TLS. Default value is 0
# Number: 0, 1, 2
P50848 = 0

# Local SIP Port. Default value is 5076
# Number: 0 or 90 - 65535
P50813 = 5076

# SIP URI Scheme When Using TLS
# 0 -sip, 1 - sips. Default value is 0.
# Number: 0, 1
P51829 = 0

# Use Actual Ephemeral Port in Contact with TCP/TLS
# 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P51831 = 0

# Support SIP Instance ID. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P50889 = 1

# SIP T1 Timeout. RFC 3261 T1 value (RTT estimate)
# 50 - 0.5 sec, 100 - 1 sec, 200 - 2 sec. Default value is 50
# Number: 50, 100, 200
P50840 = 50

# SIP T2 Interval. RFC 3261 T2 value. The maximum retransmit interval for non-INVITE requests and INVITE responses
# 200 - 2 sec, 400 - 4 sec, 800 - 8 sec. Default 400
# Number: 200, 400, 800
P50841 = 400

# SIP Timer D Interval (Seconds)
# Number 0-64. Default value is 0
P51887 = 0

# Remove OBP from route. 0 - Disable, 1 - Enable. Default value is 0
# Number: 0, 1
P51805 = 0

# Enable 100rel. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P50835 = 0

#######################################################################
##  Account 9 Session Timer                                          ##
#######################################################################

# Enable Session Timer/ Session Expiration(s).  In seconds. Default value is 180 seconds.
# By default,  Session Timer is Enabled.  Session Timer is disabled if the value is 0.
# Number: 0 or 90 - 64800
P50834 = 180

# Min-SE (s). Default value is 90 seconds
# Number: 0 or 90 - 64800
P50827 = 90

# UAC Specify Refresher. 0 - Omit, 1 - UAC, 2 - UAS. Default value is 0
# Number: 0, 1, 2
P50832 = 0

# UAS Specify Refresher. 1 - UAC, 2 - UAS. Default value is 1
# Number: 1, 2
P50833 = 1

# Caller Request Timer (Request for timer when calling)
# 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1.
P50828 = 0

# Callee Request Timer. Request for timer when called (i.e. if remote party supports timer but did not request for one)
# 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P50829 = 0

# Force Timer (Still use timer when remote party does not support timer). 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P50830 = 0

# Force INVITE (Always refresh with INVITE instead of UPDATE even when remote party supports UPDATE)
# 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P50831 = 0

#######################################################################
##  Account 9 Codec Settings                                         ##
#######################################################################
# Preferred Vocoder
# First codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 103 - G722.1C, 104 - G722.1, 123 - Opus. Default value is 0
# Number: 0, 2, 8, 9, 18, 98, 103, 104, 123
P50851 = 0

# Second codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 103 - G722.1C, 104 - G722.1, 123 - Opus. Default value is 8
# Number: 0, 2, 8, 9, 18, 98, 103, 104, 123
P50852 = 8

# Third codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 103 - G722.1C, 104 - G722.1, 123 - Opus. Default value is 9
# Number: 0, 2, 8, 9, 18, 98, 103, 104, 123
P50853 = 9

# Forth codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 103 - G722.1C, 104 - G722.1, 123 - Opus. Default value is 104
# Number: 0, 2, 8, 9, 18, 98, 103, 104, 123
P50854 = 104

# Fifth codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 103 - G722.1C, 104 - G722.1, 123 - Opus. Default value is 104
# Number: 0, 2, 8, 9, 18, 98, 103, 104, 123
P50855 = 104

# Sixth codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 103 - G722.1C, 104 - G722.1, 123 - Opus. Default value is 104
# Number: 0, 2, 8, 9, 18, 98, 103, 104, 123
P50856 = 104

# Seventh codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 103 - G722.1C, 104 - G722.1, 123 - Opus. Default value is 104
# Number: 0, 2, 8, 9, 18, 98, 103, 104, 123
P50857 = 104

# Eigth codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 103 - G722.1C, 104 - G722.1, 123 - Opus. Default value is 104
# Number: 0, 2, 8, 9, 18, 98, 103, 104, 123
P50858 = 104

# Codec Negotiation Priority. 0 - Caller, 1 - Callee. Default value is 1.
# Number: 0, 1
P53861 = 1

# Use First Matching Vocoder in 200OK SDP. 0 - No, 1 - Yes. The default value is 0.
# Number: 0, 1
P51848 = 0

# iLBC Frame Size. 0 - 20 ms, 1 - 30 ms. Default value is 1.
# Number: 0, 1
P50895 = 1

# G726-32 ITU Payload. 0 - 2, 1 - Dynamic. Default value is 0.
# Number: 0, 1
P51869 = 0

# G726-32 Dynamic PT. Default value is 126.
# Number
P51865 = 126

# Opus Payload Type. Default value is 123.
P51885 = 123

# DTMF: in audio. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P51801 = 0

# DTMF: in RFC2833. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P51802 = 1

# DTMF: in SIP INFO. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P51803 = 0

# DTMF Payload Type. Default value is 101
# Number: 96 - 127
P50896 = 101

# Enable Audio RED with FEC. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P52873 = 0

# Audio FEC Payload Type. Default value is 121
# Number: 96 - 126
P52874 = 121

# Audio RED Payload Type. Default value is 124
# Number: 96 - 126
P52875 = 124

# Silence Suppression. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P50885 = 0

# Voice Frames per TX. Default valule is 2
# Number: 1 - 64
P50886 = 2

#######################################################################
##  Account 9 RTP Settings                                           ##
#######################################################################
# SRTP Mode. 0 - Disable, 1 - Enabled but not forced, 2 - Enabled and forced. Default value is 0
# Number: 0, 1, 2
P50843 = 0

# SRTP Key Length. 0 - AES 128&256 bit, 1 - AES 128 bit, 2 - AES 256 bit. Default value is 0
#Number:0, 1, 2
P51883 = 0

# Enable SRTP Key Life Time. 0 - No, 1 - Yes.
# Number: 0,1
P51863 = 1

# RTCP Destination
P51890 =

# Symmetric RTP. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P50860 = 0

# RTP IP Filter. 0 - Disable, 1 - IP Only, 2 - IP and Port. Default value is 0
# Number: 0, 1, 2
P52826 = 0

#######################################################################
##  Account 9 Call Settings                                          ##
#######################################################################
# Play warning tone for Auto Answer Intercom. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P52872 = 1

# Send Anonymous. 0 - No, 1 - Yes (caller ID will be blocked if set to Yes). Default value is 0
# Number: 0, 1
P50821 = 0

# Intercept Anonymous Calls. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P50846 = 0

# Call Log. 0 - Log All, 1 - Log Incoming/Outgoing only (Missed Calls Not Recorded), 2 - Disable Call All. Default value is 0
# Number: 0, 1
P50842 = 0

# Ring Timeout. Default value is 60 seconds
# Number: 0 - 300
P50876 = 60

# Refer-To Use Target Contact. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P50869 = 0

# Incoming Call Rules. 0 - Block, 1 - Set Password, 2 - Auto Answer, 3 - Ringing, 4 - Disable. Default value is 4.
# Number: 0, 1, 2 ,3 ,4
P60844 = 4

# Set Password Rules. 
# Numbers
P60845

# Dial Plan Prefix
# String
P50819 =

# Disable DialPlan. 0 - No Selection, 1 - Dial Page, 2 - Contact, 4 - Incoming Call History, 8 -  Outgoing Call History, 16 - MPK & Click2Dial. 
# If need to check multiple selections, add the specific values for each selections together. Default value is 0
# Number: 0-31
P51882 = 0

# Dial Plan. Default value is { x+ | \+x+ | *x+ | *xx*x+ }
P50859 = { x+ | \+x+ | *x+ | *xx*x+ }

# Account Ringtone. See ring tone options and value in the Ring Tone Value Table below.
P50823 = content://settings/system/ringtone

# Ignore Alert-Info Header. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1
P52818 = 0

# Matching Incoming Caller ID. Matching Rule 1.
# String
P52877 =

# Matching Rule 1 Distinctive Ringtone. See ring tone options and value in the Ring Tone Value Table below.
# String
P52878 = content://settings/system/ringtone

# Matching Incoming Caller ID. Matching Rule 2.
# String
P52879 =

# Matching Rule 2 Distinctive Ringtone. See ring tone options and value in the Ring Tone Value Table below.
# String
P52880 = content://settings/system/ringtone

# Matching Incoming Caller ID. Matching Rule 3.
# String
P52881 =

# Matching Rule 3 Distinctive Ringtone. See ring tone options and value in the Ring Tone Value Table below.
# String
P52882 = content://settings/system/ringtone

############Ring Tone Value Table###############
# Web GUI Option                            Value
# Use System Ring tone                      content://settings/system/ringtone 
# Andromeda					/system/media/audio/ringtones/ANDROMEDA.ogg
# Aquila					/system/media/audio/ringtones/Aquila.ogg
# Argo Navis					/system/media/audio/ringtones/ArgoNavis.ogg
# Atria					/system/media/audio/ringtones/Atria.ogg
# Backroad					/system/media/audio/ringtones/Backroad.ogg
# Beat Plucker					/system/media/audio/ringtones/BeatPlucker.ogg
# Bell Phone					/system/media/audio/ringtones/Ring_Classic_02.ogg
# Bentley Dubs					/system/media/audio/ringtones/BentleyDubs.ogg
# Big Easy					/system/media/audio/ringtones/Big_Easy.ogg
# Bird Loop					/system/media/audio/ringtones/BirdLoop.ogg
# Bollywood					/system/media/audio/ringtones/Bollywood.ogg
# Boötes					/system/media/audio/ringtones/BOOTES.ogg
# Bus' a Move					/system/media/audio/ringtones/BussaMove.ogg
# Cairo					/system/media/audio/ringtones/Cairo.ogg
# Calypso Steel					/system/media/audio/ringtones/Calypso_Steel.ogg
# Canis Major					/system/media/audio/ringtones/CANISMAJOR.ogg
# Caribbean Ice					/system/media/audio/ringtones/CaribbeanIce.ogg
# Carina					/system/media/audio/ringtones/Carina.ogg
# Cassiopeia					/system/media/audio/ringtones/CASSIOPEIA.ogg
# Centaurus					/system/media/audio/ringtones/Centaurus.ogg
# Champagne Edition					/system/media/audio/ringtones/Champagne_Edition.ogg
# Chimey Phone					/system/media/audio/ringtones/Ring_Synth_02.ogg
# Club Cubano					/system/media/audio/ringtones/Club_Cubano.ogg
# Crayon Rock					/system/media/audio/ringtones/CrayonRock.ogg
# Crazy Dream					/system/media/audio/ringtones/CrazyDream.ogg
# Curve Ball Blend					/system/media/audio/ringtones/CurveBall.ogg
# Cygnus					/system/media/audio/ringtones/Cygnus.ogg
# Dancin' Fool					/system/media/audio/ringtones/DancinFool.ogg
# Digital Phone					/system/media/audio/ringtones/Ring_Digital_02.ogg
# Ding					/system/media/audio/ringtones/Ding.ogg
# DingDong					/system/media/audio/ringtones/DingDong.wav
# Don' Mess Wiv It					/system/media/audio/ringtones/DonMessWivIt.ogg
# Draco					/system/media/audio/ringtones/Draco.ogg
# Dream Theme					/system/media/audio/ringtones/DreamTheme.ogg
# Eastern Sky					/system/media/audio/ringtones/Eastern_Sky.ogg
# Enter the Nexus					/system/media/audio/ringtones/Enter_the_Nexus.ogg
# Eridani					/system/media/audio/ringtones/Eridani.ogg
# Ether Shake					/system/media/audio/ringtones/EtherShake.ogg
# Flutey Phone					/system/media/audio/ringtones/Ring_Synth_04.ogg
# Free Flight					/system/media/audio/ringtones/FreeFlight.ogg
# Friendly Ghost					/system/media/audio/ringtones/FriendlyGhost.ogg
# Funk Y'all					/system/media/audio/ringtones/Funk_Yall.ogg
# Game Over Guitar					/system/media/audio/ringtones/GameOverGuitar.ogg
# Gimme Mo' Town					/system/media/audio/ringtones/Gimme_Mo_Town.ogg
# Girtab					/system/media/audio/ringtones/Girtab.ogg
# Glacial Groove					/system/media/audio/ringtones/Glacial_Groove.ogg
# Growl					/system/media/audio/ringtones/Growl.ogg
# Halfway Home					/system/media/audio/ringtones/HalfwayHome.ogg
# Hydra					/system/media/audio/ringtones/Hydra.ogg
# Insert Coin					/system/media/audio/ringtones/InsertCoin.ogg
# Kuma					/system/media/audio/ringtones/Kuma.ogg
# Loopy Lounge					/system/media/audio/ringtones/LoopyLounge.ogg
# Love Flute					/system/media/audio/ringtones/LoveFlute.ogg
# Lyra					/system/media/audio/ringtones/Lyra.ogg
# Machina					/system/media/audio/ringtones/Machina.ogg
# Medieval Jaunt					/system/media/audio/ringtones/MidEvilJaunt.ogg
# Mildly Alarming					/system/media/audio/ringtones/MildlyAlarming.ogg
# Nairobi					/system/media/audio/ringtones/Nairobi.ogg
# Nassau					/system/media/audio/ringtones/Nassau.ogg
# New Player					/system/media/audio/ringtones/NewPlayer.ogg
# No Limits					/system/media/audio/ringtones/No_Limits.ogg
# Noisey One					/system/media/audio/ringtones/Noises1.ogg
# Organ Dub					/system/media/audio/ringtones/OrganDub.ogg
# Orion					/system/media/audio/ringtones/Orion.ogg
# Paradise Island					/system/media/audio/ringtones/Paradise_Island.ogg
# Pegasus					/system/media/audio/ringtones/Pegasus.ogg
# Perseus					/system/media/audio/ringtones/PERSEUS.ogg
# Playa					/system/media/audio/ringtones/Playa.ogg
# Pyxis					/system/media/audio/ringtones/Pyxis.ogg
# Rasalas					/system/media/audio/ringtones/Rasalas.ogg
# Revelation					/system/media/audio/ringtones/Revelation.ogg
# Rigel					/system/media/audio/ringtones/Rigel.ogg
# Road Trip					/system/media/audio/ringtones/Road_Trip.ogg
# Romancing The Tone					/system/media/audio/ringtones/RomancingTheTone.ogg
# Safari					/system/media/audio/ringtones/Safari.ogg
# Savannah					/system/media/audio/ringtones/Savannah.ogg
# Scarabaeus					/system/media/audio/ringtones/Scarabaeus.ogg
# Sceptrum					/system/media/audio/ringtones/Sceptrum.ogg
# Seville					/system/media/audio/ringtones/Seville.ogg
# She's All That					/system/media/audio/ringtones/Shes_All_That.ogg
# Silky Way					/system/media/audio/ringtones/SilkyWay.ogg
# Sitar Versus Sitar					/system/media/audio/ringtones/SitarVsSitar.ogg
# Solarium					/system/media/audio/ringtones/Solarium.ogg
# Springy Jalopy					/system/media/audio/ringtones/SpringyJalopy.ogg
# Steppin' Out					/system/media/audio/ringtones/Steppin_Out.ogg
# Terminated					/system/media/audio/ringtones/Terminated.ogg
# Terrible Twos					/system/media/audio/ringtones/Noises2.ogg
# Testudo					/system/media/audio/ringtones/Testudo.ogg
# Themos					/system/media/audio/ringtones/Themos.ogg
# Third Eye					/system/media/audio/ringtones/Third_Eye.ogg
# Thriller Three					/system/media/audio/ringtones/Noises3.ogg
# Thunderfoot					/system/media/audio/ringtones/Thunderfoot.ogg
# Twirl Away					/system/media/audio/ringtones/TwirlAway.ogg
# Ursa Minor					/system/media/audio/ringtones/URSAMINOR.ogg
# UrsaMinor					/system/media/audio/ringtones/UrsaMinor.ogg
# Very Alarmed					/system/media/audio/ringtones/VeryAlarmed.ogg
# Vespa					/system/media/audio/ringtones/Vespa.ogg
# World					/system/media/audio/ringtones/World.ogg
# Zeta					/system/media/audio/ringtones/Zeta.ogg
# bellcore-dr1					/system/media/audio/ringtones/bellcore-dr1.ogg
# bellcore-dr2					/system/media/audio/ringtones/bellcore-dr2.ogg
# bellcore-dr3					/system/media/audio/ringtones/bellcore-dr3.ogg
# bellcore-dr4					/system/media/audio/ringtones/bellcore-dr4.ogg
# bellcore-dr5					/system/media/audio/ringtones/bellcore-dr5.ogg
# speaker					/system/media/audio/ringtones/speaker.wav

#######################################################################
##  Account 9 Advanced Settings                                      ##
#######################################################################
# Check Domain Certificates. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P51811 = 0

# Validate Certificate Chain. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P51867 = 0

# Validate Incoming SIP Messages. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P51806 = 0

# Allow Unsolicited REFER. 0 - Disabled, 1 - Enabled, 2 - Enabled/Force Auth. Default value is 0.
# Number: 0, 1, 2
P52823 = 0

# Only Accept SIP Requests from Known Servers. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P51847 = 0

# Check SIP User ID for Incoming INVITE. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P50849 = 0

# Allow SIP Reset. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P52815 = 0

# Authenticate Incoming INVITE. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P51846 = 0

# SIP Realm Used for Challenge INVITE & NOTIFY.
# String
P52821 =

# Enable Local MOH
# Number: 0, 1 
P51857 = 0

# Virtual Account Group. -1 - Default,  0 - Virtual Account Group 1, 1 - Virtual Account Group 2, 2 - Virtual Account Group 3
# 3 - Virtual Account Group 4, 4 - Virtual Account Group 5, 5 - Virtual Account Group 6, 6 - Virtual Account Group 7, 7 - Virtual Account Group 8
# 8 - Virtual Account Group 9, 9 - Virtual Account Group 10, 10 - Virtual Account Group 11, 11 - Virtual Account Group 12, 12 - Virtual Account Group 13
# 13 - Virtual Account Group 14, 14 - Virtual Account Group 15, 15 - Virtual Account Group 16. Default value is -1.
# Number: -1 - 15 
P51891 = -1

# Special Feature. Default value is 100
# 100 - Standard, 102 - Broadsoft, 113 - China Mobile, 114 - ZTE IMS, 115 - Mobotix
# 116 - ZTE NGN, 117 - Huawei IMS, 123 - NEC, 125 - WorldStone, 129 - Telefonica Spain
# Number: 100, 102, 113, 114, 115, 116, 117, 123, 125, 129
P50824 = 100

# Feature Key Synchronization.  0 - Disable, 0 - Broadsoft/Metaswitch. Default Value is 0.
# Number: 0, 1
# P51825 = 0

# Allow Sync Phonebook via SIP Notify. 0 - No, 1 - Yes. Default is 1.
# Number: 0, 1
P52899 = 1

##############################################################################
##  Account 10 Settings                                                     ##
##############################################################################
#######################################################################
##  Account 10 General Settings                                      ##
#######################################################################
# Account Active. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P50901 = 0

# Account Name
P50917 = 

# SIP Server
P50902 = 

# SIP User ID
P50904 =

# SIP Authentication ID
P50905 =

# SIP Authentication Password
P50906 =

# Tel URI. 0 - Disable, 1 - User=Phone, 2 - Enabled. Default value is 0
# Number: 0, 1, 2
P50909 = 0

#######################################################################
##  Account 10 Network Settings                                      ##
#######################################################################
# Outbound Proxy
P50903 =

# Secondary Outbound Proxy
P51933 =

# DNS Mode.  0 - A Record, 1 - SRV, 2 - NAPTR/SRV. Default value is 0
# Number: 0, 1, 2
P50908 = 0

# DNS SRV Fail-over Mode. 0 - Default, 1 - Saved one until DNS TTL, 2 - Saved one until no response. Defualt value is 1
# Number
P52940 = 0

# Register Before DNS SRV Fail-over. 0 - No, 1 - Yes. Default Value is 0.
# Number: 0, 1
P53995 = 1

# NAT Traversal. 0 - NAT No, 1 - STUN, 2 - Keep-alive, 3 - UPnP, 4 - Auto, 5 - VPN. Default value is 2
# Number: 0, 1, 2, 3, 4, 5
P50914 = 2

# Proxy-Require
P50918 =

#######################################################################
##  Account 10 SIP Settings                                          ##
#######################################################################
# SIP Registration. 0 - No, 1 - Yes. Default is 1
# Number: 0, 1
P50910 = 1

# Unregister Before New Registration. 0 - No, 1 - All, 2 -  Instance . Default value is 0
# Number: 0, 1, 2
P50911 = 2

# Register Expiration (m). In minutes. Default value is 60
# Number: 60 - 64800
P50912 = 60

# Subscribe Expiration (m). In minutes. Default value is blank
# Number: 0 - 64800
P52951 = 60

# Re-register before Expiration (s). Default value is 0
# Number: 0 - 3600
P51930 = 0

# Registration Retry Wait Time (s). In seconds. Default value is 20
# Number: 20 - 3600
P50971 = 20

# Add Auth Header On RE-REGISTER
# 0 - No, 1- Yes
P51959 = 1

# Enable SIP OPTIONS Keep Alive. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P51997 = 0

# SIP OPTIONS Keep Alive Interval(s). Default value is 30
# Number: 1 - 64800 
P51998 = 30

# SIP OPTIONS Keep Alive Maximum Tries. Default value is 3
# Number: 3 
P51999 = 3

# Use Privacy Header. 0 - Default, 1 - No, 2 - Yes. Default value is 0
# Number: 0, 1, 2
P51938 = 0

# Use P-Preferred-Identity Header. 0 - Default, 1 - No, 2 - Yes. Default value is 0
# Number: 0, 1, 2
P51939 = 0

# SIP Transport. 0 - UDP, 1 - TCP, 2 - TLS. Default value is 0
# Number: 0, 1, 2
P50948 = 0

# Local SIP Port. Default value is 5078
# Number: 0 or 90 - 65535
P50913 = 5078

# SIP URI Scheme When Using TLS
# 0 -sip, 1 - sips. Default value is 0.
# Number: 0, 1
P51929 = 0

# Use Actual Ephemeral Port in Contact with TCP/TLS
# 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P51931 = 0

# Support SIP Instance ID. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P50989 = 1

# SIP T1 Timeout. RFC 3261 T1 value (RTT estimate)
# 50 - 0.5 sec, 100 - 1 sec, 200 - 2 sec. Default value is 50
# Number: 50, 100, 200
P50940 = 50

# SIP T2 Interval. RFC 3261 T2 value. The maximum retransmit interval for non-INVITE requests and INVITE responses
# 200 - 2 sec, 400 - 4 sec, 800 - 8 sec. Default 400
# Number: 200, 400, 800
P50941 = 400

# SIP Timer D Interval (Seconds)
# Number 0-64. Default value is 0
P51987 = 0

# Remove OBP from route. 0 - Disable, 1 - Enable. Default value is 0
# Number: 0, 1
P51905 = 0

# Enable 100rel. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P50935 = 0

#######################################################################
##  Account 10 Session Timer                                          ##
#######################################################################

# Enable Session Timer/ Session Expiration(s).  In seconds. Default value is 180 seconds.
# By default,  Session Timer is Enabled.  Session Timer is disabled if the value is 0.
# Number: 0 or 90 - 64800
P50934 = 180

# Min-SE (s). Default value is 90 seconds
# Number: 0 or 90 - 64800
P50927 = 90

# UAC Specify Refresher. 0 - Omit, 1 - UAC, 2 - UAS. Default value is 0
# Number: 0, 1, 2
P50932 = 0

# UAS Specify Refresher. 1 - UAC, 2 - UAS. Default value is 1
# Number: 1, 2
P50933 = 1

# Caller Request Timer (Request for timer when calling)
# 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1.
P50928 = 0

# Callee Request Timer. Request for timer when called (i.e. if remote party supports timer but did not request for one)
# 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P50929 = 0

# Force Timer (Still use timer when remote party does not support timer). 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P50930 = 0

# Force INVITE (Always refresh with INVITE instead of UPDATE even when remote party supports UPDATE)
# 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P50931 = 0

#######################################################################
##  Account 10 Codec Settings                                         ##
#######################################################################
# Preferred Vocoder
# First codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 103 - G722.1C, 104 - G722.1, 123 - Opus. Default value is 0
# Number: 0, 2, 8, 9, 18, 98, 103, 104, 123
P50951 = 0

# Second codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 103 - G722.1C, 104 - G722.1, 123 - Opus. Default value is 8
# Number: 0, 2, 8, 9, 18, 98, 103, 104, 123
P50952 = 8

# Third codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 103 - G722.1C, 104 - G722.1, 123 - Opus. Default value is 9
# Number: 0, 2, 8, 9, 18, 98, 103, 104, 123
P50953 = 9

# Forth codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 103 - G722.1C, 104 - G722.1, 123 - Opus. Default value is 104
# Number: 0, 2, 8, 9, 18, 98, 103, 104, 123
P50954 = 104

# Fifth codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 103 - G722.1C, 104 - G722.1, 123 - Opus. Default value is 104
# Number: 0, 2, 8, 9, 18, 98, 103, 104, 123
P50955 = 104

# Sixth codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 103 - G722.1C, 104 - G722.1, 123 - Opus. Default value is 104
# Number: 0, 2, 8, 9, 18, 98, 103, 104, 123
P50956 = 104

# Seventh codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 103 - G722.1C, 104 - G722.1, 123 - Opus. Default value is 104
# Number: 0, 2, 8, 9, 18, 98, 103, 104, 123
P50957 = 104

# Eigth codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 103 - G722.1C, 104 - G722.1, 123 - Opus. Default value is 104
# Number: 0, 2, 8, 9, 18, 98, 103, 104, 123
P50958 = 104

# Codec Negotiation Priority. 0 - Caller, 1 - Callee. Default value is 1.
# Number: 0, 1
P53961 = 1

# Use First Matching Vocoder in 200OK SDP. 0 - No, 1 - Yes. The default value is 0.
# Number: 0, 1
P51948 = 0

# iLBC Frame Size. 0 - 20 ms, 1 - 30 ms. Default value is 1.
# Number: 0, 1
P50995 = 1

# G726-32 ITU Payload. 0 - 2, 1 - Dynamic. Default value is 0.
# Number: 0, 1
P51969 = 0

# G726-32 Dynamic PT. Default value is 126.
# Number
P51965 = 126

# Opus Payload Type. Default value is 123.
P51985 = 123

# DTMF: in audio. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P51901 = 0

# DTMF: in RFC2833. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P51902 = 1

# DTMF: in SIP INFO. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P51903 = 0

# DTMF Payload Type. Default value is 101
# Number: 96 - 127
P50996 = 101

# Enable Audio RED with FEC. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P52973 = 0

# Audio FEC Payload Type. Default value is 121
# Number: 96 - 126
P52974 = 121

# Audio RED Payload Type. Default value is 124
# Number: 96 - 126
P52975 = 124

# Silence Suppression. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P50985 = 0

# Voice Frames per TX. Default valule is 2
# Number: 1 - 64
P50986 = 2

#######################################################################
##  Account 10 RTP Settings                                          ##
#######################################################################
# SRTP Mode. 0 - Disable, 1 - Enabled but not forced, 2 - Enabled and forced. Default value is 0
# Number: 0, 1, 2
P50943 = 0

# SRTP Key Length. 0 - AES 128&256 bit, 1 - AES 128 bit, 2 - AES 256 bit. Default value is 0
#Number:0, 1, 2
P51983 = 0

# Enable SRTP Key Life Time. 0 - No, 1 - Yes.
# Number: 0,1
P51963 = 1

# RTCP Destination
P51990 = 

# Symmetric RTP. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P50960 = 0

# RTP IP Filter. 0 - Disable, 1 - IP Only, 2 - IP and Port. Default value is 0
# Number: 0, 1, 2
P52926 = 0

#######################################################################
##  Account 10 Call Settings                                          ##
#######################################################################
# Play warning tone for Auto Answer Intercom. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P52972 = 1

# Send Anonymous. 0 - No, 1 - Yes (caller ID will be blocked if set to Yes). Default value is 0
# Number: 0, 1
P50921 = 0

# Intercept Anonymous Calls. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P50946 = 0

# Call Log. 0 - Log All, 1 - Log Incoming/Outgoing only (Missed Calls Not Recorded), 2 - Disable Call All. Default value is 0
# Number: 0, 1
P50942 = 0

# Ring Timeout. Default value is 60 seconds
# Number: 0 - 300
P50976 = 60

# Refer-To Use Target Contact. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P50969 = 0

# Incoming Call Rules. 0 - Block, 1 - Set Password, 2 - Auto Answer, 3 - Ringing, 4 - Disable. Default value is 4.
# Number: 0, 1, 2 ,3 ,4
P60944 = 4

# Set Password Rules. 
# Numbers
P60945

# Dial Plan Prefix
# String
P50919 =

# Disable DialPlan. 0 - No Selection, 1 - Dial Page, 2 - Contact, 4 - Incoming Call History, 8 -  Outgoing Call History, 16 - MPK & Click2Dial. 
# If need to check multiple selections, add the specific values for each selections together. Default value is 0
# Number: 0-31
P51982 = 0

# Dial Plan. Default value is { x+ | \+x+ | *x+ | *xx*x+ }
P50959 = { x+ | \+x+ | *x+ | *xx*x+ }

# Account Ringtone. See ring tone options and value in the Ring Tone Value Table below.
P50923 = content://settings/system/ringtone

# Ignore Alert-Info Header. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1
P52918 = 0

# Matching Incoming Caller ID. Matching Rule 1.
# String
P52977 =

# Matching Rule 1 Distinctive Ringtone. See ring tone options and value in the Ring Tone Value Table below.
# String
P52978 = content://settings/system/ringtone

# Matching Incoming Caller ID. Matching Rule 2.
# String
P52979 =

# Matching Rule 2 Distinctive Ringtone. See ring tone options and value in the Ring Tone Value Table below.
# String
P52980 = content://settings/system/ringtone

# Matching Incoming Caller ID. Matching Rule 3.
# String
P52981 =

# Matching Rule 3 Distinctive Ringtone. See ring tone options and value in the Ring Tone Value Table below.
# String
P52982 = content://settings/system/ringtone

############Ring Tone Value Table###############
# Web GUI Option                            Value
# Use System Ring tone                      content://settings/system/ringtone 
# Andromeda					/system/media/audio/ringtones/ANDROMEDA.ogg
# Aquila					/system/media/audio/ringtones/Aquila.ogg
# Argo Navis					/system/media/audio/ringtones/ArgoNavis.ogg
# Atria					/system/media/audio/ringtones/Atria.ogg
# Backroad					/system/media/audio/ringtones/Backroad.ogg
# Beat Plucker					/system/media/audio/ringtones/BeatPlucker.ogg
# Bell Phone					/system/media/audio/ringtones/Ring_Classic_02.ogg
# Bentley Dubs					/system/media/audio/ringtones/BentleyDubs.ogg
# Big Easy					/system/media/audio/ringtones/Big_Easy.ogg
# Bird Loop					/system/media/audio/ringtones/BirdLoop.ogg
# Bollywood					/system/media/audio/ringtones/Bollywood.ogg
# Boötes					/system/media/audio/ringtones/BOOTES.ogg
# Bus' a Move					/system/media/audio/ringtones/BussaMove.ogg
# Cairo					/system/media/audio/ringtones/Cairo.ogg
# Calypso Steel					/system/media/audio/ringtones/Calypso_Steel.ogg
# Canis Major					/system/media/audio/ringtones/CANISMAJOR.ogg
# Caribbean Ice					/system/media/audio/ringtones/CaribbeanIce.ogg
# Carina					/system/media/audio/ringtones/Carina.ogg
# Cassiopeia					/system/media/audio/ringtones/CASSIOPEIA.ogg
# Centaurus					/system/media/audio/ringtones/Centaurus.ogg
# Champagne Edition					/system/media/audio/ringtones/Champagne_Edition.ogg
# Chimey Phone					/system/media/audio/ringtones/Ring_Synth_02.ogg
# Club Cubano					/system/media/audio/ringtones/Club_Cubano.ogg
# Crayon Rock					/system/media/audio/ringtones/CrayonRock.ogg
# Crazy Dream					/system/media/audio/ringtones/CrazyDream.ogg
# Curve Ball Blend					/system/media/audio/ringtones/CurveBall.ogg
# Cygnus					/system/media/audio/ringtones/Cygnus.ogg
# Dancin' Fool					/system/media/audio/ringtones/DancinFool.ogg
# Digital Phone					/system/media/audio/ringtones/Ring_Digital_02.ogg
# Ding					/system/media/audio/ringtones/Ding.ogg
# DingDong					/system/media/audio/ringtones/DingDong.wav
# Don' Mess Wiv It					/system/media/audio/ringtones/DonMessWivIt.ogg
# Draco					/system/media/audio/ringtones/Draco.ogg
# Dream Theme					/system/media/audio/ringtones/DreamTheme.ogg
# Eastern Sky					/system/media/audio/ringtones/Eastern_Sky.ogg
# Enter the Nexus					/system/media/audio/ringtones/Enter_the_Nexus.ogg
# Eridani					/system/media/audio/ringtones/Eridani.ogg
# Ether Shake					/system/media/audio/ringtones/EtherShake.ogg
# Flutey Phone					/system/media/audio/ringtones/Ring_Synth_04.ogg
# Free Flight					/system/media/audio/ringtones/FreeFlight.ogg
# Friendly Ghost					/system/media/audio/ringtones/FriendlyGhost.ogg
# Funk Y'all					/system/media/audio/ringtones/Funk_Yall.ogg
# Game Over Guitar					/system/media/audio/ringtones/GameOverGuitar.ogg
# Gimme Mo' Town					/system/media/audio/ringtones/Gimme_Mo_Town.ogg
# Girtab					/system/media/audio/ringtones/Girtab.ogg
# Glacial Groove					/system/media/audio/ringtones/Glacial_Groove.ogg
# Growl					/system/media/audio/ringtones/Growl.ogg
# Halfway Home					/system/media/audio/ringtones/HalfwayHome.ogg
# Hydra					/system/media/audio/ringtones/Hydra.ogg
# Insert Coin					/system/media/audio/ringtones/InsertCoin.ogg
# Kuma					/system/media/audio/ringtones/Kuma.ogg
# Loopy Lounge					/system/media/audio/ringtones/LoopyLounge.ogg
# Love Flute					/system/media/audio/ringtones/LoveFlute.ogg
# Lyra					/system/media/audio/ringtones/Lyra.ogg
# Machina					/system/media/audio/ringtones/Machina.ogg
# Medieval Jaunt					/system/media/audio/ringtones/MidEvilJaunt.ogg
# Mildly Alarming					/system/media/audio/ringtones/MildlyAlarming.ogg
# Nairobi					/system/media/audio/ringtones/Nairobi.ogg
# Nassau					/system/media/audio/ringtones/Nassau.ogg
# New Player					/system/media/audio/ringtones/NewPlayer.ogg
# No Limits					/system/media/audio/ringtones/No_Limits.ogg
# Noisey One					/system/media/audio/ringtones/Noises1.ogg
# Organ Dub					/system/media/audio/ringtones/OrganDub.ogg
# Orion					/system/media/audio/ringtones/Orion.ogg
# Paradise Island					/system/media/audio/ringtones/Paradise_Island.ogg
# Pegasus					/system/media/audio/ringtones/Pegasus.ogg
# Perseus					/system/media/audio/ringtones/PERSEUS.ogg
# Playa					/system/media/audio/ringtones/Playa.ogg
# Pyxis					/system/media/audio/ringtones/Pyxis.ogg
# Rasalas					/system/media/audio/ringtones/Rasalas.ogg
# Revelation					/system/media/audio/ringtones/Revelation.ogg
# Rigel					/system/media/audio/ringtones/Rigel.ogg
# Road Trip					/system/media/audio/ringtones/Road_Trip.ogg
# Romancing The Tone					/system/media/audio/ringtones/RomancingTheTone.ogg
# Safari					/system/media/audio/ringtones/Safari.ogg
# Savannah					/system/media/audio/ringtones/Savannah.ogg
# Scarabaeus					/system/media/audio/ringtones/Scarabaeus.ogg
# Sceptrum					/system/media/audio/ringtones/Sceptrum.ogg
# Seville					/system/media/audio/ringtones/Seville.ogg
# She's All That					/system/media/audio/ringtones/Shes_All_That.ogg
# Silky Way					/system/media/audio/ringtones/SilkyWay.ogg
# Sitar Versus Sitar					/system/media/audio/ringtones/SitarVsSitar.ogg
# Solarium					/system/media/audio/ringtones/Solarium.ogg
# Springy Jalopy					/system/media/audio/ringtones/SpringyJalopy.ogg
# Steppin' Out					/system/media/audio/ringtones/Steppin_Out.ogg
# Terminated					/system/media/audio/ringtones/Terminated.ogg
# Terrible Twos					/system/media/audio/ringtones/Noises2.ogg
# Testudo					/system/media/audio/ringtones/Testudo.ogg
# Themos					/system/media/audio/ringtones/Themos.ogg
# Third Eye					/system/media/audio/ringtones/Third_Eye.ogg
# Thriller Three					/system/media/audio/ringtones/Noises3.ogg
# Thunderfoot					/system/media/audio/ringtones/Thunderfoot.ogg
# Twirl Away					/system/media/audio/ringtones/TwirlAway.ogg
# Ursa Minor					/system/media/audio/ringtones/URSAMINOR.ogg
# UrsaMinor					/system/media/audio/ringtones/UrsaMinor.ogg
# Very Alarmed					/system/media/audio/ringtones/VeryAlarmed.ogg
# Vespa					/system/media/audio/ringtones/Vespa.ogg
# World					/system/media/audio/ringtones/World.ogg
# Zeta					/system/media/audio/ringtones/Zeta.ogg
# bellcore-dr1					/system/media/audio/ringtones/bellcore-dr1.ogg
# bellcore-dr2					/system/media/audio/ringtones/bellcore-dr2.ogg
# bellcore-dr3					/system/media/audio/ringtones/bellcore-dr3.ogg
# bellcore-dr4					/system/media/audio/ringtones/bellcore-dr4.ogg
# bellcore-dr5					/system/media/audio/ringtones/bellcore-dr5.ogg
# speaker					/system/media/audio/ringtones/speaker.wav

#######################################################################
##  Account 10 Advanced Settings                                      ##
#######################################################################
# Check Domain Certificates. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P51911 = 0

# Validate Certificate Chain. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P51967 = 0

# Validate Incoming SIP Messages. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P51906 = 0

# Allow Unsolicited REFER. 0 - Disabled, 1 - Enabled, 2 - Enabled/Force Auth. Default value is 0.
# Number: 0, 1, 2
P52923 = 0

# Only Accept SIP Requests from Known Servers. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P51947 = 0

# Check SIP User ID for Incoming INVITE. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P50949 = 0

# Allow SIP Reset. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P52915 = 0

# Authenticate Incoming INVITE. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P51946 = 0

# SIP Realm Used for Challenge INVITE & NOTIFY.
# String
P52921 =

# Enable Local MOH
# Number: 0, 1 
P51957 = 0

# Virtual Account Group. -1 - Default,  0 - Virtual Account Group 1, 1 - Virtual Account Group 2, 2 - Virtual Account Group 3
# 3 - Virtual Account Group 4, 4 - Virtual Account Group 5, 5 - Virtual Account Group 6, 6 - Virtual Account Group 7, 7 - Virtual Account Group 8
# 8 - Virtual Account Group 9, 9 - Virtual Account Group 10, 10 - Virtual Account Group 11, 11 - Virtual Account Group 12, 12 - Virtual Account Group 13
# 13 - Virtual Account Group 14, 14 - Virtual Account Group 15, 15 - Virtual Account Group 16. Default value is -1.
# Number: -1 - 15 
P51991 = -1

# Special Feature. Default value is 100
# 100 - Standard, 102 - Broadsoft, 113 - China Mobile, 114 - ZTE IMS, 115 - Mobotix
# 116 - ZTE NGN, 117 - Huawei IMS, 123 - NEC, 125 - WorldStone, 129 - Telefonica Spain
# Number: 100, 102, 113, 114, 115, 116, 117, 123, 125, 129
P50924 = 100

# Feature Key Synchronization.  0 - Disable, 0 - Broadsoft/Metaswitch. Default Value is 0.
# Number: 0, 1
# P51925 = 0

# Allow Sync Phonebook via SIP Notify. 0 - No, 1 - Yes. Default is 1.
# Number: 0, 1
P52999 = 1

##############################################################################
##  Account 11 Settings                                                     ##
##############################################################################
#######################################################################
##  Account 11 General Settings                                      ##
#######################################################################
# Account Active. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P51001 = 0

# Account Name
P51017 = 

# SIP Server
P51002 =

# SIP User ID
P51004 =

# SIP Authentication ID
P51005 =

# SIP Authentication Password
P51006 =

# Tel URI. 0 - Disable, 1 - User=Phone, 2 - Enabled. Default value is 0
# Number: 0, 1, 2
P51009 = 0

#######################################################################
##  Account 11 Network Settings                                      ##
#######################################################################
# Outbound Proxy
P51003 =

# Secondary Outbound Proxy
P52033 =

# DNS Mode.  0 - A Record, 1 - SRV, 2 - NAPTR/SRV. Default value is 0
# Number: 0, 1, 2
P51008 = 0

# DNS SRV Fail-over Mode. 0 - Default, 1 - Saved one until DNS TTL, 2 - Saved one until no response. Defualt value is 1
# Number
P53040 = 0

# Register Before DNS SRV Fail-over. 0 - No, 1 - Yes. Default Value is 0.
# Number: 0, 1
P54095 = 1

# NAT Traversal. 0 - NAT No, 1 - STUN, 2 - Keep-alive, 3 - UPnP, 4 - Auto, 5 - VPN. Default value is 2
# Number: 0, 1, 2, 3, 4, 5
P51014 = 2

# Proxy-Require
P51018 =

#######################################################################
##  Account 11 SIP Settings                                          ##
#######################################################################
# SIP Registration. 0 - No, 1 - Yes. Default is 1
# Number: 0, 1
P51010 = 1

# Unregister Before New Registration. 0 - No, 1 - All, 2 -  Instance . Default value is 0
# Number: 0, 1, 2
P51011 = 2

# Register Expiration (m). In minutes. Default value is 60
# Number: 60 - 64800
P51012 = 60

# Subscribe Expiration (m). In minutes. Default value is blank
# Number: 0 - 64800
P53051 = 60

# Re-register before Expiration (s). Default value is 0
# Number: 0 - 3600
P52030 = 0

# Registration Retry Wait Time (s). In seconds. Default value is 20
# Number: 20 - 3600
P51071 = 20

# Add Auth Header On RE-REGISTER
# 0 - No, 1- Yes
P52059 = 1

# Enable SIP OPTIONS Keep Alive. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P52097 = 0

# SIP OPTIONS Keep Alive Interval(s). Default value is 30
# Number: 1 - 64800 
P52098 = 30

# SIP OPTIONS Keep Alive Maximum Tries. Default value is 3
# Number: 3 
P52099 = 3

# Use Privacy Header. 0 - Default, 1 - No, 2 - Yes. Default value is 0
# Number: 0, 1, 2
P52038 = 0

# Use P-Preferred-Identity Header. 0 - Default, 1 - No, 2 - Yes. Default value is 0
# Number: 0, 1, 2
P52039 = 0

# SIP Transport. 0 - UDP, 1 - TCP, 2 - TLS. Default value is 0
# Number: 0, 1, 2
P51048 = 0

# Local SIP Port. Default value is 5080
# Number: 0 or 90 - 65535
P51013 = 5080

# SIP URI Scheme When Using TLS
# 0 -sip, 1 - sips. Default value is 0.
# Number: 0, 1
P52029 = 0

# Use Actual Ephemeral Port in Contact with TCP/TLS
# 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P52031 = 0

# Support SIP Instance ID. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P51089 = 1

# SIP T1 Timeout. RFC 3261 T1 value (RTT estimate)
# 50 - 0.5 sec, 100 - 1 sec, 200 - 2 sec. Default value is 50
# Number: 50, 100, 200
P51040 = 50

# SIP T2 Interval. RFC 3261 T2 value. The maximum retransmit interval for non-INVITE requests and INVITE responses
# 200 - 2 sec, 400 - 4 sec, 800 - 8 sec. Default 400
# Number: 200, 400, 800
P51041 = 400

# SIP Timer D Interval (Seconds)
# Number 0-64. Default value is 0
P52087 = 0

# Remove OBP from route. 0 - Disable, 1 - Enable. Default value is 0
# Number: 0, 1
P52005 = 0

# Enable 100rel. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P51035 = 0

#######################################################################
##  Account 11 Session Timer                                          ##
#######################################################################

# Enable Session Timer/ Session Expiration(s).  In seconds. Default value is 180 seconds.
# By default,  Session Timer is Enabled.  Session Timer is disabled if the value is 0.
# Number: 0 or 90 - 64800
P51034 = 180

# Min-SE (s). Default value is 90 seconds
# Number: 0 or 90 - 64800
P51027 = 90

# UAC Specify Refresher. 0 - Omit, 1 - UAC, 2 - UAS. Default value is 0
# Number: 0, 1, 2
P51032 = 0

# UAS Specify Refresher. 1 - UAC, 2 - UAS. Default value is 1
# Number: 1, 2
P51033 = 1

# Caller Request Timer (Request for timer when calling)
# 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1.
P51028 = 0

# Callee Request Timer. Request for timer when called (i.e. if remote party supports timer but did not request for one)
# 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P51029 = 0

# Force Timer (Still use timer when remote party does not support timer). 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P51030 = 0

# Force INVITE (Always refresh with INVITE instead of UPDATE even when remote party supports UPDATE)
# 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P51031 = 0

#######################################################################
##  Account 11 Codec Settings                                         ##
#######################################################################
# Preferred Vocoder
# First codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 103 - G722.1C, 104 - G722.1, 123 - Opus. Default value is 0
# Number: 0, 2, 8, 9, 18, 98, 103, 104, 123
P51051 = 0

# Second codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 103 - G722.1C, 104 - G722.1, 123 - Opus. Default value is 8
# Number: 0, 2, 8, 9, 18, 98, 103, 104, 123
P51052 = 8

# Third codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 103 - G722.1C, 104 - G722.1, 123 - Opus. Default value is 9
# Number: 0, 2, 8, 9, 18, 98, 103, 104, 123
P51053 = 9

# Forth codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 103 - G722.1C, 104 - G722.1, 123 - Opus. Default value is 104
# Number: 0, 2, 8, 9, 18, 98, 103, 104, 123
P51054 = 104

# Fifth codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 103 - G722.1C, 104 - G722.1, 123 - Opus. Default value is 104
# Number: 0, 2, 8, 9, 18, 98, 103, 104, 123
P51055 = 104

# Sixth codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 103 - G722.1C, 104 - G722.1, 123 - Opus. Default value is 104
# Number: 0, 2, 8, 9, 18, 98, 103, 104, 123
P51056 = 104

# Seventh codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 103 - G722.1C, 104 - G722.1, 123 - Opus. Default value is 104
# Number: 0, 2, 8, 9, 18, 98, 103, 104, 123
P51057 = 104

# Eigth codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 103 - G722.1C, 104 - G722.1, 123 - Opus. Default value is 104
# Number: 0, 2, 8, 9, 18, 98, 103, 104, 123
P51058 = 104

# Codec Negotiation Priority. 0 - Caller, 1 - Callee. Default value is 1.
# Number: 0, 1
P54061 = 1

# Use First Matching Vocoder in 200OK SDP. 0 - No, 1 - Yes. The default value is 0.
# Number: 0, 1
P52048 = 0

# iLBC Frame Size. 0 - 20 ms, 1 - 30 ms. Default value is 1.
# Number: 0, 1
P51095 = 1

# G726-32 ITU Payload. 0 - 2, 1 - Dynamic. Default value is 0.
# Number: 0, 1
P52069 = 0

# G726-32 Dynamic PT. Default value is 126.
# Number
P52065 = 126

# Opus Payload Type. Default value is 123.
P52085 = 123

# DTMF: in audio. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P52001 = 0

# DTMF: in RFC2833. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P52002 = 1

# DTMF: in SIP INFO. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P52003 = 0

# DTMF Payload Type. Default value is 101
# Number: 96 - 127
P51096 = 101

# Enable Audio RED with FEC. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P53073 = 0

# Audio FEC Payload Type. Default value is 121
# Number: 96 - 126
P53074 = 121

# Audio RED Payload Type. Default value is 124
# Number: 96 - 126
P53075 = 124

# Silence Suppression. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P51085 = 0

# Voice Frames per TX. Default valule is 2
# Number: 1 - 64
P51086 = 2

#######################################################################
##  Account 11 RTP Settings                                          ##
#######################################################################
# SRTP Mode. 0 - Disable, 1 - Enabled but not forced, 2 - Enabled and forced. Default value is 0
# Number: 0, 1, 2
P51043 = 0

# SRTP Key Length. 0 - AES 128&256 bit, 1 - AES 128 bit, 2 - AES 256 bit. Default value is 0
#Number:0, 1, 2
P52083 = 0 

# Enable SRTP Key Life Time. 0 - No, 1 - Yes.
# Number: 0,1
P52063 = 1

# RTCP Destination
P52090 = 

# Symmetric RTP. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P51060 = 0

# RTP IP Filter. 0 - Disable, 1 - IP Only, 2 - IP and Port. Default value is 0
# Number: 0, 1, 2
P53026 = 0
#######################################################################
##  Account 11 Call Settings                                          ##
#######################################################################
# Play warning tone for Auto Answer Intercom. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P53072 = 1

# Send Anonymous. 0 - No, 1 - Yes (caller ID will be blocked if set to Yes). Default value is 0
# Number: 0, 1
P51021 = 0

# Intercept Anonymous Calls. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P51046 = 0

# Call Log. 0 - Log All, 1 - Log Incoming/Outgoing only (Missed Calls Not Recorded), 2 - Disable Call All. Default value is 0
# Number: 0, 1
P51042 = 0

# Ring Timeout. Default value is 60 seconds
# Number: 0 - 300
P51076 = 60

# Refer-To Use Target Contact. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P51069 = 0

# Incoming Call Rules. 0 - Block, 1 - Set Password, 2 - Auto Answer, 3 - Ringing, 4 - Disable. Default value is 4.
# Number: 0, 1, 2 ,3 ,4
P61044 = 4

# Set Password Rules. 
# Numbers
P61045

# Dial Plan Prefix
# String
P51019 =

# Disable DialPlan. 0 - No Selection, 1 - Dial Page, 2 - Contact, 4 - Incoming Call History, 8 -  Outgoing Call History, 16 - MPK & Click2Dial. 
# If need to check multiple selections, add the specific values for each selections together. Default value is 0
# Number: 0-31
P52082 = 0

# Dial Plan. Default value is { x+ | \+x+ | *x+ | *xx*x+ }
P51059 = { x+ | \+x+ | *x+ | *xx*x+ }

# Account Ringtone. See ring tone options and value in the Ring Tone Value Table below.
P51023 = content://settings/system/ringtone

# Ignore Alert-Info Header. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1
P53018 = 0

# Matching Incoming Caller ID. Matching Rule 1.
# String
P53077 =

# Matching Rule 1 Distinctive Ringtone. See ring tone options and value in the Ring Tone Value Table below.
# String
P53078 = content://settings/system/ringtone

# Matching Incoming Caller ID. Matching Rule 2.
# String
P53079 =

# Matching Rule 2 Distinctive Ringtone. See ring tone options and value in the Ring Tone Value Table below.
# String
P53080 = content://settings/system/ringtone

# Matching Incoming Caller ID. Matching Rule 3.
# String
P53081 =

# Matching Rule 3 Distinctive Ringtone. See ring tone options and value in the Ring Tone Value Table below.
# String
P53082 = content://settings/system/ringtone

############Ring Tone Value Table###############
# Web GUI Option                            Value
# Use System Ring tone                      content://settings/system/ringtone 
# Andromeda					/system/media/audio/ringtones/ANDROMEDA.ogg
# Aquila					/system/media/audio/ringtones/Aquila.ogg
# Argo Navis					/system/media/audio/ringtones/ArgoNavis.ogg
# Atria					/system/media/audio/ringtones/Atria.ogg
# Backroad					/system/media/audio/ringtones/Backroad.ogg
# Beat Plucker					/system/media/audio/ringtones/BeatPlucker.ogg
# Bell Phone					/system/media/audio/ringtones/Ring_Classic_02.ogg
# Bentley Dubs					/system/media/audio/ringtones/BentleyDubs.ogg
# Big Easy					/system/media/audio/ringtones/Big_Easy.ogg
# Bird Loop					/system/media/audio/ringtones/BirdLoop.ogg
# Bollywood					/system/media/audio/ringtones/Bollywood.ogg
# Boötes					/system/media/audio/ringtones/BOOTES.ogg
# Bus' a Move					/system/media/audio/ringtones/BussaMove.ogg
# Cairo					/system/media/audio/ringtones/Cairo.ogg
# Calypso Steel					/system/media/audio/ringtones/Calypso_Steel.ogg
# Canis Major					/system/media/audio/ringtones/CANISMAJOR.ogg
# Caribbean Ice					/system/media/audio/ringtones/CaribbeanIce.ogg
# Carina					/system/media/audio/ringtones/Carina.ogg
# Cassiopeia					/system/media/audio/ringtones/CASSIOPEIA.ogg
# Centaurus					/system/media/audio/ringtones/Centaurus.ogg
# Champagne Edition					/system/media/audio/ringtones/Champagne_Edition.ogg
# Chimey Phone					/system/media/audio/ringtones/Ring_Synth_02.ogg
# Club Cubano					/system/media/audio/ringtones/Club_Cubano.ogg
# Crayon Rock					/system/media/audio/ringtones/CrayonRock.ogg
# Crazy Dream					/system/media/audio/ringtones/CrazyDream.ogg
# Curve Ball Blend					/system/media/audio/ringtones/CurveBall.ogg
# Cygnus					/system/media/audio/ringtones/Cygnus.ogg
# Dancin' Fool					/system/media/audio/ringtones/DancinFool.ogg
# Digital Phone					/system/media/audio/ringtones/Ring_Digital_02.ogg
# Ding					/system/media/audio/ringtones/Ding.ogg
# DingDong					/system/media/audio/ringtones/DingDong.wav
# Don' Mess Wiv It					/system/media/audio/ringtones/DonMessWivIt.ogg
# Draco					/system/media/audio/ringtones/Draco.ogg
# Dream Theme					/system/media/audio/ringtones/DreamTheme.ogg
# Eastern Sky					/system/media/audio/ringtones/Eastern_Sky.ogg
# Enter the Nexus					/system/media/audio/ringtones/Enter_the_Nexus.ogg
# Eridani					/system/media/audio/ringtones/Eridani.ogg
# Ether Shake					/system/media/audio/ringtones/EtherShake.ogg
# Flutey Phone					/system/media/audio/ringtones/Ring_Synth_04.ogg
# Free Flight					/system/media/audio/ringtones/FreeFlight.ogg
# Friendly Ghost					/system/media/audio/ringtones/FriendlyGhost.ogg
# Funk Y'all					/system/media/audio/ringtones/Funk_Yall.ogg
# Game Over Guitar					/system/media/audio/ringtones/GameOverGuitar.ogg
# Gimme Mo' Town					/system/media/audio/ringtones/Gimme_Mo_Town.ogg
# Girtab					/system/media/audio/ringtones/Girtab.ogg
# Glacial Groove					/system/media/audio/ringtones/Glacial_Groove.ogg
# Growl					/system/media/audio/ringtones/Growl.ogg
# Halfway Home					/system/media/audio/ringtones/HalfwayHome.ogg
# Hydra					/system/media/audio/ringtones/Hydra.ogg
# Insert Coin					/system/media/audio/ringtones/InsertCoin.ogg
# Kuma					/system/media/audio/ringtones/Kuma.ogg
# Loopy Lounge					/system/media/audio/ringtones/LoopyLounge.ogg
# Love Flute					/system/media/audio/ringtones/LoveFlute.ogg
# Lyra					/system/media/audio/ringtones/Lyra.ogg
# Machina					/system/media/audio/ringtones/Machina.ogg
# Medieval Jaunt					/system/media/audio/ringtones/MidEvilJaunt.ogg
# Mildly Alarming					/system/media/audio/ringtones/MildlyAlarming.ogg
# Nairobi					/system/media/audio/ringtones/Nairobi.ogg
# Nassau					/system/media/audio/ringtones/Nassau.ogg
# New Player					/system/media/audio/ringtones/NewPlayer.ogg
# No Limits					/system/media/audio/ringtones/No_Limits.ogg
# Noisey One					/system/media/audio/ringtones/Noises1.ogg
# Organ Dub					/system/media/audio/ringtones/OrganDub.ogg
# Orion					/system/media/audio/ringtones/Orion.ogg
# Paradise Island					/system/media/audio/ringtones/Paradise_Island.ogg
# Pegasus					/system/media/audio/ringtones/Pegasus.ogg
# Perseus					/system/media/audio/ringtones/PERSEUS.ogg
# Playa					/system/media/audio/ringtones/Playa.ogg
# Pyxis					/system/media/audio/ringtones/Pyxis.ogg
# Rasalas					/system/media/audio/ringtones/Rasalas.ogg
# Revelation					/system/media/audio/ringtones/Revelation.ogg
# Rigel					/system/media/audio/ringtones/Rigel.ogg
# Road Trip					/system/media/audio/ringtones/Road_Trip.ogg
# Romancing The Tone					/system/media/audio/ringtones/RomancingTheTone.ogg
# Safari					/system/media/audio/ringtones/Safari.ogg
# Savannah					/system/media/audio/ringtones/Savannah.ogg
# Scarabaeus					/system/media/audio/ringtones/Scarabaeus.ogg
# Sceptrum					/system/media/audio/ringtones/Sceptrum.ogg
# Seville					/system/media/audio/ringtones/Seville.ogg
# She's All That					/system/media/audio/ringtones/Shes_All_That.ogg
# Silky Way					/system/media/audio/ringtones/SilkyWay.ogg
# Sitar Versus Sitar					/system/media/audio/ringtones/SitarVsSitar.ogg
# Solarium					/system/media/audio/ringtones/Solarium.ogg
# Springy Jalopy					/system/media/audio/ringtones/SpringyJalopy.ogg
# Steppin' Out					/system/media/audio/ringtones/Steppin_Out.ogg
# Terminated					/system/media/audio/ringtones/Terminated.ogg
# Terrible Twos					/system/media/audio/ringtones/Noises2.ogg
# Testudo					/system/media/audio/ringtones/Testudo.ogg
# Themos					/system/media/audio/ringtones/Themos.ogg
# Third Eye					/system/media/audio/ringtones/Third_Eye.ogg
# Thriller Three					/system/media/audio/ringtones/Noises3.ogg
# Thunderfoot					/system/media/audio/ringtones/Thunderfoot.ogg
# Twirl Away					/system/media/audio/ringtones/TwirlAway.ogg
# Ursa Minor					/system/media/audio/ringtones/URSAMINOR.ogg
# UrsaMinor					/system/media/audio/ringtones/UrsaMinor.ogg
# Very Alarmed					/system/media/audio/ringtones/VeryAlarmed.ogg
# Vespa					/system/media/audio/ringtones/Vespa.ogg
# World					/system/media/audio/ringtones/World.ogg
# Zeta					/system/media/audio/ringtones/Zeta.ogg
# bellcore-dr1					/system/media/audio/ringtones/bellcore-dr1.ogg
# bellcore-dr2					/system/media/audio/ringtones/bellcore-dr2.ogg
# bellcore-dr3					/system/media/audio/ringtones/bellcore-dr3.ogg
# bellcore-dr4					/system/media/audio/ringtones/bellcore-dr4.ogg
# bellcore-dr5					/system/media/audio/ringtones/bellcore-dr5.ogg
# speaker					/system/media/audio/ringtones/speaker.wav

#######################################################################
##  Account 11 Advanced Settings                                      ##
#######################################################################
# Check Domain Certificates. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P52011 = 0

# Validate Certificate Chain. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P52067 = 0

# Validate Incoming SIP Messages. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P52006 = 0

# Allow Unsolicited REFER. 0 - Disabled, 1 - Enabled, 2 - Enabled/Force Auth. Default value is 0.
# Number: 0, 1, 2
P53023 = 0

# Only Accept SIP Requests from Known Servers. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P52047 = 0

# Check SIP User ID for Incoming INVITE. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P51049 = 0

# Allow SIP Reset. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P53015 = 0

# Authenticate Incoming INVITE. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P52046 = 0

# SIP Realm Used for Challenge INVITE & NOTIFY.
# String
P53021 =

# Enable Local MOH
# Number: 0, 1 
P52057 = 0

# Virtual Account Group. -1 - Default,  0 - Virtual Account Group 1, 1 - Virtual Account Group 2, 2 - Virtual Account Group 3
# 3 - Virtual Account Group 4, 4 - Virtual Account Group 5, 5 - Virtual Account Group 6, 6 - Virtual Account Group 7, 7 - Virtual Account Group 8
# 8 - Virtual Account Group 9, 9 - Virtual Account Group 10, 10 - Virtual Account Group 11, 11 - Virtual Account Group 12, 12 - Virtual Account Group 13
# 13 - Virtual Account Group 14, 14 - Virtual Account Group 15, 15 - Virtual Account Group 16. Default value is -1.
# Number: -1 - 15 
P52091 = -1

# Special Feature. Default value is 100
# 100 - Standard, 102 - Broadsoft, 113 - China Mobile, 114 - ZTE IMS, 115 - Mobotix
# 116 - ZTE NGN, 117 - Huawei IMS, 123 - NEC, 125 - WorldStone, 129 - Telefonica Spain
# Number: 100, 102, 113, 114, 115, 116, 117, 123, 125, 129
P51024 = 100

# Feature Key Synchronization.  0 - Disable, 0 - Broadsoft/Metaswitch. Default Value is 0.
# Number: 0, 1
# P52025 = 0

# Allow Sync Phonebook via SIP Notify. 0 - No, 1 - Yes. Default is 1.
# Number: 0, 1
P53099 = 1

##############################################################################
##  Account 12 Settings                                                     ##
##############################################################################
#######################################################################
##  Account 12 General Settings                                      ##
#######################################################################
# Account Active. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P51101 = 0

# Account Name
P51117 = 

# SIP Server
P51102 = 

# SIP User ID
P51104 =

# SIP Authentication ID
P51105 =

# SIP Authentication Password
P51106 =

# Tel URI. 0 - Disable, 1 - User=Phone, 2 - Enabled. Default value is 0
# Number: 0, 1, 2
P51109 = 0

#######################################################################
##  Account 12 Network Settings                                      ##
#######################################################################
# Outbound Proxy
P51103 =

# Secondary Outbound Proxy
P52133 =

# DNS Mode.  0 - A Record, 1 - SRV, 2 - NAPTR/SRV. Default value is 0
# Number: 0, 1, 2
P51108 = 0

# DNS SRV Fail-over Mode. 0 - Default, 1 - Saved one until DNS TTL, 2 - Saved one until no response. Defualt value is 1
# Number
P53140 = 0

# Register Before DNS SRV Fail-over. 0 - No, 1 - Yes. Default Value is 0.
# Number: 0, 1
P54195 = 1

# NAT Traversal. 0 - NAT No, 1 - STUN, 2 - Keep-alive, 3 - UPnP, 4 - Auto, 5 - VPN. Default value is 2
# Number: 0, 1, 2, 3, 4, 5
P51114 = 2

# Proxy-Require
P51118 =

#######################################################################
##  Account 12 SIP Settings                                          ##
#######################################################################
# SIP Registration. 0 - No, 1 - Yes. Default is 1
# Number: 0, 1
P51110 = 1

# Unregister Before New Registration. 0 - No, 1 - All, 2 -  Instance . Default value is 0
# Number: 0, 1, 2
P51111 = 2

# Register Expiration (m). In minutes. Default value is 60
# Number: 60 - 64800
P51112 = 60

# Subscribe Expiration (m). In minutes. Default value is blank
# Number: 0 - 64800
P53151 = 60

# Re-register before Expiration (s). Default value is 0
# Number: 0 - 3600
P52130 = 0

# Registration Retry Wait Time (s). In seconds. Default value is 20
# Number: 20 - 3600
P51171 = 20

# Add Auth Header On RE-REGISTER
# 0 - No, 1- Yes
P52159 = 1

# Enable SIP OPTIONS Keep Alive. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P52197 = 0

# SIP OPTIONS Keep Alive Interval(s). Default value is 30
# Number: 1 - 64800
P52198 = 30

# SIP OPTIONS Keep Alive Maximum Tries. Default value is 3
# Number: 3 
P52199 = 3

# Use Privacy Header. 0 - Default, 1 - No, 2 - Yes. Default value is 0
# Number: 0, 1, 2
P52138 = 0

# Use P-Preferred-Identity Header. 0 - Default, 1 - No, 2 - Yes. Default value is 0
# Number: 0, 1, 2
P52139 = 0

# SIP Transport. 0 - UDP, 1 - TCP, 2 - TLS. Default value is 0
# Number: 0, 1, 2
P51148 = 0

# Local SIP Port. Default value is 5082
# Number: 0 or 90 - 65535
P51113 = 5082

# SIP URI Scheme When Using TLS
# 0 -sip, 1 - sips. Default value is 0.
# Number: 0, 1
P52129 = 0

# Use Actual Ephemeral Port in Contact with TCP/TLS
# 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P52131 = 0

# Support SIP Instance ID. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P51189 = 1

# SIP T1 Timeout. RFC 3261 T1 value (RTT estimate)
# 50 - 0.5 sec, 100 - 1 sec, 200 - 2 sec. Default value is 50
# Number: 50, 100, 200
P51140 = 50

# SIP T2 Interval. RFC 3261 T2 value. The maximum retransmit interval for non-INVITE requests and INVITE responses
# 200 - 2 sec, 400 - 4 sec, 800 - 8 sec. Default 400
# Number: 200, 400, 800
P51141 = 400

# SIP Timer D Interval (Seconds)
# Number 0-64. Default value is 0
P52187 = 0

# Remove OBP from route. 0 - Disable, 1 - Enable. Default value is 0
# Number: 0, 1
P52105 = 0

# Enable 100rel. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P51135 = 0

#######################################################################
##  Account 12 Session Timer                                          ##
#######################################################################

# Enable Session Timer/ Session Expiration(s).  In seconds. Default value is 180 seconds.
# By default,  Session Timer is Enabled.  Session Timer is disabled if the value is 0.
# Number: 0 or 90 - 64800
P51134 = 180

# Min-SE (s). Default value is 90 seconds
# Number: 0 or 90 - 64800
P51127 = 90

# UAC Specify Refresher. 0 - Omit, 1 - UAC, 2 - UAS. Default value is 0
# Number: 0, 1, 2
P51132 = 0

# UAS Specify Refresher. 1 - UAC, 2 - UAS. Default value is 1
# Number: 1, 2
P51133 = 1

# Caller Request Timer (Request for timer when calling)
# 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1.
P51128 = 0

# Callee Request Timer. Request for timer when called (i.e. if remote party supports timer but did not request for one)
# 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P51129 = 0

# Force Timer (Still use timer when remote party does not support timer). 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P51130 = 0

# Force INVITE (Always refresh with INVITE instead of UPDATE even when remote party supports UPDATE)
# 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P51131 = 0

#######################################################################
##  Account 12 Codec Settings                                         ##
#######################################################################
# Preferred Vocoder
# First codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 103 - G722.1C, 104 - G722.1, 123 - Opus. Default value is 0
# Number: 0, 2, 8, 9, 18, 98, 103, 104, 123
P51151 = 0

# Second codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 103 - G722.1C, 104 - G722.1, 123 - Opus. Default value is 8
# Number: 0, 2, 8, 9, 18, 98, 103, 104, 123
P51152 = 8

# Third codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 103 - G722.1C, 104 - G722.1, 123 - Opus. Default value is 9
# Number: 0, 2, 8, 9, 18, 98, 103, 104, 123
P51153 = 9

# Forth codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 103 - G722.1C, 104 - G722.1, 123 - Opus. Default value is 104
# Number: 0, 2, 8, 9, 18, 98, 103, 104, 123
P51154 = 104

# Fifth codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 103 - G722.1C, 104 - G722.1, 123 - Opus. Default value is 104
# Number: 0, 2, 8, 9, 18, 98, 103, 104, 123
P51155 = 104

# Sixth codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 103 - G722.1C, 104 - G722.1, 123 - Opus. Default value is 104
# Number: 0, 2, 8, 9, 18, 98, 103, 104, 123
P51156 = 104

# Seventh codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 103 - G722.1C, 104 - G722.1, 123 - Opus. Default value is 104
# Number: 0, 2, 8, 9, 18, 98, 103, 104, 123
P51157 = 104

# Eigth codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 103 - G722.1C, 104 - G722.1, 123 - Opus. Default value is 104
# Number: 0, 2, 8, 9, 18, 98, 103, 104, 123
P51158 = 104

# Codec Negotiation Priority. 0 - Caller, 1 - Callee. Default value is 1.
# Number: 0, 1
P54161 = 1

# Use First Matching Vocoder in 200OK SDP. 0 - No, 1 - Yes. The default value is 0.
# Number: 0, 1
P52148 = 0

# iLBC Frame Size. 0 - 20 ms, 1 - 30 ms. Default value is 1.
# Number: 0, 1
P51195 = 1

# G726-32 ITU Payload. 0 - 2, 1 - Dynamic. Default value is 0.
# Number: 0, 1
P52169 = 0

# G726-32 Dynamic PT. Default value is 126.
# Number
P52165 = 126

# Opus Payload Type. Default value is 123.
P52185 = 123

# DTMF: in audio. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P52101 = 0

# DTMF: in RFC2833. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P52102 = 1

# DTMF: in SIP INFO. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P52103 = 0

# DTMF Payload Type. Default value is 101
# Number: 96 - 127
P51196 = 101

# Enable Audio RED with FEC. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P53173 = 0

# Audio FEC Payload Type. Default value is 121
# Number: 96 - 126
P53174 = 121

# Audio RED Payload Type. Default value is 124
# Number: 96 - 126
PP53175 = 124

# Silence Suppression. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P51185 = 0

# Voice Frames per TX. Default valule is 2
# Number: 1 - 64
P51186 = 2

#######################################################################
##  Account 12 RTP Settings                                          ##
#######################################################################
# SRTP Mode. 0 - Disable, 1 - Enabled but not forced, 2 - Enabled and forced. Default value is 0
# Number: 0, 1, 2
P51143 = 0

# SRTP Key Length. 0 - AES 128&256 bit, 1 - AES 128 bit, 2 - AES 256 bit. Default value is 0
#Number:0, 1, 2
P52183 = 0 

# Enable SRTP Key Life Time. 0 - No, 1 - Yes.
# Number: 0,1
P52163 = 1

# RTCP Destination
P52190 = 

# Symmetric RTP. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P51160 = 0

# RTP IP Filter. 0 - Disable, 1 - IP Only, 2 - IP and Port. Default value is 0
# Number: 0, 1, 2
P53126 = 0

#######################################################################
##  Account 12 Call Settings                                          ##
#######################################################################
# Play warning tone for Auto Answer Intercom. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P53172 = 1

# Send Anonymous. 0 - No, 1 - Yes (caller ID will be blocked if set to Yes). Default value is 0
# Number: 0, 1
P51121 = 0

# Intercept Anonymous Calls. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P51146 = 0

# Call Log. 0 - Log All, 1 - Log Incoming/Outgoing only (Missed Calls Not Recorded), 2 - Disable Call All. Default value is 0
# Number: 0, 1
P51142 = 0

# Ring Timeout. Default value is 60 seconds
# Number: 0 - 300
P51176 = 60

# Refer-To Use Target Contact. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P51169 = 0

# Incoming Call Rules. 0 - Block, 1 - Set Password, 2 - Auto Answer, 3 - Ringing, 4 - Disable. Default value is 4.
# Number: 0, 1, 2 ,3 ,4
P61144 = 4

# Set Password Rules. 
# Numbers
P61145

# Dial Plan Prefix
# String
P51119 =

# Disable DialPlan. 0 - No Selection, 1 - Dial Page, 2 - Contact, 4 - Incoming Call History, 8 -  Outgoing Call History, 16 - MPK & Click2Dial. 
# If need to check multiple selections, add the specific values for each selections together. Default value is 0
# Number: 0-31
P52182 = 0

# Dial Plan. Default value is { x+ | \+x+ | *x+ | *xx*x+ }
P51159 = { x+ | \+x+ | *x+ | *xx*x+ }

# Account Ringtone. See ring tone options and value in the Ring Tone Value Table below.
P51123 = content://settings/system/ringtone

# Ignore Alert-Info Header. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1
P53118 = 0

# Matching Incoming Caller ID. Matching Rule 1.
# String
P53177 =

# Matching Rule 1 Distinctive Ringtone. See ring tone options and value in the Ring Tone Value Table below.
# String
P53178 = content://settings/system/ringtone

# Matching Incoming Caller ID. Matching Rule 2.
# String
P53179 =

# Matching Rule 2 Distinctive Ringtone. See ring tone options and value in the Ring Tone Value Table below.
# String
P53180 = content://settings/system/ringtone

# Matching Incoming Caller ID. Matching Rule 3.
# String
P53181 =

# Matching Rule 3 Distinctive Ringtone. See ring tone options and value in the Ring Tone Value Table below.
# String
P53182 = content://settings/system/ringtone

############Ring Tone Value Table###############
# Web GUI Option                            Value
# Use System Ring tone                      content://settings/system/ringtone 
# Andromeda					/system/media/audio/ringtones/ANDROMEDA.ogg
# Aquila					/system/media/audio/ringtones/Aquila.ogg
# Argo Navis					/system/media/audio/ringtones/ArgoNavis.ogg
# Atria					/system/media/audio/ringtones/Atria.ogg
# Backroad					/system/media/audio/ringtones/Backroad.ogg
# Beat Plucker					/system/media/audio/ringtones/BeatPlucker.ogg
# Bell Phone					/system/media/audio/ringtones/Ring_Classic_02.ogg
# Bentley Dubs					/system/media/audio/ringtones/BentleyDubs.ogg
# Big Easy					/system/media/audio/ringtones/Big_Easy.ogg
# Bird Loop					/system/media/audio/ringtones/BirdLoop.ogg
# Bollywood					/system/media/audio/ringtones/Bollywood.ogg
# Boötes					/system/media/audio/ringtones/BOOTES.ogg
# Bus' a Move					/system/media/audio/ringtones/BussaMove.ogg
# Cairo					/system/media/audio/ringtones/Cairo.ogg
# Calypso Steel					/system/media/audio/ringtones/Calypso_Steel.ogg
# Canis Major					/system/media/audio/ringtones/CANISMAJOR.ogg
# Caribbean Ice					/system/media/audio/ringtones/CaribbeanIce.ogg
# Carina					/system/media/audio/ringtones/Carina.ogg
# Cassiopeia					/system/media/audio/ringtones/CASSIOPEIA.ogg
# Centaurus					/system/media/audio/ringtones/Centaurus.ogg
# Champagne Edition					/system/media/audio/ringtones/Champagne_Edition.ogg
# Chimey Phone					/system/media/audio/ringtones/Ring_Synth_02.ogg
# Club Cubano					/system/media/audio/ringtones/Club_Cubano.ogg
# Crayon Rock					/system/media/audio/ringtones/CrayonRock.ogg
# Crazy Dream					/system/media/audio/ringtones/CrazyDream.ogg
# Curve Ball Blend					/system/media/audio/ringtones/CurveBall.ogg
# Cygnus					/system/media/audio/ringtones/Cygnus.ogg
# Dancin' Fool					/system/media/audio/ringtones/DancinFool.ogg
# Digital Phone					/system/media/audio/ringtones/Ring_Digital_02.ogg
# Ding					/system/media/audio/ringtones/Ding.ogg
# DingDong					/system/media/audio/ringtones/DingDong.wav
# Don' Mess Wiv It					/system/media/audio/ringtones/DonMessWivIt.ogg
# Draco					/system/media/audio/ringtones/Draco.ogg
# Dream Theme					/system/media/audio/ringtones/DreamTheme.ogg
# Eastern Sky					/system/media/audio/ringtones/Eastern_Sky.ogg
# Enter the Nexus					/system/media/audio/ringtones/Enter_the_Nexus.ogg
# Eridani					/system/media/audio/ringtones/Eridani.ogg
# Ether Shake					/system/media/audio/ringtones/EtherShake.ogg
# Flutey Phone					/system/media/audio/ringtones/Ring_Synth_04.ogg
# Free Flight					/system/media/audio/ringtones/FreeFlight.ogg
# Friendly Ghost					/system/media/audio/ringtones/FriendlyGhost.ogg
# Funk Y'all					/system/media/audio/ringtones/Funk_Yall.ogg
# Game Over Guitar					/system/media/audio/ringtones/GameOverGuitar.ogg
# Gimme Mo' Town					/system/media/audio/ringtones/Gimme_Mo_Town.ogg
# Girtab					/system/media/audio/ringtones/Girtab.ogg
# Glacial Groove					/system/media/audio/ringtones/Glacial_Groove.ogg
# Growl					/system/media/audio/ringtones/Growl.ogg
# Halfway Home					/system/media/audio/ringtones/HalfwayHome.ogg
# Hydra					/system/media/audio/ringtones/Hydra.ogg
# Insert Coin					/system/media/audio/ringtones/InsertCoin.ogg
# Kuma					/system/media/audio/ringtones/Kuma.ogg
# Loopy Lounge					/system/media/audio/ringtones/LoopyLounge.ogg
# Love Flute					/system/media/audio/ringtones/LoveFlute.ogg
# Lyra					/system/media/audio/ringtones/Lyra.ogg
# Machina					/system/media/audio/ringtones/Machina.ogg
# Medieval Jaunt					/system/media/audio/ringtones/MidEvilJaunt.ogg
# Mildly Alarming					/system/media/audio/ringtones/MildlyAlarming.ogg
# Nairobi					/system/media/audio/ringtones/Nairobi.ogg
# Nassau					/system/media/audio/ringtones/Nassau.ogg
# New Player					/system/media/audio/ringtones/NewPlayer.ogg
# No Limits					/system/media/audio/ringtones/No_Limits.ogg
# Noisey One					/system/media/audio/ringtones/Noises1.ogg
# Organ Dub					/system/media/audio/ringtones/OrganDub.ogg
# Orion					/system/media/audio/ringtones/Orion.ogg
# Paradise Island					/system/media/audio/ringtones/Paradise_Island.ogg
# Pegasus					/system/media/audio/ringtones/Pegasus.ogg
# Perseus					/system/media/audio/ringtones/PERSEUS.ogg
# Playa					/system/media/audio/ringtones/Playa.ogg
# Pyxis					/system/media/audio/ringtones/Pyxis.ogg
# Rasalas					/system/media/audio/ringtones/Rasalas.ogg
# Revelation					/system/media/audio/ringtones/Revelation.ogg
# Rigel					/system/media/audio/ringtones/Rigel.ogg
# Road Trip					/system/media/audio/ringtones/Road_Trip.ogg
# Romancing The Tone					/system/media/audio/ringtones/RomancingTheTone.ogg
# Safari					/system/media/audio/ringtones/Safari.ogg
# Savannah					/system/media/audio/ringtones/Savannah.ogg
# Scarabaeus					/system/media/audio/ringtones/Scarabaeus.ogg
# Sceptrum					/system/media/audio/ringtones/Sceptrum.ogg
# Seville					/system/media/audio/ringtones/Seville.ogg
# She's All That					/system/media/audio/ringtones/Shes_All_That.ogg
# Silky Way					/system/media/audio/ringtones/SilkyWay.ogg
# Sitar Versus Sitar					/system/media/audio/ringtones/SitarVsSitar.ogg
# Solarium					/system/media/audio/ringtones/Solarium.ogg
# Springy Jalopy					/system/media/audio/ringtones/SpringyJalopy.ogg
# Steppin' Out					/system/media/audio/ringtones/Steppin_Out.ogg
# Terminated					/system/media/audio/ringtones/Terminated.ogg
# Terrible Twos					/system/media/audio/ringtones/Noises2.ogg
# Testudo					/system/media/audio/ringtones/Testudo.ogg
# Themos					/system/media/audio/ringtones/Themos.ogg
# Third Eye					/system/media/audio/ringtones/Third_Eye.ogg
# Thriller Three					/system/media/audio/ringtones/Noises3.ogg
# Thunderfoot					/system/media/audio/ringtones/Thunderfoot.ogg
# Twirl Away					/system/media/audio/ringtones/TwirlAway.ogg
# Ursa Minor					/system/media/audio/ringtones/URSAMINOR.ogg
# UrsaMinor					/system/media/audio/ringtones/UrsaMinor.ogg
# Very Alarmed					/system/media/audio/ringtones/VeryAlarmed.ogg
# Vespa					/system/media/audio/ringtones/Vespa.ogg
# World					/system/media/audio/ringtones/World.ogg
# Zeta					/system/media/audio/ringtones/Zeta.ogg
# bellcore-dr1					/system/media/audio/ringtones/bellcore-dr1.ogg
# bellcore-dr2					/system/media/audio/ringtones/bellcore-dr2.ogg
# bellcore-dr3					/system/media/audio/ringtones/bellcore-dr3.ogg
# bellcore-dr4					/system/media/audio/ringtones/bellcore-dr4.ogg
# bellcore-dr5					/system/media/audio/ringtones/bellcore-dr5.ogg
# speaker					/system/media/audio/ringtones/speaker.wav

#######################################################################
##  Account 12 Advanced Settings                                      ##
#######################################################################
# Check Domain Certificates. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P52111 = 0

# Validate Certificate Chain. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P52167 = 0

# Validate Incoming SIP Messages. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P52106 = 0

# Allow Unsolicited REFER. 0 - Disabled, 1 - Enabled, 2 - Enabled/Force Auth. Default value is 0.
# Number: 0, 1, 2
P53123 = 0

# Only Accept SIP Requests from Known Servers. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P52147 = 0

# Check SIP User ID for Incoming INVITE. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P51149 = 0

# Allow SIP Reset. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P53115 = 0

# Authenticate Incoming INVITE. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P52146 = 0

# SIP Realm Used for Challenge INVITE & NOTIFY.
# String
P53121 =

# Enable Local MOH
# Number: 0, 1 
P52157 = 0

# Virtual Account Group. -1 - Default,  0 - Virtual Account Group 1, 1 - Virtual Account Group 2, 2 - Virtual Account Group 3
# 3 - Virtual Account Group 4, 4 - Virtual Account Group 5, 5 - Virtual Account Group 6, 6 - Virtual Account Group 7, 7 - Virtual Account Group 8
# 8 - Virtual Account Group 9, 9 - Virtual Account Group 10, 10 - Virtual Account Group 11, 11 - Virtual Account Group 12, 12 - Virtual Account Group 13
# 13 - Virtual Account Group 14, 14 - Virtual Account Group 15, 15 - Virtual Account Group 16. Default value is -1.
# Number: -1 - 15 
P52191 = -1

# Special Feature. Default value is 100
# 100 - Standard, 102 - Broadsoft, 113 - China Mobile, 114 - ZTE IMS, 115 - Mobotix
# 116 - ZTE NGN, 117 - Huawei IMS, 123 - NEC, 125 - WorldStone, 129 - Telefonica Spain
# Number: 100, 102, 113, 114, 115, 116, 117, 123, 125, 129
P51124 = 100

# Feature Key Synchronization.  0 - Disable, 0 - Broadsoft/Metaswitch. Default Value is 0.
# Number: 0, 1
# P52125 = 0

# Allow Sync Phonebook via SIP Notify. 0 - No, 1 - Yes. Default is 1.
# Number: 0, 1
P53199 = 1

##############################################################################
##  Account 13 Settings                                                     ##
##############################################################################
#######################################################################
##  Account 13 General Settings                                      ##
#######################################################################
# Account Active. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P51201 = 0

# Account Name
P51217 = 

# SIP Server
P51202 = 

# SIP User ID
P51204 =

# SIP Authentication ID
P51205 =

# SIP Authentication Password
P51206 =

# Tel URI. 0 - Disable, 1 - User=Phone, 2 - Enabled. Default value is 0
# Number: 0, 1, 2
P51209 = 0

#######################################################################
##  Account 13 Network Settings                                      ##
#######################################################################
# Outbound Proxy
P51203 =

# Secondary Outbound Proxy
P52233 =

# DNS Mode.  0 - A Record, 1 - SRV, 2 - NAPTR/SRV. Default value is 0
# Number: 0, 1, 2
P51208 = 0

# DNS SRV Fail-over Mode. 0 - Default, 1 - Saved one until DNS TTL, 2 - Saved one until no response. Defualt value is 1
# Number
P53240 = 0

# Register Before DNS SRV Fail-over. 0 - No, 1 - Yes. Default Value is 0.
# Number: 0, 1
P54295 = 1

# NAT Traversal. 0 - NAT No, 1 - STUN, 2 - Keep-alive, 3 - UPnP, 4 - Auto, 5 - VPN. Default value is 2
# Number: 0, 1, 2, 3, 4, 5
P51214 = 2

# Proxy-Require
P51218 =

#######################################################################
##  Account 13 SIP Settings                                          ##
#######################################################################
# SIP Registration. 0 - No, 1 - Yes. Default is 1
# Number: 0, 1
P51210 = 1

# Unregister Before New Registration. 0 - No, 1 - All, 2 -  Instance . Default value is 0
# Number: 0, 1, 2
P51211 = 2

# Register Expiration (m). In minutes. Default value is 60
# Number: 60 - 64800
P51212 = 60

# Subscribe Expiration (m). In minutes. Default value is blank
# Number: 0 - 64800
P53251 = 60

# Re-register before Expiration (s). Default value is 0
# Number: 0 - 3600
P52230 = 0

# Registration Retry Wait Time (s). In seconds. Default value is 20
# Number: 20 - 3600
P51271 = 20

# Add Auth Header On RE-REGISTER
# 0 - No, 1- Yes
P52259 = 1

# Enable SIP OPTIONS Keep Alive. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P52297 = 0

# SIP OPTIONS Keep Alive Interval(s). Default value is 30
# Number: 1 - 64800 
P52298 = 30

# SIP OPTIONS Keep Alive Maximum Tries. Default value is 3
# Number: 3 
P52299 = 3

# Use Privacy Header. 0 - Default, 1 - No, 2 - Yes. Default value is 0
# Number: 0, 1, 2
P52238 = 0

# Use P-Preferred-Identity Header. 0 - Default, 1 - No, 2 - Yes. Default value is 0
# Number: 0, 1, 2
P52239 = 0

# SIP Transport. 0 - UDP, 1 - TCP, 2 - TLS. Default value is 0
# Number: 0, 1, 2
P51248 = 0

# Local SIP Port. Default value is 5084
# Number: 0 or 90 - 65535
P51213 = 5084

# SIP URI Scheme When Using TLS
# 0 -sip, 1 - sips. Default value is 0.
# Number: 0, 1
P52229 = 0

# Use Actual Ephemeral Port in Contact with TCP/TLS
# 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P52231 = 0

# Support SIP Instance ID. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P51289 = 1

# SIP T1 Timeout. RFC 3261 T1 value (RTT estimate)
# 50 - 0.5 sec, 100 - 1 sec, 200 - 2 sec. Default value is 50
# Number: 50, 100, 200
P51240 = 50

# SIP T2 Interval. RFC 3261 T2 value. The maximum retransmit interval for non-INVITE requests and INVITE responses
# 200 - 2 sec, 400 - 4 sec, 800 - 8 sec. Default 400
# Number: 200, 400, 800
P51241 = 400

# SIP Timer D Interval (Seconds)
# Number 0-64. Default value is 0
P52287 = 0

# Remove OBP from route. 0 - Disable, 1 - Enable. Default value is 0
# Number: 0, 1
P52205 = 0

# Enable 100rel. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P51235 = 0

#######################################################################
##  Account 13 Session Timer                                          ##
#######################################################################

# Enable Session Timer/ Session Expiration(s).  In seconds. Default value is 180 seconds.
# By default,  Session Timer is Enabled.  Session Timer is disabled if the value is 0.
# Number: 0 or 90 - 64800
P51234 = 180

# Min-SE (s). Default value is 90 seconds
# Number: 0 or 90 - 64800
P51227 = 90

# UAC Specify Refresher. 0 - Omit, 1 - UAC, 2 - UAS. Default value is 0
# Number: 0, 1, 2
P51232 = 0

# UAS Specify Refresher. 1 - UAC, 2 - UAS. Default value is 1
# Number: 1, 2
P51233 = 1

# Caller Request Timer (Request for timer when calling)
# 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1.
P51228 = 0

# Callee Request Timer. Request for timer when called (i.e. if remote party supports timer but did not request for one)
# 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P51229 = 0

# Force Timer (Still use timer when remote party does not support timer). 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P51230 = 0

# Force INVITE (Always refresh with INVITE instead of UPDATE even when remote party supports UPDATE)
# 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P51231 = 0

#######################################################################
##  Account 13 Codec Settings                                         ##
#######################################################################
# Preferred Vocoder
# First codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 103 - G722.1C, 104 - G722.1, 123 - Opus. Default value is 0
# Number: 0, 2, 8, 9, 18, 98, 103, 104, 123
P51251 = 0

# Second codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 103 - G722.1C, 104 - G722.1, 123 - Opus. Default value is 8
# Number: 0, 2, 8, 9, 18, 98, 103, 104, 123
P51252 = 8

# Third codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 103 - G722.1C, 104 - G722.1, 123 - Opus. Default value is 9
# Number: 0, 2, 8, 9, 18, 98, 103, 104, 123
P51253 = 9

# Forth codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 103 - G722.1C, 104 - G722.1, 123 - Opus. Default value is 104
# Number: 0, 2, 8, 9, 18, 98, 103, 104, 123
P51254 = 104

# Fifth codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 103 - G722.1C, 104 - G722.1, 123 - Opus. Default value is 104
# Number: 0, 2, 8, 9, 18, 98, 103, 104, 123
P51255 = 104

# Sixth codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 103 - G722.1C, 104 - G722.1, 123 - Opus. Default value is 104
# Number: 0, 2, 8, 9, 18, 98, 103, 104, 123
P51256 = 104

# Seventh codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 103 - G722.1C, 104 - G722.1, 123 - Opus. Default value is 104
# Number: 0, 2, 8, 9, 18, 98, 103, 104, 123
P51257 = 104

# Eigth codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 103 - G722.1C, 104 - G722.1, 123 - Opus. Default value is 104
# Number: 0, 2, 8, 9, 18, 98, 103, 104, 123
P51258 = 104

# Codec Negotiation Priority. 0 - Caller, 1 - Callee. Default value is 1.
# Number: 0, 1
P54261 = 1

# Use First Matching Vocoder in 200OK SDP. 0 - No, 1 - Yes. The default value is 0.
# Number: 0, 1
P52248 = 0

# iLBC Frame Size. 0 - 20 ms, 1 - 30 ms. Default value is 1.
# Number: 0, 1
P51295 = 1

# G726-32 ITU Payload. 0 - 2, 1 - Dynamic. Default value is 0.
# Number: 0, 1
P52269 = 0

# G726-32 Dynamic PT. Default value is 126.
# Number
P52265 = 126

# Opus Payload Type. Default value is 123.
P52285 = 123

# DTMF: in audio. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P52201 = 0

# DTMF: in RFC2833. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P52202 = 1

# DTMF: in SIP INFO. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P52203 = 0

# DTMF Payload Type. Default value is 101
# Number: 96 - 127
P51296 = 101

# Enable Audio RED with FEC. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P53273 = 0

# Audio FEC Payload Type. Default value is 121
# Number: 96 - 126
P53274 = 121

# Audio RED Payload Type. Default value is 124
# Number: 96 - 126
P53275 = 124

# Silence Suppression. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P51285 = 0

# Voice Frames per TX. Default valule is 2
# Number: 1 - 64
P51286 = 2

#######################################################################
##  Account 13 RTP Settings                                          ##
#######################################################################
# SRTP Mode. 0 - Disable, 1 - Enabled but not forced, 2 - Enabled and forced. Default value is 0
# Number: 0, 1, 2
P51243 = 0

# SRTP Key Length. 0 - AES 128&256 bit, 1 - AES 128 bit, 2 - AES 256 bit. Default value is 0
#Number:0, 1, 2
P52283 = 0

# Enable SRTP Key Life Time. 0 - No, 1 - Yes.
# Number: 0,1
P52263 = 1

# RTCP Destination
P52290 = 

# Symmetric RTP. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P51260 = 0

# RTP IP Filter. 0 - Disable, 1 - IP Only, 2 - IP and Port. Default value is 0
# Number: 0, 1, 2
P53226 = 0

#######################################################################
##  Account 13 Call Settings                                          ##
#######################################################################
# Play warning tone for Auto Answer Intercom. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P53272 = 1

# Send Anonymous. 0 - No, 1 - Yes (caller ID will be blocked if set to Yes). Default value is 0
# Number: 0, 1
P51221 = 0

# Intercept Anonymous Calls. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P51246 = 0

# Call Log. 0 - Log All, 1 - Log Incoming/Outgoing only (Missed Calls Not Recorded), 2 - Disable Call All. Default value is 0
# Number: 0, 1
P51242 = 0

# Ring Timeout. Default value is 60 seconds
# Number: 0 - 300
P51276 = 60

# Refer-To Use Target Contact. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P51269 = 0

# Incoming Call Rules. 0 - Block, 1 - Set Password, 2 - Auto Answer, 3 - Ringing, 4 - Disable. Default value is 4.
# Number: 0, 1, 2 ,3 ,4
P61244 = 4

# Set Password Rules. 
# Numbers
P61245

# Dial Plan Prefix
# String
P51219 =

# Disable DialPlan. 0 - No Selection, 1 - Dial Page, 2 - Contact, 4 - Incoming Call History, 8 -  Outgoing Call History, 16 - MPK & Click2Dial. 
# If need to check multiple selections, add the specific values for each selections together. Default value is 0
# Number: 0-31
P52282 = 0

# Dial Plan. Default value is { x+ | \+x+ | *x+ | *xx*x+ }
P51259 = { x+ | \+x+ | *x+ | *xx*x+ }

# Account Ringtone. See ring tone options and value in the Ring Tone Value Table below.
P51223 = content://settings/system/ringtone

# Ignore Alert-Info Header. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1
P53218 = 0

# Matching Incoming Caller ID. Matching Rule 1.
# String
P53277 =

# Matching Rule 1 Distinctive Ringtone. See ring tone options and value in the Ring Tone Value Table below.
# String
P53278 = content://settings/system/ringtone

# Matching Incoming Caller ID. Matching Rule 2.
# String
P53279 =

# Matching Rule 2 Distinctive Ringtone. See ring tone options and value in the Ring Tone Value Table below.
# String
P53280 = content://settings/system/ringtone

# Matching Incoming Caller ID. Matching Rule 3.
# String
P53281 =

# Matching Rule 3 Distinctive Ringtone. See ring tone options and value in the Ring Tone Value Table below.
# String
P53282 = content://settings/system/ringtone

############Ring Tone Value Table###############
# Web GUI Option                            Value
# Use System Ring tone                      content://settings/system/ringtone 
# Andromeda					/system/media/audio/ringtones/ANDROMEDA.ogg
# Aquila					/system/media/audio/ringtones/Aquila.ogg
# Argo Navis					/system/media/audio/ringtones/ArgoNavis.ogg
# Atria					/system/media/audio/ringtones/Atria.ogg
# Backroad					/system/media/audio/ringtones/Backroad.ogg
# Beat Plucker					/system/media/audio/ringtones/BeatPlucker.ogg
# Bell Phone					/system/media/audio/ringtones/Ring_Classic_02.ogg
# Bentley Dubs					/system/media/audio/ringtones/BentleyDubs.ogg
# Big Easy					/system/media/audio/ringtones/Big_Easy.ogg
# Bird Loop					/system/media/audio/ringtones/BirdLoop.ogg
# Bollywood					/system/media/audio/ringtones/Bollywood.ogg
# Boötes					/system/media/audio/ringtones/BOOTES.ogg
# Bus' a Move					/system/media/audio/ringtones/BussaMove.ogg
# Cairo					/system/media/audio/ringtones/Cairo.ogg
# Calypso Steel					/system/media/audio/ringtones/Calypso_Steel.ogg
# Canis Major					/system/media/audio/ringtones/CANISMAJOR.ogg
# Caribbean Ice					/system/media/audio/ringtones/CaribbeanIce.ogg
# Carina					/system/media/audio/ringtones/Carina.ogg
# Cassiopeia					/system/media/audio/ringtones/CASSIOPEIA.ogg
# Centaurus					/system/media/audio/ringtones/Centaurus.ogg
# Champagne Edition					/system/media/audio/ringtones/Champagne_Edition.ogg
# Chimey Phone					/system/media/audio/ringtones/Ring_Synth_02.ogg
# Club Cubano					/system/media/audio/ringtones/Club_Cubano.ogg
# Crayon Rock					/system/media/audio/ringtones/CrayonRock.ogg
# Crazy Dream					/system/media/audio/ringtones/CrazyDream.ogg
# Curve Ball Blend					/system/media/audio/ringtones/CurveBall.ogg
# Cygnus					/system/media/audio/ringtones/Cygnus.ogg
# Dancin' Fool					/system/media/audio/ringtones/DancinFool.ogg
# Digital Phone					/system/media/audio/ringtones/Ring_Digital_02.ogg
# Ding					/system/media/audio/ringtones/Ding.ogg
# DingDong					/system/media/audio/ringtones/DingDong.wav
# Don' Mess Wiv It					/system/media/audio/ringtones/DonMessWivIt.ogg
# Draco					/system/media/audio/ringtones/Draco.ogg
# Dream Theme					/system/media/audio/ringtones/DreamTheme.ogg
# Eastern Sky					/system/media/audio/ringtones/Eastern_Sky.ogg
# Enter the Nexus					/system/media/audio/ringtones/Enter_the_Nexus.ogg
# Eridani					/system/media/audio/ringtones/Eridani.ogg
# Ether Shake					/system/media/audio/ringtones/EtherShake.ogg
# Flutey Phone					/system/media/audio/ringtones/Ring_Synth_04.ogg
# Free Flight					/system/media/audio/ringtones/FreeFlight.ogg
# Friendly Ghost					/system/media/audio/ringtones/FriendlyGhost.ogg
# Funk Y'all					/system/media/audio/ringtones/Funk_Yall.ogg
# Game Over Guitar					/system/media/audio/ringtones/GameOverGuitar.ogg
# Gimme Mo' Town					/system/media/audio/ringtones/Gimme_Mo_Town.ogg
# Girtab					/system/media/audio/ringtones/Girtab.ogg
# Glacial Groove					/system/media/audio/ringtones/Glacial_Groove.ogg
# Growl					/system/media/audio/ringtones/Growl.ogg
# Halfway Home					/system/media/audio/ringtones/HalfwayHome.ogg
# Hydra					/system/media/audio/ringtones/Hydra.ogg
# Insert Coin					/system/media/audio/ringtones/InsertCoin.ogg
# Kuma					/system/media/audio/ringtones/Kuma.ogg
# Loopy Lounge					/system/media/audio/ringtones/LoopyLounge.ogg
# Love Flute					/system/media/audio/ringtones/LoveFlute.ogg
# Lyra					/system/media/audio/ringtones/Lyra.ogg
# Machina					/system/media/audio/ringtones/Machina.ogg
# Medieval Jaunt					/system/media/audio/ringtones/MidEvilJaunt.ogg
# Mildly Alarming					/system/media/audio/ringtones/MildlyAlarming.ogg
# Nairobi					/system/media/audio/ringtones/Nairobi.ogg
# Nassau					/system/media/audio/ringtones/Nassau.ogg
# New Player					/system/media/audio/ringtones/NewPlayer.ogg
# No Limits					/system/media/audio/ringtones/No_Limits.ogg
# Noisey One					/system/media/audio/ringtones/Noises1.ogg
# Organ Dub					/system/media/audio/ringtones/OrganDub.ogg
# Orion					/system/media/audio/ringtones/Orion.ogg
# Paradise Island					/system/media/audio/ringtones/Paradise_Island.ogg
# Pegasus					/system/media/audio/ringtones/Pegasus.ogg
# Perseus					/system/media/audio/ringtones/PERSEUS.ogg
# Playa					/system/media/audio/ringtones/Playa.ogg
# Pyxis					/system/media/audio/ringtones/Pyxis.ogg
# Rasalas					/system/media/audio/ringtones/Rasalas.ogg
# Revelation					/system/media/audio/ringtones/Revelation.ogg
# Rigel					/system/media/audio/ringtones/Rigel.ogg
# Road Trip					/system/media/audio/ringtones/Road_Trip.ogg
# Romancing The Tone					/system/media/audio/ringtones/RomancingTheTone.ogg
# Safari					/system/media/audio/ringtones/Safari.ogg
# Savannah					/system/media/audio/ringtones/Savannah.ogg
# Scarabaeus					/system/media/audio/ringtones/Scarabaeus.ogg
# Sceptrum					/system/media/audio/ringtones/Sceptrum.ogg
# Seville					/system/media/audio/ringtones/Seville.ogg
# She's All That					/system/media/audio/ringtones/Shes_All_That.ogg
# Silky Way					/system/media/audio/ringtones/SilkyWay.ogg
# Sitar Versus Sitar					/system/media/audio/ringtones/SitarVsSitar.ogg
# Solarium					/system/media/audio/ringtones/Solarium.ogg
# Springy Jalopy					/system/media/audio/ringtones/SpringyJalopy.ogg
# Steppin' Out					/system/media/audio/ringtones/Steppin_Out.ogg
# Terminated					/system/media/audio/ringtones/Terminated.ogg
# Terrible Twos					/system/media/audio/ringtones/Noises2.ogg
# Testudo					/system/media/audio/ringtones/Testudo.ogg
# Themos					/system/media/audio/ringtones/Themos.ogg
# Third Eye					/system/media/audio/ringtones/Third_Eye.ogg
# Thriller Three					/system/media/audio/ringtones/Noises3.ogg
# Thunderfoot					/system/media/audio/ringtones/Thunderfoot.ogg
# Twirl Away					/system/media/audio/ringtones/TwirlAway.ogg
# Ursa Minor					/system/media/audio/ringtones/URSAMINOR.ogg
# UrsaMinor					/system/media/audio/ringtones/UrsaMinor.ogg
# Very Alarmed					/system/media/audio/ringtones/VeryAlarmed.ogg
# Vespa					/system/media/audio/ringtones/Vespa.ogg
# World					/system/media/audio/ringtones/World.ogg
# Zeta					/system/media/audio/ringtones/Zeta.ogg
# bellcore-dr1					/system/media/audio/ringtones/bellcore-dr1.ogg
# bellcore-dr2					/system/media/audio/ringtones/bellcore-dr2.ogg
# bellcore-dr3					/system/media/audio/ringtones/bellcore-dr3.ogg
# bellcore-dr4					/system/media/audio/ringtones/bellcore-dr4.ogg
# bellcore-dr5					/system/media/audio/ringtones/bellcore-dr5.ogg
# speaker					/system/media/audio/ringtones/speaker.wav

#######################################################################
##  Account 13 Advanced Settings                                      ##
#######################################################################
# Check Domain Certificates. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P52211 = 0

# Validate Certificate Chain. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P52267 = 0

# Validate Incoming SIP Messages. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P52206 = 0

# Allow Unsolicited REFER. 0 - Disabled, 1 - Enabled, 2 - Enabled/Force Auth. Default value is 0.
# Number: 0, 1, 2
P53223 = 0

# Only Accept SIP Requests from Known Servers. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P52247 = 0

# Check SIP User ID for Incoming INVITE. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P51249 = 0

# Allow SIP Reset. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P53215 = 0

# Authenticate Incoming INVITE. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P52246 = 0

# SIP Realm Used for Challenge INVITE & NOTIFY.
# String
P53221 =

# Enable Local MOH
# Number: 0, 1 
P52257 = 0

# Virtual Account Group. -1 - Default,  0 - Virtual Account Group 1, 1 - Virtual Account Group 2, 2 - Virtual Account Group 3
# 3 - Virtual Account Group 4, 4 - Virtual Account Group 5, 5 - Virtual Account Group 6, 6 - Virtual Account Group 7, 7 - Virtual Account Group 8
# 8 - Virtual Account Group 9, 9 - Virtual Account Group 10, 10 - Virtual Account Group 11, 11 - Virtual Account Group 12, 12 - Virtual Account Group 13
# 13 - Virtual Account Group 14, 14 - Virtual Account Group 15, 15 - Virtual Account Group 16. Default value is -1.
# Number: -1 - 15 
P52291 = -1

# Special Feature. Default value is 100
# 100 - Standard, 102 - Broadsoft, 113 - China Mobile, 114 - ZTE IMS, 115 - Mobotix
# 116 - ZTE NGN, 117 - Huawei IMS, 123 - NEC, 125 - WorldStone, 129 - Telefonica Spain
# Number: 100, 102, 113, 114, 115, 116, 117, 123, 125, 129
P51224 = 100

# Feature Key Synchronization.  0 - Disable, 0 - Broadsoft/Metaswitch. Default Value is 0.
# Number: 0, 1
# P52225 = 0

# Allow Sync Phonebook via SIP Notify. 0 - No, 1 - Yes. Default is 1.
# Number: 0, 1
P53299 = 1

##############################################################################
##  Account 14 Settings                                                     ##
##############################################################################
#######################################################################
##  Account 14 General Settings                                      ##
#######################################################################
# Account Active. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P51301 = 0

# Account Name
P51317 = 

# SIP Server
P51302 = 

# SIP User ID
P51304 =

# SIP Authentication ID
P51305 =

# SIP Authentication Password
P51306 =

# Tel URI. 0 - Disable, 1 - User=Phone, 2 - Enabled. Default value is 0
# Number: 0, 1, 2
P51309 = 0

#######################################################################
##  Account 14 Network Settings                                      ##
#######################################################################
# Outbound Proxy
P51303 =

# Secondary Outbound Proxy
P52333 =

# DNS Mode.  0 - A Record, 1 - SRV, 2 - NAPTR/SRV. Default value is 0
# Number: 0, 1, 2
P51308 = 0

# DNS SRV Fail-over Mode. 0 - Default, 1 - Saved one until DNS TTL, 2 - Saved one until no response. Defualt value is 1
# Number
P53340 = 0

# Register Before DNS SRV Fail-over. 0 - No, 1 - Yes. Default Value is 0.
# Number: 0, 1
P54395 = 1

# NAT Traversal. 0 - NAT No, 1 - STUN, 2 - Keep-alive, 3 - UPnP, 4 - Auto, 5 - VPN. Default value is 2
# Number: 0, 1, 2, 3, 4, 5
P51314 = 2

# Proxy-Require
P51318 =

#######################################################################
##  Account 14 SIP Settings                                          ##
#######################################################################
# SIP Registration. 0 - No, 1 - Yes. Default is 1
# Number: 0, 1
P51310 = 1

# Unregister Before New Registration. 0 - No, 1 - All, 2 -  Instance . Default value is 0
# Number: 0, 1, 2
P51311 = 2

# Register Expiration (m). In minutes. Default value is 60
# Number: 60 - 64800
P51312 = 60

# Subscribe Expiration (m). In minutes. Default value is blank
# Number: 0 - 64800
P53351 = 60

# Re-register before Expiration (s). Default value is 0
# Number: 0 - 3600
P52330 = 0

# Registration Retry Wait Time (s). In seconds. Default value is 20
# Number: 20 - 3600
P51371 = 20

# Add Auth Header On RE-REGISTER
# 0 - No, 1- Yes
P52359 = 1

# Enable SIP OPTIONS Keep Alive. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P52397 = 0

# SIP OPTIONS Keep Alive Interval(s). Default value is 30
# Number: 1 - 64800
P52398 = 30

# SIP OPTIONS Keep Alive Maximum Tries. Default value is 3
# Number: 3 
P52399 = 3

# Use Privacy Header. 0 - Default, 1 - No, 2 - Yes. Default value is 0
# Number: 0, 1, 2
P52338 = 0

# Use P-Preferred-Identity Header. 0 - Default, 1 - No, 2 - Yes. Default value is 0
# Number: 0, 1, 2
P52339 = 0

# SIP Transport. 0 - UDP, 1 - TCP, 2 - TLS. Default value is 0
# Number: 0, 1, 2
P51348 = 0

# Local SIP Port. Default value is 5086
# Number: 0 or 90 - 65535
P51313 = 5086

# SIP URI Scheme When Using TLS
# 0 -sip, 1 - sips. Default value is 0.
# Number: 0, 1
P52329 = 0

# Use Actual Ephemeral Port in Contact with TCP/TLS
# 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P52331 = 0

# Support SIP Instance ID. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P51389 = 1

# SIP T1 Timeout. RFC 3261 T1 value (RTT estimate)
# 50 - 0.5 sec, 100 - 1 sec, 200 - 2 sec. Default value is 50
# Number: 50, 100, 200
P51340 = 50

# SIP T2 Interval. RFC 3261 T2 value. The maximum retransmit interval for non-INVITE requests and INVITE responses
# 200 - 2 sec, 400 - 4 sec, 800 - 8 sec. Default 400
# Number: 200, 400, 800
P51341 = 400

# SIP Timer D Interval (Seconds)
# Number 0-64. Default value is 0
P52387 = 0

# Remove OBP from route. 0 - Disable, 1 - Enable. Default value is 0
# Number: 0, 1
P52305 = 0

# Enable 100rel. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P51335 = 0

#######################################################################
##  Account 14 Session Timer                                          ##
#######################################################################

# Enable Session Timer/ Session Expiration(s).  In seconds. Default value is 180 seconds.
# By default,  Session Timer is Enabled.  Session Timer is disabled if the value is 0.
# Number: 0 or 90 - 64800
P51334 = 180

# Min-SE (s). Default value is 90 seconds
# Number: 0 or 90 - 64800
P51327 = 90

# UAC Specify Refresher. 0 - Omit, 1 - UAC, 2 - UAS. Default value is 0
# Number: 0, 1, 2
P51332 = 0

# UAS Specify Refresher. 1 - UAC, 2 - UAS. Default value is 1
# Number: 1, 2
P51333 = 1

# Caller Request Timer (Request for timer when calling)
# 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1.
P51328 = 0

# Callee Request Timer. Request for timer when called (i.e. if remote party supports timer but did not request for one)
# 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P51329 = 0

# Force Timer (Still use timer when remote party does not support timer). 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P51330 = 0

# Force INVITE (Always refresh with INVITE instead of UPDATE even when remote party supports UPDATE)
# 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P51331 = 0

#######################################################################
##  Account 14 Codec Settings                                         ##
#######################################################################
# Preferred Vocoder
# First codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 103 - G722.1C, 104 - G722.1, 123 - Opus. Default value is 0
# Number: 0, 2, 8, 9, 18, 98, 103, 104, 123
P51351 = 0

# Second codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 103 - G722.1C, 104 - G722.1, 123 - Opus. Default value is 8
# Number: 0, 2, 8, 9, 18, 98, 103, 104, 123
P51352 = 8

# Third codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 103 - G722.1C, 104 - G722.1, 123 - Opus. Default value is 9
# Number: 0, 2, 8, 9, 18, 98, 103, 104, 123
P51353 = 9

# Forth codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 103 - G722.1C, 104 - G722.1, 123 - Opus. Default value is 104
# Number: 0, 2, 8, 9, 18, 98, 103, 104, 123
P51354 = 104

# Fifth codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 103 - G722.1C, 104 - G722.1, 123 - Opus. Default value is 104
# Number: 0, 2, 8, 9, 18, 98, 103, 104, 123
P51355 = 104

# Sixth codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 103 - G722.1C, 104 - G722.1, 123 - Opus. Default value is 104
# Number: 0, 2, 8, 9, 18, 98, 103, 104, 123
P51356 = 104

# Seventh codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 103 - G722.1C, 104 - G722.1, 123 - Opus. Default value is 104
# Number: 0, 2, 8, 9, 18, 98, 103, 104, 123
P51357 = 104

# Eigth codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 103 - G722.1C, 104 - G722.1, 123 - Opus. Default value is 104
# Number: 0, 2, 8, 9, 18, 98, 103, 104, 123
P51358 = 104

# Codec Negotiation Priority. 0 - Caller, 1 - Callee. Default value is 1.
# Number: 0, 1
P54361 = 1

# Use First Matching Vocoder in 200OK SDP. 0 - No, 1 - Yes. The default value is 0.
# Number: 0, 1
P52348 = 0

# iLBC Frame Size. 0 - 20 ms, 1 - 30 ms. Default value is 1.
# Number: 0, 1
P51395 = 1

# G726-32 ITU Payload. 0 - 2, 1 - Dynamic. Default value is 0.
# Number: 0, 1
P52369 = 0

# G726-32 Dynamic PT. Default value is 126.
# Number
P52365 = 126

# Opus Payload Type. Default value is 123.
P52385 = 123

# DTMF: in audio. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P52301 = 0

# DTMF: in RFC2833. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P52302 = 1

# DTMF: in SIP INFO. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P52303 = 0

# DTMF Payload Type. Default value is 101
# Number: 96 - 127
P51396 = 101

# Enable Audio RED with FEC. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P53373 = 0

# Audio FEC Payload Type. Default value is 121
# Number: 96 - 126
P53374 = 121

# Audio RED Payload Type. Default value is 124
# Number: 96 - 126
P53375 = 124

# Silence Suppression. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P51385 = 0

# Voice Frames per TX. Default valule is 2
# Number: 1 - 64
P51386 = 2

#######################################################################
##  Account 14 RTP Settings                                          ##
#######################################################################
# SRTP Mode. 0 - Disable, 1 - Enabled but not forced, 2 - Enabled and forced. Default value is 0
# Number: 0, 1, 2
P51343 = 0

# SRTP Key Length. 0 - AES 128&256 bit, 1 - AES 128 bit, 2 - AES 256 bit. Default value is 0
#Number:0, 1, 2
P52383 = 0

# Enable SRTP Key Life Time. 0 - No, 1 - Yes.
# Number: 0,1
P52363 = 1

# RTCP Destination
P52390 =

# Symmetric RTP. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P51360 = 0

# RTP IP Filter. 0 - Disable, 1 - IP Only, 2 - IP and Port. Default value is 0
# Number: 0, 1, 2
P53326 = 0

#######################################################################
##  Account 14 Call Settings                                          ##
#######################################################################
# Play warning tone for Auto Answer Intercom. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P53372 = 1

# Send Anonymous. 0 - No, 1 - Yes (caller ID will be blocked if set to Yes). Default value is 0
# Number: 0, 1
P51321 = 0

# Intercept Anonymous Calls. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P51346 = 0

# Call Log. 0 - Log All, 1 - Log Incoming/Outgoing only (Missed Calls Not Recorded), 2 - Disable Call All. Default value is 0
# Number: 0, 1
P51342 = 0

# Ring Timeout. Default value is 60 seconds
# Number: 0 - 300
P51376 = 60

# Refer-To Use Target Contact. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P51369 = 0

# Incoming Call Rules. 0 - Block, 1 - Set Password, 2 - Auto Answer, 3 - Ringing, 4 - Disable. Default value is 4.
# Number: 0, 1, 2 ,3 ,4
P61344 = 4

# Set Password Rules. 
# Numbers
P61345

# Dial Plan Prefix
# String
P51319 =

# Disable DialPlan. 0 - No Selection, 1 - Dial Page, 2 - Contact, 4 - Incoming Call History, 8 -  Outgoing Call History, 16 - MPK & Click2Dial. 
# If need to check multiple selections, add the specific values for each selections together. Default value is 0
# Number: 0-31
P52382 = 0

# Dial Plan. Default value is { x+ | \+x+ | *x+ | *xx*x+ }
P51359 = { x+ | \+x+ | *x+ | *xx*x+ }

# Account Ringtone. See ring tone options and value in the Ring Tone Value Table below.
P51323 = content://settings/system/ringtone

# Ignore Alert-Info Header. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1
P53318 = 0

# Matching Incoming Caller ID. Matching Rule 1.
# String
P53377 =

# Matching Rule 1 Distinctive Ringtone. See ring tone options and value in the Ring Tone Value Table below.
# String
P53378 = content://settings/system/ringtone

# Matching Incoming Caller ID. Matching Rule 2.
# String
P53379 =

# Matching Rule 2 Distinctive Ringtone. See ring tone options and value in the Ring Tone Value Table below.
# String
P53380 = content://settings/system/ringtone

# Matching Incoming Caller ID. Matching Rule 3.
# String
P53381 =

# Matching Rule 3 Distinctive Ringtone. See ring tone options and value in the Ring Tone Value Table below.
# String
P53382 = content://settings/system/ringtone

############Ring Tone Value Table###############
# Web GUI Option                            Value
# Use System Ring tone                      content://settings/system/ringtone 
# Andromeda					/system/media/audio/ringtones/ANDROMEDA.ogg
# Aquila					/system/media/audio/ringtones/Aquila.ogg
# Argo Navis					/system/media/audio/ringtones/ArgoNavis.ogg
# Atria					/system/media/audio/ringtones/Atria.ogg
# Backroad					/system/media/audio/ringtones/Backroad.ogg
# Beat Plucker					/system/media/audio/ringtones/BeatPlucker.ogg
# Bell Phone					/system/media/audio/ringtones/Ring_Classic_02.ogg
# Bentley Dubs					/system/media/audio/ringtones/BentleyDubs.ogg
# Big Easy					/system/media/audio/ringtones/Big_Easy.ogg
# Bird Loop					/system/media/audio/ringtones/BirdLoop.ogg
# Bollywood					/system/media/audio/ringtones/Bollywood.ogg
# Boötes					/system/media/audio/ringtones/BOOTES.ogg
# Bus' a Move					/system/media/audio/ringtones/BussaMove.ogg
# Cairo					/system/media/audio/ringtones/Cairo.ogg
# Calypso Steel					/system/media/audio/ringtones/Calypso_Steel.ogg
# Canis Major					/system/media/audio/ringtones/CANISMAJOR.ogg
# Caribbean Ice					/system/media/audio/ringtones/CaribbeanIce.ogg
# Carina					/system/media/audio/ringtones/Carina.ogg
# Cassiopeia					/system/media/audio/ringtones/CASSIOPEIA.ogg
# Centaurus					/system/media/audio/ringtones/Centaurus.ogg
# Champagne Edition					/system/media/audio/ringtones/Champagne_Edition.ogg
# Chimey Phone					/system/media/audio/ringtones/Ring_Synth_02.ogg
# Club Cubano					/system/media/audio/ringtones/Club_Cubano.ogg
# Crayon Rock					/system/media/audio/ringtones/CrayonRock.ogg
# Crazy Dream					/system/media/audio/ringtones/CrazyDream.ogg
# Curve Ball Blend					/system/media/audio/ringtones/CurveBall.ogg
# Cygnus					/system/media/audio/ringtones/Cygnus.ogg
# Dancin' Fool					/system/media/audio/ringtones/DancinFool.ogg
# Digital Phone					/system/media/audio/ringtones/Ring_Digital_02.ogg
# Ding					/system/media/audio/ringtones/Ding.ogg
# DingDong					/system/media/audio/ringtones/DingDong.wav
# Don' Mess Wiv It					/system/media/audio/ringtones/DonMessWivIt.ogg
# Draco					/system/media/audio/ringtones/Draco.ogg
# Dream Theme					/system/media/audio/ringtones/DreamTheme.ogg
# Eastern Sky					/system/media/audio/ringtones/Eastern_Sky.ogg
# Enter the Nexus					/system/media/audio/ringtones/Enter_the_Nexus.ogg
# Eridani					/system/media/audio/ringtones/Eridani.ogg
# Ether Shake					/system/media/audio/ringtones/EtherShake.ogg
# Flutey Phone					/system/media/audio/ringtones/Ring_Synth_04.ogg
# Free Flight					/system/media/audio/ringtones/FreeFlight.ogg
# Friendly Ghost					/system/media/audio/ringtones/FriendlyGhost.ogg
# Funk Y'all					/system/media/audio/ringtones/Funk_Yall.ogg
# Game Over Guitar					/system/media/audio/ringtones/GameOverGuitar.ogg
# Gimme Mo' Town					/system/media/audio/ringtones/Gimme_Mo_Town.ogg
# Girtab					/system/media/audio/ringtones/Girtab.ogg
# Glacial Groove					/system/media/audio/ringtones/Glacial_Groove.ogg
# Growl					/system/media/audio/ringtones/Growl.ogg
# Halfway Home					/system/media/audio/ringtones/HalfwayHome.ogg
# Hydra					/system/media/audio/ringtones/Hydra.ogg
# Insert Coin					/system/media/audio/ringtones/InsertCoin.ogg
# Kuma					/system/media/audio/ringtones/Kuma.ogg
# Loopy Lounge					/system/media/audio/ringtones/LoopyLounge.ogg
# Love Flute					/system/media/audio/ringtones/LoveFlute.ogg
# Lyra					/system/media/audio/ringtones/Lyra.ogg
# Machina					/system/media/audio/ringtones/Machina.ogg
# Medieval Jaunt					/system/media/audio/ringtones/MidEvilJaunt.ogg
# Mildly Alarming					/system/media/audio/ringtones/MildlyAlarming.ogg
# Nairobi					/system/media/audio/ringtones/Nairobi.ogg
# Nassau					/system/media/audio/ringtones/Nassau.ogg
# New Player					/system/media/audio/ringtones/NewPlayer.ogg
# No Limits					/system/media/audio/ringtones/No_Limits.ogg
# Noisey One					/system/media/audio/ringtones/Noises1.ogg
# Organ Dub					/system/media/audio/ringtones/OrganDub.ogg
# Orion					/system/media/audio/ringtones/Orion.ogg
# Paradise Island					/system/media/audio/ringtones/Paradise_Island.ogg
# Pegasus					/system/media/audio/ringtones/Pegasus.ogg
# Perseus					/system/media/audio/ringtones/PERSEUS.ogg
# Playa					/system/media/audio/ringtones/Playa.ogg
# Pyxis					/system/media/audio/ringtones/Pyxis.ogg
# Rasalas					/system/media/audio/ringtones/Rasalas.ogg
# Revelation					/system/media/audio/ringtones/Revelation.ogg
# Rigel					/system/media/audio/ringtones/Rigel.ogg
# Road Trip					/system/media/audio/ringtones/Road_Trip.ogg
# Romancing The Tone					/system/media/audio/ringtones/RomancingTheTone.ogg
# Safari					/system/media/audio/ringtones/Safari.ogg
# Savannah					/system/media/audio/ringtones/Savannah.ogg
# Scarabaeus					/system/media/audio/ringtones/Scarabaeus.ogg
# Sceptrum					/system/media/audio/ringtones/Sceptrum.ogg
# Seville					/system/media/audio/ringtones/Seville.ogg
# She's All That					/system/media/audio/ringtones/Shes_All_That.ogg
# Silky Way					/system/media/audio/ringtones/SilkyWay.ogg
# Sitar Versus Sitar					/system/media/audio/ringtones/SitarVsSitar.ogg
# Solarium					/system/media/audio/ringtones/Solarium.ogg
# Springy Jalopy					/system/media/audio/ringtones/SpringyJalopy.ogg
# Steppin' Out					/system/media/audio/ringtones/Steppin_Out.ogg
# Terminated					/system/media/audio/ringtones/Terminated.ogg
# Terrible Twos					/system/media/audio/ringtones/Noises2.ogg
# Testudo					/system/media/audio/ringtones/Testudo.ogg
# Themos					/system/media/audio/ringtones/Themos.ogg
# Third Eye					/system/media/audio/ringtones/Third_Eye.ogg
# Thriller Three					/system/media/audio/ringtones/Noises3.ogg
# Thunderfoot					/system/media/audio/ringtones/Thunderfoot.ogg
# Twirl Away					/system/media/audio/ringtones/TwirlAway.ogg
# Ursa Minor					/system/media/audio/ringtones/URSAMINOR.ogg
# UrsaMinor					/system/media/audio/ringtones/UrsaMinor.ogg
# Very Alarmed					/system/media/audio/ringtones/VeryAlarmed.ogg
# Vespa					/system/media/audio/ringtones/Vespa.ogg
# World					/system/media/audio/ringtones/World.ogg
# Zeta					/system/media/audio/ringtones/Zeta.ogg
# bellcore-dr1					/system/media/audio/ringtones/bellcore-dr1.ogg
# bellcore-dr2					/system/media/audio/ringtones/bellcore-dr2.ogg
# bellcore-dr3					/system/media/audio/ringtones/bellcore-dr3.ogg
# bellcore-dr4					/system/media/audio/ringtones/bellcore-dr4.ogg
# bellcore-dr5					/system/media/audio/ringtones/bellcore-dr5.ogg
# speaker					/system/media/audio/ringtones/speaker.wav

#######################################################################
##  Account 14 Advanced Settings                                      ##
#######################################################################
# Check Domain Certificates. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P52311 = 0

# Validate Certificate Chain. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P52367 = 0

# Validate Incoming SIP Messages. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P52306 = 0

# Allow Unsolicited REFER. 0 - Disabled, 1 - Enabled, 2 - Enabled/Force Auth. Default value is 0.
# Number: 0, 1, 2
P53323 = 0

# Only Accept SIP Requests from Known Servers. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P52347 = 0

# Check SIP User ID for Incoming INVITE. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P51349 = 0

# Allow SIP Reset. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P53315 = 0

# Authenticate Incoming INVITE. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P52346 = 0

# SIP Realm Used for Challenge INVITE & NOTIFY.
# String
P53321 =

# Enable Local MOH
# Number: 0, 1 
P52357 = 0

# Virtual Account Group. -1 - Default,  0 - Virtual Account Group 1, 1 - Virtual Account Group 2, 2 - Virtual Account Group 3
# 3 - Virtual Account Group 4, 4 - Virtual Account Group 5, 5 - Virtual Account Group 6, 6 - Virtual Account Group 7, 7 - Virtual Account Group 8
# 8 - Virtual Account Group 9, 9 - Virtual Account Group 10, 10 - Virtual Account Group 11, 11 - Virtual Account Group 12, 12 - Virtual Account Group 13
# 13 - Virtual Account Group 14, 14 - Virtual Account Group 15, 15 - Virtual Account Group 16. Default value is -1.
# Number: -1 - 15 
P52391 = -1

# Special Feature. Default value is 100
# 100 - Standard, 102 - Broadsoft, 113 - China Mobile, 114 - ZTE IMS, 115 - Mobotix
# 116 - ZTE NGN, 117 - Huawei IMS, 123 - NEC, 125 - WorldStone, 129 - Telefonica Spain
# Number: 100, 102, 113, 114, 115, 116, 117, 123, 125, 129
P51324 = 100

# Feature Key Synchronization.  0 - Disable, 0 - Broadsoft/Metaswitch. Default Value is 0.
# Number: 0, 1
# P52325 = 0

# Allow Sync Phonebook via SIP Notify. 0 - No, 1 - Yes. Default is 1.
# Number: 0, 1
P53399 = 1

##############################################################################
##  Account 15 Settings                                                     ##
##############################################################################
#######################################################################
##  Account 15 General Settings                                      ##
#######################################################################
# Account Active. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P51401 = 0

# Account Name
P51417 = 

# SIP Server
P51402 = 

# SIP User ID
P51404 =
 
# SIP Authentication ID
P51405 =

# SIP Authentication Password
P51406 =

# Tel URI. 0 - Disable, 1 - User=Phone, 2 - Enabled. Default value is 0
# Number: 0, 1, 2
P51409 = 0

#######################################################################
##  Account 15 Network Settings                                      ##
#######################################################################
# Outbound Proxy
P51403 =

# Secondary Outbound Proxy
P52433 =

# DNS Mode.  0 - A Record, 1 - SRV, 2 - NAPTR/SRV. Default value is 0
# Number: 0, 1, 2
P51408 = 0

# DNS SRV Fail-over Mode. 0 - Default, 1 - Saved one until DNS TTL, 2 - Saved one until no response. Defualt value is 1
# Number
P53440 = 0

# Register Before DNS SRV Fail-over. 0 - No, 1 - Yes. Default Value is 0.
# Number: 0, 1
P54495 = 1

# NAT Traversal. 0 - NAT No, 1 - STUN, 2 - Keep-alive, 3 - UPnP, 4 - Auto, 5 - VPN. Default value is 2
# Number: 0, 1, 2, 3, 4, 5
P51414 = 2

# Proxy-Require
P51418 =

#######################################################################
##  Account 15 SIP Settings                                          ##
#######################################################################
# SIP Registration. 0 - No, 1 - Yes. Default is 1
# Number: 0, 1
P51410 = 1

# Unregister Before New Registration. 0 - No, 1 - All, 2 -  Instance . Default value is 2
# Number: 0, 1, 2
P51411 = 2

# Register Expiration (m). In minutes. Default value is 60
# Number: 60 - 64800
P51412 = 60

# Subscribe Expiration (m). In minutes. Default value is blank
# Number: 0 - 64800
P53451 = 60

# Re-register before Expiration (s). Default value is 0
# Number: 0 - 3600
P52430 = 0

# Registration Retry Wait Time (s). In seconds. Default value is 20
# Number: 20 - 3600
P51471 = 20

# Add Auth Header On RE-REGISTER
# 0 - No, 1- Yes
P52459 = 1

# Enable SIP OPTIONS Keep Alive. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P52497 = 0

# SIP OPTIONS Keep Alive Interval(s). Default value is 30
# Number: 1 - 64800 
P52498 = 30

# SIP OPTIONS Keep Alive Maximum Tries. Default value is 3
# Number: 3 
P52499 = 3

# Use Privacy Header. 0 - Default, 1 - No, 2 - Yes. Default value is 0
# Number: 0, 1, 2
P52438 = 0

# Use P-Preferred-Identity Header. 0 - Default, 1 - No, 2 - Yes. Default value is 0
# Number: 0, 1, 2
P52439 = 0

# SIP Transport. 0 - UDP, 1 - TCP, 2 - TLS. Default value is 0
# Number: 0, 1, 2
P51448 = 0

# Local SIP Port. Default value is 5088
# Number: 0 or 90 - 65535
P51413 = 5088

# SIP URI Scheme When Using TLS
# 0 -sip, 1 - sips. Default value is 0.
# Number: 0, 1
P52429 = 0

# Use Actual Ephemeral Port in Contact with TCP/TLS
# 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P52431 = 0

# Support SIP Instance ID. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P51489 = 1

# SIP T1 Timeout. RFC 3261 T1 value (RTT estimate)
# 50 - 0.5 sec, 100 - 1 sec, 200 - 2 sec. Default value is 50
# Number: 50, 100, 200
P51440 = 50

# SIP T2 Interval. RFC 3261 T2 value. The maximum retransmit interval for non-INVITE requests and INVITE responses
# 200 - 2 sec, 400 - 4 sec, 800 - 8 sec. Default 400
# Number: 200, 400, 800
P51441 = 400

# SIP Timer D Interval (Seconds)
# Number 0-64. Default value is 0
P52487 = 0

# Remove OBP from route. 0 - Disable, 1 - Enable. Default value is 0
# Number: 0, 1
P52405 = 0

# Enable 100rel. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P51435 = 0

#######################################################################
##  Account 15 Session Timer                                          ##
#######################################################################

# Enable Session Timer/ Session Expiration(s).  In seconds. Default value is 180 seconds.
# By default,  Session Timer is Enabled.  Session Timer is disabled if the value is 0.
# Number: 0 or 90 - 64800
P51434 = 180

# Min-SE (s). Default value is 90 seconds
# Number: 0 or 90 - 64800
P51427 = 90

# UAC Specify Refresher. 0 - Omit, 1 - UAC, 2 - UAS. Default value is 0
# Number: 0, 1, 2
P51432 = 0

# UAS Specify Refresher. 1 - UAC, 2 - UAS. Default value is 1
# Number: 1, 2
P51433 = 1

# Caller Request Timer. Request for timer when calling
# 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P51428 = 0

# Callee Request Timer
# Request for timer when being called (i.e., if remote party supports timer but did not request for one)
# 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P51429 = 0

# Force Timer (Still use timer when remote party does not support timer). 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P51430 = 0

# Force INVITE (Always refresh with INVITE instead of UPDATE even when remote party supports UPDATE)
# 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P51431 = 0

#######################################################################
##  Account 15 Codec Settings                                         ##
#######################################################################
# Preferred Vocoder
# First codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 103 - G722.1C, 104 - G722.1, 123 - Opus. Default value is 0
# Number: 0, 2, 8, 9, 18, 98, 103, 104, 123
P51451 = 0

# Second codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 103 - G722.1C, 104 - G722.1, 123 - Opus. Default value is 8
# Number: 0, 2, 8, 9, 18, 98, 103, 104, 123
P51452 = 8

# Third codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 103 - G722.1C, 104 - G722.1, 123 - Opus. Default value is 9
# Number: 0, 2, 8, 9, 18, 98, 103, 104, 123
P51453 = 9

# Forth codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 103 - G722.1C, 104 - G722.1, 123 - Opus. Default value is 104
# Number: 0, 2, 8, 9, 18, 98, 103, 104, 123
P51454 = 104

# Fifth codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 103 - G722.1C, 104 - G722.1, 123 - Opus. Default value is 104
# Number: 0, 2, 8, 9, 18, 98, 103, 104, 123
P51455 = 104

# Sixth codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 103 - G722.1C, 104 - G722.1, 123 - Opus. Default value is 104
# Number: 0, 2, 8, 9, 18, 98, 103, 104, 123
P51456 = 104

# Seventh codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 103 - G722.1C, 104 - G722.1, 123 - Opus. Default value is 104
# Number: 0, 2, 8, 9, 18, 98, 103, 104, 123
P51457 = 104

# Eigth codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 103 - G722.1C, 104 - G722.1, 123 - Opus. Default value is 104
# Number: 0, 2, 8, 9, 18, 98, 103, 104, 123
P51458 = 104

# Codec Negotiation Priority. 0 - Caller, 1 - Callee. Default value is 1.
# Number: 0, 1
P54461 = 1

# Use First Matching Vocoder in 200OK SDP. 0 - No, 1 - Yes. The default value is 0.
# Number: 0, 1
P52448 = 0

# iLBC Frame Size. 0 - 20 ms, 1 - 30 ms. Default value is 1.
# Number: 0, 1
P51495 = 1

# G726-32 ITU Payload. 0 - 2, 1 - Dynamic. Default value is 0.
# Number: 0, 1
P52469 = 0

# G726-32 Dynamic PT. Default value is 126.
# Number
P52465 = 126

# Opus Payload Type. Default value is 123.
P52485 = 123

# DTMF: in audio. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P52401 = 0

# DTMF: in RFC2833. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P52402 = 1

# DTMF: in SIP INFO. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P52403 = 0

# DTMF Payload Type. Default value is 101
# Number: 96 - 127
P51496 = 101

# Enable Audio RED with FEC. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P53473 = 0

# Audio FEC Payload Type. Default value is 121
# Number: 96 - 126
P53474 = 121

# Audio RED Payload Type. Default value is 124
# Number: 96 - 126
P53475 = 124

# Silence Suppression. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P51485 = 0

# Voice Frames per TX. Default valule is 2
# Number: 1 - 64
P51486 = 2

#######################################################################
##  Account 15 RTP Settings                                          ##
#######################################################################
# SRTP Mode. 0 - Disable, 1 - Enabled but not forced, 2 - Enabled and forced. Default value is 0
# Number: 0, 1, 2
P51443 = 0

# SRTP Key Length. 0 - AES 128&256 bit, 1 - AES 128 bit, 2 - AES 256 bit. Default value is 0
#Number:0, 1, 2
P52483 = 0

# Enable SRTP Key Life Time. 0 - No, 1 - Yes.
# Number: 0,1
P52463 = 1

# RTCP Destination
P52490 =

# Symmetric RTP. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P51460 = 0

# RTP IP Filter. 0 - Disable, 1 - IP Only, 2 - IP and Port. Default value is 0
# Number: 0, 1, 2
P53426 = 0

#######################################################################
##  Account 15 Call Settings                                          ##
#######################################################################
# Play warning tone for Auto Answer Intercom. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P53472 = 1

# Send Anonymous. 0 - No, 1 - Yes (caller ID will be blocked if set to Yes). Default value is 0
# Number: 0, 1
P51421 = 0

# Intercept Anonymous Calls. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P51446 = 0

# Call Log. 0 - Log All, 1 - Log Incoming/Outgoing only (Missed Calls Not Recorded), 2 - Disable Call All. Default value is 0
# Number: 0, 1
P51442 = 0

# Ring Timeout. Default value is 60 seconds
# Number: 0 - 300
P51476 = 60

# Refer-To Use Target Contact. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P51469 = 0

# Incoming Call Rules. 0 - Block, 1 - Set Password, 2 - Auto Answer, 3 - Ringing, 4 - Disable. Default value is 4.
# Number: 0, 1, 2 ,3 ,4
P61444 = 4

# Set Password Rules. 
# Numbers
P61445

# Dial Plan Prefix
# String
P51419 =

# Disable DialPlan. 0 - No Selection, 1 - Dial Page, 2 - Contact, 4 - Incoming Call History, 8 -  Outgoing Call History, 16 - MPK & Click2Dial. 
# If need to check multiple selections, add the specific values for each selections together. Default value is 0
# Number: 0-31
P52482 = 0

# Dial Plan. Default value is { x+ | \+x+ | *x+ | *xx*x+ }
P51459 = { x+ | \+x+ | *x+ | *xx*x+ }

# Account Ringtone. See ring tone options and value in the Ring Tone Value Table below.
P51423 = content://settings/system/ringtone

# Ignore Alert-Info Header. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1
P53418 = 0

# Matching Incoming Caller ID. Matching Rule 1.
# String
P53477 =

# Matching Rule 1 Distinctive Ringtone. See ring tone options and value in the Ring Tone Value Table below.
# String
P53478 = content://settings/system/ringtone

# Matching Incoming Caller ID. Matching Rule 2.
# String
P53479 =

# Matching Rule 2 Distinctive Ringtone. See ring tone options and value in the Ring Tone Value Table below.
# String
P53480 = content://settings/system/ringtone

# Matching Incoming Caller ID. Matching Rule 3.
# String
P53481 =

# Matching Rule 3 Distinctive Ringtone. See ring tone options and value in the Ring Tone Value Table below.
# String
P53482 = content://settings/system/ringtone

############Ring Tone Value Table###############
# Web GUI Option                            Value
# Use System Ring tone                      content://settings/system/ringtone 
# Andromeda					/system/media/audio/ringtones/ANDROMEDA.ogg
# Aquila					/system/media/audio/ringtones/Aquila.ogg
# Argo Navis					/system/media/audio/ringtones/ArgoNavis.ogg
# Atria					/system/media/audio/ringtones/Atria.ogg
# Backroad					/system/media/audio/ringtones/Backroad.ogg
# Beat Plucker					/system/media/audio/ringtones/BeatPlucker.ogg
# Bell Phone					/system/media/audio/ringtones/Ring_Classic_02.ogg
# Bentley Dubs					/system/media/audio/ringtones/BentleyDubs.ogg
# Big Easy					/system/media/audio/ringtones/Big_Easy.ogg
# Bird Loop					/system/media/audio/ringtones/BirdLoop.ogg
# Bollywood					/system/media/audio/ringtones/Bollywood.ogg
# Boötes					/system/media/audio/ringtones/BOOTES.ogg
# Bus' a Move					/system/media/audio/ringtones/BussaMove.ogg
# Cairo					/system/media/audio/ringtones/Cairo.ogg
# Calypso Steel					/system/media/audio/ringtones/Calypso_Steel.ogg
# Canis Major					/system/media/audio/ringtones/CANISMAJOR.ogg
# Caribbean Ice					/system/media/audio/ringtones/CaribbeanIce.ogg
# Carina					/system/media/audio/ringtones/Carina.ogg
# Cassiopeia					/system/media/audio/ringtones/CASSIOPEIA.ogg
# Centaurus					/system/media/audio/ringtones/Centaurus.ogg
# Champagne Edition					/system/media/audio/ringtones/Champagne_Edition.ogg
# Chimey Phone					/system/media/audio/ringtones/Ring_Synth_02.ogg
# Club Cubano					/system/media/audio/ringtones/Club_Cubano.ogg
# Crayon Rock					/system/media/audio/ringtones/CrayonRock.ogg
# Crazy Dream					/system/media/audio/ringtones/CrazyDream.ogg
# Curve Ball Blend					/system/media/audio/ringtones/CurveBall.ogg
# Cygnus					/system/media/audio/ringtones/Cygnus.ogg
# Dancin' Fool					/system/media/audio/ringtones/DancinFool.ogg
# Digital Phone					/system/media/audio/ringtones/Ring_Digital_02.ogg
# Ding					/system/media/audio/ringtones/Ding.ogg
# DingDong					/system/media/audio/ringtones/DingDong.wav
# Don' Mess Wiv It					/system/media/audio/ringtones/DonMessWivIt.ogg
# Draco					/system/media/audio/ringtones/Draco.ogg
# Dream Theme					/system/media/audio/ringtones/DreamTheme.ogg
# Eastern Sky					/system/media/audio/ringtones/Eastern_Sky.ogg
# Enter the Nexus					/system/media/audio/ringtones/Enter_the_Nexus.ogg
# Eridani					/system/media/audio/ringtones/Eridani.ogg
# Ether Shake					/system/media/audio/ringtones/EtherShake.ogg
# Flutey Phone					/system/media/audio/ringtones/Ring_Synth_04.ogg
# Free Flight					/system/media/audio/ringtones/FreeFlight.ogg
# Friendly Ghost					/system/media/audio/ringtones/FriendlyGhost.ogg
# Funk Y'all					/system/media/audio/ringtones/Funk_Yall.ogg
# Game Over Guitar					/system/media/audio/ringtones/GameOverGuitar.ogg
# Gimme Mo' Town					/system/media/audio/ringtones/Gimme_Mo_Town.ogg
# Girtab					/system/media/audio/ringtones/Girtab.ogg
# Glacial Groove					/system/media/audio/ringtones/Glacial_Groove.ogg
# Growl					/system/media/audio/ringtones/Growl.ogg
# Halfway Home					/system/media/audio/ringtones/HalfwayHome.ogg
# Hydra					/system/media/audio/ringtones/Hydra.ogg
# Insert Coin					/system/media/audio/ringtones/InsertCoin.ogg
# Kuma					/system/media/audio/ringtones/Kuma.ogg
# Loopy Lounge					/system/media/audio/ringtones/LoopyLounge.ogg
# Love Flute					/system/media/audio/ringtones/LoveFlute.ogg
# Lyra					/system/media/audio/ringtones/Lyra.ogg
# Machina					/system/media/audio/ringtones/Machina.ogg
# Medieval Jaunt					/system/media/audio/ringtones/MidEvilJaunt.ogg
# Mildly Alarming					/system/media/audio/ringtones/MildlyAlarming.ogg
# Nairobi					/system/media/audio/ringtones/Nairobi.ogg
# Nassau					/system/media/audio/ringtones/Nassau.ogg
# New Player					/system/media/audio/ringtones/NewPlayer.ogg
# No Limits					/system/media/audio/ringtones/No_Limits.ogg
# Noisey One					/system/media/audio/ringtones/Noises1.ogg
# Organ Dub					/system/media/audio/ringtones/OrganDub.ogg
# Orion					/system/media/audio/ringtones/Orion.ogg
# Paradise Island					/system/media/audio/ringtones/Paradise_Island.ogg
# Pegasus					/system/media/audio/ringtones/Pegasus.ogg
# Perseus					/system/media/audio/ringtones/PERSEUS.ogg
# Playa					/system/media/audio/ringtones/Playa.ogg
# Pyxis					/system/media/audio/ringtones/Pyxis.ogg
# Rasalas					/system/media/audio/ringtones/Rasalas.ogg
# Revelation					/system/media/audio/ringtones/Revelation.ogg
# Rigel					/system/media/audio/ringtones/Rigel.ogg
# Road Trip					/system/media/audio/ringtones/Road_Trip.ogg
# Romancing The Tone					/system/media/audio/ringtones/RomancingTheTone.ogg
# Safari					/system/media/audio/ringtones/Safari.ogg
# Savannah					/system/media/audio/ringtones/Savannah.ogg
# Scarabaeus					/system/media/audio/ringtones/Scarabaeus.ogg
# Sceptrum					/system/media/audio/ringtones/Sceptrum.ogg
# Seville					/system/media/audio/ringtones/Seville.ogg
# She's All That					/system/media/audio/ringtones/Shes_All_That.ogg
# Silky Way					/system/media/audio/ringtones/SilkyWay.ogg
# Sitar Versus Sitar					/system/media/audio/ringtones/SitarVsSitar.ogg
# Solarium					/system/media/audio/ringtones/Solarium.ogg
# Springy Jalopy					/system/media/audio/ringtones/SpringyJalopy.ogg
# Steppin' Out					/system/media/audio/ringtones/Steppin_Out.ogg
# Terminated					/system/media/audio/ringtones/Terminated.ogg
# Terrible Twos					/system/media/audio/ringtones/Noises2.ogg
# Testudo					/system/media/audio/ringtones/Testudo.ogg
# Themos					/system/media/audio/ringtones/Themos.ogg
# Third Eye					/system/media/audio/ringtones/Third_Eye.ogg
# Thriller Three					/system/media/audio/ringtones/Noises3.ogg
# Thunderfoot					/system/media/audio/ringtones/Thunderfoot.ogg
# Twirl Away					/system/media/audio/ringtones/TwirlAway.ogg
# Ursa Minor					/system/media/audio/ringtones/URSAMINOR.ogg
# UrsaMinor					/system/media/audio/ringtones/UrsaMinor.ogg
# Very Alarmed					/system/media/audio/ringtones/VeryAlarmed.ogg
# Vespa					/system/media/audio/ringtones/Vespa.ogg
# World					/system/media/audio/ringtones/World.ogg
# Zeta					/system/media/audio/ringtones/Zeta.ogg
# bellcore-dr1					/system/media/audio/ringtones/bellcore-dr1.ogg
# bellcore-dr2					/system/media/audio/ringtones/bellcore-dr2.ogg
# bellcore-dr3					/system/media/audio/ringtones/bellcore-dr3.ogg
# bellcore-dr4					/system/media/audio/ringtones/bellcore-dr4.ogg
# bellcore-dr5					/system/media/audio/ringtones/bellcore-dr5.ogg
# speaker					/system/media/audio/ringtones/speaker.wav

#######################################################################
##  Account 15 Advanced Settings                                      ##
#######################################################################
# Check Domain Certificates. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P52411 = 0

# Validate Certificate Chain. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P52467 = 0

# Validate Incoming SIP Messages. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P52406 = 0

# Allow Unsolicited REFER. 0 - Disabled, 1 - Enabled, 2 - Enabled/Force Auth. Default value is 0.
# Number: 0, 1, 2
P53423 = 0

# Only Accept SIP Requests from Known Servers. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P52447 = 0

# Check SIP User ID for Incoming INVITE. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P51449 = 0

# Allow SIP Reset. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P53415 = 0

# Authenticate Incoming INVITE. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P52446 = 0

# SIP Realm Used for Challenge INVITE & NOTIFY.
# String
P53421 =

# Enable Local MOH
# Number: 0, 1 
P52457 = 0

# Virtual Account Group. -1 - Default,  0 - Virtual Account Group 1, 1 - Virtual Account Group 2, 2 - Virtual Account Group 3
# 3 - Virtual Account Group 4, 4 - Virtual Account Group 5, 5 - Virtual Account Group 6, 6 - Virtual Account Group 7, 7 - Virtual Account Group 8
# 8 - Virtual Account Group 9, 9 - Virtual Account Group 10, 10 - Virtual Account Group 11, 11 - Virtual Account Group 12, 12 - Virtual Account Group 13
# 13 - Virtual Account Group 14, 14 - Virtual Account Group 15, 15 - Virtual Account Group 16. Default value is -1.
# Number: -1 - 15 
P52491 = -1

# Special Feature. Default value is 100
# 100 - Standard, 102 - Broadsoft, 113 - China Mobile, 114 - ZTE IMS, 115 - Mobotix
# 116 - ZTE NGN, 117 - Huawei IMS, 123 - NEC, 125 - WorldStone, 129 - Telefonica Spain
# Number: 100, 102, 113, 114, 115, 116, 117, 123, 125, 129
P51424 = 100

# Feature Key Synchronization.  0 - Disable, 0 - Broadsoft/Metaswitch. Default Value is 0.
# Number: 0, 1
# P52425 = 0

# Allow Sync Phonebook via SIP Notify. 0 - No, 1 - Yes. Default is 1.
# Number: 0, 1
P53499 = 1

##############################################################################
##  Account 16 Settings                                                     ##
##############################################################################
#######################################################################
##  Account 16 General Settings                                      ##
#######################################################################
# Account Active. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P51501 = 0

# Account Name
P51517 = 

# SIP Server
P51502 = 

# SIP User ID
P51504 =
 
# SIP Authentication ID
P51505 =

# SIP Authentication Password
P51506 =

# Tel URI. 0 - Disable, 1 - User=Phone, 2 - Enabled. Default value is 0
# Number: 0, 1, 2
P51509 = 0

#######################################################################
##  Account 16 Network Settings                                      ##
#######################################################################
# Outbound Proxy
P51503 =

# Secondary Outbound Proxy
P52533 =

# DNS Mode.  0 - A Record, 1 - SRV, 2 - NAPTR/SRV. Default value is 0
# Number: 0, 1, 2
P51508 = 0

# DNS SRV Fail-over Mode. 0 - Default, 1 - Saved one until DNS TTL, 2 - Saved one until no response. Defualt value is 1
# Number
P53540 = 0

# Register Before DNS SRV Fail-over. 0 - No, 1 - Yes. Default Value is 0.
# Number: 0, 1
P54595 = 1

# NAT Traversal. 0 - NAT No, 1 - STUN, 2 - Keep-alive, 3 - UPnP, 4 - Auto, 5 - VPN. Default value is 2
# Number: 0, 1, 2, 3, 4, 5
P51514 = 2

# Proxy-Require
P51518 =

#######################################################################
##  Account 16 SIP Settings                                          ##
#######################################################################
# SIP Registration. 0 - No, 1 - Yes. Default is 1
# Number: 0, 1
P51510 = 1

# Unregister Before New Registration. 0 - No, 1 - All, 2 -  Instance . Default value is 2
# Number: 0, 1, 2
P51511 = 2

# Register Expiration (m). In minutes. Default value is 60
# Number: 60 - 64800
P51512 = 60

# Subscribe Expiration (m). In minutes. Default value is blank
# Number: 0 - 64800
P53551 = 60

# Re-register before Expiration (s). Default value is 0
# Number: 0 - 3600
P52530 = 0

# Registration Retry Wait Time (s). In seconds. Default value is 20
# Number: 20 - 3600
P51571 = 20

# Add Auth Header On RE-REGISTER
# 0 - No, 1- Yes
P52559 = 1

# Enable SIP OPTIONS Keep Alive. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P52597 = 0

# SIP OPTIONS Keep Alive Interval(s). Default value is 30
# Number: 1 - 64800 
P52598 = 30

# SIP OPTIONS Keep Alive Maximum Tries. Default value is 3
# Number: 3 
P52599 = 3

# Use Privacy Header. 0 - Default, 1 - No, 2 - Yes. Default value is 0
# Number: 0, 1, 2
P52538 = 0

# Use P-Preferred-Identity Header. 0 - Default, 1 - No, 2 - Yes. Default value is 0
# Number: 0, 1, 2
P52539 = 0

# SIP Transport. 0 - UDP, 1 - TCP, 2 - TLS. Default value is 0
# Number: 0, 1, 2
P51548 = 0

# Local SIP Port. Default value is 5090
# Number: 0 or 90 - 65535
P51513 = 5090

# SIP URI Scheme When Using TLS
# 0 -sip, 1 - sips. Default value is 0.
# Number: 0, 1
P52529 = 0

# Use Actual Ephemeral Port in Contact with TCP/TLS
# 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P52531 = 0

# Support SIP Instance ID. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P51589 = 1

# SIP T1 Timeout. RFC 3261 T1 value (RTT estimate)
# 50 - 0.5 sec, 100 - 1 sec, 200 - 2 sec. Default value is 50
# Number: 50, 100, 200
P51540 = 50

# SIP T2 Interval. RFC 3261 T2 value. The maximum retransmit interval for non-INVITE requests and INVITE responses
# 200 - 2 sec, 400 - 4 sec, 800 - 8 sec. Default 400
# Number: 200, 400, 800
P51541 = 400

# SIP Timer D Interval (Seconds)
# Number 0-64. Default value is 0
P52587 = 0

# Remove OBP from route. 0 - Disable, 1 - Enable. Default value is 0
# Number: 0, 1
P52505 = 0

# Enable 100rel. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P51535 = 0

#######################################################################
##  Account 16 Session Timer                                          ##
#######################################################################

# Enable Session Timer/ Session Expiration(s).  In seconds. Default value is 180 seconds.
# By default,  Session Timer is Enabled.  Session Timer is disabled if the value is 0.
# Number: 0 or 90 - 64800
P51534 = 180

# Min-SE (s). Default value is 90 seconds
# Number: 0 or 90 - 64800
P51527 = 90

# UAC Specify Refresher. 0 - Omit, 1 - UAC, 2 - UAS. Default value is 0
# Number: 0, 1, 2
P51532 = 0

# UAS Specify Refresher. 1 - UAC, 2 - UAS. Default value is 1
# Number: 1, 2
P51533 = 1

# Caller Request Timer. Request for timer when calling
# 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P51528 = 0

# Callee Request Timer
# Request for timer when being called (i.e., if remote party supports timer but did not request for one)
# 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P51529 = 0

# Force Timer (Still use timer when remote party does not support timer). 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P51530 = 0

# Force INVITE (Always refresh with INVITE instead of UPDATE even when remote party supports UPDATE)
# 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P51531 = 0

#######################################################################
##  Account 16 Codec Settings                                         ##
#######################################################################
# Preferred Vocoder
# First codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 103 - G722.1C, 104 - G722.1, 123 - Opus. Default value is 0
# Number: 0, 2, 8, 9, 18, 98, 103, 104, 123
P51551 = 0

# Second codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 103 - G722.1C, 104 - G722.1, 123 - Opus. Default value is 8
# Number: 0, 2, 8, 9, 18, 98, 103, 104, 123
P51552 = 8

# Third codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 103 - G722.1C, 104 - G722.1, 123 - Opus. Default value is 9
# Number: 0, 2, 8, 9, 18, 98, 103, 104, 123
P51553 = 9

# Forth codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 103 - G722.1C, 104 - G722.1, 123 - Opus. Default value is 104
# Number: 0, 2, 8, 9, 18, 98, 103, 104, 123
P51554 = 104

# Fifth codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 103 - G722.1C, 104 - G722.1, 123 - Opus. Default value is 104
# Number: 0, 2, 8, 9, 18, 98, 103, 104, 123
P51555 = 104

# Sixth codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 103 - G722.1C, 104 - G722.1, 123 - Opus. Default value is 104
# Number: 0, 2, 8, 9, 18, 98, 103, 104, 123
P51556 = 104

# Seventh codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 103 - G722.1C, 104 - G722.1, 123 - Opus. Default value is 104
# Number: 0, 2, 8, 9, 18, 98, 103, 104, 123
P51557 = 104

# Eigth codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 103 - G722.1C, 104 - G722.1, 123 - Opus. Default value is 104
# Number: 0, 2, 8, 9, 18, 98, 103, 104, 123
P51558 = 104

# Codec Negotiation Priority. 0 - Caller, 1 - Callee. Default value is 1.
# Number: 0, 1
P54561 = 1

# Use First Matching Vocoder in 200OK SDP. 0 - No, 1 - Yes. The default value is 0.
# Number: 0, 1
P52548 = 0

# iLBC Frame Size. 0 - 20 ms, 1 - 30 ms. Default value is 1.
# Number: 0, 1
P51595 = 1

# G726-32 ITU Payload. 0 - 2, 1 - Dynamic. Default value is 0.
# Number: 0, 1
P52569 = 0

# G726-32 Dynamic PT. Default value is 126.
# Number
P52565 = 126

# Opus Payload Type. Default value is 123.
P52585 = 123

# DTMF: in audio. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P52501 = 0

# DTMF: in RFC2833. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P52502 = 1

# DTMF: in SIP INFO. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P52503 = 0

# DTMF Payload Type. Default value is 101
# Number: 96 - 127
P51596 = 101

# Enable Audio RED with FEC. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P53573 = 0

# Audio FEC Payload Type. Default value is 121
# Number: 96 - 126
P53574 = 121

# Audio RED Payload Type. Default value is 124
# Number: 96 - 126
P53575 = 124

# Silence Suppression. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P51585 = 0

# Voice Frames per TX. Default valule is 2
# Number: 1 - 64
P51586 = 2

#######################################################################
##  Account 16 RTP Settings                                          ##
#######################################################################
# SRTP Mode. 0 - Disable, 1 - Enabled but not forced, 2 - Enabled and forced. Default value is 0
# Number: 0, 1, 2
P51543 = 0

# SRTP Key Length. 0 - AES 128&256 bit, 1 - AES 128 bit, 2 - AES 256 bit. Default value is 0
#Number:0, 1, 2
P52583 = 0

# Enable SRTP Key Life Time. 0 - No, 1 - Yes.
# Number: 0,1
P52563 = 1

# RTCP Destination
P52590 =

# Symmetric RTP. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P51560 = 0

# RTP IP Filter. 0 - Disable, 1 - IP Only, 2 - IP and Port. Default value is 0
# Number: 0, 1, 2
P53526 = 0

#######################################################################
##  Account 16 Call Settings                                          ##
#######################################################################
# Play warning tone for Auto Answer Intercom. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P53572 = 1

# Send Anonymous. 0 - No, 1 - Yes (caller ID will be blocked if set to Yes). Default value is 0
# Number: 0, 1
P51521 = 0

# Intercept Anonymous Calls. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P51546 = 0

# Call Log. 0 - Log All, 1 - Log Incoming/Outgoing only (Missed Calls Not Recorded), 2 - Disable Call All. Default value is 0
# Number: 0, 1
P51542 = 0

# Ring Timeout. Default value is 60 seconds
# Number: 0 - 300
P51576 = 60

# Refer-To Use Target Contact. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P51569 = 0

# Incoming Call Rules. 0 - Block, 1 - Set Password, 2 - Auto Answer, 3 - Ringing, 4 - Disable. Default value is 4.
# Number: 0, 1, 2 ,3 ,4
P61544 = 4

# Set Password Rules. 
# Numbers
P61545

# Dial Plan Prefix
# String
P51519 =

# Disable DialPlan. 0 - No Selection, 1 - Dial Page, 2 - Contact, 4 - Incoming Call History, 8 -  Outgoing Call History, 16 - MPK & Click2Dial. 
# If need to check multiple selections, add the specific values for each selections together. Default value is 0
# Number: 0-31
P52582 = 0

# Dial Plan. Default value is { x+ | \+x+ | *x+ | *xx*x+ }
P51559 = { x+ | \+x+ | *x+ | *xx*x+ }

# Account Ringtone. See ring tone options and value in the Ring Tone Value Table below.
P51523 = content://settings/system/ringtone

# Ignore Alert-Info Header. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1
P53518 = 0

# Matching Incoming Caller ID. Matching Rule 1.
# String
P53577 =

# Matching Rule 1 Distinctive Ringtone. See ring tone options and value in the Ring Tone Value Table below.
# String
P53578 = content://settings/system/ringtone

# Matching Incoming Caller ID. Matching Rule 2.
# String
P53579 =

# Matching Rule 2 Distinctive Ringtone. See ring tone options and value in the Ring Tone Value Table below.
# String
P53580 = content://settings/system/ringtone

# Matching Incoming Caller ID. Matching Rule 3.
# String
P53581 =

# Matching Rule 3 Distinctive Ringtone. See ring tone options and value in the Ring Tone Value Table below.
# String
P53582 = content://settings/system/ringtone

############Ring Tone Value Table###############
# Web GUI Option                            Value
# Use System Ring tone                      content://settings/system/ringtone 
# Andromeda					/system/media/audio/ringtones/ANDROMEDA.ogg
# Aquila					/system/media/audio/ringtones/Aquila.ogg
# Argo Navis					/system/media/audio/ringtones/ArgoNavis.ogg
# Atria					/system/media/audio/ringtones/Atria.ogg
# Backroad					/system/media/audio/ringtones/Backroad.ogg
# Beat Plucker					/system/media/audio/ringtones/BeatPlucker.ogg
# Bell Phone					/system/media/audio/ringtones/Ring_Classic_02.ogg
# Bentley Dubs					/system/media/audio/ringtones/BentleyDubs.ogg
# Big Easy					/system/media/audio/ringtones/Big_Easy.ogg
# Bird Loop					/system/media/audio/ringtones/BirdLoop.ogg
# Bollywood					/system/media/audio/ringtones/Bollywood.ogg
# Boötes					/system/media/audio/ringtones/BOOTES.ogg
# Bus' a Move					/system/media/audio/ringtones/BussaMove.ogg
# Cairo					/system/media/audio/ringtones/Cairo.ogg
# Calypso Steel					/system/media/audio/ringtones/Calypso_Steel.ogg
# Canis Major					/system/media/audio/ringtones/CANISMAJOR.ogg
# Caribbean Ice					/system/media/audio/ringtones/CaribbeanIce.ogg
# Carina					/system/media/audio/ringtones/Carina.ogg
# Cassiopeia					/system/media/audio/ringtones/CASSIOPEIA.ogg
# Centaurus					/system/media/audio/ringtones/Centaurus.ogg
# Champagne Edition					/system/media/audio/ringtones/Champagne_Edition.ogg
# Chimey Phone					/system/media/audio/ringtones/Ring_Synth_02.ogg
# Club Cubano					/system/media/audio/ringtones/Club_Cubano.ogg
# Crayon Rock					/system/media/audio/ringtones/CrayonRock.ogg
# Crazy Dream					/system/media/audio/ringtones/CrazyDream.ogg
# Curve Ball Blend					/system/media/audio/ringtones/CurveBall.ogg
# Cygnus					/system/media/audio/ringtones/Cygnus.ogg
# Dancin' Fool					/system/media/audio/ringtones/DancinFool.ogg
# Digital Phone					/system/media/audio/ringtones/Ring_Digital_02.ogg
# Ding					/system/media/audio/ringtones/Ding.ogg
# DingDong					/system/media/audio/ringtones/DingDong.wav
# Don' Mess Wiv It					/system/media/audio/ringtones/DonMessWivIt.ogg
# Draco					/system/media/audio/ringtones/Draco.ogg
# Dream Theme					/system/media/audio/ringtones/DreamTheme.ogg
# Eastern Sky					/system/media/audio/ringtones/Eastern_Sky.ogg
# Enter the Nexus					/system/media/audio/ringtones/Enter_the_Nexus.ogg
# Eridani					/system/media/audio/ringtones/Eridani.ogg
# Ether Shake					/system/media/audio/ringtones/EtherShake.ogg
# Flutey Phone					/system/media/audio/ringtones/Ring_Synth_04.ogg
# Free Flight					/system/media/audio/ringtones/FreeFlight.ogg
# Friendly Ghost					/system/media/audio/ringtones/FriendlyGhost.ogg
# Funk Y'all					/system/media/audio/ringtones/Funk_Yall.ogg
# Game Over Guitar					/system/media/audio/ringtones/GameOverGuitar.ogg
# Gimme Mo' Town					/system/media/audio/ringtones/Gimme_Mo_Town.ogg
# Girtab					/system/media/audio/ringtones/Girtab.ogg
# Glacial Groove					/system/media/audio/ringtones/Glacial_Groove.ogg
# Growl					/system/media/audio/ringtones/Growl.ogg
# Halfway Home					/system/media/audio/ringtones/HalfwayHome.ogg
# Hydra					/system/media/audio/ringtones/Hydra.ogg
# Insert Coin					/system/media/audio/ringtones/InsertCoin.ogg
# Kuma					/system/media/audio/ringtones/Kuma.ogg
# Loopy Lounge					/system/media/audio/ringtones/LoopyLounge.ogg
# Love Flute					/system/media/audio/ringtones/LoveFlute.ogg
# Lyra					/system/media/audio/ringtones/Lyra.ogg
# Machina					/system/media/audio/ringtones/Machina.ogg
# Medieval Jaunt					/system/media/audio/ringtones/MidEvilJaunt.ogg
# Mildly Alarming					/system/media/audio/ringtones/MildlyAlarming.ogg
# Nairobi					/system/media/audio/ringtones/Nairobi.ogg
# Nassau					/system/media/audio/ringtones/Nassau.ogg
# New Player					/system/media/audio/ringtones/NewPlayer.ogg
# No Limits					/system/media/audio/ringtones/No_Limits.ogg
# Noisey One					/system/media/audio/ringtones/Noises1.ogg
# Organ Dub					/system/media/audio/ringtones/OrganDub.ogg
# Orion					/system/media/audio/ringtones/Orion.ogg
# Paradise Island					/system/media/audio/ringtones/Paradise_Island.ogg
# Pegasus					/system/media/audio/ringtones/Pegasus.ogg
# Perseus					/system/media/audio/ringtones/PERSEUS.ogg
# Playa					/system/media/audio/ringtones/Playa.ogg
# Pyxis					/system/media/audio/ringtones/Pyxis.ogg
# Rasalas					/system/media/audio/ringtones/Rasalas.ogg
# Revelation					/system/media/audio/ringtones/Revelation.ogg
# Rigel					/system/media/audio/ringtones/Rigel.ogg
# Road Trip					/system/media/audio/ringtones/Road_Trip.ogg
# Romancing The Tone					/system/media/audio/ringtones/RomancingTheTone.ogg
# Safari					/system/media/audio/ringtones/Safari.ogg
# Savannah					/system/media/audio/ringtones/Savannah.ogg
# Scarabaeus					/system/media/audio/ringtones/Scarabaeus.ogg
# Sceptrum					/system/media/audio/ringtones/Sceptrum.ogg
# Seville					/system/media/audio/ringtones/Seville.ogg
# She's All That					/system/media/audio/ringtones/Shes_All_That.ogg
# Silky Way					/system/media/audio/ringtones/SilkyWay.ogg
# Sitar Versus Sitar					/system/media/audio/ringtones/SitarVsSitar.ogg
# Solarium					/system/media/audio/ringtones/Solarium.ogg
# Springy Jalopy					/system/media/audio/ringtones/SpringyJalopy.ogg
# Steppin' Out					/system/media/audio/ringtones/Steppin_Out.ogg
# Terminated					/system/media/audio/ringtones/Terminated.ogg
# Terrible Twos					/system/media/audio/ringtones/Noises2.ogg
# Testudo					/system/media/audio/ringtones/Testudo.ogg
# Themos					/system/media/audio/ringtones/Themos.ogg
# Third Eye					/system/media/audio/ringtones/Third_Eye.ogg
# Thriller Three					/system/media/audio/ringtones/Noises3.ogg
# Thunderfoot					/system/media/audio/ringtones/Thunderfoot.ogg
# Twirl Away					/system/media/audio/ringtones/TwirlAway.ogg
# Ursa Minor					/system/media/audio/ringtones/URSAMINOR.ogg
# UrsaMinor					/system/media/audio/ringtones/UrsaMinor.ogg
# Very Alarmed					/system/media/audio/ringtones/VeryAlarmed.ogg
# Vespa					/system/media/audio/ringtones/Vespa.ogg
# World					/system/media/audio/ringtones/World.ogg
# Zeta					/system/media/audio/ringtones/Zeta.ogg
# bellcore-dr1					/system/media/audio/ringtones/bellcore-dr1.ogg
# bellcore-dr2					/system/media/audio/ringtones/bellcore-dr2.ogg
# bellcore-dr3					/system/media/audio/ringtones/bellcore-dr3.ogg
# bellcore-dr4					/system/media/audio/ringtones/bellcore-dr4.ogg
# bellcore-dr5					/system/media/audio/ringtones/bellcore-dr5.ogg
# speaker					/system/media/audio/ringtones/speaker.wav

#######################################################################
##  Account 16 Advanced Settings                                      ##
#######################################################################
# Check Domain Certificates. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1 
P52511 = 0

# Validate Certificate Chain. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1 
P52567 = 0

# Validate Incoming SIP Messages. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1 
P52506 = 0

# Allow Unsolicited REFER. 0 - Disabled, 1 - Enabled, 2 - Enabled/Force Auth. Default value is 0
# Number: 0, 1, 2
P53523 = 0

# Only Accept SIP Requests from Known Servers. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1 
P52547 = 0

# Check SIP User ID for Incoming INVITE. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1 
P51549 = 0

# Allow SIP Reset. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1 
P53515 = 0

# Authenticate Incoming INVITE. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1 
P52546 = 0

# SIP Realm Used for Challenge INVITE & NOTIFY.
# String
P53521 =

# Enable Local MOH
# Number: 0, 1 
P52557 = 0

# Virtual Account Group. -1 - Default,  0 - Virtual Account Group 1, 1 - Virtual Account Group 2, 2 - Virtual Account Group 3
# 3 - Virtual Account Group 4, 4 - Virtual Account Group 5, 5 - Virtual Account Group 6, 6 - Virtual Account Group 7, 7 - Virtual Account Group 8
# 8 - Virtual Account Group 9, 9 - Virtual Account Group 10, 10 - Virtual Account Group 11, 11 - Virtual Account Group 12, 12 - Virtual Account Group 13
# 13 - Virtual Account Group 14, 14 - Virtual Account Group 15, 15 - Virtual Account Group 16. Default value is -1.
# Number: -1 - 15 
P52591 = -1

# Special Feature. Default value is 100
# 100 - Standard, 102 - Broadsoft, 113 - China Mobile, 114 - ZTE IMS, 115 - Mobotix
# 116 - ZTE NGN, 117 - Huawei IMS, 123 - NEC, 125 - WorldStone, 129 - Telefonica Spain
# Number: 100, 102, 113, 114, 115, 116, 117, 123, 125, 129
P51524 = 100

# Feature Key Synchronization.  0 - Disable, 0 - Broadsoft/Metaswitch. Default Value is 0.
# Number: 0, 1
# P52525 = 0

# Allow Sync Phonebook via SIP Notify. 0 - No, 1 - Yes. Default is 1
# Number: 0, 1
P53599 = 1

##############################################################################
##  Calls                                                                   ##
##############################################################################
#######################################################################
##  Contacts -> Download Contacts                                    ##
#######################################################################
# Clear The Old List/Clear Old History Mode. 0 - No, 1 - Clear all, 2 - Keep Local Contacts. Default value is 0
# Number: 0, 1, 2
P1435 = 0

# Replace Duplicate Items/Replace Duplicate Entries Mode. Default value is 0
# Number: 0, 1
P1436 = 0

# Download Mode. 0 - OFF, 1 - TFTP, 2 - HTTP, 3 - HTTPS. Default value is 0
# Number: 0, 1, 2, 3
P330 = 0

# File Encoding. GBK - GBK, UTF-8 - UTF-8, UTF-16 - UTF-16, UTF-32 - UTF-32, Big5 - Big5, Big5-HKSCS - Big5-HKSCS, Shift-JIS - Shift-JIS
# ISO 2022-JP - ISO 2022-JP, KOI8-R - KOI8-R, ISO8859-1 - ISO8859-1, ISO8859-15 - ISO8859-15, Windows-1251 - Windows-1251, EUC-KR - EUC-KR
# Default Value is UTF-8
# String : GBK, UTF-8, UTF-16, UTF-32, Big5, Big5-HKSCS,  Shift-JIS, ISO 2022-JP, KOI8-R, ISO8859-1, ISO8859-15, Windows-1251, EUC-KR 
P1681 = UTF-8

# Download Server. It MUST be in the host/path format
# For example: directory.grandstream.com/engineering
# String
P331 = 

# HTTP/HTTPS User Name
P6713 =

# HTTP/HTTPS Password
P6714 = 

# Download Interval (m). Default value is 0 for disabled
# Number: 0, 120, 240, 360, 480, 720
P332 = 0

#######################################################################
##  Contacts -> Blacklist/Whitelist Settings -> Blocking Rules       ##
#######################################################################
# Whitelist
# Format is numbers, name. Example: 123, John Doe.
P22313 = 

# Blacklist
# Format is numbers, name. Example: 123, John Doe.
P28127 =

# Greylist. 0 - Block,  1 - Set Password, 2 - Auto answer, 3 - Ringing. Default value is 0.
# Number: 0, 1, 2, 3
P22209 = 0

##############################################################################
##  Phone Settings                                                          ##
##############################################################################
#######################################################################
##  Phone Settings -> General Settings                               ##
#######################################################################
# Local RTP Port. Default value is 50040
# Number: 1024 - 65535
P39 = 50040

# Use Random Port. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P78 = 0

# Keep-alive Interval (s). Default value is 20 seconds
# Number: 10 - 160
P84 = 20

# STUN Server
P76 = stun.ipvideotalk.com

# TURN Server Username
P22042 = 

# TURN Server Password
P22043 = 

# Use NAT IP. This will enable our SIP client to use this IP in the SIP message.
# Example 64.3.153.50
P101 =

#######################################################################
##  Phone Settings - Call Settings                                   ##
#######################################################################
# Enable Call-Waiting. 0 - Yes, 1 - No. Default value is 0
# Number: 0, 1
P91 = 0

# Enable Call-Waiting Tone. 0 - Yes, 1 - No. Default value is 0
# Number: 0, 1
P186 = 0

# Automatic answer ringing time (s). Default value is 5 seconds.
# Number: 0 - 60
P8486 = 5

# Virtual Account Group Avaya Mode. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P22018 = 0

# Record Mode. 0 - Locally, 1 - on PortaOne, 2 - on UCM. Default value is 0.
# Number: 0, 1, 2
P6760 = 0

# Environment. 0 - Small and medium size room & used on desk,  1 - Large room & used on empty area. Default value is 1. 
# Number: 0, 1
P22093 = 1

#######################################################################
##  Phone Settings - Ring Tone                                       ##
#######################################################################
# Auto Config CPT by Region. 0 - No, 1 - Yes. Default value is 1
# Number : 0, 1
P22041 = 0

# Call-Waiting Tone
P4005 = f1=440@-13,c=300/10000-300/10000-0/0;

# Call-Waiting Tone Gain. 0 - Low, 1 - Medium, 2 - High. Default value is 0
P1555 = 0

#######################################################################
##  Phone Settings - Multicast Paging                    	         ##
#######################################################################

# Paging Barge. 0 - Disable, 1 - 1, 2 - 2, 3 - 3, 4 - 4, 5 - 5, 6 - 6, 7 - 7, 8 - 8, 9 - 9, 10 - 10. Default Value is 0
# Number : 0 - 10
P1566 = 0

# Paging Priority Active. 0 - No, 1 - Yes. Default Value is 0
# Number : 0, 1
P1567 = 0

# Multicast Paging Codec. 0 - PCMU, 2 - G726-32, 8 - PCMA, 9 - G722, 18 - G729A/B. Default value is 0
# Number : 0, 2, 8, 9, 18
P1568 = 0

##############################################################################
##  Multicast Paging - Multicast Listening                                  ##
##############################################################################

# Priority 1
# Listening Address and Port
# String
P1569 = 

# Label
# String
P1570 = 

# Priority 2
# Listening Address and Port
# String
P1571 = 

# Label
# String
P1572 = 

# Priority 3
# Listening Address and Port
# String
P1573 = 

# Label
# String
P1574 = 

# Priority 4
# Listening Address and Port
# String
P1575 = 

# Label
# String
P1576 = 

# Priority 5
# Listening Address and Port
# String
P1577 = 

# Label
# String
P1578 = 

# Priority 6
# Listening Address and Port
# String
P1579 = 

# Label
# String
P1580 = 

# Priority 7
# Listening Address and Port
# String
P1581 = 

# Label
# String
P1582 = 

# Priority 8
# LListening Address and Port
# String
P1583 = 

# Label
# String
P1584 = 

# Priority 9
# Listening Address and Port
# String
P1585 = 

# Label
# String
P1586 = 

# Priority 10
# Listening Address and Port
# String
P1587 = 

# Label
# String
P1588 = 

##############################################################################
##  Network Settings                                                        ##
##############################################################################
#######################################################################
##  Network Settings - Ethernet                                      ##
#######################################################################
# Preferred Internet Protocol. 0 - Both, prefer IPv4, 1 - Both, prefer IPv6, 2 - IPv4 Only, 3 - IPv6 Only. Default value is 0.
# Number: 0, 1
# P1415 = 2

# Different Networks for Data and VoIP Calls. 0 - No, 1 - Yes. Default value is 0.
# Number: 0,1
# P22104 = 0

#######################################################################
##  IPv4 Network Configuration of Data                               ##
#######################################################################
# Address Type. 0 - DHCP, 1 - Static, 2 - PPPoE. Default value is 0
# Number: 0, 1, 2
# P8 = 0

# DHCP VLAN Override. 0 - Disable, 1 - DHCP Option 132 and DHCP Option 133, 2 - Encapsulated in DHCP Option 43. Default value is 0.
# Number: 0, 1, 2
# P8300 = 0

# Host name (DHCP option 12)
# P146 =

# Vendor Class ID (DHCP option 60)
# P148 = Grandstream GSC3510

# Layer 2 QoS. 802.1Q/VLAN Tag(Ethernet). Default value is 0
# Number: 0 - 4095
# P51 = 0

# Layer 2 QoS. 802.1p priority value(Ethernet). Default value is 0
# Number: 0 - 7
# P87 = 0

# Static IP. IP address
# P9 = 192
# P10 = 168
# P11 = 0
# P12 = 160

# Static IP. Subnet Mask
# P13 = 255
# P14 = 255
# P15 = 255
# P16 = 0

# Static IP. Default Gateway
# P17 = 192
# P18 = 168
# P19 = 0
# P20 = 1

# Static IP. DNS Server 1. Ignore if DHCP or PPPoE is used
# P21 = 0
# P22 = 0
# P23 = 0
# P24 = 0

# Static IP. DNS Server 2. Ignore if DHCP or PPPoE is used
# P25 = 0
# P26 = 0
# P27 = 0
# P28 = 0

# PPPoE Account ID
# P82 =

# PPPoE Password
# P83 =

#######################################################################
##  IPv6 Network Configuration of Data                               ##
#######################################################################
# IPv6 Address. 0 - Auto-configured, 1 - Statically configured. Default value is 0.
# Number: 0, 1
# P1419 = 0

# Static IPv6 Address.
# P1420 =

# IPv6 Prefix Length. Default value is 64
# P1421 = 64

# IPv6 DNS Server 1.
# P1424 =

# IPv6 DNS Server 2.
# P1425 =

# IPv6 Preferred DNS Server.
# P1423 =

#######################################################################
##  802.1X Mode                                                      ##
#######################################################################

# 802.1x Mode. 0 - Disable, 1 - EAP-MD5, 2 - EAP-TLS, 3-EAP-PEAP
# Number: 0, 1, 2, 3
# P7901 = 0

# 802.1x Identity
# P7902 =

# 802.1 Secret & Password
# P7903 =

#######################################################################
##  Network Settings - Bluetooth      								 ##
#######################################################################
# Enabling Bluetooth. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1
# P2910 = 0

# Bluetooth  visibility. 0 - Disable, 1 - Enable. Default value is 0.
# Number: 0, 1
# P22330 = 0

# Bluetooth visibility timeout. 0 - Never, 2 - 2mins, 5 - 5mins, 60 - 1hr. Default value is 2.
# Number: 0, 2, 5, 60
# P22331 = 5

# Bluetooth Pair Pin Code
# Number
#P22291 = 

#######################################################################
##  Network Settings - Wi-Fi Setting -> Add Network                  ##
#######################################################################
# Wi-Fi Function. 0- Disable, 1- Enable
# P7800 = 0

# ESSID 
# P7812 = 

# Security Mode for Hidden SSID. 0 - None, 1 - WEP, 2 - WPA WPA2 PSK, 3 - 802.1X EAP. Default value is 0.
# Number: 0, 1, 2, 3
# P7814 = 0

# Password
# P7830 = 

# Layer 2 QoS 802.1p Priority Value (Wi-Fi). The default value is 0
# P22048 = 0

#######################################################################
##  Network Settings - OpenVPN Settings                              ##
#######################################################################
# Enable OpenVPN. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
# P7050 = 0

# Enable OpenVPN Comp-Izo. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
# P8508 = 0

# OpenVPN Server Address.
# Strings
# P7051 = 

# OpenVPN Port. The default value is 1194.
# P7052 = 1194

# OpenVPN Transport. 0 - UDP, 1 - TCP. Default value is 0
# Number: 0, 1
# P2912 = 0

# OpenVPN CA.
# Strings
# P9902 = 

# OpenVPN Client Certificate.
# Strings
# P9903 =

# OpenVPN Client Key.
# Strings
# P9904 =

# OpenVPN Cipher Method. 0 - Blowfish, 1 - AES - 128, 2 - AES - 256, 3 - Triple - DES. Default value is 0.
# Number: 0, 1, 2, 3
# P8396 = 0

# OpenVPN Username.
# P8394 = 

# OpenVPN Password.
# P8395 = 

#######################################################################
##  Network Settings - Advanced Network Settings                     ##
#######################################################################
# Alternate DNS Server
# P92 = 0
# P93 = 0
# P94 = 0
# P95 = 0

# Second Alternate DNS Server
# P5026 = 
# P5027 = 
# P5028 = 
# P5029 = 

# Enable LLDP. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
# P1684 = 1

# LLDP TX Interval(s).
# P22122 = 30

# Enable CDP. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
# P22119 = 1

# Layer 3 QoS for SIP. Default value is 48
# P1558 = 26

# Layer 3 QoS for Audio. Default value is 48
# P1559 = 46

# HTTP/HTTPS User-Agent
# P1541 = 

# SIP User-Agent
# P26027 = Grandstream GSC3505 $version

# HTTP/HTTPS Proxy Hostname
# String
# P1552 =

# HTTP/HTTPS Proxy Port
# String
# P1552 =

# Bypass Proxy For
# String
# P22011 =

##############################################################################
##  System Settings                                                        ##
##############################################################################
#######################################################################
##  System Settings - Time Settings                                  ##
#######################################################################
# Assign NTP Server Address
# String
P30 = pool.ntp.org 

# DHCP Option 42 Override NTP Server. 0 - No, 1 - Yes. Default value is 0
# When set to Yes(1), it will override the configured NTP server
# Number: 0, 1
# Mandatory
P144 = 1

# DHCP Option 2 to Override Time Zone Settings. 0 - No, 1 - Yes. Default value is 0
# When set to Yes(1), it will override the configured Time Zone setting if available
# Number: 0, 1
# Mandatory
P143 = 1

# Time Zone
# Web GUI Option       			   							    P Value            							
# GMT-11:00(Midway Island)             							TZB+11
# GMT-10:00(Hawaii)                    							HAW10
# GMT-9:00(Alaska)                     							AKST9AKDT
# GMT-8:00(Pacific Time)               							PST8PDT
# GMT-8:00(Tijuana)                    							PST8PDT,M4.1.0,M10.5.0
# GMT-7:00(Arizona)												MST7
# GMT-7:00(Chihuahua)                  							MST7MDT,M4.1.0,M10.5.0
# GMT-7:00(Mountain Time)										MST7MDT
# GMT-6:00(Central America)            							CST+6
# GMT-6:00(Central Time)               							CST6CDT     
# GMT-6:00(Mexico City)              							CST6CDT,M4.1.0,M10.5.0
# GMT-6:00(Saskatchewan)										CST6CDT,M3.2.0,M11.1.0	
# GMT-5:00(Bogota)												COT5
# GMT-5:00(Eastern Time)                                        EST5EDT
# GMT-4:00(Venezuela)											TZf+4:30
# GMT-4:00(Atlantic Time (Barbados))                           	AST4
# GMT-4:00(Atlantic Time (Canada))                           	AST4ADT
# GMT-4:00(Manaus)												AMT4
# GMT-3:30(Newfoundland)                            			NST+3:30NDT+2:30,M4.1.0/00:01:00,M10.5.0/00:01:00
# *GMT-4:00(Santiago
# GMT-3:00(Recife)  
# GMT-3:00(Buenos Aires)										UTC+3
# GMT-3:00(Greenland)                               			TZK+3
# GMT-3:00(Montevideo)											UYT3UYST,M10.1.0,M3.2.0
# GMT-3:00(São Paulo)                                			UTC-3
# GMT-2:00(Mid-Atlantic)                            			TZL+2
# GMT-1:00(Azores)                                  			TZM+1
# GMT-1:00(Cape Verde Islands)									CVT1
# GMT+0:00(GMT)
# GMT+0:00(Casablanca)                              			TZN+0
# GMT+0:00(London)                                  			GMT+0BST-1,M3.5.0/01:00:00,M10.5.0/02:00:00
# GMT+1:00(Amsterdam)											CET-1CEST-2,M3.5.0/02:00:00,M10.5.0/03:00:00
# GMT+1:00(Belgrade)											CET-1CEST,M3.5.0,M10.5.0/3
# GMT+1:00(Brussels)											TZO-1
# GMT+1:00(Madrid)												CET-1CEST-2,M3.5.0/02:00:00,M10.5.0/03:00:00
# GMT+1:00(Sarajevo)											CET-1CEST,M3.5.0,M10.5.0/3
# *GMT+1:00(W. Africa Time)										WAT-1
# GMT+2:00(Windhoek)											WAT-1WAST,M9.1.0,M4.1.0
# *GMT+2:00(Amman, Jordan)
# GMT+2:00(Helsinki, Athens, Tallinn, Eastern European Time)	EET-2EEST-3,M3.5.0/03:00:00,M10.5.0/04:00:00
# GMT+3:00(Istanbul)											TZQ-3
# GMT+2:00(Beirut, Lebanon)										EET-2EEST,M3.5.0/0,M10.5.0/0
# GMT+2:00(Cairo)												TZP-2
# GMT+2:00(Jerusalem)											TZP-2
# GMT+2:00(Harare)												CAT-2
# GMT+3:00(Minsk)												EET-2EEST,M3.5.0,M10.5.0/3
# GMT+3:00(Baghdad)												AST-3
# GMT+3:00(Moscow)												MST-3MDT,M3.5.0/2,M10.5.0/3
# GMT+3:00(Kuwait)												TZQ-3
# GMT+3:00(Nairobi)												TZQ-3
# GMT+3:30(Tehran)												TZQ-3
# GMT+4:00(Baku)												TZR-4
# GMT+4:00(Tbilisi)												GET-4
# GMT+4:00(Yerevan)												AMT-4AMST,M3.5.0,M10.5.0/3
# GMT+4:00(Dubai)												GST-4
# GMT+4:30(Kabul)												AFT-4:30
# GMT+5:00(Islamabad, Karachi)									TZS-5
# GMT+5:00(Ural'sk)												ORAT-5
# GMT+5:00(Yekaterinburg)										YEKT-5YEKST,M3.5.0,M10.5.0/3
# GMT+5:30(Kolkata)												IST-5:30
# *GMT+5:30(Sri Lanka)
# GMT+5:45(Kathmandu)											TZU-5:45
# GMT+6:00(Astana)												TZV-6
# GMT+6:30(Yangon)												TZW-6:30
# GMT+7:00(Krasnoyarsk)											TZX-7
# GMT+7:00(Bangkok)												TZX-7
# GMT+7:00(Jakarta)												WIB-7
# GMT+8:00(Beijing)												TZY-8
# GMT+8:00(Hong Kong)											TZY-8
# GMT+8:00(Irkutsk)												TZY-8
# GMT+8:00(Kuala Lumpur)										MYT-8
# GMT+8:00(Perth)												WST-8
# GMT+8:00(Taipei)                                				TZY-8
# GMT+9:00(Seoul)												TZZ-9
# GMT+9:00(Tokyo, Osaka)										TZZ-9
# GMT+9:00(Yakutsk)												TZZ-9
# GMT+9:30(Darwin)												CST-9:30
# GMT+10:00(Brisbane)											EST-10
# GMT+10:00(Vladivostok)										VLAT-10VLAST,M3.5.0,M10.5.0/3
# GMT+10:00(Guam)												TZb-10
# GMT+9:30(Adelaide)											CST-9:30CDT-10:30,M10.5.0/02:00:00,M3.5.0/03:00:00
# GMT+10:00(Hobart)												EST-10EDT-11,M10.1.0/02:00:00,M3.5.0/03:00:00
# GMT+10:00(Sydney, Canberra)									EST-10EDT-11,M10.5.0/02:00:00,M3.5.0/03:00:00
# GMT+11:00(Magadan)											TZc-11
# GMT+11:00(Noumea, New Caledonia)								TZc-11
# GMT+12:00(Majuro, Marshall Islands)                           MHT-12
# GMT+12:00(Auckland)											NZST-12NZDT-13,M10.1.0/02:00:00,M3.3.0/03:00:00
# GMT+12:00(Fiji)												TZd-12
# GMT+13:00(Tonga)                                              TZe-13
# Time zone with * are TBA

# Time Zone
P64 = EST5EDT

# Time Display Format. 0 - 12 Hour, 1 - 24 Hour. Default value is 1
# Number: 0, 1
# Mandatory
P122 = 1

# Date Display Format. 0 - Normal(YYYY/M/D), 1 - MM/DD/YYYY, 2 - DD/MM/YYYY, 3 - YYYY/MM/DD.  Default value is 1.
# Number: 0, 1, 2, 3
# Mandatory
P102 = 1

#######################################################################
##  System Settings - Security Settings - Web/SSH Access             ##
#######################################################################
# Enable SSH. 0 - Yes, 1 - No. Default value is 0
# Number: 0, 1
P276 = 0

# Allow Web Page Access. 0 - Yes, 1 - No. Default value is 0.
# Number: 0, 1
P29605 = 0

# SSH Port. Default value is 22
# Number
P27006 = 22

# Acccess Method. 0 - HTTP, 1 - HTTPS. Default value is 0
# Number: 0, 1
P900 = 0

# Port. Default value is 80
# Number
P901 = 80

#######################################################################
##  System Settings - Security Settings - User Info Management       ##
#######################################################################
# Admin password for web interface
P2 = admin

# End User Password
P196 = user

#######################################################################
##  System Settings - Security Settings - SIP TLS                    ##
#######################################################################
# Minimum TLS Version. 10 - 1.0, 11 - 1.1, 12 - 1.2. Default value is 11
# Number: 10, 11, 12
P22293: 11

# Maximum TLS Version. 10 - 1.0, 11 - 1.1, 12 - 1.2, 99 - No Limit. Default value is 99
# Number: 10, 11, 12 , 99
P22294: 99

# SIP TLS Certificate
# String: a-z, A-Z, 0-9
P280 =

# SIP TLS Private Key
# String: a-z, A-Z, 0-9
P279 = 

# SIP TLS Private Key Password
# String: a-z, A-Z, 0-9
P281 = s1pphone

#######################################################################
##  System Settings - Preferences - LCD&LED Management               ##
#######################################################################
# Enable Missed Call Indicator. 0 - Yes, 1 - No. Default value is 0
# Number: 0, 1
P1691 = 0

#######################################################################
##  System Settings - Preferences - Volume Settings                  ##
#######################################################################
# Call Volume. Default Value is 8.
# Number: 0 - 8
P22317 = 8

# Ringtone Volume. Default Value is 8.
# Number: 0 - 15
P8352 = 8

# Media Volum. Default Value is 12.
# Number: 0 - 15
P43025 = 12

#######################################################################
##  System Settings - TR069                                          ##
#######################################################################
# Enable TR-069. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
# Mandatory
# Reboot
P1409 = 0

# ACS URL
# String 
P4503 =

# ACS Username
# String 
P4504 = 

# ACS Password
# String 
P4505 = 

# Periodic Inform Enable. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P4506 = 0

# Periodic Inform Interval (s). Default value is 86400
# Number: 1 - 4294967295
P4507 = 86400

# Connection Request Username
# String: a-z, A-Z, 0-9
P4511 = 

# Connection Request Password
# String: a-z, A-Z, 0-9
P4512 = 

# Connection Request Port
# Number
P4518 =

# CPE Cert File
# String
P8220 =

# CPE Cert Key
# String
P8221 =

#######################################################################
##  System Settings - Sensor setting                                 ##
#######################################################################
# Sensor type. 0 - Normally Close, 1 - Normally Open. Default value is 0
# Number: 0, 1
P22210 = 0
 
# Trigger type. 0 - Level Triggered, 1 - Edge Triggered. Default value is 0
# Number: 0, 1
P22211 = 0

# Cycle Time.  - All Days, - Period of Time
# Schedule 1 - 7
# Number 
P22215 = 
P22216 = 
P22217 = 
P22218 =
P22219 = 
P22220 = 
P22221 = 

# Play audio. 0 - Disable, 1 - Enable. Default value is 0
# Number: 0, 1
P22212 = 0

# Make call/Dial out extension. 0 - Disable, 1 - Enable. Default value is 1
# Number: 0, 1
P22213 = 0

# Recording. 0 - Disable, 1 - Enable. Default value is 0
# Nubmer: 0, 1
P22214 = 0

##############################################################################
##  Maintenance                                                             ##
##############################################################################
#######################################################################
##  Maintenance - Upgrade - Firmware                                 ##
#######################################################################
# Complete Upgrade. 0 - No, 1 - Yes. Default is 0.
#P-upgradeall = 0

# Firmware Upgrade Mode. 0 - TFTP, 1 - HTTP, 2 - HTTPS, 3 - Manual Upload. Default value is 1.
# Number: 0, 1, 2, 3
P6767 = 1

# Firmware Server Path
P192 = fm.ipvideotalk.com/gs

# Firmware HTTP/HTTPS User Name
P6768 = 

# Firmware HTTP/HTTPS Password
P6769 =

# Firmware File Prefix
P232 =

# Firmware File Postfix
P233 =

#######################################################################
##  Maintenance - Upgrade - Config File                              ##
#######################################################################
# Config Update Via. 0 - TFTP, 1 - HTTP, 2 - HTTPS. Default value is 2.
# Number: 0, 1, 2
P212 = 2

# Config Server Path
P237 = fm.grandstream.com/gs

# Config HTTP/HTTPS User Name
P1360 = 

# Config HTTP/HTTPS Password
P1361 =

# Always send HTTP Basic Authentication Information. 0 - No, 1 - Yes.
# Number: 0, 1
P20713 = 0

# Config File Prefix
P234 =

# Config File Postfix
P235 =

# Authenticate Conf File. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P240 = 0

# XML Config File Password
P1359 =

#######################################################################
##  Maintenance - Upgrade - Provision                                ##
#######################################################################
# Automatic Upgrade. 0 - No, 1 - Check Every Day, 2 - Check Every Week, 3 - Check at a Period Time. Default value is 0
# Number: 0, 1, 2, 3
P194 = 0

# Automatic Upgrade Check Interval (m). Minimum 60 minutes. Default value is 10080 (7 days)
# Number: 60 - 5256000
P193 = 10080

# Enable Randomized Automatic Upgrade. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P8458 = 0

# Starting/Ending Hour of the Day(0-23)
# Number: 0 - 23
P285 = 1
P8459 = 

# Day of the Week (0-6)
# Number: 0 - 6
P286 = 1

# Firmware Upgrade and Provisioning. Default value is 0
# 0 - Always Check at Bootup
# 1 - When F/W pre/suffix changes
# 2 - Skip the Firmware Check
# Number: 0, 1, 2
P238 = 0

# Allow DHCP Option 43 and Option 66 to Override server. 0 - No, 1 - Yes. Default value is 1
# When set to Yes(1), it will override the configured provision path and method
# Number: 0, 1
P145 = 1

# DHCP Option 120 Override SIP Server.  0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P1411 = 1

# Allow DHCP Option 242 (Avaya IP Phones). 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P22053 = 1

# Download and Process All Available Config Files. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P8467 = 0

# PnP (3CX) Auto Provision. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P1414 = 1

#######################################################################
##  Maintenance - Upgrade - Advanced Settings                        ##
#######################################################################
# Enable SIP NOTIFY Authentication. 0 - No, 1 - Yes. Default Value is 0.
# Number : 0, 1
P4428 = 1

# Validate Certification Chain. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1
P22030 = 0

# Allow AutoConfig Service Access. 0 - No, 1 - Yes. Default value is 1.
# Number: 0, 1
P7070 = 1

# mDNS Override Server. 0 - Disable, 1 - Use Type A, 2 - Use Type SRV. Default value is 1.
# Number: 0, 1
P1407 = 1

#######################################################################
##  Maintenance - System Diagnosis - Syslog                          ##
#######################################################################
# Syslog Protocol
# 0 - UDP, 1 - SSL/TLS. Default Value is 0.
P8402 = 0

# Syslog Server. Name of the server.
P207 = log.ipvideotalk.com

# Syslog Level
# 0 - NONE, 1 - DEBUG, 2 - INFO, 3 - WARNING, 4 - ERROR. Default value is 0.
# Number: 0, 1, 2, 3, 4
P208 = 0

# Send SIP Log. 0 - Disable, 1 - Enable. Default value is 1.
# Number: 0, 1
P1387 = 1

# Syslog Keyword Filter
# String
P22129 = 

####################################################################
#  Maintenance - System Diagnosis - Logcat                        ##
####################################################################
# Log Tag (Not stored in pvalue)

# Log Priority (Not stored in pvalue)

####################################################################
#  Maintenance - System Diagnosis - Debug                         ##
####################################################################
# Debug Info List (Not stored in pvalue)

# Enable Core Dump Generation. 0 - Disabled, 1 - Enabled.
# Number: 0, 1. Default is 0
P29611 = 0

# Core Dump List (Not stored in pvalue)

# Recording List (Not stored in pvalue)

# Screenshot List (Not stored in pvalue)

####################################################################
#  Maintenance - System Diagnosis - Traceroute                    ##
####################################################################
# Target Host (Not stored in pvalue)

####################################################################
#  Maintenance - System Diagnosis - Ping                          #2#
####################################################################
# Target Host (Not stored in pvalue)

####################################################################
#  Maintenance - System Diagnosis - NSLookup                      ##
####################################################################
# Host Name (Not stored in pvalue)

##############################################################################
##  Applications                                                            ##
##############################################################################
#######################################################################
##  Applications - Music                                             ##
#######################################################################
# Audio File Address.
# String
# Format:  rtsp//IPADDRESS/MUSICFILE.MUSICEXTENSION
# Example: rtsp://192.168.160.124/SummerVibe-WalkOffTheEarth.ts or rtsp://192.168.160.124/LadyAntebellumNeedYouNow.mp3
P953 = 

# Play Mode. 0 - Manual, 1 - Auto. Default value is 0.
# Number: 0, 1
P22328: 0

# Schedule 1.
# String
# Format: FREQ=WEEKLY;byday=(MO,TU,WE,TH,FR,SA,SU);ByPeriod=(0000-2359);Action={voice=(RTSP file)
# Example: FREQ=WEEKLY;byday=TU,TH,SA;ByPeriod=0730-0735,1245-1300;Action={voice=rtsp://192.168.160.124/LadyAntebellumNeedYouNow.mp3
P22336

# Schedule 2.
# String
# Format: FREQ=WEEKLY;byday=(MO,TU,WE,TH,FR,SA,SU);ByPeriod=(0000-2359);Action={voice=(RTSP file)
# Example: FREQ=WEEKLY;byday=TU,TH,SA;ByPeriod=0730-0735,1245-1300;Action={voice=rtsp://192.168.160.124/LadyAntebellumNeedYouNow.mp3
P22337

# Schedule 3.
# String
# Format: FREQ=WEEKLY;byday=(MO,TU,WE,TH,FR,SA,SU);ByPeriod=(0000-2359);Action={voice=(RTSP file)
# Example: FREQ=WEEKLY;byday=TU,TH,SA;ByPeriod=0730-0735,1245-1300;Action={voice=rtsp://192.168.160.124/LadyAntebellumNeedYouNow.mp3
P22338

# Schedule 4.
# String
# Format: FREQ=WEEKLY;byday=(MO,TU,WE,TH,FR,SA,SU);ByPeriod=(0000-2359);Action={voice=(RTSP file)
# Example: FREQ=WEEKLY;byday=TU,TH,SA;ByPeriod=0730-0735,1245-1300;Action={voice=rtsp://192.168.160.124/LadyAntebellumNeedYouNow.mp3
P22339

# Schedule 5.
# String
# Format: FREQ=WEEKLY;byday=(MO,TU,WE,TH,FR,SA,SU);ByPeriod=(0000-2359);Action={voice=(RTSP file)
# Example: FREQ=WEEKLY;byday=TU,TH,SA;ByPeriod=0730-0735,1245-1300;Action={voice=rtsp://192.168.160.124/LadyAntebellumNeedYouNow.mp3
P22340

# Schedule 6.
# String
# Format: FREQ=WEEKLY;byday=(MO,TU,WE,TH,FR,SA,SU);ByPeriod=(0000-2359);Action={voice=(RTSP file)
# Example: FREQ=WEEKLY;byday=TU,TH,SA;ByPeriod=0730-0735,1245-1300;Action={voice=rtsp://192.168.160.124/LadyAntebellumNeedYouNow.mp3
P22341

# Schedule 7.
# String
# Format: FREQ=WEEKLY;byday=(MO,TU,WE,TH,FR,SA,SU);ByPeriod=(0000-2359);Action={voice=(RTSP file)
# Example: FREQ=WEEKLY;byday=TU,TH,SA;ByPeriod=0730-0735,1245-1300;Action={voice=rtsp://192.168.160.124/LadyAntebellumNeedYouNow.mp3
P22342

###############################################################################################
####                                                                                       ####  
####                          End of Configuration Template                                ####
####                                                                                       ####
###############################################################################################