##############################################################################################
####            Configuration Template for GXV3370 Firmware Version 1.0.3.19             ####
##############################################################################################

##############################################################################
##  Account 1 Settings                                                      ##
##############################################################################

#######################################################################
##  Account 1 General Settings                                       ##
#######################################################################
# Account Active. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P271=1

# Account Name
P270=

# SIP Server
P47=

# SIP User ID
P35=
 
# SIP Authentication ID
P36=

# SIP Authentication Password
P34=

# Voice Mail Access Number
P33=

# Name (Display Name, e.g., John Doe)
P3=

# Tel URI. 0 - Disable, 1 - User=Phone, 2 - Enabled. Default value is 0
# Number: 0, 1, 2
P63=0
#######################################################################
##  Account 1 Network Settings                                       ##
#######################################################################
# Outbound Proxy
P48=

# Secondary Outbound Proxy
P2333=

# DNS Mode. 0 - A Record, 1 - SRV, 2 - NAPTR/SRV. Default value is 0
# Number: 0, 1, 2
P103=0

# DNS SRV Fail-over Mode. 0 - Default, 1 - Saved one until DNS TTL, 2 - Saved one until no response. Defualt value is 1
# Number
P26040=0

# Register Before DNS SRV Fail-over. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P29095=0

# NAT Traversal. 0 - NAT No, 1 - STUN, 2 - Keep-alive, 3 - UPnP, 4 - Auto, 5 - VPN. Default value is 2
# Number: 0, 1, 2, 3, 4, 5
P52=2

# Proxy-Require
P197=
#######################################################################
##  Account 1 SIP Settings                                           ##
#######################################################################
# SIP Registration. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P31=1

# Unregister Before New Registration. 0 - No, 1 - All, 2 -  Instance . Default value is 2
# Number: 0, 1, 2
P81=2

# Register Expiration (m). In minutes. Default value is 60
# Number: 0 - 64800
P32=60

# Subscribe Expiration (m). Default is 60
# Number: 0 - 64800
P26051=60

# Re-register before Expiration (s). Default Value is 0
# Number : 0
P2330=0

# Registration Retry Wait Time (s). In seconds. Default value is 20
# Number: 1 - 3600
P138=20

# Local SIP Port. Default value is 5060
# Number: 5 - 65535
P40=5060

# SUBSCRIBE For MWI. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P99=0

# Add Auth Header On RE-REGISTER
# 0 - No, 1- Yes
P2359=1

# Enable SIP OPTIONS Keep Alive. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P2397=0

# SIP OPTIONS Keep Alive Interval(s). Default value is 30
# Number 
P2398=30

# SIP OPTIONS Keep Alive Maximum Tries. Default value is 3
# Number 
P2399=3

# Enable Session Timer/ Session Expiration(s).  In seconds. Default value is 180 seconds.
# By default,  Session Timer is Enabled.  Session Timer is disabled if the value is 0.
# Number: 0 or 90 - 64800
P260=180

# Min-SE(s). Default value is 90 seconds
# Number: 90 - 64800
P261=90

# UAC Specify Refresher. 0 - Omit, 1 - UAC, 2 - UAS. Default value is 0
# Number: 0, 1, 2
P266=0

# UAS Specify Refresher. 1 - UAC, 2 - UAS. Default value is 1
# Number: 1, 2
P267=1


# Caller Request Timer. Request for timer when calling
# 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P262=0

# Callee Request Timer
# Request for timer when being called (i.e., if remote party supports timer but did not request for one)
# 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P263=0

# Force Timer. Still use timer when remote party does not support timer
# 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P264=0

# Force INVITE. Always refresh with INVITE instead of UPDATE even when remote party supports UPDATE
# 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P265=0

# Enable 100rel. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P272=0

# Use Privacy Header
# 0 - Default, 1 - No, 2 - Yes. Default is 0
# Number: 0, 1, 2
P2338=0

# Use P-Preferred-Identity Header
# 0 - Default, 1 - No, 2 - Yes. Default is 0
# Number: 0, 1, 2
P2339=0

# Use P-Access-Network-Info Header. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P26058=1

# Use P-Emergency-Info Header. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P26059=1

# Use MAC Header.  0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P26061=0

# SIP Transport
# 0 - UDP , 1 - TCP, 2 - TLS. Default value is 0
# Number: 0, 1, 2
P130=0

# SIP URI Scheme When Using TLS
# 0 -sip, 1 - sips. Default value is 0.
# Number: 0, 1
P2329=0

# Use Actual Ephemeral Port in Contact with TCP/TLS
# 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P2331=0

# Support SIP Instance ID
# 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P288=1


# SIP T1 Timeout. RFC 3261 T1 value (RTT estimate)
# 50 - 0.5 sec, 100 - 1 sec, 200 - 2 sec. Default value is 50
# Number: 50, 100, 200
P209=50

# SIP T2 Interval. RFC 3261 T2 value
# The maximum retransmit interval for non-INVITE requests and INVITE responses
# 200 - 2 sec, 400 - 4 sec, 800 - 8 sec. Default value is 400
# Number: 200, 400, 800.
P250=400

# SIP Timer D Interval (Seconds)
# Number 0-64. Default value is 0
P2387=0

# Remove OBP from Route
# 0 - Disable, 1 - Enable, 2 - Always. Default value is 0
# Number: 0, 1, 2
P2305=0
#######################################################################
##  Account 1 Codec Settings                                         ##
#######################################################################
# Preferred Vocoder
# First codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 123 - Opus. Default value is 0
# Number: 0, 8, 9, 2, 18, 98, 123
P57=0

# Second codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 123 - Opus. Default value is 8
# Number: 0, 8, 9, 2, 18, 98, 123
P58=8

# Third codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 123 - Opus. Default value is 9
# Number: 0, 8, 9, 2, 18, 98, 123
P59=9

# Forth codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 123 - Opus. Default value is 9
# Number: 0, 8, 9, 2, 18, 98, 123
P60=9

# Fifth codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 123 - Opus. Default value is 9
# Number: 0, 8, 9, 2, 18, 98, 123
P61=9

# Sixth codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 123 - Opus. Default value is 9
# Number: 0, 8, 9, 2, 18, 98, 123
P62=9

# Seventh codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 123 - Opus. Default value is 9
# Number: 0, 8, 9, 2, 18, 98, 123
P46=9

# Eigth codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 123 - Opus. Default value is 9
# Number: 0, 8, 9, 2, 18, 98, 123
P98=9

# Codec Negotiation Priority. 0 - Caller, 1 - Callee. Default value is 1.
# Number: 0, 1
P29061=1

# Use First Matching Vocoder in 200OK SDP. 0 - No, 1 - Yes. The default value is 0.
# Number: 0, 1
P2348=0

# iLBC Frame Size. 0 - 20 ms, 1 - 30 ms. Default value is 1.
# Number: 0, 1
P97=1

# G726-32 ITU Payload. 0 - 2, 1 - Dynamic. Default value is 0.
# Number: 0, 1
P2369=0

# G726-32 Dynamic PT. Default value is 126.
# Number
P2365=126

# Opus Payload Type
P2385=123

# DTMF: in audio. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P2301=0

# DTMF: via RFC2833. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P2302=1

# DTMF: via SIP INFO. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P2303=0

# DTMF Payload Type. Default value is 101
# Number: 96 - 126
P79=101

# Enable Audio RED with FEC. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P26073=0

# Audio FEC Payload Type. Default value is 121
# Number: 96 - 126
P26074=121

# Audio RED Payload Type. Default value is 124
# Number: 96 - 126
P26075=124

# Silence Suppression. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P50=0

# Voice Frames Per TX. Default value is 2
# Number: 1 - 64.
P37=2

# Preferred Video Codec. 99 - H.264. Default is 99.
P295=99

# Enable Video FEC. 0 - No, 1 - Yes. Default value is 1.
# Number: 0, 1
P2393=1

# Enable RFC5168 Support. 0 - No, 1 - Yes. Default value is 1.
# Number: 0, 1
P1331=1

# Video FEC Mode. 0 - 0, 1 - 1. Default value is 0.
# Number: 0, 1
P26022=0

# FEC Payload Type. Default value is 120.
P2394=120

# Packetization mode. 0 - Single NAL Unit Mode, 1 - Non-Interleaved Mode. Default value is 1.
# Number: 0, 1, 10
P26005=1

# H.264 Image Size. 9 - 720P, 1 - VGA, 5 - CIF, 4 - 4CIF, 0 - QVGA, 6 - QCIF. Default value is 9
# Number: 9, 1, 5, 4, 0, 6
P2307=9

# Use H.264 Constrained Profiles. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1
P26045=0

# H.264 Profile Type. 0 - Baseline Profile, 1 - Main Profile, 2 - High Profile, 3 - BP&MP&HP
# Number: 0, 1, 2, 3
P2362=0

# Video Bit Rate. 64 - 64 kbps, 96 - 96 kbps, 128 - 128 kbps, 160 - 160 kbps, 192 - 192 kbps
# 210 - 210 kbps, 256 - 256 kbps, 384 - 384 kbps, 512 - 512 kbps, 640 - 640 kbps, 768 - 768 kbps
# 1024 - 1024 kbps, 1280 - 1280 kbps, 1536 - 1536 kbps, 2048 - 2048 kbps. Default value is 2048.
# Number: 250, 500, 750
P2315=2048

# SDP Bandwidth Attribute. 0 - Standard, 1 - Media Level, 2 - Session Level, 3 - None. Default value is Media Level.
# Number: 0, 1, 2, 3
P2360=1

# H.264 Payload Type. Default value is 99.
P293=99

# Disable BFCP. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1
P26001=0

# Presentation H.264 Image Size. 10 - 1080P, 9 - 720P. Default value is 10.
# Number: 10, 9
P2376=10

# Presentation H.264 Profile Type. 0 - Baseline Profile, 1 - Main Profile, 2 - High Profile, 3 - BP&MP&HP
# Number: 0, 1, 2, 3
P2377=3

# Presentation Video Bit Rate. 512 - 512 kbps, 640 - 640 kbps, 768 - 768 kbps
# 1024 - 1024 kbps, 1280 - 1280 kbps, 1536 - 1536 kbps, 2048 - 2048 kbps. Default value is 1024.
# Number: 250, 500, 750
P2378=1024

# Presentation Video Frame Rate. 5 - 5 frames/second, 10 - 10 frames/second, 15 - 15 frames/second. Default value is 15.
# Number: 5, 10, 15
P26042=15

# BFCP Transport Protocol. 0 - Automatic, 1 - UDP, 2 - TCP. Default value is 1.
# Number: 0, 1, 2
P26041=

# SRTP Mode. 0 - Disable, 1 - Enable but not forced, 2 - Enable and forced. Default value is 0.
# Number:0, 1, 2
P183=0

# SRTP Key Length. 0 - AES 128&256 bit, 1 - AES 128 bit, 2 - AES 256 bit. Default value is 0
#Number:0, 1, 2
P2383=0 

# Enable SRTP Key Lifetime. 0 - No, 1 - Yes.
# Number: 0,1
P2363=0

# RTCP Destination
P2390=

# Symmetric RTP. 0 - No, 1 - Yes. Default value is 0
# Number:0, 1
P291=0

# RTP IP Filter. 0 - Disable, 1 - IP Only, 2 - IP and Port. Default value is 0
# Number:0, 1, 2
P26026=0

# RTP Timeout(s). Default is 0. If set to 0, the device would not hangup.
# number: 0 - 600
P29068=0
#######################################################################
##  Account 1 Call Settings                                          ##
#######################################################################
# Enable Video Call. 0 - Default, 1 - No, 2 - Yes. Default is 0
# Number: 0, 1, 2
P60043=0

# Start Video Automatically. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P2314=1

# Remote Video Request. 0 - Prompt, 1 - Accept, 2 - Deny. Default value is 0
# Number: 0, 1, 2
P2326=0

# Video Layout. 0 - Default, 1 - Full screen, 3 - Equal split screen, 2 - Only display remote screen
P2332=0

# Auto Answer. 0 - No, 1 - Yes, 2 - Enable Intercom/Paging. Default value is 0
# Number: 0, 1, 2
P90=0

# Play warning tone for Auto Answer Intercom. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P26072=1

# Intercom Barging. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P26019=1

# Auto Preview. 0 - No, 1 - Yes, 2 - Yes with Ringing. Default value is 0
# Number: 0, 1, 2
P29062=0

# Send Anonymous. 0 - No, 1 - Yes (caller ID will be blocked if set to Yes). Default value is 0
# Number: 0, 1
P65=0

# Anonymous Call Rejection. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P129=0

# Call Log
# 0 - Log All, 1 - Log Incoming/Outgoing only (Missed Calls Not Recorded), 2 - Disable Call All, 3 - Don't Prompt Missed Call. Default value is 0
# Number: 0, 1, 2
P182=0

# Enable Call Features. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P191=0

# Enable Call Waiting. 0 - Default, 1 - No, 2 - Yes.
# Number: 0, 1, 2
P26063=0

# Mute on Answer Intercom Call. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
P26071=0

# Transfer on 3 way conference Hangup. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P2304=0

# Use # as Dial Key. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P72=1

# Use # as Redial Key. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P29069=1

# DND Call Feature On.
# String
P2344=

# DND Call Feature Off.
# String
P2345=

# No Key Entry Timeout (s). Default value is 4
# Number: 1 - 15
P85=4

# Ring Timeout (s). Default value is 60
# Number: 10 - 300
P1328=60

# Refer-To Use Target Contact. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P135=0

# RFC2543 Hold. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1 
P26062=1

# Dial Plan Prefix
# String
P66=

# Disable DialPlan. 0 - No Selection, 1 - Dial Page, 2 - Contact, 4 - Incoming Call History, 8 -  Outgoing Call History, 16 - MPK & Click2Dial. 
# If need to check multiple selections, add the specific values for each selections together. Default value is 0
# Number: 0-31
P2382=0

# DialPlan. Default value is { x+ | \+x+ | *x+ | *xx*x+ | x+*x+*x+*x+ | x+*x+*x+*x+#x+ }
P290={ x+ | \+x+ | *x+ | *xx*x+ | x+*x+*x+*x+ | x+*x+*x+*x+#x+ }

# Caller ID Display. 0 - Auto, 1 - Disabled, 2 - From Header. The default value is 0.
# Number: 0, 1, 2, 3
P2324=0

# Account Ringtone. See ring tone options and value in the Ring Tone Value Table below
P104=content://settings/system/ringtone

# Ignore Alert-Info Header. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1
P26018=0

# Matching Incoming Caller ID. Matching Rule 1
# String
P1488=

# Matching Rule 1 Distinctive Ringtone. See ring tone options and value in the Ring Tone Value Table below
# String
P1489=content://settings/system/ringtone

# Matching Incoming Caller ID. Matching Rule 2
# String
P1490=

# Matching Rule 2 Distinctive Ringtone. See ring tone options and value in the Ring Tone Value Table below
# String
P1491=content://settings/system/ringtone

# Matching Incoming Caller ID. Matching Rule 3
# String
P1492=

# Matching Rule 3 Distinctive Ringtone. See ring tone options and value in the Ring Tone Value Table below
# String
P1493=content://settings/system/ringtone

############Ring Tone Value Table###############
# Web GUI Option                            Value
# Use System Ring tone                      content://settings/system/ringtone 
# Andromeda					/system/media/audio/ringtones/ANDROMEDA.ogg
# Aquila					/system/media/audio/ringtones/Aquila.ogg
# Argo Navis					/system/media/audio/ringtones/ArgoNavis.ogg
# Atria					/system/media/audio/ringtones/Atria.ogg
# Backroad					/system/media/audio/ringtones/Backroad.ogg
# Beat Plucker					/system/media/audio/ringtones/BeatPlucker.ogg
# Bell Phone					/system/media/audio/ringtones/Ring_Classic_02.ogg
# Bentley Dubs					/system/media/audio/ringtones/BentleyDubs.ogg
# Big Easy					/system/media/audio/ringtones/Big_Easy.ogg
# Bird Loop					/system/media/audio/ringtones/BirdLoop.ogg
# Bollywood					/system/media/audio/ringtones/Bollywood.ogg
# Boötes					/system/media/audio/ringtones/BOOTES.ogg
# Bus' a Move					/system/media/audio/ringtones/BussaMove.ogg
# Cairo					/system/media/audio/ringtones/Cairo.ogg
# Calypso Steel					/system/media/audio/ringtones/Calypso_Steel.ogg
# Canis Major					/system/media/audio/ringtones/CANISMAJOR.ogg
# Caribbean Ice					/system/media/audio/ringtones/CaribbeanIce.ogg
# Carina					/system/media/audio/ringtones/Carina.ogg
# Cassiopeia					/system/media/audio/ringtones/CASSIOPEIA.ogg
# Centaurus					/system/media/audio/ringtones/Centaurus.ogg
# Champagne Edition					/system/media/audio/ringtones/Champagne_Edition.ogg
# Chimey Phone					/system/media/audio/ringtones/Ring_Synth_02.ogg
# Club Cubano					/system/media/audio/ringtones/Club_Cubano.ogg
# Crayon Rock					/system/media/audio/ringtones/CrayonRock.ogg
# Crazy Dream					/system/media/audio/ringtones/CrazyDream.ogg
# Curve Ball Blend					/system/media/audio/ringtones/CurveBall.ogg
# Cygnus					/system/media/audio/ringtones/Cygnus.ogg
# Dancin' Fool					/system/media/audio/ringtones/DancinFool.ogg
# Digital Phone					/system/media/audio/ringtones/Ring_Digital_02.ogg
# Ding					/system/media/audio/ringtones/Ding.ogg
# DingDong					/system/media/audio/ringtones/DingDong.wav
# Don' Mess Wiv It					/system/media/audio/ringtones/DonMessWivIt.ogg
# Draco					/system/media/audio/ringtones/Draco.ogg
# Dream Theme					/system/media/audio/ringtones/DreamTheme.ogg
# Eastern Sky					/system/media/audio/ringtones/Eastern_Sky.ogg
# Enter the Nexus					/system/media/audio/ringtones/Enter_the_Nexus.ogg
# Eridani					/system/media/audio/ringtones/Eridani.ogg
# Ether Shake					/system/media/audio/ringtones/EtherShake.ogg
# Flutey Phone					/system/media/audio/ringtones/Ring_Synth_04.ogg
# Free Flight					/system/media/audio/ringtones/FreeFlight.ogg
# Friendly Ghost					/system/media/audio/ringtones/FriendlyGhost.ogg
# Funk Y'all					/system/media/audio/ringtones/Funk_Yall.ogg
# Game Over Guitar					/system/media/audio/ringtones/GameOverGuitar.ogg
# Gimme Mo' Town					/system/media/audio/ringtones/Gimme_Mo_Town.ogg
# Girtab					/system/media/audio/ringtones/Girtab.ogg
# Glacial Groove					/system/media/audio/ringtones/Glacial_Groove.ogg
# Growl					/system/media/audio/ringtones/Growl.ogg
# Halfway Home					/system/media/audio/ringtones/HalfwayHome.ogg
# Hydra					/system/media/audio/ringtones/Hydra.ogg
# Insert Coin					/system/media/audio/ringtones/InsertCoin.ogg
# Kuma					/system/media/audio/ringtones/Kuma.ogg
# Loopy Lounge					/system/media/audio/ringtones/LoopyLounge.ogg
# Love Flute					/system/media/audio/ringtones/LoveFlute.ogg
# Lyra					/system/media/audio/ringtones/Lyra.ogg
# Machina					/system/media/audio/ringtones/Machina.ogg
# Medieval Jaunt					/system/media/audio/ringtones/MidEvilJaunt.ogg
# Mildly Alarming					/system/media/audio/ringtones/MildlyAlarming.ogg
# Nairobi					/system/media/audio/ringtones/Nairobi.ogg
# Nassau					/system/media/audio/ringtones/Nassau.ogg
# New Player					/system/media/audio/ringtones/NewPlayer.ogg
# No Limits					/system/media/audio/ringtones/No_Limits.ogg
# Noisey One					/system/media/audio/ringtones/Noises1.ogg
# Organ Dub					/system/media/audio/ringtones/OrganDub.ogg
# Orion					/system/media/audio/ringtones/Orion.ogg
# Paradise Island					/system/media/audio/ringtones/Paradise_Island.ogg
# Pegasus					/system/media/audio/ringtones/Pegasus.ogg
# Perseus					/system/media/audio/ringtones/PERSEUS.ogg
# Playa					/system/media/audio/ringtones/Playa.ogg
# Pyxis					/system/media/audio/ringtones/Pyxis.ogg
# Rasalas					/system/media/audio/ringtones/Rasalas.ogg
# Revelation					/system/media/audio/ringtones/Revelation.ogg
# Rigel					/system/media/audio/ringtones/Rigel.ogg
# Road Trip					/system/media/audio/ringtones/Road_Trip.ogg
# Romancing The Tone					/system/media/audio/ringtones/RomancingTheTone.ogg
# Safari					/system/media/audio/ringtones/Safari.ogg
# Savannah					/system/media/audio/ringtones/Savannah.ogg
# Scarabaeus					/system/media/audio/ringtones/Scarabaeus.ogg
# Sceptrum					/system/media/audio/ringtones/Sceptrum.ogg
# Seville					/system/media/audio/ringtones/Seville.ogg
# She's All That					/system/media/audio/ringtones/Shes_All_That.ogg
# Silky Way					/system/media/audio/ringtones/SilkyWay.ogg
# Sitar Versus Sitar					/system/media/audio/ringtones/SitarVsSitar.ogg
# Solarium					/system/media/audio/ringtones/Solarium.ogg
# Springy Jalopy					/system/media/audio/ringtones/SpringyJalopy.ogg
# Steppin' Out					/system/media/audio/ringtones/Steppin_Out.ogg
# Terminated					/system/media/audio/ringtones/Terminated.ogg
# Terrible Twos					/system/media/audio/ringtones/Noises2.ogg
# Testudo					/system/media/audio/ringtones/Testudo.ogg
# Themos					/system/media/audio/ringtones/Themos.ogg
# Third Eye					/system/media/audio/ringtones/Third_Eye.ogg
# Thriller Three					/system/media/audio/ringtones/Noises3.ogg
# Thunderfoot					/system/media/audio/ringtones/Thunderfoot.ogg
# Twirl Away					/system/media/audio/ringtones/TwirlAway.ogg
# Ursa Minor					/system/media/audio/ringtones/URSAMINOR.ogg
# UrsaMinor					/system/media/audio/ringtones/UrsaMinor.ogg
# Very Alarmed					/system/media/audio/ringtones/VeryAlarmed.ogg
# Vespa					/system/media/audio/ringtones/Vespa.ogg
# World					/system/media/audio/ringtones/World.ogg
# Zeta					/system/media/audio/ringtones/Zeta.ogg
# bellcore-dr1					/system/media/audio/ringtones/bellcore-dr1.ogg
# bellcore-dr2					/system/media/audio/ringtones/bellcore-dr2.ogg
# bellcore-dr3					/system/media/audio/ringtones/bellcore-dr3.ogg
# bellcore-dr4					/system/media/audio/ringtones/bellcore-dr4.ogg
# bellcore-dr5					/system/media/audio/ringtones/bellcore-dr5.ogg
# speaker					/system/media/audio/ringtones/speaker.wav

#######################################################################
##  Account 1 Advanced Settings                                      ##
#######################################################################
# Check Domain Certificates. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P2311=0

# Validate Certificate Chain. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P2367=0

# Validate Incoming SIP Messages. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P2306=0

# Allow Unsolicited REFER. 0 - Disabled, 1 - Enabled, 2 - Enabled/Force Auth. Default value is 0.
# Number: 0, 1, 2
P26023=0

# Only Accept SIP Requests from Known Servers. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P2347=0

# Check SIP User ID for Incoming INVITE. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P258=0

# Allow SIP Reset. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P26015=0

# Authenticate Incoming INVITE. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P2346=0

# SIP Realm Used for Challenge INVITE & NOTIFY.
# String
P26021=

# Enable Local MOH. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P2357=0

# Virtual Account Group. -1 - Default,  0 - Virtual Account Group 1, 1 - Virtual Account Group 2, 2 - Virtual Account Group 3
# 3 - Virtual Account Group 4, 4 - Virtual Account Group 5, 5 - Virtual Account Group 6, 6 - Virtual Account Group 7, 7 - Virtual Account Group 8
# 8 - Virtual Account Group 9, 9 - Virtual Account Group 10, 10 - Virtual Account Group 11, 11 - Virtual Account Group 12, 12 - Virtual Account Group 13
# 13 - Virtual Account Group 14, 14 - Virtual Account Group 15, 15 - Virtual Account Group 16. Default value is -1.
# Number: -1 - 15 
P2391=-1

# Special Feature. Default value is 100
# 100 - Standard, 102 - Broadsoft, 113 - China Mobile
# 114 - ZTE IMS, 115 - Mobotix, 116 - ZTE NGN, 117 - Huawei IMS, 123 - NEC, 125 - WorldStone
# Number: 100, 102, 113, 114, 115, 116, 117, 123, 125
P198=100

# Allow Sync Phonebook via SIP Notify. 0 - No, 1 - Yes. Default is 1.
# Number: 0, 1
P26099=1
##############################################################################
##  Account 2 Settings                                                      ##
##############################################################################
#######################################################################
##  Account 2 General Settings                                       ##
#######################################################################
# Account Active. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P401=0

# Account Name
P417=

# SIP Server
P402=

# SIP User ID
P404=

# SIP Authentication ID
P405=

# SIP Authentication Password
P406=

# Voice Mail Access Number
P426=

# Name (Display name, e.g., John Doe)
P407=

# Tel URI. 0 - Disabled, 1 - User=Phone, 2 - Enabled. Default value is 0
# Number: 0, 1, 2
P409=0
#######################################################################
##  Account 2 Network Settings                                       ##
#######################################################################
# Outbound Proxy
P403=

# Secondary Outbound Proxy
P2433=

# DNS Mode. 0 - A Record, 1 - SRV, 2 - NAPTR/SRV. Default value is 0
# Number: 0, 1, 2
P408=0

# DNS SRV Fail-over Mode. 0 - Default, 1 - Saved one until DNS TTL, 2 - Saved one until no response. Defualt value is 1
# Number
P26140=0

# Register Before DNS SRV Fail-over. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P29195=0

# NAT Traversal. 0 - No, 1 - STUN, 2 - Keep-alive, 3 - UPnP, 4 - Auto, 5 - VPN. Default value is 2
# Number: 0, 1, 2, 3, 4, 5
P414=2

# Proxy-Require
P418=

#######################################################################
##  Account 2 SIP Settings                                           ##
#######################################################################
# SIP Registration. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P410=1

# Unregister Before New Registration. 0 - No, 1 - Yes, 2 -  Instance . Default value is 0
# Number: 0, 1, 2
P411=0

# Register Expiration (m). In minutes. Default value is 60
# Number: 0 - 64800
P412=60

# Subscribe Expiration (m). Default is 60
# Number: 0 - 64800
P26151=60

# Re-register before Expiration (s). Default value is 0
# Number
P2430=0

# Registration Retry Wait Time(s). In seconds. Default value is 20
# Number: 1 - 3600
P471=20

# Local SIP Port. Default value is 5062
# Number: 5 - 65535
P413=5062

# SUBSCRIBE for MWI (Whether or not send SUBSCRIBE for Message Waiting Indication)
# 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1.
P415=0

# Enable OPTIONS Keep Alive. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P2497=0

# OPTIONS Keep Alive Interval(s). Default value is 30
# Number 
P2498=30

# OPTIONS Keep Alive Maximum Tries. Default value is 3
# Number 
P2499=3

# Enable Session Timer/ Session Expiration(s).  In seconds. Default value is 180 seconds.
# By default,  Session Timer is Enabled.  Session Timer is disabled if the value is 0.
# Number: 0 or 90 - 64800
P434=180

# Min-SE (s). Default value is 90 seconds
# Number: 90 - 64800
P427=90

# UAC Specify Refresher. 0 - Omit, 1 - UAC, 2 - UAS. Default value is 0
# Number: 0, 1, 2
P432=0

# UAS Specify Refresher. 1 - UAC, 2 - UAS. Default value is 1
# Number: 1, 2
P433=1

# Force INVITE (Always refresh with INVITE instead of UPDATE even when remote party supports UPDATE)
# 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P431=0

# Caller Request Timer (Request for timer when calling). 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P428=0

# Callee Request Timer (Request for timer when being called, i.e. if remote party supports timer but did not request for one)
# 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P429=0

# Force Timer (Still use timer when remote party does not support timer). 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P430=0

# Enable 100rel. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P435=0 

# Use Privacy Header. 0 - Default, 1 - No, 2 - Yes. Default value is 0
# Number: 0, 1, 2
P2438=0

# Use P-Preferred-Identity Header. 0 - Default, 1 - No, 2 - Yes. Default value is 0
# Number: 0, 1, 2
P2439=0

# Use P-Access-Network-Info Header. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P26158=1

# Use P-Emergency-Info Header. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P26159=1

# Use MAC Header.  0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P26161=0

# SIP Transport. 0 - UDP, 1 - TCP, 2 - TLS. Default value is 0
# Number: 0, 1, 2
P448=0

# SIP URI Scheme When Using TLS
# 0 -sip, 1 - sips. Default value is 0.
# Number: 0, 1
P2429=0

# Use Actual Ephemeral Port in Contact with TCP/TLS
# 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P2431=0

# Support SIP Instance ID. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P489=1

# Add Auth Header On RE-REGISTER
# 0 - No, 1- Yes
P2459=0

# SIP T1 Timeout. RFC 3261 T1 value (RTT estimate). 50 - 0.5 sec, 100 - 1 sec, 200 - 2 sec. Default value is 50
# Number: 50, 100, 200
P440=50

# SIP T2 Interval. RFC 3261 T2 value. The maximum retransmit interval for non-INVITE requests and INVITE responses
# 200 - 2 sec, 400 - 4 sec, 800 - 8 sec. Default value is 400
# Number: 200, 400, 800
P441=400

# SIP Timer D Interval (Seconds)
# Number 0-64. Default value is 0
P2487=0

# Remove OBP from route. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P2405=0
#######################################################################
##  Account 2 Codec Settings                                         ##
#######################################################################
# Preferred Vocoder
# First codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 98 - iLBC, 123 - Opus. Default value is 0
# Number: 0, 2, 8, 9, 98, 123
P451=0

# Second codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 98 - iLBC, 123 - Opus. Default value is 8
# Number: 0, 2, 8, 9, 98, 123
P452=8

# Third codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 98 - iLBC, 123 - Opus. Default value is 9
# Number: 0, 2, 8, 9, 98, 123
P453=9

# Forth codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 98 - iLBC, 123 - Opus. Default value is 9
# Number: 0, 2, 8, 9, 98, 123
P454=9

# Fifth codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 98 - iLBC, 123 - Opus. Default value is 9
# Number: 0, 2, 8, 9, 98, 123
P455=9

# Sixth codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 123 - Opus. Default value is 9
# Number: 0, 8, 9, 2, 18, 98, 123
P456=9

# Seventh codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 123 - Opus. Default value is 9
# Number: 0, 8, 9, 2, 18, 98, 123
P457=9

# Eigth codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 123 - Opus. Default value is 9
# Number: 0, 8, 9, 2, 18, 98, 123
P458=9

# Codec Negotiation Priority. 0 - Caller, 1 - Callee. Default value is 1.
# Number: 0, 1
P29161=1

# Use First Matching Vocoder in 200OK SDP. 0 - No, 1 - Yes. The default value is 0.
# Number: 0, 1
P2448=0

# iLBC Frame Size. 0 - 20 ms, 1 - 30 ms. Default value is 1.
# Number: 0, 1
P495=1

#G726-32 ITU Payload. 0 - 2, 1 - Dynamic. Default value is 0.
# Number: 0, 1
P2469=0

#G726-32 Dynamic PT. Default value is 126.
# Number
P2465=126

#Opus Payload Type
P2485=123

# DTMF: in audio. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P2401=0

# DTMF: via RFC2833. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P2402=1

# DTMF: via SIP INFO. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P2403=0

# DTMF Payload Type. Default value is 101
# Number: 96 - 126
P496=101

# Enable Audio RED with FEC. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P26173=0

# Audio FEC Payload Type. Default value is 121
# Number: 96 - 126
P26174=121

# Audio RED Payload Type. Default value is 124
# Number: 96 - 126
P26175=124

# Silence Suppression. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P485=0

# Voice Frames per TX. Default value is 2
# Number: 1 - 64
P486=2

# Preferred Video Codec. 99 - H.264. Default is 99.
P464=99

# Enable Video FEC. 0 - No, 1 - Yes. Default value is 1.
# Number: 0, 1
P2493=1

# Enable RFC5168 support. 0 - No, 1 - Yes. Default value is 1.
# Number: 0, 1
P478=1

# Video FEC Mode. 0 - 0, 1 - 1. Default value is 0.
# Number: 0, 1
P26122=0

# FEC Payload Type. Default value is 120.
P2494=120

# Packetization mode. 0 - Single NAL Unit Mode, 1 - Non-Interleaved Mode. Default value is 1.
# Number: 0, 1, 10
P26105=1

# H.264 Image Size. 9 - 720P, 1 - VGA, 5 - CIF, 4 - 4CIF, 0 - QVGA, 6 - QCIF. Default value is 9
# Number: 9, 1, 5, 4, 0, 6
P2407=9

# Use H.264 Constrained Profiles. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1
P26145=0

# H.264 Profile Type. 0 - Baseline Profile, 1 - Main Profile, 2 - High Profile, 3 - BP&MP&HP
# Number: 0, 1, 2, 3
P2462=0

# Video Bit Rate. 64 - 64 kbps, 96 - 96 kbps, 128 - 128 kbps, 160 - 160 kbps, 192 - 192 kbps
# 210 - 210 kbps, 256 - 256 kbps, 384 - 384 kbps, 512 - 512 kbps, 640 - 640 kbps, 768 - 768 kbps
# 1024 - 1024 kbps, 1280 - 1280 kbps, 1536 - 1536 kbps, 2048 - 2048 kbps. Default value is 2048.
# Number: 
P2415=2048

# SDP Bandwidth Attribute. 0 - Standard, 1 - Media Level, 2 - Session Level, 3 - None. Default value is Media Level.
# Number: 0, 1, 2, 3
P2460=1

# H.264 Payload Type
P462=99

# Disable BFCP. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1
P26101=0

# Presentation H.264 Image Size. 10 - 1080P, 9 - 720P. Default value is 10.
# Number: 10, 9
P2476=10

# Presentation H.264 Profile Type. 0 - Baseline Profile, 1 - Main Profile, 2 - High Profile, 3 - BP&MP&HP
# Number: 0, 1, 2, 3
P2477=3

# Presentation Video Bit Rate. 512 - 512 kbps, 640 - 640 kbps, 768 - 768 kbps
# 1024 - 1024 kbps, 1280 - 1280 kbps, 1536 - 1536 kbps, 2048 - 2048 kbps. Default value is 1024.
# Number: 250, 500, 750
P2478=1024

# Presentation Video Frame Rate. 5 - 5 frames/second, 10 - 10 frames/second, 15 - 15 frames/second. Default value is 15.
# Number: 5, 10, 15
P26142=

# BFCP Transport Protocol. 0 - Automatic, 1 - UDP, 2 - TCP. Default value is 1.
# Number: 0, 1, 2
P26141=

# SRTP Mode. 0 - Disabled, 1 - Enabled but not forced, 2 - Enabled and forced. Default value is 0
# Number: 0, 1, 2
P443=0

# SRTP Key Length. 0 - AES 128&256 bit, 1 - AES 128 bit, 2 - AES 256 bit. Default value is 0
#Number:0, 1, 2
P2483=0 

# Enable SRTP Key Lift Time. 0 - No, 1 - Yes.
# Number: 0,1
P2463=0

# RTCP Destination
P2490=

# Symmetric RTP. 0 - No, 1 - Yes. Default value is 0
# Number:0, 1
P460=0

# RTP IP Filter. 0 - Disable, 1 - IP Only, 2 - IP and Port. Default value is 0
# Number:0, 1, 2
P26126=0

# RTP Timeout(s). Default is 0. If set to 0, the device would not hangup.
# number: 0 - 600
P29168=0
#######################################################################
##  Account 2 Call Settings                                          ##
#######################################################################
# Enable Video Call. 0 - Default, 1 - No, 2 - Yes. Default is 0
# Number: 0, 1, 2
P60143=0

# Start Video Automatically. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P2414=1

# Remote Video Request. 0 - Prompt, 1 - Accept, 2 - Deny. Default value is 0
# Number: 0, 1, 2
P2426=0

# Video Layout. 0 - Default, 1 - Full screen, 3 - Equal split screen, 2 - Only display remote screen
P2432=0

# Auto Answer. 0 - No, 1 - Yes, 2 - Enable Intercom/Paging. Default value is 0
# Number: 0, 1, 2
P425=0

# Play warning tone for Auto Answer Intercom. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P26172=1

# Intercom Barging. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P26119=1

# Auto Preview. 0 - No, 1 - Yes, 2 - Yes with Ringing. Default value is 0
# Number: 0, 1, 2
P29162=0

# Send Anonymous. 0 - No, 1 - Yes (caller ID will be blocked if set to Yes). Default value is 0
# Number: 0, 1
P421=0

# Anonymous Call Rejection. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P446=0

# Call Log
# 0 - Log All, 1 - Log Incoming/Outgoing only (Missed Calls Not Recorded), 2 - Disable Call All, 3 - Don't Prompt Missed Call. Default value is 0
# Number: 0, 1, 2
P442=0

# Enable Call Features. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P420=0

# Enable Call Waiting. 0 - Default, 1 - No, 2 - Yes.
# Number: 0, 1, 2
P26163=0

# Mute on Answer Intercom Call. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
P26171=0

# Transfer on 3 way conference Hangup. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P2404=0

# Use # as Dial Key. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P492=1

# Use # as Redial Key. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P29169=1

# DND Call Feature On.
# String
P2444=

# DND Call Feature Off.
# String
P2445=

# No Key Entry Timeout (s). Default value is 4
# Number: 1 - 15
P491=4

# Ring Timeout (s). Default value is 60
# Number: 10 - 300
P476=60

# Refer-To Use Target Contact. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P469=0

# RFC2543 Hold. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1 
P26162=1

# Dial Plan Prefix
# String
P419=

# Disable DialPlan. 0 - No Selection, 1 - Dial Page, 2 - Contact, 4 - Incoming Call History, 8 -  Outgoing Call History, 16 - MPK & Click2Dial. 
# If need to check multiple selections, add the specific values for each selections together. Default value is 0
# Number: 0-31
P2482=0

# DialPlan. Default value is { x+ | \+x+ | *x+ | *xx*x+ | x+*x+*x+*x+ | x+*x+*x+*x+#x+ }
P459={ x+ | \+x+ | *x+ | *xx*x+ | x+*x+*x+*x+ | x+*x+*x+*x+#x+ }

# Caller ID Display. 0 - Auto, 1 - Disabled, 2 - From Header. The default value is 0.
# Number: 0, 1, 2, 3
P2424=0

# Account Ringtone. See ring tone options and value in the Ring Tone Value Table below
P423=content://settings/system/ringtone

# Ignore Alert-Info Header. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1
P26118=0

# Matching Incoming Caller ID. Matching Rule 1
# String
P1494=

# Matching Rule 1 Distinctive Ringtone. See ring tone options and value in the Ring Tone Value Table below
# String
P1495=content://settings/system/ringtone

# Matching Incoming Caller ID. Matching Rule 2
# String
P1496=

# Matching Rule 2 Distinctive Ringtone. See ring tone options and value in the Ring Tone Value Table below
# String
P1497=content://settings/system/ringtone

# Matching Incoming Caller ID. Matching Rule 3
# String
P1498=

# Matching Rule 3 Distinctive Ringtone. See ring tone options and value in the Ring Tone Value Table below
# String
P1499=content://settings/system/ringtone

############Ring Tone Value Table###############
# Web GUI Option                            Value
# Use System Ring tone                      content://settings/system/ringtone 
# Silent                                    ringtone_silence
# Andromeda					/system/media/audio/ringtones/ANDROMEDA.ogg
# Aquila					/system/media/audio/ringtones/Aquila.ogg
# Argo Navis					/system/media/audio/ringtones/ArgoNavis.ogg
# Atria					/system/media/audio/ringtones/Atria.ogg
# Backroad					/system/media/audio/ringtones/Backroad.ogg
# Beat Plucker					/system/media/audio/ringtones/BeatPlucker.ogg
# Bell Phone					/system/media/audio/ringtones/Ring_Classic_02.ogg
# Bentley Dubs					/system/media/audio/ringtones/BentleyDubs.ogg
# Big Easy					/system/media/audio/ringtones/Big_Easy.ogg
# Bird Loop					/system/media/audio/ringtones/BirdLoop.ogg
# Bollywood					/system/media/audio/ringtones/Bollywood.ogg
# Boötes					/system/media/audio/ringtones/BOOTES.ogg
# Bus' a Move					/system/media/audio/ringtones/BussaMove.ogg
# Cairo					/system/media/audio/ringtones/Cairo.ogg
# Calypso Steel					/system/media/audio/ringtones/Calypso_Steel.ogg
# Canis Major					/system/media/audio/ringtones/CANISMAJOR.ogg
# Caribbean Ice					/system/media/audio/ringtones/CaribbeanIce.ogg
# Carina					/system/media/audio/ringtones/Carina.ogg
# Cassiopeia					/system/media/audio/ringtones/CASSIOPEIA.ogg
# Centaurus					/system/media/audio/ringtones/Centaurus.ogg
# Champagne Edition					/system/media/audio/ringtones/Champagne_Edition.ogg
# Chimey Phone					/system/media/audio/ringtones/Ring_Synth_02.ogg
# Club Cubano					/system/media/audio/ringtones/Club_Cubano.ogg
# Crayon Rock					/system/media/audio/ringtones/CrayonRock.ogg
# Crazy Dream					/system/media/audio/ringtones/CrazyDream.ogg
# Curve Ball Blend					/system/media/audio/ringtones/CurveBall.ogg
# Cygnus					/system/media/audio/ringtones/Cygnus.ogg
# Dancin' Fool					/system/media/audio/ringtones/DancinFool.ogg
# Digital Phone					/system/media/audio/ringtones/Ring_Digital_02.ogg
# Ding					/system/media/audio/ringtones/Ding.ogg
# DingDong					/system/media/audio/ringtones/DingDong.wav
# Don' Mess Wiv It					/system/media/audio/ringtones/DonMessWivIt.ogg
# Draco					/system/media/audio/ringtones/Draco.ogg
# Dream Theme					/system/media/audio/ringtones/DreamTheme.ogg
# Eastern Sky					/system/media/audio/ringtones/Eastern_Sky.ogg
# Enter the Nexus					/system/media/audio/ringtones/Enter_the_Nexus.ogg
# Eridani					/system/media/audio/ringtones/Eridani.ogg
# Ether Shake					/system/media/audio/ringtones/EtherShake.ogg
# Flutey Phone					/system/media/audio/ringtones/Ring_Synth_04.ogg
# Free Flight					/system/media/audio/ringtones/FreeFlight.ogg
# Friendly Ghost					/system/media/audio/ringtones/FriendlyGhost.ogg
# Funk Y'all					/system/media/audio/ringtones/Funk_Yall.ogg
# Game Over Guitar					/system/media/audio/ringtones/GameOverGuitar.ogg
# Gimme Mo' Town					/system/media/audio/ringtones/Gimme_Mo_Town.ogg
# Girtab					/system/media/audio/ringtones/Girtab.ogg
# Glacial Groove					/system/media/audio/ringtones/Glacial_Groove.ogg
# Growl					/system/media/audio/ringtones/Growl.ogg
# Halfway Home					/system/media/audio/ringtones/HalfwayHome.ogg
# Hydra					/system/media/audio/ringtones/Hydra.ogg
# Insert Coin					/system/media/audio/ringtones/InsertCoin.ogg
# Kuma					/system/media/audio/ringtones/Kuma.ogg
# Loopy Lounge					/system/media/audio/ringtones/LoopyLounge.ogg
# Love Flute					/system/media/audio/ringtones/LoveFlute.ogg
# Lyra					/system/media/audio/ringtones/Lyra.ogg
# Machina					/system/media/audio/ringtones/Machina.ogg
# Medieval Jaunt					/system/media/audio/ringtones/MidEvilJaunt.ogg
# Mildly Alarming					/system/media/audio/ringtones/MildlyAlarming.ogg
# Nairobi					/system/media/audio/ringtones/Nairobi.ogg
# Nassau					/system/media/audio/ringtones/Nassau.ogg
# New Player					/system/media/audio/ringtones/NewPlayer.ogg
# No Limits					/system/media/audio/ringtones/No_Limits.ogg
# Noisey One					/system/media/audio/ringtones/Noises1.ogg
# Organ Dub					/system/media/audio/ringtones/OrganDub.ogg
# Orion					/system/media/audio/ringtones/Orion.ogg
# Paradise Island					/system/media/audio/ringtones/Paradise_Island.ogg
# Pegasus					/system/media/audio/ringtones/Pegasus.ogg
# Perseus					/system/media/audio/ringtones/PERSEUS.ogg
# Playa					/system/media/audio/ringtones/Playa.ogg
# Pyxis					/system/media/audio/ringtones/Pyxis.ogg
# Rasalas					/system/media/audio/ringtones/Rasalas.ogg
# Revelation					/system/media/audio/ringtones/Revelation.ogg
# Rigel					/system/media/audio/ringtones/Rigel.ogg
# Road Trip					/system/media/audio/ringtones/Road_Trip.ogg
# Romancing The Tone					/system/media/audio/ringtones/RomancingTheTone.ogg
# Safari					/system/media/audio/ringtones/Safari.ogg
# Savannah					/system/media/audio/ringtones/Savannah.ogg
# Scarabaeus					/system/media/audio/ringtones/Scarabaeus.ogg
# Sceptrum					/system/media/audio/ringtones/Sceptrum.ogg
# Seville					/system/media/audio/ringtones/Seville.ogg
# She's All That					/system/media/audio/ringtones/Shes_All_That.ogg
# Silky Way					/system/media/audio/ringtones/SilkyWay.ogg
# Sitar Versus Sitar					/system/media/audio/ringtones/SitarVsSitar.ogg
# Solarium					/system/media/audio/ringtones/Solarium.ogg
# Springy Jalopy					/system/media/audio/ringtones/SpringyJalopy.ogg
# Steppin' Out					/system/media/audio/ringtones/Steppin_Out.ogg
# Terminated					/system/media/audio/ringtones/Terminated.ogg
# Terrible Twos					/system/media/audio/ringtones/Noises2.ogg
# Testudo					/system/media/audio/ringtones/Testudo.ogg
# Themos					/system/media/audio/ringtones/Themos.ogg
# Third Eye					/system/media/audio/ringtones/Third_Eye.ogg
# Thriller Three					/system/media/audio/ringtones/Noises3.ogg
# Thunderfoot					/system/media/audio/ringtones/Thunderfoot.ogg
# Twirl Away					/system/media/audio/ringtones/TwirlAway.ogg
# Ursa Minor					/system/media/audio/ringtones/URSAMINOR.ogg
# UrsaMinor					/system/media/audio/ringtones/UrsaMinor.ogg
# Very Alarmed					/system/media/audio/ringtones/VeryAlarmed.ogg
# Vespa					/system/media/audio/ringtones/Vespa.ogg
# World					/system/media/audio/ringtones/World.ogg
# Zeta					/system/media/audio/ringtones/Zeta.ogg
# bellcore-dr1					/system/media/audio/ringtones/bellcore-dr1.ogg
# bellcore-dr2					/system/media/audio/ringtones/bellcore-dr2.ogg
# bellcore-dr3					/system/media/audio/ringtones/bellcore-dr3.ogg
# bellcore-dr4					/system/media/audio/ringtones/bellcore-dr4.ogg
# bellcore-dr5					/system/media/audio/ringtones/bellcore-dr5.ogg
# speaker					/system/media/audio/ringtones/speaker.wav
#######################################################################
##  Account 2 Advanced Settings                                      ##
#######################################################################
# Check Domain Certificates. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P2411=0

# Validate Certificate Chain. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P2467=0

# Validate Incoming SIP Messages. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P2406=0

# Allow Unsolicited REFER. 0 - Disabled, 1 - Enabled, 2 - Enabled/Force Auth. Default value is 0.
# Number: 0, 1, 2
P26123=0

# Only Accept SIP Requests from Known Servers. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P2447=0

# Check SIP User ID for Incoming INVITE. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P449=0

# Allow SIP Reset. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P26115=0

# Authenticate Incoming INVITE. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P2446=0

# SIP Realm Used for Challenge INVITE & NOTIFY.
# String
P26121=


# Enable Local MOH. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P2457=0

# Virtual Account Group. -1 - Default,  0 - Virtual Account Group 1, 1 - Virtual Account Group 2, 2 - Virtual Account Group 3
# 3 - Virtual Account Group 4, 4 - Virtual Account Group 5, 5 - Virtual Account Group 6, 6 - Virtual Account Group 7, 7 - Virtual Account Group 8
# 8 - Virtual Account Group 9, 9 - Virtual Account Group 10, 10 - Virtual Account Group 11, 11 - Virtual Account Group 12, 12 - Virtual Account Group 13
# 13 - Virtual Account Group 14, 14 - Virtual Account Group 15, 15 - Virtual Account Group 16. Default value is -1.
# Number: -1 - 15 
P2491=-1

# Special Feature. Default value is 100
# 100 - Standard, 102 - Broadsoft, 113 - China Mobile
# 114 - ZTE IMS, 115 - Mobotix, 116 - ZTE NGN, 117 - Huawei IMS, 123 - NEC, 125 - WorldStone
# Number: 100, 102, 113, 114, 115, 116, 117, 123, 125
P424=100

# Allow Sync Phonebook via SIP Notify. 0 - No, 1 - Yes. Default is 1.
# Number: 0, 1
P26199=1
##############################################################################
##  Account 3 Settings                                                      ##
##############################################################################
#######################################################################
##  Account 3 General Settings                                       ##
#######################################################################
# Account Active. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P501=0

# Account Name
P517=

# SIP Server
P502=

# SIP User ID
P504=

# SIP Authentication ID
P505=

# SIP Authentication Password
P506=

# Voice Mail Access Number
P526=

# Name (Display name: John Doe)
P507=

# Tel URI. 0 - Disable, 1 - User=Phone, 2 - Enabled. Default value is 0
# Number: 0, 1, 2
P509=0
#######################################################################
##  Account 3 Network Settings                                       ##
#######################################################################
# Outbound Proxy
P503=

# Secondary Outbound Proxy
P2533=

# DNS Mode  0 - A Record, 1 - SRV, 2 - NAPTR/SRV. Default is 0
# Number: 0, 1, 2.
P508=0

# DNS SRV Fail-over Mode. 0 - Default, 1 - Saved one until DNS TTL, 2 - Saved one until no response. Defualt value is 1
# Number
P26240=0

# Register Before DNS SRV Fail-over. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P29295=0

# NAT Traversal. 0 - No, 1 - STUN, 2 - Keep-alive, 3 - UPnP, 4 - Auto, 5 - VPN. Default value is 2
# Number: 0, 1, 2, 3, 4, 5
P514=2

# Proxy-Require
P518=
#######################################################################
##  Account 3 SIP Settings                                           ##
#######################################################################
# SIP Registration. 0 - No, 1 - Yes. Default is 1
# Number: 0, 1
P510=1

# Unregister Before New Registration. 0 - No, 1 - Yes, 2 -  Instance . Default value is 0
# Number: 0, 1, 2
P511=0

# Register Expiration (m). In minutes. Default value is 60
# Number: 0 - 64800
P512=60

# Subscribe Expiration (m). Default is 60
# Number: 0 - 64800
P26251=60

# Re-register before Expiration (s). Default value is 0
# Number
P2530=0

# Registration Retry Wait Time(s). In seconds. Default value is 20
# Number: 1 - 3600
P571=20

# Local SIP Port. Default value is 5064
# Number: 5 - 65535
P513=5064

# SUBSCRIBE for MWI. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P515=0

# Enable OPTIONS Keep Alive. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P2597=0

# OPTIONS Keep Alive Interval(s). Default value is 30
# Number 
P2598=30

# OPTIONS Keep Alive Maximum Tries. Default value is 3
# Number 
P2599=3

# Enable Session Timer/ Session Expiration(s).  In seconds. Default value is 180 seconds.
# By default,  Session Timer is Enabled.  Session Timer is disabled if the value is 0.
# Number: 0 or 90 - 64800
P534=180

# Min-SE (s). Default value is 90 seconds
# Number: 5 - 65535
P527=90

# UAC Specify Refresher. 0 - Omit, 1 - UAC, 2 - UAS. Default value is 0
# Number: 0, 1, 2
P532=0

# UAS Specify Refresher. 1 - UAC, 2 - UAS. Default value is 1
# Number: 1, 2
P533=1

# Force INVITE (Always refresh with INVITE instead of UPDATE even when remote party supports UPDATE)
# 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P531=0

# Caller Request Timer (Request for timer when calling)
# 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1.
P528=0

# Callee Request Timer. Request for timer when called (i.e. if remote party supports timer but did not request for one)
# 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P529=0

# Force Timer (Still use timer when remote party does not support timer). 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P530=0

# Enable 100rel. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P535=0

# Use Privacy Header. 0 - Default, 1 - No, 2 - Yes. Default is 0
# Number: 0, 1, 2
P2538=0

# Use P-Preferred-Identity Header. 0 - Default, 1 - No, 2 - Yes. Default is 0
# Number: 0, 1, 2
P2539=0

# Use P-Access-Network-Info Header. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P26258=1

# Use P-Emergency-Info Header. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P26259=1

# Use MAC Header.  0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P26261=0

# SIP Transport. 0 - UDP, 1 - TCP, 2 - TLS. Default value is 0
# Number: 0, 1, 2
P548=0

# SIP URI Scheme When Using TLS
# 0 -sip, 1 - sips. Default value is 0.
# Number: 0, 1
P2529=0

# Use Actual Ephemeral Port in Contact with TCP/TLS
# 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P2531=0

# Support SIP Instance ID. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P589=1

# Add Auth Header On RE-REGISTER
# 0 - No, 1- Yes
P2559=0

# SIP T1 Timeout. RFC 3261 T1 value (RTT estimate)
# 50 - 0.5 sec, 100 - 1 sec, 200 - 2 sec. Default value is 50
# Number: 50, 100, 200
P540=50

# SIP T2 Interval. RFC 3261 T2 value. The maximum retransmit interval for non-INVITE requests and INVITE responses
# 200 - 2 sec, 400 - 4 sec, 800 - 8 sec. Default 400
# Number: 200, 400, 800
P541=400

# SIP Timer D Interval (Seconds)
# Number 0-64. Default value is 0
P2587=0

# Remove OBP from route. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P2505=0
#######################################################################
##  Account 3 Codec Settings                                         ##
#######################################################################
# Preferred Vocoder
# First codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 98 - iLBC, 123 -Opus. Default value is 0
# Number: 0, 2, 8, 9, 98, 123
P551=0

# Second codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 98 - iLBC, 123 -Opus. Default value is 8
# Number: 0, 2, 8, 9, 98, 123
P552=8

# Third codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 98 - iLBC, 123 -Opus. Default value is 9
# Number: 0, 2, 8, 9, 98, 123
P553=9

# Forth codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 98 - iLBC, 123 -Opus. Default value is 9
# Number: 0, 2, 8, 9, 98, 123
P554=9

# Fifth codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 98 - iLBC, 123 -Opus. Default value is 9
# Number: 0, 2, 8, 9, 98, 123
P555=9

# Sixth codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 123 - Opus. Default value is 9
# Number: 0, 8, 9, 2, 18, 98, 123
P556=9

# Seventh codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 123 - Opus. Default value is 9
# Number: 0, 8, 9, 2, 18, 98, 123
P557=9

# Eigth codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 123 - Opus. Default value is 9
# Number: 0, 8, 9, 2, 18, 98, 123
P558=9

# Codec Negotiation Priority. 0 - Caller, 1 - Callee. Default value is 1.
# Number: 0, 1
P29261=1

# Use First Matching Vocoder in 200OK SDP. 0 - No, 1 - Yes. The default value is 0.
# Number: 0, 1
P2548=0

# iLBC Frame Size. 0 - 20 ms, 1 - 30 ms. Default value is 1.
# Number: 0, 1
P595=1

#G726-32 ITU Payload. 0 - 2, 1 - Dynamic. Default value is 0.
# Number: 0, 1
P2569=0

#G726-32 Dynamic PT. Default value is 126.
# Number
P2565=126

#Opus Payload Type
P2585=123

# DTMF: in audio. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P2501=0

# DTMF: in RFC2833. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P2502=1

# DTMF: in SIP INFO. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P2503=0

# DTMF Payload Type. Default value is 101
# Number: 96 - 126
P596=101

# Enable Audio RED with FEC. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P26273=0

# Audio FEC Payload Type. Default value is 121
# Number: 96 - 126
P26274=121

# Audio RED Payload Type. Default value is 124
# Number: 96 - 126
P26275=124

# Silence Suppression. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P585=0

# Voice Frames per TX. Default valule is 2
# Number: 1 - 64
P586=2


# Preferred Video Codec. 99 - H.264. Default is 99.
P564=99

# Enable Video FEC. 0 - No, 1 - Yes. Default value is 1.
# Number: 0, 1
P2593=1

# Enable RFC5168 support. 0 - No, 1 - Yes. Default value is 1.
# Number: 0, 1
P578=1

# Video FEC Mode. 0 - 0, 1 - 1. Default value is 0.
# Number: 0, 1
P26222=0

# FEC Payload Type. Default value is 120.
P2594=120

# Packetization mode. 0 - Single NAL Unit Mode, 1 - Non-Interleaved Mode. Default value is 1.
# Number: 0, 1, 10
P26205=1

# H.264 Image Size. 9 - 720P, 1 - VGA, 5 - CIF, 4 - 4CIF, 0 - QVGA, 6 - QCIF. Default value is 9
# Number: 9, 1, 5, 4, 0, 6
P2507=9

# Use H.264 Constrained Profiles. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1
P26245=0

# H.264 Profile Type. 0 - Baseline Profile, 1 - Main Profile, 2 - High Profile, 3 - BP&MP&HP
# Number: 0, 1, 2, 3
P2562=0

# Video Bit Rate. 64 - 64 kbps, 96 - 96 kbps, 128 - 128 kbps, 160 - 160 kbps, 192 - 192 kbps
# 210 - 210 kbps, 256 - 256 kbps, 384 - 384 kbps, 512 - 512 kbps, 640 - 640 kbps, 768 - 768 kbps
# 1024 - 1024 kbps, 1280 - 1280 kbps, 1536 - 1536 kbps, 2048 - 2048 kbps. Default value is 2048.
# Number: 250, 500, 750
P2515=2048

# SDP Bandwidth Attribute. 0 - Standard, 1 - Media Level, 2 - Session Level, 3 - None. Default value is Media Level.
# Number: 0, 1, 2, 3
P2560=1

# H.264 Payload Type
P562=99

# Disable BFCP. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1
P26201=0

# Presentation H.264 Image Size. 10 - 1080P, 9 - 720P. Default value is 10.
# Number: 10, 9
P2576=10

# Presentation H.264 Profile Type. 0 - Baseline Profile, 1 - Main Profile, 2 - High Profile, 3 - BP&MP&HP
# Number: 0, 1, 2, 3
P2577=3

# Presentation Video Bit Rate. 512 - 512 kbps, 640 - 640 kbps, 768 - 768 kbps
# 1024 - 1024 kbps, 1280 - 1280 kbps, 1536 - 1536 kbps, 2048 - 2048 kbps. Default value is 1024.
# Number: 250, 500, 750
P2578=1024

# Presentation Video Frame Rate. 5 - 5 frames/second, 10 - 10 frames/second, 15 - 15 frames/second. Default value is 15.
# Number: 5, 10, 15
P26242=

# BFCP Transport Protocol. 0 - Automatic, 1 - UDP, 2 - TCP. Default value is 1.
# Number: 0, 1, 2
P26241=

# SRTP Mode. 0 - Disabled, 1 - Enabled but not forced, 2 - Enabled and forced. Default value is 0
# Number: 0, 1, 2
P543=0

# SRTP Key Length. 0 - AES 128&256 bit, 1 - AES 128 bit, 2 - AES 256 bit. Default value is 0
#Number:0, 1, 2
P2583=0

# Enable SRTP Key Life Time. 0 - No, 1 - Yes.
# Number: 0,1
P2563=0

# RTCP Destination
P2590=

# Symmetric RTP. 0 - No, 1 - Yes. Default value is 0
# Number:0, 1
P560=0

# RTP IP Filter. 0 - Disable, 1 - IP Only, 2 - IP and Port. Default value is 0
# Number:0, 1, 2
P26226=0

# RTP Timeout(s). Default is 0. If set to 0, the device would not hangup.
# number: 0 - 600
P29268=0
#######################################################################
##  Account 3 Call Settings                                          ##
#######################################################################
# Enable Video Call. 0 - Default, 1 - No, 2 - Yes. Default is 0
# Number: 0, 1, 2
P60243=0

# Start Video Automatically. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P2514=1

# Remote Video Request. 0 - Prompt, 1 - Accept, 2 - Deny. Default value is 0
# Number: 0, 1, 2
P2526=0

# Video Layout. 0 - Default, 1 - Full screen, 3 - Equal split screen, 2 - Only display remote screen
P2532=0

# Auto Answer. 0 - No, 1 - Yes, 2 - Enable Intercom/Paging. Default value is 0
# Number: 0, 1, 2
P525=0

# Play warning tone for Auto Answer Intercom. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P26272=1

# Intercom Barging. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P26219=1

# Auto Preview. 0 - No, 1 - Yes, 2 - Yes with Ringing. Default value is 0
# Number: 0, 1, 2
P29262=0

# Send Anonymous. 0 - No, 1 - Yes (caller ID will be blocked if set to Yes). Default value is 0
# Number: 0, 1
P521=0

# Anonymous Call Rejection. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P546=0

# Call Log. 0 - Log All, 1 - Log Incoming/Outgoing only (Missed Calls Not Recorded), 2 - Disable Call All. Default value is 0
# Number: 0, 1
P542=0

# Enable Call Features. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P520=0

# Enable Call Waiting. 0 - Default, 1 - No, 2 - Yes.
# Number: 0, 1, 2
P26263=0

# Mute on Answer Intercom Call. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
P26271=0

# Transfer on 3 way conference Hangup. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P2504=0

# Use # as Dial Key. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P592=1 

# Use # as Redial Key. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P29269=1

# DND Call Feature On.
# String
P2544=

# DND Call Feature Off.
# String
P2545=

# No Key Entry Timeout (s). Default value is 4
# Number: 1 - 15
P591=4

# Ring Timeout. Default value is 60 seconds
# Number: 10 - 300
P576=60

# Refer-To Use Target Contact. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P569=0

# RFC2543 Hold. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1 
P26262=1

# Dial Plan Prefix
# String
P519=

# Disable DialPlan. 0 - No Selection, 1 - Dial Page, 2 - Contact, 4 - Incoming Call History, 8 -  Outgoing Call History, 16 - MPK & Click2Dial. 
# If need to check multiple selections, add the specific values for each selections together. Default value is 0
# Number: 0-31
P2582=0

# Dial Plan. Default value is { x+ | \+x+ | *x+ | *xx*x+ | x+*x+*x+*x+ | x+*x+*x+*x+#x+ }
P559={ x+ | \+x+ | *x+ | *xx*x+ | x+*x+*x+*x+ | x+*x+*x+*x+#x+ }

# Caller ID Display. 0 - Auto, 1 - Disabled, 2 - From Header. The default value is 0.
# Number: 0, 1, 2, 3
P2524=0

# Account Ringtone. See ring tone options and value in the Ring Tone value table below
P523=content://settings/system/ringtone

# Ignore Alert-Info Header. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1
P26218=0

# Matching Incoming Caller ID. Matching Rule 1
# String
P1500=

# Matching Rule 1 Distinctive Ringtone. See ring tone options and value in the Ring Tone value table below
# String
P1501=content://settings/system/ringtone

# Matching Incoming Caller ID. Matching Rule 2
# String
P1502=

# Matching Rule 2 Distinctive Ringtone. See ring tone options and value in the Ring Tone value table below
# String
P1503=content://settings/system/ringtone 

# Matching Incoming Caller ID. Matching Rule 3
# String
P1504=

# Matching Rule 3 Distinctive Ringtone. See ring tone options and value in the Ring Tone value table below
# String
P1505=content://settings/system/ringtone

############Ring Tone Value Table###############
# Web GUI Option                            Value
# Use System Ring tone                      content://settings/system/ringtone 
# Andromeda					/system/media/audio/ringtones/ANDROMEDA.ogg
# Aquila					/system/media/audio/ringtones/Aquila.ogg
# Argo Navis					/system/media/audio/ringtones/ArgoNavis.ogg
# Atria					/system/media/audio/ringtones/Atria.ogg
# Backroad					/system/media/audio/ringtones/Backroad.ogg
# Beat Plucker					/system/media/audio/ringtones/BeatPlucker.ogg
# Bell Phone					/system/media/audio/ringtones/Ring_Classic_02.ogg
# Bentley Dubs					/system/media/audio/ringtones/BentleyDubs.ogg
# Big Easy					/system/media/audio/ringtones/Big_Easy.ogg
# Bird Loop					/system/media/audio/ringtones/BirdLoop.ogg
# Bollywood					/system/media/audio/ringtones/Bollywood.ogg
# Boötes					/system/media/audio/ringtones/BOOTES.ogg
# Bus' a Move					/system/media/audio/ringtones/BussaMove.ogg
# Cairo					/system/media/audio/ringtones/Cairo.ogg
# Calypso Steel					/system/media/audio/ringtones/Calypso_Steel.ogg
# Canis Major					/system/media/audio/ringtones/CANISMAJOR.ogg
# Caribbean Ice					/system/media/audio/ringtones/CaribbeanIce.ogg
# Carina					/system/media/audio/ringtones/Carina.ogg
# Cassiopeia					/system/media/audio/ringtones/CASSIOPEIA.ogg
# Centaurus					/system/media/audio/ringtones/Centaurus.ogg
# Champagne Edition					/system/media/audio/ringtones/Champagne_Edition.ogg
# Chimey Phone					/system/media/audio/ringtones/Ring_Synth_02.ogg
# Club Cubano					/system/media/audio/ringtones/Club_Cubano.ogg
# Crayon Rock					/system/media/audio/ringtones/CrayonRock.ogg
# Crazy Dream					/system/media/audio/ringtones/CrazyDream.ogg
# Curve Ball Blend					/system/media/audio/ringtones/CurveBall.ogg
# Cygnus					/system/media/audio/ringtones/Cygnus.ogg
# Dancin' Fool					/system/media/audio/ringtones/DancinFool.ogg
# Digital Phone					/system/media/audio/ringtones/Ring_Digital_02.ogg
# Ding					/system/media/audio/ringtones/Ding.ogg
# DingDong					/system/media/audio/ringtones/DingDong.wav
# Don' Mess Wiv It					/system/media/audio/ringtones/DonMessWivIt.ogg
# Draco					/system/media/audio/ringtones/Draco.ogg
# Dream Theme					/system/media/audio/ringtones/DreamTheme.ogg
# Eastern Sky					/system/media/audio/ringtones/Eastern_Sky.ogg
# Enter the Nexus					/system/media/audio/ringtones/Enter_the_Nexus.ogg
# Eridani					/system/media/audio/ringtones/Eridani.ogg
# Ether Shake					/system/media/audio/ringtones/EtherShake.ogg
# Flutey Phone					/system/media/audio/ringtones/Ring_Synth_04.ogg
# Free Flight					/system/media/audio/ringtones/FreeFlight.ogg
# Friendly Ghost					/system/media/audio/ringtones/FriendlyGhost.ogg
# Funk Y'all					/system/media/audio/ringtones/Funk_Yall.ogg
# Game Over Guitar					/system/media/audio/ringtones/GameOverGuitar.ogg
# Gimme Mo' Town					/system/media/audio/ringtones/Gimme_Mo_Town.ogg
# Girtab					/system/media/audio/ringtones/Girtab.ogg
# Glacial Groove					/system/media/audio/ringtones/Glacial_Groove.ogg
# Growl					/system/media/audio/ringtones/Growl.ogg
# Halfway Home					/system/media/audio/ringtones/HalfwayHome.ogg
# Hydra					/system/media/audio/ringtones/Hydra.ogg
# Insert Coin					/system/media/audio/ringtones/InsertCoin.ogg
# Kuma					/system/media/audio/ringtones/Kuma.ogg
# Loopy Lounge					/system/media/audio/ringtones/LoopyLounge.ogg
# Love Flute					/system/media/audio/ringtones/LoveFlute.ogg
# Lyra					/system/media/audio/ringtones/Lyra.ogg
# Machina					/system/media/audio/ringtones/Machina.ogg
# Medieval Jaunt					/system/media/audio/ringtones/MidEvilJaunt.ogg
# Mildly Alarming					/system/media/audio/ringtones/MildlyAlarming.ogg
# Nairobi					/system/media/audio/ringtones/Nairobi.ogg
# Nassau					/system/media/audio/ringtones/Nassau.ogg
# New Player					/system/media/audio/ringtones/NewPlayer.ogg
# No Limits					/system/media/audio/ringtones/No_Limits.ogg
# Noisey One					/system/media/audio/ringtones/Noises1.ogg
# Organ Dub					/system/media/audio/ringtones/OrganDub.ogg
# Orion					/system/media/audio/ringtones/Orion.ogg
# Paradise Island					/system/media/audio/ringtones/Paradise_Island.ogg
# Pegasus					/system/media/audio/ringtones/Pegasus.ogg
# Perseus					/system/media/audio/ringtones/PERSEUS.ogg
# Playa					/system/media/audio/ringtones/Playa.ogg
# Pyxis					/system/media/audio/ringtones/Pyxis.ogg
# Rasalas					/system/media/audio/ringtones/Rasalas.ogg
# Revelation					/system/media/audio/ringtones/Revelation.ogg
# Rigel					/system/media/audio/ringtones/Rigel.ogg
# Road Trip					/system/media/audio/ringtones/Road_Trip.ogg
# Romancing The Tone					/system/media/audio/ringtones/RomancingTheTone.ogg
# Safari					/system/media/audio/ringtones/Safari.ogg
# Savannah					/system/media/audio/ringtones/Savannah.ogg
# Scarabaeus					/system/media/audio/ringtones/Scarabaeus.ogg
# Sceptrum					/system/media/audio/ringtones/Sceptrum.ogg
# Seville					/system/media/audio/ringtones/Seville.ogg
# She's All That					/system/media/audio/ringtones/Shes_All_That.ogg
# Silky Way					/system/media/audio/ringtones/SilkyWay.ogg
# Sitar Versus Sitar					/system/media/audio/ringtones/SitarVsSitar.ogg
# Solarium					/system/media/audio/ringtones/Solarium.ogg
# Springy Jalopy					/system/media/audio/ringtones/SpringyJalopy.ogg
# Steppin' Out					/system/media/audio/ringtones/Steppin_Out.ogg
# Terminated					/system/media/audio/ringtones/Terminated.ogg
# Terrible Twos					/system/media/audio/ringtones/Noises2.ogg
# Testudo					/system/media/audio/ringtones/Testudo.ogg
# Themos					/system/media/audio/ringtones/Themos.ogg
# Third Eye					/system/media/audio/ringtones/Third_Eye.ogg
# Thriller Three					/system/media/audio/ringtones/Noises3.ogg
# Thunderfoot					/system/media/audio/ringtones/Thunderfoot.ogg
# Twirl Away					/system/media/audio/ringtones/TwirlAway.ogg
# Ursa Minor					/system/media/audio/ringtones/URSAMINOR.ogg
# UrsaMinor					/system/media/audio/ringtones/UrsaMinor.ogg
# Very Alarmed					/system/media/audio/ringtones/VeryAlarmed.ogg
# Vespa					/system/media/audio/ringtones/Vespa.ogg
# World					/system/media/audio/ringtones/World.ogg
# Zeta					/system/media/audio/ringtones/Zeta.ogg
# bellcore-dr1					/system/media/audio/ringtones/bellcore-dr1.ogg
# bellcore-dr2					/system/media/audio/ringtones/bellcore-dr2.ogg
# bellcore-dr3					/system/media/audio/ringtones/bellcore-dr3.ogg
# bellcore-dr4					/system/media/audio/ringtones/bellcore-dr4.ogg
# bellcore-dr5					/system/media/audio/ringtones/bellcore-dr5.ogg
# speaker					/system/media/audio/ringtones/speaker.wav
#######################################################################
##  Account 3 Advanced Settings                                      ##
#######################################################################
# Check Domain Certificates. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P2511=0

# Validate Certificate Chain. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P2567=0

# Validate Incoming SIP Messages. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P2506=0

# Allow Unsolicited REFER. 0 - Disabled, 1 - Enabled, 2 - Enabled/Force Auth. Default value is 0.
# Number: 0, 1, 2
P26223=0

# Only Accept SIP Requests from Known Servers. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P2547=0

# Check SIP User ID for Incoming INVITE. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P549=0

# Allow SIP Reset. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P26215=0

# Authenticate Incoming INVITE. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P2546=0

# SIP Realm Used for Challenge INVITE & NOTIFY.
# String
P26221=


# Enable Local MOH. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P2557=0

# Enable Local MOH. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
# 2357=0

# Virtual Account Group. -1 - Default,  0 - Virtual Account Group 1, 1 - Virtual Account Group 2, 2 - Virtual Account Group 3
# 3 - Virtual Account Group 4, 4 - Virtual Account Group 5, 5 - Virtual Account Group 6, 6 - Virtual Account Group 7, 7 - Virtual Account Group 8
# 8 - Virtual Account Group 9, 9 - Virtual Account Group 10, 10 - Virtual Account Group 11, 11 - Virtual Account Group 12, 12 - Virtual Account Group 13
# 13 - Virtual Account Group 14, 14 - Virtual Account Group 15, 15 - Virtual Account Group 16. Default value is -1.
# Number: -1 - 15 
P2591=-1

# Special Feature. Default value is 100
# 100 - Standard, 102 - Broadsoft, 113 - China Mobile
# 114 - ZTE IMS, 115 - Mobotix, 116 - ZTE NGN, 117 - Huawei IMS, 123 - NEC, 125 - WorldStone
# Number: 100, 102, 113, 114, 115, 116, 117, 123, 125
P524=100

# Allow Sync Phonebook via SIP Notify. 0 - No, 1 - Yes. Default is 1.
# Number: 0, 1
P26299=1
##############################################################################
##  Account 4 Settings                                                      ##
##############################################################################
#######################################################################
##  Account 4 General Settings                                       ##
#######################################################################
# Account Active. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P601=0

# Account Name
P617=

# SIP Server
P602=

# SIP User ID
P604=

# SIP Authentication ID
P605=

# SIP Authentication Password
P606=

# Voice Mail Access Number
P626=

# Name (Display Name, e.g., John Doe)
P607=

# Tel URI. 0 - Disable, 1 - User=Phone, 2 - Enabled. Default value is 0
# Number: 0, 1, 2
P609=0
#######################################################################
##  Account 4 Network Settings                                       ##
#######################################################################
# Outbound Proxy
P603=

# Secondary Outbound Proxy
P2633=

# DNS Mode. 0 - A Record, 1 - SRV, 2 - NAPTR/SRV. Default value is 0
# Number: 0, 1, 2
P608=0

# DNS SRV Fail-over Mode. 0 - Default, 1 - Saved one until DNS TTL, 2 - Saved one until no response. Defualt value is 1
# Number
P26340=0

# Register Before DNS SRV Fail-over. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P29395=0

# NAT Traversal. 0 - NAT No, 1 - STUN, 2 - Keep-alive, 3 - UPnP, 4 - Auto, 5 - VPN. Default value is 2
# Number: 0, 1, 2, 3, 4, 5
P614=2

# Proxy-Require
P618=
#######################################################################
##  Account 4 SIP Settings                                           ##
#######################################################################
# SIP Registration. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P610=1

# Unregister Before New Registration. 0 - No, 1 - Yes, 2 -  Instance . Default value is 0
# Number: 0, 1, 2
P611=0

# Register Expiration (m). In minutes. Default value is 60
# Number: 0 - 64800
P612=60

# Subscribe Expiration (m). Default is 60
# Number: 0 - 64800
P26351=60

# Re-register before Expiration (s). Default value is 0
# Number
P2630=0

# Registration Retry Wait Time(s). In seconds. Default value is 20
# Number: 1 - 3600
P671=20

# Local SIP Port. Default value is 5066
# Number: 5 - 65535
P613=5066

# SUBSCRIBE For MWI. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P615=0

# Enable OPTIONS Keep Alive. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P2697=0

# OPTIONS Keep Alive Interval(s). Default value is 30
# Number 
P2698=30

# OPTIONS Keep Alive Maximum Tries. Default value is 3
# Number 
P2699=3

# Enable Session Timer/ Session Expiration(s).  In seconds. Default value is 180 seconds.
# By default,  Session Timer is Enabled.  Session Timer is disabled if the value is 0.
# Number: 0 or 90 - 64800
P634=180

# Min-SE (s). Default value is 90 seconds
# Number: 90 - 64800
P627=90

# UAC Specify Refresher. 0 - Omit, 1 - UAC, 2 - UAS. Default value is 0
# Number: 0, 1, 2
P632=0

# UAS Specify Refresher. 1 - UAC, 2 - UAS. Default value is 1
# Number: 1, 2
P633=1

# Force INVITE. Always refresh with INVITE instead of UPDATE even when remote party supports UPDATE
# 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P631=0

# Caller Request Timer. Request for timer when calling. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P628=0

# Callee Request Timer. Request for timer when being called (i.e., if remote party supports timer but did not request for one)
# 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P629=0

# Force Timer. Still use timer when remote party does not support timer
# 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P630=0

# Enable 100rel. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P635=0

# Use Privacy Header. 0 - Default, 1 - No, 2 - Yes. Default is 0
# Number: 0, 1, 2
P2638=0

# Use P-Preferred-Identity Header
# 0 - Default, 1 - No, 2 - Yes. Default is 0
# Number: 0, 1, 2
P2639=0

# Use P-Access-Network-Info Header. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P26358=1

# Use P-Emergency-Info Header. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P26359=1

# Use MAC Header.  0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P26361=0

# SIP Transport. 0 - UDP , 1 - TCP, 2 - TLS. Default value is 0
# Number: 0, 1, 2
P648=0

# SIP URI Scheme When Using TLS
# 0 -sip, 1 - sips. Default value is 0.
# Number: 0, 1
P2629=0

# Use Actual Ephemeral Port in Contact with TCP/TLS
# 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P2631=0

# Support SIP Instance ID. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P689=1

# Add Auth Header On RE-REGISTER
# 0 - No, 1- Yes
P2659=0

# SIP T1 Timeout. RFC 3261 T1 value (RTT estimate)
# 50 - 0.5 sec, 100 - 1 sec, 200 - 2 sec. Default value is 50
# Number: 50, 100, 200
P640=50

# SIP T2 Interval. RFC 3261 T2 value. The maximum retransmit interval for non-INVITE requests and INVITE responses
# 200 - 2 sec, 400 - 4 sec, 800 - 8 sec. Default value is 400
# Number: 200, 400, 800
P641=400

# SIP Timer D Interval (Seconds)
# Number 0-64. Default value is 0
P2687=0

# Remove OBP from route. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P2605=0
#######################################################################
##  Account 4 Codec Settings                                         ##
#######################################################################
# Preferred Vocoder
# First codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 98 - iLBC, 128 - Opus . Default value is 0
# Number: 0, 2, 8, 9, 98, 128
P651=0

# Second codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 98 - iLBC, 128 - Opus. Default value is 8
# Number: 0, 2, 8, 9, 98, 128
P652=8

# Third codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 98 - iLBC, 128 - Opus. Default value is 9
# Number: 0, 2, 8, 9, 98, 128
P653=9

# Forth codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 98 - iLBC, 128 - Opus. Default value is 9
# Number: 0, 2, 8, 9, 98, 128
P654=9

# Fifth codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 98 - iLBC, 128 - Opus. Default value is 9
# Number: 0, 2, 8, 9, 98, 128
P655=9

# Sixth codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 123 - Opus. Default value is 9
# Number: 0, 8, 9, 2, 18, 98, 123
P656=9

# Seventh codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 123 - Opus. Default value is 9
# Number: 0, 8, 9, 2, 18, 98, 123
P657=9

# Eigth codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 123 - Opus. Default value is 9
# Number: 0, 8, 9, 2, 18, 98, 123
P658=9

# Codec Negotiation Priority. 0 - Caller, 1 - Callee. Default value is 1.
# Number: 0, 1
P29361=1

# Use First Matching Vocoder in 200OK SDP. 0 - No, 1 - Yes. The default value is 0.
# Number: 0, 1
P2648=0

# iLBC Frame Size. 0 - 20 ms, 1 - 30 ms. Default value is 1.
# Number: 0, 1
P695=1

# G726-32 ITU Payload. 0 - 2, 1 - Dynamic. Default value is 0.
# Number: 0, 1
P2669=0

# G726-32 Dynamic PT. Default value is 126.
# Number
P2665=126

# Opus Payload Type
P2685=123

# DTMF: in audio. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P2601=0

# DTMF: via RFC2833. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P2602=1

# DTMF: via SIP INFO. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P2603=0

# DTMF Payload Type. Default value is 101
# Number: 96 - 126
P696=101

# Enable Audio RED with FEC. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P26373=0

# Audio FEC Payload Type. Default value is 121
# Number: 96 - 126
P26374=121

# Audio RED Payload Type. Default value is 124
# Number: 96 - 126
P26375=124

# Silence Suppression. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P685=0

# Voice Frames per TX. Default value is 2
# Number: 1 - 64
P686=2

# Preferred Video Codec. 99 - H.264. Default is 99.
P664=99

# Enable Video FEC. 0 - No, 1 - Yes. Default value is 1.
# Number: 0, 1
P2693=1

# Enable RFC5168 support. 0 - No, 1 - Yes. Default value is 1.
# Number: 0, 1
P678=1

# Video FEC Mode. 0 - 0, 1 - 1. Default value is 0.
# Number: 0, 1
P26322=0

# FEC Payload Type. Default value is 120.
P2694=120

# Packetization mode. 0 - Single NAL Unit Mode, 1 - Non-Interleaved Mode. Default value is 1.
# Number: 0, 1, 10
P26305=1

# H.264 Image Size. 9 - 720P, 1 - VGA, 5 - CIF, 4 - 4CIF, 0 - QVGA, 6 - QCIF. Default value is 9
# Number: 9, 1, 5, 4, 0, 6
P2607=9

# Use H.264 Constrained Profiles. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1
P26345=0

# H.264 Profile Type. 0 - Baseline Profile, 1 - Main Profile, 2 - High Profile, 3 - BP&MP&HP
# Number: 0, 1, 2, 3
P2662=0

# Video Bit Rate. 64 - 64 kbps, 96 - 96 kbps, 128 - 128 kbps, 160 - 160 kbps, 192 - 192 kbps
# 210 - 210 kbps, 256 - 256 kbps, 384 - 384 kbps, 512 - 512 kbps, 640 - 640 kbps, 768 - 768 kbps
# 1024 - 1024 kbps, 1280 - 1280 kbps, 1536 - 1536 kbps, 2048 - 2048 kbps. Default value is 2048.
# Number: 250, 500, 750
P2615=2048

# SDP Bandwidth Attribute. 0 - Standard, 1 - Media Level, 2 - Session Level, 3 - None. Default value is Media Level.
# Number: 0, 1, 2, 3
P2660=1

# H.264 Payload Type
P662=99

# Disable BFCP. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1
P26301=0

# Presentation H.264 Image Size. 10 - 1080P, 9 - 720P. Default value is 10.
# Number: 10, 9
P2676=10

# Presentation H.264 Profile Type. 0 - Baseline Profile, 1 - Main Profile, 2 - High Profile, 3 - BP&MP&HP
# Number: 0, 1, 2, 3
P2677=3

# Presentation Video Bit Rate. 512 - 512 kbps, 640 - 640 kbps, 768 - 768 kbps
# 1024 - 1024 kbps, 1280 - 1280 kbps, 1536 - 1536 kbps, 2048 - 2048 kbps. Default value is 1024.
# Number: 250, 500, 750
P2678=1024

# Presentation Video Frame Rate. 5 - 5 frames/second, 10 - 10 frames/second, 15 - 15 frames/second. Default value is 15.
# Number: 5, 10, 15
P26342=

# BFCP Transport Protocol. 0 - Automatic, 1 - UDP, 2 - TCP. Default value is 1.
# Number: 0, 1, 2
P26341=

# SRTP Mode. 0 - Disabled, 1 - Enabled but not forced, 2 - Enabled and forced. Default value is 0
# Number: 0, 1, 2
P643=0

# SRTP Key Length. 0 - AES 128&256 bit, 1 - AES 128 bit, 2 - AES 256 bit. Default value is 0
#Number:0, 1, 2
P2683=0 

# Enable SRTP Key Life Time. 0 - No, 1 - Yes.
# Number: 0,1
P2663=0

# RTCP Destination
P2690=

# Symmetric RTP. 0 - No, 1 - Yes. Default value is 0
# Number:0, 1
P660=0

# RTP IP Filter. 0 - Disable, 1 - IP Only, 2 - IP and Port. Default value is 0
# Number:0, 1, 2
P26326=0

# RTP Timeout(s). Default is 0. If set to 0, the device would not hangup.
# number: 0 - 600
P29368=0
#######################################################################
##  Account 4 Call Settings                                          ##
#######################################################################
# Enable Video Call. 0 - Default, 1 - No, 2 - Yes. Default is 0
# Number: 0, 1, 2
P60343=0

# Start Video Automatically. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P2614=1

# Remote Video Request. 0 - Prompt, 1 - Accept, 2 - Deny. Default value is 0
# Number: 0, 1, 2
P2626=0

# Video Layout. 0 - Default, 1 - Full screen, 3 - Equal split screen, 2 - Only display remote screen
P2632=0

# Auto Answer. 0 - No, 1 - Yes, 2 - Enable Intercom/Paging. Default value is 0
# Number: 0, 1, 2
P625=0

# Play warning tone for Auto Answer Intercom. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P26372=1

# Intercom Barging. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P26319=1

# Auto Preview. 0 - No, 1 - Yes, 2 - Yes with Ringing. Default value is 0
# Number: 0, 1, 2
P29362=0

# Send Anonymous. 0 - No, 1 - Yes (caller ID will be blocked if set to Yes). Default value is 0
# Number: 0, 1
P621=0

# Anonymous Call Rejection. 0 - No,  1 - Yes. Default value is 0
# Number: 0, 1
P646=0

# Call Log. 0 - Log All, 1 - Log Incoming/Outgoing only (Missed Calls Not Recorded), 2 - Disable All. Default value is 0
# Number: 0, 1, 2
P642=0

# Enable Call Features. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P620=0

# Enable Call Waiting. 0 - Default, 1 - No, 2 - Yes.
# Number: 0, 1, 2
P26363=0

# Mute on Answer Intercom Call. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
P26371=0

# Transfer on 3 way conference Hangup. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P2604=0

# Use # as Dial Key. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P692=1

# Use # as Redial Key. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P29369=1

# DND Call Feature On.
# String
P2644=

# DND Call Feature Off.
# String
P2645=

# No Key Entry Timeout (s). Default value is 4
# Number: 1 - 15
P691=4

# Ring Timeout (s). Default value is 60
# Number: 10 - 300
P676=60

# Refer-To Use Target Contact. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P669=0

# RFC2543 Hold. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1 
P26362=1

# Dial Plan Prefix
# String
P619=

# Disable DialPlan. 0 - No Selection, 1 - Dial Page, 2 - Contact, 4 - Incoming Call History, 8 -  Outgoing Call History, 16 - MPK & Click2Dial. 
# If need to check multiple selections, add the specific values for each selections together. Default value is 0
# Number: 0-31
P2682=0

# Dial Plan. Default value is { x+ | \+x+ | *x+ | *xx*x+ | x+*x+*x+*x+ | x+*x+*x+*x+#x+ }
P659={ x+ | \+x+ | *x+ | *xx*x+ | x+*x+*x+*x+ | x+*x+*x+*x+#x+ }

# Caller ID Display. 0 - Auto, 1 - Disabled, 2 - From Header. The default value is 0.
# Number: 0, 1, 2, 3
P2624=0

# Account Ringtone. See ring tone options and value in the Ring Tone value table below
P623=content://settings/system/ringtone

# Ignore Alert-Info Header. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1
P26318=0

# Matching Incoming Caller ID. Matching Rule 1
# String
P1506=

# Matching Rule 1 Distinctive Ringtone. See ring tone options and value in the Ring Tone value table below
# String
P1507=content://settings/system/ringtone

# Matching Incoming Caller ID. Matching Rule 2
# String
P1508=

# Matching Rule 2 Distinctive Ringtone. See ring tone options and value in the Ring Tone value table below
# String
P1509=content://settings/system/ringtone

# Matching Incoming Caller ID. Matching Rule 3
# String
P1510=

# Matching Rule 3 Distinctive Ringtone. See ring tone options and value in the Ring Tone value table below
# String
P1511=content://settings/system/ringtone

############Ring Tone Value Table###############
# Web GUI Option                            Value
# Use System Ring tone                      content://settings/system/ringtone 
# Andromeda					/system/media/audio/ringtones/ANDROMEDA.ogg
# Aquila					/system/media/audio/ringtones/Aquila.ogg
# Argo Navis					/system/media/audio/ringtones/ArgoNavis.ogg
# Atria					/system/media/audio/ringtones/Atria.ogg
# Backroad					/system/media/audio/ringtones/Backroad.ogg
# Beat Plucker					/system/media/audio/ringtones/BeatPlucker.ogg
# Bell Phone					/system/media/audio/ringtones/Ring_Classic_02.ogg
# Bentley Dubs					/system/media/audio/ringtones/BentleyDubs.ogg
# Big Easy					/system/media/audio/ringtones/Big_Easy.ogg
# Bird Loop					/system/media/audio/ringtones/BirdLoop.ogg
# Bollywood					/system/media/audio/ringtones/Bollywood.ogg
# Boötes					/system/media/audio/ringtones/BOOTES.ogg
# Bus' a Move					/system/media/audio/ringtones/BussaMove.ogg
# Cairo					/system/media/audio/ringtones/Cairo.ogg
# Calypso Steel					/system/media/audio/ringtones/Calypso_Steel.ogg
# Canis Major					/system/media/audio/ringtones/CANISMAJOR.ogg
# Caribbean Ice					/system/media/audio/ringtones/CaribbeanIce.ogg
# Carina					/system/media/audio/ringtones/Carina.ogg
# Cassiopeia					/system/media/audio/ringtones/CASSIOPEIA.ogg
# Centaurus					/system/media/audio/ringtones/Centaurus.ogg
# Champagne Edition					/system/media/audio/ringtones/Champagne_Edition.ogg
# Chimey Phone					/system/media/audio/ringtones/Ring_Synth_02.ogg
# Club Cubano					/system/media/audio/ringtones/Club_Cubano.ogg
# Crayon Rock					/system/media/audio/ringtones/CrayonRock.ogg
# Crazy Dream					/system/media/audio/ringtones/CrazyDream.ogg
# Curve Ball Blend					/system/media/audio/ringtones/CurveBall.ogg
# Cygnus					/system/media/audio/ringtones/Cygnus.ogg
# Dancin' Fool					/system/media/audio/ringtones/DancinFool.ogg
# Digital Phone					/system/media/audio/ringtones/Ring_Digital_02.ogg
# Ding					/system/media/audio/ringtones/Ding.ogg
# DingDong					/system/media/audio/ringtones/DingDong.wav
# Don' Mess Wiv It					/system/media/audio/ringtones/DonMessWivIt.ogg
# Draco					/system/media/audio/ringtones/Draco.ogg
# Dream Theme					/system/media/audio/ringtones/DreamTheme.ogg
# Eastern Sky					/system/media/audio/ringtones/Eastern_Sky.ogg
# Enter the Nexus					/system/media/audio/ringtones/Enter_the_Nexus.ogg
# Eridani					/system/media/audio/ringtones/Eridani.ogg
# Ether Shake					/system/media/audio/ringtones/EtherShake.ogg
# Flutey Phone					/system/media/audio/ringtones/Ring_Synth_04.ogg
# Free Flight					/system/media/audio/ringtones/FreeFlight.ogg
# Friendly Ghost					/system/media/audio/ringtones/FriendlyGhost.ogg
# Funk Y'all					/system/media/audio/ringtones/Funk_Yall.ogg
# Game Over Guitar					/system/media/audio/ringtones/GameOverGuitar.ogg
# Gimme Mo' Town					/system/media/audio/ringtones/Gimme_Mo_Town.ogg
# Girtab					/system/media/audio/ringtones/Girtab.ogg
# Glacial Groove					/system/media/audio/ringtones/Glacial_Groove.ogg
# Growl					/system/media/audio/ringtones/Growl.ogg
# Halfway Home					/system/media/audio/ringtones/HalfwayHome.ogg
# Hydra					/system/media/audio/ringtones/Hydra.ogg
# Insert Coin					/system/media/audio/ringtones/InsertCoin.ogg
# Kuma					/system/media/audio/ringtones/Kuma.ogg
# Loopy Lounge					/system/media/audio/ringtones/LoopyLounge.ogg
# Love Flute					/system/media/audio/ringtones/LoveFlute.ogg
# Lyra					/system/media/audio/ringtones/Lyra.ogg
# Machina					/system/media/audio/ringtones/Machina.ogg
# Medieval Jaunt					/system/media/audio/ringtones/MidEvilJaunt.ogg
# Mildly Alarming					/system/media/audio/ringtones/MildlyAlarming.ogg
# Nairobi					/system/media/audio/ringtones/Nairobi.ogg
# Nassau					/system/media/audio/ringtones/Nassau.ogg
# New Player					/system/media/audio/ringtones/NewPlayer.ogg
# No Limits					/system/media/audio/ringtones/No_Limits.ogg
# Noisey One					/system/media/audio/ringtones/Noises1.ogg
# Organ Dub					/system/media/audio/ringtones/OrganDub.ogg
# Orion					/system/media/audio/ringtones/Orion.ogg
# Paradise Island					/system/media/audio/ringtones/Paradise_Island.ogg
# Pegasus					/system/media/audio/ringtones/Pegasus.ogg
# Perseus					/system/media/audio/ringtones/PERSEUS.ogg
# Playa					/system/media/audio/ringtones/Playa.ogg
# Pyxis					/system/media/audio/ringtones/Pyxis.ogg
# Rasalas					/system/media/audio/ringtones/Rasalas.ogg
# Revelation					/system/media/audio/ringtones/Revelation.ogg
# Rigel					/system/media/audio/ringtones/Rigel.ogg
# Road Trip					/system/media/audio/ringtones/Road_Trip.ogg
# Romancing The Tone					/system/media/audio/ringtones/RomancingTheTone.ogg
# Safari					/system/media/audio/ringtones/Safari.ogg
# Savannah					/system/media/audio/ringtones/Savannah.ogg
# Scarabaeus					/system/media/audio/ringtones/Scarabaeus.ogg
# Sceptrum					/system/media/audio/ringtones/Sceptrum.ogg
# Seville					/system/media/audio/ringtones/Seville.ogg
# She's All That					/system/media/audio/ringtones/Shes_All_That.ogg
# Silky Way					/system/media/audio/ringtones/SilkyWay.ogg
# Sitar Versus Sitar					/system/media/audio/ringtones/SitarVsSitar.ogg
# Solarium					/system/media/audio/ringtones/Solarium.ogg
# Springy Jalopy					/system/media/audio/ringtones/SpringyJalopy.ogg
# Steppin' Out					/system/media/audio/ringtones/Steppin_Out.ogg
# Terminated					/system/media/audio/ringtones/Terminated.ogg
# Terrible Twos					/system/media/audio/ringtones/Noises2.ogg
# Testudo					/system/media/audio/ringtones/Testudo.ogg
# Themos					/system/media/audio/ringtones/Themos.ogg
# Third Eye					/system/media/audio/ringtones/Third_Eye.ogg
# Thriller Three					/system/media/audio/ringtones/Noises3.ogg
# Thunderfoot					/system/media/audio/ringtones/Thunderfoot.ogg
# Twirl Away					/system/media/audio/ringtones/TwirlAway.ogg
# Ursa Minor					/system/media/audio/ringtones/URSAMINOR.ogg
# UrsaMinor					/system/media/audio/ringtones/UrsaMinor.ogg
# Very Alarmed					/system/media/audio/ringtones/VeryAlarmed.ogg
# Vespa					/system/media/audio/ringtones/Vespa.ogg
# World					/system/media/audio/ringtones/World.ogg
# Zeta					/system/media/audio/ringtones/Zeta.ogg
# bellcore-dr1					/system/media/audio/ringtones/bellcore-dr1.ogg
# bellcore-dr2					/system/media/audio/ringtones/bellcore-dr2.ogg
# bellcore-dr3					/system/media/audio/ringtones/bellcore-dr3.ogg
# bellcore-dr4					/system/media/audio/ringtones/bellcore-dr4.ogg
# bellcore-dr5					/system/media/audio/ringtones/bellcore-dr5.ogg
# speaker					/system/media/audio/ringtones/speaker.wav
#######################################################################
##  Account 4 Advanced Settings                                      ##
#######################################################################
# Check Domain Certificates. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P2611=0

# Validate Certificate Chain. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P2667=0

# Validate Incoming SIP Messages. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P2606=0

# Allow Unsolicited REFER. 0 - Disabled, 1 - Enabled, 2 - Enabled/Force Auth. Default value is 0.
# Number: 0, 1, 2
P26323=0

# Only Accept SIP Requests from Known Servers. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P2647=0

# Check SIP User ID for Incoming INVITE. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P649=0

# Allow SIP Reset. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P26315=0

# Authenticate Incoming INVITE. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P2646=0

# SIP Realm Used for Challenge INVITE & NOTIFY.
# String
P26321=

# Enable Local MOH. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P2657=0

# Virtual Account Group. -1 - Default,  0 - Virtual Account Group 1, 1 - Virtual Account Group 2, 2 - Virtual Account Group 3
# 3 - Virtual Account Group 4, 4 - Virtual Account Group 5, 5 - Virtual Account Group 6, 6 - Virtual Account Group 7, 7 - Virtual Account Group 8
# 8 - Virtual Account Group 9, 9 - Virtual Account Group 10, 10 - Virtual Account Group 11, 11 - Virtual Account Group 12, 12 - Virtual Account Group 13
# 13 - Virtual Account Group 14, 14 - Virtual Account Group 15, 15 - Virtual Account Group 16. Default value is -1.
# Number: -1 - 15 
P2691=-1

# Special Feature. Default value is 100
# 100 - Standard, 102 - Broadsoft, 113 - China Mobile
# 114 - ZTE IMS, 115 - Mobotix, 116 - ZTE NGN, 117 - Huawei IMS, 123 - NEC, 125 - WorldStone
# Number: 100, 102, 113, 114, 115, 116, 117, 123, 125
P624=100

# Allow Sync Phonebook via SIP Notify. 0 - No, 1 - Yes. Default is 1.
# Number: 0, 1
P26399=1
##############################################################################
##  Account 5 Settings                                                      ##
##############################################################################
#######################################################################
##  Account 5 General Settings                                       ##
#######################################################################
# Account Active. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P1701=0

# Account Name
P1717=

# SIP Server
P1702=

# SIP User ID
P1704=

# SIP Authentication ID
P1705=

# SIP Authentication Password
P1706=

# Voice Mail Access Number
P1726=

# Name (Display name, e.g., John Doe)
P1707=

# Tel URI. 0 - Disabled, 1 - User=Phone, 2 - Enabled. Default value is 0
# Number: 0, 1, 2
P1709=0
#######################################################################
##  Account 5 Network Settings                                       ##
#######################################################################
# Outbound Proxy
P1703=

# Secondary Outbound Proxy
P2733=

# DNS Mode. 0 - A Record, 1 - SRV, 2 - NAPTR/SRV. Default value is 0
# Number: 0, 1, 2.
P1708=0

# DNS SRV Fail-over Mode. 0 - Default, 1 - Saved one until DNS TTL, 2 - Saved one until no response. Defualt value is 1
# Number
P26440=0

# Register Before DNS SRV Fail-over. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P29495=0

# NAT Traversal. 0 - No, 1 - STUN, 2 - Keep-alive, 3 - UPnP, 4 - Auto, 5 - VPN. Default value is 2
# Number: 0, 1, 2, 3, 4, 5
P1714=2

# Proxy-Require
P1718=
#######################################################################
##  Account 5 SIP Settings                                           ##
#######################################################################
# SIP Registration. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P1710=1

# Unregister Before New Registration. 0 - No, 1 - Yes, 2 -  Instance . Default value is 0
# Number: 0, 1, 2
P1711=0

# Register Expiration (m). In minutes. Default value is 60
# Number: 0 - 64800
P1712=60

# Subscribe Expiration (m). Default is 60
# Number: 0 - 64800
P26451=60

# Re-register before Expiration (s). Default value is 0
# Number
P2730=0

# Registration Retry Wait Time(s). In seconds. Default value is 20
# Number: 1 - 3600
P1771=20

# Local SIP Port. Default value is 5068
# Number: 5 - 65535
P1713=5068

# SUBSCRIBE for MWI. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P1715=0

# Enable OPTIONS Keep Alive. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P2797=0

# OPTIONS Keep Alive Interval(s). Default value is 30
# Number 
P2798=30

# OPTIONS Keep Alive Maximum Tries. Default value is 3
# Number 
P2799=3

# Enable Session Timer/ Session Expiration(s).  In seconds. Default value is 180 seconds.
# By default,  Session Timer is Enabled.  Session Timer is disabled if the value is 0.
# Number: 0 or 90 - 64800
P1734=180

# Min-SE (s). Default value is 90 seconds
# Number is 90 - 64800
P1727=90

# UAC Specify Refresher. 0 - Omit, 1 - UAC, 2 - UAS. Default value is 0
# Number: 0, 1, 2
P1732=0

# UAS Specify Refresher. 1 - UAC, 2 - UAS. Default value is 1
# Number: 1, 2
P1733=1

# Force INVITE (Always refresh with INVITE instead of UPDATE even when remote party supports UPDATE)
# 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P1731=0

# Caller Request Timer (Request for timer when calling). 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P1728=0

# Callee Request Timer (Request for timer when being called, i.e. if remote party supports timer but did not request for one)
# 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P1729=0

# Force Timer (Still use timer when remote party does not support timer). 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P1730=0

# Enable 100rel. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P1735=0

# Use Privacy Header. 0 - Default, 1 - No, 2 - Yes. Default is 0
# Number: 0, 1, 2
P2738=0

# Use P-Preferred-Identity Header. 0 - Default, 1 - No, 2 - Yes. Default is 0
# Number: 0, 1, 2
P2739=0

# Use P-Access-Network-Info Header. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P26485=1

# Use P-Emergency-Info Header. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P26459=1

# Use MAC Header.  0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P26461=0

# SIP Transport. 0 - UDP, 1 - TCP, 2 - TLS. Default value is 0
# Number: 0, 1, 2
P1748=0

# SIP URI Scheme When Using TLS
# 0 -sip, 1 - sips. Default value is 0.
# Number: 0, 1
P2729=0

# Use Actual Ephemeral Port in Contact with TCP/TLS
# 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P2731=0

# Support SIP Instance ID. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P1789=1

# Add Auth Header On RE-REGISTER
# 0 - No, 1- Yes
P2759=0

# SIP T1 Timeout. RFC 3261 T1 value (RTT estimate). 50 - 0.5 sec, 100 - 1 sec, 200 - 2 sec. Default value is 50
# Number: 50, 100, 200
P1740=50

# SIP T2 Interval. RFC 3261 T2 value. The maximum retransmit interval for non-INVITE requests and INVITE responses
# 200 - 2 sec, 400 - 4 sec, 800 - 8 sec. Default is value 400
# Number: 200, 400, 800
P1741=400

# SIP Timer D Interval (Seconds)
# Number 0-64. Default value is 0
P2787=0

# Remove OBP from route. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P2705=0
#######################################################################
##  Account 5 Codec Settings                                         ##
#######################################################################
# Preferred Vocoder
# First codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 98 - iLBC, 123 - Opus. Default value is 0
# Number: 0, 2, 8, 9, 98, 123
P1751=0

# Second codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 98 - iLBC, 123 - Opus. Default value is 8
# Number: 0, 2, 8, 9, 98, 123
P1752=8

# Third codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 98 - iLBC, 123 - Opus. Default value is 9
# Number: 0, 2, 8, 9, 98, 123
P1753=9

# Forth codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 98 - iLBC, 123 - Opus. Default value is 9
# Number: 0, 2, 8, 9, 98, 123
P1754=9

# Fifth codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 98 - iLBC, 123 - Opus. Default value is 9
# Number: 0, 2, 8, 9, 98, 123
P1755=9

# Sixth codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 123 - Opus. Default value is 9
# Number: 0, 8, 9, 2, 18, 98, 123
P1756=9

# Seventh codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 123 - Opus. Default value is 9
# Number: 0, 8, 9, 2, 18, 98, 123
P1757=9

# Eigth codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 123 - Opus. Default value is 9
# Number: 0, 8, 9, 2, 18, 98, 123
P1758=9

# Codec Negotiation Priority. 0 - Caller, 1 - Callee. Default value is 1.
# Number: 0, 1
P29461=1

# Use First Matching Vocoder in 200OK SDP. 0 - No, 1 - Yes. The default value is 0.
# Number: 0, 1
P2748=0

# iLBC Frame Size. 0 - 20 ms, 1 - 30 ms. Default value is 1.
# Number: 0, 1
P1795=1

# G726-32 ITU Payload. 0 - 2, 1 - Dynamic. Default value is 0.
# Number: 0, 1
P2769=0

# G726-32 Dynamic PT. Default value is 126.
# Number
P2765=126

# Opus Payload Type
P2785=123

# DTMF: in audio. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P2701=0

# DTMF: via RFC2833. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P2702=1

# DTMF: via SIP INFO. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P2703=0

# DTMF Payload Type. Default value is 101
# Number: 96 - 126
P1796=101

# Enable Audio RED with FEC. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P26473=0

# Audio FEC Payload Type. Default value is 121
# Number: 96 - 126
P26474=121

# Audio RED Payload Type. Default value is 124
# Number: 96 - 126
P26475=124

# Silence Suppression. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P1785=0

# Voice Frames per TX. Default value is 2
# Number: 1 - 64
P1786=2

# Preferred Video Codec. 99 - H.264. Default is 99.
P1764=99

# Enable Video FEC. 0 - No, 1 - Yes. Default value is 1.
# Number: 0, 1
P2793=1

# Enable RFC5168 support. 0 - No, 1 - Yes. Default value is 1.
# Number: 0, 1
P1778=1

# Video FEC Mode. 0 - 0, 1 - 1. Default value is 0.
# Number: 0, 1
P26422=0

# FEC Payload Type. Default value is 120.
P2794=120

# Packetization mode. 0 - Single NAL Unit Mode, 1 - Non-Interleaved Mode. Default value is 1.
# Number: 0, 1, 10
P26405=1

# H.264 Image Size. 9 - 720P, 1 - VGA, 5 - CIF, 4 - 4CIF, 0 - QVGA, 6 - QCIF. Default value is 9
# Number: 9, 1, 5, 4, 0, 6
P2707=9

# Use H.264 Constrained Profiles. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1
P26445=0

# H.264 Profile Type. 0 - Baseline Profile, 1 - Main Profile, 2 - High Profile, 3 - BP&MP&HP
# Number: 0, 1, 2, 3
P2762=0

# Video Bit Rate. 64 - 64 kbps, 96 - 96 kbps, 128 - 128 kbps, 160 - 160 kbps, 192 - 192 kbps
# 210 - 210 kbps, 256 - 256 kbps, 384 - 384 kbps, 512 - 512 kbps, 640 - 640 kbps, 768 - 768 kbps
# 1024 - 1024 kbps, 1280 - 1280 kbps, 1536 - 1536 kbps, 2048 - 2048 kbps. Default value is 2048.
# Number: 250, 500, 750
P2715=2048

# SDP Bandwidth Attribute. 0 - Standard, 1 - Media Level, 2 - Session Level, 3 - None. Default value is Media Level.
# Number: 0, 1, 2, 3
P2760=1

# H.264 Payload Type
P1762=99

# Disable BFCP. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1
P26401=0

# Presentation H.264 Image Size. 10 - 1080P, 9 - 720P. Default value is 10.
# Number: 10, 9
P2776=10

# Presentation H.264 Profile Type. 0 - Baseline Profile, 1 - Main Profile, 2 - High Profile, 3 - BP&MP&HP
# Number: 0, 1, 2, 3
P2777=3

# Presentation Video Bit Rate. 512 - 512 kbps, 640 - 640 kbps, 768 - 768 kbps
# 1024 - 1024 kbps, 1280 - 1280 kbps, 1536 - 1536 kbps, 2048 - 2048 kbps. Default value is 1024.
# Number: 250, 500, 750
P2778=1024

# Presentation Video Frame Rate. 5 - 5 frames/second, 10 - 10 frames/second, 15 - 15 frames/second. Default value is 15.
# Number: 5, 10, 15
P26442=

# BFCP Transport Protocol. 0 - Automatic, 1 - UDP, 2 - TCP. Default value is 1.
# Number: 0, 1, 2
P26441=

# SRTP Mode. 0 - Disabled, 1 - Enabled but not forced, 2 - Enabled and forced. Default value is 0
# Number: 0, 1, 2
P1743=0

# SRTP Key Length. 0 - AES 128&256 bit, 1 - AES 128 bit, 2 - AES 256 bit. Default value is 0
#Number:0, 1, 2
P2783=0 

# Enable SRTP Key Life Time. 0 - No, 1 - Yes.
# Number: 0,1
P2763=0

# RTCP Destination
P2790=

# Symmetric RTP. 0 - No, 1 - Yes. Default value is 0
# Number:0, 1
P1760=0

# RTP IP Filter. 0 - Disable, 1 - IP Only, 2 - IP and Port. Default value is 0
# Number:0, 1, 2
P26426=0

# RTP Timeout(s). Default is 0. If set to 0, the device would not hangup.
# number: 0 - 600
P29468=0
#######################################################################
##  Account 5 Call Settings                                          ##
#######################################################################
# Enable Video Call. 0 - Default, 1 - No, 2 - Yes. Default is 0
# Number: 0, 1, 2
P60443=0

# Start Video Automatically. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P2714=1

# Remote Video Request. 0 - Prompt, 1 - Accept, 2 - Deny. Default value is 0
# Number: 0, 1, 2
P2726=0

# Video Layout. 0 - Default, 1 - Full screen, 3 - Equal split screen, 2 - Only display remote screen
P2732=0

# Auto Answer. 0 - No, 1 - Yes, 2 - Enable Intercom/Paging. Default value is 0
# Number: 0, 1, 2
P1725=0

# Play warning tone for Auto Answer Intercom. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P26472=1

# Intercom Barging. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P26419=1

# Auto Preview. 0 - No, 1 - Yes, 2 - Yes with Ringing. Default value is 0
# Number: 0, 1, 2
P29462=0

# Send Anonymous. 0 - No, 1 - Yes (caller ID will be blocked if set to Yes). Default value is 0
# Number: 0, 1
P1721=0

# Anonymous Call Rejection. 0 - No,  1 - Yes. Default value is 0
# Number: 0, 1
P1746=0

# Call Log. 0 - Log All, 1 - Log Incoming/Outgoing Only (Missed Calls Not Recorded), 2 - Disable All. Default value is 0
# Number: 0, 1, 2
P1742=0

# Enable Call Features. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P1720=0

# Enable Call Waiting. 0 - Default, 1 - No, 2 - Yes.
# Number: 0, 1, 2
P26463=0

# Mute on Answer Intercom Call. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
P26471=0

# Transfer on 3 way conference Hangup. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P2704=0

# Use # as Dial Key. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P1792=1

# Use # as Redial Key. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P29469=1

# DND Call Feature On.
# String
P2744=

# DND Call Feature Off.
# String
P2745=

# No Key Entry Timeout (s). Default value is 4
# Number: 1 - 15
P1791=4

# Ring Timeout (s). Default value is 60
# Number: 10 - 300
P1776=60

# Refer-To Use Target Contact. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P1769=0

# RFC2543 Hold. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1 
P26462=1

# Dial Plan Prefix
# String
P1719=

# Disable DialPlan. 0 - No Selection, 1 - Dial Page, 2 - Contact, 4 - Incoming Call History, 8 -  Outgoing Call History, 16 - MPK & Click2Dial. 
# If need to check multiple selections, add the specific values for each selections together. Default value is 0
# Number: 0-31
P2782=0

# DialPlan. Default value is { x+ | \+x+ | *x+ | *xx*x+ | x+*x+*x+*x+ | x+*x+*x+*x+#x+ }
P1759={ x+ | \+x+ | *x+ | *xx*x+ | x+*x+*x+*x+ | x+*x+*x+*x+#x+ }

# Caller ID Display. 0 - Auto, 1 - Disabled, 2 - From Header. The default value is 0.
# Number: 0, 1, 2, 3
P2724=0

# Account Ringtone. See ring tone options and value in the Ring Tone value table below
P1723=content://settings/system/ringtone

# Ignore Alert-Info Header. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1
P26418=0

# Matching Incoming Caller ID. Matching Rule 1
# String
P1512=

# Matching Rule 1 Distinctive Ringtone. See ring tone options and value in the Ring Tone value table below
# String
P1513=content://settings/system/ringtone

# Matching Incoming Caller ID. Matching Rule 2
# String
P1514=

# Matching Rule 2 Distinctive Ringtone. See ring tone options and value in the Ring Tone value table below
# String
P1515=content://settings/system/ringtone

# Matching Incoming Caller ID. Matching Rule 3
# String
P1516=

# Matching Rule 3 Distinctive Ringtone. See ring tone options and value in the Ring Tone value table below
# String
P1517=content://settings/system/ringtone

############Ring Tone Value Table###############
# Web GUI Option                            Value
# Use System Ring tone                      content://settings/system/ringtone 
# Andromeda					/system/media/audio/ringtones/ANDROMEDA.ogg
# Aquila					/system/media/audio/ringtones/Aquila.ogg
# Argo Navis					/system/media/audio/ringtones/ArgoNavis.ogg
# Atria					/system/media/audio/ringtones/Atria.ogg
# Backroad					/system/media/audio/ringtones/Backroad.ogg
# Beat Plucker					/system/media/audio/ringtones/BeatPlucker.ogg
# Bell Phone					/system/media/audio/ringtones/Ring_Classic_02.ogg
# Bentley Dubs					/system/media/audio/ringtones/BentleyDubs.ogg
# Big Easy					/system/media/audio/ringtones/Big_Easy.ogg
# Bird Loop					/system/media/audio/ringtones/BirdLoop.ogg
# Bollywood					/system/media/audio/ringtones/Bollywood.ogg
# Boötes					/system/media/audio/ringtones/BOOTES.ogg
# Bus' a Move					/system/media/audio/ringtones/BussaMove.ogg
# Cairo					/system/media/audio/ringtones/Cairo.ogg
# Calypso Steel					/system/media/audio/ringtones/Calypso_Steel.ogg
# Canis Major					/system/media/audio/ringtones/CANISMAJOR.ogg
# Caribbean Ice					/system/media/audio/ringtones/CaribbeanIce.ogg
# Carina					/system/media/audio/ringtones/Carina.ogg
# Cassiopeia					/system/media/audio/ringtones/CASSIOPEIA.ogg
# Centaurus					/system/media/audio/ringtones/Centaurus.ogg
# Champagne Edition					/system/media/audio/ringtones/Champagne_Edition.ogg
# Chimey Phone					/system/media/audio/ringtones/Ring_Synth_02.ogg
# Club Cubano					/system/media/audio/ringtones/Club_Cubano.ogg
# Crayon Rock					/system/media/audio/ringtones/CrayonRock.ogg
# Crazy Dream					/system/media/audio/ringtones/CrazyDream.ogg
# Curve Ball Blend					/system/media/audio/ringtones/CurveBall.ogg
# Cygnus					/system/media/audio/ringtones/Cygnus.ogg
# Dancin' Fool					/system/media/audio/ringtones/DancinFool.ogg
# Digital Phone					/system/media/audio/ringtones/Ring_Digital_02.ogg
# Ding					/system/media/audio/ringtones/Ding.ogg
# DingDong					/system/media/audio/ringtones/DingDong.wav
# Don' Mess Wiv It					/system/media/audio/ringtones/DonMessWivIt.ogg
# Draco					/system/media/audio/ringtones/Draco.ogg
# Dream Theme					/system/media/audio/ringtones/DreamTheme.ogg
# Eastern Sky					/system/media/audio/ringtones/Eastern_Sky.ogg
# Enter the Nexus					/system/media/audio/ringtones/Enter_the_Nexus.ogg
# Eridani					/system/media/audio/ringtones/Eridani.ogg
# Ether Shake					/system/media/audio/ringtones/EtherShake.ogg
# Flutey Phone					/system/media/audio/ringtones/Ring_Synth_04.ogg
# Free Flight					/system/media/audio/ringtones/FreeFlight.ogg
# Friendly Ghost					/system/media/audio/ringtones/FriendlyGhost.ogg
# Funk Y'all					/system/media/audio/ringtones/Funk_Yall.ogg
# Game Over Guitar					/system/media/audio/ringtones/GameOverGuitar.ogg
# Gimme Mo' Town					/system/media/audio/ringtones/Gimme_Mo_Town.ogg
# Girtab					/system/media/audio/ringtones/Girtab.ogg
# Glacial Groove					/system/media/audio/ringtones/Glacial_Groove.ogg
# Growl					/system/media/audio/ringtones/Growl.ogg
# Halfway Home					/system/media/audio/ringtones/HalfwayHome.ogg
# Hydra					/system/media/audio/ringtones/Hydra.ogg
# Insert Coin					/system/media/audio/ringtones/InsertCoin.ogg
# Kuma					/system/media/audio/ringtones/Kuma.ogg
# Loopy Lounge					/system/media/audio/ringtones/LoopyLounge.ogg
# Love Flute					/system/media/audio/ringtones/LoveFlute.ogg
# Lyra					/system/media/audio/ringtones/Lyra.ogg
# Machina					/system/media/audio/ringtones/Machina.ogg
# Medieval Jaunt					/system/media/audio/ringtones/MidEvilJaunt.ogg
# Mildly Alarming					/system/media/audio/ringtones/MildlyAlarming.ogg
# Nairobi					/system/media/audio/ringtones/Nairobi.ogg
# Nassau					/system/media/audio/ringtones/Nassau.ogg
# New Player					/system/media/audio/ringtones/NewPlayer.ogg
# No Limits					/system/media/audio/ringtones/No_Limits.ogg
# Noisey One					/system/media/audio/ringtones/Noises1.ogg
# Organ Dub					/system/media/audio/ringtones/OrganDub.ogg
# Orion					/system/media/audio/ringtones/Orion.ogg
# Paradise Island					/system/media/audio/ringtones/Paradise_Island.ogg
# Pegasus					/system/media/audio/ringtones/Pegasus.ogg
# Perseus					/system/media/audio/ringtones/PERSEUS.ogg
# Playa					/system/media/audio/ringtones/Playa.ogg
# Pyxis					/system/media/audio/ringtones/Pyxis.ogg
# Rasalas					/system/media/audio/ringtones/Rasalas.ogg
# Revelation					/system/media/audio/ringtones/Revelation.ogg
# Rigel					/system/media/audio/ringtones/Rigel.ogg
# Road Trip					/system/media/audio/ringtones/Road_Trip.ogg
# Romancing The Tone					/system/media/audio/ringtones/RomancingTheTone.ogg
# Safari					/system/media/audio/ringtones/Safari.ogg
# Savannah					/system/media/audio/ringtones/Savannah.ogg
# Scarabaeus					/system/media/audio/ringtones/Scarabaeus.ogg
# Sceptrum					/system/media/audio/ringtones/Sceptrum.ogg
# Seville					/system/media/audio/ringtones/Seville.ogg
# She's All That					/system/media/audio/ringtones/Shes_All_That.ogg
# Silky Way					/system/media/audio/ringtones/SilkyWay.ogg
# Sitar Versus Sitar					/system/media/audio/ringtones/SitarVsSitar.ogg
# Solarium					/system/media/audio/ringtones/Solarium.ogg
# Springy Jalopy					/system/media/audio/ringtones/SpringyJalopy.ogg
# Steppin' Out					/system/media/audio/ringtones/Steppin_Out.ogg
# Terminated					/system/media/audio/ringtones/Terminated.ogg
# Terrible Twos					/system/media/audio/ringtones/Noises2.ogg
# Testudo					/system/media/audio/ringtones/Testudo.ogg
# Themos					/system/media/audio/ringtones/Themos.ogg
# Third Eye					/system/media/audio/ringtones/Third_Eye.ogg
# Thriller Three					/system/media/audio/ringtones/Noises3.ogg
# Thunderfoot					/system/media/audio/ringtones/Thunderfoot.ogg
# Twirl Away					/system/media/audio/ringtones/TwirlAway.ogg
# Ursa Minor					/system/media/audio/ringtones/URSAMINOR.ogg
# UrsaMinor					/system/media/audio/ringtones/UrsaMinor.ogg
# Very Alarmed					/system/media/audio/ringtones/VeryAlarmed.ogg
# Vespa					/system/media/audio/ringtones/Vespa.ogg
# World					/system/media/audio/ringtones/World.ogg
# Zeta					/system/media/audio/ringtones/Zeta.ogg
# bellcore-dr1					/system/media/audio/ringtones/bellcore-dr1.ogg
# bellcore-dr2					/system/media/audio/ringtones/bellcore-dr2.ogg
# bellcore-dr3					/system/media/audio/ringtones/bellcore-dr3.ogg
# bellcore-dr4					/system/media/audio/ringtones/bellcore-dr4.ogg
# bellcore-dr5					/system/media/audio/ringtones/bellcore-dr5.ogg
# speaker					/system/media/audio/ringtones/speaker.wav
#######################################################################
##  Account 5 Advanced Settings                                      ##
#######################################################################
# Check Domain Certificates. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P2711=0

# Validate Certificate Chain. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P2767=0

# Validate Incoming SIP Messages. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P2706=0

# Allow Unsolicited REFER. 0 - Disabled, 1 - Enabled, 2 - Enabled/Force Auth. Default value is 0.
# Number: 0, 1, 2
P26423=0

# Only Accept SIP Requests from Known Servers. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P2747=0

# Check SIP User ID for Incoming INVITE. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P1749=0

# Allow SIP Reset. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P26415=0

# Authenticate Incoming INVITE. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P2746=0

# SIP Realm Used for Challenge INVITE & NOTIFY.
# String
P26421=

# Enable Local MOH. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P2757=0

# Virtual Account Group. -1 - Default,  0 - Virtual Account Group 1, 1 - Virtual Account Group 2, 2 - Virtual Account Group 3
# 3 - Virtual Account Group 4, 4 - Virtual Account Group 5, 5 - Virtual Account Group 6, 6 - Virtual Account Group 7, 7 - Virtual Account Group 8
# 8 - Virtual Account Group 9, 9 - Virtual Account Group 10, 10 - Virtual Account Group 11, 11 - Virtual Account Group 12, 12 - Virtual Account Group 13
# 13 - Virtual Account Group 14, 14 - Virtual Account Group 15, 15 - Virtual Account Group 16. Default value is -1.
# Number: -1 - 15 
P2791=-1

# Special Feature. Default value is 100
# 100 - Standard, 102 - Broadsoft, 113 - China Mobile
# 114 - ZTE IMS, 115 - Mobotix, 116 - ZTE NGN, 117 - Huawei IMS, 123 - NEC, 125 - WorldStone
# Number: 100, 102, 113, 114, 115, 116, 117, 123, 125
P1724=100

# Allow Sync Phonebook via SIP Notify. 0 - No, 1 - Yes. Default is 1.
# Number: 0, 1
P26499=1
##############################################################################
##  Account 6 Settings                                                      ##
##############################################################################
#######################################################################
##  Account 6 General Settings                                       ##
#######################################################################
# Account Active. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P1801=1

# Account Name
P1817=IPVideoTalk

# SIP Server
P1802=sip.ipvideotalk.com:48879

# SIP User ID
P1804=

# SIP Authentication ID
P1805=

# SIP Authentication Password
P1806=

# Voice Mail Access Number
P1826=*26

# Name (Display name :John Doe)
P1807=

# Tel URI. 0 - Disable, 1 - User=Phone, 2 - Enabled. Default value is 0
# Number: 0, 1, 2
P1809=0
#######################################################################
##  Account 6 Network Settings                                       ##
#######################################################################
# Outbound Proxy
P1803=

# Secondary Outbound Proxy
P2833=

# DNS Mode. 0 - A Record, 1 - SRV, 2 - NAPTR/SRV. Default is 0
# Number: 0, 1, 2
P1808=0

# DNS SRV Fail-over Mode. 0 - Default, 1 - Saved one until DNS TTL, 2 - Saved one until no response. Defualt value is 1
# Number
P26540=0

# Register Before DNS SRV Fail-over. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P29595=0

# NAT Traversal. 0 - No, 1 - STUN, 2 - Keep-alive, 3 - UPnP, 4 - Auto, 5 - VPN. Default value is 2
# Number: 0, 1, 2, 3, 4, 5
P1814=2

# Proxy-Require
P1818=
#######################################################################
##  Account 6 SIP Settings                                           ##
#######################################################################
# SIP Registration. 0 - No, 1 - Yes. Default is 1
# Number: 0, 1
P1810=1

# Unregister Before New Registration. 0 - No, 1 - Yes, 2 -  Instance . Default value is 0
# Number: 0, 1, 2
P1811=1

# Register Expiration (m). In minutes. Default value is 60
# Number: 0 - 64800
P1812=60

# Subscribe Expiration (m). Default is 60
# Number: 0 - 64800
P26551=60

# Re-register before Expiration (s). Default value is 0
# Number
P2830=0

# Registration Retry Wait Time(s). In seconds. Default value is 20
# Number: 1 - 3600
P1871=20

# Local SIP Port. Default value is 5070
# Number: 5-65535
P1813=5070

# SUBSCRIBE for MWI. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P1815=0

# Enable OPTIONS Keep Alive. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P2897=0

# OPTIONS Keep Alive Interval(s). Default value is 30
# Number 
P2898=30

# OPTIONS Keep Alive Maximum Tries. Default value is 3
# Number 
P2899=3

# Enable Session Timer/ Session Expiration(s).  In seconds. Default value is 180 seconds.
# By default,  Session Timer is Enabled.  Session Timer is disabled if the value is 0.
# Number: 0 or 90 - 64800
P1834=180

# Min-SE (s). Default value is 90 seconds
# Number: 5 - 65535
P1827=90

# UAC Specify Refresher. 0 - Omit, 1 - UAC, 2 - UAS. Default value is 0
# Number: 0, 1, 2
P1832=0

# UAS Specify Refresher. 1 - UAC, 2 - UAS. Default value is 1
# Number: 1, 
P1833=1

# Force INVITE (Always refresh with INVITE instead of UPDATE even when remote party supports UPDATE)
# 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P1831=0

# Caller Request Timer (Request for timer when calling)
# 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P1828=0

# Callee Request Timer. Request for timer when called (i.e. if remote party supports timer but did not request for one)
# 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P1829=0

# Force Timer (Still use timer when remote party does not support timer). 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P1830=0

# Enable 100rel. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P1835=0

# Use Privacy Header. 0 - Default, 1 - No, 2 - Yes. Default is 0
# Number: 0, 1, 2
P2838=0

# Use P-Preferred-Identity Header. 0 - Default, 1 - No, 2 - Yes. Default is 0
# Number: 0, 1, 2
P2839=0

# Use P-Access-Network-Info Header. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P26558=1

# Use P-Emergency-Info Header. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P26559=1

# Use MAC Header.  0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P26561=0

# SIP Transport. 0 - UDP, 1 - TCP, 2 - TLS. Default value is 0
# Number: 0, 1, 2
P1848=0

# SIP URI Scheme When Using TLS
# 0 -sip, 1 - sips. Default value is 0.
# Number: 0, 1
P2829=0

# Use Actual Ephemeral Port in Contact with TCP/TLS
# 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P2831=0

# Support SIP Instance ID. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P1889=1

# Add Auth Header On RE-REGISTER
# 0 - No, 1- Yes
P2859=0

# SIP T1 Timeout. RFC 3261 T1 value (RTT estimate). 50 - 0.5 sec, 100 - 1 sec, 200 - 2 sec. Default value is 50
# Number: 50, 100, 200
P1840=50

# SIP T2 Interval. RFC 3261 T2 value. The maximum retransmit interval for non-INVITE requests and INVITE responses
# 200 - 2 sec, 400 - 4 sec, 800 - 8 sec. Default 400
# Number: 200, 400, 800
P1841=400

# SIP Timer D Interval (Seconds)
# Number 0-64. Default value is 0
P2887=0

# Remove OBP from route. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P2805=0
#######################################################################
##  Account 6 Codec Settings                                         ##
#######################################################################
# Preferred Vocoder
# First codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 98 - iLBC, 123 -Opus. Default value is 0
# Number: 0, 2, 8, 9, 98, 123
P1851=0

# Second codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 98 - iLBC, 123 -Opus. Default value is 8
# Number: 0, 2, 8, 9, 98, 123
P1852=8

# Third codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 98 - iLBC, 123 -Opus. Default value is 9
# Number: 0, 2, 8, 9, 98, 123
P1853=9

# Forth codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 98 - iLBC, 123 -Opus. Default value is 9
# Number: 0, 2, 8, 9, 98, 123
P1854=9

# Fifth codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 98 - iLBC, 123 -Opus. Default value is 9
# Number: 0, 2, 8, 9, 98, 123
P1855=9

# Sixth codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 123 - Opus. Default value is 9
# Number: 0, 8, 9, 2, 18, 98, 123
P1856=9

# Seventh codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 123 - Opus. Default value is 9
# Number: 0, 8, 9, 2, 18, 98, 123
P1857=9

# Eigth codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 123 - Opus. Default value is 9
# Number: 0, 8, 9, 2, 18, 98, 123
P1858=9

# Codec Negotiation Priority. 0 - Caller, 1 - Callee. Default value is 1.
# Number: 0, 1
P29561=1

# Use First Matching Vocoder in 200OK SDP. 0 - No, 1 - Yes. The default value is 0.
# Number: 0, 1
P2848=0

# iLBC Frame Size. 0 - 20 ms, 1 - 30 ms. Default value is 1.
# Number: 0, 1
P1895=1

# G726-32 ITU Payload. 0 - 2, 1 - Dynamic. Default value is 0.
# Number: 0, 1
P2869=0

# G726-32 Dynamic PT. Default value is 126.
# Number
P2865=126

# Opus Payload Type
P2885=123

# DTMF: in audio. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P2801=0

# DTMF: in RFC2833. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P2802=1

# DTMF: in SIP INFO. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P2803=0

# DTMF Payload Type. Default value is 101
# Number: 96 - 126
P1896=101

# Enable Audio RED with FEC. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P26573=0

# Audio FEC Payload Type. Default value is 121
# Number: 96 - 126
P26574=121

# Audio RED Payload Type. Default value is 124
# Number: 96 - 126
P26575=124

# Silence Suppression. 0 - No, 1 - Yes
# Number: 0, 1
P1885=0

# Voice Frames per TX. Default valule is 2
# Number: 1 - 64
P1886=2 

# Preferred Video Codec. 99 - H.264. Default is 99.
P1864=99

# Enable Video FEC. 0 - No, 1 - Yes. Default value is 1.
# Number: 0, 1
P2893=1

# Enable RFC5168 support. 0 - No, 1 - Yes. Default value is 1.
# Number: 0, 1
P1878=1

# Video FEC Mode. 0 - 0, 1 - 1. Default value is 0.
# Number: 0, 1
P26522=0

# FEC Payload Type. Default value is 120.
P2894=120

# Packetization mode. 0 - Single NAL Unit Mode, 1 - Non-Interleaved Mode. Default value is 1.
# Number: 0, 1, 10
P26505=1

# H.264 Image Size. 9 - 720P, 1 - VGA, 5 - CIF, 4 - 4CIF, 0 - QVGA, 6 - QCIF. Default value is 9
# Number: 9, 1, 5, 4, 0, 6
P2807=9

# Use H.264 Constrained Profiles. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1
P26545=0

# H.264 Profile Type. 0 - Baseline Profile, 1 - Main Profile, 2 - High Profile, 3 - BP&MP&HP
# Number: 0, 1, 2, 3
P2862=0

# Video Bit Rate. 64 - 64 kbps, 96 - 96 kbps, 128 - 128 kbps, 160 - 160 kbps, 192 - 192 kbps
# 210 - 210 kbps, 256 - 256 kbps, 384 - 384 kbps, 512 - 512 kbps, 640 - 640 kbps, 768 - 768 kbps
# 1024 - 1024 kbps, 1280 - 1280 kbps, 1536 - 1536 kbps, 2048 - 2048 kbps. Default value is 2048.
# Number: 250, 500, 750
P2815=2048

# SDP Bandwidth Attribute. 0 - Standard, 1 - Media Level, 2 - Session Level, 3 - None. Default value is Media Level.
# Number: 0, 1, 2, 3
P2860=1

# H.264 Payload Type
P1862=99

# Disable BFCP. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1
P26501=0

# Presentation H.264 Image Size. 10 - 1080P, 9 - 720P. Default value is 10.
# Number: 10, 9
P2876=10

# Presentation H.264 Profile Type. 0 - Baseline Profile, 1 - Main Profile, 2 - High Profile, 3 - BP&MP&HP
# Number: 0, 1, 2, 3
P2877=3

# Presentation Video Bit Rate. 512 - 512 kbps, 640 - 640 kbps, 768 - 768 kbps
# 1024 - 1024 kbps, 1280 - 1280 kbps, 1536 - 1536 kbps, 2048 - 2048 kbps. Default value is 1024.
# Number: 250, 500, 750
P2878=1024

# Presentation Video Frame Rate. 5 - 5 frames/second, 10 - 10 frames/second, 15 - 15 frames/second. Default value is 15.
# Number: 5, 10, 15
P26542=

# BFCP Transport Protocol. 0 - Automatic, 1 - UDP, 2 - TCP. Default value is 1.
# Number: 0, 1, 2
P26541=

# SRTP Mode. 0 - Disabled, 1 - Enabled but not forced, 2 - Enabled and forced. Default value is 0
# Number: 0, 1, 2
P1843=0

# SRTP Key Length. 0 - AES 128&256 bit, 1 - AES 128 bit, 2 - AES 256 bit. Default value is 0
#Number:0, 1, 2
P2883=0

# Enable SRTP Key Life Time. 0 - No, 1 - Yes.
# Number: 0,1
P2863=0

# RTCP Destination
P2890=

# Symmetric RTP. 0 - No, 1 - Yes. Default value is 0
# Number:0, 1
P1860=0

# RTP IP Filter. 0 - Disable, 1 - IP Only, 2 - IP and Port. Default value is 0
# Number:0, 1, 2
P26526=0

# RTP Timeout(s). Default is 0. If set to 0, the device would not hangup.
# number: 0 - 600
P29568=0
#######################################################################
##  Account 6 Call Settings                                          ##
#######################################################################
# Enable Video Call. 0 - Default, 1 - No, 2 - Yes. Default is 0
# Number: 0, 1, 2
P60543=0

# Start Video Automatically. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P2814=1

# Remote Video Request. 0 - Prompt, 1 - Accept, 2 - Deny. Default value is 0
# Number: 0, 1, 2
P2826=0

# Video Layout. 0 - Default, 1 - Full screen, 3 - Equal split screen, 2 - Only display remote screen
P2832=0

# Auto Answer. 0 - No, 1 - Yes, 2 - Enable Intercom/Paging. Default value is 0
# Number: 0, 1
P1825=0

# Play warning tone for Auto Answer Intercom. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P26572=1

# Intercom Barging. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P26519=1

# Auto Preview. 0 - No, 1 - Yes, 2 - Yes with Ringing. Default value is 0
# Number: 0, 1, 2
P29562=0

# Send Anonymous. 0 - No, 1 - Yes (caller ID will be blocked if set to Yes). Default value is 0
# Number: 0, 1
P1821=0

# Anonymous Call Rejection. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P1846=0

# Call Log. 0 - Log All, 1 - Log Incoming/Outgoing only (Missed Calls Not Recorded), 2 - Disable Call All. Default value is 0
# Number: 0, 1, 2
P1842=0

# Enable Call Features. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P1820=0

# Enable Call Waiting. 0 - Default, 1 - No, 2 - Yes.
# Number: 0, 1, 2
P26563=0

# Mute on Answer Intercom Call. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
P26571=0

# Transfer on 3 way conference Hangup. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P2804=0

# Use # as Dial Key. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P1892=1

# Use # as Redial Key. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P29569=1

# DND Call Feature On.
# String
P2844=

# DND Call Feature Off.
# String
P2845=

# No Key Entry Timeout (s). Default value is 4
# Number: 1 - 15
P1891=4

# Ring Timeout. Default value is 60 seconds
# Number: 10 - 300
P1876=60

# Refer-To Use Target Contact. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P1869=0

# RFC2543 Hold. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1 
P26562=1

# Dial Plan Prefix
# String
P1819=

# Disable DialPlan. 0 - No Selection, 1 - Dial Page, 2 - Contact, 4 - Incoming Call History, 8 -  Outgoing Call History, 16 - MPK & Click2Dial. 
# If need to check multiple selections, add the specific values for each selections together. Default value is 0
# Number: 0-31
P2882=0

# Dial Plan. Default value is { x+ | \+x+ | *x+ | *xx*x+ | x+*x+*x+*x+ | x+*x+*x+*x+#x+ }
P1859={ x+ | \+x+ | *x+ | *xx*x+ | x+*x+*x+*x+ | x+*x+*x+*x+#x+ }

# Caller ID Display. 0 - Auto, 1 - Disabled, 2 - From Header. The default value is 0.
# Number: 0, 1, 2, 3
P2824=0

# Account Ringtone. See ring tone options and values in the Ring Tone value table below
P1823=content://settings/system/ringtone

# Ignore Alert-Info Header. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1
P26518=0

# Matching Incoming Caller ID. Matching Rule 1
# String
P1518=

# Matching Rule 1 Distinctive Ringtone. See ring tone options and values in the Ring Tone value table below
# String
P1519=content://settings/system/ringtone

# Matching Incoming Caller ID. Matching Rule 2
# String
P1520=

# Matching Rule 2 Distinctive Ringtone. See ring tone options and values in the Ring Tone value table below
# String
P1521=content://settings/system/ringtone

# Matching Incoming Caller ID. Matching Rule 3
# String
P1522=

# Matching Rule 3 Distinctive Ringtone. See ring tone options and values in the Ring Tone value table below
# String
P1523=content://settings/system/ringtone

############Ring Tone Value Table###############
# Web GUI Option                            Value
# Use System Ring tone                      content://settings/system/ringtone 
# Andromeda					/system/media/audio/ringtones/ANDROMEDA.ogg
# Aquila					/system/media/audio/ringtones/Aquila.ogg
# Argo Navis					/system/media/audio/ringtones/ArgoNavis.ogg
# Atria					/system/media/audio/ringtones/Atria.ogg
# Backroad					/system/media/audio/ringtones/Backroad.ogg
# Beat Plucker					/system/media/audio/ringtones/BeatPlucker.ogg
# Bell Phone					/system/media/audio/ringtones/Ring_Classic_02.ogg
# Bentley Dubs					/system/media/audio/ringtones/BentleyDubs.ogg
# Big Easy					/system/media/audio/ringtones/Big_Easy.ogg
# Bird Loop					/system/media/audio/ringtones/BirdLoop.ogg
# Bollywood					/system/media/audio/ringtones/Bollywood.ogg
# Boötes					/system/media/audio/ringtones/BOOTES.ogg
# Bus' a Move					/system/media/audio/ringtones/BussaMove.ogg
# Cairo					/system/media/audio/ringtones/Cairo.ogg
# Calypso Steel					/system/media/audio/ringtones/Calypso_Steel.ogg
# Canis Major					/system/media/audio/ringtones/CANISMAJOR.ogg
# Caribbean Ice					/system/media/audio/ringtones/CaribbeanIce.ogg
# Carina					/system/media/audio/ringtones/Carina.ogg
# Cassiopeia					/system/media/audio/ringtones/CASSIOPEIA.ogg
# Centaurus					/system/media/audio/ringtones/Centaurus.ogg
# Champagne Edition					/system/media/audio/ringtones/Champagne_Edition.ogg
# Chimey Phone					/system/media/audio/ringtones/Ring_Synth_02.ogg
# Club Cubano					/system/media/audio/ringtones/Club_Cubano.ogg
# Crayon Rock					/system/media/audio/ringtones/CrayonRock.ogg
# Crazy Dream					/system/media/audio/ringtones/CrazyDream.ogg
# Curve Ball Blend					/system/media/audio/ringtones/CurveBall.ogg
# Cygnus					/system/media/audio/ringtones/Cygnus.ogg
# Dancin' Fool					/system/media/audio/ringtones/DancinFool.ogg
# Digital Phone					/system/media/audio/ringtones/Ring_Digital_02.ogg
# Ding					/system/media/audio/ringtones/Ding.ogg
# DingDong					/system/media/audio/ringtones/DingDong.wav
# Don' Mess Wiv It					/system/media/audio/ringtones/DonMessWivIt.ogg
# Draco					/system/media/audio/ringtones/Draco.ogg
# Dream Theme					/system/media/audio/ringtones/DreamTheme.ogg
# Eastern Sky					/system/media/audio/ringtones/Eastern_Sky.ogg
# Enter the Nexus					/system/media/audio/ringtones/Enter_the_Nexus.ogg
# Eridani					/system/media/audio/ringtones/Eridani.ogg
# Ether Shake					/system/media/audio/ringtones/EtherShake.ogg
# Flutey Phone					/system/media/audio/ringtones/Ring_Synth_04.ogg
# Free Flight					/system/media/audio/ringtones/FreeFlight.ogg
# Friendly Ghost					/system/media/audio/ringtones/FriendlyGhost.ogg
# Funk Y'all					/system/media/audio/ringtones/Funk_Yall.ogg
# Game Over Guitar					/system/media/audio/ringtones/GameOverGuitar.ogg
# Gimme Mo' Town					/system/media/audio/ringtones/Gimme_Mo_Town.ogg
# Girtab					/system/media/audio/ringtones/Girtab.ogg
# Glacial Groove					/system/media/audio/ringtones/Glacial_Groove.ogg
# Growl					/system/media/audio/ringtones/Growl.ogg
# Halfway Home					/system/media/audio/ringtones/HalfwayHome.ogg
# Hydra					/system/media/audio/ringtones/Hydra.ogg
# Insert Coin					/system/media/audio/ringtones/InsertCoin.ogg
# Kuma					/system/media/audio/ringtones/Kuma.ogg
# Loopy Lounge					/system/media/audio/ringtones/LoopyLounge.ogg
# Love Flute					/system/media/audio/ringtones/LoveFlute.ogg
# Lyra					/system/media/audio/ringtones/Lyra.ogg
# Machina					/system/media/audio/ringtones/Machina.ogg
# Medieval Jaunt					/system/media/audio/ringtones/MidEvilJaunt.ogg
# Mildly Alarming					/system/media/audio/ringtones/MildlyAlarming.ogg
# Nairobi					/system/media/audio/ringtones/Nairobi.ogg
# Nassau					/system/media/audio/ringtones/Nassau.ogg
# New Player					/system/media/audio/ringtones/NewPlayer.ogg
# No Limits					/system/media/audio/ringtones/No_Limits.ogg
# Noisey One					/system/media/audio/ringtones/Noises1.ogg
# Organ Dub					/system/media/audio/ringtones/OrganDub.ogg
# Orion					/system/media/audio/ringtones/Orion.ogg
# Paradise Island					/system/media/audio/ringtones/Paradise_Island.ogg
# Pegasus					/system/media/audio/ringtones/Pegasus.ogg
# Perseus					/system/media/audio/ringtones/PERSEUS.ogg
# Playa					/system/media/audio/ringtones/Playa.ogg
# Pyxis					/system/media/audio/ringtones/Pyxis.ogg
# Rasalas					/system/media/audio/ringtones/Rasalas.ogg
# Revelation					/system/media/audio/ringtones/Revelation.ogg
# Rigel					/system/media/audio/ringtones/Rigel.ogg
# Road Trip					/system/media/audio/ringtones/Road_Trip.ogg
# Romancing The Tone					/system/media/audio/ringtones/RomancingTheTone.ogg
# Safari					/system/media/audio/ringtones/Safari.ogg
# Savannah					/system/media/audio/ringtones/Savannah.ogg
# Scarabaeus					/system/media/audio/ringtones/Scarabaeus.ogg
# Sceptrum					/system/media/audio/ringtones/Sceptrum.ogg
# Seville					/system/media/audio/ringtones/Seville.ogg
# She's All That					/system/media/audio/ringtones/Shes_All_That.ogg
# Silky Way					/system/media/audio/ringtones/SilkyWay.ogg
# Sitar Versus Sitar					/system/media/audio/ringtones/SitarVsSitar.ogg
# Solarium					/system/media/audio/ringtones/Solarium.ogg
# Springy Jalopy					/system/media/audio/ringtones/SpringyJalopy.ogg
# Steppin' Out					/system/media/audio/ringtones/Steppin_Out.ogg
# Terminated					/system/media/audio/ringtones/Terminated.ogg
# Terrible Twos					/system/media/audio/ringtones/Noises2.ogg
# Testudo					/system/media/audio/ringtones/Testudo.ogg
# Themos					/system/media/audio/ringtones/Themos.ogg
# Third Eye					/system/media/audio/ringtones/Third_Eye.ogg
# Thriller Three					/system/media/audio/ringtones/Noises3.ogg
# Thunderfoot					/system/media/audio/ringtones/Thunderfoot.ogg
# Twirl Away					/system/media/audio/ringtones/TwirlAway.ogg
# Ursa Minor					/system/media/audio/ringtones/URSAMINOR.ogg
# UrsaMinor					/system/media/audio/ringtones/UrsaMinor.ogg
# Very Alarmed					/system/media/audio/ringtones/VeryAlarmed.ogg
# Vespa					/system/media/audio/ringtones/Vespa.ogg
# World					/system/media/audio/ringtones/World.ogg
# Zeta					/system/media/audio/ringtones/Zeta.ogg
# bellcore-dr1					/system/media/audio/ringtones/bellcore-dr1.ogg
# bellcore-dr2					/system/media/audio/ringtones/bellcore-dr2.ogg
# bellcore-dr3					/system/media/audio/ringtones/bellcore-dr3.ogg
# bellcore-dr4					/system/media/audio/ringtones/bellcore-dr4.ogg
# bellcore-dr5					/system/media/audio/ringtones/bellcore-dr5.ogg
# speaker					/system/media/audio/ringtones/speaker.wav
#######################################################################
##  Account 6 Advanced Settings                                      ##
#######################################################################
# Check Domain Certificates. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P2811=0

# Validate Certificate Chain. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P2867=0

# Validate Incoming SIP Messages. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P2806=0

# Allow Unsolicited REFER. 0 - Disabled, 1 - Enabled, 2 - Enabled/Force Auth. Default value is 0.
# Number: 0, 1, 2
P26523=0

# Only Accept SIP Requests from Known Servers. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P2847=0

# Check SIP User ID for Incoming INVITE. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P1849=0

# Allow SIP Reset. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P26515=0

# Authenticate Incoming INVITE. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P2846=0

# SIP Realm Used for Challenge INVITE & NOTIFY.
# String
P26521=

# Enable Local MOH. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P2857=0

# Virtual Account Group. -1 - Default,  0 - Virtual Account Group 1, 1 - Virtual Account Group 2, 2 - Virtual Account Group 3
# 3 - Virtual Account Group 4, 4 - Virtual Account Group 5, 5 - Virtual Account Group 6, 6 - Virtual Account Group 7, 7 - Virtual Account Group 8
# 8 - Virtual Account Group 9, 9 - Virtual Account Group 10, 10 - Virtual Account Group 11, 11 - Virtual Account Group 12, 12 - Virtual Account Group 13
# 13 - Virtual Account Group 14, 14 - Virtual Account Group 15, 15 - Virtual Account Group 16. Default value is -1.
# Number: -1 - 15 
P2891=-1

# Special Feature. Default value is 100
# 100 - Standard, 102 - Broadsoft, 113 - China Mobile
# 114 - ZTE IMS, 115 - Mobotix, 116 - ZTE NGN, 117 - Huawei IMS, 123 - NEC, 125 - WorldStone
# Number: 100, 102, 113, 114, 115, 116, 117, 123, 125
P1824=100

# Allow Sync Phonebook via SIP Notify. 0 - No, 1 - Yes. Default is 1.
# Number: 0, 1
P26599=1
##############################################################################
##  Account 7 Settings                                                      ##
##############################################################################
#######################################################################
##  Account 7 General Settings                                       ##
#######################################################################
# Account Active. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P50601=0

# Account Name
P50617=

# SIP Server
P50602=

# SIP User ID
P50604=
 
# SIP Authentication ID
P50605=

# SIP Authentication Password
P50606=

# Voice Mail Access Number
P50626=

# Name (Display Name, e.g., John Doe)
P50607=

# Tel URI. 0 - Disable, 1 - User=Phone, 2 - Enabled. Default value is 0
# Number: 0, 1, 2
P50609=0

#######################################################################
##  Account 7 Network Settings                                       ##
#######################################################################

# Outbound Proxy
P50603=

# Secondary Outbound Proxy
P51633=

# DNS Mode. 0 - A Record, 1 - SRV, 2 - NAPTR/SRV. Default value is 0
# Number: 0, 1, 2
P50608=0

# DNS SRV Fail-over Mode. 0 - Default, 1 - Saved one until DNS TTL, 2 - Saved one until no response. Defualt value is 1
# Number
P52640=0

#  SRV Fail-over. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P53695=0

# NAT Traversal. 0 - NAT No, 1 - STUN, 2 - Keep-alive, 3 - UPnP, 4 - Auto, 5 - VPN. Default value is 2
# Number: 0, 1, 2, 3, 4, 5
P50614=2

# Proxy-Require
P50618=

#######################################################################
##  Account 7 SIP Settings                                           ##
#######################################################################

# SIP Registration. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P50610=1

# Unregister Before New Registration. 0 - No, 1 - All, 2 -  Instance . Default value is 2
# Number: 0, 1, 2
P50611=2

# Register Expiration (m). In minutes. Default value is 60
# Number: 0 - 64800
P50612=60

# Subscribe Expiration (m). Default is 60
# Number: 0 - 64800
P52651=60

# Re-register before Expiration (s). Default Value is 0
# Number : 0
P51630=0

# Registration Retry Wait Time (s). In seconds. Default value is 20
# Number: 1 - 3600
P50671=20

# Local SIP Port. Default value is 5072
# Number: 5 - 65535
P50613=5072

# SUBSCRIBE For MWI. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P50615=0

# Enable SIP OPTIONS Keep Alive. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P51697=0

# SIP OPTIONS Keep Alive Interval(s). Default value is 30
# Number 
P51698=30

# SIP OPTIONS Keep Alive Maximum Tries. Default value is 3
# Number 
P51699=3

# Enable Session Timer/ Session Expiration(s).  In seconds. Default value is 180 seconds.
# By default,  Session Timer is Enabled.  Session Timer is disabled if the value is 0.
# Number: 0 or 90 - 64800
P50634=180

# Min-SE(s). Default value is 90 seconds
# Number: 90 - 64800
P50627=90

# UAC Specify Refresher. 0 - Omit, 1 - UAC, 2 - UAS. Default value is 0
# Number: 0, 1, 2
P50632=0

# UAS Specify Refresher. 1 - UAC, 2 - UAS. Default value is 1
# Number: 1, 2
P50633=1

# Force INVITE. Always refresh with INVITE instead of UPDATE even when remote party supports UPDATE
# 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P50631=0

# Caller Request Timer. Request for timer when calling
# 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P50628=0

# Callee Request Timer
# Request for timer when being called (i.e., if remote party supports timer but did not request for one)
# 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P50629=0

# Force Timer. Still use timer when remote party does not support timer
# 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P50630=0

# Enable 100rel. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P50635=0

# Use Privacy Header
# 0 - Default, 1 - No, 2 - Yes. Default is 0
# Number: 0, 1, 2
P51638=0

# Use P-Preferred-Identity Header
# 0 - Default, 1 - No, 2 - Yes. Default is 0
# Number: 0, 1, 2
P51639=0

# Use P-Access-Network-Info Header. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P52658=1

# Use P-Emergency-Info Header. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P52659=1

# Use MAC Header.  0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P52661=0

# SIP Transport
# 0 - UDP , 1 - TCP, 2 - TLS. Default value is 0
# Number: 0, 1, 2
P50648=0

# SIP URI Scheme When Using TLS
# 0 -sip, 1 - sips. Default value is 0.
# Number: 0, 1
P51629=0

# Use Actual Ephemeral Port in Contact with TCP/TLS
# 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P51631=0

# Support SIP Instance ID
# 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P50689=1

# Add Auth Header On RE-REGISTER
# 0 - No, 1- Yes
P51659=1

# SIP T1 Timeout. RFC 3261 T1 value (RTT estimate)
# 50 - 0.5 sec, 100 - 1 sec, 200 - 2 sec. Default value is 50
# Number: 50, 100, 200
P50640=50

# SIP T2 Interval. RFC 3261 T2 value
# The maximum retransmit interval for non-INVITE requests and INVITE responses
# 200 - 2 sec, 400 - 4 sec, 800 - 8 sec. Default value is 400
# Number: 200, 400, 800.
P50641=400

# SIP Timer D Interval (Seconds)
# Number 0-64. Default value is 0
P51687=0

# Remove OBP from Route
# 0 - Disable, 1 - Enable, 2 - Always. Default value is 0
# Number: 0, 1, 2
P51605=0
#######################################################################
##  Account 7 Codec Settings                                         ##
#######################################################################
# Preferred Vocoder
# First codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 123 - Opus. Default value is 0
# Number: 0, 8, 9, 2, 18, 98, 123
P50651=0

# Second codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 123 - Opus. Default value is 8
# Number: 0, 8, 9, 2, 18, 98, 123
P50652=8

# Third codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 123 - Opus. Default value is 9
# Number: 0, 8, 9, 2, 18, 98, 123
P50653=9

# Forth codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 123 - Opus. Default value is 9
# Number: 0, 8, 9, 2, 18, 98, 123
P50654=9

# Fifth codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 123 - Opus. Default value is 9
# Number: 0, 8, 9, 2, 18, 98, 123
P50655=9

# Sixth codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 123 - Opus. Default value is 9
# Number: 0, 8, 9, 2, 18, 98, 123
P50656=9

# Seventh codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 123 - Opus. Default value is 9
# Number: 0, 8, 9, 2, 18, 98, 123
P50657=9

# Eigth codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 123 - Opus. Default value is 9
# Number: 0, 8, 9, 2, 18, 98, 123
P50658=9

# Codec Negotiation Priority. 0 - Caller, 1 - Callee. Default value is 1.
# Number: 0, 1
P53661=1

# Use First Matching Vocoder in 200OK SDP. 0 - No, 1 - Yes. The default value is 0.
# Number: 0, 1
P51648=0

# iLBC Frame Size. 0 - 20 ms, 1 - 30 ms. Default value is 1.
# Number: 0, 1
P50695=1

# G726-32 ITU Payload. 0 - 2, 1 - Dynamic. Default value is 0.
# Number: 0, 1
P51669=0

# G726-32 Dynamic PT. Default value is 126.
# Number
P51665=126

# Opus Payload Type
P51685=123

# DTMF: in audio. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P51601=0

# DTMF: via RFC2833. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P51602=1

# DTMF: via SIP INFO. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P51603=0

# DTMF Payload Type. Default value is 101
# Number: 96 - 126
P50696=101

# Enable Audio RED with FEC. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P52673=0

# Audio FEC Payload Type. Default value is 121
# Number: 96 - 126
P52674=121

# Audio RED Payload Type. Default value is 124
# Number: 96 - 126
P52675=124

# Silence Suppression. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P50685=0

# Voice Frames Per TX. Default value is 2
# Number: 1 - 64.
P50686=2

# Preferred Video Codec. 99 - H.264. Default is 99.
P50064=99

# Enable Video FEC. 0 - No, 1 - Yes. Default value is 1.
# Number: 0, 1
P51693=1

# Enable RFC5168 Support. 0 - No, 1 - Yes. Default value is 1.
# Number: 0, 1
P50678=1

# Video FEC Mode. 0 - 0, 1 - 1. Default value is 0.
# Number: 0, 1
P52622=0

# FEC Payload Type. Default value is 120.
P51694=120

# Packetization mode. 0 - Single NAL Unit Mode, 1 - Non-Interleaved Mode. Default value is 1.
# Number: 0, 1, 10
P52605=1

# H.264 Image Size. 9 - 720P, 1 - VGA, 5 - CIF, 4 - 4CIF, 0 - QVGA, 6 - QCIF. Default value is 9
# Number: 9, 1, 5, 4, 0, 6
P51607=9

# Use H.264 Constrained Profiles. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1
P52645=0

# H.264 Profile Type. 0 - Baseline Profile, 1 - Main Profile, 2 - High Profile, 3 - BP&MP&HP
# Number: 0, 1, 2, 3
P51662=0

# Video Bit Rate. 64 - 64 kbps, 96 - 96 kbps, 128 - 128 kbps, 160 - 160 kbps, 192 - 192 kbps
# 210 - 210 kbps, 256 - 256 kbps, 384 - 384 kbps, 512 - 512 kbps, 640 - 640 kbps, 768 - 768 kbps
# 1024 - 1024 kbps, 1280 - 1280 kbps, 1536 - 1536 kbps, 2048 - 2048 kbps. Default value is 2048.
# Number: 250, 500, 750
P51615=2048

# SDP Bandwidth Attribute. 0 - Standard, 1 - Media Level, 2 - Session Level, 3 - None. Default value is Media Level.
# Number: 0, 1, 2, 3
P51660=1

# H.264 Payload Type. Default value is 99.
P50662=99

# Disable BFCP. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1
P52601=0

# Presentation H.264 Image Size. 10 - 1080P, 9 - 720P. Default value is 10.
# Number: 10, 9
P51676=10

# Presentation H.264 Profile Type. 0 - Baseline Profile, 1 - Main Profile, 2 - High Profile, 3 - BP&MP&HP
# Number: 0, 1, 2, 3
P51677=3

# Presentation Video Bit Rate. 512 - 512 kbps, 640 - 640 kbps, 768 - 768 kbps
# 1024 - 1024 kbps, 1280 - 1280 kbps, 1536 - 1536 kbps, 2048 - 2048 kbps. Default value is 1024.
# Number: 250, 500, 750
P51678=1024

# Presentation Video Frame Rate. 5 - 5 frames/second, 10 - 10 frames/second, 15 - 15 frames/second. Default value is 15.
# Number: 5, 10, 15
P52642=

# BFCP Transport Protocol. 0 - Automatic, 1 - UDP, 2 - TCP. Default value is 1.
# Number: 0, 1, 2
P52641=

# SRTP Mode. 0 - Disable, 1 - Enable but not forced, 2 - Enable and forced. Default value is 0
# Number:0, 1, 2
P50643=0

# SRTP Key Length. 0 - AES 128&256 bit, 1 - AES 128 bit, 2 - AES 256 bit. Default value is 0
# Number:0, 1, 2
P51683=0 

# Enable SRTP Key Lifetime. 0 - No, 1 - Yes.
# Number: 0,1
P51663=0

# RTCP Destination
P51690=

# Symmetric RTP. 0 - No, 1 - Yes. Default value is 0
# Number:0, 1
P50660=0

# RTP IP Filter. 0 - Disable, 1 - IP Only, 2 - IP and Port. Default value is 0
# Number:0, 1, 2
P52626=0

# RTP Timeout(s). Default is 0. If set to 0, the device would not hangup.
# number: 0 - 600
P53668=0
#######################################################################
##  Account 7 Call Settings                                          ##
#######################################################################
# Enable Video Call. 0 - Default, 1 - No, 2 - Yes. Default is 0
# Number: 0, 1, 2
P60643=0

# Start Video Automatically. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P51614=1

# Remote Video Request. 0 - Prompt, 1 - Accept, 2 - Deny. Default value is 0
# Number: 0, 1, 2
P51626=0

# Video Layout. 0 - Default, 1 - Full screen, 3 - Equal split screen, 2 - Only display remote screen
P51632=0

# Auto Answer. 0 - No, 1 - Yes, 2 - Enable Intercom/Paging. Default value is 0
# Number: 0, 1, 2
P50625=0

# Play warning tone for Auto Answer Intercom. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P52672=1

# Intercom Barging. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P52619=1

# Auto Preview. 0 - No, 1 - Yes, 2 - Yes with Ringing. Default value is 0
# Number: 0, 1, 2
P53662=0

# Send Anonymous. 0 - No, 1 - Yes (caller ID will be blocked if set to Yes). Default value is 0
# Number: 0, 1
P50621=0

# Anonymous Call Rejection. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P50646=0

# Call Log
# 0 - Log All, 1 - Log Incoming/Outgoing only (Missed Calls Not Recorded), 2 - Disable Call All, 3 - Don't Prompt Missed Call. Default value is 0
# Number: 0, 1, 2
P50642=0

# Enable Call Features. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P50620=0

# Enable Call Waiting. 0 - Default, 1 - No, 2 - Yes.
# Number: 0, 1, 2
P52663=0

# Mute on Answer Intercom Call. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
P52671=0

# Transfer on 3 way conference Hangup. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P51604=0

# Use # as Dial Key. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P50692=1

# Use # as Redial Key. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P53669=1

# DND Call Feature On.
# String
P51644=

# DND Call Feature Off.
# String
P51645=

# No Key Entry Timeout (s). Default value is 4
# Number: 1 - 15
P50691=4

# Ring Timeout (s). Default value is 60
# Number: 10 - 300
P50676=60

# Refer-To Use Target Contact. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P50669=0

# RFC2543 Hold. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1 
P52662=1

# Dial Plan Prefix
# String
P50619=

# Disable DialPlan. 0 - No Selection, 1 - Dial Page, 2 - Contact, 4 - Incoming Call History, 8 -  Outgoing Call History, 16 - MPK & Click2Dial. 
# If need to check multiple selections, add the specific values for each selections together. Default value is 0
# Number: 0-31
P51682=0

# DialPlan. Default value is { x+ | \+x+ | *x+ | *xx*x+ | x+*x+*x+*x+ | x+*x+*x+*x+#x+ }
P50659={ x+ | \+x+ | *x+ | *xx*x+ | x+*x+*x+*x+ | x+*x+*x+*x+#x+ }

# Caller ID Display. 0 - Auto, 1 - Disabled, 2 - From Header. The default value is 0.
# Number: 0, 1, 2, 3
P51624=0

# Account Ringtone. See ring tone options and value in the Ring Tone Value Table below
P50623=content://settings/system/ringtone

# Ignore Alert-Info Header. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1
P52618=0

# Matching Incoming Caller ID. Matching Rule 1
# String
P52677=

# Matching Rule 1 Distinctive Ringtone. See ring tone options and value in the Ring Tone Value Table below
# String
P52678=content://settings/system/ringtone

# Matching Incoming Caller ID. Matching Rule 2
# String
P52679=

# Matching Rule 2 Distinctive Ringtone. See ring tone options and value in the Ring Tone Value Table below
# String
P52680=content://settings/system/ringtone

# Matching Incoming Caller ID. Matching Rule 3
# String
P52681=

# Matching Rule 3 Distinctive Ringtone. See ring tone options and value in the Ring Tone Value Table below
# String
P52682=content://settings/system/ringtone

############Ring Tone Value Table###############
# Web GUI Option                            Value
# Use System Ring tone                      content://settings/system/ringtone 
# Andromeda					/system/media/audio/ringtones/ANDROMEDA.ogg
# Aquila					/system/media/audio/ringtones/Aquila.ogg
# Argo Navis					/system/media/audio/ringtones/ArgoNavis.ogg
# Atria					/system/media/audio/ringtones/Atria.ogg
# Backroad					/system/media/audio/ringtones/Backroad.ogg
# Beat Plucker					/system/media/audio/ringtones/BeatPlucker.ogg
# Bell Phone					/system/media/audio/ringtones/Ring_Classic_02.ogg
# Bentley Dubs					/system/media/audio/ringtones/BentleyDubs.ogg
# Big Easy					/system/media/audio/ringtones/Big_Easy.ogg
# Bird Loop					/system/media/audio/ringtones/BirdLoop.ogg
# Bollywood					/system/media/audio/ringtones/Bollywood.ogg
# Boötes					/system/media/audio/ringtones/BOOTES.ogg
# Bus' a Move					/system/media/audio/ringtones/BussaMove.ogg
# Cairo					/system/media/audio/ringtones/Cairo.ogg
# Calypso Steel					/system/media/audio/ringtones/Calypso_Steel.ogg
# Canis Major					/system/media/audio/ringtones/CANISMAJOR.ogg
# Caribbean Ice					/system/media/audio/ringtones/CaribbeanIce.ogg
# Carina					/system/media/audio/ringtones/Carina.ogg
# Cassiopeia					/system/media/audio/ringtones/CASSIOPEIA.ogg
# Centaurus					/system/media/audio/ringtones/Centaurus.ogg
# Champagne Edition					/system/media/audio/ringtones/Champagne_Edition.ogg
# Chimey Phone					/system/media/audio/ringtones/Ring_Synth_02.ogg
# Club Cubano					/system/media/audio/ringtones/Club_Cubano.ogg
# Crayon Rock					/system/media/audio/ringtones/CrayonRock.ogg
# Crazy Dream					/system/media/audio/ringtones/CrazyDream.ogg
# Curve Ball Blend					/system/media/audio/ringtones/CurveBall.ogg
# Cygnus					/system/media/audio/ringtones/Cygnus.ogg
# Dancin' Fool					/system/media/audio/ringtones/DancinFool.ogg
# Digital Phone					/system/media/audio/ringtones/Ring_Digital_02.ogg
# Ding					/system/media/audio/ringtones/Ding.ogg
# DingDong					/system/media/audio/ringtones/DingDong.wav
# Don' Mess Wiv It					/system/media/audio/ringtones/DonMessWivIt.ogg
# Draco					/system/media/audio/ringtones/Draco.ogg
# Dream Theme					/system/media/audio/ringtones/DreamTheme.ogg
# Eastern Sky					/system/media/audio/ringtones/Eastern_Sky.ogg
# Enter the Nexus					/system/media/audio/ringtones/Enter_the_Nexus.ogg
# Eridani					/system/media/audio/ringtones/Eridani.ogg
# Ether Shake					/system/media/audio/ringtones/EtherShake.ogg
# Flutey Phone					/system/media/audio/ringtones/Ring_Synth_04.ogg
# Free Flight					/system/media/audio/ringtones/FreeFlight.ogg
# Friendly Ghost					/system/media/audio/ringtones/FriendlyGhost.ogg
# Funk Y'all					/system/media/audio/ringtones/Funk_Yall.ogg
# Game Over Guitar					/system/media/audio/ringtones/GameOverGuitar.ogg
# Gimme Mo' Town					/system/media/audio/ringtones/Gimme_Mo_Town.ogg
# Girtab					/system/media/audio/ringtones/Girtab.ogg
# Glacial Groove					/system/media/audio/ringtones/Glacial_Groove.ogg
# Growl					/system/media/audio/ringtones/Growl.ogg
# Halfway Home					/system/media/audio/ringtones/HalfwayHome.ogg
# Hydra					/system/media/audio/ringtones/Hydra.ogg
# Insert Coin					/system/media/audio/ringtones/InsertCoin.ogg
# Kuma					/system/media/audio/ringtones/Kuma.ogg
# Loopy Lounge					/system/media/audio/ringtones/LoopyLounge.ogg
# Love Flute					/system/media/audio/ringtones/LoveFlute.ogg
# Lyra					/system/media/audio/ringtones/Lyra.ogg
# Machina					/system/media/audio/ringtones/Machina.ogg
# Medieval Jaunt					/system/media/audio/ringtones/MidEvilJaunt.ogg
# Mildly Alarming					/system/media/audio/ringtones/MildlyAlarming.ogg
# Nairobi					/system/media/audio/ringtones/Nairobi.ogg
# Nassau					/system/media/audio/ringtones/Nassau.ogg
# New Player					/system/media/audio/ringtones/NewPlayer.ogg
# No Limits					/system/media/audio/ringtones/No_Limits.ogg
# Noisey One					/system/media/audio/ringtones/Noises1.ogg
# Organ Dub					/system/media/audio/ringtones/OrganDub.ogg
# Orion					/system/media/audio/ringtones/Orion.ogg
# Paradise Island					/system/media/audio/ringtones/Paradise_Island.ogg
# Pegasus					/system/media/audio/ringtones/Pegasus.ogg
# Perseus					/system/media/audio/ringtones/PERSEUS.ogg
# Playa					/system/media/audio/ringtones/Playa.ogg
# Pyxis					/system/media/audio/ringtones/Pyxis.ogg
# Rasalas					/system/media/audio/ringtones/Rasalas.ogg
# Revelation					/system/media/audio/ringtones/Revelation.ogg
# Rigel					/system/media/audio/ringtones/Rigel.ogg
# Road Trip					/system/media/audio/ringtones/Road_Trip.ogg
# Romancing The Tone					/system/media/audio/ringtones/RomancingTheTone.ogg
# Safari					/system/media/audio/ringtones/Safari.ogg
# Savannah					/system/media/audio/ringtones/Savannah.ogg
# Scarabaeus					/system/media/audio/ringtones/Scarabaeus.ogg
# Sceptrum					/system/media/audio/ringtones/Sceptrum.ogg
# Seville					/system/media/audio/ringtones/Seville.ogg
# She's All That					/system/media/audio/ringtones/Shes_All_That.ogg
# Silky Way					/system/media/audio/ringtones/SilkyWay.ogg
# Sitar Versus Sitar					/system/media/audio/ringtones/SitarVsSitar.ogg
# Solarium					/system/media/audio/ringtones/Solarium.ogg
# Springy Jalopy					/system/media/audio/ringtones/SpringyJalopy.ogg
# Steppin' Out					/system/media/audio/ringtones/Steppin_Out.ogg
# Terminated					/system/media/audio/ringtones/Terminated.ogg
# Terrible Twos					/system/media/audio/ringtones/Noises2.ogg
# Testudo					/system/media/audio/ringtones/Testudo.ogg
# Themos					/system/media/audio/ringtones/Themos.ogg
# Third Eye					/system/media/audio/ringtones/Third_Eye.ogg
# Thriller Three					/system/media/audio/ringtones/Noises3.ogg
# Thunderfoot					/system/media/audio/ringtones/Thunderfoot.ogg
# Twirl Away					/system/media/audio/ringtones/TwirlAway.ogg
# Ursa Minor					/system/media/audio/ringtones/URSAMINOR.ogg
# UrsaMinor					/system/media/audio/ringtones/UrsaMinor.ogg
# Very Alarmed					/system/media/audio/ringtones/VeryAlarmed.ogg
# Vespa					/system/media/audio/ringtones/Vespa.ogg
# World					/system/media/audio/ringtones/World.ogg
# Zeta					/system/media/audio/ringtones/Zeta.ogg
# bellcore-dr1					/system/media/audio/ringtones/bellcore-dr1.ogg
# bellcore-dr2					/system/media/audio/ringtones/bellcore-dr2.ogg
# bellcore-dr3					/system/media/audio/ringtones/bellcore-dr3.ogg
# bellcore-dr4					/system/media/audio/ringtones/bellcore-dr4.ogg
# bellcore-dr5					/system/media/audio/ringtones/bellcore-dr5.ogg
# speaker					/system/media/audio/ringtones/speaker.wav
#######################################################################
##  Account 7 Advanced Settings                                      ##
#######################################################################
# Check Domain Certificates. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P51611=0

# Validate Certificate Chain. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P51667=0

# Validate Incoming SIP Messages. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P51606=0

# Allow Unsolicited REFER. 0 - Disabled, 1 - Enabled, 2 - Enabled/Force Auth. Default value is 0.
# Number: 0, 1, 2
P52623=0

# Only Accept SIP Requests from Known Servers. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P51647=0

# Check SIP User ID for Incoming INVITE. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P50649=0

# Allow SIP Reset. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P52615=0

# Authenticate Incoming INVITE. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P51646=0

# SIP Realm Used for Challenge INVITE & NOTIFY.
# String
P52621=

# Enable Local MOH. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P51657=0

# Virtual Account Group. -1 - Default,  0 - Virtual Account Group 1, 1 - Virtual Account Group 2, 2 - Virtual Account Group 3
# 3 - Virtual Account Group 4, 4 - Virtual Account Group 5, 5 - Virtual Account Group 6, 6 - Virtual Account Group 7, 7 - Virtual Account Group 8
# 8 - Virtual Account Group 9, 9 - Virtual Account Group 10, 10 - Virtual Account Group 11, 11 - Virtual Account Group 12, 12 - Virtual Account Group 13
# 13 - Virtual Account Group 14, 14 - Virtual Account Group 15, 15 - Virtual Account Group 16. Default value is -1.
# Number: -1 - 15 
P51691=-1

# Special Feature. Default value is 100
# 100 - Standard, 102 - Broadsoft, 113 - China Mobile
# 114 - ZTE IMS, 115 - Mobotix, 116 - ZTE NGN, 117 - Huawei IMS, 123 - NEC, 125 - WorldStone
# Number: 100, 102, 113, 114, 115, 116, 117, 123, 125
P50624=100

# Allow Sync Phonebook via SIP Notify. 0 - No, 1 - Yes. Default is 1.
# Number: 0, 1
P52699=1
##############################################################################
##  Account 8 Settings                                                      ##
##############################################################################

#######################################################################
##  Account 8 General Settings                                       ##
#######################################################################

# Account Active. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P50701=0

# Account Name
P50717=

# SIP Server
P50702=

# SIP User ID
P50704=
 
# SIP Authentication ID
P50705=

# SIP Authentication Password
P50706=

# Voice Mail Access Number
P50726=

# Name (Display Name, e.g., John Doe)
P50707=

# Tel URI. 0 - Disable, 1 - User=Phone, 2 - Enabled. Default value is 0
# Number: 0, 1, 2
P50709=0

#######################################################################
##  Account 8 Network Settings                                       ##
#######################################################################

# Outbound Proxy
P50703=

# Secondary Outbound Proxy
P51733=

# DNS Mode. 0 - A Record, 1 - SRV, 2 - NAPTR/SRV. Default value is 0
# Number: 0, 1, 2
P50708=0

# DNS SRV Fail-over Mode. 0 - Default, 1 - Saved one until DNS TTL, 2 - Saved one until no response. Defualt value is 1
# Number
P52740=0

# Register Before DNS SRV Fail-over. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P53795=0

# NAT Traversal. 0 - NAT No, 1 - STUN, 2 - Keep-alive, 3 - UPnP, 4 - Auto, 5 - VPN. Default value is 2
# Number: 0, 1, 2, 3, 4, 5
P50714=2

# Proxy-Require
P50718=

#######################################################################
##  Account 8 SIP Settings                                           ##
#######################################################################

# SIP Registration. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P50710=1

# Unregister Before New Registration. 0 - No, 1 - All, 2 -  Instance . Default value is 2
# Number: 0, 1, 2
P50711=2

# Register Expiration (m). In minutes. Default value is 60
# Number: 0 - 64800
P50712=60

# Subscribe Expiration (m). Default is 60
# Number: 0 - 64800
P52751=60

# Re-register before Expiration (s). Default Value is 0
# Number : 0
P51730=0

# Registration Retry Wait Time (s). In seconds. Default value is 20
# Number: 1 - 3600
P50771=20

# Local SIP Port. Default value is 5074
# Number: 5 - 65535
P50713=5074

# SUBSCRIBE For MWI. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P50715=0

# Enable SIP OPTIONS Keep Alive. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P51797=0

# SIP OPTIONS Keep Alive Interval(s). Default value is 30
# Number 
P51798=30

# SIP OPTIONS Keep Alive Maximum Tries. Default value is 3
# Number 
P51799=3

# Enable Session Timer/ Session Expiration(s).  In seconds. Default value is 180 seconds.
# By default,  Session Timer is Enabled.  Session Timer is disabled if the value is 0.
# Number: 0 or 90 - 64800
P50734=180

# Min-SE(s). Default value is 90 seconds
# Number: 90 - 64800
P50727=90

# UAC Specify Refresher. 0 - Omit, 1 - UAC, 2 - UAS. Default value is 0
# Number: 0, 1, 2
P50732=0

# UAS Specify Refresher. 1 - UAC, 2 - UAS. Default value is 1
# Number: 1, 2
P50733=1

# Force INVITE. Always refresh with INVITE instead of UPDATE even when remote party supports UPDATE
# 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P50731=0

# Caller Request Timer. Request for timer when calling
# 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P50728=0

# Callee Request Timer
# Request for timer when being called (i.e., if remote party supports timer but did not request for one)
# 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P50729=0

# Force Timer. Still use timer when remote party does not support timer
# 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P50730=0

# Enable 100rel. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P50735=0

# Use Privacy Header
# 0 - Default, 1 - No, 2 - Yes. Default is 0
# Number: 0, 1, 2
P51738=0

# Use P-Preferred-Identity Header
# 0 - Default, 1 - No, 2 - Yes. Default is 0
# Number: 0, 1, 2
P51739=0

# Use P-Access-Network-Info Header. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P52758=1

# Use P-Emergency-Info Header. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P52759=1

# Use MAC Header.  0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P52761=0

# SIP Transport
# 0 - UDP , 1 - TCP, 2 - TLS. Default value is 0
# Number: 0, 1, 2
P50748=0

# SIP URI Scheme When Using TLS
# 0 -sip, 1 - sips. Default value is 0.
# Number: 0, 1
P51729=0

# Use Actual Ephemeral Port in Contact with TCP/TLS
# 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P51731=0

# Support SIP Instance ID
# 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P50789=1

# Add Auth Header On RE-REGISTER
# 0 - No, 1- Yes
P51759=1

# SIP T1 Timeout. RFC 3261 T1 value (RTT estimate)
# 50 - 0.5 sec, 100 - 1 sec, 200 - 2 sec. Default value is 50
# Number: 50, 100, 200
P50740=50

# SIP T2 Interval. RFC 3261 T2 value
# The maximum retransmit interval for non-INVITE requests and INVITE responses
# 200 - 2 sec, 400 - 4 sec, 800 - 8 sec. Default value is 400
# Number: 200, 400, 800.
P50741=400

# SIP Timer D Interval (Seconds)
# Number 0-64. Default value is 0
P51787=0

# Remove OBP from Route
# 0 - Disable, 1 - Enable, 2 - Always. Default value is 0
# Number: 0, 1, 2
P51705=0
#######################################################################
##  Account 8 Codec Settings                                         ##
#######################################################################
# Preferred Vocoder
# First codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 123 - Opus. Default value is 0
# Number: 0, 8, 9, 2, 18, 98, 123
P50751=0

# Second codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 123 - Opus. Default value is 8
# Number: 0, 8, 9, 2, 18, 98, 123
P50752=8

# Third codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 123 - Opus. Default value is 9
# Number: 0, 8, 9, 2, 18, 98, 123
P50753=9

# Forth codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 123 - Opus. Default value is 9
# Number: 0, 8, 9, 2, 18, 98, 123
P50754=9

# Fifth codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 123 - Opus. Default value is 9
# Number: 0, 8, 9, 2, 18, 98, 123
P50755=9

# Sixth codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 123 - Opus. Default value is 9
# Number: 0, 8, 9, 2, 18, 98, 123
P50756=9

# Seventh codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 123 - Opus. Default value is 9
# Number: 0, 8, 9, 2, 18, 98, 123
P50757=9

# Eigth codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 123 - Opus. Default value is 9
# Number: 0, 8, 9, 2, 18, 98, 123
P50758=9

# Codec Negotiation Priority. 0 - Caller, 1 - Callee. Default value is 1.
# Number: 0, 1
P53761=1

# Use First Matching Vocoder in 200OK SDP. 0 - No, 1 - Yes. The default value is 0.
# Number: 0, 1
P51748=0

# iLBC Frame Size. 0 - 20 ms, 1 - 30 ms. Default value is 1.
# Number: 0, 1
P50795=1

# G726-32 ITU Payload. 0 - 2, 1 - Dynamic. Default value is 0.
# Number: 0, 1
P51769=0

# G726-32 Dynamic PT. Default value is 126.
# Number
P51765=126

# Opus Payload Type
P51785=123

# DTMF: in audio. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P51701=0

# DTMF: via RFC2833. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P51702=1

# DTMF: via SIP INFO. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P51703=0

# DTMF Payload Type. Default value is 101
# Number: 96 - 126
P50796=101

# Enable Audio RED with FEC. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P52773=0

# Audio FEC Payload Type. Default value is 121
# Number: 96 - 126
P52774=121

# Audio RED Payload Type. Default value is 124
# Number: 96 - 126
P52775=124

# Silence Suppression. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P50785=0

# Voice Frames Per TX. Default value is 2
# Number: 1 - 64.
P50786=2

# Preferred Video Codec. 99 - H.264. Default is 99.
P50764=99

# Enable Video FEC. 0 - No, 1 - Yes. Default value is 1.
# Number: 0, 1
P51793=1

# Enable RFC5168 Support. 0 - No, 1 - Yes. Default value is 1.
# Number: 0, 1
P50778=1

# Video FEC Mode. 0 - 0, 1 - 1. Default value is 0.
# Number: 0, 1
P52722=0

# FEC Payload Type. Default value is 120.
P51794=120

# Packetization mode. 0 - Single NAL Unit Mode, 1 - Non-Interleaved Mode. Default value is 1.
# Number: 0, 1, 10
P52705=1

# H.264 Image Size. 9 - 720P, 1 - VGA, 5 - CIF, 4 - 4CIF, 0 - QVGA, 6 - QCIF. Default value is 9
# Number: 9, 1, 5, 4, 0, 6
P51707=9

# Use H.264 Constrained Profiles. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1
P52745=0

# H.264 Profile Type. 0 - Baseline Profile, 1 - Main Profile, 2 - High Profile, 3 - BP&MP&HP
# Number: 0, 1, 2, 3
P51762=0

# Video Bit Rate. 64 - 64 kbps, 96 - 96 kbps, 128 - 128 kbps, 160 - 160 kbps, 192 - 192 kbps
# 210 - 210 kbps, 256 - 256 kbps, 384 - 384 kbps, 512 - 512 kbps, 640 - 640 kbps, 768 - 768 kbps
# 1024 - 1024 kbps, 1280 - 1280 kbps, 1536 - 1536 kbps, 2048 - 2048 kbps. Default value is 2048.
# Number: 250, 500, 750
P51715=2048

# SDP Bandwidth Attribute. 0 - Standard, 1 - Media Level, 2 - Session Level, 3 - None. Default value is Media Level.
# Number: 0, 1, 2, 3
P51760=1

# H.264 Payload Type. Default value is 99.
P50762=99

# Disable BFCP. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1
P52701=0

# Presentation H.264 Image Size. 10 - 1080P, 9 - 720P. Default value is 10.
# Number: 10, 9
P51776=10

# Presentation H.264 Profile Type. 0 - Baseline Profile, 1 - Main Profile, 2 - High Profile, 3 - BP&MP&HP
# Number: 0, 1, 2, 3
P51777=3

# Presentation Video Bit Rate. 512 - 512 kbps, 640 - 640 kbps, 768 - 768 kbps
# 1024 - 1024 kbps, 1280 - 1280 kbps, 1536 - 1536 kbps, 2048 - 2048 kbps. Default value is 1024.
# Number: 250, 500, 750
P51778=1024

# Presentation Video Frame Rate. 5 - 5 frames/second, 10 - 10 frames/second, 15 - 15 frames/second. Default value is 15.
# Number: 5, 10, 15
P52742=

# BFCP Transport Protocol. 0 - Automatic, 1 - UDP, 2 - TCP. Default value is 1.
# Number: 0, 1, 2
P52741=

# SRTP Mode. 0 - Disable, 1 - Enable but not forced, 2 - Enable and forced. Default value is 0
# Number:0, 1, 2
P50743=0

# SRTP Key Length. 0 - AES 128&256 bit, 1 - AES 128 bit, 2 - AES 256 bit. Default value is 0
# Number:0, 1, 2
P51783=0 

# Enable SRTP Key Lifetime. 0 - No, 1 - Yes.
# Number: 0,1
P51763=0

# RTCP Destination
P51790=

# Symmetric RTP. 0 - No, 1 - Yes. Default value is 0
# Number:0, 1
P50760=0

# RTP IP Filter. 0 - Disable, 1 - IP Only, 2 - IP and Port. Default value is 0
# Number:0, 1, 2
P52726=0

# RTP Timeout(s). Default is 0. If set to 0, the device would not hangup.
# number: 0 - 600
P53768=0
#######################################################################
##  Account 8 Call Settings                                          ##
#######################################################################
# Enable Video Call. 0 - Default, 1 - No, 2 - Yes. Default is 0
# Number: 0, 1, 2
P60743=0

# Start Video Automatically. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P51714=1

# Remote Video Request. 0 - Prompt, 1 - Accept, 2 - Deny. Default value is 0
# Number: 0, 1, 2
P51726=0

# Video Layout. 0 - Default, 1 - Full screen, 3 - Equal split screen, 2 - Only display remote screen
P51732=0

# Auto Answer. 0 - No, 1 - Yes, 2 - Enable Intercom/Paging. Default value is 0
# Number: 0, 1, 2
P50725=0

# Play warning tone for Auto Answer Intercom. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P52772=1

# Intercom Barging. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P52719=1

# Auto Preview. 0 - No, 1 - Yes, 2 - Yes with Ringing. Default value is 0
# Number: 0, 1, 2
P53762=0

# Send Anonymous. 0 - No, 1 - Yes (caller ID will be blocked if set to Yes). Default value is 0
# Number: 0, 1
P50721=0

# Anonymous Call Rejection. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P50746=0

# Call Log
# 0 - Log All, 1 - Log Incoming/Outgoing only (Missed Calls Not Recorded), 2 - Disable Call All, 3 - Don't Prompt Missed Call. Default value is 0
# Number: 0, 1, 2
P50742=0

# Enable Call Features. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P50720=0

# Enable Call Waiting. 0 - Default, 1 - No, 2 - Yes.
# Number: 0, 1, 2
P52763=0

# Mute on Answer Intercom Call. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
P52771=0

# Transfer on 3 way conference Hangup. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P51704=0

# Use # as Dial Key. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P50792=1

# Use # as Redial Key. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P53769=1

# DND Call Feature On.
# String
P51744=

# DND Call Feature Off.
# String
P51745=

# No Key Entry Timeout (s). Default value is 4
# Number: 1 - 15
P50791=4

# Ring Timeout (s). Default value is 60
# Number: 10 - 300
P50776=60

# Refer-To Use Target Contact. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P50769=0

# RFC2543 Hold. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1 
P52762=1

# Dial Plan Prefix
# String
P50719=

# Disable DialPlan. 0 - No Selection, 1 - Dial Page, 2 - Contact, 4 - Incoming Call History, 8 -  Outgoing Call History, 16 - MPK & Click2Dial. 
# If need to check multiple selections, add the specific values for each selections together. Default value is 0
# Number: 0-31
P51782=0

# DialPlan. Default value is { x+ | \+x+ | *x+ | *xx*x+ | x+*x+*x+*x+ | x+*x+*x+*x+#x+ }
P50759={ x+ | \+x+ | *x+ | *xx*x+ | x+*x+*x+*x+ | x+*x+*x+*x+#x+ }

# Caller ID Display. 0 - Auto, 1 - Disabled, 2 - From Header. The default value is 0.
# Number: 0, 1, 2, 3
P51724=0

# Account Ringtone. See ring tone options and value in the Ring Tone Value Table below
P50723=content://settings/system/ringtone

# Ignore Alert-Info Header. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1
P52718=0

# Matching Incoming Caller ID. Matching Rule 1
# String
P52777=

# Matching Rule 1 Distinctive Ringtone. See ring tone options and value in the Ring Tone Value Table below
# String
P52778=content://settings/system/ringtone

# Matching Incoming Caller ID. Matching Rule 2
# String
P52779=

# Matching Rule 2 Distinctive Ringtone. See ring tone options and value in the Ring Tone Value Table below
# String
P52780=content://settings/system/ringtone

# Matching Incoming Caller ID. Matching Rule 3
# String
P52781=

# Matching Rule 3 Distinctive Ringtone. See ring tone options and value in the Ring Tone Value Table below
# String
P52782=content://settings/system/ringtone

############Ring Tone Value Table###############
# Web GUI Option                            Value
# Use System Ring tone                      content://settings/system/ringtone 
# Andromeda					/system/media/audio/ringtones/ANDROMEDA.ogg
# Aquila					/system/media/audio/ringtones/Aquila.ogg
# Argo Navis					/system/media/audio/ringtones/ArgoNavis.ogg
# Atria					/system/media/audio/ringtones/Atria.ogg
# Backroad					/system/media/audio/ringtones/Backroad.ogg
# Beat Plucker					/system/media/audio/ringtones/BeatPlucker.ogg
# Bell Phone					/system/media/audio/ringtones/Ring_Classic_02.ogg
# Bentley Dubs					/system/media/audio/ringtones/BentleyDubs.ogg
# Big Easy					/system/media/audio/ringtones/Big_Easy.ogg
# Bird Loop					/system/media/audio/ringtones/BirdLoop.ogg
# Bollywood					/system/media/audio/ringtones/Bollywood.ogg
# Boötes					/system/media/audio/ringtones/BOOTES.ogg
# Bus' a Move					/system/media/audio/ringtones/BussaMove.ogg
# Cairo					/system/media/audio/ringtones/Cairo.ogg
# Calypso Steel					/system/media/audio/ringtones/Calypso_Steel.ogg
# Canis Major					/system/media/audio/ringtones/CANISMAJOR.ogg
# Caribbean Ice					/system/media/audio/ringtones/CaribbeanIce.ogg
# Carina					/system/media/audio/ringtones/Carina.ogg
# Cassiopeia					/system/media/audio/ringtones/CASSIOPEIA.ogg
# Centaurus					/system/media/audio/ringtones/Centaurus.ogg
# Champagne Edition					/system/media/audio/ringtones/Champagne_Edition.ogg
# Chimey Phone					/system/media/audio/ringtones/Ring_Synth_02.ogg
# Club Cubano					/system/media/audio/ringtones/Club_Cubano.ogg
# Crayon Rock					/system/media/audio/ringtones/CrayonRock.ogg
# Crazy Dream					/system/media/audio/ringtones/CrazyDream.ogg
# Curve Ball Blend					/system/media/audio/ringtones/CurveBall.ogg
# Cygnus					/system/media/audio/ringtones/Cygnus.ogg
# Dancin' Fool					/system/media/audio/ringtones/DancinFool.ogg
# Digital Phone					/system/media/audio/ringtones/Ring_Digital_02.ogg
# Ding					/system/media/audio/ringtones/Ding.ogg
# DingDong					/system/media/audio/ringtones/DingDong.wav
# Don' Mess Wiv It					/system/media/audio/ringtones/DonMessWivIt.ogg
# Draco					/system/media/audio/ringtones/Draco.ogg
# Dream Theme					/system/media/audio/ringtones/DreamTheme.ogg
# Eastern Sky					/system/media/audio/ringtones/Eastern_Sky.ogg
# Enter the Nexus					/system/media/audio/ringtones/Enter_the_Nexus.ogg
# Eridani					/system/media/audio/ringtones/Eridani.ogg
# Ether Shake					/system/media/audio/ringtones/EtherShake.ogg
# Flutey Phone					/system/media/audio/ringtones/Ring_Synth_04.ogg
# Free Flight					/system/media/audio/ringtones/FreeFlight.ogg
# Friendly Ghost					/system/media/audio/ringtones/FriendlyGhost.ogg
# Funk Y'all					/system/media/audio/ringtones/Funk_Yall.ogg
# Game Over Guitar					/system/media/audio/ringtones/GameOverGuitar.ogg
# Gimme Mo' Town					/system/media/audio/ringtones/Gimme_Mo_Town.ogg
# Girtab					/system/media/audio/ringtones/Girtab.ogg
# Glacial Groove					/system/media/audio/ringtones/Glacial_Groove.ogg
# Growl					/system/media/audio/ringtones/Growl.ogg
# Halfway Home					/system/media/audio/ringtones/HalfwayHome.ogg
# Hydra					/system/media/audio/ringtones/Hydra.ogg
# Insert Coin					/system/media/audio/ringtones/InsertCoin.ogg
# Kuma					/system/media/audio/ringtones/Kuma.ogg
# Loopy Lounge					/system/media/audio/ringtones/LoopyLounge.ogg
# Love Flute					/system/media/audio/ringtones/LoveFlute.ogg
# Lyra					/system/media/audio/ringtones/Lyra.ogg
# Machina					/system/media/audio/ringtones/Machina.ogg
# Medieval Jaunt					/system/media/audio/ringtones/MidEvilJaunt.ogg
# Mildly Alarming					/system/media/audio/ringtones/MildlyAlarming.ogg
# Nairobi					/system/media/audio/ringtones/Nairobi.ogg
# Nassau					/system/media/audio/ringtones/Nassau.ogg
# New Player					/system/media/audio/ringtones/NewPlayer.ogg
# No Limits					/system/media/audio/ringtones/No_Limits.ogg
# Noisey One					/system/media/audio/ringtones/Noises1.ogg
# Organ Dub					/system/media/audio/ringtones/OrganDub.ogg
# Orion					/system/media/audio/ringtones/Orion.ogg
# Paradise Island					/system/media/audio/ringtones/Paradise_Island.ogg
# Pegasus					/system/media/audio/ringtones/Pegasus.ogg
# Perseus					/system/media/audio/ringtones/PERSEUS.ogg
# Playa					/system/media/audio/ringtones/Playa.ogg
# Pyxis					/system/media/audio/ringtones/Pyxis.ogg
# Rasalas					/system/media/audio/ringtones/Rasalas.ogg
# Revelation					/system/media/audio/ringtones/Revelation.ogg
# Rigel					/system/media/audio/ringtones/Rigel.ogg
# Road Trip					/system/media/audio/ringtones/Road_Trip.ogg
# Romancing The Tone					/system/media/audio/ringtones/RomancingTheTone.ogg
# Safari					/system/media/audio/ringtones/Safari.ogg
# Savannah					/system/media/audio/ringtones/Savannah.ogg
# Scarabaeus					/system/media/audio/ringtones/Scarabaeus.ogg
# Sceptrum					/system/media/audio/ringtones/Sceptrum.ogg
# Seville					/system/media/audio/ringtones/Seville.ogg
# She's All That					/system/media/audio/ringtones/Shes_All_That.ogg
# Silky Way					/system/media/audio/ringtones/SilkyWay.ogg
# Sitar Versus Sitar					/system/media/audio/ringtones/SitarVsSitar.ogg
# Solarium					/system/media/audio/ringtones/Solarium.ogg
# Springy Jalopy					/system/media/audio/ringtones/SpringyJalopy.ogg
# Steppin' Out					/system/media/audio/ringtones/Steppin_Out.ogg
# Terminated					/system/media/audio/ringtones/Terminated.ogg
# Terrible Twos					/system/media/audio/ringtones/Noises2.ogg
# Testudo					/system/media/audio/ringtones/Testudo.ogg
# Themos					/system/media/audio/ringtones/Themos.ogg
# Third Eye					/system/media/audio/ringtones/Third_Eye.ogg
# Thriller Three					/system/media/audio/ringtones/Noises3.ogg
# Thunderfoot					/system/media/audio/ringtones/Thunderfoot.ogg
# Twirl Away					/system/media/audio/ringtones/TwirlAway.ogg
# Ursa Minor					/system/media/audio/ringtones/URSAMINOR.ogg
# UrsaMinor					/system/media/audio/ringtones/UrsaMinor.ogg
# Very Alarmed					/system/media/audio/ringtones/VeryAlarmed.ogg
# Vespa					/system/media/audio/ringtones/Vespa.ogg
# World					/system/media/audio/ringtones/World.ogg
# Zeta					/system/media/audio/ringtones/Zeta.ogg
# bellcore-dr1					/system/media/audio/ringtones/bellcore-dr1.ogg
# bellcore-dr2					/system/media/audio/ringtones/bellcore-dr2.ogg
# bellcore-dr3					/system/media/audio/ringtones/bellcore-dr3.ogg
# bellcore-dr4					/system/media/audio/ringtones/bellcore-dr4.ogg
# bellcore-dr5					/system/media/audio/ringtones/bellcore-dr5.ogg
# speaker					/system/media/audio/ringtones/speaker.wav
#######################################################################
##  Account 8 Advanced Settings                                      ##
#######################################################################
# Check Domain Certificates. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P51711=0

# Validate Certificate Chain. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P51767=0

# Validate Incoming SIP Messages. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P51706=0

# Allow Unsolicited REFER. 0 - Disabled, 1 - Enabled, 2 - Enabled/Force Auth. Default value is 0.
# Number: 0, 1, 2
P52723=0

# Only Accept SIP Requests from Known Servers. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P51747=0

# Check SIP User ID for Incoming INVITE. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P50749=0

# Allow SIP Reset. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P52715=0

# Authenticate Incoming INVITE. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P51746=0

# SIP Realm Used for Challenge INVITE & NOTIFY.
# String
P52721=

# Enable Local MOH. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P51757=0

# Virtual Account Group. -1 - Default,  0 - Virtual Account Group 1, 1 - Virtual Account Group 2, 2 - Virtual Account Group 3
# 3 - Virtual Account Group 4, 4 - Virtual Account Group 5, 5 - Virtual Account Group 6, 6 - Virtual Account Group 7, 7 - Virtual Account Group 8
# 8 - Virtual Account Group 9, 9 - Virtual Account Group 10, 10 - Virtual Account Group 11, 11 - Virtual Account Group 12, 12 - Virtual Account Group 13
# 13 - Virtual Account Group 14, 14 - Virtual Account Group 15, 15 - Virtual Account Group 16. Default value is -1.
# Number: -1 - 15 
P51791=-1

# Special Feature. Default value is 100
# 100 - Standard, 102 - Broadsoft, 113 - China Mobile
# 114 - ZTE IMS, 115 - Mobotix, 116 - ZTE NGN, 117 - Huawei IMS, 123 - NEC, 125 - WorldStone
# Number: 100, 102, 113, 114, 115, 116, 117, 123, 125
P50724=100

# Allow Sync Phonebook via SIP Notify. 0 - No, 1 - Yes. Default is 1.
# Number: 0, 1
P52799=1
##############################################################################
##  Account 9 Settings                                                      ##
##############################################################################

#######################################################################
##  Account 9 General Settings                                       ##
#######################################################################

# Account Active. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P50801=0

# Account Name
P50817=

# SIP Server
P50802=

# SIP User ID
P50804=
 
# SIP Authentication ID
P50805=

# SIP Authentication Password
P50806=

# Voice Mail Access Number
P50826=

# Name (Display Name, e.g., John Doe)
P50807=

# Tel URI. 0 - Disable, 1 - User=Phone, 2 - Enabled. Default value is 0
# Number: 0, 1, 2
P50809=0

#######################################################################
##  Account 9 Network Settings                                       ##
#######################################################################

# Outbound Proxy
P50803=

# Secondary Outbound Proxy
P51833=

# DNS Mode. 0 - A Record, 1 - SRV, 2 - NAPTR/SRV. Default value is 0
# Number: 0, 1, 2
P50808=0

# DNS SRV Fail-over Mode. 0 - Default, 1 - Saved one until DNS TTL, 2 - Saved one until no response. Defualt value is 1
# Number
P52840=0

# Register Before DNS SRV Fail-over. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P53895=0

# NAT Traversal. 0 - NAT No, 1 - STUN, 2 - Keep-alive, 3 - UPnP, 4 - Auto, 5 - VPN. Default value is 2
# Number: 0, 1, 2, 3, 4, 5
P50814=2

# Proxy-Require
P50818=

#######################################################################
##  Account 9 SIP Settings                                           ##
#######################################################################

# SIP Registration. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P50810=1

# Unregister Before New Registration. 0 - No, 1 - All, 2 -  Instance . Default value is 2
# Number: 0, 1, 2
P50811=2

# Register Expiration (m). In minutes. Default value is 60
# Number: 0 - 64800
P50812=60

# Subscribe Expiration (m). Default is 60
# Number: 0 - 64800
P52851=60

# Re-register before Expiration (s). Default Value is 0
# Number : 0
P51830=0

# Registration Retry Wait Time (s). In seconds. Default value is 20
# Number: 1 - 3600
P50871=20

# Local SIP Port. Default value is 5076
# Number: 5 - 65535
P50813=5076

# SUBSCRIBE For MWI. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P50815=0

# Enable SIP OPTIONS Keep Alive. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P51897=0

# SIP OPTIONS Keep Alive Interval(s). Default value is 30
# Number 
P51898=30

# SIP OPTIONS Keep Alive Maximum Tries. Default value is 3
# Number 
P51899=3

# Enable Session Timer/ Session Expiration(s).  In seconds. Default value is 180 seconds.
# By default,  Session Timer is Enabled.  Session Timer is disabled if the value is 0.
# Number: 0 or 90 - 64800
P50834=180

# Min-SE(s). Default value is 90 seconds
# Number: 90 - 64800
P50827=90

# UAC Specify Refresher. 0 - Omit, 1 - UAC, 2 - UAS. Default value is 0
# Number: 0, 1, 2
P50832=0

# UAS Specify Refresher. 1 - UAC, 2 - UAS. Default value is 1
# Number: 1, 2
P50833=1

# Force INVITE. Always refresh with INVITE instead of UPDATE even when remote party supports UPDATE
# 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P50831=0

# Caller Request Timer. Request for timer when calling
# 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P50828=0

# Callee Request Timer
# Request for timer when being called (i.e., if remote party supports timer but did not request for one)
# 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P50829=0

# Force Timer. Still use timer when remote party does not support timer
# 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P50830=0

# Enable 100rel. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P50835=0

# Use Privacy Header
# 0 - Default, 1 - No, 2 - Yes. Default is 0
# Number: 0, 1, 2
P51838=0

# Use P-Preferred-Identity Header
# 0 - Default, 1 - No, 2 - Yes. Default is 0
# Number: 0, 1, 2
P51839=0

# Use P-Access-Network-Info Header. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P52858=1

# Use P-Emergency-Info Header. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P52859=1

# Use MAC Header.  0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P52861=0

# SIP Transport
# 0 - UDP , 1 - TCP, 2 - TLS. Default value is 0
# Number: 0, 1, 2
P50848=0

# SIP URI Scheme When Using TLS
# 0 -sip, 1 - sips. Default value is 0.
# Number: 0, 1
P51829=0

# Use Actual Ephemeral Port in Contact with TCP/TLS
# 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P51831=0

# Support SIP Instance ID
# 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P50889=1

# Add Auth Header On RE-REGISTER
# 0 - No, 1- Yes
P51859=1

# SIP T1 Timeout. RFC 3261 T1 value (RTT estimate)
# 50 - 0.5 sec, 100 - 1 sec, 200 - 2 sec. Default value is 50
# Number: 50, 100, 200
P50840=50

# SIP T2 Interval. RFC 3261 T2 value
# The maximum retransmit interval for non-INVITE requests and INVITE responses
# 200 - 2 sec, 400 - 4 sec, 800 - 8 sec. Default value is 400
# Number: 200, 400, 800.
P50841=400

# SIP Timer D Interval (Seconds)
# Number 0-64. Default value is 0
P51887=0

# Remove OBP from Route
# 0 - Disable, 1 - Enable, 2 - Always. Default value is 0
# Number: 0, 1, 2
P51805=0
#######################################################################
##  Account 9 Codec Settings                                         ##
#######################################################################
# Preferred Vocoder
# First codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 123 - Opus. Default value is 0
# Number: 0, 8, 9, 2, 18, 98, 123
P50851=0

# Second codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 123 - Opus. Default value is 8
# Number: 0, 8, 9, 2, 18, 98, 123
P50852=8

# Third codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 123 - Opus. Default value is 9
# Number: 0, 8, 9, 2, 18, 98, 123
P50853=9

# Forth codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 123 - Opus. Default value is 9
# Number: 0, 8, 9, 2, 18, 98, 123
P50854=9

# Fifth codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 123 - Opus. Default value is 9
# Number: 0, 8, 9, 2, 18, 98, 123
P50855=9

# Sixth codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 123 - Opus. Default value is 9
# Number: 0, 8, 9, 2, 18, 98, 123
P50856=9

# Seventh codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 123 - Opus. Default value is 9
# Number: 0, 8, 9, 2, 18, 98, 123
P50857=9

# Eigth codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 123 - Opus. Default value is 9
# Number: 0, 8, 9, 2, 18, 98, 123
P50858=9

# Codec Negotiation Priority. 0 - Caller, 1 - Callee. Default value is 1.
# Number: 0, 1
P53861=1

# Use First Matching Vocoder in 200OK SDP. 0 - No, 1 - Yes. The default value is 0.
# Number: 0, 1
P51848=0

# iLBC Frame Size. 0 - 20 ms, 1 - 30 ms. Default value is 1.
# Number: 0, 1
P50895=1

# G726-32 ITU Payload. 0 - 2, 1 - Dynamic. Default value is 0.
# Number: 0, 1
P51869=0

# G726-32 Dynamic PT. Default value is 126.
# Number
P51865=126

# Opus Payload Type
P51885=123

# DTMF: in audio. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P51801=0

# DTMF: via RFC2833. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P51802=1

# DTMF: via SIP INFO. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P51803=0

# DTMF Payload Type. Default value is 101
# Number: 96 - 126
P50896=101

# Enable Audio RED with FEC. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P52873=0

# Audio FEC Payload Type. Default value is 121
# Number: 96 - 126
P52874=121

# Audio RED Payload Type. Default value is 124
# Number: 96 - 126
P52875=124

# Silence Suppression. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P50885=0

# Voice Frames Per TX. Default value is 2
# Number: 1 - 64.
P50886=2

# Preferred Video Codec. 99 - H.264. Default is 99.
P50864=99

# Enable Video FEC. 0 - No, 1 - Yes. Default value is 1.
# Number: 0, 1
P51893=1

# Enable RFC5168 Support. 0 - No, 1 - Yes. Default value is 1.
# Number: 0, 1
P50878=1

# Video FEC Mode. 0 - 0, 1 - 1. Default value is 0.
# Number: 0, 1
P52822=0

# FEC Payload Type. Default value is 120.
P51894=120

# Packetization mode. 0 - Single NAL Unit Mode, 1 - Non-Interleaved Mode. Default value is 1.
# Number: 0, 1, 10
P52805=1

# H.264 Image Size. 9 - 720P, 1 - VGA, 5 - CIF, 4 - 4CIF, 0 - QVGA, 6 - QCIF. Default value is 9
# Number: 9, 1, 5, 4, 0, 6
P51807=9

# Use H.264 Constrained Profiles. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1
P52845=0

# H.264 Profile Type. 0 - Baseline Profile, 1 - Main Profile, 2 - High Profile, 3 - BP&MP&HP
# Number: 0, 1, 2, 3
P51862=0

# Video Bit Rate. 64 - 64 kbps, 96 - 96 kbps, 128 - 128 kbps, 160 - 160 kbps, 192 - 192 kbps
# 210 - 210 kbps, 256 - 256 kbps, 384 - 384 kbps, 512 - 512 kbps, 640 - 640 kbps, 768 - 768 kbps
# 1024 - 1024 kbps, 1280 - 1280 kbps, 1536 - 1536 kbps, 2048 - 2048 kbps. Default value is 2048.
# Number: 250, 500, 750
P51815=2048

# SDP Bandwidth Attribute. 0 - Standard, 1 - Media Level, 2 - Session Level, 3 - None. Default value is Media Level.
# Number: 0, 1, 2, 3
P51860=1

# H.264 Payload Type. Default value is 99.
P50862=99

# Disable BFCP. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1
P52801=0

# Presentation H.264 Image Size. 10 - 1080P, 9 - 720P. Default value is 10.
# Number: 10, 9
P51876=10

# Presentation H.264 Profile Type. 0 - Baseline Profile, 1 - Main Profile, 2 - High Profile, 3 - BP&MP&HP
# Number: 0, 1, 2, 3
P51877=3

# Presentation Video Bit Rate. 512 - 512 kbps, 640 - 640 kbps, 768 - 768 kbps
# 1024 - 1024 kbps, 1280 - 1280 kbps, 1536 - 1536 kbps, 2048 - 2048 kbps. Default value is 1024.
# Number: 250, 500, 750
P51878=1024

# Presentation Video Frame Rate. 5 - 5 frames/second, 10 - 10 frames/second, 15 - 15 frames/second. Default value is 15.
# Number: 5, 10, 15
P52842=

# BFCP Transport Protocol. 0 - Automatic, 1 - UDP, 2 - TCP. Default value is 1.
# Number: 0, 1, 2
P52841=

# SRTP Mode. 0 - Disable, 1 - Enable but not forced, 2 - Enable and forced. Default value is 0
# Number:0, 1, 2
P50843=0

# SRTP Key Length. 0 - AES 128&256 bit, 1 - AES 128 bit, 2 - AES 256 bit. Default value is 0
# Number:0, 1, 2
P51883=0 

# Enable SRTP Key Lifetime. 0 - No, 1 - Yes.
# Number: 0,1
P51863=0

# RTCP Destination
P51890=

# Symmetric RTP. 0 - No, 1 - Yes. Default value is 0
# Number:0, 1
P50860=0

# RTP IP Filter. 0 - Disable, 1 - IP Only, 2 - IP and Port. Default value is 0
# Number:0, 1, 2
P52826=0

# RTP Timeout(s). Default is 0. If set to 0, the device would not hangup.
# number: 0 - 600
P53868=0
#######################################################################
##  Account 9 Call Settings                                          ##
#######################################################################
# Enable Video Call. 0 - Default, 1 - No, 2 - Yes. Default is 0
# Number: 0, 1, 2
P60843=0

# Start Video Automatically. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P51814=1

# Remote Video Request. 0 - Prompt, 1 - Accept, 2 - Deny. Default value is 0
# Number: 0, 1, 2
P51826=0

# Video Layout. 0 - Default, 1 - Full screen, 3 - Equal split screen, 2 - Only display remote screen
P51832=0

# Auto Answer. 0 - No, 1 - Yes, 2 - Enable Intercom/Paging. Default value is 0
# Number: 0, 1, 2
P50825=0

# Play warning tone for Auto Answer Intercom. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P52872=1

# Intercom Barging. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P52819=1

# Auto Preview. 0 - No, 1 - Yes, 2 - Yes with Ringing. Default value is 0
# Number: 0, 1, 2
P53862=0

# Send Anonymous. 0 - No, 1 - Yes (caller ID will be blocked if set to Yes). Default value is 0
# Number: 0, 1
P50821=0

# Anonymous Call Rejection. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P50846=0

# Call Log
# 0 - Log All, 1 - Log Incoming/Outgoing only (Missed Calls Not Recorded), 2 - Disable Call All, 3 - Don't Prompt Missed Call. Default value is 0
# Number: 0, 1, 2
P50842=0

# Enable Call Features. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P50820=0

# Enable Call Waiting. 0 - Default, 1 - No, 2 - Yes.
# Number: 0, 1, 2
P52863=0

# Mute on Answer Intercom Call. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
P52871=0

# Transfer on 3 way conference Hangup. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P51804=0

# Use # as Dial Key. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P50892=1

# Use # as Redial Key. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P53869=1

# DND Call Feature On.
# String
P51844=

# DND Call Feature Off.
# String
P51845=

# No Key Entry Timeout (s). Default value is 4
# Number: 1 - 15
P50891=4

# Ring Timeout (s). Default value is 60
# Number: 10 - 300
P50876=60

# Refer-To Use Target Contact. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P50869=0

# RFC2543 Hold. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1 
P52862=1

# Dial Plan Prefix
# String
P50819=

# Disable DialPlan. 0 - No Selection, 1 - Dial Page, 2 - Contact, 4 - Incoming Call History, 8 -  Outgoing Call History, 16 - MPK & Click2Dial. 
# If need to check multiple selections, add the specific values for each selections together. Default value is 0
# Number: 0-31
P51882=0

# DialPlan. Default value is { x+ | \+x+ | *x+ | *xx*x+ | x+*x+*x+*x+ | x+*x+*x+*x+#x+ }
P50859={ x+ | \+x+ | *x+ | *xx*x+ | x+*x+*x+*x+ | x+*x+*x+*x+#x+ }

# Caller ID Display. 0 - Auto, 1 - Disabled, 2 - From Header. The default value is 0.
# Number: 0, 1, 2, 3
P51824=0

# Account Ringtone. See ring tone options and value in the Ring Tone Value Table below
P50823=content://settings/system/ringtone

# Ignore Alert-Info Header. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1
P52818=0

# Matching Incoming Caller ID. Matching Rule 1
# String
P52877=

# Matching Rule 1 Distinctive Ringtone. See ring tone options and value in the Ring Tone Value Table below
# String
P52878=content://settings/system/ringtone

# Matching Incoming Caller ID. Matching Rule 2
# String
P52879=

# Matching Rule 2 Distinctive Ringtone. See ring tone options and value in the Ring Tone Value Table below
# String
P52880=content://settings/system/ringtone

# Matching Incoming Caller ID. Matching Rule 3
# String
P52881=

# Matching Rule 3 Distinctive Ringtone. See ring tone options and value in the Ring Tone Value Table below
# String
P52882=content://settings/system/ringtone

############Ring Tone Value Table###############
# Web GUI Option                            Value
# Use System Ring tone                      content://settings/system/ringtone 
# Andromeda					/system/media/audio/ringtones/ANDROMEDA.ogg
# Aquila					/system/media/audio/ringtones/Aquila.ogg
# Argo Navis					/system/media/audio/ringtones/ArgoNavis.ogg
# Atria					/system/media/audio/ringtones/Atria.ogg
# Backroad					/system/media/audio/ringtones/Backroad.ogg
# Beat Plucker					/system/media/audio/ringtones/BeatPlucker.ogg
# Bell Phone					/system/media/audio/ringtones/Ring_Classic_02.ogg
# Bentley Dubs					/system/media/audio/ringtones/BentleyDubs.ogg
# Big Easy					/system/media/audio/ringtones/Big_Easy.ogg
# Bird Loop					/system/media/audio/ringtones/BirdLoop.ogg
# Bollywood					/system/media/audio/ringtones/Bollywood.ogg
# Boötes					/system/media/audio/ringtones/BOOTES.ogg
# Bus' a Move					/system/media/audio/ringtones/BussaMove.ogg
# Cairo					/system/media/audio/ringtones/Cairo.ogg
# Calypso Steel					/system/media/audio/ringtones/Calypso_Steel.ogg
# Canis Major					/system/media/audio/ringtones/CANISMAJOR.ogg
# Caribbean Ice					/system/media/audio/ringtones/CaribbeanIce.ogg
# Carina					/system/media/audio/ringtones/Carina.ogg
# Cassiopeia					/system/media/audio/ringtones/CASSIOPEIA.ogg
# Centaurus					/system/media/audio/ringtones/Centaurus.ogg
# Champagne Edition					/system/media/audio/ringtones/Champagne_Edition.ogg
# Chimey Phone					/system/media/audio/ringtones/Ring_Synth_02.ogg
# Club Cubano					/system/media/audio/ringtones/Club_Cubano.ogg
# Crayon Rock					/system/media/audio/ringtones/CrayonRock.ogg
# Crazy Dream					/system/media/audio/ringtones/CrazyDream.ogg
# Curve Ball Blend					/system/media/audio/ringtones/CurveBall.ogg
# Cygnus					/system/media/audio/ringtones/Cygnus.ogg
# Dancin' Fool					/system/media/audio/ringtones/DancinFool.ogg
# Digital Phone					/system/media/audio/ringtones/Ring_Digital_02.ogg
# Ding					/system/media/audio/ringtones/Ding.ogg
# DingDong					/system/media/audio/ringtones/DingDong.wav
# Don' Mess Wiv It					/system/media/audio/ringtones/DonMessWivIt.ogg
# Draco					/system/media/audio/ringtones/Draco.ogg
# Dream Theme					/system/media/audio/ringtones/DreamTheme.ogg
# Eastern Sky					/system/media/audio/ringtones/Eastern_Sky.ogg
# Enter the Nexus					/system/media/audio/ringtones/Enter_the_Nexus.ogg
# Eridani					/system/media/audio/ringtones/Eridani.ogg
# Ether Shake					/system/media/audio/ringtones/EtherShake.ogg
# Flutey Phone					/system/media/audio/ringtones/Ring_Synth_04.ogg
# Free Flight					/system/media/audio/ringtones/FreeFlight.ogg
# Friendly Ghost					/system/media/audio/ringtones/FriendlyGhost.ogg
# Funk Y'all					/system/media/audio/ringtones/Funk_Yall.ogg
# Game Over Guitar					/system/media/audio/ringtones/GameOverGuitar.ogg
# Gimme Mo' Town					/system/media/audio/ringtones/Gimme_Mo_Town.ogg
# Girtab					/system/media/audio/ringtones/Girtab.ogg
# Glacial Groove					/system/media/audio/ringtones/Glacial_Groove.ogg
# Growl					/system/media/audio/ringtones/Growl.ogg
# Halfway Home					/system/media/audio/ringtones/HalfwayHome.ogg
# Hydra					/system/media/audio/ringtones/Hydra.ogg
# Insert Coin					/system/media/audio/ringtones/InsertCoin.ogg
# Kuma					/system/media/audio/ringtones/Kuma.ogg
# Loopy Lounge					/system/media/audio/ringtones/LoopyLounge.ogg
# Love Flute					/system/media/audio/ringtones/LoveFlute.ogg
# Lyra					/system/media/audio/ringtones/Lyra.ogg
# Machina					/system/media/audio/ringtones/Machina.ogg
# Medieval Jaunt					/system/media/audio/ringtones/MidEvilJaunt.ogg
# Mildly Alarming					/system/media/audio/ringtones/MildlyAlarming.ogg
# Nairobi					/system/media/audio/ringtones/Nairobi.ogg
# Nassau					/system/media/audio/ringtones/Nassau.ogg
# New Player					/system/media/audio/ringtones/NewPlayer.ogg
# No Limits					/system/media/audio/ringtones/No_Limits.ogg
# Noisey One					/system/media/audio/ringtones/Noises1.ogg
# Organ Dub					/system/media/audio/ringtones/OrganDub.ogg
# Orion					/system/media/audio/ringtones/Orion.ogg
# Paradise Island					/system/media/audio/ringtones/Paradise_Island.ogg
# Pegasus					/system/media/audio/ringtones/Pegasus.ogg
# Perseus					/system/media/audio/ringtones/PERSEUS.ogg
# Playa					/system/media/audio/ringtones/Playa.ogg
# Pyxis					/system/media/audio/ringtones/Pyxis.ogg
# Rasalas					/system/media/audio/ringtones/Rasalas.ogg
# Revelation					/system/media/audio/ringtones/Revelation.ogg
# Rigel					/system/media/audio/ringtones/Rigel.ogg
# Road Trip					/system/media/audio/ringtones/Road_Trip.ogg
# Romancing The Tone					/system/media/audio/ringtones/RomancingTheTone.ogg
# Safari					/system/media/audio/ringtones/Safari.ogg
# Savannah					/system/media/audio/ringtones/Savannah.ogg
# Scarabaeus					/system/media/audio/ringtones/Scarabaeus.ogg
# Sceptrum					/system/media/audio/ringtones/Sceptrum.ogg
# Seville					/system/media/audio/ringtones/Seville.ogg
# She's All That					/system/media/audio/ringtones/Shes_All_That.ogg
# Silky Way					/system/media/audio/ringtones/SilkyWay.ogg
# Sitar Versus Sitar					/system/media/audio/ringtones/SitarVsSitar.ogg
# Solarium					/system/media/audio/ringtones/Solarium.ogg
# Springy Jalopy					/system/media/audio/ringtones/SpringyJalopy.ogg
# Steppin' Out					/system/media/audio/ringtones/Steppin_Out.ogg
# Terminated					/system/media/audio/ringtones/Terminated.ogg
# Terrible Twos					/system/media/audio/ringtones/Noises2.ogg
# Testudo					/system/media/audio/ringtones/Testudo.ogg
# Themos					/system/media/audio/ringtones/Themos.ogg
# Third Eye					/system/media/audio/ringtones/Third_Eye.ogg
# Thriller Three					/system/media/audio/ringtones/Noises3.ogg
# Thunderfoot					/system/media/audio/ringtones/Thunderfoot.ogg
# Twirl Away					/system/media/audio/ringtones/TwirlAway.ogg
# Ursa Minor					/system/media/audio/ringtones/URSAMINOR.ogg
# UrsaMinor					/system/media/audio/ringtones/UrsaMinor.ogg
# Very Alarmed					/system/media/audio/ringtones/VeryAlarmed.ogg
# Vespa					/system/media/audio/ringtones/Vespa.ogg
# World					/system/media/audio/ringtones/World.ogg
# Zeta					/system/media/audio/ringtones/Zeta.ogg
# bellcore-dr1					/system/media/audio/ringtones/bellcore-dr1.ogg
# bellcore-dr2					/system/media/audio/ringtones/bellcore-dr2.ogg
# bellcore-dr3					/system/media/audio/ringtones/bellcore-dr3.ogg
# bellcore-dr4					/system/media/audio/ringtones/bellcore-dr4.ogg
# bellcore-dr5					/system/media/audio/ringtones/bellcore-dr5.ogg
# speaker					/system/media/audio/ringtones/speaker.wav
#######################################################################
##  Account 9 Advanced Settings                                      ##
#######################################################################
# Check Domain Certificates. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P51811=0

# Validate Certificate Chain. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P51867=0

# Validate Incoming SIP Messages. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P51806=0

# Allow Unsolicited REFER. 0 - Disabled, 1 - Enabled, 2 - Enabled/Force Auth. Default value is 0.
# Number: 0, 1, 2
P52823=0

# Only Accept SIP Requests from Known Servers. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P51847=0

# Check SIP User ID for Incoming INVITE. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P50849=0

# Allow SIP Reset. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P52815=0

# Authenticate Incoming INVITE. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P51846=0

# SIP Realm Used for Challenge INVITE & NOTIFY.
# String
P52821=

# Enable Local MOH. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P51857=0

# Virtual Account Group. -1 - Default,  0 - Virtual Account Group 1, 1 - Virtual Account Group 2, 2 - Virtual Account Group 3
# 3 - Virtual Account Group 4, 4 - Virtual Account Group 5, 5 - Virtual Account Group 6, 6 - Virtual Account Group 7, 7 - Virtual Account Group 8
# 8 - Virtual Account Group 9, 9 - Virtual Account Group 10, 10 - Virtual Account Group 11, 11 - Virtual Account Group 12, 12 - Virtual Account Group 13
# 13 - Virtual Account Group 14, 14 - Virtual Account Group 15, 15 - Virtual Account Group 16. Default value is -1.
# Number: -1 - 15 
P51891=-1

# Special Feature. Default value is 100
# 100 - Standard, 102 - Broadsoft, 113 - China Mobile
# 114 - ZTE IMS, 115 - Mobotix, 116 - ZTE NGN, 117 - Huawei IMS, 123 - NEC, 125 - WorldStone
# Number: 100, 102, 113, 114, 115, 116, 117, 123, 125
P50824=100

# Allow Sync Phonebook via SIP Notify. 0 - No, 1 - Yes. Default is 1.
# Number: 0, 1
P52899=1
##############################################################################
##  Account 10 Settings                                                     ##
##############################################################################

#######################################################################
##  Account 10 General Settings                                      ##
#######################################################################

# Account Active. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P50901=0

# Account Name
P50917=

# SIP Server
P50902=

# SIP User ID
P50904=
 
# SIP Authentication ID
P50905=

# SIP Authentication Password
P50906=

# Voice Mail Access Number
P50926=

# Name (Display Name, e.g., John Doe)
P50907=

# Tel URI. 0 - Disable, 1 - User=Phone, 2 - Enabled. Default value is 0
# Number: 0, 1, 2
P50909=0

#######################################################################
##  Account 10 Network Settings                                      ##
#######################################################################

# Outbound Proxy
P50903=

# Secondary Outbound Proxy
P51933=

# DNS Mode. 0 - A Record, 1 - SRV, 2 - NAPTR/SRV. Default value is 0
# Number: 0, 1, 2
P50908=0

# DNS SRV Fail-over Mode. 0 - Default, 1 - Saved one until DNS TTL, 2 - Saved one until no response. Defualt value is 1
# Number
P52940=0

# Register Before DNS SRV Fail-over. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P53995=0

# NAT Traversal. 0 - NAT No, 1 - STUN, 2 - Keep-alive, 3 - UPnP, 4 - Auto, 5 - VPN. Default value is 2
# Number: 0, 1, 2, 3, 4, 5
P50914=2

# Proxy-Require
P50918=

#######################################################################
##  Account 10 SIP Settings                                          ##
#######################################################################

# SIP Registration. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P50910=1

# Unregister Before New Registration. 0 - No, 1 - All, 2 -  Instance . Default value is 2
# Number: 0, 1, 2
P50911=2

# Register Expiration (m). In minutes. Default value is 60
# Number: 0 - 64800
P50912=60

# Subscribe Expiration (m). Default is 60
# Number: 0 - 64800
P52951=60

# Re-register before Expiration (s). Default Value is 0
# Number : 0
P51930=0

# Registration Retry Wait Time (s). In seconds. Default value is 20
# Number: 1 - 3600
P50971=20

# Local SIP Port. Default value is 5078
# Number: 5 - 65535
P50913=5078

# SUBSCRIBE For MWI. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P50915=0

# Enable SIP OPTIONS Keep Alive. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P51997=0

# SIP OPTIONS Keep Alive Interval(s). Default value is 30
# Number 
P51998=30

# SIP OPTIONS Keep Alive Maximum Tries. Default value is 3
# Number 
P51999=3

# Enable Session Timer/ Session Expiration(s).  In seconds. Default value is 180 seconds.
# By default,  Session Timer is Enabled.  Session Timer is disabled if the value is 0.
# Number: 0 or 90 - 64800
P50934=180

# Min-SE(s). Default value is 90 seconds
# Number: 90 - 64800
P50927=90

# UAC Specify Refresher. 0 - Omit, 1 - UAC, 2 - UAS. Default value is 0
# Number: 0, 1, 2
P50932=0

# UAS Specify Refresher. 1 - UAC, 2 - UAS. Default value is 1
# Number: 1, 2
P50933=1

# Force INVITE. Always refresh with INVITE instead of UPDATE even when remote party supports UPDATE
# 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P50931=0

# Caller Request Timer. Request for timer when calling
# 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P50928=0

# Callee Request Timer
# Request for timer when being called (i.e., if remote party supports timer but did not request for one)
# 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P50929=0

# Force Timer. Still use timer when remote party does not support timer
# 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P50930=0

# Enable 100rel. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P50935=0

# Use Privacy Header
# 0 - Default, 1 - No, 2 - Yes. Default is 0
# Number: 0, 1, 2
P51938=0

# Use P-Preferred-Identity Header
# 0 - Default, 1 - No, 2 - Yes. Default is 0
# Number: 0, 1, 2
P51939=0

# Use P-Access-Network-Info Header. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P52958=1

# Use P-Emergency-Info Header. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P52959=1

# Use MAC Header.  0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P52961=0

# SIP Transport
# 0 - UDP , 1 - TCP, 2 - TLS. Default value is 0
# Number: 0, 1, 2
P50948=0

# SIP URI Scheme When Using TLS
# 0 -sip, 1 - sips. Default value is 0.
# Number: 0, 1
P51929=0

# Use Actual Ephemeral Port in Contact with TCP/TLS
# 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P51931=0

# Support SIP Instance ID
# 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P50989=1

# Add Auth Header On RE-REGISTER
# 0 - No, 1- Yes
P51959=1

# SIP T1 Timeout. RFC 3261 T1 value (RTT estimate)
# 50 - 0.5 sec, 100 - 1 sec, 200 - 2 sec. Default value is 50
# Number: 50, 100, 200
P50940=50

# SIP T2 Interval. RFC 3261 T2 value
# The maximum retransmit interval for non-INVITE requests and INVITE responses
# 200 - 2 sec, 400 - 4 sec, 800 - 8 sec. Default value is 400
# Number: 200, 400, 800.
P50941=400

# SIP Timer D Interval (Seconds)
# Number 0-64. Default value is 0
P51987=0

# Remove OBP from Route
# 0 - Disable, 1 - Enable, 2 - Always. Default value is 0
# Number: 0, 1, 2
P51905=0
#######################################################################
##  Account 10 Codec Settings                                        ##
#######################################################################
# Preferred Vocoder
# First codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 123 - Opus. Default value is 0
# Number: 0, 8, 9, 2, 18, 98, 123
P50951=0

# Second codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 123 - Opus. Default value is 8
# Number: 0, 8, 9, 2, 18, 98, 123
P50952=8

# Third codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 123 - Opus. Default value is 9
# Number: 0, 8, 9, 2, 18, 98, 123
P50953=9

# Forth codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 123 - Opus. Default value is 9
# Number: 0, 8, 9, 2, 18, 98, 123
P50954=9

# Fifth codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 123 - Opus. Default value is 9
# Number: 0, 8, 9, 2, 18, 98, 123
P50955=9

# Sixth codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 123 - Opus. Default value is 9
# Number: 0, 8, 9, 2, 18, 98, 123
P50956=9

# Seventh codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 123 - Opus. Default value is 9
# Number: 0, 8, 9, 2, 18, 98, 123
P50957=9

# Eigth codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 123 - Opus. Default value is 9
# Number: 0, 8, 9, 2, 18, 98, 123
P50958=9

# Codec Negotiation Priority. 0 - Caller, 1 - Callee. Default value is 1.
# Number: 0, 1
P53961=1

# Use First Matching Vocoder in 200OK SDP. 0 - No, 1 - Yes. The default value is 0.
# Number: 0, 1
P51948=0

# iLBC Frame Size. 0 - 20 ms, 1 - 30 ms. Default value is 1.
# Number: 0, 1
P50995=1

# G726-32 ITU Payload. 0 - 2, 1 - Dynamic. Default value is 0.
# Number: 0, 1
P51969=0

# G726-32 Dynamic PT. Default value is 126.
# Number
P51965=126

# Opus Payload Type
P51985=123

# DTMF: in audio. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P51901=0

# DTMF: via RFC2833. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P51902=1

# DTMF: via SIP INFO. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P51903=0

# DTMF Payload Type. Default value is 101
# Number: 96 - 126
P50996=101

# Enable Audio RED with FEC. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P52973=0

# Audio FEC Payload Type. Default value is 121
# Number: 96 - 126
P52974=121

# Audio RED Payload Type. Default value is 124
# Number: 96 - 126
P52975=124

# Silence Suppression. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P50985=0

# Voice Frames Per TX. Default value is 2
# Number: 1 - 64.
P50986=2

# Preferred Video Codec. 99 - H.264. Default is 99.
P50964=99

# Enable Video FEC. 0 - No, 1 - Yes. Default value is 1.
# Number: 0, 1
P51993=1

# Enable RFC5168 Support. 0 - No, 1 - Yes. Default value is 1.
# Number: 0, 1
P50978=1

# Video FEC Mode. 0 - 0, 1 - 1. Default value is 0.
# Number: 0, 1
P52922=0

# FEC Payload Type. Default value is 120.
P51994=120

# Packetization mode. 0 - Single NAL Unit Mode, 1 - Non-Interleaved Mode. Default value is 1.
# Number: 0, 1, 10
P52905=1

# H.264 Image Size. 9 - 720P, 1 - VGA, 5 - CIF, 4 - 4CIF, 0 - QVGA, 6 - QCIF. Default value is 9
# Number: 9, 1, 5, 4, 0, 6
P51907=9

# Use H.264 Constrained Profiles. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1
P52945=0

# H.264 Profile Type. 0 - Baseline Profile, 1 - Main Profile, 2 - High Profile, 3 - BP&MP&HP
# Number: 0, 1, 2, 3
P51962=0

# Video Bit Rate. 64 - 64 kbps, 96 - 96 kbps, 128 - 128 kbps, 160 - 160 kbps, 192 - 192 kbps
# 210 - 210 kbps, 256 - 256 kbps, 384 - 384 kbps, 512 - 512 kbps, 640 - 640 kbps, 768 - 768 kbps
# 1024 - 1024 kbps, 1280 - 1280 kbps, 1536 - 1536 kbps, 2048 - 2048 kbps. Default value is 2048.
# Number: 250, 500, 750
P51915=2048

# SDP Bandwidth Attribute. 0 - Standard, 1 - Media Level, 2 - Session Level, 3 - None. Default value is Media Level.
# Number: 0, 1, 2, 3
P51960=1

# H.264 Payload Type. Default value is 99.
P50962=99

# Disable BFCP. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1
P52901=0

# Presentation H.264 Image Size. 10 - 1080P, 9 - 720P. Default value is 10.
# Number: 10, 9
P51976=10

# Presentation H.264 Profile Type. 0 - Baseline Profile, 1 - Main Profile, 2 - High Profile, 3 - BP&MP&HP
# Number: 0, 1, 2, 3
P51977=3

# Presentation Video Bit Rate. 512 - 512 kbps, 640 - 640 kbps, 768 - 768 kbps
# 1024 - 1024 kbps, 1280 - 1280 kbps, 1536 - 1536 kbps, 2048 - 2048 kbps. Default value is 1024.
# Number: 250, 500, 750
P51978=1024

# Presentation Video Frame Rate. 5 - 5 frames/second, 10 - 10 frames/second, 15 - 15 frames/second. Default value is 15.
# Number: 5, 10, 15
P52942=

# BFCP Transport Protocol. 0 - Automatic, 1 - UDP, 2 - TCP. Default value is 1.
# Number: 0, 1, 2
P52941=

# SRTP Mode. 0 - Disable, 1 - Enable but not forced, 2 - Enable and forced. Default value is 0
# Number:0, 1, 2
P50943=0

# SRTP Key Length. 0 - AES 128&256 bit, 1 - AES 128 bit, 2 - AES 256 bit. Default value is 0
# Number:0, 1, 2
P51983=0 

# Enable SRTP Key Lifetime. 0 - No, 1 - Yes.
# Number: 0,1
P51963=0

# RTCP Destination
P51990=

# Symmetric RTP. 0 - No, 1 - Yes. Default value is 0
# Number:0, 1
P50960=0

# RTP IP Filter. 0 - Disable, 1 - IP Only, 2 - IP and Port. Default value is 0
# Number:0, 1, 2
P52926=0

# RTP Timeout(s). Default is 0. If set to 0, the device would not hangup.
# number: 0 - 600
P53968=0
#######################################################################
##  Account 10 Call Settings                                         ##
#######################################################################
# Enable Video Call. 0 - Default, 1 - No, 2 - Yes. Default is 0
# Number: 0, 1, 2
P60943=0

# Start Video Automatically. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P51914=1

# Remote Video Request. 0 - Prompt, 1 - Accept, 2 - Deny. Default value is 0
# Number: 0, 1, 2
P51926=0

# Video Layout. 0 - Default, 1 - Full screen, 3 - Equal split screen, 2 - Only display remote screen
P51932=0

# Auto Answer. 0 - No, 1 - Yes, 2 - Enable Intercom/Paging. Default value is 0
# Number: 0, 1, 2
P50925=0

# Play warning tone for Auto Answer Intercom. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P52972=1

# Intercom Barging. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P52919=1

# Auto Preview. 0 - No, 1 - Yes, 2 - Yes with Ringing. Default value is 0
# Number: 0, 1, 2
P53962=0

# Send Anonymous. 0 - No, 1 - Yes (caller ID will be blocked if set to Yes). Default value is 0
# Number: 0, 1
P50921=0

# Anonymous Call Rejection. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P50946=0

# Call Log
# 0 - Log All, 1 - Log Incoming/Outgoing only (Missed Calls Not Recorded), 2 - Disable Call All, 3 - Don't Prompt Missed Call. Default value is 0
# Number: 0, 1, 2
P50942=0

# Enable Call Features. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P50920=0

# Enable Call Waiting. 0 - Default, 1 - No, 2 - Yes.
# Number: 0, 1, 2
P52963=0

# Mute on Answer Intercom Call. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
P52971=0

# Transfer on 3 way conference Hangup. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P51904=0

# Use # as Dial Key. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P50992=1

# Use # as Redial Key. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P53969=1

# DND Call Feature On.
# String
P51944=

# DND Call Feature Off.
# String
P51945=

# No Key Entry Timeout (s). Default value is 4
# Number: 1 - 15
P50991=4

# Ring Timeout (s). Default value is 60
# Number: 10 - 300
P50976=60

# Refer-To Use Target Contact. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P50969=0

# RFC2543 Hold. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1 
P52962=1

# Dial Plan Prefix
# String
P50919=

# Disable DialPlan. 0 - No Selection, 1 - Dial Page, 2 - Contact, 4 - Incoming Call History, 8 -  Outgoing Call History, 16 - MPK & Click2Dial. 
# If need to check multiple selections, add the specific values for each selections together. Default value is 0
# Number: 0-31
P51982=0

# DialPlan. Default value is { x+ | \+x+ | *x+ | *xx*x+ | x+*x+*x+*x+ | x+*x+*x+*x+#x+ }
P50959={ x+ | \+x+ | *x+ | *xx*x+ | x+*x+*x+*x+ | x+*x+*x+*x+#x+ }

# Caller ID Display. 0 - Auto, 1 - Disabled, 2 - From Header. The default value is 0.
# Number: 0, 1, 2, 3
P51924=0

# Account Ringtone. See ring tone options and value in the Ring Tone Value Table below
P50923=content://settings/system/ringtone

# Ignore Alert-Info Header. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1
P52918=0

# Matching Incoming Caller ID. Matching Rule 1
# String
P52977=

# Matching Rule 1 Distinctive Ringtone. See ring tone options and value in the Ring Tone Value Table below
# String
P52978=content://settings/system/ringtone

# Matching Incoming Caller ID. Matching Rule 2
# String
P52979=

# Matching Rule 2 Distinctive Ringtone. See ring tone options and value in the Ring Tone Value Table below
# String
P52980=content://settings/system/ringtone

# Matching Incoming Caller ID. Matching Rule 3
# String
P52981=

# Matching Rule 3 Distinctive Ringtone. See ring tone options and value in the Ring Tone Value Table below
# String
P52982=content://settings/system/ringtone

############Ring Tone Value Table###############
# Web GUI Option                            Value
# Use System Ring tone                      content://settings/system/ringtone 
# Andromeda					/system/media/audio/ringtones/ANDROMEDA.ogg
# Aquila					/system/media/audio/ringtones/Aquila.ogg
# Argo Navis					/system/media/audio/ringtones/ArgoNavis.ogg
# Atria					/system/media/audio/ringtones/Atria.ogg
# Backroad					/system/media/audio/ringtones/Backroad.ogg
# Beat Plucker					/system/media/audio/ringtones/BeatPlucker.ogg
# Bell Phone					/system/media/audio/ringtones/Ring_Classic_02.ogg
# Bentley Dubs					/system/media/audio/ringtones/BentleyDubs.ogg
# Big Easy					/system/media/audio/ringtones/Big_Easy.ogg
# Bird Loop					/system/media/audio/ringtones/BirdLoop.ogg
# Bollywood					/system/media/audio/ringtones/Bollywood.ogg
# Boötes					/system/media/audio/ringtones/BOOTES.ogg
# Bus' a Move					/system/media/audio/ringtones/BussaMove.ogg
# Cairo					/system/media/audio/ringtones/Cairo.ogg
# Calypso Steel					/system/media/audio/ringtones/Calypso_Steel.ogg
# Canis Major					/system/media/audio/ringtones/CANISMAJOR.ogg
# Caribbean Ice					/system/media/audio/ringtones/CaribbeanIce.ogg
# Carina					/system/media/audio/ringtones/Carina.ogg
# Cassiopeia					/system/media/audio/ringtones/CASSIOPEIA.ogg
# Centaurus					/system/media/audio/ringtones/Centaurus.ogg
# Champagne Edition					/system/media/audio/ringtones/Champagne_Edition.ogg
# Chimey Phone					/system/media/audio/ringtones/Ring_Synth_02.ogg
# Club Cubano					/system/media/audio/ringtones/Club_Cubano.ogg
# Crayon Rock					/system/media/audio/ringtones/CrayonRock.ogg
# Crazy Dream					/system/media/audio/ringtones/CrazyDream.ogg
# Curve Ball Blend					/system/media/audio/ringtones/CurveBall.ogg
# Cygnus					/system/media/audio/ringtones/Cygnus.ogg
# Dancin' Fool					/system/media/audio/ringtones/DancinFool.ogg
# Digital Phone					/system/media/audio/ringtones/Ring_Digital_02.ogg
# Ding					/system/media/audio/ringtones/Ding.ogg
# DingDong					/system/media/audio/ringtones/DingDong.wav
# Don' Mess Wiv It					/system/media/audio/ringtones/DonMessWivIt.ogg
# Draco					/system/media/audio/ringtones/Draco.ogg
# Dream Theme					/system/media/audio/ringtones/DreamTheme.ogg
# Eastern Sky					/system/media/audio/ringtones/Eastern_Sky.ogg
# Enter the Nexus					/system/media/audio/ringtones/Enter_the_Nexus.ogg
# Eridani					/system/media/audio/ringtones/Eridani.ogg
# Ether Shake					/system/media/audio/ringtones/EtherShake.ogg
# Flutey Phone					/system/media/audio/ringtones/Ring_Synth_04.ogg
# Free Flight					/system/media/audio/ringtones/FreeFlight.ogg
# Friendly Ghost					/system/media/audio/ringtones/FriendlyGhost.ogg
# Funk Y'all					/system/media/audio/ringtones/Funk_Yall.ogg
# Game Over Guitar					/system/media/audio/ringtones/GameOverGuitar.ogg
# Gimme Mo' Town					/system/media/audio/ringtones/Gimme_Mo_Town.ogg
# Girtab					/system/media/audio/ringtones/Girtab.ogg
# Glacial Groove					/system/media/audio/ringtones/Glacial_Groove.ogg
# Growl					/system/media/audio/ringtones/Growl.ogg
# Halfway Home					/system/media/audio/ringtones/HalfwayHome.ogg
# Hydra					/system/media/audio/ringtones/Hydra.ogg
# Insert Coin					/system/media/audio/ringtones/InsertCoin.ogg
# Kuma					/system/media/audio/ringtones/Kuma.ogg
# Loopy Lounge					/system/media/audio/ringtones/LoopyLounge.ogg
# Love Flute					/system/media/audio/ringtones/LoveFlute.ogg
# Lyra					/system/media/audio/ringtones/Lyra.ogg
# Machina					/system/media/audio/ringtones/Machina.ogg
# Medieval Jaunt					/system/media/audio/ringtones/MidEvilJaunt.ogg
# Mildly Alarming					/system/media/audio/ringtones/MildlyAlarming.ogg
# Nairobi					/system/media/audio/ringtones/Nairobi.ogg
# Nassau					/system/media/audio/ringtones/Nassau.ogg
# New Player					/system/media/audio/ringtones/NewPlayer.ogg
# No Limits					/system/media/audio/ringtones/No_Limits.ogg
# Noisey One					/system/media/audio/ringtones/Noises1.ogg
# Organ Dub					/system/media/audio/ringtones/OrganDub.ogg
# Orion					/system/media/audio/ringtones/Orion.ogg
# Paradise Island					/system/media/audio/ringtones/Paradise_Island.ogg
# Pegasus					/system/media/audio/ringtones/Pegasus.ogg
# Perseus					/system/media/audio/ringtones/PERSEUS.ogg
# Playa					/system/media/audio/ringtones/Playa.ogg
# Pyxis					/system/media/audio/ringtones/Pyxis.ogg
# Rasalas					/system/media/audio/ringtones/Rasalas.ogg
# Revelation					/system/media/audio/ringtones/Revelation.ogg
# Rigel					/system/media/audio/ringtones/Rigel.ogg
# Road Trip					/system/media/audio/ringtones/Road_Trip.ogg
# Romancing The Tone					/system/media/audio/ringtones/RomancingTheTone.ogg
# Safari					/system/media/audio/ringtones/Safari.ogg
# Savannah					/system/media/audio/ringtones/Savannah.ogg
# Scarabaeus					/system/media/audio/ringtones/Scarabaeus.ogg
# Sceptrum					/system/media/audio/ringtones/Sceptrum.ogg
# Seville					/system/media/audio/ringtones/Seville.ogg
# She's All That					/system/media/audio/ringtones/Shes_All_That.ogg
# Silky Way					/system/media/audio/ringtones/SilkyWay.ogg
# Sitar Versus Sitar					/system/media/audio/ringtones/SitarVsSitar.ogg
# Solarium					/system/media/audio/ringtones/Solarium.ogg
# Springy Jalopy					/system/media/audio/ringtones/SpringyJalopy.ogg
# Steppin' Out					/system/media/audio/ringtones/Steppin_Out.ogg
# Terminated					/system/media/audio/ringtones/Terminated.ogg
# Terrible Twos					/system/media/audio/ringtones/Noises2.ogg
# Testudo					/system/media/audio/ringtones/Testudo.ogg
# Themos					/system/media/audio/ringtones/Themos.ogg
# Third Eye					/system/media/audio/ringtones/Third_Eye.ogg
# Thriller Three					/system/media/audio/ringtones/Noises3.ogg
# Thunderfoot					/system/media/audio/ringtones/Thunderfoot.ogg
# Twirl Away					/system/media/audio/ringtones/TwirlAway.ogg
# Ursa Minor					/system/media/audio/ringtones/URSAMINOR.ogg
# UrsaMinor					/system/media/audio/ringtones/UrsaMinor.ogg
# Very Alarmed					/system/media/audio/ringtones/VeryAlarmed.ogg
# Vespa					/system/media/audio/ringtones/Vespa.ogg
# World					/system/media/audio/ringtones/World.ogg
# Zeta					/system/media/audio/ringtones/Zeta.ogg
# bellcore-dr1					/system/media/audio/ringtones/bellcore-dr1.ogg
# bellcore-dr2					/system/media/audio/ringtones/bellcore-dr2.ogg
# bellcore-dr3					/system/media/audio/ringtones/bellcore-dr3.ogg
# bellcore-dr4					/system/media/audio/ringtones/bellcore-dr4.ogg
# bellcore-dr5					/system/media/audio/ringtones/bellcore-dr5.ogg
# speaker					/system/media/audio/ringtones/speaker.wav
#######################################################################
##  Account 10 Advanced Settings                                     ##
#######################################################################
# Check Domain Certificates. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P51911=0

# Validate Certificate Chain. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P51967=0

# Validate Incoming SIP Messages. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P51906=0

# Allow Unsolicited REFER. 0 - Disabled, 1 - Enabled, 2 - Enabled/Force Auth. Default value is 0.
# Number: 0, 1, 2
P52923=0

# Only Accept SIP Requests from Known Servers. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P51947=0

# Check SIP User ID for Incoming INVITE. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P50949=0

# Allow SIP Reset. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P52915=0

# Authenticate Incoming INVITE. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P51946=0

# SIP Realm Used for Challenge INVITE & NOTIFY.
# String
P52921=


# Enable Local MOH. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P51957=0

# Virtual Account Group. -1 - Default,  0 - Virtual Account Group 1, 1 - Virtual Account Group 2, 2 - Virtual Account Group 3
# 3 - Virtual Account Group 4, 4 - Virtual Account Group 5, 5 - Virtual Account Group 6, 6 - Virtual Account Group 7, 7 - Virtual Account Group 8
# 8 - Virtual Account Group 9, 9 - Virtual Account Group 10, 10 - Virtual Account Group 11, 11 - Virtual Account Group 12, 12 - Virtual Account Group 13
# 13 - Virtual Account Group 14, 14 - Virtual Account Group 15, 15 - Virtual Account Group 16. Default value is -1.
# Number: -1 - 15 
P51991=-1

# Special Feature. Default value is 100
# 100 - Standard, 102 - Broadsoft, 113 - China Mobile
# 114 - ZTE IMS, 115 - Mobotix, 116 - ZTE NGN, 117 - Huawei IMS, 123 - NEC, 125 - WorldStone
# Number: 100, 102, 113, 114, 115, 116, 117, 123, 125
P50924=100

# Allow Sync Phonebook via SIP Notify. 0 - No, 1 - Yes. Default is 1.
# Number: 0, 1
P52999=1
##############################################################################
##  Account 11 Settings                                                     ##
##############################################################################

#######################################################################
##  Account 11 General Settings                                      ##
#######################################################################

# Account Active. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P51001=0

# Account Name
P51017=

# SIP Server
P51002=

# SIP User ID
P51004=
 
# SIP Authentication ID
P51005=

# SIP Authentication Password
P51006=

# Voice Mail Access Number
P51026=

# Name (Display Name, e.g., John Doe)
P51007=

# Tel URI. 0 - Disable, 1 - User=Phone, 2 - Enabled. Default value is 0
# Number: 0, 1, 2
P51009=0

#######################################################################
##  Account 11 Network Settings                                      ##
#######################################################################

# Outbound Proxy
P51003=

# Secondary Outbound Proxy
P52033=

# DNS Mode. 0 - A Record, 1 - SRV, 2 - NAPTR/SRV. Default value is 0
# Number: 0, 1, 2
P51008=0

# DNS SRV Fail-over Mode. 0 - Default, 1 - Saved one until DNS TTL, 2 - Saved one until no response. Defualt value is 1
# Number
P53040=0

# Register Before DNS SRV Fail-over. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P54095=0

# NAT Traversal. 0 - NAT No, 1 - STUN, 2 - Keep-alive, 3 - UPnP, 4 - Auto, 5 - VPN. Default value is 2
# Number: 0, 1, 2, 3, 4, 5
P51014=2

# Proxy-Require
P51018=

#######################################################################
##  Account 11 SIP Settings                                          ##
#######################################################################

# SIP Registration. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P51010=1

# Unregister Before New Registration. 0 - No, 1 - All, 2 -  Instance . Default value is 2
# Number: 0, 1, 2
P51011=2

# Register Expiration (m). In minutes. Default value is 60
# Number: 0 - 64800
P51012=60

# Subscribe Expiration (m). Default is 60
# Number: 0 - 64800
P53051=60

# Re-register before Expiration (s). Default Value is 0
# Number : 0
P52030=0

# Registration Retry Wait Time (s). In seconds. Default value is 20
# Number: 1 - 3600
P51071=20

# Local SIP Port. Default value is 5080
# Number: 5 - 65535
P51013=5080

# SUBSCRIBE For MWI. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P51015=0

# Enable SIP OPTIONS Keep Alive. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P52097=0

# SIP OPTIONS Keep Alive Interval(s). Default value is 30
# Number 
P52098=30

# SIP OPTIONS Keep Alive Maximum Tries. Default value is 3
# Number 
P52099=3

# Enable Session Timer/ Session Expiration(s).  In seconds. Default value is 180 seconds.
# By default,  Session Timer is Enabled.  Session Timer is disabled if the value is 0.
# Number: 0 or 90 - 64800
P51034=180

# Min-SE(s). Default value is 90 seconds
# Number: 90 - 64800
P51027=90

# UAC Specify Refresher. 0 - Omit, 1 - UAC, 2 - UAS. Default value is 0
# Number: 0, 1, 2
P51032=0

# UAS Specify Refresher. 1 - UAC, 2 - UAS. Default value is 1
# Number: 1, 2
P51033=1

# Force INVITE. Always refresh with INVITE instead of UPDATE even when remote party supports UPDATE
# 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P51031=0

# Caller Request Timer. Request for timer when calling
# 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P51028=0

# Callee Request Timer
# Request for timer when being called (i.e., if remote party supports timer but did not request for one)
# 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P51029=0

# Force Timer. Still use timer when remote party does not support timer
# 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P51030=0

# Enable 100rel. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P51035=0

# Use Privacy Header
# 0 - Default, 1 - No, 2 - Yes. Default is 0
# Number: 0, 1, 2
P52038=0

# Use P-Preferred-Identity Header
# 0 - Default, 1 - No, 2 - Yes. Default is 0
# Number: 0, 1, 2
P52039=0

# Use P-Access-Network-Info Header. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P53058=1

# Use P-Emergency-Info Header. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P53059=1

# Use MAC Header.  0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P53061=0

# SIP Transport
# 0 - UDP , 1 - TCP, 2 - TLS. Default value is 0
# Number: 0, 1, 2
P51048=0

# SIP URI Scheme When Using TLS
# 0 -sip, 1 - sips. Default value is 0.
# Number: 0, 1
P52029=0

# Use Actual Ephemeral Port in Contact with TCP/TLS
# 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P52031=0

# Support SIP Instance ID
# 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P51089=1

# Add Auth Header On RE-REGISTER
# 0 - No, 1- Yes
P52059=1

# SIP T1 Timeout. RFC 3261 T1 value (RTT estimate)
# 50 - 0.5 sec, 100 - 1 sec, 200 - 2 sec. Default value is 50
# Number: 50, 100, 200
P51040=50

# SIP T2 Interval. RFC 3261 T2 value
# The maximum retransmit interval for non-INVITE requests and INVITE responses
# 200 - 2 sec, 400 - 4 sec, 800 - 8 sec. Default value is 400
# Number: 200, 400, 800.
P51041=400

# SIP Timer D Interval (Seconds)
# Number 0-64. Default value is 0
P52087=0

# Remove OBP from Route
# 0 - Disable, 1 - Enable, 2 - Always. Default value is 0
# Number: 0, 1, 2
P52005=0
#######################################################################
##  Account 11 Codec Settings                                        ##
#######################################################################
# Preferred Vocoder
# First codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 123 - Opus. Default value is 0
# Number: 0, 8, 9, 2, 18, 98, 123
P51051=0

# Second codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 123 - Opus. Default value is 8
# Number: 0, 8, 9, 2, 18, 98, 123
P51052=8

# Third codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 123 - Opus. Default value is 9
# Number: 0, 8, 9, 2, 18, 98, 123
P51053=9

# Forth codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 123 - Opus. Default value is 9
# Number: 0, 8, 9, 2, 18, 98, 123
P51054=9

# Fifth codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 123 - Opus. Default value is 9
# Number: 0, 8, 9, 2, 18, 98, 123
P51055=9

# Sixth codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 123 - Opus. Default value is 9
# Number: 0, 8, 9, 2, 18, 98, 123
P51056=9

# Seventh codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 123 - Opus. Default value is 9
# Number: 0, 8, 9, 2, 18, 98, 123
P51057=9

# Eigth codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 123 - Opus. Default value is 9
# Number: 0, 8, 9, 2, 18, 98, 123
P51058=9

# Codec Negotiation Priority. 0 - Caller, 1 - Callee. Default value is 1.
# Number: 0, 1
P54061=1

# Use First Matching Vocoder in 200OK SDP. 0 - No, 1 - Yes. The default value is 0.
# Number: 0, 1
P52048=0

# iLBC Frame Size. 0 - 20 ms, 1 - 30 ms. Default value is 1.
# Number: 0, 1
P51095=1

# G726-32 ITU Payload. 0 - 2, 1 - Dynamic. Default value is 0.
# Number: 0, 1
P52069=0

# G726-32 Dynamic PT. Default value is 126.
# Number
P52065=126

# Opus Payload Type
P52085=123

# DTMF: in audio. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P52001=0

# DTMF: via RFC2833. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P52002=1

# DTMF: via SIP INFO. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P52003=0

# DTMF Payload Type. Default value is 101
# Number: 96 - 126
P51096=101

# Enable Audio RED with FEC. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P53073=0

# Audio FEC Payload Type. Default value is 121
# Number: 96 - 126
P53074=121

# Audio RED Payload Type. Default value is 124
# Number: 96 - 126
P53075=124

# Silence Suppression. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P51085=0

# Voice Frames Per TX. Default value is 2
# Number: 1 - 64.
P51086=2

# Preferred Video Codec. 99 - H.264. Default is 99.
P51064=99

# Enable Video FEC. 0 - No, 1 - Yes. Default value is 1.
# Number: 0, 1
P52093=1

# Enable RFC5168 Support. 0 - No, 1 - Yes. Default value is 1.
# Number: 0, 1
P51078=1

# Video FEC Mode. 0 - 0, 1 - 1. Default value is 0.
# Number: 0, 1
P53022=0

# FEC Payload Type. Default value is 120.
P52094=120

# Packetization mode. 0 - Single NAL Unit Mode, 1 - Non-Interleaved Mode. Default value is 1.
# Number: 0, 1, 10
P53005=1

# H.264 Image Size. 9 - 720P, 1 - VGA, 5 - CIF, 4 - 4CIF, 0 - QVGA, 6 - QCIF. Default value is 9
# Number: 9, 1, 5, 4, 0, 6
P52007=9

# Use H.264 Constrained Profiles. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1
P53045=0

# H.264 Profile Type. 0 - Baseline Profile, 1 - Main Profile, 2 - High Profile, 3 - BP&MP&HP
# Number: 0, 1, 2, 3
P52062=0

# Video Bit Rate. 64 - 64 kbps, 96 - 96 kbps, 128 - 128 kbps, 160 - 160 kbps, 192 - 192 kbps
# 210 - 210 kbps, 256 - 256 kbps, 384 - 384 kbps, 512 - 512 kbps, 640 - 640 kbps, 768 - 768 kbps
# 1024 - 1024 kbps, 1280 - 1280 kbps, 1536 - 1536 kbps, 2048 - 2048 kbps. Default value is 2048.
# Number: 250, 500, 750
P52015=2048

# SDP Bandwidth Attribute. 0 - Standard, 1 - Media Level, 2 - Session Level, 3 - None. Default value is Media Level.
# Number: 0, 1, 2, 3
P52060=1

# H.264 Payload Type. Default value is 99.
P51062=99

# Disable BFCP. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1
P53001=0

# Presentation H.264 Image Size. 10 - 1080P, 9 - 720P. Default value is 10.
# Number: 10, 9
P52076=10

# Presentation H.264 Profile Type. 0 - Baseline Profile, 1 - Main Profile, 2 - High Profile, 3 - BP&MP&HP
# Number: 0, 1, 2, 3
P52077=3

# Presentation Video Bit Rate. 512 - 512 kbps, 640 - 640 kbps, 768 - 768 kbps
# 1024 - 1024 kbps, 1280 - 1280 kbps, 1536 - 1536 kbps, 2048 - 2048 kbps. Default value is 1024.
# Number: 250, 500, 750
P52078=1024

# Presentation Video Frame Rate. 5 - 5 frames/second, 10 - 10 frames/second, 15 - 15 frames/second. Default value is 15.
# Number: 5, 10, 15
P53042=

# BFCP Transport Protocol. 0 - Automatic, 1 - UDP, 2 - TCP. Default value is 1.
# Number: 0, 1, 2
P53041=

# SRTP Mode. 0 - Disable, 1 - Enable but not forced, 2 - Enable and forced. Default value is 0
# Number:0, 1, 2
P51043=0

# SRTP Key Length. 0 - AES 128&256 bit, 1 - AES 128 bit, 2 - AES 256 bit. Default value is 0
# Number:0, 1, 2
P52083=0 

# Enable SRTP Key Lifetime. 0 - No, 1 - Yes.
# Number: 0,1
P52063=0

# RTCP Destination
P52090=

# Symmetric RTP. 0 - No, 1 - Yes. Default value is 0
# Number:0, 1
P51060=0

# RTP IP Filter. 0 - Disable, 1 - IP Only, 2 - IP and Port. Default value is 0
# Number:0, 1, 2
P53026=0

# RTP Timeout(s). Default is 0. If set to 0, the device would not hangup.
# number: 0 - 600
P54068=0
#######################################################################
##  Account 11 Call Settings                                         ##
#######################################################################
# Enable Video Call. 0 - Default, 1 - No, 2 - Yes. Default is 0
# Number: 0, 1, 2
P61043=0

# Start Video Automatically. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P52014=1

# Remote Video Request. 0 - Prompt, 1 - Accept, 2 - Deny. Default value is 0
# Number: 0, 1, 2
P52026=0

# Video Layout. 0 - Default, 1 - Full screen, 3 - Equal split screen, 2 - Only display remote screen
P52032=0

# Auto Answer. 0 - No, 1 - Yes, 2 - Enable Intercom/Paging. Default value is 0
# Number: 0, 1, 2
P51025=0

# Play warning tone for Auto Answer Intercom. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P53072=1

# Intercom Barging. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P53019=1

# Auto Preview. 0 - No, 1 - Yes, 2 - Yes with Ringing. Default value is 0
# Number: 0, 1, 2
P54062=0

# Send Anonymous. 0 - No, 1 - Yes (caller ID will be blocked if set to Yes). Default value is 0
# Number: 0, 1
P51021=0

# Anonymous Call Rejection. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P51046=0

# Call Log
# 0 - Log All, 1 - Log Incoming/Outgoing only (Missed Calls Not Recorded), 2 - Disable Call All, 3 - Don't Prompt Missed Call. Default value is 0
# Number: 0, 1, 2
P51042=0

# Enable Call Features. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P51020=0

# Enable Call Waiting. 0 - Default, 1 - No, 2 - Yes.
# Number: 0, 1, 2
P53063=0

# Mute on Answer Intercom Call. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
P53071=0

# Transfer on 3 way conference Hangup. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P52004=0

# Use # as Dial Key. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P51092=1

# Use # as Redial Key. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P54069=1

# DND Call Feature On.
# String
P52044=

# DND Call Feature Off.
# String
P52045=

# No Key Entry Timeout (s). Default value is 4
# Number: 1 - 15
P51091=4

# Ring Timeout (s). Default value is 60
# Number: 10 - 300
P51076=60

# Refer-To Use Target Contact. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P51069=0

# RFC2543 Hold. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1 
P53062=1

# Dial Plan Prefix
# String
P51019=

# Disable DialPlan. 0 - No Selection, 1 - Dial Page, 2 - Contact, 4 - Incoming Call History, 8 -  Outgoing Call History, 16 - MPK & Click2Dial. 
# If need to check multiple selections, add the specific values for each selections together. Default value is 0
# Number: 0-31
P52082=0

# DialPlan. Default value is { x+ | \+x+ | *x+ | *xx*x+ | x+*x+*x+*x+ | x+*x+*x+*x+#x+ }
P51059={ x+ | \+x+ | *x+ | *xx*x+ | x+*x+*x+*x+ | x+*x+*x+*x+#x+ }

# Caller ID Display. 0 - Auto, 1 - Disabled, 2 - From Header. The default value is 0.
# Number: 0, 1, 2, 3
P52024=0

# Account Ringtone. See ring tone options and value in the Ring Tone Value Table below
P51023=content://settings/system/ringtone

# Ignore Alert-Info Header. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1
P53018=0

# Matching Incoming Caller ID. Matching Rule 1
# String
P53077=

# Matching Rule 1 Distinctive Ringtone. See ring tone options and value in the Ring Tone Value Table below
# String
P53078=content://settings/system/ringtone

# Matching Incoming Caller ID. Matching Rule 2
# String
P53079=

# Matching Rule 2 Distinctive Ringtone. See ring tone options and value in the Ring Tone Value Table below
# String
P53080=content://settings/system/ringtone

# Matching Incoming Caller ID. Matching Rule 3
# String
P53081=

# Matching Rule 3 Distinctive Ringtone. See ring tone options and value in the Ring Tone Value Table below
# String
P53082=content://settings/system/ringtone

############Ring Tone Value Table###############
# Web GUI Option                            Value
# Use System Ring tone                      content://settings/system/ringtone 
# Andromeda					/system/media/audio/ringtones/ANDROMEDA.ogg
# Aquila					/system/media/audio/ringtones/Aquila.ogg
# Argo Navis					/system/media/audio/ringtones/ArgoNavis.ogg
# Atria					/system/media/audio/ringtones/Atria.ogg
# Backroad					/system/media/audio/ringtones/Backroad.ogg
# Beat Plucker					/system/media/audio/ringtones/BeatPlucker.ogg
# Bell Phone					/system/media/audio/ringtones/Ring_Classic_02.ogg
# Bentley Dubs					/system/media/audio/ringtones/BentleyDubs.ogg
# Big Easy					/system/media/audio/ringtones/Big_Easy.ogg
# Bird Loop					/system/media/audio/ringtones/BirdLoop.ogg
# Bollywood					/system/media/audio/ringtones/Bollywood.ogg
# Boötes					/system/media/audio/ringtones/BOOTES.ogg
# Bus' a Move					/system/media/audio/ringtones/BussaMove.ogg
# Cairo					/system/media/audio/ringtones/Cairo.ogg
# Calypso Steel					/system/media/audio/ringtones/Calypso_Steel.ogg
# Canis Major					/system/media/audio/ringtones/CANISMAJOR.ogg
# Caribbean Ice					/system/media/audio/ringtones/CaribbeanIce.ogg
# Carina					/system/media/audio/ringtones/Carina.ogg
# Cassiopeia					/system/media/audio/ringtones/CASSIOPEIA.ogg
# Centaurus					/system/media/audio/ringtones/Centaurus.ogg
# Champagne Edition					/system/media/audio/ringtones/Champagne_Edition.ogg
# Chimey Phone					/system/media/audio/ringtones/Ring_Synth_02.ogg
# Club Cubano					/system/media/audio/ringtones/Club_Cubano.ogg
# Crayon Rock					/system/media/audio/ringtones/CrayonRock.ogg
# Crazy Dream					/system/media/audio/ringtones/CrazyDream.ogg
# Curve Ball Blend					/system/media/audio/ringtones/CurveBall.ogg
# Cygnus					/system/media/audio/ringtones/Cygnus.ogg
# Dancin' Fool					/system/media/audio/ringtones/DancinFool.ogg
# Digital Phone					/system/media/audio/ringtones/Ring_Digital_02.ogg
# Ding					/system/media/audio/ringtones/Ding.ogg
# DingDong					/system/media/audio/ringtones/DingDong.wav
# Don' Mess Wiv It					/system/media/audio/ringtones/DonMessWivIt.ogg
# Draco					/system/media/audio/ringtones/Draco.ogg
# Dream Theme					/system/media/audio/ringtones/DreamTheme.ogg
# Eastern Sky					/system/media/audio/ringtones/Eastern_Sky.ogg
# Enter the Nexus					/system/media/audio/ringtones/Enter_the_Nexus.ogg
# Eridani					/system/media/audio/ringtones/Eridani.ogg
# Ether Shake					/system/media/audio/ringtones/EtherShake.ogg
# Flutey Phone					/system/media/audio/ringtones/Ring_Synth_04.ogg
# Free Flight					/system/media/audio/ringtones/FreeFlight.ogg
# Friendly Ghost					/system/media/audio/ringtones/FriendlyGhost.ogg
# Funk Y'all					/system/media/audio/ringtones/Funk_Yall.ogg
# Game Over Guitar					/system/media/audio/ringtones/GameOverGuitar.ogg
# Gimme Mo' Town					/system/media/audio/ringtones/Gimme_Mo_Town.ogg
# Girtab					/system/media/audio/ringtones/Girtab.ogg
# Glacial Groove					/system/media/audio/ringtones/Glacial_Groove.ogg
# Growl					/system/media/audio/ringtones/Growl.ogg
# Halfway Home					/system/media/audio/ringtones/HalfwayHome.ogg
# Hydra					/system/media/audio/ringtones/Hydra.ogg
# Insert Coin					/system/media/audio/ringtones/InsertCoin.ogg
# Kuma					/system/media/audio/ringtones/Kuma.ogg
# Loopy Lounge					/system/media/audio/ringtones/LoopyLounge.ogg
# Love Flute					/system/media/audio/ringtones/LoveFlute.ogg
# Lyra					/system/media/audio/ringtones/Lyra.ogg
# Machina					/system/media/audio/ringtones/Machina.ogg
# Medieval Jaunt					/system/media/audio/ringtones/MidEvilJaunt.ogg
# Mildly Alarming					/system/media/audio/ringtones/MildlyAlarming.ogg
# Nairobi					/system/media/audio/ringtones/Nairobi.ogg
# Nassau					/system/media/audio/ringtones/Nassau.ogg
# New Player					/system/media/audio/ringtones/NewPlayer.ogg
# No Limits					/system/media/audio/ringtones/No_Limits.ogg
# Noisey One					/system/media/audio/ringtones/Noises1.ogg
# Organ Dub					/system/media/audio/ringtones/OrganDub.ogg
# Orion					/system/media/audio/ringtones/Orion.ogg
# Paradise Island					/system/media/audio/ringtones/Paradise_Island.ogg
# Pegasus					/system/media/audio/ringtones/Pegasus.ogg
# Perseus					/system/media/audio/ringtones/PERSEUS.ogg
# Playa					/system/media/audio/ringtones/Playa.ogg
# Pyxis					/system/media/audio/ringtones/Pyxis.ogg
# Rasalas					/system/media/audio/ringtones/Rasalas.ogg
# Revelation					/system/media/audio/ringtones/Revelation.ogg
# Rigel					/system/media/audio/ringtones/Rigel.ogg
# Road Trip					/system/media/audio/ringtones/Road_Trip.ogg
# Romancing The Tone					/system/media/audio/ringtones/RomancingTheTone.ogg
# Safari					/system/media/audio/ringtones/Safari.ogg
# Savannah					/system/media/audio/ringtones/Savannah.ogg
# Scarabaeus					/system/media/audio/ringtones/Scarabaeus.ogg
# Sceptrum					/system/media/audio/ringtones/Sceptrum.ogg
# Seville					/system/media/audio/ringtones/Seville.ogg
# She's All That					/system/media/audio/ringtones/Shes_All_That.ogg
# Silky Way					/system/media/audio/ringtones/SilkyWay.ogg
# Sitar Versus Sitar					/system/media/audio/ringtones/SitarVsSitar.ogg
# Solarium					/system/media/audio/ringtones/Solarium.ogg
# Springy Jalopy					/system/media/audio/ringtones/SpringyJalopy.ogg
# Steppin' Out					/system/media/audio/ringtones/Steppin_Out.ogg
# Terminated					/system/media/audio/ringtones/Terminated.ogg
# Terrible Twos					/system/media/audio/ringtones/Noises2.ogg
# Testudo					/system/media/audio/ringtones/Testudo.ogg
# Themos					/system/media/audio/ringtones/Themos.ogg
# Third Eye					/system/media/audio/ringtones/Third_Eye.ogg
# Thriller Three					/system/media/audio/ringtones/Noises3.ogg
# Thunderfoot					/system/media/audio/ringtones/Thunderfoot.ogg
# Twirl Away					/system/media/audio/ringtones/TwirlAway.ogg
# Ursa Minor					/system/media/audio/ringtones/URSAMINOR.ogg
# UrsaMinor					/system/media/audio/ringtones/UrsaMinor.ogg
# Very Alarmed					/system/media/audio/ringtones/VeryAlarmed.ogg
# Vespa					/system/media/audio/ringtones/Vespa.ogg
# World					/system/media/audio/ringtones/World.ogg
# Zeta					/system/media/audio/ringtones/Zeta.ogg
# bellcore-dr1					/system/media/audio/ringtones/bellcore-dr1.ogg
# bellcore-dr2					/system/media/audio/ringtones/bellcore-dr2.ogg
# bellcore-dr3					/system/media/audio/ringtones/bellcore-dr3.ogg
# bellcore-dr4					/system/media/audio/ringtones/bellcore-dr4.ogg
# bellcore-dr5					/system/media/audio/ringtones/bellcore-dr5.ogg
# speaker					/system/media/audio/ringtones/speaker.wav
#######################################################################
##  Account 11 Advanced Settings                                     ##
#######################################################################
# Check Domain Certificates. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P52011=0

# Validate Certificate Chain. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P52067=0

# Validate Incoming SIP Messages. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P52006=0

# Allow Unsolicited REFER. 0 - Disabled, 1 - Enabled, 2 - Enabled/Force Auth. Default value is 0.
# Number: 0, 1, 2
P53023=0

# Only Accept SIP Requests from Known Servers. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P52047=0

# Check SIP User ID for Incoming INVITE. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P51049=0

# Allow SIP Reset. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P53015=0

# Authenticate Incoming INVITE. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P52046=0

# SIP Realm Used for Challenge INVITE & NOTIFY.
# String
P53021=


# Enable Local MOH. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P52057=0

# Virtual Account Group. -1 - Default,  0 - Virtual Account Group 1, 1 - Virtual Account Group 2, 2 - Virtual Account Group 3
# 3 - Virtual Account Group 4, 4 - Virtual Account Group 5, 5 - Virtual Account Group 6, 6 - Virtual Account Group 7, 7 - Virtual Account Group 8
# 8 - Virtual Account Group 9, 9 - Virtual Account Group 10, 10 - Virtual Account Group 11, 11 - Virtual Account Group 12, 12 - Virtual Account Group 13
# 13 - Virtual Account Group 14, 14 - Virtual Account Group 15, 15 - Virtual Account Group 16. Default value is -1.
# Number: -1 - 15 
P52091=-1

# Special Feature. Default value is 100
# 100 - Standard, 102 - Broadsoft, 113 - China Mobile
# 114 - ZTE IMS, 115 - Mobotix, 116 - ZTE NGN, 117 - Huawei IMS, 123 - NEC, 125 - WorldStone
# Number: 100, 102, 113, 114, 115, 116, 117, 123, 125
P51024=100

# Allow Sync Phonebook via SIP Notify. 0 - No, 1 - Yes. Default is 1.
# Number: 0, 1
P53099=1
##############################################################################
##  Account 12 Settings                                                     ##
##############################################################################

#######################################################################
##  Account 12 General Settings                                      ##
#######################################################################

# Account Active. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P51101=0

# Account Name
P51117=

# SIP Server
P51102=

# SIP User ID
P51104=
 
# SIP Authentication ID
P51105=

# SIP Authentication Password
P51106=

# Voice Mail Access Number
P51126=

# Name (Display Name, e.g., John Doe)
P51107=

# Tel URI. 0 - Disable, 1 - User=Phone, 2 - Enabled. Default value is 0
# Number: 0, 1, 2
P51109=0

#######################################################################
##  Account 12 Network Settings                                      ##
#######################################################################

# Outbound Proxy
P51103=

# Secondary Outbound Proxy
P52133=

# DNS Mode. 0 - A Record, 1 - SRV, 2 - NAPTR/SRV. Default value is 0
# Number: 0, 1, 2
P51108=0

# DNS SRV Fail-over Mode. 0 - Default, 1 - Saved one until DNS TTL, 2 - Saved one until no response. Defualt value is 1
# Number
P53140=0

# Register Before DNS SRV Fail-over. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P54195=0

# NAT Traversal. 0 - NAT No, 1 - STUN, 2 - Keep-alive, 3 - UPnP, 4 - Auto, 5 - VPN. Default value is 2
# Number: 0, 1, 2, 3, 4, 5
P51114=2

# Proxy-Require
P51118=

#######################################################################
##  Account 12 SIP Settings                                          ##
#######################################################################

# SIP Registration. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P51110=1

# Unregister Before New Registration. 0 - No, 1 - All, 2 -  Instance . Default value is 2
# Number: 0, 1, 2
P51111=2

# Register Expiration (m). In minutes. Default value is 60
# Number: 0 - 64800
P51112=60

# Subscribe Expiration (m). Default is 60
# Number: 0 - 64800
P53151=60

# Re-register before Expiration (s). Default Value is 0
# Number : 0
P52130=0

# Registration Retry Wait Time (s). In seconds. Default value is 20
# Number: 1 - 3600
P51171=20

# Local SIP Port. Default value is 5082
# Number: 5 - 65535
P51113=5082

# SUBSCRIBE For MWI. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P51115=0

# Enable SIP OPTIONS Keep Alive. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P52197=0

# SIP OPTIONS Keep Alive Interval(s). Default value is 30
# Number 
P52198=30

# SIP OPTIONS Keep Alive Maximum Tries. Default value is 3
# Number 
P52199=3

# Enable Session Timer/ Session Expiration(s).  In seconds. Default value is 180 seconds.
# By default,  Session Timer is Enabled.  Session Timer is disabled if the value is 0.
# Number: 0 or 90 - 64800
P51134=180

# Min-SE(s). Default value is 90 seconds
# Number: 90 - 64800
P51127=90

# UAC Specify Refresher. 0 - Omit, 1 - UAC, 2 - UAS. Default value is 0
# Number: 0, 1, 2
P51132=0

# UAS Specify Refresher. 1 - UAC, 2 - UAS. Default value is 1
# Number: 1, 2
P51133=1

# Force INVITE. Always refresh with INVITE instead of UPDATE even when remote party supports UPDATE
# 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P51131=0

# Caller Request Timer. Request for timer when calling
# 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P51128=0

# Callee Request Timer
# Request for timer when being called (i.e., if remote party supports timer but did not request for one)
# 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P51129=0

# Force Timer. Still use timer when remote party does not support timer
# 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P51130=0

# Enable 100rel. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P51135=0

# Use Privacy Header
# 0 - Default, 1 - No, 2 - Yes. Default is 0
# Number: 0, 1, 2
P52138=0

# Use P-Preferred-Identity Header
# 0 - Default, 1 - No, 2 - Yes. Default is 0
# Number: 0, 1, 2
P52139=0

# Use P-Access-Network-Info Header. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P53158=1

# Use P-Emergency-Info Header. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P53159=1

# Use MAC Header.  0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P53161=0

# SIP Transport
# 0 - UDP , 1 - TCP, 2 - TLS. Default value is 0
# Number: 0, 1, 2
P51148=0

# SIP URI Scheme When Using TLS
# 0 -sip, 1 - sips. Default value is 0.
# Number: 0, 1
P52129=0

# Use Actual Ephemeral Port in Contact with TCP/TLS
# 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P52131=0

# Support SIP Instance ID
# 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P51189=1

# Add Auth Header On RE-REGISTER
# 0 - No, 1- Yes
P52159=1

# SIP T1 Timeout. RFC 3261 T1 value (RTT estimate)
# 50 - 0.5 sec, 100 - 1 sec, 200 - 2 sec. Default value is 50
# Number: 50, 100, 200
P51140=50

# SIP T2 Interval. RFC 3261 T2 value
# The maximum retransmit interval for non-INVITE requests and INVITE responses
# 200 - 2 sec, 400 - 4 sec, 800 - 8 sec. Default value is 400
# Number: 200, 400, 800.
P51141=400

# SIP Timer D Interval (Seconds)
# Number 0-64. Default value is 0
P52187=0

# Remove OBP from Route
# 0 - Disable, 1 - Enable, 2 - Always. Default value is 0
# Number: 0, 1, 2
P52105=0
#######################################################################
##  Account 12 Codec Settings                                        ##
#######################################################################
# Preferred Vocoder
# First codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 123 - Opus. Default value is 0
# Number: 0, 8, 9, 2, 18, 98, 123
P51151=0

# Second codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 123 - Opus. Default value is 8
# Number: 0, 8, 9, 2, 18, 98, 123
P51152=8

# Third codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 123 - Opus. Default value is 9
# Number: 0, 8, 9, 2, 18, 98, 123
P51153=9

# Forth codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 123 - Opus. Default value is 9
# Number: 0, 8, 9, 2, 18, 98, 123
P51154=9

# Fifth codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 123 - Opus. Default value is 9
# Number: 0, 8, 9, 2, 18, 98, 123
P51155=9

# Sixth codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 123 - Opus. Default value is 9
# Number: 0, 8, 9, 2, 18, 98, 123
P51156=9

# Seventh codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 123 - Opus. Default value is 9
# Number: 0, 8, 9, 2, 18, 98, 123
P51157=9

# Eigth codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 123 - Opus. Default value is 9
# Number: 0, 8, 9, 2, 18, 98, 123
P51158=9

# Codec Negotiation Priority. 0 - Caller, 1 - Callee. Default value is 1.
# Number: 0, 1
P54161=1

# Use First Matching Vocoder in 200OK SDP. 0 - No, 1 - Yes. The default value is 0.
# Number: 0, 1
P52148=0

# iLBC Frame Size. 0 - 20 ms, 1 - 30 ms. Default value is 1.
# Number: 0, 1
P51195=1

# G726-32 ITU Payload. 0 - 2, 1 - Dynamic. Default value is 0.
# Number: 0, 1
P52169=0

# G726-32 Dynamic PT. Default value is 126.
# Number
P52165=126

# Opus Payload Type
P52185=123

# DTMF: in audio. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P52101=0

# DTMF: via RFC2833. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P52102=1

# DTMF: via SIP INFO. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P52103=0

# DTMF Payload Type. Default value is 101
# Number: 96 - 126
P51196=101

# Enable Audio RED with FEC. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P53173=0

# Audio FEC Payload Type. Default value is 121
# Number: 96 - 126
P53174=121

# Audio RED Payload Type. Default value is 124
# Number: 96 - 126
P53175=124

# Silence Suppression. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P51185=0

# Voice Frames Per TX. Default value is 2
# Number: 1 - 64.
P51186=2

# Preferred Video Codec. 99 - H.264. Default is 99.
P51164=99

# Enable Video FEC. 0 - No, 1 - Yes. Default value is 1.
# Number: 0, 1
P52193=1

# Enable RFC5168 Support. 0 - No, 1 - Yes. Default value is 1.
# Number: 0, 1
P51178=1

# Video FEC Mode. 0 - 0, 1 - 1. Default value is 0.
# Number: 0, 1
P53122=0

# FEC Payload Type. Default value is 120.
P52194=120

# Packetization mode. 0 - Single NAL Unit Mode, 1 - Non-Interleaved Mode. Default value is 1.
# Number: 0, 1, 10
P53105=1

# H.264 Image Size. 9 - 720P, 1 - VGA, 5 - CIF, 4 - 4CIF, 0 - QVGA, 6 - QCIF. Default value is 9
# Number: 9, 1, 5, 4, 0, 6
P52107=9

# Use H.264 Constrained Profiles. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1
P53145=0

# H.264 Profile Type. 0 - Baseline Profile, 1 - Main Profile, 2 - High Profile, 3 - BP&MP&HP
# Number: 0, 1, 2, 3
P52162=0

# Video Bit Rate. 64 - 64 kbps, 96 - 96 kbps, 128 - 128 kbps, 160 - 160 kbps, 192 - 192 kbps
# 210 - 210 kbps, 256 - 256 kbps, 384 - 384 kbps, 512 - 512 kbps, 640 - 640 kbps, 768 - 768 kbps
# 1024 - 1024 kbps, 1280 - 1280 kbps, 1536 - 1536 kbps, 2048 - 2048 kbps. Default value is 2048.
# Number: 250, 500, 750
P52115=2048

# SDP Bandwidth Attribute. 0 - Standard, 1 - Media Level, 2 - Session Level, 3 - None. Default value is Media Level.
# Number: 0, 1, 2, 3
P52160=1

# H.264 Payload Type. Default value is 99.
P51162=99

# Disable BFCP. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1
P53101=0

# Presentation H.264 Image Size. 10 - 1080P, 9 - 720P. Default value is 10.
# Number: 10, 9
P52176=10

# Presentation H.264 Profile Type. 0 - Baseline Profile, 1 - Main Profile, 2 - High Profile, 3 - BP&MP&HP
# Number: 0, 1, 2, 3
P52177=3

# Presentation Video Bit Rate. 512 - 512 kbps, 640 - 640 kbps, 768 - 768 kbps
# 1024 - 1024 kbps, 1280 - 1280 kbps, 1536 - 1536 kbps, 2048 - 2048 kbps. Default value is 1024.
# Number: 250, 500, 750
P52178=1024

# Presentation Video Frame Rate. 5 - 5 frames/second, 10 - 10 frames/second, 15 - 15 frames/second. Default value is 15.
# Number: 5, 10, 15
P53142=

# BFCP Transport Protocol. 0 - Automatic, 1 - UDP, 2 - TCP. Default value is 1.
# Number: 0, 1, 2
P53141=

# SRTP Mode. 0 - Disable, 1 - Enable but not forced, 2 - Enable and forced. Default value is 0
# Number:0, 1, 2
P51143=0

# SRTP Key Length. 0 - AES 128&256 bit, 1 - AES 128 bit, 2 - AES 256 bit. Default value is 0
# Number:0, 1, 2
P52183=0 

# Enable SRTP Key Lifetime. 0 - No, 1 - Yes.
# Number: 0,1
P52163=0

# RTCP Destination
P52190=

# Symmetric RTP. 0 - No, 1 - Yes. Default value is 0
# Number:0, 1
P51160=0

# RTP IP Filter. 0 - Disable, 1 - IP Only, 2 - IP and Port. Default value is 0
# Number:0, 1, 2
P53126=0

# RTP Timeout(s). Default is 0. If set to 0, the device would not hangup.
# number: 0 - 600
P54168=0
#######################################################################
##  Account 12 Call Settings                                         ##
#######################################################################
# Enable Video Call. 0 - Default, 1 - No, 2 - Yes. Default is 0
# Number: 0, 1, 2
P61143=0

# Start Video Automatically. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P52114=1

# Remote Video Request. 0 - Prompt, 1 - Accept, 2 - Deny. Default value is 0
# Number: 0, 1, 2
P52126=0

# Video Layout. 0 - Default, 1 - Full screen, 3 - Equal split screen, 2 - Only display remote screen
P52132=0

# Auto Answer. 0 - No, 1 - Yes, 2 - Enable Intercom/Paging. Default value is 0
# Number: 0, 1, 2
P51125=0

# Play warning tone for Auto Answer Intercom. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P53172=1

# Intercom Barging. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P53119=1

# Auto Preview. 0 - No, 1 - Yes, 2 - Yes with Ringing. Default value is 0
# Number: 0, 1, 2
P54162=0

# Send Anonymous. 0 - No, 1 - Yes (caller ID will be blocked if set to Yes). Default value is 0
# Number: 0, 1
P51121=0

# Anonymous Call Rejection. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P51146=0

# Call Log
# 0 - Log All, 1 - Log Incoming/Outgoing only (Missed Calls Not Recorded), 2 - Disable Call All, 3 - Don't Prompt Missed Call. Default value is 0
# Number: 0, 1, 2
P51142=0

# Enable Call Features. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P51120=0

# Enable Call Waiting. 0 - Default, 1 - No, 2 - Yes.
# Number: 0, 1, 2
P53163=0

# Mute on Answer Intercom Call. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
P53171=0

# Transfer on 3 way conference Hangup. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P52104=0

# Use # as Dial Key. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P51192=1

# Use # as Redial Key. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P54169=1

# DND Call Feature On.
# String
P52144=

# DND Call Feature Off.
# String
P52145=

# No Key Entry Timeout (s). Default value is 4
# Number: 1 - 15
P51191=4

# Ring Timeout (s). Default value is 60
# Number: 10 - 300
P51176=60

# Refer-To Use Target Contact. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P51169=0

# RFC2543 Hold. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1 
P53162=1

# Dial Plan Prefix
# String
P51119=

# Disable DialPlan. 0 - No Selection, 1 - Dial Page, 2 - Contact, 4 - Incoming Call History, 8 -  Outgoing Call History, 16 - MPK & Click2Dial. 
# If need to check multiple selections, add the specific values for each selections together. Default value is 0
# Number: 0-31
P52182=0

# DialPlan. Default value is { x+ | \+x+ | *x+ | *xx*x+ | x+*x+*x+*x+ | x+*x+*x+*x+#x+ }
P51159={ x+ | \+x+ | *x+ | *xx*x+ | x+*x+*x+*x+ | x+*x+*x+*x+#x+ }

# Caller ID Display. 0 - Auto, 1 - Disabled, 2 - From Header. The default value is 0.
# Number: 0, 1, 2, 3
P52124=0

# Account Ringtone. See ring tone options and value in the Ring Tone Value Table below
P51123=content://settings/system/ringtone

# Ignore Alert-Info Header. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1
P53118=0

# Matching Incoming Caller ID. Matching Rule 1
# String
P53177=

# Matching Rule 1 Distinctive Ringtone. See ring tone options and value in the Ring Tone Value Table below
# String
P53178=content://settings/system/ringtone

# Matching Incoming Caller ID. Matching Rule 2
# String
P53179=

# Matching Rule 2 Distinctive Ringtone. See ring tone options and value in the Ring Tone Value Table below
# String
P53180=content://settings/system/ringtone

# Matching Incoming Caller ID. Matching Rule 3
# String
P53181=

# Matching Rule 3 Distinctive Ringtone. See ring tone options and value in the Ring Tone Value Table below
# String
P53182=content://settings/system/ringtone

############Ring Tone Value Table###############
# Web GUI Option                            Value
# Use System Ring tone                      content://settings/system/ringtone 
# Andromeda					/system/media/audio/ringtones/ANDROMEDA.ogg
# Aquila					/system/media/audio/ringtones/Aquila.ogg
# Argo Navis					/system/media/audio/ringtones/ArgoNavis.ogg
# Atria					/system/media/audio/ringtones/Atria.ogg
# Backroad					/system/media/audio/ringtones/Backroad.ogg
# Beat Plucker					/system/media/audio/ringtones/BeatPlucker.ogg
# Bell Phone					/system/media/audio/ringtones/Ring_Classic_02.ogg
# Bentley Dubs					/system/media/audio/ringtones/BentleyDubs.ogg
# Big Easy					/system/media/audio/ringtones/Big_Easy.ogg
# Bird Loop					/system/media/audio/ringtones/BirdLoop.ogg
# Bollywood					/system/media/audio/ringtones/Bollywood.ogg
# Boötes					/system/media/audio/ringtones/BOOTES.ogg
# Bus' a Move					/system/media/audio/ringtones/BussaMove.ogg
# Cairo					/system/media/audio/ringtones/Cairo.ogg
# Calypso Steel					/system/media/audio/ringtones/Calypso_Steel.ogg
# Canis Major					/system/media/audio/ringtones/CANISMAJOR.ogg
# Caribbean Ice					/system/media/audio/ringtones/CaribbeanIce.ogg
# Carina					/system/media/audio/ringtones/Carina.ogg
# Cassiopeia					/system/media/audio/ringtones/CASSIOPEIA.ogg
# Centaurus					/system/media/audio/ringtones/Centaurus.ogg
# Champagne Edition					/system/media/audio/ringtones/Champagne_Edition.ogg
# Chimey Phone					/system/media/audio/ringtones/Ring_Synth_02.ogg
# Club Cubano					/system/media/audio/ringtones/Club_Cubano.ogg
# Crayon Rock					/system/media/audio/ringtones/CrayonRock.ogg
# Crazy Dream					/system/media/audio/ringtones/CrazyDream.ogg
# Curve Ball Blend					/system/media/audio/ringtones/CurveBall.ogg
# Cygnus					/system/media/audio/ringtones/Cygnus.ogg
# Dancin' Fool					/system/media/audio/ringtones/DancinFool.ogg
# Digital Phone					/system/media/audio/ringtones/Ring_Digital_02.ogg
# Ding					/system/media/audio/ringtones/Ding.ogg
# DingDong					/system/media/audio/ringtones/DingDong.wav
# Don' Mess Wiv It					/system/media/audio/ringtones/DonMessWivIt.ogg
# Draco					/system/media/audio/ringtones/Draco.ogg
# Dream Theme					/system/media/audio/ringtones/DreamTheme.ogg
# Eastern Sky					/system/media/audio/ringtones/Eastern_Sky.ogg
# Enter the Nexus					/system/media/audio/ringtones/Enter_the_Nexus.ogg
# Eridani					/system/media/audio/ringtones/Eridani.ogg
# Ether Shake					/system/media/audio/ringtones/EtherShake.ogg
# Flutey Phone					/system/media/audio/ringtones/Ring_Synth_04.ogg
# Free Flight					/system/media/audio/ringtones/FreeFlight.ogg
# Friendly Ghost					/system/media/audio/ringtones/FriendlyGhost.ogg
# Funk Y'all					/system/media/audio/ringtones/Funk_Yall.ogg
# Game Over Guitar					/system/media/audio/ringtones/GameOverGuitar.ogg
# Gimme Mo' Town					/system/media/audio/ringtones/Gimme_Mo_Town.ogg
# Girtab					/system/media/audio/ringtones/Girtab.ogg
# Glacial Groove					/system/media/audio/ringtones/Glacial_Groove.ogg
# Growl					/system/media/audio/ringtones/Growl.ogg
# Halfway Home					/system/media/audio/ringtones/HalfwayHome.ogg
# Hydra					/system/media/audio/ringtones/Hydra.ogg
# Insert Coin					/system/media/audio/ringtones/InsertCoin.ogg
# Kuma					/system/media/audio/ringtones/Kuma.ogg
# Loopy Lounge					/system/media/audio/ringtones/LoopyLounge.ogg
# Love Flute					/system/media/audio/ringtones/LoveFlute.ogg
# Lyra					/system/media/audio/ringtones/Lyra.ogg
# Machina					/system/media/audio/ringtones/Machina.ogg
# Medieval Jaunt					/system/media/audio/ringtones/MidEvilJaunt.ogg
# Mildly Alarming					/system/media/audio/ringtones/MildlyAlarming.ogg
# Nairobi					/system/media/audio/ringtones/Nairobi.ogg
# Nassau					/system/media/audio/ringtones/Nassau.ogg
# New Player					/system/media/audio/ringtones/NewPlayer.ogg
# No Limits					/system/media/audio/ringtones/No_Limits.ogg
# Noisey One					/system/media/audio/ringtones/Noises1.ogg
# Organ Dub					/system/media/audio/ringtones/OrganDub.ogg
# Orion					/system/media/audio/ringtones/Orion.ogg
# Paradise Island					/system/media/audio/ringtones/Paradise_Island.ogg
# Pegasus					/system/media/audio/ringtones/Pegasus.ogg
# Perseus					/system/media/audio/ringtones/PERSEUS.ogg
# Playa					/system/media/audio/ringtones/Playa.ogg
# Pyxis					/system/media/audio/ringtones/Pyxis.ogg
# Rasalas					/system/media/audio/ringtones/Rasalas.ogg
# Revelation					/system/media/audio/ringtones/Revelation.ogg
# Rigel					/system/media/audio/ringtones/Rigel.ogg
# Road Trip					/system/media/audio/ringtones/Road_Trip.ogg
# Romancing The Tone					/system/media/audio/ringtones/RomancingTheTone.ogg
# Safari					/system/media/audio/ringtones/Safari.ogg
# Savannah					/system/media/audio/ringtones/Savannah.ogg
# Scarabaeus					/system/media/audio/ringtones/Scarabaeus.ogg
# Sceptrum					/system/media/audio/ringtones/Sceptrum.ogg
# Seville					/system/media/audio/ringtones/Seville.ogg
# She's All That					/system/media/audio/ringtones/Shes_All_That.ogg
# Silky Way					/system/media/audio/ringtones/SilkyWay.ogg
# Sitar Versus Sitar					/system/media/audio/ringtones/SitarVsSitar.ogg
# Solarium					/system/media/audio/ringtones/Solarium.ogg
# Springy Jalopy					/system/media/audio/ringtones/SpringyJalopy.ogg
# Steppin' Out					/system/media/audio/ringtones/Steppin_Out.ogg
# Terminated					/system/media/audio/ringtones/Terminated.ogg
# Terrible Twos					/system/media/audio/ringtones/Noises2.ogg
# Testudo					/system/media/audio/ringtones/Testudo.ogg
# Themos					/system/media/audio/ringtones/Themos.ogg
# Third Eye					/system/media/audio/ringtones/Third_Eye.ogg
# Thriller Three					/system/media/audio/ringtones/Noises3.ogg
# Thunderfoot					/system/media/audio/ringtones/Thunderfoot.ogg
# Twirl Away					/system/media/audio/ringtones/TwirlAway.ogg
# Ursa Minor					/system/media/audio/ringtones/URSAMINOR.ogg
# UrsaMinor					/system/media/audio/ringtones/UrsaMinor.ogg
# Very Alarmed					/system/media/audio/ringtones/VeryAlarmed.ogg
# Vespa					/system/media/audio/ringtones/Vespa.ogg
# World					/system/media/audio/ringtones/World.ogg
# Zeta					/system/media/audio/ringtones/Zeta.ogg
# bellcore-dr1					/system/media/audio/ringtones/bellcore-dr1.ogg
# bellcore-dr2					/system/media/audio/ringtones/bellcore-dr2.ogg
# bellcore-dr3					/system/media/audio/ringtones/bellcore-dr3.ogg
# bellcore-dr4					/system/media/audio/ringtones/bellcore-dr4.ogg
# bellcore-dr5					/system/media/audio/ringtones/bellcore-dr5.ogg
# speaker					/system/media/audio/ringtones/speaker.wav
#######################################################################
##  Account 12 Advanced Settings                                     ##
#######################################################################
# Check Domain Certificates. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P52111=0

# Validate Certificate Chain. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P52167=0

# Validate Incoming SIP Messages. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P52106=0

# Allow Unsolicited REFER. 0 - Disabled, 1 - Enabled, 2 - Enabled/Force Auth. Default value is 0.
# Number: 0, 1, 2
P53123=0

# Only Accept SIP Requests from Known Servers. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P52147=0

# Check SIP User ID for Incoming INVITE. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P51149=0

# Allow SIP Reset. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P53115=0

# Authenticate Incoming INVITE. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P52146=0

# SIP Realm Used for Challenge INVITE & NOTIFY.
# String
P53121=


# Enable Local MOH. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P52157=0

# Virtual Account Group. -1 - Default,  0 - Virtual Account Group 1, 1 - Virtual Account Group 2, 2 - Virtual Account Group 3
# 3 - Virtual Account Group 4, 4 - Virtual Account Group 5, 5 - Virtual Account Group 6, 6 - Virtual Account Group 7, 7 - Virtual Account Group 8
# 8 - Virtual Account Group 9, 9 - Virtual Account Group 10, 10 - Virtual Account Group 11, 11 - Virtual Account Group 12, 12 - Virtual Account Group 13
# 13 - Virtual Account Group 14, 14 - Virtual Account Group 15, 15 - Virtual Account Group 16. Default value is -1.
# Number: -1 - 15 
P52191=-1

# Special Feature. Default value is 100
# 100 - Standard, 102 - Broadsoft, 113 - China Mobile
# 114 - ZTE IMS, 115 - Mobotix, 116 - ZTE NGN, 117 - Huawei IMS, 123 - NEC, 125 - WorldStone
# Number: 100, 102, 113, 114, 115, 116, 117, 123, 125
P51124=100

# Allow Sync Phonebook via SIP Notify. 0 - No, 1 - Yes. Default is 1.
# Number: 0, 1
P53199=1
##############################################################################
##  Account 13 Settings                                                     ##
##############################################################################

#######################################################################
##  Account 13 General Settings                                      ##
#######################################################################

# Account Active. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P51201=0

# Account Name
P51217=

# SIP Server
P51202=

# SIP User ID
P51204=
 
# SIP Authentication ID
P51205=

# SIP Authentication Password
P51206=

# Voice Mail Access Number
P51226=

# Name (Display Name, e.g., John Doe)
P51207=

# Tel URI. 0 - Disable, 1 - User=Phone, 2 - Enabled. Default value is 0
# Number: 0, 1, 2
P51209=0

#######################################################################
##  Account 13 Network Settings                                      ##
#######################################################################

# Outbound Proxy
P51203=

# Secondary Outbound Proxy
P52233=

# DNS Mode. 0 - A Record, 1 - SRV, 2 - NAPTR/SRV. Default value is 0
# Number: 0, 1, 2
P51208=0

# DNS SRV Fail-over Mode. 0 - Default, 1 - Saved one until DNS TTL, 2 - Saved one until no response. Defualt value is 1
# Number
P53240=0

# Register Before DNS SRV Fail-over. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P54295=0

# NAT Traversal. 0 - NAT No, 1 - STUN, 2 - Keep-alive, 3 - UPnP, 4 - Auto, 5 - VPN. Default value is 2
# Number: 0, 1, 2, 3, 4, 5
P51214=2

# Proxy-Require
P51218=

#######################################################################
##  Account 13 SIP Settings                                          ##
#######################################################################

# SIP Registration. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P51210=1

# Unregister Before New Registration. 0 - No, 1 - All, 2 -  Instance . Default value is 2
# Number: 0, 1, 2
P51211=2

# Register Expiration (m). In minutes. Default value is 60
# Number: 0 - 64800
P51212=60

# Subscribe Expiration (m). Default is 60
# Number: 0 - 64800
P53251=60

# Re-register before Expiration (s). Default Value is 0
# Number : 0
P52230=0

# Registration Retry Wait Time (s). In seconds. Default value is 20
# Number: 1 - 3600
P51271=20

# Local SIP Port. Default value is 5084
# Number: 5 - 65535
P51213=5084

# SUBSCRIBE For MWI. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P51215=0

# Enable SIP OPTIONS Keep Alive. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P52297=0

# SIP OPTIONS Keep Alive Interval(s). Default value is 30
# Number 
P52298=30

# SIP OPTIONS Keep Alive Maximum Tries. Default value is 3
# Number 
P52299=3

# Enable Session Timer/ Session Expiration(s).  In seconds. Default value is 180 seconds.
# By default,  Session Timer is Enabled.  Session Timer is disabled if the value is 0.
# Number: 0 or 90 - 64800
P51234=180

# Min-SE(s). Default value is 90 seconds
# Number: 90 - 64800
P51227=90

# UAC Specify Refresher. 0 - Omit, 1 - UAC, 2 - UAS. Default value is 0
# Number: 0, 1, 2
P51232=0

# UAS Specify Refresher. 1 - UAC, 2 - UAS. Default value is 1
# Number: 1, 2
P51233=1

# Force INVITE. Always refresh with INVITE instead of UPDATE even when remote party supports UPDATE
# 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P51231=0

# Caller Request Timer. Request for timer when calling
# 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P51228=0

# Callee Request Timer
# Request for timer when being called (i.e., if remote party supports timer but did not request for one)
# 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P51229=0

# Force Timer. Still use timer when remote party does not support timer
# 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P51230=0

# Enable 100rel. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P51235=0

# Use Privacy Header
# 0 - Default, 1 - No, 2 - Yes. Default is 0
# Number: 0, 1, 2
P52238=0

# Use P-Preferred-Identity Header
# 0 - Default, 1 - No, 2 - Yes. Default is 0
# Number: 0, 1, 2
P52239=0

# Use P-Access-Network-Info Header. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P53258=1

# Use P-Emergency-Info Header. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P53259=1

# Use MAC Header.  0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P53261=0

# SIP Transport
# 0 - UDP , 1 - TCP, 2 - TLS. Default value is 0
# Number: 0, 1, 2
P51248=0

# SIP URI Scheme When Using TLS
# 0 -sip, 1 - sips. Default value is 0.
# Number: 0, 1
P52229=0

# Use Actual Ephemeral Port in Contact with TCP/TLS
# 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P52231=0

# Support SIP Instance ID
# 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P51289=1

# Add Auth Header On RE-REGISTER
# 0 - No, 1- Yes
P52259=1

# SIP T1 Timeout. RFC 3261 T1 value (RTT estimate)
# 50 - 0.5 sec, 100 - 1 sec, 200 - 2 sec. Default value is 50
# Number: 50, 100, 200
P51240=50

# SIP T2 Interval. RFC 3261 T2 value
# The maximum retransmit interval for non-INVITE requests and INVITE responses
# 200 - 2 sec, 400 - 4 sec, 800 - 8 sec. Default value is 400
# Number: 200, 400, 800.
P51241=400

# SIP Timer D Interval (Seconds)
# Number 0-64. Default value is 0
P52287=0

# Remove OBP from Route
# 0 - Disable, 1 - Enable, 2 - Always. Default value is 0
# Number: 0, 1, 2
P52205=0
#######################################################################
##  Account 13 Codec Settings                                        ##
#######################################################################
# Preferred Vocoder
# First codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 123 - Opus. Default value is 0
# Number: 0, 8, 9, 2, 18, 98, 123
P51251=0

# Second codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 123 - Opus. Default value is 8
# Number: 0, 8, 9, 2, 18, 98, 123
P51252=8

# Third codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 123 - Opus. Default value is 9
# Number: 0, 8, 9, 2, 18, 98, 123
P51253=9

# Forth codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 123 - Opus. Default value is 9
# Number: 0, 8, 9, 2, 18, 98, 123
P51254=9

# Fifth codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 123 - Opus. Default value is 9
# Number: 0, 8, 9, 2, 18, 98, 123
P51255=9

# Sixth codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 123 - Opus. Default value is 9
# Number: 0, 8, 9, 2, 18, 98, 123
P51256=9

# Seventh codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 123 - Opus. Default value is 9
# Number: 0, 8, 9, 2, 18, 98, 123
P51257=9

# Eigth codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 123 - Opus. Default value is 9
# Number: 0, 8, 9, 2, 18, 98, 123
P51258=9

# Codec Negotiation Priority. 0 - Caller, 1 - Callee. Default value is 1.
# Number: 0, 1
P54261=1

# Use First Matching Vocoder in 200OK SDP. 0 - No, 1 - Yes. The default value is 0.
# Number: 0, 1
P52248=0

# iLBC Frame Size. 0 - 20 ms, 1 - 30 ms. Default value is 1.
# Number: 0, 1
P51295=1

# G726-32 ITU Payload. 0 - 2, 1 - Dynamic. Default value is 0.
# Number: 0, 1
P52269=0

# G726-32 Dynamic PT. Default value is 126.
# Number
P52265=126

# Opus Payload Type
P52285=123

# DTMF: in audio. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P52201=0

# DTMF: via RFC2833. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P52202=1

# DTMF: via SIP INFO. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P52203=0

# DTMF Payload Type. Default value is 101
# Number: 96 - 126
P51296=101

# Enable Audio RED with FEC. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P53273=0

# Audio FEC Payload Type. Default value is 121
# Number: 96 - 126
P53274=121

# Audio RED Payload Type. Default value is 124
# Number: 96 - 126
P53275=124

# Silence Suppression. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P51285=0

# Voice Frames Per TX. Default value is 2
# Number: 1 - 64.
P51286=2

# Preferred Video Codec. 99 - H.264. Default is 99.
P51264=99

# Enable Video FEC. 0 - No, 1 - Yes. Default value is 1.
# Number: 0, 1
P52293=1

# Enable RFC5168 Support. 0 - No, 1 - Yes. Default value is 1.
# Number: 0, 1
P51278=1

# Video FEC Mode. 0 - 0, 1 - 1. Default value is 0.
# Number: 0, 1
P53222=0

# FEC Payload Type. Default value is 120.
P52294=120

# Packetization mode. 0 - Single NAL Unit Mode, 1 - Non-Interleaved Mode. Default value is 1.
# Number: 0, 1, 10
P53205=1

# H.264 Image Size. 9 - 720P, 1 - VGA, 5 - CIF, 4 - 4CIF, 0 - QVGA, 6 - QCIF. Default value is 9
# Number: 9, 1, 5, 4, 0, 6
P52207=9

# Use H.264 Constrained Profiles. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1
P53245=0

# H.264 Profile Type. 0 - Baseline Profile, 1 - Main Profile, 2 - High Profile, 3 - BP&MP&HP
# Number: 0, 1, 2, 3
P52262=0

# Video Bit Rate. 64 - 64 kbps, 96 - 96 kbps, 128 - 128 kbps, 160 - 160 kbps, 192 - 192 kbps
# 210 - 210 kbps, 256 - 256 kbps, 384 - 384 kbps, 512 - 512 kbps, 640 - 640 kbps, 768 - 768 kbps
# 1024 - 1024 kbps, 1280 - 1280 kbps, 1536 - 1536 kbps, 2048 - 2048 kbps. Default value is 2048.
# Number: 250, 500, 750
P52215=2048

# SDP Bandwidth Attribute. 0 - Standard, 1 - Media Level, 2 - Session Level, 3 - None. Default value is Media Level.
# Number: 0, 1, 2, 3
P52260=1

# H.264 Payload Type. Default value is 99.
P51262=99

# Disable BFCP. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1
P53201=0

# Presentation H.264 Image Size. 10 - 1080P, 9 - 720P. Default value is 10.
# Number: 10, 9
P52276=10

# Presentation H.264 Profile Type. 0 - Baseline Profile, 1 - Main Profile, 2 - High Profile, 3 - BP&MP&HP
# Number: 0, 1, 2, 3
P52277=3

# Presentation Video Bit Rate. 512 - 512 kbps, 640 - 640 kbps, 768 - 768 kbps
# 1024 - 1024 kbps, 1280 - 1280 kbps, 1536 - 1536 kbps, 2048 - 2048 kbps. Default value is 1024.
# Number: 250, 500, 750
P52278=1024

# Presentation Video Frame Rate. 5 - 5 frames/second, 10 - 10 frames/second, 15 - 15 frames/second. Default value is 15.
# Number: 5, 10, 15
P53242=

# BFCP Transport Protocol. 0 - Automatic, 1 - UDP, 2 - TCP. Default value is 1.
# Number: 0, 1, 2
P53241=

# SRTP Mode. 0 - Disable, 1 - Enable but not forced, 2 - Enable and forced. Default value is 0
# Number:0, 1, 2
P51243=0

# SRTP Key Length. 0 - AES 128&256 bit, 1 - AES 128 bit, 2 - AES 256 bit. Default value is 0
# Number:0, 1, 2
P52283=0 

# Enable SRTP Key Lifetime. 0 - No, 1 - Yes.
# Number: 0,1
P52263=0

# RTCP Destination
P52290=

# Symmetric RTP. 0 - No, 1 - Yes. Default value is 0
# Number:0, 1
P51260=0

# RTP IP Filter. 0 - Disable, 1 - IP Only, 2 - IP and Port. Default value is 0
# Number:0, 1, 2
P53226=0

# RTP Timeout(s). Default is 0. If set to 0, the device would not hangup.
# number: 0 - 600
P54268=0
#######################################################################
##  Account 13 Call Settings                                         ##
#######################################################################
# Enable Video Call. 0 - Default, 1 - No, 2 - Yes. Default is 0
# Number: 0, 1, 2
P61243=0

# Start Video Automatically. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P52214=1

# Remote Video Request. 0 - Prompt, 1 - Accept, 2 - Deny. Default value is 0
# Number: 0, 1, 2
P52226=0

# Video Layout. 0 - Default, 1 - Full screen, 3 - Equal split screen, 2 - Only display remote screen
P52232=0

# Auto Answer. 0 - No, 1 - Yes, 2 - Enable Intercom/Paging. Default value is 0
# Number: 0, 1, 2
P51225=0

# Play warning tone for Auto Answer Intercom. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P53272=1

# Intercom Barging. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P53219=1

# Auto Preview. 0 - No, 1 - Yes, 2 - Yes with Ringing. Default value is 0
# Number: 0, 1, 2
P54262=0

# Send Anonymous. 0 - No, 1 - Yes (caller ID will be blocked if set to Yes). Default value is 0
# Number: 0, 1
P51221=0

# Anonymous Call Rejection. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P51246=0

# Call Log
# 0 - Log All, 1 - Log Incoming/Outgoing only (Missed Calls Not Recorded), 2 - Disable Call All, 3 - Don't Prompt Missed Call. Default value is 0
# Number: 0, 1, 2
P51242=0

# Enable Call Features. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P51220=0

# Enable Call Waiting. 0 - Default, 1 - No, 2 - Yes.
# Number: 0, 1, 2
P53263=0

# Mute on Answer Intercom Call. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
P53271=0

# Transfer on 3 way conference Hangup. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P52204=0

# Use # as Dial Key. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P51292=1

# Use # as Redial Key. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P54269=1

# DND Call Feature On.
# String
P52244=

# DND Call Feature Off.
# String
P52245=

# No Key Entry Timeout (s). Default value is 4
# Number: 1 - 15
P51291=4

# Ring Timeout (s). Default value is 60
# Number: 10 - 300
P51276=60

# Refer-To Use Target Contact. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P51269=0

# RFC2543 Hold. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1 
P53262=1

# Dial Plan Prefix
# String
P51219=

# Disable DialPlan. 0 - No Selection, 1 - Dial Page, 2 - Contact, 4 - Incoming Call History, 8 -  Outgoing Call History, 16 - MPK & Click2Dial. 
# If need to check multiple selections, add the specific values for each selections together. Default value is 0
# Number: 0-31
P52282=0

# DialPlan. Default value is { x+ | \+x+ | *x+ | *xx*x+ | x+*x+*x+*x+ | x+*x+*x+*x+#x+ }
P51259={ x+ | \+x+ | *x+ | *xx*x+ | x+*x+*x+*x+ | x+*x+*x+*x+#x+ }

# Caller ID Display. 0 - Auto, 1 - Disabled, 2 - From Header. The default value is 0.
# Number: 0, 1, 2, 3
P52224=0

# Account Ringtone. See ring tone options and value in the Ring Tone Value Table below
P51223=content://settings/system/ringtone

# Ignore Alert-Info Header. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1
P53218=0

# Matching Incoming Caller ID. Matching Rule 1
# String
P53277=

# Matching Rule 1 Distinctive Ringtone. See ring tone options and value in the Ring Tone Value Table below
# String
P53278=content://settings/system/ringtone

# Matching Incoming Caller ID. Matching Rule 2
# String
P53279=

# Matching Rule 2 Distinctive Ringtone. See ring tone options and value in the Ring Tone Value Table below
# String
P53280=content://settings/system/ringtone

# Matching Incoming Caller ID. Matching Rule 3
# String
P53281=

# Matching Rule 3 Distinctive Ringtone. See ring tone options and value in the Ring Tone Value Table below
# String
P53282=content://settings/system/ringtone

############Ring Tone Value Table###############
# Web GUI Option                            Value
# Use System Ring tone                      content://settings/system/ringtone 
# Andromeda					/system/media/audio/ringtones/ANDROMEDA.ogg
# Aquila					/system/media/audio/ringtones/Aquila.ogg
# Argo Navis					/system/media/audio/ringtones/ArgoNavis.ogg
# Atria					/system/media/audio/ringtones/Atria.ogg
# Backroad					/system/media/audio/ringtones/Backroad.ogg
# Beat Plucker					/system/media/audio/ringtones/BeatPlucker.ogg
# Bell Phone					/system/media/audio/ringtones/Ring_Classic_02.ogg
# Bentley Dubs					/system/media/audio/ringtones/BentleyDubs.ogg
# Big Easy					/system/media/audio/ringtones/Big_Easy.ogg
# Bird Loop					/system/media/audio/ringtones/BirdLoop.ogg
# Bollywood					/system/media/audio/ringtones/Bollywood.ogg
# Boötes					/system/media/audio/ringtones/BOOTES.ogg
# Bus' a Move					/system/media/audio/ringtones/BussaMove.ogg
# Cairo					/system/media/audio/ringtones/Cairo.ogg
# Calypso Steel					/system/media/audio/ringtones/Calypso_Steel.ogg
# Canis Major					/system/media/audio/ringtones/CANISMAJOR.ogg
# Caribbean Ice					/system/media/audio/ringtones/CaribbeanIce.ogg
# Carina					/system/media/audio/ringtones/Carina.ogg
# Cassiopeia					/system/media/audio/ringtones/CASSIOPEIA.ogg
# Centaurus					/system/media/audio/ringtones/Centaurus.ogg
# Champagne Edition					/system/media/audio/ringtones/Champagne_Edition.ogg
# Chimey Phone					/system/media/audio/ringtones/Ring_Synth_02.ogg
# Club Cubano					/system/media/audio/ringtones/Club_Cubano.ogg
# Crayon Rock					/system/media/audio/ringtones/CrayonRock.ogg
# Crazy Dream					/system/media/audio/ringtones/CrazyDream.ogg
# Curve Ball Blend					/system/media/audio/ringtones/CurveBall.ogg
# Cygnus					/system/media/audio/ringtones/Cygnus.ogg
# Dancin' Fool					/system/media/audio/ringtones/DancinFool.ogg
# Digital Phone					/system/media/audio/ringtones/Ring_Digital_02.ogg
# Ding					/system/media/audio/ringtones/Ding.ogg
# DingDong					/system/media/audio/ringtones/DingDong.wav
# Don' Mess Wiv It					/system/media/audio/ringtones/DonMessWivIt.ogg
# Draco					/system/media/audio/ringtones/Draco.ogg
# Dream Theme					/system/media/audio/ringtones/DreamTheme.ogg
# Eastern Sky					/system/media/audio/ringtones/Eastern_Sky.ogg
# Enter the Nexus					/system/media/audio/ringtones/Enter_the_Nexus.ogg
# Eridani					/system/media/audio/ringtones/Eridani.ogg
# Ether Shake					/system/media/audio/ringtones/EtherShake.ogg
# Flutey Phone					/system/media/audio/ringtones/Ring_Synth_04.ogg
# Free Flight					/system/media/audio/ringtones/FreeFlight.ogg
# Friendly Ghost					/system/media/audio/ringtones/FriendlyGhost.ogg
# Funk Y'all					/system/media/audio/ringtones/Funk_Yall.ogg
# Game Over Guitar					/system/media/audio/ringtones/GameOverGuitar.ogg
# Gimme Mo' Town					/system/media/audio/ringtones/Gimme_Mo_Town.ogg
# Girtab					/system/media/audio/ringtones/Girtab.ogg
# Glacial Groove					/system/media/audio/ringtones/Glacial_Groove.ogg
# Growl					/system/media/audio/ringtones/Growl.ogg
# Halfway Home					/system/media/audio/ringtones/HalfwayHome.ogg
# Hydra					/system/media/audio/ringtones/Hydra.ogg
# Insert Coin					/system/media/audio/ringtones/InsertCoin.ogg
# Kuma					/system/media/audio/ringtones/Kuma.ogg
# Loopy Lounge					/system/media/audio/ringtones/LoopyLounge.ogg
# Love Flute					/system/media/audio/ringtones/LoveFlute.ogg
# Lyra					/system/media/audio/ringtones/Lyra.ogg
# Machina					/system/media/audio/ringtones/Machina.ogg
# Medieval Jaunt					/system/media/audio/ringtones/MidEvilJaunt.ogg
# Mildly Alarming					/system/media/audio/ringtones/MildlyAlarming.ogg
# Nairobi					/system/media/audio/ringtones/Nairobi.ogg
# Nassau					/system/media/audio/ringtones/Nassau.ogg
# New Player					/system/media/audio/ringtones/NewPlayer.ogg
# No Limits					/system/media/audio/ringtones/No_Limits.ogg
# Noisey One					/system/media/audio/ringtones/Noises1.ogg
# Organ Dub					/system/media/audio/ringtones/OrganDub.ogg
# Orion					/system/media/audio/ringtones/Orion.ogg
# Paradise Island					/system/media/audio/ringtones/Paradise_Island.ogg
# Pegasus					/system/media/audio/ringtones/Pegasus.ogg
# Perseus					/system/media/audio/ringtones/PERSEUS.ogg
# Playa					/system/media/audio/ringtones/Playa.ogg
# Pyxis					/system/media/audio/ringtones/Pyxis.ogg
# Rasalas					/system/media/audio/ringtones/Rasalas.ogg
# Revelation					/system/media/audio/ringtones/Revelation.ogg
# Rigel					/system/media/audio/ringtones/Rigel.ogg
# Road Trip					/system/media/audio/ringtones/Road_Trip.ogg
# Romancing The Tone					/system/media/audio/ringtones/RomancingTheTone.ogg
# Safari					/system/media/audio/ringtones/Safari.ogg
# Savannah					/system/media/audio/ringtones/Savannah.ogg
# Scarabaeus					/system/media/audio/ringtones/Scarabaeus.ogg
# Sceptrum					/system/media/audio/ringtones/Sceptrum.ogg
# Seville					/system/media/audio/ringtones/Seville.ogg
# She's All That					/system/media/audio/ringtones/Shes_All_That.ogg
# Silky Way					/system/media/audio/ringtones/SilkyWay.ogg
# Sitar Versus Sitar					/system/media/audio/ringtones/SitarVsSitar.ogg
# Solarium					/system/media/audio/ringtones/Solarium.ogg
# Springy Jalopy					/system/media/audio/ringtones/SpringyJalopy.ogg
# Steppin' Out					/system/media/audio/ringtones/Steppin_Out.ogg
# Terminated					/system/media/audio/ringtones/Terminated.ogg
# Terrible Twos					/system/media/audio/ringtones/Noises2.ogg
# Testudo					/system/media/audio/ringtones/Testudo.ogg
# Themos					/system/media/audio/ringtones/Themos.ogg
# Third Eye					/system/media/audio/ringtones/Third_Eye.ogg
# Thriller Three					/system/media/audio/ringtones/Noises3.ogg
# Thunderfoot					/system/media/audio/ringtones/Thunderfoot.ogg
# Twirl Away					/system/media/audio/ringtones/TwirlAway.ogg
# Ursa Minor					/system/media/audio/ringtones/URSAMINOR.ogg
# UrsaMinor					/system/media/audio/ringtones/UrsaMinor.ogg
# Very Alarmed					/system/media/audio/ringtones/VeryAlarmed.ogg
# Vespa					/system/media/audio/ringtones/Vespa.ogg
# World					/system/media/audio/ringtones/World.ogg
# Zeta					/system/media/audio/ringtones/Zeta.ogg
# bellcore-dr1					/system/media/audio/ringtones/bellcore-dr1.ogg
# bellcore-dr2					/system/media/audio/ringtones/bellcore-dr2.ogg
# bellcore-dr3					/system/media/audio/ringtones/bellcore-dr3.ogg
# bellcore-dr4					/system/media/audio/ringtones/bellcore-dr4.ogg
# bellcore-dr5					/system/media/audio/ringtones/bellcore-dr5.ogg
# speaker					/system/media/audio/ringtones/speaker.wav
#######################################################################
##  Account 13 Advanced Settings                                     ##
#######################################################################
# Check Domain Certificates. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P52211=0

# Validate Certificate Chain. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P52267=0

# Validate Incoming SIP Messages. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P52206=0

# Allow Unsolicited REFER. 0 - Disabled, 1 - Enabled, 2 - Enabled/Force Auth. Default value is 0.
# Number: 0, 1, 2
P53223=0

# Only Accept SIP Requests from Known Servers. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P52247=0

# Check SIP User ID for Incoming INVITE. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P51249=0

# Allow SIP Reset. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P53215=0

# Authenticate Incoming INVITE. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P52246=0

# SIP Realm Used for Challenge INVITE & NOTIFY.
# String
P53221=


# Enable Local MOH. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P52257=0

# Virtual Account Group. -1 - Default,  0 - Virtual Account Group 1, 1 - Virtual Account Group 2, 2 - Virtual Account Group 3
# 3 - Virtual Account Group 4, 4 - Virtual Account Group 5, 5 - Virtual Account Group 6, 6 - Virtual Account Group 7, 7 - Virtual Account Group 8
# 8 - Virtual Account Group 9, 9 - Virtual Account Group 10, 10 - Virtual Account Group 11, 11 - Virtual Account Group 12, 12 - Virtual Account Group 13
# 13 - Virtual Account Group 14, 14 - Virtual Account Group 15, 15 - Virtual Account Group 16. Default value is -1.
# Number: -1 - 15 
P52291=-1

# Special Feature. Default value is 100
# 100 - Standard, 102 - Broadsoft, 113 - China Mobile
# 114 - ZTE IMS, 115 - Mobotix, 116 - ZTE NGN, 117 - Huawei IMS, 123 - NEC, 125 - WorldStone
# Number: 100, 102, 113, 114, 115, 116, 117, 123, 125
P51224=100

# Allow Sync Phonebook via SIP Notify. 0 - No, 1 - Yes. Default is 1.
# Number: 0, 1
P53299=1
##############################################################################
##  Account 14 Settings                                                     ##
##############################################################################

#######################################################################
##  Account 14 General Settings                                      ##
#######################################################################

# Account Active. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P51301=0

# Account Name
P51317=

# SIP Server
P51302=

# SIP User ID
P51304=
 
# SIP Authentication ID
P51305=

# SIP Authentication Password
P51306=

# Voice Mail Access Number
P51326=

# Name (Display Name, e.g., John Doe)
P51307=

# Tel URI. 0 - Disable, 1 - User=Phone, 2 - Enabled. Default value is 0
# Number: 0, 1, 2
P51309=0

#######################################################################
##  Account 14 Network Settings                                      ##
#######################################################################

# Outbound Proxy
P51303=

# Secondary Outbound Proxy
P52333=

# DNS Mode. 0 - A Record, 1 - SRV, 2 - NAPTR/SRV. Default value is 0
# Number: 0, 1, 2
P51308=0

# DNS SRV Fail-over Mode. 0 - Default, 1 - Saved one until DNS TTL, 2 - Saved one until no response. Defualt value is 1
# Number
P53340=0

# Register Before DNS SRV Fail-over. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P54395=0

# NAT Traversal. 0 - NAT No, 1 - STUN, 2 - Keep-alive, 3 - UPnP, 4 - Auto, 5 - VPN. Default value is 2
# Number: 0, 1, 2, 3, 4, 5
P51314=2

# Proxy-Require
P51318=

#######################################################################
##  Account 14 SIP Settings                                          ##
#######################################################################

# SIP Registration. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P51310=1

# Unregister Before New Registration. 0 - No, 1 - All, 2 -  Instance . Default value is 2
# Number: 0, 1, 2
P51311=2

# Register Expiration (m). In minutes. Default value is 60
# Number: 0 - 64800
P51312=60

# Subscribe Expiration (m). Default is 60
# Number: 0 - 64800
P53351=60

# Re-register before Expiration (s). Default Value is 0
# Number : 0
P52330=0

# Registration Retry Wait Time (s). In seconds. Default value is 20
# Number: 1 - 3600
P51371=20

# Local SIP Port. Default value is 5086
# Number: 5 - 65535
P51313=5086

# SUBSCRIBE For MWI. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P51315=0

# Enable SIP OPTIONS Keep Alive. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P52397=0

# SIP OPTIONS Keep Alive Interval(s). Default value is 30
# Number 
P52398=30

# SIP OPTIONS Keep Alive Maximum Tries. Default value is 3
# Number 
P52399=3

# Enable Session Timer/ Session Expiration(s).  In seconds. Default value is 180 seconds.
# By default,  Session Timer is Enabled.  Session Timer is disabled if the value is 0.
# Number: 0 or 90 - 64800
P51334=180

# Min-SE(s). Default value is 90 seconds
# Number: 90 - 64800
P51327=90

# UAC Specify Refresher. 0 - Omit, 1 - UAC, 2 - UAS. Default value is 0
# Number: 0, 1, 2
P51332=0

# UAS Specify Refresher. 1 - UAC, 2 - UAS. Default value is 1
# Number: 1, 2
P51333=1

# Force INVITE. Always refresh with INVITE instead of UPDATE even when remote party supports UPDATE
# 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P51331=0

# Caller Request Timer. Request for timer when calling
# 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P51328=0

# Callee Request Timer
# Request for timer when being called (i.e., if remote party supports timer but did not request for one)
# 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P51329=0

# Force Timer. Still use timer when remote party does not support timer
# 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P51330=0

# Enable 100rel. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P51335=0

# Use Privacy Header
# 0 - Default, 1 - No, 2 - Yes. Default is 0
# Number: 0, 1, 2
P52338=0

# Use P-Preferred-Identity Header
# 0 - Default, 1 - No, 2 - Yes. Default is 0
# Number: 0, 1, 2
P52339=0

# Use P-Access-Network-Info Header. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P53358=1

# Use P-Emergency-Info Header. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P53359=1

# Use MAC Header.  0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P53361=0

# SIP Transport
# 0 - UDP , 1 - TCP, 2 - TLS. Default value is 0
# Number: 0, 1, 2
P51348=0

# SIP URI Scheme When Using TLS
# 0 -sip, 1 - sips. Default value is 0.
# Number: 0, 1
P52329=0

# Use Actual Ephemeral Port in Contact with TCP/TLS
# 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P52331=0

# Support SIP Instance ID
# 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P51389=1

# Add Auth Header On RE-REGISTER
# 0 - No, 1- Yes
P52359=1

# SIP T1 Timeout. RFC 3261 T1 value (RTT estimate)
# 50 - 0.5 sec, 100 - 1 sec, 200 - 2 sec. Default value is 50
# Number: 50, 100, 200
P51340=50

# SIP T2 Interval. RFC 3261 T2 value
# The maximum retransmit interval for non-INVITE requests and INVITE responses
# 200 - 2 sec, 400 - 4 sec, 800 - 8 sec. Default value is 400
# Number: 200, 400, 800.
P51341=400

# SIP Timer D Interval (Seconds)
# Number 0-64. Default value is 0
P52387=0

# Remove OBP from Route
# 0 - Disable, 1 - Enable, 2 - Always. Default value is 0
# Number: 0, 1, 2
P52305=0
#######################################################################
##  Account 14 Codec Settings                                        ##
#######################################################################
# Preferred Vocoder
# First codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 123 - Opus. Default value is 0
# Number: 0, 8, 9, 2, 18, 98, 123
P51351=0

# Second codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 123 - Opus. Default value is 8
# Number: 0, 8, 9, 2, 18, 98, 123
P51352=8

# Third codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 123 - Opus. Default value is 9
# Number: 0, 8, 9, 2, 18, 98, 123
P51353=9

# Forth codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 123 - Opus. Default value is 9
# Number: 0, 8, 9, 2, 18, 98, 123
P51354=9

# Fifth codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 123 - Opus. Default value is 9
# Number: 0, 8, 9, 2, 18, 98, 123
P51355=9

# Sixth codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 123 - Opus. Default value is 9
# Number: 0, 8, 9, 2, 18, 98, 123
P51356=9

# Seventh codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 123 - Opus. Default value is 9
# Number: 0, 8, 9, 2, 18, 98, 123
P51357=9

# Eigth codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 123 - Opus. Default value is 9
# Number: 0, 8, 9, 2, 18, 98, 123
P51358=9

# Codec Negotiation Priority. 0 - Caller, 1 - Callee. Default value is 1.
# Number: 0, 1
P54361=1

# Use First Matching Vocoder in 200OK SDP. 0 - No, 1 - Yes. The default value is 0.
# Number: 0, 1
P52348=0

# iLBC Frame Size. 0 - 20 ms, 1 - 30 ms. Default value is 1.
# Number: 0, 1
P51395=1

# G726-32 ITU Payload. 0 - 2, 1 - Dynamic. Default value is 0.
# Number: 0, 1
P52369=0

# G726-32 Dynamic PT. Default value is 126.
# Number
P52365=126

# Opus Payload Type
P52385=123

# DTMF: in audio. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P52301=0

# DTMF: via RFC2833. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P52302=1

# DTMF: via SIP INFO. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P52303=0

# DTMF Payload Type. Default value is 101
# Number: 96 - 126
P51396=101

# Enable Audio RED with FEC. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P53373=0

# Audio FEC Payload Type. Default value is 121
# Number: 96 - 126
P53374=121

# Audio RED Payload Type. Default value is 124
# Number: 96 - 126
P53375=124

# Silence Suppression. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P51385=0

# Voice Frames Per TX. Default value is 2
# Number: 1 - 64.
P51386=2

# Preferred Video Codec. 99 - H.264. Default is 99.
P51364=99

# Enable Video FEC. 0 - No, 1 - Yes. Default value is 1.
# Number: 0, 1
P52393=1

# Enable RFC5168 Support. 0 - No, 1 - Yes. Default value is 1.
# Number: 0, 1
P51378=1

# Video FEC Mode. 0 - 0, 1 - 1. Default value is 0.
# Number: 0, 1
P53322=0

# FEC Payload Type. Default value is 120.
P52394=120

# Packetization mode. 0 - Single NAL Unit Mode, 1 - Non-Interleaved Mode. Default value is 1.
# Number: 0, 1, 10
P53305=1

# H.264 Image Size. 9 - 720P, 1 - VGA, 5 - CIF, 4 - 4CIF, 0 - QVGA, 6 - QCIF. Default value is 9
# Number: 9, 1, 5, 4, 0, 6
P52307=9

# Use H.264 Constrained Profiles. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1
P53345=0

# H.264 Profile Type. 0 - Baseline Profile, 1 - Main Profile, 2 - High Profile, 3 - BP&MP&HP
# Number: 0, 1, 2, 3
P52362=0

# Video Bit Rate. 64 - 64 kbps, 96 - 96 kbps, 128 - 128 kbps, 160 - 160 kbps, 192 - 192 kbps
# 210 - 210 kbps, 256 - 256 kbps, 384 - 384 kbps, 512 - 512 kbps, 640 - 640 kbps, 768 - 768 kbps
# 1024 - 1024 kbps, 1280 - 1280 kbps, 1536 - 1536 kbps, 2048 - 2048 kbps. Default value is 2048.
# Number: 250, 500, 750
P52315=2048

# SDP Bandwidth Attribute. 0 - Standard, 1 - Media Level, 2 - Session Level, 3 - None. Default value is Media Level.
# Number: 0, 1, 2, 3
P52360=1

# H.264 Payload Type. Default value is 99.
P51362=99

# Disable BFCP. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1
P53301=0

# Presentation H.264 Image Size. 10 - 1080P, 9 - 720P. Default value is 10.
# Number: 10, 9
P52376=10

# Presentation H.264 Profile Type. 0 - Baseline Profile, 1 - Main Profile, 2 - High Profile, 3 - BP&MP&HP
# Number: 0, 1, 2, 3
P52377=3

# Presentation Video Bit Rate. 512 - 512 kbps, 640 - 640 kbps, 768 - 768 kbps
# 1024 - 1024 kbps, 1280 - 1280 kbps, 1536 - 1536 kbps, 2048 - 2048 kbps. Default value is 1024.
# Number: 250, 500, 750
P52378=1024

# Presentation Video Frame Rate. 5 - 5 frames/second, 10 - 10 frames/second, 15 - 15 frames/second. Default value is 15.
# Number: 5, 10, 15
P53342=

# BFCP Transport Protocol. 0 - Automatic, 1 - UDP, 2 - TCP. Default value is 1.
# Number: 0, 1, 2
P53341=

# SRTP Mode. 0 - Disable, 1 - Enable but not forced, 2 - Enable and forced. Default value is 0
# Number:0, 1, 2
P51343=0

# SRTP Key Length. 0 - AES 128&256 bit, 1 - AES 128 bit, 2 - AES 256 bit. Default value is 0
# Number:0, 1, 2
P52383=0 

# Enable SRTP Key Lifetime. 0 - No, 1 - Yes.
# Number: 0,1
P52363=0

# RTCP Destination
P52390=

# Symmetric RTP. 0 - No, 1 - Yes. Default value is 0
# Number:0, 1
P51360=0

# RTP IP Filter. 0 - Disable, 1 - IP Only, 2 - IP and Port. Default value is 0
# Number:0, 1, 2
P53326=0

# RTP Timeout(s). Default is 0. If set to 0, the device would not hangup.
# number: 0 - 600
P54368=0
#######################################################################
##  Account 14 Call Settings                                         ##
#######################################################################
# Enable Video Call. 0 - Default, 1 - No, 2 - Yes. Default is 0
# Number: 0, 1, 2
P61343=0

# Start Video Automatically. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P52314=1

# Remote Video Request. 0 - Prompt, 1 - Accept, 2 - Deny. Default value is 0
# Number: 0, 1, 2
P52326=0

# Video Layout. 0 - Default, 1 - Full screen, 3 - Equal split screen, 2 - Only display remote screen
P52332=0

# Auto Answer. 0 - No, 1 - Yes, 2 - Enable Intercom/Paging. Default value is 0
# Number: 0, 1, 2
P51325=0

# Play warning tone for Auto Answer Intercom. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P53372=1

# Intercom Barging. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P53319=1

# Auto Preview. 0 - No, 1 - Yes, 2 - Yes with Ringing. Default value is 0
# Number: 0, 1, 2
P54362=0

# Send Anonymous. 0 - No, 1 - Yes (caller ID will be blocked if set to Yes). Default value is 0
# Number: 0, 1
P51321=0

# Anonymous Call Rejection. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P51346=0

# Call Log
# 0 - Log All, 1 - Log Incoming/Outgoing only (Missed Calls Not Recorded), 2 - Disable Call All, 3 - Don't Prompt Missed Call. Default value is 0
# Number: 0, 1, 2
P51342=0

# Enable Call Features. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P51320=0

# Enable Call Waiting. 0 - Default, 1 - No, 2 - Yes.
# Number: 0, 1, 2
P53363=0

# Mute on Answer Intercom Call. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
P53371=0

# Transfer on 3 way conference Hangup. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P52304=0

# Use # as Dial Key. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P51392=1

# Use # as Redial Key. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P54369=1

# DND Call Feature On.
# String
P52344=

# DND Call Feature Off.
# String
P52345=

# No Key Entry Timeout (s). Default value is 4
# Number: 1 - 15
P51391=4

# Ring Timeout (s). Default value is 60
# Number: 10 - 300
P51376=60

# Refer-To Use Target Contact. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P51369=0

# RFC2543 Hold. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1 
P53362=1

# Dial Plan Prefix
# String
P51319=

# Disable DialPlan. 0 - No Selection, 1 - Dial Page, 2 - Contact, 4 - Incoming Call History, 8 -  Outgoing Call History, 16 - MPK & Click2Dial. 
# If need to check multiple selections, add the specific values for each selections together. Default value is 0
# Number: 0-31
P52382=0

# DialPlan. Default value is { x+ | \+x+ | *x+ | *xx*x+ | x+*x+*x+*x+ | x+*x+*x+*x+#x+ }
P51359={ x+ | \+x+ | *x+ | *xx*x+ | x+*x+*x+*x+ | x+*x+*x+*x+#x+ }

# Caller ID Display. 0 - Auto, 1 - Disabled, 2 - From Header. The default value is 0.
# Number: 0, 1, 2, 3
P52324=0

# Account Ringtone. See ring tone options and value in the Ring Tone Value Table below
P51323=content://settings/system/ringtone

# Ignore Alert-Info Header. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1
P53318=0

# Matching Incoming Caller ID. Matching Rule 1
# String
P53377=

# Matching Rule 1 Distinctive Ringtone. See ring tone options and value in the Ring Tone Value Table below
# String
P53378=content://settings/system/ringtone

# Matching Incoming Caller ID. Matching Rule 2
# String
P53379=

# Matching Rule 2 Distinctive Ringtone. See ring tone options and value in the Ring Tone Value Table below
# String
P53380=content://settings/system/ringtone

# Matching Incoming Caller ID. Matching Rule 3
# String
P53381=

# Matching Rule 3 Distinctive Ringtone. See ring tone options and value in the Ring Tone Value Table below
# String
P53382=content://settings/system/ringtone

############Ring Tone Value Table###############
# Web GUI Option                            Value
# Use System Ring tone                      content://settings/system/ringtone 
# Andromeda					/system/media/audio/ringtones/ANDROMEDA.ogg
# Aquila					/system/media/audio/ringtones/Aquila.ogg
# Argo Navis					/system/media/audio/ringtones/ArgoNavis.ogg
# Atria					/system/media/audio/ringtones/Atria.ogg
# Backroad					/system/media/audio/ringtones/Backroad.ogg
# Beat Plucker					/system/media/audio/ringtones/BeatPlucker.ogg
# Bell Phone					/system/media/audio/ringtones/Ring_Classic_02.ogg
# Bentley Dubs					/system/media/audio/ringtones/BentleyDubs.ogg
# Big Easy					/system/media/audio/ringtones/Big_Easy.ogg
# Bird Loop					/system/media/audio/ringtones/BirdLoop.ogg
# Bollywood					/system/media/audio/ringtones/Bollywood.ogg
# Boötes					/system/media/audio/ringtones/BOOTES.ogg
# Bus' a Move					/system/media/audio/ringtones/BussaMove.ogg
# Cairo					/system/media/audio/ringtones/Cairo.ogg
# Calypso Steel					/system/media/audio/ringtones/Calypso_Steel.ogg
# Canis Major					/system/media/audio/ringtones/CANISMAJOR.ogg
# Caribbean Ice					/system/media/audio/ringtones/CaribbeanIce.ogg
# Carina					/system/media/audio/ringtones/Carina.ogg
# Cassiopeia					/system/media/audio/ringtones/CASSIOPEIA.ogg
# Centaurus					/system/media/audio/ringtones/Centaurus.ogg
# Champagne Edition					/system/media/audio/ringtones/Champagne_Edition.ogg
# Chimey Phone					/system/media/audio/ringtones/Ring_Synth_02.ogg
# Club Cubano					/system/media/audio/ringtones/Club_Cubano.ogg
# Crayon Rock					/system/media/audio/ringtones/CrayonRock.ogg
# Crazy Dream					/system/media/audio/ringtones/CrazyDream.ogg
# Curve Ball Blend					/system/media/audio/ringtones/CurveBall.ogg
# Cygnus					/system/media/audio/ringtones/Cygnus.ogg
# Dancin' Fool					/system/media/audio/ringtones/DancinFool.ogg
# Digital Phone					/system/media/audio/ringtones/Ring_Digital_02.ogg
# Ding					/system/media/audio/ringtones/Ding.ogg
# DingDong					/system/media/audio/ringtones/DingDong.wav
# Don' Mess Wiv It					/system/media/audio/ringtones/DonMessWivIt.ogg
# Draco					/system/media/audio/ringtones/Draco.ogg
# Dream Theme					/system/media/audio/ringtones/DreamTheme.ogg
# Eastern Sky					/system/media/audio/ringtones/Eastern_Sky.ogg
# Enter the Nexus					/system/media/audio/ringtones/Enter_the_Nexus.ogg
# Eridani					/system/media/audio/ringtones/Eridani.ogg
# Ether Shake					/system/media/audio/ringtones/EtherShake.ogg
# Flutey Phone					/system/media/audio/ringtones/Ring_Synth_04.ogg
# Free Flight					/system/media/audio/ringtones/FreeFlight.ogg
# Friendly Ghost					/system/media/audio/ringtones/FriendlyGhost.ogg
# Funk Y'all					/system/media/audio/ringtones/Funk_Yall.ogg
# Game Over Guitar					/system/media/audio/ringtones/GameOverGuitar.ogg
# Gimme Mo' Town					/system/media/audio/ringtones/Gimme_Mo_Town.ogg
# Girtab					/system/media/audio/ringtones/Girtab.ogg
# Glacial Groove					/system/media/audio/ringtones/Glacial_Groove.ogg
# Growl					/system/media/audio/ringtones/Growl.ogg
# Halfway Home					/system/media/audio/ringtones/HalfwayHome.ogg
# Hydra					/system/media/audio/ringtones/Hydra.ogg
# Insert Coin					/system/media/audio/ringtones/InsertCoin.ogg
# Kuma					/system/media/audio/ringtones/Kuma.ogg
# Loopy Lounge					/system/media/audio/ringtones/LoopyLounge.ogg
# Love Flute					/system/media/audio/ringtones/LoveFlute.ogg
# Lyra					/system/media/audio/ringtones/Lyra.ogg
# Machina					/system/media/audio/ringtones/Machina.ogg
# Medieval Jaunt					/system/media/audio/ringtones/MidEvilJaunt.ogg
# Mildly Alarming					/system/media/audio/ringtones/MildlyAlarming.ogg
# Nairobi					/system/media/audio/ringtones/Nairobi.ogg
# Nassau					/system/media/audio/ringtones/Nassau.ogg
# New Player					/system/media/audio/ringtones/NewPlayer.ogg
# No Limits					/system/media/audio/ringtones/No_Limits.ogg
# Noisey One					/system/media/audio/ringtones/Noises1.ogg
# Organ Dub					/system/media/audio/ringtones/OrganDub.ogg
# Orion					/system/media/audio/ringtones/Orion.ogg
# Paradise Island					/system/media/audio/ringtones/Paradise_Island.ogg
# Pegasus					/system/media/audio/ringtones/Pegasus.ogg
# Perseus					/system/media/audio/ringtones/PERSEUS.ogg
# Playa					/system/media/audio/ringtones/Playa.ogg
# Pyxis					/system/media/audio/ringtones/Pyxis.ogg
# Rasalas					/system/media/audio/ringtones/Rasalas.ogg
# Revelation					/system/media/audio/ringtones/Revelation.ogg
# Rigel					/system/media/audio/ringtones/Rigel.ogg
# Road Trip					/system/media/audio/ringtones/Road_Trip.ogg
# Romancing The Tone					/system/media/audio/ringtones/RomancingTheTone.ogg
# Safari					/system/media/audio/ringtones/Safari.ogg
# Savannah					/system/media/audio/ringtones/Savannah.ogg
# Scarabaeus					/system/media/audio/ringtones/Scarabaeus.ogg
# Sceptrum					/system/media/audio/ringtones/Sceptrum.ogg
# Seville					/system/media/audio/ringtones/Seville.ogg
# She's All That					/system/media/audio/ringtones/Shes_All_That.ogg
# Silky Way					/system/media/audio/ringtones/SilkyWay.ogg
# Sitar Versus Sitar					/system/media/audio/ringtones/SitarVsSitar.ogg
# Solarium					/system/media/audio/ringtones/Solarium.ogg
# Springy Jalopy					/system/media/audio/ringtones/SpringyJalopy.ogg
# Steppin' Out					/system/media/audio/ringtones/Steppin_Out.ogg
# Terminated					/system/media/audio/ringtones/Terminated.ogg
# Terrible Twos					/system/media/audio/ringtones/Noises2.ogg
# Testudo					/system/media/audio/ringtones/Testudo.ogg
# Themos					/system/media/audio/ringtones/Themos.ogg
# Third Eye					/system/media/audio/ringtones/Third_Eye.ogg
# Thriller Three					/system/media/audio/ringtones/Noises3.ogg
# Thunderfoot					/system/media/audio/ringtones/Thunderfoot.ogg
# Twirl Away					/system/media/audio/ringtones/TwirlAway.ogg
# Ursa Minor					/system/media/audio/ringtones/URSAMINOR.ogg
# UrsaMinor					/system/media/audio/ringtones/UrsaMinor.ogg
# Very Alarmed					/system/media/audio/ringtones/VeryAlarmed.ogg
# Vespa					/system/media/audio/ringtones/Vespa.ogg
# World					/system/media/audio/ringtones/World.ogg
# Zeta					/system/media/audio/ringtones/Zeta.ogg
# bellcore-dr1					/system/media/audio/ringtones/bellcore-dr1.ogg
# bellcore-dr2					/system/media/audio/ringtones/bellcore-dr2.ogg
# bellcore-dr3					/system/media/audio/ringtones/bellcore-dr3.ogg
# bellcore-dr4					/system/media/audio/ringtones/bellcore-dr4.ogg
# bellcore-dr5					/system/media/audio/ringtones/bellcore-dr5.ogg
# speaker					/system/media/audio/ringtones/speaker.wav
#######################################################################
##  Account 14 Advanced Settings                                     ##
#######################################################################
# Check Domain Certificates. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P52311=0

# Validate Certificate Chain. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P52367=0

# Validate Incoming SIP Messages. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P52306=0

# Allow Unsolicited REFER. 0 - Disabled, 1 - Enabled, 2 - Enabled/Force Auth. Default value is 0.
# Number: 0, 1, 2
P53323=0

# Only Accept SIP Requests from Known Servers. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P52347=0

# Check SIP User ID for Incoming INVITE. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P51349=0

# Allow SIP Reset. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P53315=0

# Authenticate Incoming INVITE. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P52346=0

# SIP Realm Used for Challenge INVITE & NOTIFY.
# String
P53321=


# Enable Local MOH. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P52357=0

# Virtual Account Group. -1 - Default,  0 - Virtual Account Group 1, 1 - Virtual Account Group 2, 2 - Virtual Account Group 3
# 3 - Virtual Account Group 4, 4 - Virtual Account Group 5, 5 - Virtual Account Group 6, 6 - Virtual Account Group 7, 7 - Virtual Account Group 8
# 8 - Virtual Account Group 9, 9 - Virtual Account Group 10, 10 - Virtual Account Group 11, 11 - Virtual Account Group 12, 12 - Virtual Account Group 13
# 13 - Virtual Account Group 14, 14 - Virtual Account Group 15, 15 - Virtual Account Group 16. Default value is -1.
# Number: -1 - 15 
P52391=-1

# Special Feature. Default value is 100
# 100 - Standard, 102 - Broadsoft, 113 - China Mobile
# 114 - ZTE IMS, 115 - Mobotix, 116 - ZTE NGN, 117 - Huawei IMS, 123 - NEC, 125 - WorldStone
# Number: 100, 102, 113, 114, 115, 116, 117, 123, 125
P51324=100

# Allow Sync Phonebook via SIP Notify. 0 - No, 1 - Yes. Default is 1.
# Number: 0, 1
P53399=1
##############################################################################
##  Account 15 Settings                                                     ##
##############################################################################

#######################################################################
##  Account 15 General Settings                                      ##
#######################################################################

# Account Active. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P51401=0

# Account Name
P51417=

# SIP Server
P51402=

# SIP User ID
P51404=
 
# SIP Authentication ID
P51405=

# SIP Authentication Password
P51406=

# Voice Mail Access Number
P51426=

# Name (Display Name, e.g., John Doe)
P51407=

# Tel URI. 0 - Disable, 1 - User=Phone, 2 - Enabled. Default value is 0
# Number: 0, 1, 2
P51409=0

#######################################################################
##  Account 15 Network Settings                                      ##
#######################################################################

# Outbound Proxy
P51403=

# Secondary Outbound Proxy
P52433=

# DNS Mode. 0 - A Record, 1 - SRV, 2 - NAPTR/SRV. Default value is 0
# Number: 0, 1, 2
P51408=0

# DNS SRV Fail-over Mode. 0 - Default, 1 - Saved one until DNS TTL, 2 - Saved one until no response. Defualt value is 1
# Number
P53440=0

# Register Before DNS SRV Fail-over. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P54495=0

# NAT Traversal. 0 - NAT No, 1 - STUN, 2 - Keep-alive, 3 - UPnP, 4 - Auto, 5 - VPN. Default value is 2
# Number: 0, 1, 2, 3, 4, 5
P51414=2

# Proxy-Require
P51418=

#######################################################################
##  Account 15 SIP Settings                                          ##
#######################################################################

# SIP Registration. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P51410=1

# Unregister Before New Registration. 0 - No, 1 - All, 2 -  Instance . Default value is 2
# Number: 0, 1, 2
P51411=2

# Register Expiration (m). In minutes. Default value is 60
# Number: 0 - 64800
P51412=60

# Subscribe Expiration (m). Default is 60
# Number: 0 - 64800
P53451=60

# Re-register before Expiration (s). Default Value is 0
# Number : 0
P52430=0

# Registration Retry Wait Time (s). In seconds. Default value is 20
# Number: 1 - 3600
P51471=20

# Local SIP Port. Default value is 5088
# Number: 5 - 65535
P51413=5088

# SUBSCRIBE For MWI. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P51415=0

# Enable SIP OPTIONS Keep Alive. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P52497=0

# SIP OPTIONS Keep Alive Interval(s). Default value is 30
# Number 
P52498=30

# SIP OPTIONS Keep Alive Maximum Tries. Default value is 3
# Number 
P52499=3

# Enable Session Timer/ Session Expiration(s).  In seconds. Default value is 180 seconds.
# By default,  Session Timer is Enabled.  Session Timer is disabled if the value is 0.
# Number: 0 or 90 - 64800
P51434=180

# Min-SE(s). Default value is 90 seconds
# Number: 90 - 64800
P51427=90

# UAC Specify Refresher. 0 - Omit, 1 - UAC, 2 - UAS. Default value is 0
# Number: 0, 1, 2
P51432=0

# UAS Specify Refresher. 1 - UAC, 2 - UAS. Default value is 1
# Number: 1, 2
P51433=1

# Force INVITE. Always refresh with INVITE instead of UPDATE even when remote party supports UPDATE
# 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P51431=0

# Caller Request Timer. Request for timer when calling
# 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P51428=0

# Callee Request Timer
# Request for timer when being called (i.e., if remote party supports timer but did not request for one)
# 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P51429=0

# Force Timer. Still use timer when remote party does not support timer
# 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P51430=0

# Enable 100rel. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P51435=0

# Use Privacy Header
# 0 - Default, 1 - No, 2 - Yes. Default is 0
# Number: 0, 1, 2
P52438=0

# Use P-Preferred-Identity Header
# 0 - Default, 1 - No, 2 - Yes. Default is 0
# Number: 0, 1, 2
P52439=0

# Use P-Access-Network-Info Header. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P53458=1

# Use P-Emergency-Info Header. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P53459=1

# Use MAC Header.  0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P53461=0

# SIP Transport
# 0 - UDP , 1 - TCP, 2 - TLS. Default value is 0
# Number: 0, 1, 2
P51448=0

# SIP URI Scheme When Using TLS
# 0 -sip, 1 - sips. Default value is 0.
# Number: 0, 1
P52429=0

# Use Actual Ephemeral Port in Contact with TCP/TLS
# 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P52431=0

# Support SIP Instance ID
# 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P51489=1

# Add Auth Header On RE-REGISTER
# 0 - No, 1- Yes
P52459=1

# SIP T1 Timeout. RFC 3261 T1 value (RTT estimate)
# 50 - 0.5 sec, 100 - 1 sec, 200 - 2 sec. Default value is 50
# Number: 50, 100, 200
P51440=50

# SIP T2 Interval. RFC 3261 T2 value
# The maximum retransmit interval for non-INVITE requests and INVITE responses
# 200 - 2 sec, 400 - 4 sec, 800 - 8 sec. Default value is 400
# Number: 200, 400, 800.
P51441=400

# SIP Timer D Interval (Seconds)
# Number 0-64. Default value is 0
P52487=0

# Remove OBP from Route
# 0 - Disable, 1 - Enable, 2 - Always. Default value is 0
# Number: 0, 1, 2
P52405=0
#######################################################################
##  Account 15 Codec Settings                                        ##
#######################################################################
# Preferred Vocoder
# First codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 123 - Opus. Default value is 0
# Number: 0, 8, 9, 2, 18, 98, 123
P51451=0

# Second codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 123 - Opus. Default value is 8
# Number: 0, 8, 9, 2, 18, 98, 123
P51452=8

# Third codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 123 - Opus. Default value is 9
# Number: 0, 8, 9, 2, 18, 98, 123
P51453=9

# Forth codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 123 - Opus. Default value is 9
# Number: 0, 8, 9, 2, 18, 98, 123
P51454=9

# Fifth codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 123 - Opus. Default value is 9
# Number: 0, 8, 9, 2, 18, 98, 123
P51455=9

# Sixth codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 123 - Opus. Default value is 9
# Number: 0, 8, 9, 2, 18, 98, 123
P51456=9

# Seventh codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 123 - Opus. Default value is 9
# Number: 0, 8, 9, 2, 18, 98, 123
P51457=9

# Eigth codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 123 - Opus. Default value is 9
# Number: 0, 8, 9, 2, 18, 98, 123
P51458=9

# Codec Negotiation Priority. 0 - Caller, 1 - Callee. Default value is 1.
# Number: 0, 1
P54461=1

# Use First Matching Vocoder in 200OK SDP. 0 - No, 1 - Yes. The default value is 0.
# Number: 0, 1
P52448=0

# iLBC Frame Size. 0 - 20 ms, 1 - 30 ms. Default value is 1.
# Number: 0, 1
P51495=1

# G726-32 ITU Payload. 0 - 2, 1 - Dynamic. Default value is 0.
# Number: 0, 1
P52469=0

# G726-32 Dynamic PT. Default value is 126.
# Number
P52465=126

# Opus Payload Type
P52485=123

# DTMF: in audio. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P52401=0

# DTMF: via RFC2833. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P52402=1

# DTMF: via SIP INFO. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P52403=0

# DTMF Payload Type. Default value is 101
# Number: 96 - 126
P51496=101

# Enable Audio RED with FEC. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P53473=0

# Audio FEC Payload Type. Default value is 121
# Number: 96 - 126
P53474=121

# Audio RED Payload Type. Default value is 124
# Number: 96 - 126
P53475=124

# Silence Suppression. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P51485=0

# Voice Frames Per TX. Default value is 2
# Number: 1 - 64.
P51486=2

# Preferred Video Codec. 99 - H.264. Default is 99.
P51464=99

# Enable Video FEC. 0 - No, 1 - Yes. Default value is 1.
# Number: 0, 1
P52493=1

# Enable RFC5168 Support. 0 - No, 1 - Yes. Default value is 1.
# Number: 0, 1
P51478=1

# Video FEC Mode. 0 - 0, 1 - 1. Default value is 0.
# Number: 0, 1
P53422=0

# FEC Payload Type. Default value is 120.
P52494=120

# Packetization mode. 0 - Single NAL Unit Mode, 1 - Non-Interleaved Mode. Default value is 1.
# Number: 0, 1, 10
P53405=1

# H.264 Image Size. 9 - 720P, 1 - VGA, 5 - CIF, 4 - 4CIF, 0 - QVGA, 6 - QCIF. Default value is 9
# Number: 9, 1, 5, 4, 0, 6
P52407=9

# Use H.264 Constrained Profiles. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1
P53445=0

# H.264 Profile Type. 0 - Baseline Profile, 1 - Main Profile, 2 - High Profile, 3 - BP&MP&HP
# Number: 0, 1, 2, 3
P52462=0

# Video Bit Rate. 64 - 64 kbps, 96 - 96 kbps, 128 - 128 kbps, 160 - 160 kbps, 192 - 192 kbps
# 210 - 210 kbps, 256 - 256 kbps, 384 - 384 kbps, 512 - 512 kbps, 640 - 640 kbps, 768 - 768 kbps
# 1024 - 1024 kbps, 1280 - 1280 kbps, 1536 - 1536 kbps, 2048 - 2048 kbps. Default value is 2048.
# Number: 250, 500, 750
P52415=2048

# SDP Bandwidth Attribute. 0 - Standard, 1 - Media Level, 2 - Session Level, 3 - None. Default value is Media Level.
# Number: 0, 1, 2, 3
P52460=1

# H.264 Payload Type. Default value is 99.
P51462=99

# Disable BFCP. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1
P53401=0

# Presentation H.264 Image Size. 10 - 1080P, 9 - 720P. Default value is 10.
# Number: 10, 9
P52476=10

# Presentation H.264 Profile Type. 0 - Baseline Profile, 1 - Main Profile, 2 - High Profile, 3 - BP&MP&HP
# Number: 0, 1, 2, 3
P52477=3

# Presentation Video Bit Rate. 512 - 512 kbps, 640 - 640 kbps, 768 - 768 kbps
# 1024 - 1024 kbps, 1280 - 1280 kbps, 1536 - 1536 kbps, 2048 - 2048 kbps. Default value is 1024.
# Number: 250, 500, 750
P52478=1024

# Presentation Video Frame Rate. 5 - 5 frames/second, 10 - 10 frames/second, 15 - 15 frames/second. Default value is 15.
# Number: 5, 10, 15
P53442=

# BFCP Transport Protocol. 0 - Automatic, 1 - UDP, 2 - TCP. Default value is 1.
# Number: 0, 1, 2
P53441=

# SRTP Mode. 0 - Disable, 1 - Enable but not forced, 2 - Enable and forced. Default value is 0
# Number:0, 1, 2
P51443=0

# SRTP Key Length. 0 - AES 128&256 bit, 1 - AES 128 bit, 2 - AES 256 bit. Default value is 0
# Number:0, 1, 2
P52483=0 

# Enable SRTP Key Lifetime. 0 - No, 1 - Yes.
# Number: 0,1
P52463=0

# RTCP Destination
P52490=

# Symmetric RTP. 0 - No, 1 - Yes. Default value is 0
# Number:0, 1
P51460=0

# RTP IP Filter. 0 - Disable, 1 - IP Only, 2 - IP and Port. Default value is 0
# Number:0, 1, 2
P53426=0

# RTP Timeout(s). Default is 0. If set to 0, the device would not hangup.
# number: 0 - 600
P54468=0
#######################################################################
##  Account 15 Call Settings                                         ##
#######################################################################
# Enable Video Call. 0 - Default, 1 - No, 2 - Yes. Default is 0
# Number: 0, 1, 2
P61443=0

# Start Video Automatically. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P52414=1

# Remote Video Request. 0 - Prompt, 1 - Accept, 2 - Deny. Default value is 0
# Number: 0, 1, 2
P52426=0

# Video Layout. 0 - Default, 1 - Full screen, 3 - Equal split screen, 2 - Only display remote screen
P52432=0

# Auto Answer. 0 - No, 1 - Yes, 2 - Enable Intercom/Paging. Default value is 0
# Number: 0, 1, 2
P51425=0

# Play warning tone for Auto Answer Intercom. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P53472=1

# Intercom Barging. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P53419=1

# Auto Preview. 0 - No, 1 - Yes, 2 - Yes with Ringing. Default value is 0
# Number: 0, 1, 2
P54462=0

# Send Anonymous. 0 - No, 1 - Yes (caller ID will be blocked if set to Yes). Default value is 0
# Number: 0, 1
P51421=0

# Anonymous Call Rejection. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P51446=0

# Call Log
# 0 - Log All, 1 - Log Incoming/Outgoing only (Missed Calls Not Recorded), 2 - Disable Call All, 3 - Don't Prompt Missed Call. Default value is 0
# Number: 0, 1, 2
P51442=0

# Enable Call Features. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P51420=0

# Enable Call Waiting. 0 - Default, 1 - No, 2 - Yes.
# Number: 0, 1, 2
P53463=0

# Mute on Answer Intercom Call. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
P53471=0

# Transfer on 3 way conference Hangup. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P52404=0

# Use # as Dial Key. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P51492=1

# Use # as Redial Key. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P54469=1

# DND Call Feature On.
# String
P52444=

# DND Call Feature Off.
# String
P52445=

# No Key Entry Timeout (s). Default value is 4
# Number: 1 - 15
P51491=4

# Ring Timeout (s). Default value is 60
# Number: 10 - 300
P51476=60

# Refer-To Use Target Contact. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P51469=0

# RFC2543 Hold. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1 
P53462=1

# Dial Plan Prefix
# String
P51419=

# Disable DialPlan. 0 - No Selection, 1 - Dial Page, 2 - Contact, 4 - Incoming Call History, 8 -  Outgoing Call History, 16 - MPK & Click2Dial. 
# If need to check multiple selections, add the specific values for each selections together. Default value is 0
# Number: 0-31
P52482=0

# DialPlan. Default value is { x+ | \+x+ | *x+ | *xx*x+ | x+*x+*x+*x+ | x+*x+*x+*x+#x+ }
P51459={ x+ | \+x+ | *x+ | *xx*x+ | x+*x+*x+*x+ | x+*x+*x+*x+#x+ }

# Caller ID Display. 0 - Auto, 1 - Disabled, 2 - From Header. The default value is 0.
# Number: 0, 1, 2, 3
P52424=0

# Account Ringtone. See ring tone options and value in the Ring Tone Value Table below
P51423=content://settings/system/ringtone

# Ignore Alert-Info Header. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1
P53418=0

# Matching Incoming Caller ID. Matching Rule 1
# String
P53477=

# Matching Rule 1 Distinctive Ringtone. See ring tone options and value in the Ring Tone Value Table below
# String
P53478=content://settings/system/ringtone

# Matching Incoming Caller ID. Matching Rule 2
# String
P53479=

# Matching Rule 2 Distinctive Ringtone. See ring tone options and value in the Ring Tone Value Table below
# String
P53480=content://settings/system/ringtone

# Matching Incoming Caller ID. Matching Rule 3
# String
P53481=

# Matching Rule 3 Distinctive Ringtone. See ring tone options and value in the Ring Tone Value Table below
# String
P53482=content://settings/system/ringtone

############Ring Tone Value Table###############
# Web GUI Option                            Value
# Use System Ring tone                      content://settings/system/ringtone 
# Andromeda					/system/media/audio/ringtones/ANDROMEDA.ogg
# Aquila					/system/media/audio/ringtones/Aquila.ogg
# Argo Navis					/system/media/audio/ringtones/ArgoNavis.ogg
# Atria					/system/media/audio/ringtones/Atria.ogg
# Backroad					/system/media/audio/ringtones/Backroad.ogg
# Beat Plucker					/system/media/audio/ringtones/BeatPlucker.ogg
# Bell Phone					/system/media/audio/ringtones/Ring_Classic_02.ogg
# Bentley Dubs					/system/media/audio/ringtones/BentleyDubs.ogg
# Big Easy					/system/media/audio/ringtones/Big_Easy.ogg
# Bird Loop					/system/media/audio/ringtones/BirdLoop.ogg
# Bollywood					/system/media/audio/ringtones/Bollywood.ogg
# Boötes					/system/media/audio/ringtones/BOOTES.ogg
# Bus' a Move					/system/media/audio/ringtones/BussaMove.ogg
# Cairo					/system/media/audio/ringtones/Cairo.ogg
# Calypso Steel					/system/media/audio/ringtones/Calypso_Steel.ogg
# Canis Major					/system/media/audio/ringtones/CANISMAJOR.ogg
# Caribbean Ice					/system/media/audio/ringtones/CaribbeanIce.ogg
# Carina					/system/media/audio/ringtones/Carina.ogg
# Cassiopeia					/system/media/audio/ringtones/CASSIOPEIA.ogg
# Centaurus					/system/media/audio/ringtones/Centaurus.ogg
# Champagne Edition					/system/media/audio/ringtones/Champagne_Edition.ogg
# Chimey Phone					/system/media/audio/ringtones/Ring_Synth_02.ogg
# Club Cubano					/system/media/audio/ringtones/Club_Cubano.ogg
# Crayon Rock					/system/media/audio/ringtones/CrayonRock.ogg
# Crazy Dream					/system/media/audio/ringtones/CrazyDream.ogg
# Curve Ball Blend					/system/media/audio/ringtones/CurveBall.ogg
# Cygnus					/system/media/audio/ringtones/Cygnus.ogg
# Dancin' Fool					/system/media/audio/ringtones/DancinFool.ogg
# Digital Phone					/system/media/audio/ringtones/Ring_Digital_02.ogg
# Ding					/system/media/audio/ringtones/Ding.ogg
# DingDong					/system/media/audio/ringtones/DingDong.wav
# Don' Mess Wiv It					/system/media/audio/ringtones/DonMessWivIt.ogg
# Draco					/system/media/audio/ringtones/Draco.ogg
# Dream Theme					/system/media/audio/ringtones/DreamTheme.ogg
# Eastern Sky					/system/media/audio/ringtones/Eastern_Sky.ogg
# Enter the Nexus					/system/media/audio/ringtones/Enter_the_Nexus.ogg
# Eridani					/system/media/audio/ringtones/Eridani.ogg
# Ether Shake					/system/media/audio/ringtones/EtherShake.ogg
# Flutey Phone					/system/media/audio/ringtones/Ring_Synth_04.ogg
# Free Flight					/system/media/audio/ringtones/FreeFlight.ogg
# Friendly Ghost					/system/media/audio/ringtones/FriendlyGhost.ogg
# Funk Y'all					/system/media/audio/ringtones/Funk_Yall.ogg
# Game Over Guitar					/system/media/audio/ringtones/GameOverGuitar.ogg
# Gimme Mo' Town					/system/media/audio/ringtones/Gimme_Mo_Town.ogg
# Girtab					/system/media/audio/ringtones/Girtab.ogg
# Glacial Groove					/system/media/audio/ringtones/Glacial_Groove.ogg
# Growl					/system/media/audio/ringtones/Growl.ogg
# Halfway Home					/system/media/audio/ringtones/HalfwayHome.ogg
# Hydra					/system/media/audio/ringtones/Hydra.ogg
# Insert Coin					/system/media/audio/ringtones/InsertCoin.ogg
# Kuma					/system/media/audio/ringtones/Kuma.ogg
# Loopy Lounge					/system/media/audio/ringtones/LoopyLounge.ogg
# Love Flute					/system/media/audio/ringtones/LoveFlute.ogg
# Lyra					/system/media/audio/ringtones/Lyra.ogg
# Machina					/system/media/audio/ringtones/Machina.ogg
# Medieval Jaunt					/system/media/audio/ringtones/MidEvilJaunt.ogg
# Mildly Alarming					/system/media/audio/ringtones/MildlyAlarming.ogg
# Nairobi					/system/media/audio/ringtones/Nairobi.ogg
# Nassau					/system/media/audio/ringtones/Nassau.ogg
# New Player					/system/media/audio/ringtones/NewPlayer.ogg
# No Limits					/system/media/audio/ringtones/No_Limits.ogg
# Noisey One					/system/media/audio/ringtones/Noises1.ogg
# Organ Dub					/system/media/audio/ringtones/OrganDub.ogg
# Orion					/system/media/audio/ringtones/Orion.ogg
# Paradise Island					/system/media/audio/ringtones/Paradise_Island.ogg
# Pegasus					/system/media/audio/ringtones/Pegasus.ogg
# Perseus					/system/media/audio/ringtones/PERSEUS.ogg
# Playa					/system/media/audio/ringtones/Playa.ogg
# Pyxis					/system/media/audio/ringtones/Pyxis.ogg
# Rasalas					/system/media/audio/ringtones/Rasalas.ogg
# Revelation					/system/media/audio/ringtones/Revelation.ogg
# Rigel					/system/media/audio/ringtones/Rigel.ogg
# Road Trip					/system/media/audio/ringtones/Road_Trip.ogg
# Romancing The Tone					/system/media/audio/ringtones/RomancingTheTone.ogg
# Safari					/system/media/audio/ringtones/Safari.ogg
# Savannah					/system/media/audio/ringtones/Savannah.ogg
# Scarabaeus					/system/media/audio/ringtones/Scarabaeus.ogg
# Sceptrum					/system/media/audio/ringtones/Sceptrum.ogg
# Seville					/system/media/audio/ringtones/Seville.ogg
# She's All That					/system/media/audio/ringtones/Shes_All_That.ogg
# Silky Way					/system/media/audio/ringtones/SilkyWay.ogg
# Sitar Versus Sitar					/system/media/audio/ringtones/SitarVsSitar.ogg
# Solarium					/system/media/audio/ringtones/Solarium.ogg
# Springy Jalopy					/system/media/audio/ringtones/SpringyJalopy.ogg
# Steppin' Out					/system/media/audio/ringtones/Steppin_Out.ogg
# Terminated					/system/media/audio/ringtones/Terminated.ogg
# Terrible Twos					/system/media/audio/ringtones/Noises2.ogg
# Testudo					/system/media/audio/ringtones/Testudo.ogg
# Themos					/system/media/audio/ringtones/Themos.ogg
# Third Eye					/system/media/audio/ringtones/Third_Eye.ogg
# Thriller Three					/system/media/audio/ringtones/Noises3.ogg
# Thunderfoot					/system/media/audio/ringtones/Thunderfoot.ogg
# Twirl Away					/system/media/audio/ringtones/TwirlAway.ogg
# Ursa Minor					/system/media/audio/ringtones/URSAMINOR.ogg
# UrsaMinor					/system/media/audio/ringtones/UrsaMinor.ogg
# Very Alarmed					/system/media/audio/ringtones/VeryAlarmed.ogg
# Vespa					/system/media/audio/ringtones/Vespa.ogg
# World					/system/media/audio/ringtones/World.ogg
# Zeta					/system/media/audio/ringtones/Zeta.ogg
# bellcore-dr1					/system/media/audio/ringtones/bellcore-dr1.ogg
# bellcore-dr2					/system/media/audio/ringtones/bellcore-dr2.ogg
# bellcore-dr3					/system/media/audio/ringtones/bellcore-dr3.ogg
# bellcore-dr4					/system/media/audio/ringtones/bellcore-dr4.ogg
# bellcore-dr5					/system/media/audio/ringtones/bellcore-dr5.ogg
# speaker					/system/media/audio/ringtones/speaker.wav
#######################################################################
##  Account 15 Advanced Settings                                     ##
#######################################################################
# Check Domain Certificates. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P52411=0

# Validate Certificate Chain. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P52467=0

# Validate Incoming SIP Messages. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P52406=0

# Allow Unsolicited REFER. 0 - Disabled, 1 - Enabled, 2 - Enabled/Force Auth. Default value is 0.
# Number: 0, 1, 2
P53423=0

# Only Accept SIP Requests from Known Servers. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P52447=0

# Check SIP User ID for Incoming INVITE. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P51449=0

# Allow SIP Reset. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P53415=0

# Authenticate Incoming INVITE. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P52446=0

# SIP Realm Used for Challenge INVITE & NOTIFY.
# String
P53421=

# Enable Local MOH. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P52457=0

# Virtual Account Group. -1 - Default,  0 - Virtual Account Group 1, 1 - Virtual Account Group 2, 2 - Virtual Account Group 3
# 3 - Virtual Account Group 4, 4 - Virtual Account Group 5, 5 - Virtual Account Group 6, 6 - Virtual Account Group 7, 7 - Virtual Account Group 8
# 8 - Virtual Account Group 9, 9 - Virtual Account Group 10, 10 - Virtual Account Group 11, 11 - Virtual Account Group 12, 12 - Virtual Account Group 13
# 13 - Virtual Account Group 14, 14 - Virtual Account Group 15, 15 - Virtual Account Group 16. Default value is -1.
# Number: -1 - 15 
P52491=-1

# Special Feature. Default value is 100
# 100 - Standard, 102 - Broadsoft, 113 - China Mobile
# 114 - ZTE IMS, 115 - Mobotix, 116 - ZTE NGN, 117 - Huawei IMS, 123 - NEC, 125 - WorldStone
# Number: 100, 102, 113, 114, 115, 116, 117, 123, 125
P51424=100

# Allow Sync Phonebook via SIP Notify. 0 - No, 1 - Yes. Default is 1.
# Number: 0, 1
P53499=1
##############################################################################
##  Account 16 Settings                                                     ##
##############################################################################

#######################################################################
##  Account 16 General Settings                                      ##
#######################################################################

# Account Active. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P51501=0

# Account Name
P51517=

# SIP Server
P51502=

# SIP User ID
P51504=
 
# SIP Authentication ID
P51505=

# SIP Authentication Password
P51506=

# Voice Mail Access Number
P51526=

# Name (Display Name, e.g., John Doe)
P51507=

# Tel URI. 0 - Disable, 1 - User=Phone, 2 - Enabled. Default value is 0
# Number: 0, 1, 2
P51509=0

#######################################################################
##  Account 16 Network Settings                                      ##
#######################################################################

# Outbound Proxy
P51503=

# Secondary Outbound Proxy
P52533=

# DNS Mode. 0 - A Record, 1 - SRV, 2 - NAPTR/SRV. Default value is 0
# Number: 0, 1, 2
P51508=0

# DNS SRV Fail-over Mode. 0 - Default, 1 - Saved one until DNS TTL, 2 - Saved one until no response. Defualt value is 1
# Number
P53540=0

# Register Before DNS SRV Fail-over. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P54595=0

# NAT Traversal. 0 - NAT No, 1 - STUN, 2 - Keep-alive, 3 - UPnP, 4 - Auto, 5 - VPN. Default value is 2
# Number: 0, 1, 2, 3, 4, 5
P51514=2

# Proxy-Require
P51518=

#######################################################################
##  Account 16 SIP Settings                                          ##
#######################################################################

# SIP Registration. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P51510=1

# Unregister Before New Registration. 0 - No, 1 - All, 2 -  Instance . Default value is 2
# Number: 0, 1, 2
P51511=2

# Register Expiration (m). In minutes. Default value is 60
# Number: 0 - 64800
P51512=60

# Subscribe Expiration (m). Default is 60
# Number: 0 - 64800
P53551=60

# Re-register before Expiration (s). Default Value is 0
# Number : 0
P52530=0

# Registration Retry Wait Time (s). In seconds. Default value is 20
# Number: 1 - 3600
P51571=20

# Local SIP Port. Default value is 5090
# Number: 5 - 65535
P51513=5090

# SUBSCRIBE For MWI. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P51515=0

# Enable SIP OPTIONS Keep Alive. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P52597=0

# SIP OPTIONS Keep Alive Interval(s). Default value is 30
# Number 
P52598=30

# SIP OPTIONS Keep Alive Maximum Tries. Default value is 3
# Number 
P52599=3

# Enable Session Timer/ Session Expiration(s).  In seconds. Default value is 180 seconds.
# By default,  Session Timer is Enabled.  Session Timer is disabled if the value is 0.
# Number: 0 or 90 - 64800
P51534=180

# Min-SE(s). Default value is 90 seconds
# Number: 90 - 64800
P51527=90

# UAC Specify Refresher. 0 - Omit, 1 - UAC, 2 - UAS. Default value is 0
# Number: 0, 1, 2
P51532=0

# UAS Specify Refresher. 1 - UAC, 2 - UAS. Default value is 1
# Number: 1, 2
P51533=1

# Force INVITE. Always refresh with INVITE instead of UPDATE even when remote party supports UPDATE
# 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P51531=0

# Caller Request Timer. Request for timer when calling
# 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P51528=0

# Callee Request Timer
# Request for timer when being called (i.e., if remote party supports timer but did not request for one)
# 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P51529=0

# Force Timer. Still use timer when remote party does not support timer
# 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P51530=0

# Enable 100rel. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P51535=0

# Use Privacy Header
# 0 - Default, 1 - No, 2 - Yes. Default is 0
# Number: 0, 1, 2
P52538=0

# Use P-Preferred-Identity Header
# 0 - Default, 1 - No, 2 - Yes. Default is 0
# Number: 0, 1, 2
P52539=0

# Use P-Access-Network-Info Header. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P53558=1

# Use P-Emergency-Info Header. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P53559=1

# Use MAC Header.  0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P53561=0

# SIP Transport
# 0 - UDP , 1 - TCP, 2 - TLS. Default value is 0
# Number: 0, 1, 2
P51548=0

# SIP URI Scheme When Using TLS
# 0 -sip, 1 - sips. Default value is 0.
# Number: 0, 1
P52529=0

# Use Actual Ephemeral Port in Contact with TCP/TLS
# 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P52531=0

# Support SIP Instance ID
# 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P51589=1

# Add Auth Header On RE-REGISTER
# 0 - No, 1- Yes
P52559=1

# SIP T1 Timeout. RFC 3261 T1 value (RTT estimate)
# 50 - 0.5 sec, 100 - 1 sec, 200 - 2 sec. Default value is 50
# Number: 50, 100, 200
P51540=50

# SIP T2 Interval. RFC 3261 T2 value
# The maximum retransmit interval for non-INVITE requests and INVITE responses
# 200 - 2 sec, 400 - 4 sec, 800 - 8 sec. Default value is 400
# Number: 200, 400, 800.
P51541=400

# SIP Timer D Interval (Seconds)
# Number 0-64. Default value is 0
P52587=0

# Remove OBP from Route
# 0 - Disable, 1 - Enable, 2 - Always. Default value is 0
# Number: 0, 1, 2
P52505=0
#######################################################################
##  Account 16 Codec Settings                                        ##
#######################################################################
# Preferred Vocoder
# First codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 123 - Opus. Default value is 0
# Number: 0, 8, 9, 2, 18, 98, 123
P51551=0

# Second codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 123 - Opus. Default value is 8
# Number: 0, 8, 9, 2, 18, 98, 123
P51552=8

# Third codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 123 - Opus. Default value is 9
# Number: 0, 8, 9, 2, 18, 98, 123
P51553=9

# Forth codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 123 - Opus. Default value is 9
# Number: 0, 8, 9, 2, 18, 98, 123
P51554=9

# Fifth codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 123 - Opus. Default value is 9
# Number: 0, 8, 9, 2, 18, 98, 123
P51555=9

# Sixth codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 123 - Opus. Default value is 9
# Number: 0, 8, 9, 2, 18, 98, 123
P51556=9

# Seventh codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 123 - Opus. Default value is 9
# Number: 0, 8, 9, 2, 18, 98, 123
P51557=9

# Eigth codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 123 - Opus. Default value is 9
# Number: 0, 8, 9, 2, 18, 98, 123
P51558=9

# Codec Negotiation Priority. 0 - Caller, 1 - Callee. Default value is 1.
# Number: 0, 1
P54561=1

# Use First Matching Vocoder in 200OK SDP. 0 - No, 1 - Yes. The default value is 0.
# Number: 0, 1
P52548=0

# iLBC Frame Size. 0 - 20 ms, 1 - 30 ms. Default value is 1.
# Number: 0, 1
P51595=1

# G726-32 ITU Payload. 0 - 2, 1 - Dynamic. Default value is 0.
# Number: 0, 1
P52569=0

# G726-32 Dynamic PT. Default value is 126.
# Number
P52565=126

# Opus Payload Type
P52585=123

# DTMF: in audio. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P52501=0

# DTMF: via RFC2833. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P52502=1

# DTMF: via SIP INFO. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P52503=0

# DTMF Payload Type. Default value is 101
# Number: 96 - 126
P51596=101

# Enable Audio RED with FEC. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P53573=0

# Audio FEC Payload Type. Default value is 121
# Number: 96 - 126
P53574=121

# Audio RED Payload Type. Default value is 124
# Number: 96 - 126
P53575=124

# Silence Suppression. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P51585=0

# Voice Frames Per TX. Default value is 2
# Number: 1 - 64.
P51586=2

# Preferred Video Codec. 99 - H.264. Default is 99.
P51564=99

# Enable Video FEC. 0 - No, 1 - Yes. Default value is 1.
# Number: 0, 1
P52593=1

# Enable RFC5168 Support. 0 - No, 1 - Yes. Default value is 1.
# Number: 0, 1
P51578=1

# Video FEC Mode. 0 - 0, 1 - 1. Default value is 0.
# Number: 0, 1
P53522=0

# FEC Payload Type. Default value is 120.
P52594=120

# Packetization mode. 0 - Single NAL Unit Mode, 1 - Non-Interleaved Mode. Default value is 1.
# Number: 0, 1, 10
P53505=1

# H.264 Image Size. 9 - 720P, 1 - VGA, 5 - CIF, 4 - 4CIF, 0 - QVGA, 6 - QCIF. Default value is 9
# Number: 9, 1, 5, 4, 0, 6
P52507=9

# Use H.264 Constrained Profiles. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1
P53545=0

# H.264 Profile Type. 0 - Baseline Profile, 1 - Main Profile, 2 - High Profile, 3 - BP&MP&HP
# Number: 0, 1, 2, 3
P52562=0

# Video Bit Rate. 64 - 64 kbps, 96 - 96 kbps, 128 - 128 kbps, 160 - 160 kbps, 192 - 192 kbps
# 210 - 210 kbps, 256 - 256 kbps, 384 - 384 kbps, 512 - 512 kbps, 640 - 640 kbps, 768 - 768 kbps
# 1024 - 1024 kbps, 1280 - 1280 kbps, 1536 - 1536 kbps, 2048 - 2048 kbps. Default value is 2048.
# Number: 250, 500, 750
P52515=2048

# SDP Bandwidth Attribute. 0 - Standard, 1 - Media Level, 2 - Session Level, 3 - None. Default value is Media Level.
# Number: 0, 1, 2, 3
P52560=1

# H.264 Payload Type. Default value is 99.
P51562=99

# Disable BFCP. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1
P53501=0

# Presentation H.264 Image Size. 10 - 1080P, 9 - 720P. Default value is 10.
# Number: 10, 9
P52576=10

# Presentation H.264 Profile Type. 0 - Baseline Profile, 1 - Main Profile, 2 - High Profile, 3 - BP&MP&HP
# Number: 0, 1, 2, 3
P52577=3

# Presentation Video Bit Rate. 512 - 512 kbps, 640 - 640 kbps, 768 - 768 kbps
# 1024 - 1024 kbps, 1280 - 1280 kbps, 1536 - 1536 kbps, 2048 - 2048 kbps. Default value is 1024.
# Number: 250, 500, 750
P52578=1024

# Presentation Video Frame Rate. 5 - 5 frames/second, 10 - 10 frames/second, 15 - 15 frames/second. Default value is 15.
# Number: 5, 10, 15
P53542=

# BFCP Transport Protocol. 0 - Automatic, 1 - UDP, 2 - TCP. Default value is 1.
# Number: 0, 1, 2
P53541=

# SRTP Mode. 0 - Disable, 1 - Enable but not forced, 2 - Enable and forced. Default value is 0
# Number:0, 1, 2
P51543=0

# SRTP Key Length. 0 - AES 128&256 bit, 1 - AES 128 bit, 2 - AES 256 bit. Default value is 0
# Number:0, 1, 2
P52583=0 

# Enable SRTP Key Lifetime. 0 - No, 1 - Yes.
# Number: 0,1
P52563=0

# RTCP Destination
P52590=

# Symmetric RTP. 0 - No, 1 - Yes. Default value is 0
# Number:0, 1
P51560=0

# RTP IP Filter. 0 - Disable, 1 - IP Only, 2 - IP and Port. Default value is 0
# Number:0, 1, 2
P53526=0

# RTP Timeout(s). Default is 0. If set to 0, the device would not hangup.
# number: 0 - 600
P54568=0
#######################################################################
##  Account 16 Call Settings                                         ##
#######################################################################
# Enable Video Call. 0 - Default, 1 - No, 2 - Yes. Default is 0
# Number: 0, 1, 2
P61543=0

# Start Video Automatically. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P52514=1

# Remote Video Request. 0 - Prompt, 1 - Accept, 2 - Deny. Default value is 0
# Number: 0, 1, 2
P52526=0

# Video Layout. 0 - Default, 1 - Full screen, 3 - Equal split screen, 2 - Only display remote screen
P52532=0

# Auto Answer. 0 - No, 1 - Yes, 2 - Enable Intercom/Paging. Default value is 0
# Number: 0, 1, 2
P51525=0

# Play warning tone for Auto Answer Intercom. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P53572=1

# Intercom Barging. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P53519=1

# Auto Preview. 0 - No, 1 - Yes, 2 - Yes with Ringing. Default value is 0
# Number: 0, 1, 2
P54562=0

# Send Anonymous. 0 - No, 1 - Yes (caller ID will be blocked if set to Yes). Default value is 0
# Number: 0, 1
P51521=0

# Anonymous Call Rejection. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P51546=0

# Call Log
# 0 - Log All, 1 - Log Incoming/Outgoing only (Missed Calls Not Recorded), 2 - Disable Call All, 3 - Don't Prompt Missed Call. Default value is 0
# Number: 0, 1, 2
P51542=0

# Enable Call Features. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P51520=0

# Enable Call Waiting. 0 - Default, 1 - No, 2 - Yes.
# Number: 0, 1, 2
P53563=0

# Mute on Answer Intercom Call. 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
P53571=0

# Transfer on 3 way conference Hangup. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P52504=0

# Use # as Dial Key. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P51592=1

# Use # as Redial Key. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P54569=1

# DND Call Feature On.
# String
P52544=

# DND Call Feature Off.
# String
P52545=

# No Key Entry Timeout (s). Default value is 4
# Number: 1 - 15
P51591=4

# Ring Timeout (s). Default value is 60
# Number: 10 - 300
P51576=60

# Refer-To Use Target Contact. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P51569=0

# RFC2543 Hold. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1 
P53562=1

# Dial Plan Prefix
# String
P51519=

# Disable DialPlan. 0 - No Selection, 1 - Dial Page, 2 - Contact, 4 - Incoming Call History, 8 -  Outgoing Call History, 16 - MPK & Click2Dial. 
# If need to check multiple selections, add the specific values for each selections together. Default value is 0
# Number: 0-31
P52582=0

# DialPlan. Default value is { x+ | \+x+ | *x+ | *xx*x+ | x+*x+*x+*x+ | x+*x+*x+*x+#x+ }
P51559={ x+ | \+x+ | *x+ | *xx*x+ | x+*x+*x+*x+ | x+*x+*x+*x+#x+ }

# Caller ID Display. 0 - Auto, 1 - Disabled, 2 - From Header. The default value is 0.
# Number: 0, 1, 2, 3
P52524=0

# Account Ringtone. See ring tone options and value in the Ring Tone Value Table below
P51523=content://settings/system/ringtone

# Ignore Alert-Info Header. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1
P53518=0

# Matching Incoming Caller ID. Matching Rule 1
# String
P53577=

# Matching Rule 1 Distinctive Ringtone. See ring tone options and value in the Ring Tone Value Table below
# String
P53578=content://settings/system/ringtone

# Matching Incoming Caller ID. Matching Rule 2
# String
P53579=

# Matching Rule 2 Distinctive Ringtone. See ring tone options and value in the Ring Tone Value Table below
# String
P53580=content://settings/system/ringtone

# Matching Incoming Caller ID. Matching Rule 3
# String
P53581=

# Matching Rule 3 Distinctive Ringtone. See ring tone options and value in the Ring Tone Value Table below
# String
P53582=content://settings/system/ringtone

############Ring Tone Value Table###############
# Web GUI Option                            Value
# Use System Ring tone                      content://settings/system/ringtone 
# Andromeda					/system/media/audio/ringtones/ANDROMEDA.ogg
# Aquila					/system/media/audio/ringtones/Aquila.ogg
# Argo Navis					/system/media/audio/ringtones/ArgoNavis.ogg
# Atria					/system/media/audio/ringtones/Atria.ogg
# Backroad					/system/media/audio/ringtones/Backroad.ogg
# Beat Plucker					/system/media/audio/ringtones/BeatPlucker.ogg
# Bell Phone					/system/media/audio/ringtones/Ring_Classic_02.ogg
# Bentley Dubs					/system/media/audio/ringtones/BentleyDubs.ogg
# Big Easy					/system/media/audio/ringtones/Big_Easy.ogg
# Bird Loop					/system/media/audio/ringtones/BirdLoop.ogg
# Bollywood					/system/media/audio/ringtones/Bollywood.ogg
# Boötes					/system/media/audio/ringtones/BOOTES.ogg
# Bus' a Move					/system/media/audio/ringtones/BussaMove.ogg
# Cairo					/system/media/audio/ringtones/Cairo.ogg
# Calypso Steel					/system/media/audio/ringtones/Calypso_Steel.ogg
# Canis Major					/system/media/audio/ringtones/CANISMAJOR.ogg
# Caribbean Ice					/system/media/audio/ringtones/CaribbeanIce.ogg
# Carina					/system/media/audio/ringtones/Carina.ogg
# Cassiopeia					/system/media/audio/ringtones/CASSIOPEIA.ogg
# Centaurus					/system/media/audio/ringtones/Centaurus.ogg
# Champagne Edition					/system/media/audio/ringtones/Champagne_Edition.ogg
# Chimey Phone					/system/media/audio/ringtones/Ring_Synth_02.ogg
# Club Cubano					/system/media/audio/ringtones/Club_Cubano.ogg
# Crayon Rock					/system/media/audio/ringtones/CrayonRock.ogg
# Crazy Dream					/system/media/audio/ringtones/CrazyDream.ogg
# Curve Ball Blend					/system/media/audio/ringtones/CurveBall.ogg
# Cygnus					/system/media/audio/ringtones/Cygnus.ogg
# Dancin' Fool					/system/media/audio/ringtones/DancinFool.ogg
# Digital Phone					/system/media/audio/ringtones/Ring_Digital_02.ogg
# Ding					/system/media/audio/ringtones/Ding.ogg
# DingDong					/system/media/audio/ringtones/DingDong.wav
# Don' Mess Wiv It					/system/media/audio/ringtones/DonMessWivIt.ogg
# Draco					/system/media/audio/ringtones/Draco.ogg
# Dream Theme					/system/media/audio/ringtones/DreamTheme.ogg
# Eastern Sky					/system/media/audio/ringtones/Eastern_Sky.ogg
# Enter the Nexus					/system/media/audio/ringtones/Enter_the_Nexus.ogg
# Eridani					/system/media/audio/ringtones/Eridani.ogg
# Ether Shake					/system/media/audio/ringtones/EtherShake.ogg
# Flutey Phone					/system/media/audio/ringtones/Ring_Synth_04.ogg
# Free Flight					/system/media/audio/ringtones/FreeFlight.ogg
# Friendly Ghost					/system/media/audio/ringtones/FriendlyGhost.ogg
# Funk Y'all					/system/media/audio/ringtones/Funk_Yall.ogg
# Game Over Guitar					/system/media/audio/ringtones/GameOverGuitar.ogg
# Gimme Mo' Town					/system/media/audio/ringtones/Gimme_Mo_Town.ogg
# Girtab					/system/media/audio/ringtones/Girtab.ogg
# Glacial Groove					/system/media/audio/ringtones/Glacial_Groove.ogg
# Growl					/system/media/audio/ringtones/Growl.ogg
# Halfway Home					/system/media/audio/ringtones/HalfwayHome.ogg
# Hydra					/system/media/audio/ringtones/Hydra.ogg
# Insert Coin					/system/media/audio/ringtones/InsertCoin.ogg
# Kuma					/system/media/audio/ringtones/Kuma.ogg
# Loopy Lounge					/system/media/audio/ringtones/LoopyLounge.ogg
# Love Flute					/system/media/audio/ringtones/LoveFlute.ogg
# Lyra					/system/media/audio/ringtones/Lyra.ogg
# Machina					/system/media/audio/ringtones/Machina.ogg
# Medieval Jaunt					/system/media/audio/ringtones/MidEvilJaunt.ogg
# Mildly Alarming					/system/media/audio/ringtones/MildlyAlarming.ogg
# Nairobi					/system/media/audio/ringtones/Nairobi.ogg
# Nassau					/system/media/audio/ringtones/Nassau.ogg
# New Player					/system/media/audio/ringtones/NewPlayer.ogg
# No Limits					/system/media/audio/ringtones/No_Limits.ogg
# Noisey One					/system/media/audio/ringtones/Noises1.ogg
# Organ Dub					/system/media/audio/ringtones/OrganDub.ogg
# Orion					/system/media/audio/ringtones/Orion.ogg
# Paradise Island					/system/media/audio/ringtones/Paradise_Island.ogg
# Pegasus					/system/media/audio/ringtones/Pegasus.ogg
# Perseus					/system/media/audio/ringtones/PERSEUS.ogg
# Playa					/system/media/audio/ringtones/Playa.ogg
# Pyxis					/system/media/audio/ringtones/Pyxis.ogg
# Rasalas					/system/media/audio/ringtones/Rasalas.ogg
# Revelation					/system/media/audio/ringtones/Revelation.ogg
# Rigel					/system/media/audio/ringtones/Rigel.ogg
# Road Trip					/system/media/audio/ringtones/Road_Trip.ogg
# Romancing The Tone					/system/media/audio/ringtones/RomancingTheTone.ogg
# Safari					/system/media/audio/ringtones/Safari.ogg
# Savannah					/system/media/audio/ringtones/Savannah.ogg
# Scarabaeus					/system/media/audio/ringtones/Scarabaeus.ogg
# Sceptrum					/system/media/audio/ringtones/Sceptrum.ogg
# Seville					/system/media/audio/ringtones/Seville.ogg
# She's All That					/system/media/audio/ringtones/Shes_All_That.ogg
# Silky Way					/system/media/audio/ringtones/SilkyWay.ogg
# Sitar Versus Sitar					/system/media/audio/ringtones/SitarVsSitar.ogg
# Solarium					/system/media/audio/ringtones/Solarium.ogg
# Springy Jalopy					/system/media/audio/ringtones/SpringyJalopy.ogg
# Steppin' Out					/system/media/audio/ringtones/Steppin_Out.ogg
# Terminated					/system/media/audio/ringtones/Terminated.ogg
# Terrible Twos					/system/media/audio/ringtones/Noises2.ogg
# Testudo					/system/media/audio/ringtones/Testudo.ogg
# Themos					/system/media/audio/ringtones/Themos.ogg
# Third Eye					/system/media/audio/ringtones/Third_Eye.ogg
# Thriller Three					/system/media/audio/ringtones/Noises3.ogg
# Thunderfoot					/system/media/audio/ringtones/Thunderfoot.ogg
# Twirl Away					/system/media/audio/ringtones/TwirlAway.ogg
# Ursa Minor					/system/media/audio/ringtones/URSAMINOR.ogg
# UrsaMinor					/system/media/audio/ringtones/UrsaMinor.ogg
# Very Alarmed					/system/media/audio/ringtones/VeryAlarmed.ogg
# Vespa					/system/media/audio/ringtones/Vespa.ogg
# World					/system/media/audio/ringtones/World.ogg
# Zeta					/system/media/audio/ringtones/Zeta.ogg
# bellcore-dr1					/system/media/audio/ringtones/bellcore-dr1.ogg
# bellcore-dr2					/system/media/audio/ringtones/bellcore-dr2.ogg
# bellcore-dr3					/system/media/audio/ringtones/bellcore-dr3.ogg
# bellcore-dr4					/system/media/audio/ringtones/bellcore-dr4.ogg
# bellcore-dr5					/system/media/audio/ringtones/bellcore-dr5.ogg
# speaker					/system/media/audio/ringtones/speaker.wav
#######################################################################
##  Account 16 Advanced Settings                                     ##
#######################################################################
# Check Domain Certificates. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P52511=0

# Validate Certificate Chain. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P52567=0

# Validate Incoming SIP Messages. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P52506=0

# Allow Unsolicited REFER. 0 - Disabled, 1 - Enabled, 2 - Enabled/Force Auth. Default value is 0.
# Number: 0, 1, 2
P53523=0

# Only Accept SIP Requests from Known Servers. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P52547=0

# Check SIP User ID for Incoming INVITE. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P51549=0

# Allow SIP Reset. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P53515=0

# Authenticate Incoming INVITE. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P52546=0

# SIP Realm Used for Challenge INVITE & NOTIFY.
# String
P53521=

# Enable Local MOH. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1 
P52557=0

# Virtual Account Group. -1 - Default,  0 - Virtual Account Group 1, 1 - Virtual Account Group 2, 2 - Virtual Account Group 3
# 3 - Virtual Account Group 4, 4 - Virtual Account Group 5, 5 - Virtual Account Group 6, 6 - Virtual Account Group 7, 7 - Virtual Account Group 8
# 8 - Virtual Account Group 9, 9 - Virtual Account Group 10, 10 - Virtual Account Group 11, 11 - Virtual Account Group 12, 12 - Virtual Account Group 13
# 13 - Virtual Account Group 14, 14 - Virtual Account Group 15, 15 - Virtual Account Group 16. Default value is -1.
# Number: -1 - 15 
P52591=-1

# Special Feature. Default value is 100
# 100 - Standard, 102 - Broadsoft, 113 - China Mobile
# 114 - ZTE IMS, 115 - Mobotix, 116 - ZTE NGN, 117 - Huawei IMS, 123 - NEC, 125 - WorldStone
# Number: 100, 102, 113, 114, 115, 116, 117, 123, 125
P51524=100

# Allow Sync Phonebook via SIP Notify. 0 - No, 1 - Yes. Default is 1.
# Number: 0, 1
P53599=1
##############################################################################
##  Phone Settings                                                          ##
##############################################################################
#######################################################################
##  Phone Settings -> General Settings                               ##
#######################################################################
# Local RTP Port. Default value is 50040
# Number: 1024 - 65535
P39=50040

# Use Random Port. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P78=0

# Enable in-call DTMF display.  0 - Yes, 1 - No. Default value is 0
# Number: 0, 1
P338=0

# Enable Enterprise Contacts Timeout Auto Search. 0 - No, 1 - Yes. Default is 1
P22128=1

# Keep-alive Interval (s). Default value is 20 seconds
# Number: 10 - 160
P84=20

# STUN Server
P76=stun.ipvideotalk.com

# TURN Server Username
P22042=

# TURN Server Password
P22043=

# Use NAT IP. This will enable our SIP client to use this IP in the SIP message.
# Example 64.3.153.50
P101=
#######################################################################
##  Phone Settings - Call Settings                                   ##
#######################################################################
# Enable Video Call Feature. 0 - Yes, 1 - No. Default value is 0
# Number: 0, 1
P22091=0

# Enable Direct IP Call Mode. 0 - Yes, 1 - No. Default value is 0
# Number: 0, 1
P277=0

# Enable Paging Call Mode. 0 - Yes, 1 - No. Default value is 0
# Number: 0, 1
P22278=0

# Enable Call Waiting. 0 - Yes, 1 - No. Default value is 0
# Number: 0, 1
P91=0

# Enable Call Waiting Tone. 0 - Yes, 1 - No. Default value is 0
# Number: 0, 1
P186=0

# Enable DND Reminder Ring. 0 - Yes, 1 - No. Default value is 0
# Number: 0, 1
P1486=0

# Enable Transfer. 0 - Yes, 1 - No. Default value is 0
# Number: 0, 1
P1341=0

# Hold Call Before Completing Transfer. 0 - No, 1 - Yes. Default is 1
# Number: 0, 1
P8466=1

# Default Transfer Mode. 0 - Blind Transfer, 1 - Attended Transfer, 2 - Attended Transfer Only. Default value is 0.
# Number: 0, 1
P1685=0

# Enable Transfer via non-Transfer Programmable Key. 
# 0 - No, 1 - Yes. Default is 0
# Number: 0, 1
P22162=0

# Special Function for Incoming Call. 0 - None, 1 - Preview, 2 - Call transfer. Default is 0.
# Number: 0, 1, 2
P29762=0

# Enable Conference. 0 - Yes, 1 - No. Default value is 0
# Number: 0, 1
P1311=0

# Auto Conference. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P1682=0

# Hold Call before Adding confere. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P22346=0

# Auto Mute on Entry. 0 - Disable, 1 - Auto Mute on Incoming Call, 2 - Auto Mute on Outgoing Call
# 3 - Auto Mute on Incoming & Outgoing Call. Default value is 0.
# Number: 0, 1, 2, 3
P29607=

# Always Ring Speaker. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P1439=0

# Offhook Auto Dial
P71=

#Offhook Auto Dial Delay (s)
P8388=

# Offhook/Onhook Timeout (in seconds)
P1485=30

# Handset Option. 0 - Auto, 1 - Enable, 2 - Disable. Default is 0
# Number: 0, 1, 2
P22290=0

# Auto Unhold When Press the Line Key. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1
P29067=0

# Virtual Account Group Avaya Mode. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P22018=0

# Number of Accounts The Virtual Account Group Register
# Number, default is 2
P22133=2

# Filter Characters
# String
P22012=[()- ]

# Escape '#' as %23 in SIP URI. 0 - No, 1 - Yes
# Number: 0, 1
P1406=1

# Default Phone APP
P22289=com.base.module.phone/.service.PhoneService

# Quickly Launch Specified APP.
# String. Requires the installed app launcher.
# Example: com.microsoft.teams/com.microsoft.skype.teams.Launcher, com.android.vending/com.android.vending.AssetBrowserActivity
# P22276=

# Record Mode. 0 - Locally, 1 - on PortaOne, 2 - on UCM. Default is 0.
# Number: 0,1,2
P6760=0

# Enable Auto Record When Call Established.  0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P22295=0


# Rejected Call Notification. 0 - No, 1 - Yes. Default is 0.
# Number: 0, 1
P8393=0

# Return Code When Refusing Incoming Call.
# 0 - Busy, 1 -TemporarilyUnavailable, 2 - NotFound, 3 - Decline
P8360=0

# Return Code When Enable DND
# 0 - Busy, 1 -TemporarilyUnavailable, 2 - NotFound, 3 - Decline
P8361=0

#Group Listen with Speaker. 0 - No, 1 - Yes. Default is 0.
P22163=0

#######################################################################
##  Phone Settings - Ring Tone                                       ##
#######################################################################
# Auto Config CPT by Region. 0 - No, 1 - Yes. Default value is 1
# Number : 0, 1
P22041=0

# Dial Tone
P4000=f1=350@-13,f2=440@-13,c=0/0;

# Second Dial Tone
P2909=

# Ring Back Tone
P4001=f1=440@-19,f2=480@-19,c=2000/4000;

# Busy Tone
P4002=f1=480@-24,f2=620@-24,c=500/500;

# Reorder Tone
P4003=f1=480@-24,f2=620@-24,c=250/250;

# Confirmation Tone
P4004=f1=350@-11,f2=440@-11,c=100/100-100/100-100/100;

# Call Waiting Tone
P4005=f1=440@-13,c=300/10000-300/10000-0/0;

# Call Waiting Tone Gain. 0 - Low, 1 - Medium, 2 - High. Default value is 0
P1555=0

# Default Ring Cadence
P4040=c=2000/4000;

#######################################################################
##  Phone Settings - Video Settings                                  ##
#######################################################################
# Video Frame Rate. 5 - 5 frames/second,  15 - 15 frames/second, 25 - 25 frames/second, 30 - 30 frames/second, 29 - Variable frames rate. Default value is 15
# Number: 5, 15, 25, 29, 30
P904=15

# Video Display Mode. 0 - Original proportion, 1 - Cut proportionally cutting, 2 - Add black margin proportionally. Default value is 1
# Number: 0, 1, 2
P921=1

# Enable Frame Skipping in Video Decoder. 0 - No, 1 - Yes, default is 1.
# Number: 0, 1
P22008=1
#######################################################################
##  Phone Settings - Multicast Paging                    	         ##
#######################################################################
# Paging Barge. 0 - Disable, 1 - 1, 2 - 2, 3 - 3, 4 - 4, 5 - 5, 6 - 6, 7 - 7, 8 - 8, 9 - 9, 10 - 10. Default Value is 0
# Number : 0 - 10
P1566=0

# Paging Priority Active. 0 - No, 1 - Yes. Default Value is 0
# Number : 0, 1
P1567=0

# Multicast Paging Codec. 0 - PCMU, 8 - PCMA, 9 - G.722, 2 - G.726-32, 18 - G729A/B, 98 - iLBC, 123 - Opus. Default value is 0
# Number : 0, 2, 8, 9, 18, 98, 123
P1568=0 

# Enable Multicast Paging Video. 0 - No, 1 - Yes 
# Number : 0, 1
P22031=0

# Multicast Paging Video Codec. 99 - H.264. Default value is 99
# Number : 99
P22024=99

# Multicast Paging Image Size. 0 - QVGA, 1 - VGA, 4 - 4CIF, 5 - CIF, 6 - QCIF, 9 - 720P. Default Value is 1
# Number : 0, 1, 4 ,5, 6, 9 
P22025=1

# Multicast Paging Video Bit Rate. 32 - 32kbps, 64 - 64kbps, 96 - 96kbps, 128 - 128kbps, 160 - 160kbps
# 192 - 192kbps, 210 - 210kbps, 256 - 256kbps, 384 - 384kbps, 512 - 512kbps,  640 - 640kbps, 768 - 768kbps
# 1024 - 1024kbps, 1280 - 1280kbps, 1536 - 1536kbps, 2048 - 2048kbps. Default Value is 256
# Number : 32, 64, 96, 128, 160, 192, 210, 256, 384, 512, 640, 768, 1024, 1280, 1536, 2048
P22026=256

# Multicast Paging Video Frame Rate. 15 - 15 frames/second, 25 - 25 frames/second, 30 - 30 frames/second, 29 - Variable frames rate. Default Value is 15
#Number : 15, 25, 29, 30 
P22027=15

# Multicast Paging H.264 Profile Type. 1 - Baseline profile, 2 - Main profile, 3 - High profile. Default Value is  
# Number : 1, 2, 3
P22028=1

# Multicast Paging H.264 Payload Type. The default Value is 99
# Number
P22029=99

# Multicast Listening Address 1
# IP:Port number
P1569=

# Multicast Listening Label 1
P1570=

# Multicast Listening Address 2
# IP:Port number
P1571=

# Multicast Listening Label 2
P1572=

# Multicast Listening Address 3
# IP:Port number
P1573=

# Multicast Listening Label 3
P1574=

# Multicast Listening Address 4
# IP:Port number
P1575=

# Multicast Listening Label 4
P1576=

# Multicast Listening Address 5
# IP:Port number
P1577=

# Multicast Listening Label 5
P1578=

# Multicast Listening Address 6
# IP:Port number
P1579=

# Multicast Listening Label 6
P1580=

# Multicast Listening Address 7
# IP:Port number
P1581=

# Multicast Listening Label 7
P1582=

# Multicast Listening Address 8
# IP:Port number
P1583=

# Multicast Listening Label 8
P1584=

# Multicast Listening Address 9
# IP:Port number
P1585=

# Multicast Listening Label 9
P1586=

# Multicast Listening Address 10
# IP:Port number
P1587=

# Multicast Listening Label 10
P1588=
##############################################################################
##  Network Settings                                                        ##
##############################################################################
#######################################################################
##  Network Settings - Ethernet                                      ##
#######################################################################
# IP Mode. 0 - Prefer IPv4, 1 - Prefer IPv6, 2 - IPv4 Only, 3 - IPv6 Only. Default value is 2.
# Number: 0, 1, 2, 3
P1415=2

# Different Networks for Data and VoIP Calls. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1
P22104=0

# Network Configuration of Data

# IPv4 Address Type. 0 - DHCP, 1 - Static, 2 - PPPoE. Default value is 0
# Number: 0, 1, 2
P8=0

# DHCP VLAN Override. 0 - Disable, 1 - DHCP Option 132 and DHCP Option 133, 2 - Encapsulated in DHCP Option 43. Default value is 2.
# Number: 0, 1, 2
P8300=2

# Host name (DHCP option 12)
P146=

# Vendor Class ID (DHCP option 60)
P148=Grandstream GXV3370

# Layer 2 QoS. 802.1Q/VLAN Tag(Ethernet). Default value is 0
# Number: 0 - 4094
P51=0

# Layer 2 QoS. 802.1p priority value(Ethernet). Default value is 0
# Number: 0 - 7
P87=0

# IPv6
# IPv6 Address. 0 - Auto-configured, 1 - Statically configured. Default value is 0.
# Number: 0, 1
P1419=0

# Static IPv6 Address.
P1420=

# IPv6 Prefix Length. Default value is 64.
P1421=64

# IPv6 DNS Server 1.
P1424=

# IPv6 DNS Server 2.
P1425=

# IPv6 Preferred DNS Server.
P1423=

# Static IP. IP address
#P9=192
#P10=168
#P11=0
#P12=160

# Static IP. Subnet Mask
#P13=255
#P14=255
#P15=255
#P16=0

# Static IP. Default Gateway
#P17=192
#P18=168
#P19=0
#P20=1

# Static IP. DNS Server 1. Ignore if DHCP or PPPoE is used
#P21=0
#P22=0
#P23=0
#P24=0

# Static IP. DNS Server 2. Ignore if DHCP or PPPoE is used
#P25=0
#P26=0
#P27=0
#P28=0

# PPPoE Account ID
# P82=

# PPPoE Password
# P83=

# Network Configuration of VoIP Calls

# IPv4 Address Type. 0 - DHCP, 1 - Static IP. Default value is 0.
# Number: 0, 1
P22105=0

# IP Address.
P22106=

# Subnet Mask.
P22107=

# Default Gateway.
P22108=

# DNS Server 1.
P22109=

# DNS Server 2.
P22110=

# Layer 2 QoS. 802.1Q/VLAN Tag(Ethernet) for VOIP Calls. Default value is 0
# Number: 0 - 4095
P22111=0

# Layer 2 QoS. 802.1p priority value(Ethernet) for VOIP Calls. Default value is 0
# Number: 0 - 7
P22112=0

# 802.1x Mode. 0 - Disable, 1 - EAP-MD5, 2 - EAP-TLS, 3-EAP-PEAP
# Number: 0, 1, 2, 3
P7901=0

# 802.1x Identity
P7902=

# 802.1 Secret & Password
P7903=

# CA Certificate
P8439=

# Client Certificate
P8440=
#######################################################################
##  Network Settings - Wi-Fi Setting                                 ##
#######################################################################
# Wi-Fi Function. 0- Disable, 1- Enable
P7800=0

# WiFi Band. Combination: 2.4G: 0 - No, 1 - Yes. 5G: 0 - No, 1 - Yes.
P25420=1
P25421=1

# ESSID 
P7812=

# Security Mode for Hidden SSID. 0 - None, 1 - WEP, 2 - WPA WPA2 PSK. Default value is 0.
# Number: 0, 1, 2
P7814=0

# Password
P7830=

# Layer 2 QoS 802.1p Priority Value (Wi-Fi). The default value is 0.
P22048=

# Country Code. Default is US.
# String
P7831=US
#######################################################################
##  Network Settings - OpenVPN Settings                              ##
#######################################################################
# Enable OpenVPN. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1
P7050=0

# OpenVPN® Mode. 0 - simple mode, 1 - expert mode
P22292=0

# Enable OpenVPN® Comp-lzo
# Number: 0, 1
P8508=0

# OpenVPN Server Address.
# Strings
P7051=

# OpenVPN Port. The default value is 1194.
P7052=1194

# OpenVPN Transport. 0 - UDP, 1 - TCP. Default value is 0.
# Number: 0, 1
P2912=0

# OpenVPN CA.
# Strings
P9902=

# OpenVPN Client Certificate.
# Strings
P9903=

# OpenVPN Client Key.
# Strings
P9904=

# OpenVPN Cipher Method. 0 - Blowfish, 1 - AES - 128, 2 - AES - 256, 3 - Triple - DES. Default value is 0.
# Number: 0, 1, 2, 3
P8396=0

# OpenVPN Username.
P8394=

# OpenVPN Password.
P8395=
#######################################################################
##  Network Settings - Advanced Network Settings                     ##
#######################################################################
# DNS Refresh Time (m). Default 0.
# Number 0 - 1440
P4208=0

# DNS Failure Cache Duration (m).  Default 0.
# Number 0 - 1440
P28160=0

# Preferred DNS 1
#P92=0
#P93=0
#P94=0
#P95=0

# Preferred DNS 2
#P5026=
#P5027=
#P5028=
#P5029=

# Enable LLDP. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P1684=1

# LLDP TX Interval(s).
P22122=30

# Enable CDP. 0 - No, 1 - Yes. Default value is 1.
# Number: 0, 1
P22119=1

# Layer 3 QoS for SIP. Default value is 48
P1558=26

# Layer 3 QoS for Audio. Default value is 48
P1559=46

# Layer 3 QoS for Video. Default is 48.
P1560=34

# HTTP/HTTPS User-Agent
P1541=

# SIP User-Agent
P26027=Grandstream GXV3370 $version

# PC Port Mode. 0 - Enable, 1 - Disable, 2 - Mirrored.
# Number: 0, 1, 2
P1348=0

# PC Port VLAN Tag. Default is 0
# Number
P229=0

# PC Port Priority Value. Default is 0
# Number
P230=0

# HTTP/HTTPS Proxy Hostname
# String
P1552=

# HTTP/HTTPS Proxy Port
# String
P1553=

# Bypass Proxy For
# String
P22011=

# CSTA Control. 0 - No, 1 - Yes. Default value is 0
P32053=0

# Action URI Support. 0 - No, 1 - Yes. Default value is 1
P32050=1

# Remote Control Pop up Window Support. 0 - No, 1 - Yes. Default value is 1
P32051=1

# Action URI Allow IP List
# String
P32052=
#######################################################################
##  System Settings - Time and Language - Time Settings              ##
#######################################################################
# NTP Server
P30=us.pool.ntp.org

# Allow DHCP Option 42 to Override NTP Server. 0 - No, 1 - Yes. Default value is 1
# When set to Yes (1), it will override the configured NTP server
# Number: 0, 1
P144=1

# Allow DHCP Option 2 to Override Time Zone Setting. 0 - No, 1 - Yes. Default value is 1
# When set to Yes (1), it will override the configured Time Zone setting if available
# Number: 0, 1
P143=1

# Time Zone
# Time zone p-value support both Olson value and POSIX value. By default, the device uses Olson. User can also customize POSIX value.
# P-Value        			   		Web GUI Option	                 							

# Pacific/Midway					Midway,GMT-11:00,                           
# Pacific/Honolulu					Hawaii-Aleutian Standard Time,GMT-10:00,                         
# America/Anchorage					Alaska Daylight Time/Anchorage,GMT-08:00,                
# America/Los_Angeles				Pacific Daylight Time/Los Angeles,GMT-07:00,       
# America/Tijuana					Tijuana,GMT-07:00,                            
# America/Phoenix					Mountain Standard Time/Phoenix,GMT-07:00,         
# America/Chihuahua					Chihuahua,GMT-07:00,                        
# America/Denver					Mountain Daylight Time/Denver,GMT-06:00,           
# America/Costa_Rica				Costa Rica,GMT-06:00,
# America/Mexico_City				Mexico City,GMT-06:00,   
# America/Regina					Regina,GMT-06:00,                       
# America/Chicago					Central Daylight Time/Chicago,GMT-05:00,       
# America/Bogota					Bogota,GMT-05:00,                              
# America/New_York					New York,GMT-04:00,                          
# America/Caracas					Caracas,GMT-04:00,                            
# America/Barbados					Barbados,GMT-04:00,      
# America/Manaus					Manaus,GMT-04:00, 
# America/Halifax					Halifax,GMT-03:00,           
# America/Santiago					Santiago,GMT-03:00,                            
# America/Recife					Recife,GMT-03:00,                                
# America/Sao_Paulo					Sao Paulo,GMT-03:00,                          
# America/Buenos_Aires				Buenos Aires,GMT-03:00,                    
# America/Godthab					Nuuk,GMT-03:00,                                  
# America/Montevideo				Montevideo,GMT-03:00, 
# America/St_Johns					St. John’s,GMT-02:30,                           
# Atlantic/South_Georgia			South Georgia,GMT-02:00,                  
# Atlantic/Azores					Azores,GMT-01:00,                                 
# Atlantic/Cape_Verde				Cape Verde,GMT-01:00,                         
# Africa/Casablanca					Casablanca,GMT+00:00,                           
# Europe/London						London,GMT+00:00,                                   
# Europe/Amsterdam					Amsterdam,GMT+01:00,                            
# Europe/Belgrade					Belgrade,GMT+01:00,                              
# Europe/Brussels					Brussels,GMT+01:00,                              
# Europe/Madrid						Madrid,GMT+01:00,                                  
# Europe/Sarajevo					Sarajevo,GMT+01:00,                              
# Africa/Brazzaville				Brazzaville,GMT+01:00,                       
# Africa/Windhoek					West Africa Standard Time/Windhoek,GMT+02:00, 
# Asia/Amman						Amman,GMT+02:00,                                      
# Europe/Athens						Athens,GMT+02:00,                                  
# Asia/Beirut						Beirut,GMT+02:00,                                    
# Africa/Cairo						Cairo,GMT+02:00,                                   
# Europe/Helsinki					Helsinki,GMT+02:00,                            
# Asia/Jerusalem					Jerusalem,GMT+02:00,                            
# Africa/Harare						Harare,GMT+02:00,                                
# Europe/Istanbul					Istanbul,GMT+03:00,                         
# Europe/Minsk						Minsk,GMT+03:00,   
# Europe/Kiev                       Eastern European Summer Time
# Asia/Baghdad						Baghdad,GMT+03:00,                               
# Europe/Moscow						Moscow,GMT+03:00,                                
# Asia/Kuwait						Kuwait,GMT+03:00,                                 
# Africa/Nairobi					Nairobi,GMT+03:00,       
# Asia/Baku							Baku,GMT+04:00,                                     
# Asia/Tbilisi						Tbilisi,GMT+04:00,                               
# Asia/Yerevan						Yerevan,GMT+04:00,                               
# Asia/Dubai						Dubai,GMT+04:00, 
# Asia/Tehran						Tehran,GMT+04:30,                                   
# Asia/Kabul						Kabul,GMT+04:30,                                   
# Asia/Karachi						Karachi,GMT+05:00,                               
# Asia/Oral							Oral,GMT+05:00,                                     
# Asia/Yekaterinburg				Yekaterinburg,GMT+05:00,                   
# Asia/Calcutta						Kolkata,GMT+05:30,                              
# Asia/Colombo						Colombo,GMT+05:30,                               
# Asia/Katmandu						Kathmandu,GMT+05:45,                            
# Asia/Almaty						Almaty,GMT+06:00,                                 
# Asia/Rangoon						Rangoon,GMT+06:30,                               
# Asia/Krasnoyarsk					Krasnoyarsk,GMT+07:00,                       
# Asia/Bangkok						Bangkok,GMT+07:00,                               
# Asia/Jakarta						Jakarta,GMT+07:00,                               
# Asia/Shanghai						Shanghai,GMT+08:00,                             
# Asia/Hong_Kong					Hong Kong,GMT+08:00,                           
# Asia/Irkutsk						Irkutsk,GMT+08:00,                               
# Asia/Kuala_Lumpur					Kuala Lumpur,GMT+08:00,                     
# Australia/Perth					Perth,GMT+08:00,                              
# Asia/Taipei						Taipei,GMT+08:00,                                 
# Asia/Seoul						Seoul,GMT+09:00,                                   
# Asia/Tokyo						Tokyo,GMT+09:00,                                   
# Asia/Yakutsk						Yakutsk,GMT+09:00,                               
# Australia/Darwin					Darwin,GMT+09:30,                            
# Australia/Brisbane				Brisbane,GMT+10:00,                        
# Asia/Vladivostok					Vladivostok,GMT+10:00,                       
# Pacific/Guam						Guam,GMT+10:00,                                  
# Australia/Adelaide				Adelaide,GMT+10:30,                        
# Australia/Hobart					Hobart,GMT+11:00,                            
# Australia/Sydney					Sydney,GMT+11:00,                            
# Asia/Magadan						Magadan,GMT+11:00,                               
# Pacific/Noumea					Noumea,GMT+11:00,                              
# Pacific/Majuro					Majuro,GMT+12:00,                              
# Pacific/Fiji						Fiji,GMT+12:00,                                  
# Pacific/Auckland					Auckland,GMT+13:00,                          
# Pacific/Tongatapu					Tongatapu,GMT+13:00

# Time Zone
# P64=PST8PDT

# Time Display Format. 0 - 12 Hour, 1 - 24 Hour. Default value is 1
# Number: 0, 1
P122=1

# Date Display Format. Default value is 1
# 0: YYYY-MM-DD
# 1: MM-DD-YYYY
# 2: DD-MM-YYYY
# 3: Normal (YYYY-M-D)
# Number: 0, 1, 2, 3
P102=1
#######################################################################
##  System Settings - Time and Language - Language                   ##
#######################################################################
# Language. Configure the language to be displayed on LCD
# Note: for some languages that have 2 codes avaiable, both are working
# af_ZA - Afrikaans
# am_ET - አማርኛ
# ar_EG - العربية
# ca_ES - CatalC 
# cs_CZ - CeE!tina
# da_DK - Dansk
# de_AT - Deutsch (Österreich)
# de_CH - Deutsch (Schweiz)
# de_DE - Deutsch
# de_LI - Deutsch (Liechtenstein)
# en_AU - English (Australia)
# en_CA - English (Canada)
# en_GB - English (United Kingdom)
# en_NZ - English (New Zealand)
# en_SG - English (Singapore)
# en_US - English (United States), en - English (United States)
# es_ES - EspaC1ol (EspaC1a)
# es_US - EspaC1ol (Estados Unidos)
# fa_IR - فارسی
# fr_BE - FranC'ais (Belgique)
# fr_CA - FranC'ais (Canada)
# fr_CH - FranC'ais (Suisse)
# fr_FR - FranC'ais, fr - FranC'ais
# iw_IL - Hebrew
# hr_HR - Hrvatski
# in_ID - Indonesian
# it_CH - Italiano (Svizzera)
# it_IT - Italiano, or it - Italiano
# lv_LV - LatvieE!u
# lt_LT - Lietuviu
# ja_JP - 日本語
# hu_HU - Magyar, or hu - Magyar
# ko_KR - Korean
# ms_MY - Bahasa Melayu
# nl_BE - Nederlands (België)
# nl_NL - Nederlands, or nld - Nederlands
# nb_NO - Norsk bokmål
# pl_PL - Polski, or pl - Polski
# pt_BR - Português (Brasil)
# pt_PT - Português (Portugal)
# ro_RO - Româna
# rm_CH - Romansh
# sk_SK - Slovencina
# sl_SI - Slovenšcina
# fi_FI - Suomi, or fi
# sv_SE - Svenska, or sv - Svenska
# tl_PH - Filipino
# vi_VN - Tiếng Việt
# tr_TR - Türkçe, or tr - Türkçe
# el_GR - Greek
# bg_BG - Bulgarian
# ru_RU - Russian, or ru - Russian
# sr_RS - Serbian
# sw_TZ - Kiswahili
# th_TH - ไทย
# uk_UA - Ukrainian
# ko_KR - Korean, or kr - Korean
# zh_TW - 中文 (繁體), or zh-tw - 中文 (繁體)
# zh_CN - 中文 (简体), or zh - 中文 (简体)
# zu_ZA - IsiZulu

# P1362=en_US

#######################################################################
##  System Settings - Security Settings - Web/SSH Access             ##
#######################################################################
# Disable SSH. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P276=0

# SSH Port.
# Number
P27006=22

# Web Access Method. 0 - HTTP, 1 - HTTPS. Default value is 0
# Number: 0, 1
P900=0

# Web Port. HTTP default is 80, HTTPS default is 443
# Number: 0 - 65535
P901=80

# Configuration via Keypad Menu. 0 - Unrestricted, 1 - Basic Settings Only, 2 - Constraint Mode, 3 - Basic settings & Network settings. Default value is 0.
# Number: 0, 1, 2, 3
P1357=0

# Permission to Install/Uninstall Apps. 0 - Allow, 1 - Require admin password, 2 - Require admin password if the app source is unknown
# 3 - Not allow. Default value is 0.
# Number: 0, 1, 2, 3
P29604=0
#######################################################################
##  System Settings - Security Settings - User Info Management       ##
#######################################################################
# Admin password for web interface
P2=admin

# End User Password
P196=user
#######################################################################
##  System Settings - Security Settings - SIP TLS                    ##
#######################################################################
# Minimum TLS Version
# 10 - TLS1.0, 11 - TLS1.1, 12 - TLS1.2
P22293=11

# Maximum TLS Version
# 10 - TLS1.0, 11 - TLS1.1, 12 - TLS1.2, 99 - No Limit
P22294=99

# Enable Weak TLS Cipher Suites
# 0 - Enable, 1 - Disable_RC4/DES/3DES
P8536=0

# SIP TLS Certificate
# P280=

# SIP TLS Private Key
# P279=

# SIP TLS Private Key Password
P281=s1pphone
#######################################################################
##  System Settings - Preferences - LCD&LED Management               ##
#######################################################################
# Enable Missed Call Backlight. 1 - No, 0 - Yes. Default is 0
# Number: 0, 1
P351=0

# Enable Missed Call Indicator. 1 - No, 0 - Yes. Default is 0
# Number: 0, 1
P1691=0

# Enable MWI Indicator. 1 - No, 0 - Yes. Default is 0
# Number: 0, 1
P1692=0

# Enable New Message Indicator. 1 - No, 0 - Yes. Default is 0
# Number: 0, 1
P1693=0

# Enable Contact Full Indicator. 1 - No, 0 - Yes. Default is 0
# Number: 0, 1
P1694=0

# Enable Indicator When LCD is OFF. 1 - No, 0 - Yes. Default is 0
# Number: 0, 1
P1695=0

# Font size
# Number: 0 - small, 1 - default, 2 - large, 3 - largest
P22275=1

# Enable HDMI audio
# Number: 0, 1
P22279=1
#######################################################################
##  System Settings - Preferences - Audio Control                    ##
#######################################################################
# RJ9 Headset TX Gain (dB). 0 - 0, -6 - -6, 6 - +6, 12 - +12, -12 - -12, 18 - +18, -18 - -18, 24 - +24, -24 - -24. Default value is 0
# Number: 0, -6, 6, 12, -12, 18, -18, 24, - 24
P1301=0

# RJ9 Headset RX Gain (dB). 0 - 0, -6 - -6, 6 - +6, 9 - +9, -9 - -9. Default value is 0
# Number: 0, -6, 6, -9, 9
P1302=0

# 3.5mm Earphone TX Gain (dB). 0 - 0, -6 - -6, 6 - +6, 12 - +12, -12 - -12, 18 - +18, -18 - -18, 24 - +24, -24 - -24. Default value is 0
# Number: 0, -6, 6, 12, -12, 18, -18, 24, - 24
P22002=0

# 3.5mm Earphone RX Gain (dB). 0 - 0, -6 - -6, 6 - +6, 9 - +9, -9 - -9. Default value is 0
# Number: 0, -6, 6, -9, 9
P22003=0

# Headset Type. 0 - Normal Headset, 1 - Plantronics EHS. Default value is 0
# Number: 0, 1
P1487=0

# Enable 3.5mm Headset Control
# 0 - No, 1 - Yes, default is 0
# P22113=0

# Handset TX Gain (dB). 0 - 0, 1 - -6, 2 - +6. Default value is 0
# Number: 0, 1, 2
P1464=1

# Handset RX Gain (dB). 0 - 0, 1 - -6, 2 - +6. Default value is 0
# Number: 0, 1, 2
P2906=1

# Ringtone Volume
#Number: 0 to 15. Default value is 8
P8352=8

# Media volume
#Number: 0 to 15. Default value is 8
P43025=8

#Alarm volume
#Number: 0 to 15. Default value is 8
P22332=8

#######################################################################
##  System Settings - TR069                                          ##
#######################################################################
# Enable TR-069. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P1409=0

# ACS URL
P4503=

# ACS Username
P4504=

# ACS Password
P4505=

# Periodic Inform Enable. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P4506=0

# Periodic Inform Interval (s). Default value is 86400
# Number: 1 - 4294967295
P4507=86400

# Connection Request Username
P4511=

# Connection Request Password
P4512=

# Connection Request Port
P4518=

# CPE Cert File
P8220=

# CPE Cert Key
P8221=
#######################################################################
##  Maintenance - Upgrade - Firmware                                 ##
#######################################################################
# Firmware Upgrade Mode. 0 - TFTP, 1 - HTTP, 2 - HTTPS, 3 - Manual Upload. Default value is 1.
# Number: 0, 1, 2, 3
P6767=1

# Firmware Server Path
P192=fm.ipvideotalk.com/gs

# Firmware HTTP/HTTPS User Name
P6768=

# Firmware HTTP/HTTPS Password
P6769=

# Firmware File Prefix
P232=

# Firmware File Postfix
P233=
#######################################################################
##  Maintenance - Upgrade - Config File                              ##
#######################################################################
# Config Update Via. 0 - TFTP, 1 - HTTP, 2 - HTTPS. Default value is 2.
# Number: 0, 1, 2
P212=2

# Config Server Path
P237=fm.grandstream.com/gs

# Config HTTP/HTTPS Username
P1360=

# Config HTTP/HTTPS Password
P1361=

# Always send HTTP Basic Authentication Information. 0 - No, 1 - Yes.
# Number: 0, 1
P20713=0

# Config File Prefix
P234=

# Config File Postfix
P235=

# Authenticate Conf File. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P240=0

# XML Config File Password
P1359=

# CUST File
# GUI Customization File Download Mode. 0 - TFTP, 1 - HTTP, 2 - HTTPS. Default value is 1.
# Number: 0, 1, 2
P6775=0

# GUI Customization File URL.
P6774=fm.grandstream.com/gs

# GUI Customization File HTTP/HTTPS Username.
P6776=

# GUI Customization File HTTP/HTTPS Password.
P6777=

# Use Configurations of Config File Server. 0 - No, 1 - Yes. Default value is 0.
# Number: 0, 1
P6778=0
#######################################################################
##  Maintenance - Upgrade - Provision                                ##
#######################################################################
# Automatic Upgrade. 0 - No, 1 - Check Every Day, 2 - Check Every Week, 3 - Check Every Interval. Default value is 0
# Number: 0, 1, 2, 3
P194=0

# Automatic Upgrade Check Interval (m). Minimum 60 minutes. Default value is 10080 (7 days)
# Number: 60 - 5256000
P193=10080

# Enable Randomized Automatic Upgrade. 0 - No, 1 - Yes. Default value is 0
P8458=0

# Starting/Ending Hour of the Day(0-23)
# Number: 0 - 23
P285=1
P8459=

# Day of the Week (0-6)
# Number: 0 - 6
P286=1

# Firmware Upgrade and Provisioning. Default value is 0
# 0 - Always Check at Bootup
# 1 - When F/W pre/suffix changes
# 2 - Skip the Firmware Check
# Number: 0, 1, 2
P238=0

# Upgrade Without Prompt. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P1549=0

# Allow DHCP Option 43 and Option 66 to Override server. 0 - No, 1 - Yes. Default value is 1
# When set to Yes(1), it will override the configured provision path and method
# Number: 0, 1
P145=1

# DHCP Option 120 Override SIP Server.  0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P1411=1

# Allow DHCP Option 242 (Avaya IP Phones). 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P22053=1

# Download and Process All Available Config Files. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P8467=0

# Config Provision
# cfg.xml;cfg$mac;cfg$mac.xml;cfg$product.xml#
# cfg.xml;cfg$mac;cfg$product.xml;cfg$mac.xml#
# cfg.xml;cfg$mac.xml;cfg.xml;cfg$product.xml#
# cfg.xml;cfg$mac.xml;cfg$product.xml;cfg.xml#
# cfg.xml;cfg$product.xml;cfg.xml;cfg$mac.xml#
# cfg.xml;cfg$product.xml;cfg$mac.xml;cfg.xml#
# cfg$mac;cfg.xml;cfg$mac.xml;cfg$product.xml#
# cfg$mac;cfg.xml;cfg$product.xml;cfg$mac.xml#
# cfg$mac;cfg$mac.xml;cfg.xml;cfg$product.xml#
# cfg$mac;cfg$mac.xml;cfg$product.xml;cfg.xml#
# cfg$mac;cfg$product.xml;cfg$mac.xml;cfg.xml#
# cfg$mac;cfg$product.xml;cfg.xml;cfg$mac.xml#
# cfg$mac.xml;cfg.xml;cfg$mac;cfg$product.xml#
# cfg$mac.xml;cfg.xml;cfg$product.xml;cfg$mac#
# cfg$mac.xml;cfg$mac;cfg.xml;cfg$product.xml#
# cfg$mac.xml;cfg$mac;cfg$product.xml;cfg.xml#
# cfg$mac.xml;cfg$product.xml;cfg$mac;cfg.xml#
# cfg$mac.xml;cfg$product.xml;cfg.xml;cfg$mac#
# cfg$product.xml;cfg.xml;cfg$mac;cfg$mac.xml#
# cfg$product.xml;cfg.xml;cfg$mac.xml;cfg$mac#
# cfg$product.xml;cfg$mac;cfg.xml;cfg$mac.xml#
# cfg$product.xml;cfg$mac;cfg$mac.xml;cfg.xml#
# cfg$product.xml;cfg$mac.xml;cfg$mac;cfg.xml#
# cfg$product.xml;cfg$mac.xml;cfg.xml;cfg$mac#
P8501=cfg$mac;cfg$mac.xml;cfg$product.xml;cfg.xml

# Enable PNP Feature
#0 - No, 1 - Yes. Default value is 0
P22032=0

# PNP URL
P22033=

# PnP (3CX) Auto Provision. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P1414=1
#######################################################################
##  Maintenance - Upgrade - Advanced Settings                        ##
#######################################################################
# Disable SIP NOTIFY Authentication. 0 - Yes, 1 - No. Default Value is 0
# Number : 0, 1
P4428=0

# Validate Certification Chain
# 0 - No, 1 - Yes. Default value is 0
P22030=0

# Enable EEE Mode
# 0 - No, 1 - Yes. Default value is 0
P8499=0

# mDNS Override Server. 0 - Disable, 1 - Use Type A, 2 - Use Type SRV. Default value is 1.
# Number: 0, 1
P1407=1
#######################################################################
##  Maintenance - System Diagnosis - Syslog                          ##
#######################################################################
# Syslog Protocol
# 0 - UDP, 1 - SSL/TLS. Default Value is 0
P8402=0

# Syslog Server. Name of the server
P207=log.ipvideotalk.com

# Syslog Level
# 0 - NONE, 1 - DEBUG, 2 - INFO, 3 - WARNING, 4 - ERROR. Default value is 0
# Number: 0, 1, 2, 3, 4
P208=0

# Send SIP Log
# 0 - No, 1 - Yes. Default value is 1
P1387=1

# Syslog Keyword Filter
# String
P22129=

# Enable Core Dump Generation. 0 - No, 1 - Yes. Default is 0.
# Number: 0, 1
P29611=0
#######################################################################
##  Applications - MPK Settings			                  			 ##
#######################################################################
# Show Display Name from Server. 0 - No, 1 - Yes. Default is 0.
P22130=0

# Display Format. 0 - Name, 1 - User ID, 2 - Name(User ID), 3 - Name,User ID, Key mode
P22127=0
#######################################################################
##  Applications - MPK General Settings                              ##
#######################################################################
# Account 1 BLF Call-Pickup Prefix. Default value is **
# String
P1347=**

# Account 1 Force BLF Call-pickup by Prefix. 0 - No, 1 - Yes. Default Value is 0
# Number : 0, 1
P6752=0

# Account 1 BLF URI
P134=

# Account 2 BLF Call-Pickup Prefix. Default value is **
# String
P481=**

# Account 2 Force BLF Call-pickup by Prefix. 0 - No, 1 - Yes. Default Value is 0
# Number : 0, 1
P6753=0

# Account 2 BLF URI
P444=

# Account 3 BLF Call-Pickup Prefix. Default value is **
# String
P581=**

# Account 3 Force BLF Call-pickup by Prefix. 0 - No, 1 - Yes. Default Value is 0
# Number : 0, 1
P6754=0

# Account 3 BLF URI
P544=

# Account 4 BLF Call-Pickup Prefix. Default value is **
# String
P681=**

# Account 4 Force BLF Call-pickup by Prefix. 0 - No, 1 - Yes. Default Value is 0
# Number : 0, 1
P6755=0

# Account 4 BLF URI
P644=

# Account 5 BLF Call-Pickup Prefix. Default value is **
# String
P1781=**

# Account 5 Force BLF Call-pickup by Prefix. 0 - No, 1 - Yes. Default Value is 0
# Number : 0, 1
P6756=0

# Account 5 BLF URI
P1744=

# Account 6 BLF Call-Pickup Prefix. Default value is **
# String
P1881=**

# Account 6 Force BLF Call-pickup by Prefix. 0 - No, 1 - Yes. Default Value is 0
# Number : 0, 1
P6757=0

# Account 6 BLF URI
P1844=

# Account 7 BLF Call-Pickup Prefix. Default value is **
# String
P50681=**

# Account 7 Force BLF Call-pickup by Prefix. 0 - No, 1 - Yes. Default Value is 0
# Number : 0, 1
P52683=0

# Account 7 BLF URI
P50644=

# Account 8 BLF Call-Pickup Prefix. Default value is **
# String
P50781=**

# Account 8 Force BLF Call-pickup by Prefix. 0 - No, 1 - Yes. Default Value is 0
# Number : 0, 1
P52783=0

# Account 8 BLF URI
P50744=

# Account 9 BLF Call-Pickup Prefix. Default value is **
# String
P50881=**

# Account 9 Force BLF Call-pickup by Prefix. 0 - No, 1 - Yes. Default Value is 0
# Number : 0, 1
P52883=0

# Account 9 BLF URI
P50844=

# Account 10 BLF Call-Pickup Prefix. Default value is **
# String
P50981=**

# Account 10 Force BLF Call-pickup by Prefix. 0 - No, 1 - Yes. Default Value is 0
# Number : 0, 1
P52983=0

# Account 10 BLF URI
P50944=

# Account 11 BLF Call-Pickup Prefix. Default value is **
# String
P51081=**

# Account 11 Force BLF Call-pickup by Prefix. 0 - No, 1 - Yes. Default Value is 0
# Number : 0, 1
P53083=0

# Account 11 BLF URI
P51044=

# Account 12 BLF Call-Pickup Prefix. Default value is **
# String
P51181=**

# Account 12 Force BLF Call-pickup by Prefix. 0 - No, 1 - Yes. Default Value is 0
# Number : 0, 1
P53183=0

# Account 12 BLF URI
P51144=

# Account 13 BLF Call-Pickup Prefix. Default value is **
# String
P51281=**

# Account 13 Force BLF Call-pickup by Prefix. 0 - No, 1 - Yes. Default Value is 0
# Number : 0, 1
P53283=0

# Account 13 BLF URI
P51244=

# Account 14 BLF Call-Pickup Prefix. Default value is **
# String
P51381=**

# Account 14 Force BLF Call-pickup by Prefix. 0 - No, 1 - Yes. Default Value is 0
# Number : 0, 1
P53383=0

# Account 14 BLF URI
P51344=

# Account 15 BLF Call-Pickup Prefix. Default value is **
# String
P51481=**

# Account 15 Force BLF Call-pickup by Prefix. 0 - No, 1 - Yes. Default Value is 0
# Number : 0, 1
P53483=0

# Account 15 BLF URI
P51444=

# Account 16 BLF Call-Pickup Prefix. Default value is **
# String
P51581=**

# Account 16 Force BLF Call-pickup by Prefix. 0 - No, 1 - Yes. Default Value is 0
# Number : 0, 1
P53583=0

# Account 16 BLF URI
P51544=
#######################################################################
##  Applications - Contacts - General Settings                       ##
#######################################################################
# Sort Phonebook by. 1 - Last Name, 0 - First Name. Default Value is 0
# Number : 0, 1
P2914=

# Phonebook Key Function. 0 - Default, 1 - LDAP Search, 2 - Local Phonebook, 3 - Local Group, 4 - Broadsoft Phonebook, 5 - Favorites. Default value is 0.
# Number : 0, 1, 2, 3, 4, 5
P1526=0

# Emergency Call Numbers. Default Value is 911
# String 
#Example 911,921,931,941
P25675=911
#######################################################################
##  Applications - Contacts - Download Contacts                 ##
#######################################################################
# Clear The Old List / Clear Old History Mode. 
# 0 - No, 1 - Clear all, 2 - Keep Local Contacts. Default value is 0
# Number: 0, 1, 2
P1435=0

# Replace Duplicate Items / Replace Duplicate Entries Mode. 
# 0 - No, 1 - Replace by name, 2 - Replace by number. Default value is 1
# Number: 0, 1, 2
P1436=1

# Download Mode. 0 - OFF, 1 - TFTP, 2 - HTTP, 3 - HTTPS. Default value is 0
# Number: 0, 1, 2, 3
P330=0

# File Encoding. GBK - GBK, UTF-8 - UTF-8, UTF-16 - UTF-16, UTF-32 - UTF-32, Big5 - Big5, Big5-HKSCS - Big5-HKSCS, Shift-JIS - Shift-JIS
# ISO 2022-JP - ISO 2022-JP, KOI8-R - KOI8-R, ISO8859-1 - ISO8859-1, ISO8859-15 - ISO8859-15, Windows-1251 - Windows-1251, EUC-KR - EUC-KR
# Default Value is UTF-8
# String : GBK, UTF-8, UTF-16, UTF-32, Big5, Big5-HKSCS,  Shift-JIS, ISO 2022-JP, KOI8-R, ISO8859-1, ISO8859-15, Windows-1251, EUC-KR 
P1681=UTF-8

# Download Server. It MUST be in the host/path format
# For example: directory.grandstream.com/engineering
# String
P331=

#HTTP/HTTPS User Name
P6713=

#HTTP/HTTPS Password
P6714=

# Download Interval. Default is 0 for disabled
# Number: 0, 120, 240, 360, 480, 720
P332=0
#######################################################################
##  Applications - LDAP Book                                         ##
#######################################################################
# Connection Mode. 0 - LDAP, 1 - LDAPS. Default Value is 0
# Number : 0, 1
P8037=0

# Server Address
# LDAP Server Address, up to 256 characters can be used. It can be IP address or Domain name
# String
P8020=

# Port
# Number: 1 - 65535. Default value is 389
P8021=389

# Base DN. The LDAP search base refers to the location in the directory where the search is requested to begin
# Example 1: dc=grandstream,dc=com
# Example 2: ou=Boston, dc=grandstream,dc=com
# String
P8022=

# User Name. The bind "Username" for querying LDAP servers. Some LDAP servers allow anonymous binds in which case the setting can be left blank
# String
P8023=

# Password. The bind "Password" for querying LDAP servers. And the field can be left blank if the LDAP server allows anonymous binds
# String
P8024=

# LDAP Name Attributes. This setting specifies the "name" attributes of each record which are returned in the LDAP search result
# The setting allows the users to configure multiple space separated name attributes
# String
P8028=

# LDAP Number Attributes. This setting specifies the "number" attributes of each record which are returned in the LDAP search result
# The setting allows the users to configure multiple space separated number attributes
# String
P8029=

# LDAP Mail Attributes. This setting specifies the "mail" attributes of each record which are returned in the LDAP search result
# The setting allows the users to configure multiple space separated mail attributes
# String
P8038=

# LDAP Name Filter
# LDAP name filter is the filter used for name look ups. Please refer to usermanual for examples
# String
P8026=

# LDAP Number Filter
# LDAP name filter is the filter used for number look ups. Please refer to usermanual for examples
# String
P8025=

# LDAP Mail Filter
# LDAP mail filter is the filter used for mail look ups. Please refer to usermanual for examples
# String
P8039=

# LDAP Displaying Name Attributes. The entry information to be shown on phone LCD. Grandstream phones will display up to 3 fields
# String
P8030=

# Max Hits. The setting specifies the maximum number of results to be returned by the LDAP server
# If the value is set to 0, server will return all search results. Default is 50
# Number: 0 - 32000
P8031=50

# Search Timeout (in seconds). Default is 4
# The setting specifies how long the server should process the request and client waits for server to return
# Number: 0 - 180
P8032=4

# LDAP Lookup For Dial. 0 - No, 1 - Yes. Default is 0
P8034=0

# LDAP Lookup For Incoming Calls. 0 - No, 1 - Yes. Default is 0
P8035=0

# LDAP Dialing Default Account. -1 - Default, 0 - Account 1, 1 - Account 2, 2 - Account 3, 3 - Account 4, 4 - Account 5, 5 - Account 6, etc. Default is 0
# Number : 0-6
P22039=0
########################################################################
##            Applications - Programmable key                    ##
########################################################################
########################################################################
# The MPKs in this section are for the MPK APP installed on GXV3370    #
########################################################################
# 160 MPKs can be configured via MPK APP                               #
########################################################################
#######################################################################################
# EXT MPK 1
#######################################################################################

# Key Mode.# 0 - Speed Dial, 1 - BLF, 4 - Speed Dial via active account, 5 - DialDTMF, 8 - Call Transfer, 9 - CallPark, 10 - Call Intercom, 13 - Multicast Paging, 15 - Speed Conference, 16 - Dial prefix
# Number: 0, 1, 4, 5, 8, 9, 10, 13, 15, 16
P23000=0

# Account. 0 - Account 1, 1 - Account 2, 2 - Account 3, 3 - Account 4, 4 - Account 5, 5 - Account 6
# Number: 0 - 5
P23001=0

# Name
# String
P23002=

# UserID
# String
P23003=

#######################################################################################
# EXT MPK 2
#######################################################################################

# Key Mode.# 0 - Speed Dial, 1 - BLF, 4 - Speed Dial via active account, 5 - DialDTMF, 8 - Call Transfer, 9 - CallPark, 10 - Call Intercom, 13 - Multicast Paging, 15 - Speed Conference, 16 - Dial prefix
# Number: 0, 1, 4, 5, 8, 9, 10, 13, 15, 16
P23005=0

# Account. 0 - Account 1, 1 - Account 2, 2 - Account 3, 3 - Account 4, 4 - Account 5, 5 - Account 6
# Number: 0 - 5
P23006=0

# Name
# String
P23007=

# UserID
# String
P23008=

#######################################################################################
# EXT MPK 3
#######################################################################################

# Key Mode.# 0 - Speed Dial, 1 - BLF, 4 - Speed Dial via active account, 5 - DialDTMF, 8 - Call Transfer, 9 - CallPark, 10 - Call Intercom, 13 - Multicast Paging, 15 - Speed Conference, 16 - Dial prefix
# Number: 0, 1, 4, 5, 8, 9, 10, 13, 15, 16
P23010=0

# Account. 0 - Account 1, 1 - Account 2, 2 - Account 3, 3 - Account 4, 4 - Account 5, 5 - Account 6
# Number: 0 - 5
P23011=0

# Name
# String
P23012=

# UserID
# String
P23013=

#######################################################################################
# EXT MPK 4
#######################################################################################

# Key Mode.# 0 - Speed Dial, 1 - BLF, 4 - Speed Dial via active account, 5 - DialDTMF, 8 - Call Transfer, 9 - CallPark, 10 - Call Intercom, 13 - Multicast Paging, 15 - Speed Conference, 16 - Dial prefix
# Number: 0, 1, 4, 5, 8, 9, 10, 13, 15, 16
P23015=0

# Account. 0 - Account 1, 1 - Account 2, 2 - Account 3, 3 - Account 4, 4 - Account 5, 5 - Account 6
# Number: 0 - 5
P23016=0

# Name
# String
P23017=

# UserID
# String
P23018=

#######################################################################################
# EXT MPK 5
#######################################################################################

# Key Mode.# 0 - Speed Dial, 1 - BLF, 4 - Speed Dial via active account, 5 - DialDTMF, 8 - Call Transfer, 9 - CallPark, 10 - Call Intercom, 13 - Multicast Paging, 15 - Speed Conference, 16 - Dial prefix
# Number: 0, 1, 4, 5, 8, 9, 10, 13, 15, 16
P23020=0

# Account. 0 - Account 1, 1 - Account 2, 2 - Account 3, 3 - Account 4, 4 - Account 5, 5 - Account 6
# Number: 0 - 5
P23021=0

# Name
# String
P23022=

# UserID
# String
P23023=

#######################################################################################
# EXT MPK 6
#######################################################################################

# Key Mode.# 0 - Speed Dial, 1 - BLF, 4 - Speed Dial via active account, 5 - DialDTMF, 8 - Call Transfer, 9 - CallPark, 10 - Call Intercom, 13 - Multicast Paging, 15 - Speed Conference, 16 - Dial prefix
# Number: 0, 1, 4, 5, 8, 9, 10, 13, 15, 16
P23025=0

# Account. 0 - Account 1, 1 - Account 2, 2 - Account 3, 3 - Account 4, 4 - Account 5, 5 - Account 6
# Number: 0 - 5
P23026=0

# Name
# String
P23027=

# UserID
# String
P23028=

#######################################################################################
# EXT MPK 7
#######################################################################################

# Key Mode.# 0 - Speed Dial, 1 - BLF, 4 - Speed Dial via active account, 5 - DialDTMF, 8 - Call Transfer, 9 - CallPark, 10 - Call Intercom, 13 - Multicast Paging, 15 - Speed Conference, 16 - Dial prefix
# Number: 0, 1, 4, 5, 8, 9, 10, 13, 15, 16
P23030=0

# Account. 0 - Account 1, 1 - Account 2, 2 - Account 3, 3 - Account 4, 4 - Account 5, 5 - Account 6
# Number: 0 - 5
P23031=0

# Name
# String
P23032=

# UserID
# String
P23033=

#######################################################################################
# EXT MPK 8
#######################################################################################

# Key Mode.# 0 - Speed Dial, 1 - BLF, 4 - Speed Dial via active account, 5 - DialDTMF, 8 - Call Transfer, 9 - CallPark, 10 - Call Intercom, 13 - Multicast Paging, 15 - Speed Conference, 16 - Dial prefix
# Number: 0, 1, 4, 5, 8, 9, 10, 13, 15, 16
P23035=0

# Account. 0 - Account 1, 1 - Account 2, 2 - Account 3, 3 - Account 4, 4 - Account 5, 5 - Account 6
# Number: 0 - 5
P23036=0

# Name
# String
P23037=

# UserID
# String
P23038=

#######################################################################################
# EXT MPK 9
#######################################################################################

# Key Mode.# 0 - Speed Dial, 1 - BLF, 4 - Speed Dial via active account, 5 - DialDTMF, 8 - Call Transfer, 9 - CallPark, 10 - Call Intercom, 13 - Multicast Paging, 15 - Speed Conference, 16 - Dial prefix
# Number: 0, 1, 4, 5, 8, 9, 10, 13, 15, 16
P23040=0

# Account. 0 - Account 1, 1 - Account 2, 2 - Account 3, 3 - Account 4, 4 - Account 5, 5 - Account 6
# Number: 0 - 5
P23041=0

# Name
# String
P23042=

# UserID
# String
P23043=

#######################################################################################
# EXT MPK 10
#######################################################################################

# Key Mode.# 0 - Speed Dial, 1 - BLF, 4 - Speed Dial via active account, 5 - DialDTMF, 8 - Call Transfer, 9 - CallPark, 10 - Call Intercom, 13 - Multicast Paging, 15 - Speed Conference, 16 - Dial prefix
# Number: 0, 1, 4, 5, 8, 9, 10, 13, 15, 16
P23045=0

# Account. 0 - Account 1, 1 - Account 2, 2 - Account 3, 3 - Account 4, 4 - Account 5, 5 - Account 6
# Number: 0 - 5
P23046=0

# Name
# String
P23047=

# UserID
# String
P23048=

#######################################################################################
# EXT MPK 11
#######################################################################################

# Key Mode.# 0 - Speed Dial, 1 - BLF, 4 - Speed Dial via active account, 5 - DialDTMF, 8 - Call Transfer, 9 - CallPark, 10 - Call Intercom, 13 - Multicast Paging, 15 - Speed Conference, 16 - Dial prefix
# Number: 0, 1, 4, 5, 8, 9, 10, 13, 15, 16
P23050=0

# Account. 0 - Account 1, 1 - Account 2, 2 - Account 3, 3 - Account 4, 4 - Account 5, 5 - Account 6
# Number: 0 - 5
P23051=0

# Name
# String
P23052=

# UserID
# String
P23053=

#######################################################################################
# EXT MPK 12
#######################################################################################

# Key Mode.# 0 - Speed Dial, 1 - BLF, 4 - Speed Dial via active account, 5 - DialDTMF, 8 - Call Transfer, 9 - CallPark, 10 - Call Intercom, 13 - Multicast Paging, 15 - Speed Conference, 16 - Dial prefix
# Number: 0, 1, 4, 5, 8, 9, 10, 13, 15, 16
P23055=0

# Account. 0 - Account 1, 1 - Account 2, 2 - Account 3, 3 - Account 4, 4 - Account 5, 5 - Account 6
# Number: 0 - 5
P23056=0

# Name
# String
P23057=

# UserID
# String
P23058=

#######################################################################################
# EXT MPK 13
#######################################################################################

# Key Mode.# 0 - Speed Dial, 1 - BLF, 4 - Speed Dial via active account, 5 - DialDTMF, 8 - Call Transfer, 9 - CallPark, 10 - Call Intercom, 13 - Multicast Paging, 15 - Speed Conference, 16 - Dial prefix
# Number: 0, 1, 4, 5, 8, 9, 10, 13, 15, 16
P23060=0

# Account. 0 - Account 1, 1 - Account 2, 2 - Account 3, 3 - Account 4, 4 - Account 5, 5 - Account 6
# Number: 0 - 5
P23061=0

# Name
# String
P23062=

# UserID
# String
P23063=

#######################################################################################
# EXT MPK 14
#######################################################################################

# Key Mode.# 0 - Speed Dial, 1 - BLF, 4 - Speed Dial via active account, 5 - DialDTMF, 8 - Call Transfer, 9 - CallPark, 10 - Call Intercom, 13 - Multicast Paging, 15 - Speed Conference, 16 - Dial prefix
# Number: 0, 1, 4, 5, 8, 9, 10, 13, 15, 16
P23065=0

# Account. 0 - Account 1, 1 - Account 2, 2 - Account 3, 3 - Account 4, 4 - Account 5, 5 - Account 6
# Number: 0 - 5
P23066=0

# Name
# String
P23067=

# UserID
# String
P23068=

#######################################################################################
# EXT MPK 15
#######################################################################################

# Key Mode.# 0 - Speed Dial, 1 - BLF, 4 - Speed Dial via active account, 5 - DialDTMF, 8 - Call Transfer, 9 - CallPark, 10 - Call Intercom, 13 - Multicast Paging, 15 - Speed Conference, 16 - Dial prefix
# Number: 0, 1, 4, 5, 8, 9, 10, 13, 15, 16
P23070=0

# Account. 0 - Account 1, 1 - Account 2, 2 - Account 3, 3 - Account 4, 4 - Account 5, 5 - Account 6
# Number: 0 - 5
P23071=0

# Name
# String
P23072=

# UserID
# String
P23073=

#######################################################################################
# EXT MPK 16
#######################################################################################

# Key Mode.# 0 - Speed Dial, 1 - BLF, 4 - Speed Dial via active account, 5 - DialDTMF, 8 - Call Transfer, 9 - CallPark, 10 - Call Intercom, 13 - Multicast Paging, 15 - Speed Conference, 16 - Dial prefix
# Number: 0, 1, 4, 5, 8, 9, 10, 13, 15, 16
P23075=0

# Account. 0 - Account 1, 1 - Account 2, 2 - Account 3, 3 - Account 4, 4 - Account 5, 5 - Account 6
# Number: 0 - 5
P23076=0

# Name
# String
P23077=

# UserID
# String
P23078=

#######################################################################################
# EXT MPK 17
#######################################################################################

# Key Mode.# 0 - Speed Dial, 1 - BLF, 4 - Speed Dial via active account, 5 - DialDTMF, 8 - Call Transfer, 9 - CallPark, 10 - Call Intercom, 13 - Multicast Paging, 15 - Speed Conference, 16 - Dial prefix
# Number: 0, 1, 4, 5, 8, 9, 10, 13, 15, 16
P23080=0

# Account. 0 - Account 1, 1 - Account 2, 2 - Account 3, 3 - Account 4, 4 - Account 5, 5 - Account 6
# Number: 0 - 5
P23081=0

# Name
# String
P23082=

# UserID
# String
P23083=

#######################################################################################
# EXT MPK 18
#######################################################################################

# Key Mode.# 0 - Speed Dial, 1 - BLF, 4 - Speed Dial via active account, 5 - DialDTMF, 8 - Call Transfer, 9 - CallPark, 10 - Call Intercom, 13 - Multicast Paging, 15 - Speed Conference, 16 - Dial prefix
# Number: 0, 1, 4, 5, 8, 9, 10, 13, 15, 16
P23085=0

# Account. 0 - Account 1, 1 - Account 2, 2 - Account 3, 3 - Account 4, 4 - Account 5, 5 - Account 6
# Number: 0 - 5
P23086=0

# Name
# String
P23087=

# UserID
# String
P23088=

#######################################################################################
# EXT MPK 19
#######################################################################################

# Key Mode.# 0 - Speed Dial, 1 - BLF, 4 - Speed Dial via active account, 5 - DialDTMF, 8 - Call Transfer, 9 - CallPark, 10 - Call Intercom, 13 - Multicast Paging, 15 - Speed Conference, 16 - Dial prefix
# Number: 0, 1, 4, 5, 8, 9, 10, 13, 15, 16
P23090=0

# Account. 0 - Account 1, 1 - Account 2, 2 - Account 3, 3 - Account 4, 4 - Account 5, 5 - Account 6
# Number: 0 - 5
P23091=0

# Name
# String
P23092=

# UserID
# String
P23093=

#######################################################################################
# EXT MPK 20
#######################################################################################

# Key Mode.# 0 - Speed Dial, 1 - BLF, 4 - Speed Dial via active account, 5 - DialDTMF, 8 - Call Transfer, 9 - CallPark, 10 - Call Intercom, 13 - Multicast Paging, 15 - Speed Conference, 16 - Dial prefix
# Number: 0, 1, 4, 5, 8, 9, 10, 13, 15, 16
P23095=0

# Account. 0 - Account 1, 1 - Account 2, 2 - Account 3, 3 - Account 4, 4 - Account 5, 5 - Account 6
# Number: 0 - 5
P23096=0

# Name
# String
P23097=

# UserID
# String
P23098=

#######################################################################################
# EXT MPK 21
#######################################################################################

# Key Mode.# 0 - Speed Dial, 1 - BLF, 4 - Speed Dial via active account, 5 - DialDTMF, 8 - Call Transfer, 9 - CallPark, 10 - Call Intercom, 13 - Multicast Paging, 15 - Speed Conference, 16 - Dial prefix
# Number: 0, 1, 4, 5, 8, 9, 10, 13, 15, 16
P23100=0

# Account. 0 - Account 1, 1 - Account 2, 2 - Account 3, 3 - Account 4, 4 - Account 5, 5 - Account 6
# Number: 0 - 5
P23101=0

# Name
# String
P23102=

# UserID
# String
P23103=

#######################################################################################
# EXT MPK 22
#######################################################################################

# Key Mode.# 0 - Speed Dial, 1 - BLF, 4 - Speed Dial via active account, 5 - DialDTMF, 8 - Call Transfer, 9 - CallPark, 10 - Call Intercom, 13 - Multicast Paging, 15 - Speed Conference, 16 - Dial prefix
# Number: 0, 1, 4, 5, 8, 9, 10, 13, 15, 16
P23105=0

# Account. 0 - Account 1, 1 - Account 2, 2 - Account 3, 3 - Account 4, 4 - Account 5, 5 - Account 6
# Number: 0 - 5
P23106=0

# Name
# String
P23107=

# UserID
# String
P23108=

#######################################################################################
# EXT MPK 23
#######################################################################################

# Key Mode.# 0 - Speed Dial, 1 - BLF, 4 - Speed Dial via active account, 5 - DialDTMF, 8 - Call Transfer, 9 - CallPark, 10 - Call Intercom, 13 - Multicast Paging, 15 - Speed Conference, 16 - Dial prefix
# Number: 0, 1, 4, 5, 8, 9, 10, 13, 15, 16
P23110=0

# Account. 0 - Account 1, 1 - Account 2, 2 - Account 3, 3 - Account 4, 4 - Account 5, 5 - Account 6
# Number: 0 - 5
P23111=0

# Name
# String
P23112=

# UserID
# String
P23113=

#######################################################################################
# EXT MPK 24
#######################################################################################

# Key Mode.# 0 - Speed Dial, 1 - BLF, 4 - Speed Dial via active account, 5 - DialDTMF, 8 - Call Transfer, 9 - CallPark, 10 - Call Intercom, 13 - Multicast Paging, 15 - Speed Conference, 16 - Dial prefix
# Number: 0, 1, 4, 5, 8, 9, 10, 13, 15, 16
P23115=0

# Account. 0 - Account 1, 1 - Account 2, 2 - Account 3, 3 - Account 4, 4 - Account 5, 5 - Account 6
# Number: 0 - 5
P23116=0

# Name
# String
P23117=

# UserID
# String
P23118=

#######################################################################################
# EXT MPK 25
#######################################################################################

# Key Mode.# 0 - Speed Dial, 1 - BLF, 4 - Speed Dial via active account, 5 - DialDTMF, 8 - Call Transfer, 9 - CallPark, 10 - Call Intercom, 13 - Multicast Paging, 15 - Speed Conference, 16 - Dial prefix
# Number: 0, 1, 4, 5, 8, 9, 10, 13, 15, 16
P23120=0

# Account. 0 - Account 1, 1 - Account 2, 2 - Account 3, 3 - Account 4, 4 - Account 5, 5 - Account 6
# Number: 0 - 5
P23121=0

# Name
# String
P23122=

# UserID
# String
P23123=

#######################################################################################
# EXT MPK 26
#######################################################################################

# Key Mode.# 0 - Speed Dial, 1 - BLF, 4 - Speed Dial via active account, 5 - DialDTMF, 8 - Call Transfer, 9 - CallPark, 10 - Call Intercom, 13 - Multicast Paging, 15 - Speed Conference, 16 - Dial prefix
# Number: 0, 1, 4, 5, 8, 9, 10, 13, 15, 16
P23125=0

# Account. 0 - Account 1, 1 - Account 2, 2 - Account 3, 3 - Account 4, 4 - Account 5, 5 - Account 6
# Number: 0 - 5
P23126=0

# Name
# String
P23127=

# UserID
# String
P23128=

#######################################################################################
# EXT MPK 27
#######################################################################################

# Key Mode.# 0 - Speed Dial, 1 - BLF, 4 - Speed Dial via active account, 5 - DialDTMF, 8 - Call Transfer, 9 - CallPark, 10 - Call Intercom, 13 - Multicast Paging, 15 - Speed Conference, 16 - Dial prefix
# Number: 0, 1, 4, 5, 8, 9, 10, 13, 15, 16
P23130=0

# Account. 0 - Account 1, 1 - Account 2, 2 - Account 3, 3 - Account 4, 4 - Account 5, 5 - Account 6
# Number: 0 - 5
P23131=0

# Name
# String
P23132=

# UserID
# String
P23133=

#######################################################################################
# EXT MPK 28
#######################################################################################

# Key Mode.# 0 - Speed Dial, 1 - BLF, 4 - Speed Dial via active account, 5 - DialDTMF, 8 - Call Transfer, 9 - CallPark, 10 - Call Intercom, 13 - Multicast Paging, 15 - Speed Conference, 16 - Dial prefix
# Number: 0, 1, 4, 5, 8, 9, 10, 13, 15, 16
P23135=0

# Account. 0 - Account 1, 1 - Account 2, 2 - Account 3, 3 - Account 4, 4 - Account 5, 5 - Account 6
# Number: 0 - 5
P23136=0

# Name
# String
P23137=

# UserID
# String
P23138=

#######################################################################################
# EXT MPK 29
#######################################################################################

# Key Mode.# 0 - Speed Dial, 1 - BLF, 4 - Speed Dial via active account, 5 - DialDTMF, 8 - Call Transfer, 9 - CallPark, 10 - Call Intercom, 13 - Multicast Paging, 15 - Speed Conference, 16 - Dial prefix
# Number: 0, 1, 4, 5, 8, 9, 10, 13, 15, 16
P23140=0

# Account. 0 - Account 1, 1 - Account 2, 2 - Account 3, 3 - Account 4, 4 - Account 5, 5 - Account 6
# Number: 0 - 5
P23141=0

# Name
# String
P23142=

# UserID
# String
P23143=

#######################################################################################
# EXT MPK 30
#######################################################################################

# Key Mode.# 0 - Speed Dial, 1 - BLF, 4 - Speed Dial via active account, 5 - DialDTMF, 8 - Call Transfer, 9 - CallPark, 10 - Call Intercom, 13 - Multicast Paging, 15 - Speed Conference, 16 - Dial prefix
# Number: 0, 1, 4, 5, 8, 9, 10, 13, 15, 16
P23145=0

# Account. 0 - Account 1, 1 - Account 2, 2 - Account 3, 3 - Account 4, 4 - Account 5, 5 - Account 6
# Number: 0 - 5
P23146=0

# Name
# String
P23147=

# UserID
# String
P23148=

#######################################################################################
# EXT MPK 31
#######################################################################################

# Key Mode.# 0 - Speed Dial, 1 - BLF, 4 - Speed Dial via active account, 5 - DialDTMF, 8 - Call Transfer, 9 - CallPark, 10 - Call Intercom, 13 - Multicast Paging, 15 - Speed Conference, 16 - Dial prefix
# Number: 0, 1, 4, 5, 8, 9, 10, 13, 15, 16
P23150=0

# Account. 0 - Account 1, 1 - Account 2, 2 - Account 3, 3 - Account 4, 4 - Account 5, 5 - Account 6
# Number: 0 - 5
P23151=0

# Name
# String
P23152=

# UserID
# String
P23153=

#######################################################################################
# EXT MPK 32
#######################################################################################

# Key Mode.# 0 - Speed Dial, 1 - BLF, 4 - Speed Dial via active account, 5 - DialDTMF, 8 - Call Transfer, 9 - CallPark, 10 - Call Intercom, 13 - Multicast Paging, 15 - Speed Conference, 16 - Dial prefix
# Number: 0, 1, 4, 5, 8, 9, 10, 13, 15, 16
P23155=0

# Account. 0 - Account 1, 1 - Account 2, 2 - Account 3, 3 - Account 4, 4 - Account 5, 5 - Account 6
# Number: 0 - 5
P23156=0

# Name
# String
P23157=

# UserID
# String
P23158=

#######################################################################################
# EXT MPK 33
#######################################################################################

# Key Mode.# 0 - Speed Dial, 1 - BLF, 4 - Speed Dial via active account, 5 - DialDTMF, 8 - Call Transfer, 9 - CallPark, 10 - Call Intercom, 13 - Multicast Paging, 15 - Speed Conference, 16 - Dial prefix
# Number: 0, 1, 4, 5, 8, 9, 10, 13, 15, 16
P23160=0

# Account. 0 - Account 1, 1 - Account 2, 2 - Account 3, 3 - Account 4, 4 - Account 5, 5 - Account 6
# Number: 0 - 5
P23161=0

# Name
# String
P23162=

# UserID
# String
P23163=

#######################################################################################
# EXT MPK 34
#######################################################################################

# Key Mode.# 0 - Speed Dial, 1 - BLF, 4 - Speed Dial via active account, 5 - DialDTMF, 8 - Call Transfer, 9 - CallPark, 10 - Call Intercom, 13 - Multicast Paging, 15 - Speed Conference, 16 - Dial prefix
# Number: 0, 1, 4, 5, 8, 9, 10, 13, 15, 16
P23165=0

# Account. 0 - Account 1, 1 - Account 2, 2 - Account 3, 3 - Account 4, 4 - Account 5, 5 - Account 6
# Number: 0 - 5
P23166=0

# Name
# String
P23167=

# UserID
# String
P23168=

#######################################################################################
# EXT MPK 35
#######################################################################################

# Key Mode.# 0 - Speed Dial, 1 - BLF, 4 - Speed Dial via active account, 5 - DialDTMF, 8 - Call Transfer, 9 - CallPark, 10 - Call Intercom, 13 - Multicast Paging, 15 - Speed Conference, 16 - Dial prefix
# Number: 0, 1, 4, 5, 8, 9, 10, 13, 15, 16
P23170=0

# Account. 0 - Account 1, 1 - Account 2, 2 - Account 3, 3 - Account 4, 4 - Account 5, 5 - Account 6
# Number: 0 - 5
P23171=0

# Name
# String
P23172=

# UserID
# String
P23173=

#######################################################################################
# EXT MPK 36
#######################################################################################

# Key Mode.# 0 - Speed Dial, 1 - BLF, 4 - Speed Dial via active account, 5 - DialDTMF, 8 - Call Transfer, 9 - CallPark, 10 - Call Intercom, 13 - Multicast Paging, 15 - Speed Conference, 16 - Dial prefix
# Number: 0, 1, 4, 5, 8, 9, 10, 13, 15, 16
P23175=0

# Account. 0 - Account 1, 1 - Account 2, 2 - Account 3, 3 - Account 4, 4 - Account 5, 5 - Account 6
# Number: 0 - 5
P23176=0

# Name
# String
P23177=

# UserID
# String
P23178=

#######################################################################################
# EXT MPK 37
#######################################################################################

# Key Mode.# 0 - Speed Dial, 1 - BLF, 4 - Speed Dial via active account, 5 - DialDTMF, 8 - Call Transfer, 9 - CallPark, 10 - Call Intercom, 13 - Multicast Paging, 15 - Speed Conference, 16 - Dial prefix
# Number: 0, 1, 4, 5, 8, 9, 10, 13, 15, 16
P23180=0

# Account. 0 - Account 1, 1 - Account 2, 2 - Account 3, 3 - Account 4, 4 - Account 5, 5 - Account 6
# Number: 0 - 5
P23181=0

# Name
# String
P23182=

# UserID
# String
P23183=

#######################################################################################
# EXT MPK 38
#######################################################################################

# Key Mode.# 0 - Speed Dial, 1 - BLF, 4 - Speed Dial via active account, 5 - DialDTMF, 8 - Call Transfer, 9 - CallPark, 10 - Call Intercom, 13 - Multicast Paging, 15 - Speed Conference, 16 - Dial prefix
# Number: 0, 1, 4, 5, 8, 9, 10, 13, 15, 16
P23185=0

# Account. 0 - Account 1, 1 - Account 2, 2 - Account 3, 3 - Account 4, 4 - Account 5, 5 - Account 6
# Number: 0 - 5
P23186=0

# Name
# String
P23187=

# UserID
# String
P23188=

#######################################################################################
# EXT MPK 39
#######################################################################################

# Key Mode.# 0 - Speed Dial, 1 - BLF, 4 - Speed Dial via active account, 5 - DialDTMF, 8 - Call Transfer, 9 - CallPark, 10 - Call Intercom, 13 - Multicast Paging, 15 - Speed Conference, 16 - Dial prefix
# Number: 0, 1, 4, 5, 8, 9, 10, 13, 15, 16
P23190=0

# Account. 0 - Account 1, 1 - Account 2, 2 - Account 3, 3 - Account 4, 4 - Account 5, 5 - Account 6
# Number: 0 - 5
P23191=0

# Name
# String
P23192=

# UserID
# String
P23193=

#######################################################################################
# EXT MPK 40
#######################################################################################

# Key Mode.# 0 - Speed Dial, 1 - BLF, 4 - Speed Dial via active account, 5 - DialDTMF, 8 - Call Transfer, 9 - CallPark, 10 - Call Intercom, 13 - Multicast Paging, 15 - Speed Conference, 16 - Dial prefix
# Number: 0, 1, 4, 5, 8, 9, 10, 13, 15, 16
P23195=0

# Account. 0 - Account 1, 1 - Account 2, 2 - Account 3, 3 - Account 4, 4 - Account 5, 5 - Account 6
# Number: 0 - 5
P23196=0

# Name
# String
P23197=

# UserID
# String
P23198=

#######################################################################################
# EXT MPK 41
#######################################################################################

# Key Mode.# 0 - Speed Dial, 1 - BLF, 4 - Speed Dial via active account, 5 - DialDTMF, 8 - Call Transfer, 9 - CallPark, 10 - Call Intercom, 13 - Multicast Paging, 15 - Speed Conference, 16 - Dial prefix
# Number: 0, 1, 4, 5, 8, 9, 10, 13, 15, 16
P23200=0

# Account. 0 - Account 1, 1 - Account 2, 2 - Account 3, 3 - Account 4, 4 - Account 5, 5 - Account 6
# Number: 0 - 5
P23201=0

# Name
# String
P23202=

# UserID
# String
P23203=

#######################################################################################
# EXT MPK 42
#######################################################################################

# Key Mode.# 0 - Speed Dial, 1 - BLF, 4 - Speed Dial via active account, 5 - DialDTMF, 8 - Call Transfer, 9 - CallPark, 10 - Call Intercom, 13 - Multicast Paging, 15 - Speed Conference, 16 - Dial prefix
# Number: 0, 1, 4, 5, 8, 9, 10, 13, 15, 16
P23205=0

# Account. 0 - Account 1, 1 - Account 2, 2 - Account 3, 3 - Account 4, 4 - Account 5, 5 - Account 6
# Number: 0 - 5
P23206=0

# Name
# String
P23207=

# UserID
# String
P23208=

#######################################################################################
# EXT MPK 43
#######################################################################################

# Key Mode.# 0 - Speed Dial, 1 - BLF, 4 - Speed Dial via active account, 5 - DialDTMF, 8 - Call Transfer, 9 - CallPark, 10 - Call Intercom, 13 - Multicast Paging, 15 - Speed Conference, 16 - Dial prefix
# Number: 0, 1, 4, 5, 8, 9, 10, 13, 15, 16
P23210=0

# Account. 0 - Account 1, 1 - Account 2, 2 - Account 3, 3 - Account 4, 4 - Account 5, 5 - Account 6
# Number: 0 - 5
P23211=0

# Name
# String
P23212=

# UserID
# String
P23213=

#######################################################################################
# EXT MPK 44
#######################################################################################

# Key Mode.# 0 - Speed Dial, 1 - BLF, 4 - Speed Dial via active account, 5 - DialDTMF, 8 - Call Transfer, 9 - CallPark, 10 - Call Intercom, 13 - Multicast Paging, 15 - Speed Conference, 16 - Dial prefix
# Number: 0, 1, 4, 5, 8, 9, 10, 13, 15, 16
P23215=0

# Account. 0 - Account 1, 1 - Account 2, 2 - Account 3, 3 - Account 4, 4 - Account 5, 5 - Account 6
# Number: 0 - 5
P23216=0

# Name
# String
P23217=

# UserID
# String
P23218=

#######################################################################################
# EXT MPK 45
#######################################################################################

# Key Mode.# 0 - Speed Dial, 1 - BLF, 4 - Speed Dial via active account, 5 - DialDTMF, 8 - Call Transfer, 9 - CallPark, 10 - Call Intercom, 13 - Multicast Paging, 15 - Speed Conference, 16 - Dial prefix
# Number: 0, 1, 4, 5, 8, 9, 10, 13, 15, 16
P23220=0

# Account. 0 - Account 1, 1 - Account 2, 2 - Account 3, 3 - Account 4, 4 - Account 5, 5 - Account 6
# Number: 0 - 5
P23221=0

# Name
# String
P23222=

# UserID
# String
P23223=

#######################################################################################
# EXT MPK 46
#######################################################################################

# Key Mode.# 0 - Speed Dial, 1 - BLF, 4 - Speed Dial via active account, 5 - DialDTMF, 8 - Call Transfer, 9 - CallPark, 10 - Call Intercom, 13 - Multicast Paging, 15 - Speed Conference, 16 - Dial prefix
# Number: 0, 1, 4, 5, 8, 9, 10, 13, 15, 16
P23225=0

# Account. 0 - Account 1, 1 - Account 2, 2 - Account 3, 3 - Account 4, 4 - Account 5, 5 - Account 6
# Number: 0 - 5
P23226=0

# Name
# String
P23227=

# UserID
# String
P23228=

#######################################################################################
# EXT MPK 47
#######################################################################################

# Key Mode.# 0 - Speed Dial, 1 - BLF, 4 - Speed Dial via active account, 5 - DialDTMF, 8 - Call Transfer, 9 - CallPark, 10 - Call Intercom, 13 - Multicast Paging, 15 - Speed Conference, 16 - Dial prefix
# Number: 0, 1, 4, 5, 8, 9, 10, 13, 15, 16
P23230=0

# Account. 0 - Account 1, 1 - Account 2, 2 - Account 3, 3 - Account 4, 4 - Account 5, 5 - Account 6
# Number: 0 - 5
P23231=0

# Name
# String
P23232=

# UserID
# String
P23233=

#######################################################################################
# EXT MPK 48
#######################################################################################

# Key Mode.# 0 - Speed Dial, 1 - BLF, 4 - Speed Dial via active account, 5 - DialDTMF, 8 - Call Transfer, 9 - CallPark, 10 - Call Intercom, 13 - Multicast Paging, 15 - Speed Conference, 16 - Dial prefix
# Number: 0, 1, 4, 5, 8, 9, 10, 13, 15, 16
P23235=0

# Account. 0 - Account 1, 1 - Account 2, 2 - Account 3, 3 - Account 4, 4 - Account 5, 5 - Account 6
# Number: 0 - 5
P23236=0

# Name
# String
P23237=

# UserID
# String
P23238=

#######################################################################################
# EXT MPK 49
#######################################################################################

# Key Mode.# 0 - Speed Dial, 1 - BLF, 4 - Speed Dial via active account, 5 - DialDTMF, 8 - Call Transfer, 9 - CallPark, 10 - Call Intercom, 13 - Multicast Paging, 15 - Speed Conference, 16 - Dial prefix
# Number: 0, 1, 4, 5, 8, 9, 10, 13, 15, 16
P23240=0

# Account. 0 - Account 1, 1 - Account 2, 2 - Account 3, 3 - Account 4, 4 - Account 5, 5 - Account 6
# Number: 0 - 5
P23241=0

# Name
# String
P23242=

# UserID
# String
P23243=

#######################################################################################
# EXT MPK 50
#######################################################################################

# Key Mode.# 0 - Speed Dial, 1 - BLF, 4 - Speed Dial via active account, 5 - DialDTMF, 8 - Call Transfer, 9 - CallPark, 10 - Call Intercom, 13 - Multicast Paging, 15 - Speed Conference, 16 - Dial prefix
# Number: 0, 1, 4, 5, 8, 9, 10, 13, 15, 16
P23245=0

# Account. 0 - Account 1, 1 - Account 2, 2 - Account 3, 3 - Account 4, 4 - Account 5, 5 - Account 6
# Number: 0 - 5
P23246=0

# Name
# String
P23247=

# UserID
# String
P23248=

#######################################################################################
# EXT MPK 51
#######################################################################################

# Key Mode.# 0 - Speed Dial, 1 - BLF, 4 - Speed Dial via active account, 5 - DialDTMF, 8 - Call Transfer, 9 - CallPark, 10 - Call Intercom, 13 - Multicast Paging, 15 - Speed Conference, 16 - Dial prefix
# Number: 0, 1, 4, 5, 8, 9, 10, 13, 15, 16
P23250=0

# Account. 0 - Account 1, 1 - Account 2, 2 - Account 3, 3 - Account 4, 4 - Account 5, 5 - Account 6
# Number: 0 - 5
P23251=0

# Name
# String
P23252=

# UserID
# String
P23253=

#######################################################################################
# EXT MPK 52
#######################################################################################

# Key Mode.# 0 - Speed Dial, 1 - BLF, 4 - Speed Dial via active account, 5 - DialDTMF, 8 - Call Transfer, 9 - CallPark, 10 - Call Intercom, 13 - Multicast Paging, 15 - Speed Conference, 16 - Dial prefix
# Number: 0, 1, 4, 5, 8, 9, 10, 13, 15, 16
P23255=0

# Account. 0 - Account 1, 1 - Account 2, 2 - Account 3, 3 - Account 4, 4 - Account 5, 5 - Account 6
# Number: 0 - 5
P23256=0

# Name
# String
P23257=

# UserID
# String
P23258=

#######################################################################################
# EXT MPK 53
#######################################################################################

# Key Mode.# 0 - Speed Dial, 1 - BLF, 4 - Speed Dial via active account, 5 - DialDTMF, 8 - Call Transfer, 9 - CallPark, 10 - Call Intercom, 13 - Multicast Paging, 15 - Speed Conference, 16 - Dial prefix
# Number: 0, 1, 4, 5, 8, 9, 10, 13, 15, 16
P23260=0

# Account. 0 - Account 1, 1 - Account 2, 2 - Account 3, 3 - Account 4, 4 - Account 5, 5 - Account 6
# Number: 0 - 5
P23261=0

# Name
# String
P23262=

# UserID
# String
P23263=

#######################################################################################
# EXT MPK 54
#######################################################################################

# Key Mode.# 0 - Speed Dial, 1 - BLF, 4 - Speed Dial via active account, 5 - DialDTMF, 8 - Call Transfer, 9 - CallPark, 10 - Call Intercom, 13 - Multicast Paging, 15 - Speed Conference, 16 - Dial prefix
# Number: 0, 1, 4, 5, 8, 9, 10, 13, 15, 16
P23265=0

# Account. 0 - Account 1, 1 - Account 2, 2 - Account 3, 3 - Account 4, 4 - Account 5, 5 - Account 6
# Number: 0 - 5
P23266=0

# Name
# String
P23267=

# UserID
# String
P23268=

#######################################################################################
# EXT MPK 55
#######################################################################################

# Key Mode.# 0 - Speed Dial, 1 - BLF, 4 - Speed Dial via active account, 5 - DialDTMF, 8 - Call Transfer, 9 - CallPark, 10 - Call Intercom, 13 - Multicast Paging, 15 - Speed Conference, 16 - Dial prefix
# Number: 0, 1, 4, 5, 8, 9, 10, 13, 15, 16
P23270=0

# Account. 0 - Account 1, 1 - Account 2, 2 - Account 3, 3 - Account 4, 4 - Account 5, 5 - Account 6
# Number: 0 - 5
P23271=0

# Name
# String
P23272=

# UserID
# String
P23273=

#######################################################################################
# EXT MPK 56
#######################################################################################

# Key Mode.# 0 - Speed Dial, 1 - BLF, 4 - Speed Dial via active account, 5 - DialDTMF, 8 - Call Transfer, 9 - CallPark, 10 - Call Intercom, 13 - Multicast Paging, 15 - Speed Conference, 16 - Dial prefix
# Number: 0, 1, 4, 5, 8, 9, 10, 13, 15, 16
P23275=0

# Account. 0 - Account 1, 1 - Account 2, 2 - Account 3, 3 - Account 4, 4 - Account 5, 5 - Account 6
# Number: 0 - 5
P23276=0

# Name
# String
P23277=

# UserID
# String
P23278=

#######################################################################################
# EXT MPK 57
#######################################################################################

# Key Mode.# 0 - Speed Dial, 1 - BLF, 4 - Speed Dial via active account, 5 - DialDTMF, 8 - Call Transfer, 9 - CallPark, 10 - Call Intercom, 13 - Multicast Paging, 15 - Speed Conference, 16 - Dial prefix
# Number: 0, 1, 4, 5, 8, 9, 10, 13, 15, 16
P23280=0

# Account. 0 - Account 1, 1 - Account 2, 2 - Account 3, 3 - Account 4, 4 - Account 5, 5 - Account 6
# Number: 0 - 5
P23281=0

# Name
# String
P23282=

# UserID
# String
P23283=

#######################################################################################
# EXT MPK 58
#######################################################################################

# Key Mode.# 0 - Speed Dial, 1 - BLF, 4 - Speed Dial via active account, 5 - DialDTMF, 8 - Call Transfer, 9 - CallPark, 10 - Call Intercom, 13 - Multicast Paging, 15 - Speed Conference, 16 - Dial prefix
# Number: 0, 1, 4, 5, 8, 9, 10, 13, 15, 16
P23285=0

# Account. 0 - Account 1, 1 - Account 2, 2 - Account 3, 3 - Account 4, 4 - Account 5, 5 - Account 6
# Number: 0 - 5
P23286=0

# Name
# String
P23287=

# UserID
# String
P23288=

#######################################################################################
# EXT MPK 59
#######################################################################################

# Key Mode.# 0 - Speed Dial, 1 - BLF, 4 - Speed Dial via active account, 5 - DialDTMF, 8 - Call Transfer, 9 - CallPark, 10 - Call Intercom, 13 - Multicast Paging, 15 - Speed Conference, 16 - Dial prefix
# Number: 0, 1, 4, 5, 8, 9, 10, 13, 15, 16
P23290=0

# Account. 0 - Account 1, 1 - Account 2, 2 - Account 3, 3 - Account 4, 4 - Account 5, 5 - Account 6
# Number: 0 - 5
P23291=0

# Name
# String
P23292=

# UserID
# String
P23293=

#######################################################################################
# EXT MPK 60
#######################################################################################

# Key Mode.# 0 - Speed Dial, 1 - BLF, 4 - Speed Dial via active account, 5 - DialDTMF, 8 - Call Transfer, 9 - CallPark, 10 - Call Intercom, 13 - Multicast Paging, 15 - Speed Conference, 16 - Dial prefix
# Number: 0, 1, 4, 5, 8, 9, 10, 13, 15, 16
P23295=0

# Account. 0 - Account 1, 1 - Account 2, 2 - Account 3, 3 - Account 4, 4 - Account 5, 5 - Account 6
# Number: 0 - 5
P23296=0

# Name
# String
P23297=

# UserID
# String
P23298=

#######################################################################################
# EXT MPK 61
#######################################################################################

# Key Mode.# 0 - Speed Dial, 1 - BLF, 4 - Speed Dial via active account, 5 - DialDTMF, 8 - Call Transfer, 9 - CallPark, 10 - Call Intercom, 13 - Multicast Paging, 15 - Speed Conference, 16 - Dial prefix
# Number: 0, 1, 4, 5, 8, 9, 10, 13, 15, 16
P23300=0

# Account. 0 - Account 1, 1 - Account 2, 2 - Account 3, 3 - Account 4, 4 - Account 5, 5 - Account 6
# Number: 0 - 5
P23301=0

# Name
# String
P23302=

# UserID
# String
P23303=

#######################################################################################
# EXT MPK 62
#######################################################################################

# Key Mode.# 0 - Speed Dial, 1 - BLF, 4 - Speed Dial via active account, 5 - DialDTMF, 8 - Call Transfer, 9 - CallPark, 10 - Call Intercom, 13 - Multicast Paging, 15 - Speed Conference, 16 - Dial prefix
# Number: 0, 1, 4, 5, 8, 9, 10, 13, 15, 16
P23305=0

# Account. 0 - Account 1, 1 - Account 2, 2 - Account 3, 3 - Account 4, 4 - Account 5, 5 - Account 6
# Number: 0 - 5
P23306=0

# Name
# String
P23307=

# UserID
# String
P23308=

#######################################################################################
# EXT MPK 63
#######################################################################################

# Key Mode.# 0 - Speed Dial, 1 - BLF, 4 - Speed Dial via active account, 5 - DialDTMF, 8 - Call Transfer, 9 - CallPark, 10 - Call Intercom, 13 - Multicast Paging, 15 - Speed Conference, 16 - Dial prefix
# Number: 0, 1, 4, 5, 8, 9, 10, 13, 15, 16
P23310=0

# Account. 0 - Account 1, 1 - Account 2, 2 - Account 3, 3 - Account 4, 4 - Account 5, 5 - Account 6
# Number: 0 - 5
P23311=0

# Name
# String
P23312=

# UserID
# String
P23313=

#######################################################################################
# EXT MPK 64
#######################################################################################

# Key Mode.# 0 - Speed Dial, 1 - BLF, 4 - Speed Dial via active account, 5 - DialDTMF, 8 - Call Transfer, 9 - CallPark, 10 - Call Intercom, 13 - Multicast Paging, 15 - Speed Conference, 16 - Dial prefix
# Number: 0, 1, 4, 5, 8, 9, 10, 13, 15, 16
P23315=0

# Account. 0 - Account 1, 1 - Account 2, 2 - Account 3, 3 - Account 4, 4 - Account 5, 5 - Account 6
# Number: 0 - 5
P23316=0

# Name
# String
P23317=

# UserID
# String
P23318=

#######################################################################################
# EXT MPK 65
#######################################################################################

# Key Mode.# 0 - Speed Dial, 1 - BLF, 4 - Speed Dial via active account, 5 - DialDTMF, 8 - Call Transfer, 9 - CallPark, 10 - Call Intercom, 13 - Multicast Paging, 15 - Speed Conference, 16 - Dial prefix
# Number: 0, 1, 4, 5, 8, 9, 10, 13, 15, 16
P23320=0

# Account. 0 - Account 1, 1 - Account 2, 2 - Account 3, 3 - Account 4, 4 - Account 5, 5 - Account 6
# Number: 0 - 5
P23321=0

# Name
# String
P23322=

# UserID
# String
P23323=

#######################################################################################
# EXT MPK 66
#######################################################################################

# Key Mode.# 0 - Speed Dial, 1 - BLF, 4 - Speed Dial via active account, 5 - DialDTMF, 8 - Call Transfer, 9 - CallPark, 10 - Call Intercom, 13 - Multicast Paging, 15 - Speed Conference, 16 - Dial prefix
# Number: 0, 1, 4, 5, 8, 9, 10, 13, 15, 16
P23325=0

# Account. 0 - Account 1, 1 - Account 2, 2 - Account 3, 3 - Account 4, 4 - Account 5, 5 - Account 6
# Number: 0 - 5
P23326=0

# Name
# String
P23327=

# UserID
# String
P23328=

#######################################################################################
# EXT MPK 67
#######################################################################################

# Key Mode.# 0 - Speed Dial, 1 - BLF, 4 - Speed Dial via active account, 5 - DialDTMF, 8 - Call Transfer, 9 - CallPark, 10 - Call Intercom, 13 - Multicast Paging, 15 - Speed Conference, 16 - Dial prefix
# Number: 0, 1, 4, 5, 8, 9, 10, 13, 15, 16
P23330=0

# Account. 0 - Account 1, 1 - Account 2, 2 - Account 3, 3 - Account 4, 4 - Account 5, 5 - Account 6
# Number: 0 - 5
P23331=0

# Name
# String
P23332=

# UserID
# String
P23333=

#######################################################################################
# EXT MPK 68
#######################################################################################

# Key Mode.# 0 - Speed Dial, 1 - BLF, 4 - Speed Dial via active account, 5 - DialDTMF, 8 - Call Transfer, 9 - CallPark, 10 - Call Intercom, 13 - Multicast Paging, 15 - Speed Conference, 16 - Dial prefix
# Number: 0, 1, 4, 5, 8, 9, 10, 13, 15, 16
P23335=0

# Account. 0 - Account 1, 1 - Account 2, 2 - Account 3, 3 - Account 4, 4 - Account 5, 5 - Account 6
# Number: 0 - 5
P23336=0

# Name
# String
P23337=

# UserID
# String
P23338=

#######################################################################################
# EXT MPK 69
#######################################################################################

# Key Mode.# 0 - Speed Dial, 1 - BLF, 4 - Speed Dial via active account, 5 - DialDTMF, 8 - Call Transfer, 9 - CallPark, 10 - Call Intercom, 13 - Multicast Paging, 15 - Speed Conference, 16 - Dial prefix
# Number: 0, 1, 4, 5, 8, 9, 10, 13, 15, 16
P23340=0

# Account. 0 - Account 1, 1 - Account 2, 2 - Account 3, 3 - Account 4, 4 - Account 5, 5 - Account 6
# Number: 0 - 5
P23341=0

# Name
# String
P23342=

# UserID
# String
P23343=

#######################################################################################
# EXT MPK 70
#######################################################################################

# Key Mode.# 0 - Speed Dial, 1 - BLF, 4 - Speed Dial via active account, 5 - DialDTMF, 8 - Call Transfer, 9 - CallPark, 10 - Call Intercom, 13 - Multicast Paging, 15 - Speed Conference, 16 - Dial prefix
# Number: 0, 1, 4, 5, 8, 9, 10, 13, 15, 16
P23345=0

# Account. 0 - Account 1, 1 - Account 2, 2 - Account 3, 3 - Account 4, 4 - Account 5, 5 - Account 6
# Number: 0 - 5
P23346=0

# Name
# String
P23347=

# UserID
# String
P23348=

#######################################################################################
# EXT MPK 71
#######################################################################################

# Key Mode.# 0 - Speed Dial, 1 - BLF, 4 - Speed Dial via active account, 5 - DialDTMF, 8 - Call Transfer, 9 - CallPark, 10 - Call Intercom, 13 - Multicast Paging, 15 - Speed Conference, 16 - Dial prefix
# Number: 0, 1, 4, 5, 8, 9, 10, 13, 15, 16
P23350=0

# Account. 0 - Account 1, 1 - Account 2, 2 - Account 3, 3 - Account 4, 4 - Account 5, 5 - Account 6
# Number: 0 - 5
P23351=0

# Name
# String
P23352=

# UserID
# String
P23353=

#######################################################################################
# EXT MPK 72
#######################################################################################

# Key Mode.# 0 - Speed Dial, 1 - BLF, 4 - Speed Dial via active account, 5 - DialDTMF, 8 - Call Transfer, 9 - CallPark, 10 - Call Intercom, 13 - Multicast Paging, 15 - Speed Conference, 16 - Dial prefix
# Number: 0, 1, 4, 5, 8, 9, 10, 13, 15, 16
P23355=0

# Account. 0 - Account 1, 1 - Account 2, 2 - Account 3, 3 - Account 4, 4 - Account 5, 5 - Account 6
# Number: 0 - 5
P23356=0

# Name
# String
P23357=

# UserID
# String
P23358=

#######################################################################################
# EXT MPK 73
#######################################################################################

# Key Mode.# 0 - Speed Dial, 1 - BLF, 4 - Speed Dial via active account, 5 - DialDTMF, 8 - Call Transfer, 9 - CallPark, 10 - Call Intercom, 13 - Multicast Paging, 15 - Speed Conference, 16 - Dial prefix
# Number: 0, 1, 4, 5, 8, 9, 10, 13, 15, 16
P23360=0

# Account. 0 - Account 1, 1 - Account 2, 2 - Account 3, 3 - Account 4, 4 - Account 5, 5 - Account 6
# Number: 0 - 5
P23361=0

# Name
# String
P23362=

# UserID
# String
P23363=

#######################################################################################
# EXT MPK 74
#######################################################################################

# Key Mode.# 0 - Speed Dial, 1 - BLF, 4 - Speed Dial via active account, 5 - DialDTMF, 8 - Call Transfer, 9 - CallPark, 10 - Call Intercom, 13 - Multicast Paging, 15 - Speed Conference, 16 - Dial prefix
# Number: 0, 1, 4, 5, 8, 9, 10, 13, 15, 16
P23365=0

# Account. 0 - Account 1, 1 - Account 2, 2 - Account 3, 3 - Account 4, 4 - Account 5, 5 - Account 6
# Number: 0 - 5
P23366=0

# Name
# String
P23367=

# UserID
# String
P23368=

#######################################################################################
# EXT MPK 75
#######################################################################################

# Key Mode.# 0 - Speed Dial, 1 - BLF, 4 - Speed Dial via active account, 5 - DialDTMF, 8 - Call Transfer, 9 - CallPark, 10 - Call Intercom, 13 - Multicast Paging, 15 - Speed Conference, 16 - Dial prefix
# Number: 0, 1, 4, 5, 8, 9, 10, 13, 15, 16
P23370=0

# Account. 0 - Account 1, 1 - Account 2, 2 - Account 3, 3 - Account 4, 4 - Account 5, 5 - Account 6
# Number: 0 - 5
P23371=0

# Name
# String
P23372=

# UserID
# String
P23373=

#######################################################################################
# EXT MPK 76
#######################################################################################

# Key Mode.# 0 - Speed Dial, 1 - BLF, 4 - Speed Dial via active account, 5 - DialDTMF, 8 - Call Transfer, 9 - CallPark, 10 - Call Intercom, 13 - Multicast Paging, 15 - Speed Conference, 16 - Dial prefix
# Number: 0, 1, 4, 5, 8, 9, 10, 13, 15, 16
P23375=0

# Account. 0 - Account 1, 1 - Account 2, 2 - Account 3, 3 - Account 4, 4 - Account 5, 5 - Account 6
# Number: 0 - 5
P23376=0

# Name
# String
P23377=

# UserID
# String
P23378=

#######################################################################################
# EXT MPK 77
#######################################################################################

# Key Mode.# 0 - Speed Dial, 1 - BLF, 4 - Speed Dial via active account, 5 - DialDTMF, 8 - Call Transfer, 9 - CallPark, 10 - Call Intercom, 13 - Multicast Paging, 15 - Speed Conference, 16 - Dial prefix
# Number: 0, 1, 4, 5, 8, 9, 10, 13, 15, 16
P23380=0

# Account. 0 - Account 1, 1 - Account 2, 2 - Account 3, 3 - Account 4, 4 - Account 5, 5 - Account 6
# Number: 0 - 5
P23381=0

# Name
# String
P23382=

# UserID
# String
P23383=

#######################################################################################
# EXT MPK 78
#######################################################################################

# Key Mode.# 0 - Speed Dial, 1 - BLF, 4 - Speed Dial via active account, 5 - DialDTMF, 8 - Call Transfer, 9 - CallPark, 10 - Call Intercom, 13 - Multicast Paging, 15 - Speed Conference, 16 - Dial prefix
# Number: 0, 1, 4, 5, 8, 9, 10, 13, 15, 16
P23385=0

# Account. 0 - Account 1, 1 - Account 2, 2 - Account 3, 3 - Account 4, 4 - Account 5, 5 - Account 6
# Number: 0 - 5
P23386=0

# Name
# String
P23387=

# UserID
# String
P23388=

#######################################################################################
# EXT MPK 79
#######################################################################################

# Key Mode.# 0 - Speed Dial, 1 - BLF, 4 - Speed Dial via active account, 5 - DialDTMF, 8 - Call Transfer, 9 - CallPark, 10 - Call Intercom, 13 - Multicast Paging, 15 - Speed Conference, 16 - Dial prefix
# Number: 0, 1, 4, 5, 8, 9, 10, 13, 15, 16
P23390=0

# Account. 0 - Account 1, 1 - Account 2, 2 - Account 3, 3 - Account 4, 4 - Account 5, 5 - Account 6
# Number: 0 - 5
P23391=0

# Name
# String
P23392=

# UserID
# String
P23393=

#######################################################################################
# EXT MPK 80
#######################################################################################

# Key Mode.# 0 - Speed Dial, 1 - BLF, 4 - Speed Dial via active account, 5 - DialDTMF, 8 - Call Transfer, 9 - CallPark, 10 - Call Intercom, 13 - Multicast Paging, 15 - Speed Conference, 16 - Dial prefix
# Number: 0, 1, 4, 5, 8, 9, 10, 13, 15, 16
P23395=0

# Account. 0 - Account 1, 1 - Account 2, 2 - Account 3, 3 - Account 4, 4 - Account 5, 5 - Account 6
# Number: 0 - 5
P23396=0

# Name
# String
P23397=

# UserID
# String
P23398=

#######################################################################################
# EXT MPK 81
#######################################################################################

# Key Mode.# 0 - Speed Dial, 1 - BLF, 4 - Speed Dial via active account, 5 - DialDTMF, 8 - Call Transfer, 9 - CallPark, 10 - Call Intercom, 13 - Multicast Paging, 15 - Speed Conference, 16 - Dial prefix
# Number: 0, 1, 4, 5, 8, 9, 10, 13, 15, 16
P23400=0

# Account. 0 - Account 1, 1 - Account 2, 2 - Account 3, 3 - Account 4, 4 - Account 5, 5 - Account 6
# Number: 0 - 5
P23401=0

# Name
# String
P23402=

# UserID
# String
P23403=

#######################################################################################
# EXT MPK 82
#######################################################################################

# Key Mode.# 0 - Speed Dial, 1 - BLF, 4 - Speed Dial via active account, 5 - DialDTMF, 8 - Call Transfer, 9 - CallPark, 10 - Call Intercom, 13 - Multicast Paging, 15 - Speed Conference, 16 - Dial prefix
# Number: 0, 1, 4, 5, 8, 9, 10, 13, 15, 16
P23405=0

# Account. 0 - Account 1, 1 - Account 2, 2 - Account 3, 3 - Account 4, 4 - Account 5, 5 - Account 6
# Number: 0 - 5
P23406=0

# Name
# String
P23407=

# UserID
# String
P23408=

#######################################################################################
# EXT MPK 83
#######################################################################################

# Key Mode.# 0 - Speed Dial, 1 - BLF, 4 - Speed Dial via active account, 5 - DialDTMF, 8 - Call Transfer, 9 - CallPark, 10 - Call Intercom, 13 - Multicast Paging, 15 - Speed Conference, 16 - Dial prefix
# Number: 0, 1, 4, 5, 8, 9, 10, 13, 15, 16
P23410=0

# Account. 0 - Account 1, 1 - Account 2, 2 - Account 3, 3 - Account 4, 4 - Account 5, 5 - Account 6
# Number: 0 - 5
P23411=0

# Name
# String
P23412=

# UserID
# String
P23413=

#######################################################################################
# EXT MPK 84
#######################################################################################

# Key Mode.# 0 - Speed Dial, 1 - BLF, 4 - Speed Dial via active account, 5 - DialDTMF, 8 - Call Transfer, 9 - CallPark, 10 - Call Intercom, 13 - Multicast Paging, 15 - Speed Conference, 16 - Dial prefix
# Number: 0, 1, 4, 5, 8, 9, 10, 13, 15, 16
P23415=0

# Account. 0 - Account 1, 1 - Account 2, 2 - Account 3, 3 - Account 4, 4 - Account 5, 5 - Account 6
# Number: 0 - 5
P23416=0

# Name
# String
P23417=

# UserID
# String
P23418=

#######################################################################################
# EXT MPK 85
#######################################################################################

# Key Mode.# 0 - Speed Dial, 1 - BLF, 4 - Speed Dial via active account, 5 - DialDTMF, 8 - Call Transfer, 9 - CallPark, 10 - Call Intercom, 13 - Multicast Paging, 15 - Speed Conference, 16 - Dial prefix
# Number: 0, 1, 4, 5, 8, 9, 10, 13, 15, 16
P23420=0

# Account. 0 - Account 1, 1 - Account 2, 2 - Account 3, 3 - Account 4, 4 - Account 5, 5 - Account 6
# Number: 0 - 5
P23421=0

# Name
# String
P23422=

# UserID
# String
P23423=

#######################################################################################
# EXT MPK 86
#######################################################################################

# Key Mode.# 0 - Speed Dial, 1 - BLF, 4 - Speed Dial via active account, 5 - DialDTMF, 8 - Call Transfer, 9 - CallPark, 10 - Call Intercom, 13 - Multicast Paging, 15 - Speed Conference, 16 - Dial prefix
# Number: 0, 1, 4, 5, 8, 9, 10, 13, 15, 16
P23425=0

# Account. 0 - Account 1, 1 - Account 2, 2 - Account 3, 3 - Account 4, 4 - Account 5, 5 - Account 6
# Number: 0 - 5
P23426=0

# Name
# String
P23427=

# UserID
# String
P23428=

#######################################################################################
# EXT MPK 87
#######################################################################################

# Key Mode.# 0 - Speed Dial, 1 - BLF, 4 - Speed Dial via active account, 5 - DialDTMF, 8 - Call Transfer, 9 - CallPark, 10 - Call Intercom, 13 - Multicast Paging, 15 - Speed Conference, 16 - Dial prefix
# Number: 0, 1, 4, 5, 8, 9, 10, 13, 15, 16
P23430=0

# Account. 0 - Account 1, 1 - Account 2, 2 - Account 3, 3 - Account 4, 4 - Account 5, 5 - Account 6
# Number: 0 - 5
P23431=0

# Name
# String
P23432=

# UserID
# String
P23433=

#######################################################################################
# EXT MPK 88
#######################################################################################

# Key Mode.# 0 - Speed Dial, 1 - BLF, 4 - Speed Dial via active account, 5 - DialDTMF, 8 - Call Transfer, 9 - CallPark, 10 - Call Intercom, 13 - Multicast Paging, 15 - Speed Conference, 16 - Dial prefix
# Number: 0, 1, 4, 5, 8, 9, 10, 13, 15, 16
P23435=0

# Account. 0 - Account 1, 1 - Account 2, 2 - Account 3, 3 - Account 4, 4 - Account 5, 5 - Account 6
# Number: 0 - 5
P23436=0

# Name
# String
P23437=

# UserID
# String
P23438=

#######################################################################################
# EXT MPK 89
#######################################################################################

# Key Mode.# 0 - Speed Dial, 1 - BLF, 4 - Speed Dial via active account, 5 - DialDTMF, 8 - Call Transfer, 9 - CallPark, 10 - Call Intercom, 13 - Multicast Paging, 15 - Speed Conference, 16 - Dial prefix
# Number: 0, 1, 4, 5, 8, 9, 10, 13, 15, 16
P23440=0

# Account. 0 - Account 1, 1 - Account 2, 2 - Account 3, 3 - Account 4, 4 - Account 5, 5 - Account 6
# Number: 0 - 5
P23441=0

# Name
# String
P23442=

# UserID
# String
P23443=

#######################################################################################
# EXT MPK 90
#######################################################################################

# Key Mode.# 0 - Speed Dial, 1 - BLF, 4 - Speed Dial via active account, 5 - DialDTMF, 8 - Call Transfer, 9 - CallPark, 10 - Call Intercom, 13 - Multicast Paging, 15 - Speed Conference, 16 - Dial prefix
# Number: 0, 1, 4, 5, 8, 9, 10, 13, 15, 16
P23445=0

# Account. 0 - Account 1, 1 - Account 2, 2 - Account 3, 3 - Account 4, 4 - Account 5, 5 - Account 6
# Number: 0 - 5
P23446=0

# Name
# String
P23447=

# UserID
# String
P23448=

#######################################################################################
# EXT MPK 91
#######################################################################################

# Key Mode.# 0 - Speed Dial, 1 - BLF, 4 - Speed Dial via active account, 5 - DialDTMF, 8 - Call Transfer, 9 - CallPark, 10 - Call Intercom, 13 - Multicast Paging, 15 - Speed Conference, 16 - Dial prefix
# Number: 0, 1, 4, 5, 8, 9, 10, 13, 15, 16
P23450=0

# Account. 0 - Account 1, 1 - Account 2, 2 - Account 3, 3 - Account 4, 4 - Account 5, 5 - Account 6
# Number: 0 - 5
P23451=0

# Name
# String
P23452=

# UserID
# String
P23453=

#######################################################################################
# EXT MPK 92
#######################################################################################

# Key Mode.# 0 - Speed Dial, 1 - BLF, 4 - Speed Dial via active account, 5 - DialDTMF, 8 - Call Transfer, 9 - CallPark, 10 - Call Intercom, 13 - Multicast Paging, 15 - Speed Conference, 16 - Dial prefix
# Number: 0, 1, 4, 5, 8, 9, 10, 13, 15, 16
P23455=0

# Account. 0 - Account 1, 1 - Account 2, 2 - Account 3, 3 - Account 4, 4 - Account 5, 5 - Account 6
# Number: 0 - 5
P23456=0

# Name
# String
P23457=

# UserID
# String
P23458=

#######################################################################################
# EXT MPK 93
#######################################################################################

# Key Mode.# 0 - Speed Dial, 1 - BLF, 4 - Speed Dial via active account, 5 - DialDTMF, 8 - Call Transfer, 9 - CallPark, 10 - Call Intercom, 13 - Multicast Paging, 15 - Speed Conference, 16 - Dial prefix
# Number: 0, 1, 4, 5, 8, 9, 10, 13, 15, 16
P23460=0

# Account. 0 - Account 1, 1 - Account 2, 2 - Account 3, 3 - Account 4, 4 - Account 5, 5 - Account 6
# Number: 0 - 5
P23461=0

# Name
# String
P23462=

# UserID
# String
P23463=

#######################################################################################
# EXT MPK 94
#######################################################################################

# Key Mode.# 0 - Speed Dial, 1 - BLF, 4 - Speed Dial via active account, 5 - DialDTMF, 8 - Call Transfer, 9 - CallPark, 10 - Call Intercom, 13 - Multicast Paging, 15 - Speed Conference, 16 - Dial prefix
# Number: 0, 1, 4, 5, 8, 9, 10, 13, 15, 16
P23465=0

# Account. 0 - Account 1, 1 - Account 2, 2 - Account 3, 3 - Account 4, 4 - Account 5, 5 - Account 6
# Number: 0 - 5
P23466=0

# Name
# String
P23467=

# UserID
# String
P23468=

#######################################################################################
# EXT MPK 95
#######################################################################################

# Key Mode.# 0 - Speed Dial, 1 - BLF, 4 - Speed Dial via active account, 5 - DialDTMF, 8 - Call Transfer, 9 - CallPark, 10 - Call Intercom, 13 - Multicast Paging, 15 - Speed Conference, 16 - Dial prefix
# Number: 0, 1, 4, 5, 8, 9, 10, 13, 15, 16
P23470=0

# Account. 0 - Account 1, 1 - Account 2, 2 - Account 3, 3 - Account 4, 4 - Account 5, 5 - Account 6
# Number: 0 - 5
P23471=0

# Name
# String
P23472=

# UserID
# String
P23473=

#######################################################################################
# EXT MPK 96
#######################################################################################

# Key Mode.# 0 - Speed Dial, 1 - BLF, 4 - Speed Dial via active account, 5 - DialDTMF, 8 - Call Transfer, 9 - CallPark, 10 - Call Intercom, 13 - Multicast Paging, 15 - Speed Conference, 16 - Dial prefix
# Number: 0, 1, 4, 5, 8, 9, 10, 13, 15, 16
P23475=0

# Account. 0 - Account 1, 1 - Account 2, 2 - Account 3, 3 - Account 4, 4 - Account 5, 5 - Account 6
# Number: 0 - 5
P23476=0

# Name
# String
P23477=

# UserID
# String
P23478=

#######################################################################################
# EXT MPK 97
#######################################################################################

# Key Mode.# 0 - Speed Dial, 1 - BLF, 4 - Speed Dial via active account, 5 - DialDTMF, 8 - Call Transfer, 9 - CallPark, 10 - Call Intercom, 13 - Multicast Paging, 15 - Speed Conference, 16 - Dial prefix
# Number: 0, 1, 4, 5, 8, 9, 10, 13, 15, 16
P23480=0

# Account. 0 - Account 1, 1 - Account 2, 2 - Account 3, 3 - Account 4, 4 - Account 5, 5 - Account 6
# Number: 0 - 5
P23481=0

# Name
# String
P23482=

# UserID
# String
P23483=

#######################################################################################
# EXT MPK 98
#######################################################################################

# Key Mode.# 0 - Speed Dial, 1 - BLF, 4 - Speed Dial via active account, 5 - DialDTMF, 8 - Call Transfer, 9 - CallPark, 10 - Call Intercom, 13 - Multicast Paging, 15 - Speed Conference, 16 - Dial prefix
# Number: 0, 1, 4, 5, 8, 9, 10, 13, 15, 16
P23485=0

# Account. 0 - Account 1, 1 - Account 2, 2 - Account 3, 3 - Account 4, 4 - Account 5, 5 - Account 6
# Number: 0 - 5
P23486=0

# Name
# String
P23487=

# UserID
# String
P23488=

#######################################################################################
# EXT MPK 99
#######################################################################################

# Key Mode.# 0 - Speed Dial, 1 - BLF, 4 - Speed Dial via active account, 5 - DialDTMF, 8 - Call Transfer, 9 - CallPark, 10 - Call Intercom, 13 - Multicast Paging, 15 - Speed Conference, 16 - Dial prefix
# Number: 0, 1, 4, 5, 8, 9, 10, 13, 15, 16
P23490=0

# Account. 0 - Account 1, 1 - Account 2, 2 - Account 3, 3 - Account 4, 4 - Account 5, 5 - Account 6
# Number: 0 - 5
P23491=0

# Name
# String
P23492=

# UserID
# String
P23493=

#######################################################################################
# EXT MPK 100
#######################################################################################

# Key Mode.# 0 - Speed Dial, 1 - BLF, 4 - Speed Dial via active account, 5 - DialDTMF, 8 - Call Transfer, 9 - CallPark, 10 - Call Intercom, 13 - Multicast Paging, 15 - Speed Conference, 16 - Dial prefix
# Number: 0, 1, 4, 5, 8, 9, 10, 13, 15, 16
P23495=0

# Account. 0 - Account 1, 1 - Account 2, 2 - Account 3, 3 - Account 4, 4 - Account 5, 5 - Account 6
# Number: 0 - 5
P23496=0

# Name
# String
P23497=

# UserID
# String
P23498=

#######################################################################################
# EXT MPK 101
#######################################################################################

# Key Mode.# 0 - Speed Dial, 1 - BLF, 4 - Speed Dial via active account, 5 - DialDTMF, 8 - Call Transfer, 9 - CallPark, 10 - Call Intercom, 13 - Multicast Paging, 15 - Speed Conference, 16 - Dial prefix
# Number: 0, 1, 4, 5, 8, 9, 10, 13, 15, 16
P23500=0

# Account. 0 - Account 1, 1 - Account 2, 2 - Account 3, 3 - Account 4, 4 - Account 5, 5 - Account 6
# Number: 0 - 5
P23501=0

# Name
# String
P23502=

# UserID
# String
P23503=

#######################################################################################
# EXT MPK 102
#######################################################################################

# Key Mode.# 0 - Speed Dial, 1 - BLF, 4 - Speed Dial via active account, 5 - DialDTMF, 8 - Call Transfer, 9 - CallPark, 10 - Call Intercom, 13 - Multicast Paging, 15 - Speed Conference, 16 - Dial prefix
# Number: 0, 1, 4, 5, 8, 9, 10, 13, 15, 16
P23505=0

# Account. 0 - Account 1, 1 - Account 2, 2 - Account 3, 3 - Account 4, 4 - Account 5, 5 - Account 6
# Number: 0 - 5
P23506=0

# Name
# String
P23507=

# UserID
# String
P23508=

#######################################################################################
# EXT MPK 103
#######################################################################################

# Key Mode.# 0 - Speed Dial, 1 - BLF, 4 - Speed Dial via active account, 5 - DialDTMF, 8 - Call Transfer, 9 - CallPark, 10 - Call Intercom, 13 - Multicast Paging, 15 - Speed Conference, 16 - Dial prefix
# Number: 0, 1, 4, 5, 8, 9, 10, 13, 15, 16
P23510=0

# Account. 0 - Account 1, 1 - Account 2, 2 - Account 3, 3 - Account 4, 4 - Account 5, 5 - Account 6
# Number: 0 - 5
P23511=0

# Name
# String
P23512=

# UserID
# String
P23513=

#######################################################################################
# EXT MPK 104
#######################################################################################

# Key Mode.# 0 - Speed Dial, 1 - BLF, 4 - Speed Dial via active account, 5 - DialDTMF, 8 - Call Transfer, 9 - CallPark, 10 - Call Intercom, 13 - Multicast Paging, 15 - Speed Conference, 16 - Dial prefix
# Number: 0, 1, 4, 5, 8, 9, 10, 13, 15, 16
P23515=0

# Account. 0 - Account 1, 1 - Account 2, 2 - Account 3, 3 - Account 4, 4 - Account 5, 5 - Account 6
# Number: 0 - 5
P23516=0

# Name
# String
P23517=

# UserID
# String
P23518=

#######################################################################################
# EXT MPK 105
#######################################################################################

# Key Mode.# 0 - Speed Dial, 1 - BLF, 4 - Speed Dial via active account, 5 - DialDTMF, 8 - Call Transfer, 9 - CallPark, 10 - Call Intercom, 13 - Multicast Paging, 15 - Speed Conference, 16 - Dial prefix
# Number: 0, 1, 4, 5, 8, 9, 10, 13, 15, 16
P23520=0

# Account. 0 - Account 1, 1 - Account 2, 2 - Account 3, 3 - Account 4, 4 - Account 5, 5 - Account 6
# Number: 0 - 5
P23521=0

# Name
# String
P23522=

# UserID
# String
P23523=

#######################################################################################
# EXT MPK 106
#######################################################################################

# Key Mode.# 0 - Speed Dial, 1 - BLF, 4 - Speed Dial via active account, 5 - DialDTMF, 8 - Call Transfer, 9 - CallPark, 10 - Call Intercom, 13 - Multicast Paging, 15 - Speed Conference, 16 - Dial prefix
# Number: 0, 1, 4, 5, 8, 9, 10, 13, 15, 16
P23525=0

# Account. 0 - Account 1, 1 - Account 2, 2 - Account 3, 3 - Account 4, 4 - Account 5, 5 - Account 6
# Number: 0 - 5
P23526=0

# Name
# String
P23527=

# UserID
# String
P23528=

#######################################################################################
# EXT MPK 107
#######################################################################################

# Key Mode.# 0 - Speed Dial, 1 - BLF, 4 - Speed Dial via active account, 5 - DialDTMF, 8 - Call Transfer, 9 - CallPark, 10 - Call Intercom, 13 - Multicast Paging, 15 - Speed Conference, 16 - Dial prefix
# Number: 0, 1, 4, 5, 8, 9, 10, 13, 15, 16
P23530=0

# Account. 0 - Account 1, 1 - Account 2, 2 - Account 3, 3 - Account 4, 4 - Account 5, 5 - Account 6
# Number: 0 - 5
P23531=0

# Name
# String
P23532=

# UserID
# String
P23533=

#######################################################################################
# EXT MPK 108
#######################################################################################

# Key Mode.# 0 - Speed Dial, 1 - BLF, 4 - Speed Dial via active account, 5 - DialDTMF, 8 - Call Transfer, 9 - CallPark, 10 - Call Intercom, 13 - Multicast Paging, 15 - Speed Conference, 16 - Dial prefix
# Number: 0, 1, 4, 5, 8, 9, 10, 13, 15, 16
P23535=0

# Account. 0 - Account 1, 1 - Account 2, 2 - Account 3, 3 - Account 4, 4 - Account 5, 5 - Account 6
# Number: 0 - 5
P23536=0

# Name
# String
P23537=

# UserID
# String
P23538=

#######################################################################################
# EXT MPK 109
#######################################################################################

# Key Mode.# 0 - Speed Dial, 1 - BLF, 4 - Speed Dial via active account, 5 - DialDTMF, 8 - Call Transfer, 9 - CallPark, 10 - Call Intercom, 13 - Multicast Paging, 15 - Speed Conference, 16 - Dial prefix
# Number: 0, 1, 4, 5, 8, 9, 10, 13, 15, 16
P23540=0

# Account. 0 - Account 1, 1 - Account 2, 2 - Account 3, 3 - Account 4, 4 - Account 5, 5 - Account 6
# Number: 0 - 5
P23541=0

# Name
# String
P23542=

# UserID
# String
P23543=

#######################################################################################
# EXT MPK 110
#######################################################################################

# Key Mode.# 0 - Speed Dial, 1 - BLF, 4 - Speed Dial via active account, 5 - DialDTMF, 8 - Call Transfer, 9 - CallPark, 10 - Call Intercom, 13 - Multicast Paging, 15 - Speed Conference, 16 - Dial prefix
# Number: 0, 1, 4, 5, 8, 9, 10, 13, 15, 16
P23545=0

# Account. 0 - Account 1, 1 - Account 2, 2 - Account 3, 3 - Account 4, 4 - Account 5, 5 - Account 6
# Number: 0 - 5
P23546=0

# Name
# String
P23547=

# UserID
# String
P23548=

#######################################################################################
# EXT MPK 111
#######################################################################################

# Key Mode.# 0 - Speed Dial, 1 - BLF, 4 - Speed Dial via active account, 5 - DialDTMF, 8 - Call Transfer, 9 - CallPark, 10 - Call Intercom, 13 - Multicast Paging, 15 - Speed Conference, 16 - Dial prefix
# Number: 0, 1, 4, 5, 8, 9, 10, 13, 15, 16
P23550=0

# Account. 0 - Account 1, 1 - Account 2, 2 - Account 3, 3 - Account 4, 4 - Account 5, 5 - Account 6
# Number: 0 - 5
P23551=0

# Name
# String
P23552=

# UserID
# String
P23553=

#######################################################################################
# EXT MPK 112
#######################################################################################

# Key Mode.# 0 - Speed Dial, 1 - BLF, 4 - Speed Dial via active account, 5 - DialDTMF, 8 - Call Transfer, 9 - CallPark, 10 - Call Intercom, 13 - Multicast Paging, 15 - Speed Conference, 16 - Dial prefix
# Number: 0, 1, 4, 5, 8, 9, 10, 13, 15, 16
P23555=0

# Account. 0 - Account 1, 1 - Account 2, 2 - Account 3, 3 - Account 4, 4 - Account 5, 5 - Account 6
# Number: 0 - 5
P23556=0

# Name
# String
P23557=

# UserID
# String
P23558=

#######################################################################################
# EXT MPK 113
#######################################################################################

# Key Mode.# 0 - Speed Dial, 1 - BLF, 4 - Speed Dial via active account, 5 - DialDTMF, 8 - Call Transfer, 9 - CallPark, 10 - Call Intercom, 13 - Multicast Paging, 15 - Speed Conference, 16 - Dial prefix
# Number: 0, 1, 4, 5, 8, 9, 10, 13, 15, 16
P23560=0

# Account. 0 - Account 1, 1 - Account 2, 2 - Account 3, 3 - Account 4, 4 - Account 5, 5 - Account 6
# Number: 0 - 5
P23561=0

# Name
# String
P23562=

# UserID
# String
P23563=

#######################################################################################
# EXT MPK 114
#######################################################################################

# Key Mode.# 0 - Speed Dial, 1 - BLF, 4 - Speed Dial via active account, 5 - DialDTMF, 8 - Call Transfer, 9 - CallPark, 10 - Call Intercom, 13 - Multicast Paging, 15 - Speed Conference, 16 - Dial prefix
# Number: 0, 1, 4, 5, 8, 9, 10, 13, 15, 16
P23565=0

# Account. 0 - Account 1, 1 - Account 2, 2 - Account 3, 3 - Account 4, 4 - Account 5, 5 - Account 6
# Number: 0 - 5
P23566=0

# Name
# String
P23567=

# UserID
# String
P23568=

#######################################################################################
# EXT MPK 115
#######################################################################################

# Key Mode.# 0 - Speed Dial, 1 - BLF, 4 - Speed Dial via active account, 5 - DialDTMF, 8 - Call Transfer, 9 - CallPark, 10 - Call Intercom, 13 - Multicast Paging, 15 - Speed Conference, 16 - Dial prefix
# Number: 0, 1, 4, 5, 8, 9, 10, 13, 15, 16
P23570=0

# Account. 0 - Account 1, 1 - Account 2, 2 - Account 3, 3 - Account 4, 4 - Account 5, 5 - Account 6
# Number: 0 - 5
P23571=0

# Name
# String
P23572=

# UserID
# String
P23573=

#######################################################################################
# EXT MPK 116
#######################################################################################

# Key Mode.# 0 - Speed Dial, 1 - BLF, 4 - Speed Dial via active account, 5 - DialDTMF, 8 - Call Transfer, 9 - CallPark, 10 - Call Intercom, 13 - Multicast Paging, 15 - Speed Conference, 16 - Dial prefix
# Number: 0, 1, 4, 5, 8, 9, 10, 13, 15, 16
P23575=0

# Account. 0 - Account 1, 1 - Account 2, 2 - Account 3, 3 - Account 4, 4 - Account 5, 5 - Account 6
# Number: 0 - 5
P23576=0

# Name
# String
P23577=

# UserID
# String
P23578=

#######################################################################################
# EXT MPK 117
#######################################################################################

# Key Mode.# 0 - Speed Dial, 1 - BLF, 4 - Speed Dial via active account, 5 - DialDTMF, 8 - Call Transfer, 9 - CallPark, 10 - Call Intercom, 13 - Multicast Paging, 15 - Speed Conference, 16 - Dial prefix
# Number: 0, 1, 4, 5, 8, 9, 10, 13, 15, 16
P23580=0

# Account. 0 - Account 1, 1 - Account 2, 2 - Account 3, 3 - Account 4, 4 - Account 5, 5 - Account 6
# Number: 0 - 5
P23581=0

# Name
# String
P23582=

# UserID
# String
P23583=

#######################################################################################
# EXT MPK 118
#######################################################################################

# Key Mode.# 0 - Speed Dial, 1 - BLF, 4 - Speed Dial via active account, 5 - DialDTMF, 8 - Call Transfer, 9 - CallPark, 10 - Call Intercom, 13 - Multicast Paging, 15 - Speed Conference, 16 - Dial prefix
# Number: 0, 1, 4, 5, 8, 9, 10, 13, 15, 16
P23585=0

# Account. 0 - Account 1, 1 - Account 2, 2 - Account 3, 3 - Account 4, 4 - Account 5, 5 - Account 6
# Number: 0 - 5
P23586=0

# Name
# String
P23587=

# UserID
# String
P23588=

#######################################################################################
# EXT MPK 119
#######################################################################################

# Key Mode.# 0 - Speed Dial, 1 - BLF, 4 - Speed Dial via active account, 5 - DialDTMF, 8 - Call Transfer, 9 - CallPark, 10 - Call Intercom, 13 - Multicast Paging, 15 - Speed Conference, 16 - Dial prefix
# Number: 0, 1, 4, 5, 8, 9, 10, 13, 15, 16
P23590=0

# Account. 0 - Account 1, 1 - Account 2, 2 - Account 3, 3 - Account 4, 4 - Account 5, 5 - Account 6
# Number: 0 - 5
P23591=0

# Name
# String
P23592=

# UserID
# String
P23593=

#######################################################################################
# EXT MPK 120
#######################################################################################

# Key Mode.# 0 - Speed Dial, 1 - BLF, 4 - Speed Dial via active account, 5 - DialDTMF, 8 - Call Transfer, 9 - CallPark, 10 - Call Intercom, 13 - Multicast Paging, 15 - Speed Conference, 16 - Dial prefix
# Number: 0, 1, 4, 5, 8, 9, 10, 13, 15, 16
P23595=0

# Account. 0 - Account 1, 1 - Account 2, 2 - Account 3, 3 - Account 4, 4 - Account 5, 5 - Account 6
# Number: 0 - 5
P23596=0

# Name
# String
P23597=

# UserID
# String
P23598=

#######################################################################################
# EXT MPK 121
#######################################################################################

# Key Mode.# 0 - Speed Dial, 1 - BLF, 4 - Speed Dial via active account, 5 - DialDTMF, 8 - Call Transfer, 9 - CallPark, 10 - Call Intercom, 13 - Multicast Paging, 15 - Speed Conference, 16 - Dial prefix
# Number: 0, 1, 4, 5, 8, 9, 10, 13, 15, 16
P23600=0

# Account. 0 - Account 1, 1 - Account 2, 2 - Account 3, 3 - Account 4, 4 - Account 5, 5 - Account 6
# Number: 0 - 5
P23601=0

# Name
# String
P23602=

# UserID
# String
P23603=

#######################################################################################
# EXT MPK 122
#######################################################################################

# Key Mode.# 0 - Speed Dial, 1 - BLF, 4 - Speed Dial via active account, 5 - DialDTMF, 8 - Call Transfer, 9 - CallPark, 10 - Call Intercom, 13 - Multicast Paging, 15 - Speed Conference, 16 - Dial prefix
# Number: 0, 1, 4, 5, 8, 9, 10, 13, 15, 16
P23605=0

# Account. 0 - Account 1, 1 - Account 2, 2 - Account 3, 3 - Account 4, 4 - Account 5, 5 - Account 6
# Number: 0 - 5
P23606=0

# Name
# String
P23607=

# UserID
# String
P23608=

#######################################################################################
# EXT MPK 123
#######################################################################################

# Key Mode.# 0 - Speed Dial, 1 - BLF, 4 - Speed Dial via active account, 5 - DialDTMF, 8 - Call Transfer, 9 - CallPark, 10 - Call Intercom, 13 - Multicast Paging, 15 - Speed Conference, 16 - Dial prefix
# Number: 0, 1, 4, 5, 8, 9, 10, 13, 15, 16
P23610=0

# Account. 0 - Account 1, 1 - Account 2, 2 - Account 3, 3 - Account 4, 4 - Account 5, 5 - Account 6
# Number: 0 - 5
P23611=0

# Name
# String
P23612=

# UserID
# String
P23613=

#######################################################################################
# EXT MPK 124
#######################################################################################

# Key Mode.# 0 - Speed Dial, 1 - BLF, 4 - Speed Dial via active account, 5 - DialDTMF, 8 - Call Transfer, 9 - CallPark, 10 - Call Intercom, 13 - Multicast Paging, 15 - Speed Conference, 16 - Dial prefix
# Number: 0, 1, 4, 5, 8, 9, 10, 13, 15, 16
P23615=0

# Account. 0 - Account 1, 1 - Account 2, 2 - Account 3, 3 - Account 4, 4 - Account 5, 5 - Account 6
# Number: 0 - 5
P23616=0

# Name
# String
P23617=

# UserID
# String
P23618=

#######################################################################################
# EXT MPK 125
#######################################################################################

# Key Mode.# 0 - Speed Dial, 1 - BLF, 4 - Speed Dial via active account, 5 - DialDTMF, 8 - Call Transfer, 9 - CallPark, 10 - Call Intercom, 13 - Multicast Paging, 15 - Speed Conference, 16 - Dial prefix
# Number: 0, 1, 4, 5, 8, 9, 10, 13, 15, 16
P23620=0

# Account. 0 - Account 1, 1 - Account 2, 2 - Account 3, 3 - Account 4, 4 - Account 5, 5 - Account 6
# Number: 0 - 5
P23621=0

# Name
# String
P23622=

# UserID
# String
P23623=

#######################################################################################
# EXT MPK 126
#######################################################################################

# Key Mode.# 0 - Speed Dial, 1 - BLF, 4 - Speed Dial via active account, 5 - DialDTMF, 8 - Call Transfer, 9 - CallPark, 10 - Call Intercom, 13 - Multicast Paging, 15 - Speed Conference, 16 - Dial prefix
# Number: 0, 1, 4, 5, 8, 9, 10, 13, 15, 16
P23625=0

# Account. 0 - Account 1, 1 - Account 2, 2 - Account 3, 3 - Account 4, 4 - Account 5, 5 - Account 6
# Number: 0 - 5
P23626=0

# Name
# String
P23627=

# UserID
# String
P23628=

#######################################################################################
# EXT MPK 127
#######################################################################################

# Key Mode.# 0 - Speed Dial, 1 - BLF, 4 - Speed Dial via active account, 5 - DialDTMF, 8 - Call Transfer, 9 - CallPark, 10 - Call Intercom, 13 - Multicast Paging, 15 - Speed Conference, 16 - Dial prefix
# Number: 0, 1, 4, 5, 8, 9, 10, 13, 15, 16
P23630=0

# Account. 0 - Account 1, 1 - Account 2, 2 - Account 3, 3 - Account 4, 4 - Account 5, 5 - Account 6
# Number: 0 - 5
P23631=0

# Name
# String
P23632=

# UserID
# String
P23633=

#######################################################################################
# EXT MPK 128
#######################################################################################

# Key Mode.# 0 - Speed Dial, 1 - BLF, 4 - Speed Dial via active account, 5 - DialDTMF, 8 - Call Transfer, 9 - CallPark, 10 - Call Intercom, 13 - Multicast Paging, 15 - Speed Conference, 16 - Dial prefix
# Number: 0, 1, 4, 5, 8, 9, 10, 13, 15, 16
P23635=0

# Account. 0 - Account 1, 1 - Account 2, 2 - Account 3, 3 - Account 4, 4 - Account 5, 5 - Account 6
# Number: 0 - 5
P23636=0

# Name
# String
P23637=

# UserID
# String
P23638=

#######################################################################################
# EXT MPK 129
#######################################################################################

# Key Mode.# 0 - Speed Dial, 1 - BLF, 4 - Speed Dial via active account, 5 - DialDTMF, 8 - Call Transfer, 9 - CallPark, 10 - Call Intercom, 13 - Multicast Paging, 15 - Speed Conference, 16 - Dial prefix
# Number: 0, 1, 4, 5, 8, 9, 10, 13, 15, 16
P23640=0

# Account. 0 - Account 1, 1 - Account 2, 2 - Account 3, 3 - Account 4, 4 - Account 5, 5 - Account 6
# Number: 0 - 5
P23641=0

# Name
# String
P23642=

# UserID
# String
P23643=

#######################################################################################
# EXT MPK 130
#######################################################################################

# Key Mode.# 0 - Speed Dial, 1 - BLF, 4 - Speed Dial via active account, 5 - DialDTMF, 8 - Call Transfer, 9 - CallPark, 10 - Call Intercom, 13 - Multicast Paging, 15 - Speed Conference, 16 - Dial prefix
# Number: 0, 1, 4, 5, 8, 9, 10, 13, 15, 16
P23645=0

# Account. 0 - Account 1, 1 - Account 2, 2 - Account 3, 3 - Account 4, 4 - Account 5, 5 - Account 6
# Number: 0 - 5
P23646=0

# Name
# String
P23647=

# UserID
# String
P23648=

#######################################################################################
# EXT MPK 131
#######################################################################################

# Key Mode.# 0 - Speed Dial, 1 - BLF, 4 - Speed Dial via active account, 5 - DialDTMF, 8 - Call Transfer, 9 - CallPark, 10 - Call Intercom, 13 - Multicast Paging, 15 - Speed Conference, 16 - Dial prefix
# Number: 0, 1, 4, 5, 8, 9, 10, 13, 15, 16
P23650=0

# Account. 0 - Account 1, 1 - Account 2, 2 - Account 3, 3 - Account 4, 4 - Account 5, 5 - Account 6
# Number: 0 - 5
P23651=0

# Name
# String
P23652=

# UserID
# String
P23653=

#######################################################################################
# EXT MPK 132
#######################################################################################

# Key Mode.# 0 - Speed Dial, 1 - BLF, 4 - Speed Dial via active account, 5 - DialDTMF, 8 - Call Transfer, 9 - CallPark, 10 - Call Intercom, 13 - Multicast Paging, 15 - Speed Conference, 16 - Dial prefix
# Number: 0, 1, 4, 5, 8, 9, 10, 13, 15, 16
P23655=0

# Account. 0 - Account 1, 1 - Account 2, 2 - Account 3, 3 - Account 4, 4 - Account 5, 5 - Account 6
# Number: 0 - 5
P23656=0

# Name
# String
P23657=

# UserID
# String
P23658=

#######################################################################################
# EXT MPK 133
#######################################################################################

# Key Mode.# 0 - Speed Dial, 1 - BLF, 4 - Speed Dial via active account, 5 - DialDTMF, 8 - Call Transfer, 9 - CallPark, 10 - Call Intercom, 13 - Multicast Paging, 15 - Speed Conference, 16 - Dial prefix
# Number: 0, 1, 4, 5, 8, 9, 10, 13, 15, 16
P23660=0

# Account. 0 - Account 1, 1 - Account 2, 2 - Account 3, 3 - Account 4, 4 - Account 5, 5 - Account 6
# Number: 0 - 5
P23661=0

# Name
# String
P23662=

# UserID
# String
P23663=

#######################################################################################
# EXT MPK 134
#######################################################################################

# Key Mode.# 0 - Speed Dial, 1 - BLF, 4 - Speed Dial via active account, 5 - DialDTMF, 8 - Call Transfer, 9 - CallPark, 10 - Call Intercom, 13 - Multicast Paging, 15 - Speed Conference, 16 - Dial prefix
# Number: 0, 1, 4, 5, 8, 9, 10, 13, 15, 16
P23665=0

# Account. 0 - Account 1, 1 - Account 2, 2 - Account 3, 3 - Account 4, 4 - Account 5, 5 - Account 6
# Number: 0 - 5
P23666=0

# Name
# String
P23667=

# UserID
# String
P23668=

#######################################################################################
# EXT MPK 135
#######################################################################################

# Key Mode.# 0 - Speed Dial, 1 - BLF, 4 - Speed Dial via active account, 5 - DialDTMF, 8 - Call Transfer, 9 - CallPark, 10 - Call Intercom, 13 - Multicast Paging, 15 - Speed Conference, 16 - Dial prefix
# Number: 0, 1, 4, 5, 8, 9, 10, 13, 15, 16
P23670=0

# Account. 0 - Account 1, 1 - Account 2, 2 - Account 3, 3 - Account 4, 4 - Account 5, 5 - Account 6
# Number: 0 - 5
P23671=0

# Name
# String
P23672=

# UserID
# String
P23673=

#######################################################################################
# EXT MPK 136
#######################################################################################

# Key Mode.# 0 - Speed Dial, 1 - BLF, 4 - Speed Dial via active account, 5 - DialDTMF, 8 - Call Transfer, 9 - CallPark, 10 - Call Intercom, 13 - Multicast Paging, 15 - Speed Conference, 16 - Dial prefix
# Number: 0, 1, 4, 5, 8, 9, 10, 13, 15, 16
P23675=0

# Account. 0 - Account 1, 1 - Account 2, 2 - Account 3, 3 - Account 4, 4 - Account 5, 5 - Account 6
# Number: 0 - 5
P23676=0

# Name
# String
P23677=

# UserID
# String
P23678=

#######################################################################################
# EXT MPK 137
#######################################################################################

# Key Mode.# 0 - Speed Dial, 1 - BLF, 4 - Speed Dial via active account, 5 - DialDTMF, 8 - Call Transfer, 9 - CallPark, 10 - Call Intercom, 13 - Multicast Paging, 15 - Speed Conference, 16 - Dial prefix
# Number: 0, 1, 4, 5, 8, 9, 10, 13, 15, 16
P23680=0

# Account. 0 - Account 1, 1 - Account 2, 2 - Account 3, 3 - Account 4, 4 - Account 5, 5 - Account 6
# Number: 0 - 5
P23681=0

# Name
# String
P23682=

# UserID
# String
P23683=

#######################################################################################
# EXT MPK 138
#######################################################################################

# Key Mode.# 0 - Speed Dial, 1 - BLF, 4 - Speed Dial via active account, 5 - DialDTMF, 8 - Call Transfer, 9 - CallPark, 10 - Call Intercom, 13 - Multicast Paging, 15 - Speed Conference, 16 - Dial prefix
# Number: 0, 1, 4, 5, 8, 9, 10, 13, 15, 16
P23685=0

# Account. 0 - Account 1, 1 - Account 2, 2 - Account 3, 3 - Account 4, 4 - Account 5, 5 - Account 6
# Number: 0 - 5
P23686=0

# Name
# String
P23687=

# UserID
# String
P23688=

#######################################################################################
# EXT MPK 139
#######################################################################################

# Key Mode.# 0 - Speed Dial, 1 - BLF, 4 - Speed Dial via active account, 5 - DialDTMF, 8 - Call Transfer, 9 - CallPark, 10 - Call Intercom, 13 - Multicast Paging, 15 - Speed Conference, 16 - Dial prefix
# Number: 0, 1, 4, 5, 8, 9, 10, 13, 15, 16
P23690=0

# Account. 0 - Account 1, 1 - Account 2, 2 - Account 3, 3 - Account 4, 4 - Account 5, 5 - Account 6
# Number: 0 - 5
P23691=0

# Name
# String
P23692=

# UserID
# String
P23693=

#######################################################################################
# EXT MPK 140
#######################################################################################

# Key Mode.# 0 - Speed Dial, 1 - BLF, 4 - Speed Dial via active account, 5 - DialDTMF, 8 - Call Transfer, 9 - CallPark, 10 - Call Intercom, 13 - Multicast Paging, 15 - Speed Conference, 16 - Dial prefix
# Number: 0, 1, 4, 5, 8, 9, 10, 13, 15, 16
P23695=0

# Account. 0 - Account 1, 1 - Account 2, 2 - Account 3, 3 - Account 4, 4 - Account 5, 5 - Account 6
# Number: 0 - 5
P23696=0

# Name
# String
P23697=

# UserID
# String
P23698=

#######################################################################################
# EXT MPK 141
#######################################################################################

# Key Mode.# 0 - Speed Dial, 1 - BLF, 4 - Speed Dial via active account, 5 - DialDTMF, 8 - Call Transfer, 9 - CallPark, 10 - Call Intercom, 13 - Multicast Paging, 15 - Speed Conference, 16 - Dial prefix
# Number: 0, 1, 4, 5, 8, 9, 10, 13, 15, 16
P23700=0

# Account. 0 - Account 1, 1 - Account 2, 2 - Account 3, 3 - Account 4, 4 - Account 5, 5 - Account 6
# Number: 0 - 5
P23701=0

# Name
# String
P23702=

# UserID
# String
P23703=

#######################################################################################
# EXT MPK 142
#######################################################################################

# Key Mode.# 0 - Speed Dial, 1 - BLF, 4 - Speed Dial via active account, 5 - DialDTMF, 8 - Call Transfer, 9 - CallPark, 10 - Call Intercom, 13 - Multicast Paging, 15 - Speed Conference, 16 - Dial prefix
# Number: 0, 1, 4, 5, 8, 9, 10, 13, 15, 16
P23705=0

# Account. 0 - Account 1, 1 - Account 2, 2 - Account 3, 3 - Account 4, 4 - Account 5, 5 - Account 6
# Number: 0 - 5
P23706=0

# Name
# String
P23707=

# UserID
# String
P23708=

#######################################################################################
# EXT MPK 143
#######################################################################################

# Key Mode.# 0 - Speed Dial, 1 - BLF, 4 - Speed Dial via active account, 5 - DialDTMF, 8 - Call Transfer, 9 - CallPark, 10 - Call Intercom, 13 - Multicast Paging, 15 - Speed Conference, 16 - Dial prefix
# Number: 0, 1, 4, 5, 8, 9, 10, 13, 15, 16
P23710=0

# Account. 0 - Account 1, 1 - Account 2, 2 - Account 3, 3 - Account 4, 4 - Account 5, 5 - Account 6
# Number: 0 - 5
P23711=0

# Name
# String
P23712=

# UserID
# String
P23713=

#######################################################################################
# EXT MPK 144
#######################################################################################

# Key Mode.# 0 - Speed Dial, 1 - BLF, 4 - Speed Dial via active account, 5 - DialDTMF, 8 - Call Transfer, 9 - CallPark, 10 - Call Intercom, 13 - Multicast Paging, 15 - Speed Conference, 16 - Dial prefix
# Number: 0, 1, 4, 5, 8, 9, 10, 13, 15, 16
P23715=0

# Account. 0 - Account 1, 1 - Account 2, 2 - Account 3, 3 - Account 4, 4 - Account 5, 5 - Account 6
# Number: 0 - 5
P23716=0

# Name
# String
P23717=

# UserID
# String
P23718=

#######################################################################################
# EXT MPK 145
#######################################################################################

# Key Mode.# 0 - Speed Dial, 1 - BLF, 4 - Speed Dial via active account, 5 - DialDTMF, 8 - Call Transfer, 9 - CallPark, 10 - Call Intercom, 13 - Multicast Paging, 15 - Speed Conference, 16 - Dial prefix
# Number: 0, 1, 4, 5, 8, 9, 10, 13, 15, 16
P23720=0

# Account. 0 - Account 1, 1 - Account 2, 2 - Account 3, 3 - Account 4, 4 - Account 5, 5 - Account 6
# Number: 0 - 5
P23721=0

# Name
# String
P23722=

# UserID
# String
P23723=

#######################################################################################
# EXT MPK 146
#######################################################################################

# Key Mode.# 0 - Speed Dial, 1 - BLF, 4 - Speed Dial via active account, 5 - DialDTMF, 8 - Call Transfer, 9 - CallPark, 10 - Call Intercom, 13 - Multicast Paging, 15 - Speed Conference, 16 - Dial prefix
# Number: 0, 1, 4, 5, 8, 9, 10, 13, 15, 16
P23725=0

# Account. 0 - Account 1, 1 - Account 2, 2 - Account 3, 3 - Account 4, 4 - Account 5, 5 - Account 6
# Number: 0 - 5
P23726=0

# Name
# String
P23727=

# UserID
# String
P23728=

#######################################################################################
# EXT MPK 147
#######################################################################################

# Key Mode.# 0 - Speed Dial, 1 - BLF, 4 - Speed Dial via active account, 5 - DialDTMF, 8 - Call Transfer, 9 - CallPark, 10 - Call Intercom, 13 - Multicast Paging, 15 - Speed Conference, 16 - Dial prefix
# Number: 0, 1, 4, 5, 8, 9, 10, 13, 15, 16
P23730=0

# Account. 0 - Account 1, 1 - Account 2, 2 - Account 3, 3 - Account 4, 4 - Account 5, 5 - Account 6
# Number: 0 - 5
P23731=0

# Name
# String
P23732=

# UserID
# String
P23733=

#######################################################################################
# EXT MPK 148
#######################################################################################

# Key Mode.# 0 - Speed Dial, 1 - BLF, 4 - Speed Dial via active account, 5 - DialDTMF, 8 - Call Transfer, 9 - CallPark, 10 - Call Intercom, 13 - Multicast Paging, 15 - Speed Conference, 16 - Dial prefix
# Number: 0, 1, 4, 5, 8, 9, 10, 13, 15, 16
P23735=0

# Account. 0 - Account 1, 1 - Account 2, 2 - Account 3, 3 - Account 4, 4 - Account 5, 5 - Account 6
# Number: 0 - 5
P23736=0

# Name
# String
P23737=

# UserID
# String
P23738=

#######################################################################################
# EXT MPK 149
#######################################################################################

# Key Mode.# 0 - Speed Dial, 1 - BLF, 4 - Speed Dial via active account, 5 - DialDTMF, 8 - Call Transfer, 9 - CallPark, 10 - Call Intercom, 13 - Multicast Paging, 15 - Speed Conference, 16 - Dial prefix
# Number: 0, 1, 4, 5, 8, 9, 10, 13, 15, 16
P23740=0 

# Account. 0 - Account 1, 1 - Account 2, 2 - Account 3, 3 - Account 4, 4 - Account 5, 5 - Account 6
# Number: 0 - 5
P23741=0

# Name
# String
P23742=

# UserID
# String
P23743=

#######################################################################################
# EXT MPK 150
#######################################################################################

# Key Mode.# 0 - Speed Dial, 1 - BLF, 4 - Speed Dial via active account, 5 - DialDTMF, 8 - Call Transfer, 9 - CallPark, 10 - Call Intercom, 13 - Multicast Paging, 15 - Speed Conference, 16 - Dial prefix
# Number: 0, 1, 4, 5, 8, 9, 10, 13, 15, 16
P23745=0

# Account. 0 - Account 1, 1 - Account 2, 2 - Account 3, 3 - Account 4, 4 - Account 5, 5 - Account 6
# Number: 0 - 5
P23746=0

# Name
# String
P23747=

# UserID
# String
P23748=

#######################################################################################
# EXT MPK 151
#######################################################################################

# Key Mode.# 0 - Speed Dial, 1 - BLF, 4 - Speed Dial via active account, 5 - DialDTMF, 8 - Call Transfer, 9 - CallPark, 10 - Call Intercom, 13 - Multicast Paging, 15 - Speed Conference, 16 - Dial prefix
# Number: 0, 1, 4, 5, 8, 9, 10, 13, 15, 16
P23750=0

# Account. 0 - Account 1, 1 - Account 2, 2 - Account 3, 3 - Account 4, 4 - Account 5, 5 - Account 6
# Number: 0 - 5
P23751=0

# Name
# String
P23752=

# UserID
# String
P23753=

#######################################################################################
# EXT MPK 152
#######################################################################################

# Key Mode.# 0 - Speed Dial, 1 - BLF, 4 - Speed Dial via active account, 5 - DialDTMF, 8 - Call Transfer, 9 - CallPark, 10 - Call Intercom, 13 - Multicast Paging, 15 - Speed Conference, 16 - Dial prefix
# Number: 0, 1, 4, 5, 8, 9, 10, 13, 15, 16
P23755=0

# Account. 0 - Account 1, 1 - Account 2, 2 - Account 3, 3 - Account 4, 4 - Account 5, 5 - Account 6
# Number: 0 - 5
P23756=0

# Name
# String
P23757=

# UserID
# String
P23758=

#######################################################################################
# EXT MPK 153
#######################################################################################

# Key Mode.# 0 - Speed Dial, 1 - BLF, 4 - Speed Dial via active account, 5 - DialDTMF, 8 - Call Transfer, 9 - CallPark, 10 - Call Intercom, 13 - Multicast Paging, 15 - Speed Conference, 16 - Dial prefix
# Number: 0, 1, 4, 5, 8, 9, 10, 13, 15, 16
P23760=0

# Account. 0 - Account 1, 1 - Account 2, 2 - Account 3, 3 - Account 4, 4 - Account 5, 5 - Account 6
# Number: 0 - 5
P23761=0

# Name
# String
P23762=

# UserID
# String
P23763=

#######################################################################################
# EXT MPK 154
#######################################################################################

# Key Mode.# 0 - Speed Dial, 1 - BLF, 4 - Speed Dial via active account, 5 - DialDTMF, 8 - Call Transfer, 9 - CallPark, 10 - Call Intercom, 13 - Multicast Paging, 15 - Speed Conference, 16 - Dial prefix
# Number: 0, 1, 4, 5, 8, 9, 10, 13, 15, 16
P23765=0

# Account. 0 - Account 1, 1 - Account 2, 2 - Account 3, 3 - Account 4, 4 - Account 5, 5 - Account 6
# Number: 0 - 5
P23766=0

# Name
# String
P23767=

# UserID
# String
P23768=

#######################################################################################
# EXT MPK 155
#######################################################################################

# Key Mode.# 0 - Speed Dial, 1 - BLF, 4 - Speed Dial via active account, 5 - DialDTMF, 8 - Call Transfer, 9 - CallPark, 10 - Call Intercom, 13 - Multicast Paging, 15 - Speed Conference, 16 - Dial prefix
# Number: 0, 1, 4, 5, 8, 9, 10, 13, 15, 16
P23770=0

# Account. 0 - Account 1, 1 - Account 2, 2 - Account 3, 3 - Account 4, 4 - Account 5, 5 - Account 6
# Number: 0 - 5
P23771=0

# Name
# String
P23772=

# UserID
# String
P23773=

#######################################################################################
# EXT MPK 156
#######################################################################################

# Key Mode.# 0 - Speed Dial, 1 - BLF, 4 - Speed Dial via active account, 5 - DialDTMF, 8 - Call Transfer, 9 - CallPark, 10 - Call Intercom, 13 - Multicast Paging, 15 - Speed Conference, 16 - Dial prefix
# Number: 0, 1, 4, 5, 8, 9, 10, 13, 15, 16
P23775=0

# Account. 0 - Account 1, 1 - Account 2, 2 - Account 3, 3 - Account 4, 4 - Account 5, 5 - Account 6
# Number: 0 - 5
P23776=0

# Name
# String
P23777=

# UserID
# String
P23778=

#######################################################################################
# EXT MPK 157
#######################################################################################

# Key Mode.# 0 - Speed Dial, 1 - BLF, 4 - Speed Dial via active account, 5 - DialDTMF, 8 - Call Transfer, 9 - CallPark, 10 - Call Intercom, 13 - Multicast Paging, 15 - Speed Conference, 16 - Dial prefix
# Number: 0, 1, 4, 5, 8, 9, 10, 13, 15, 16
P23780=0

# Account. 0 - Account 1, 1 - Account 2, 2 - Account 3, 3 - Account 4, 4 - Account 5, 5 - Account 6
# Number: 0 - 5
P23781=0

# Name
# String
P23782=

# UserID
# String
P23783=

#######################################################################################
# EXT MPK 158
#######################################################################################

# Key Mode.# 0 - Speed Dial, 1 - BLF, 4 - Speed Dial via active account, 5 - DialDTMF, 8 - Call Transfer, 9 - CallPark, 10 - Call Intercom, 13 - Multicast Paging, 15 - Speed Conference, 16 - Dial prefix
# Number: 0, 1, 4, 5, 8, 9, 10, 13, 15, 16
P23785=0

# Account. 0 - Account 1, 1 - Account 2, 2 - Account 3, 3 - Account 4, 4 - Account 5, 5 - Account 6
# Number: 0 - 5
P23786=0

# Name
# String
P23787=

# UserID
# String
P23788=

#######################################################################################
# EXT MPK 159
#######################################################################################

# Key Mode.# 0 - Speed Dial, 1 - BLF, 4 - Speed Dial via active account, 5 - DialDTMF, 8 - Call Transfer, 9 - CallPark, 10 - Call Intercom, 13 - Multicast Paging, 15 - Speed Conference, 16 - Dial prefix
# Number: 0, 1, 4, 5, 8, 9, 10, 13, 15, 16
P23790=0

# Account. 0 - Account 1, 1 - Account 2, 2 - Account 3, 3 - Account 4, 4 - Account 5, 5 - Account 6
# Number: 0 - 5
P23791=0

# Name
# String
P23792=

# UserID
# String
P23793=

#######################################################################################
# EXT MPK 160
#######################################################################################

# Key Mode.# 0 - Speed Dial, 1 - BLF, 4 - Speed Dial via active account, 5 - DialDTMF, 8 - Call Transfer, 9 - CallPark, 10 - Call Intercom, 13 - Multicast Paging, 15 - Speed Conference, 16 - Dial prefix
# Number: 0, 1, 4, 5, 8, 9, 10, 13, 15, 16
P23795=0

# Account. 0 - Account 1, 1 - Account 2, 2 - Account 3, 3 - Account 4, 4 - Account 5, 5 - Account 6
# Number: 0 - 5
P23796=0

# Name
# String
P23797=

# UserID
# String
P23798=

#######################################################################
##  Value-added Service - Value-added Service                        ##
#######################################################################
#######################################################################
# GDS Settings No.1                                                   #
#######################################################################
# Service Type
# 0 - Door System, 1 - DTMF
P32000=0
# Door System Type
# 0 - GDS, 1 - Others, 2 - Baudisch
P32001=0
# Display Name. String
P32002=
# System Number. Number
P32003=
# Access Password/DTMF Content. String
P32004=
# System Ringtone
P22241=/system/media/audio/ringtones/DingDong.wav
#######################################################################
# GDS Settings No.2                                                   #
#######################################################################
# Service Type
# 0 - Door System, 1 - DTMF
P32005=0
# Door System Type
# 0 - GDS, 1 - Others, 2 - Baudisch
P32006=0
# Display Name. String
P32007=
# System Number. Number
P32008=
# Access Password/DTMF Content. String
P32009=
# System Ringtone
P22242=/system/media/audio/ringtones/DingDong.wav
#######################################################################
# GDS Settings No.3                                                   #
#######################################################################
# Service Type
# 0 - Door System, 1 - DTMF
P32010=0
# Door System Type
# 0 - GDS, 1 - Others, 2 - Baudisch
P32011=0
# Display Name. String
P32012=
# System Number. Number
P32013=
# Access Password/DTMF Content. String
P32014=
# System Ringtone
P22243=/system/media/audio/ringtones/DingDong.wav
#######################################################################
# GDS Settings No.4                                                   #
#######################################################################
# Service Type
# 0 - Door System, 1 - DTMF
P32015=0
# Door System Type
# 0 - GDS, 1 - Others, 2 - Baudisch
P32016=0 
# Display Name. String
P32017=
# System Number. Number
P32018=
# Access Password/DTMF Content. String
P32019=
# System Ringtone
P22244=/system/media/audio/ringtones/DingDong.wav
#######################################################################
# GDS Settings No.5                                                   #
#######################################################################
# Service Type
# 0 - Door System, 1 - DTMF
P32020=0
# Door System Type
# 0 - GDS, 1 - Others, 2 - Baudisch
P32021=0
# Display Name. String
P32022=
# System Number. Number
P32023=
# Access Password/DTMF Content. String
P32024=
# System Ringtone
P22245=/system/media/audio/ringtones/DingDong.wav
#######################################################################
# GDS Settings No.6                                                   #
#######################################################################
# Service Type
# 0 - Door System, 1 - DTMF
P32025=0
# Door System Type
# 0 - GDS, 1 - Others, 2 - Baudisch
P32026=0
# Display Name. String
P32027=
# System Number. Number
P32028=
# Access Password/DTMF Content. String
P32029=
# System Ringtone
P22246=/system/media/audio/ringtones/DingDong.wav
#######################################################################
# GDS Settings No.7                                                   #
#######################################################################
# Service Type
# 0 - Door System, 1 - DTMF
P32030=0
# Door System Type
# 0 - GDS, 1 - Others, 2 - Baudisch
P32031=0
# Display Name. String
P32032=
# System Number. Number
P32033=
# Access Password/DTMF Content. String
P32034=
# System Ringtone
P22247=/system/media/audio/ringtones/DingDong.wav
#######################################################################
# GDS Settings No.8                                                   #
#######################################################################
# Service Type
# 0 - Door System, 1 - DTMF
P32035=0
# Door System Type
# 0 - GDS, 1 - Others, 2 - Baudisch
P32036=0
# Display Name. String
P32037=
# System Number. Number
P32038=
# Access Password/DTMF Content. String
P32039=
# System Ringtone
P22248=/system/media/audio/ringtones/DingDong.wav
#######################################################################
# GDS Settings No.9                                                   #
#######################################################################
# Service Type
# 0 - Door System, 1 - DTMF
P32040=0
# Door System Type
# 0 - GDS, 1 - Others, 2 - Baudisch
P32041=0
# Display Name. String
P32042=
# System Number. Number
P32043=
# Access Password/DTMF Content. String
P32044=
# System Ringtone
P22249=/system/media/audio/ringtones/DingDong.wav
#######################################################################
# GDS Settings No.10                                                  #
#######################################################################
# Service Type
# 0 - Door System, 1 - DTMF
P32045=0
# Door System Type
# 0 - GDS, 1 - Others, 2 - Baudisch
P32046=0
# Display Name. String
P32047=
# System Number. Number
P32048=
# Access Password/DTMF Content. String
P32049=
# System Ringtone
P22250=/system/media/audio/ringtones/DingDong.wav

#######################################################################
##  Value-added Service - General Settings                           ##
#######################################################################
# Display Open Door Button when Calling
# Number: 0,1
P22316=1

# Enable Preview
# Number: 0,1
P22357=1
#######################################################################
##  Value-added Service - BroadSoft Settings                         ##
#######################################################################
#######################################################################
##  Account 1                                                        ##
#######################################################################
# Feature Key Synchronization. 0 - Disable,  1 - Broadsoft/Metaswitch. Default value is 0
# Number: 0, 1
P2325=0

# Enable BroadSoft Call Park. 0 - Disable, 1 - Enable. Default value is 0
# Number: 0, 1
P2388=0 

# Conference URI
# String
P2318=


# BroadSoft Call Center. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P2341=0

# Hoteling Event. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P2342=0

# Call Center Status. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P2343=0

# Enable SCA (Shared Call Appearance). 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P1363=0

# Enable Barge-in. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P2337=0

# Auto-filling Callpark Feature code. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P2335=1

# Callpark Feature Code
P2336=

# Line-seize Timeout (in seconds). Number: 15 - 60. Default value is 15
P2313=15
#######################################################################
##  Account 2                                                        ##
#######################################################################
# Feature Key Synchronization. 0 - Disable,  1 - Broadsoft. Default value is 0
# Number: 0, 1
P2425=0

# Enable BroadSoft Call Park. 0 - Disable, 1 - Enable. Default value is 0
# Number: 0, 1
P2488=0 

# Conference URI
# String
P2418=

# Enable SCA (Shared Call Appearance). 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P1365=0

# BroadSoft Call Center. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P2441=0

# Hoteling Event. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P2442=0

# Call Center Status. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P2443=0

# Enable BargeIn. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P2437=0

# Auto-filling Callpark Feature code. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P2435=1

# Callpark Feature Code
P2436=

# Line-seize Timeout (in seconds). Number: 15 - 60. Default value is 15
P2413=15
#######################################################################
##  Account 3                                                        ##
#######################################################################
# Feature Key Synchronization. 0 - Disable,  1 - Broadsoft. Default value is 0
# Number: 0, 1
P2525=0

# Enable BroadSoft Call Park. 0 - Disable, 1 - Enable. Default value is 0
# Number: 0, 1
P2588=0 

# Conference URI
# String
P2518=

# Enable SCA (Shared Call Appearance). 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P1367=0

# BroadSoft Call Center. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P2541=0

# Hoteling Event. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P2542=0

# Call Center Status. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P2543=0

# Enable BargeIn. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P2537=0

# Auto-filling Callpark Feature code. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P2535=1

# Callpark Feature Code
P2536=

# Line-seize Timeout (in seconds). Number: 15 - 60. Default value is 15
P2513=15
#######################################################################
##  Account 4                                                        ##
#######################################################################
# Feature Key Synchronization. 0 - Disable,  1 - Broadsoft. Default value is 0
# Number: 0, 1
P2625=0

# Enable BroadSoft Call Park. 0 - Disable, 1 - Enable. Default value is 0
# Number: 0, 1
P2688=0 

# Conference URI
# String
P2618=

# Enable SCA (Shared Call Appearance). 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P1369=0

# BroadSoft Call Center. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P2641=0

# Hoteling Event. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P2642=0

# Call Center Status. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P2643=0

# Enable BargeIn. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P2637=0

# Auto-filling Callpark Feature code. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P2635=1

# Callpark Feature Code
P2636=

# Line-seize Timeout (in seconds). Number: 15 - 60. Default value is 15
P2613=15
#######################################################################
##  Account 5                                                        ##
#######################################################################
# Feature Key Synchronization. 0 - Disable,  1 - Broadsoft. Default value is 0
# Number: 0, 1
P2725=0

# Enable BroadSoft Call Park. 0 - Disable, 1 - Enable. Default value is 0
# Number: 0, 1
P2788=0 

# Conference URI
# String
P2718=

# Enable SCA (Shared Call Appearance). 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P1371=0

# BroadSoft Call Center. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P2741=0

# Hoteling Event. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P2742=0

# Call Center Status. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P2743=0

# Enable BargeIn. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P2737=0

# Auto-filling Callpark Feature code. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P2735=1

# Callpark Feature Code
P2736=

# Line-seize Timeout (in seconds). Number: 15 - 60. Default value is 15
P2713=15
#######################################################################
##  Account 6                                                        ##
#######################################################################
# Feature Key Synchronization. 0 - Disable,  1 - Broadsoft. Default value is 0
# Number: 0, 1
P2825=0

# Enable BroadSoft Call Park. 0 - Disable, 1 - Enable. Default value is 0
# Number: 0, 1
P2888=0 

# Conference URI
# String
P2818=

# Enable SCA (Shared Call Appearance). 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P1373=0

# BroadSoft Call Center. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P2841=0

# Hoteling Event. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P2842=0

# Call Center Status. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P2843=0

# Enable BargeIn. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P2837=0

# Auto-filling Callpark Feature code. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P2835=1

# Callpark Feature Code
P2836=

# Line-seize Timeout (in seconds). Number: 15 - 60. Default value is 15
P2813=15
#######################################################################
##  Account 7                                                        ##
#######################################################################
# Feature Key Synchronization. 0 - Disable,  1 - Broadsoft. Default value is 0
# Number: 0, 1
P51625=0

# Enable BroadSoft Call Park. 0 - Disable, 1 - Enable. Default value is 0
# Number: 0, 1
P51688=0 

# Conference URI
# String
P51618=

# Enable SCA (Shared Call Appearance). 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P29613=0

# BroadSoft Call Center. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P51641=0

# Hoteling Event. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P51642=0

# Call Center Status. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P51643=0

# Enable BargeIn. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P51637=0

# Auto-filling Callpark Feature code. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P51635=1

# Callpark Feature Code
P51636=

# Line-seize Timeout (in seconds). Number: 15 - 60. Default value is 15
P51613=15
#######################################################################
##  Account 8                                                        ##
#######################################################################
# Feature Key Synchronization. 0 - Disable,  1 - Broadsoft. Default value is 0
# Number: 0, 1
P51725=0

# Enable BroadSoft Call Park. 0 - Disable, 1 - Enable. Default value is 0
# Number: 0, 1
P51788=0 

# Conference URI
# String
P51718=

# Enable SCA (Shared Call Appearance). 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P29615=0

# BroadSoft Call Center. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P51741=0

# Hoteling Event. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P51742=0

# Call Center Status. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P51743=0

# Enable BargeIn. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P51737=0

# Auto-filling Callpark Feature code. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P51735=1

# Callpark Feature Code
P51736=

# Line-seize Timeout (in seconds). Number: 15 - 60. Default value is 15
P51713=15
#######################################################################
##  Account 9                                                        ##
#######################################################################
# Feature Key Synchronization. 0 - Disable,  1 - Broadsoft. Default value is 0
# Number: 0, 1
P51825=0

# Enable BroadSoft Call Park. 0 - Disable, 1 - Enable. Default value is 0
# Number: 0, 1
P51888=0 

# Conference URI
# String
P51818=

# Enable SCA (Shared Call Appearance). 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P29617=0

# BroadSoft Call Center. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P51841=0

# Hoteling Event. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P51842=0

# Call Center Status. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P51843=0

# Enable BargeIn. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P51837=0

# Auto-filling Callpark Feature code. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P51835=1

# Callpark Feature Code
P51836=

# Line-seize Timeout (in seconds). Number: 15 - 60. Default value is 15
P51813=15
#######################################################################
##  Account 10                                                       ##
#######################################################################
# Feature Key Synchronization. 0 - Disable,  1 - Broadsoft. Default value is 0
# Number: 0, 1
P51925=0

# Enable BroadSoft Call Park. 0 - Disable, 1 - Enable. Default value is 0
# Number: 0, 1
P51988=0 

# Conference URI
# String
P51918=

# Enable SCA (Shared Call Appearance). 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P29619=0

# BroadSoft Call Center. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P51941=0

# Hoteling Event. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P51942=0

# Call Center Status. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P51943=0

# Enable BargeIn. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P51937=0

# Auto-filling Callpark Feature code. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P51935=1

# Callpark Feature Code
P51936=

# Line-seize Timeout (in seconds). Number: 15 - 60. Default value is 15
P51913=15
#######################################################################
##  Account 11                                                       ##
#######################################################################
# Feature Key Synchronization. 0 - Disable,  1 - Broadsoft. Default value is 0
# Number: 0, 1
P52025=0

# Enable BroadSoft Call Park. 0 - Disable, 1 - Enable. Default value is 0
# Number: 0, 1
P52088=0 

# Conference URI
# String
P52018=

# Enable SCA (Shared Call Appearance). 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P29621=0

# BroadSoft Call Center. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P52041=0

# Hoteling Event. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P52042=0

# Call Center Status. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P52043=0

# Enable BargeIn. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P52037=0

# Auto-filling Callpark Feature code. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P52035=1

# Callpark Feature Code
P52036=

# Line-seize Timeout (in seconds). Number: 15 - 60. Default value is 15
P52013=15
#######################################################################
##  Account 12                                                       ##
#######################################################################
# Feature Key Synchronization. 0 - Disable,  1 - Broadsoft. Default value is 0
# Number: 0, 1
P52125=0

# Enable BroadSoft Call Park. 0 - Disable, 1 - Enable. Default value is 0
# Number: 0, 1
P52188=0 

# Conference URI
# String
P52118=

# Enable SCA (Shared Call Appearance). 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P29623=0

# BroadSoft Call Center. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P52141=0

# Hoteling Event. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P52142=0

# Call Center Status. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P52143=0

# Enable BargeIn. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P52137=0

# Auto-filling Callpark Feature code. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P52135=1

# Callpark Feature Code
P52136=

# Line-seize Timeout (in seconds). Number: 15 - 60. Default value is 15
P52113=15
#######################################################################
##  Account 13                                                       ##
#######################################################################
# Feature Key Synchronization. 0 - Disable,  1 - Broadsoft. Default value is 0
# Number: 0, 1
P52225=0

# Enable BroadSoft Call Park. 0 - Disable, 1 - Enable. Default value is 0
# Number: 0, 1
P52288=0 

# Conference URI
# String
P52218=

# Enable SCA (Shared Call Appearance). 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P29625=0

# BroadSoft Call Center. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P52241=0

# Hoteling Event. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P52242=0

# Call Center Status. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P52243=0

# Enable BargeIn. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P52237=0

# Auto-filling Callpark Feature code. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P52235=1

# Callpark Feature Code
P52236=

# Line-seize Timeout (in seconds). Number: 15 - 60. Default value is 15
P52213=15
#######################################################################
##  Account 14                                                       ##
#######################################################################
# Feature Key Synchronization. 0 - Disable,  1 - Broadsoft. Default value is 0
# Number: 0, 1
P52325=0

# Enable BroadSoft Call Park. 0 - Disable, 1 - Enable. Default value is 0
# Number: 0, 1
P52388=0 

# Conference URI
# String
P52318=

# Enable SCA (Shared Call Appearance). 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P29627=0

# BroadSoft Call Center. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P52341=0

# Hoteling Event. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P52342=0

# Call Center Status. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P52343=0

# Enable BargeIn. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P52337=0

# Auto-filling Callpark Feature code. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P52335=1

# Callpark Feature Code
P52336=

# Line-seize Timeout (in seconds). Number: 15 - 60. Default value is 15
P52313=15
#######################################################################
##  Account 15                                                       ##
#######################################################################
# Feature Key Synchronization. 0 - Disable,  1 - Broadsoft. Default value is 0
# Number: 0, 1
P52425=0

# Enable BroadSoft Call Park. 0 - Disable, 1 - Enable. Default value is 0
# Number: 0, 1
P52488=0 

# Conference URI
# String
P52418=

# Enable SCA (Shared Call Appearance). 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P29629=0

# BroadSoft Call Center. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P52441=0

# Hoteling Event. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P52442=0

# Call Center Status. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P52443=0

# Enable BargeIn. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P52437=0

# Auto-filling Callpark Feature code. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P52435=1

# Callpark Feature Code
P52436=

# Line-seize Timeout (in seconds). Number: 15 - 60. Default value is 15
P52413=15
#######################################################################
##  Account 16                                                       ##
#######################################################################
# Feature Key Synchronization. 0 - Disable,  1 - Broadsoft. Default value is 0
# Number: 0, 1
P52525=0

# Enable BroadSoft Call Park. 0 - Disable, 1 - Enable. Default value is 0
# Number: 0, 1
P52588=0 

# Conference URI
# String
P52518=

# Enable SCA (Shared Call Appearance). 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P29631=0

# BroadSoft Call Center. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P52541=0

# Hoteling Event. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P52542=0

# Call Center Status. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P52543=0

# Enable BargeIn. 0 - No, 1 - Yes. Default value is 0
# Number: 0, 1
P52537=0

# Auto-filling Callpark Feature code. 0 - No, 1 - Yes. Default value is 1
# Number: 0, 1
P52535=1

# Callpark Feature Code
P52536=

# Line-seize Timeout (in seconds). Number: 15 - 60. Default value is 15
P52513=15

####################################################################
####   BroadSoft Directories                                    ####
####################################################################
# Authentication Type. 0 - SIP Credentials, 1 - LogIn Credentials.
# Number: 0, 1
P22054=0

# Server. Broadsoft XSI server address with protocol.
# String
P1591=

# Port. Port of the Broadsoft XSI server.
# String
P1592=

# Action Path. Action Path for BroadSoft XSI server.
# String
P2937=

# BroadWorks User ID. User IDfor Broadsoft XSI server.
# String
P22034=

# SIP Authentication ID. Username for Broadsoft XSI server.
# String
P1593=

# SIP Authentication Password. Password for Broadsoft XSI server.
# String
P1594=

# Login Password
# String
P22103=

# BroadSoft Directory Hits
# Number
P22014=

# Group Directory. 0 - Disabled, 1 - Enabled. Default value is 1.
# Number: 0, 1
P2971=1

# Group Directory Name.
# String
P2972=

# Enterprise Directory. 0 - Disabled, 1 - Enabled. Default value is 1.
# Number: 0, 1
P2973=1

# Enterprise Directory Name.
# String
P2974=

# Group Common. 0 - Disabled, 1 - Enabled. Default value is 1.
# Number: 0, 1
P2975=1

# Group Common Name.
# String
P2976=

# Enterprise Common. 0 - Disabled, 1 - Enabled. Default value is 1.
# Number: 0, 1
P2977=1

# Enterprise Common Name.
# String
P2978=

# Personal Directory. 0 - Disabled, 1 - Enabled. Default value is 1.
# Number: 0, 1
P2979=1

# Personal Directory Name.
# String
P2980=

# Polycom Phonebook. 0 - Disabled, 1 - Enabled. Default value is 0.
# Number: 0, 1
P8343=0

# Polycome Phonebook Name.
# String
P8344=

# Missed Call Log. 0 - Disabled, 1 - Enabled. Default value is 1.
# Number: 0, 1
P2981=1

# Missed Call Log Name.
# String
P2982=

# Placed Call Log. 0 - Disabled, 1 - Enabled. Default value is 1.
# Number: 0, 1
P2983=1

# Placed Call Log Name.
# String
P2984=

# Received Call Log. 0 - Disabled, 1 - Enabled. Default value is 1.
# Number: 0, 1
P2985=1

# Received Call Log Name.
# String
P2986=

##########################################################
##   Broadsoft IM&P                                     ##
##########################################################

# Server
P6006=

# Port
P6005=

# Username
P2966=

# Password
P2967=

# Enable Broadsoft IM&P. 0 - No, 1 - Yes. Default Value is 0
P2964=

# Associated Broadsoft Account. 0 - Account1, 1 - Account2, 2 - Account3, 3 - Account4, 4 - Account5, 5 - Account6, ..., 15 - Account16
# Default Vaule is 0
# Number
P2965=

# Auto Login. 0 - No, 1 - Yes. Default Value is 0
# Number
P2968=

# Display Non XMPP Contacts. 0 - No, 1 - Yes. Default Value is 0
# Number
P2969=